## HSV0001

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0001 ERROR DURING SVP FUNCTION DIAGNOSE MSSFCALL OBTAIN SYSTEM INFORMATION

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0010 OK, information delivered.
06F0 The SVP function is not executable on this configuration.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0005

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0005 ERROR DURING SVP FUNCTION OBTAIN CHANNEL PATH INFORMATION

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0300 Command not supported.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0006

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0006 ERROR DURING SVP FUNCTION VARY CHANNEL PATH ONLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0300 Command not supported.
0400 Hardware error.
0401 The CHANNEL PATH is not installed or already "online"
or switching online is disabled.
0402 The CHANNEL CONTROLLER is not "online".
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0007

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0007 ERROR DURING SVP FUNCTION CHANNEL PATH OFFLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0300 Command not supported.
0400 Hardware error.
0401 The CHANNEL PATH is not installed or switching offline is
disabled.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0020

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0020 ERROR DURING THE SVP FUNCTION DIAGNOSE WRITE CONSOLE.

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.

## HSV0023

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0023 ERROR DURING SVP FUNCTION READ IORSF

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0001 The IORSF end was exceeded.
0300 Command not supported.
1101 The indicated SVP cannot operate.
1102 The IORSF number is too large.
1103 The start sector number exceeded the maximum sector of the
IORSF file.
3000 IORSF file access error.
3500 The buffer busy condition was detected.
3600 The IO-configuration is not supported or a logical error
was detected.
PARE Parameter error.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0024

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0024 ERROR DURING SVP FUNCTION WRITE IORSF

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0001 The IORSF end was exceeded.
0300 Command not supported.
1101 The indicated SVP cannot operate.
1102 The IORSF number is too large.
1103 The start sector number exceeded the maximum sector of the
IORSF file.
3000 IORSF file access error.
3100 Write-open operation for IORSF failed.
3101 Write-close operation for IORSF failed.
3200 The IORSF is already in write-open status.
3300 The IORSF is not in write-open status.
3400 The IORSF is write-protected.
3500 The buffer busy condition was detected.
3600 The IO-configuration is not supported or a logical error
was detected.
PARE Parameter error.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0025

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0025 ERROR DURING SVP FUNCTION READ ACTIVE IORSF

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0001 The IORSF end was exceeded.
1103 The start sector number exceeded the maximum sector of the
IORSF file.
3000 IORSF file access error.
PARE Parameter error.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0030

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0030 ERROR DURING THE SVP FUNCTION READ HARDWARE STORAGE AREA

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
0020 OK, information delivered.
0040 Hardware error.
4040 Error during open or read of the HSA.
41F0 The HSA-file is not open.
50F0 The end of HSA-file was exceeded.
06F0 The SVP function is not executable on this configuration.
PARE Parameter error.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0034

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0034 ERROR DURING SVP FUNCTION VARY CPU ONLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0300 Command not supported.
1101 The CPU belongs to another configuration.
1102 The CPU was already "online".
0400 Hardware error.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0035

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0035 ERROR DURING SVP FUNCTION CPU OFFLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0300 Command not supported.
1101 The CPU belongs to another configuration.
1102 The CPU was already "offline".
1103 The CPU is last online CPU.
0400 Hardware error.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0036

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0036 ERROR DURING THE SVP FUNCTION START CPU

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The SVP driver is busy.
NSUP The function is not supported.
CC=1 The SIGP instruction was completed with condition code 1.
CC=2 The SIGP instruction was completed with condition code 2.
CC=3 The SIGP instruction was completed with condition code 3.

## HSV0037

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0037 ERROR DURING THE SVP FUNCTION STOP CPU

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The SVP driver is busy.
NSUP The function is not supported.
CC=1 The SIGP instruction was completed with condition code 1.
CC=2 The SIGP instruction was completed with condition code 2.
CC=3 The SIGP instruction was completed with condition code 3.

## HSV0041

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0041 ERROR DURING THE SVP FUNCTION GET IPL DEVICE LIST

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0042

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0042 ERROR DURING THE SVP FUNCTION MODIFY IPL DEVICE LIST

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
GERR The DIAGNOSE instruction could not be executed because
of a global error.

## HSV0048

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0048 ERROR DURING SVP FUNCTION GET NUMBER OF CPUS

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0300 Command not supported.
0400 Hardware error.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
CC=3 The DIAGNOSE instruction was completed with condition code 3.

## HSV0049

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0049 ERROR DURING SVP FUNCTION NOTIFY CPU OFFLINE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0300 Command not supported.
0400 Hardware error.
0401 Wrong CPU.
BUSY The DIAGNOSE instruction was completed with condition code 2
or the SVP driver is busy.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0050

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0050 ERROR DURING THE SVP FUNCTION DIAGNOSE SDAP READ IO-UNIT FROM IORSF

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0300 Command not supported.
0301 The caller has no authorization for this function.
1104 The specified unit type is unknown.
1105 The specified I/O unit does not exist in IORSF.
BUSY The DIAGNOSE instruction was completed with condition code 1
or 2.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0051

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0051 ERROR DURING THE SVP FUNCTION DIAGNOSE SDAP ADD IO-UNIT TO IORSF

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0300 Command not supported.
0301 The caller has no authorization for this function.
0421 Insufficient hardware space to store control information.
1103 No empty area to store specified I/O unit.
1104 The specified unit type is unknown.
1105 The specified I/O unit does not exist or already exist.
1106 Effective byte length is wrong.
1107 No unit to which specified i/0 unit can be connected.
1108 Condition for replacing or adding an I/O unit is not met.
1109 Replacement code or unit type not supported by hardware.
BUSY The DIAGNOSE instruction was completed with condition code 1
or 2.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0052

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0052 ERROR DURING THE SVP FUNCTION DIAGNOSE SDAP DELETE IO-UNIT FROM IORSF

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
FFxx Hardware error.
0300 Command not supported.
0301 The caller has no authorization for this function.
0421 Insufficient hardware space to store control information.
1103 No empty area to store specified I/O unit.
1104 The specified unit type is unknown.
1105 The specified I/O unit does not exist.
1106 Effective byte length is wrong.
1107 A lower-level unit is connected to specified I/O unit.
1108 Condition for replacing or deleting an I/O unit is not met.
1109 Replacement code or unit type not supported by hardware.
BUSY The DIAGNOSE instruction was completed with condition code 1
or 2.
NSUP The DIAGNOSE instruction was completed with condition code 3.
TOUT The DIAGNOSE instruction was not terminated with a service
signal interrupt during the waiting time.

## HSV0062

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0062 ERROR DURING THE SVP FUNCTION DIAGNOSE RSC DR-CONTROL

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The SVP driver is busy.
NSUP The function is not supported.
CC=1 The DIAGNOSE instruction was completed with condition code 1.
CC=2 The DIAGNOSE instruction was completed with condition code 2.
CC=3 The DIAGNOSE instruction was completed with condition code 3.

## HSV0063

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0063 ERROR DURING THE SVP FUNCTION DIAGNOSE RSC DR-RESPONSE

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The SVP driver is busy.
NSUP The function is not supported.
CC=1 The DIAGNOSE instruction was completed with condition code 1.
CC=2 The DIAGNOSE instruction was completed with condition code 2.
CC=3 The DIAGNOSE instruction was completed with condition code 3.

## HSV0064

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0064 ERROR DURING THE SVP FUNCTION DIAGNOSE READ FIRMWARE-INFO

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The SVP driver is busy.
NSUP The function is not supported.
CC=1 The DIAGNOSE instruction was completed with condition code 1.
CC=2 The DIAGNOSE instruction was completed with condition code 2.
CC=3 The DIAGNOSE instruction was completed with condition code 3.

## HSV0069

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0069 ERROR DURING THE SVP FUNCTION DIAGNOSE DEFINE MEMORY DOMAINS

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The SVP driver is busy.
NSUP The function is not supported.
CC=1 The DIAGNOSE instruction was completed with condition code 1.
CC=2 The DIAGNOSE instruction was completed with condition code 2.
CC=3 The DIAGNOSE instruction was completed with condition code 3.

## HSV0070

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0070 ERROR DURING THE SVP FUNCTION DIAGNOSE WRITE VM DATA

### Meaning

During the function an error was reported by the SVP.
The returncode has the following meaning:
BUSY The SVP driver is busy.
NSUP The function is not supported.
CC=1 The DIAGNOSE instruction was completed with condition code 1.
CC=2 The DIAGNOSE instruction was completed with condition code 2.
CC=3 The DIAGNOSE instruction was completed with condition code 3.

## HSV0999

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HSV0999 FUNCTION NO LONGER SUPPORTED BY SVP.

### Meaning

The called function is no longer supported by the SVP.

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages