## SROCOPY

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SROCOPY COPYRIGHT (C) '(&00)' '(&01)' ALL RIGHTS RESERVED.

## SROLOAD

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SROLOAD PROGRAM '(&00)',VERSION '(&01)' OF '(&02)' LOADED.

## SRO0001

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0001 SUBSYSTEM 'RSO' CANNOT BE INITIALIZED

### Meaning

Possible reasons:
- error during creation of the bourse
- error during a current error recovery function
- error during the initialization of the SRAM tables
- error during the processing of the EQUISAM file.

### Response

Contact the system support to solve the problem
and try to initialize RSO again.

## SRO0002

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0002 RSO DEVICE STARTUP INITIATED

### Meaning

The file $SYSSPOOL.RSO.START.DEVICES exists and all /START-PRINTER-OUTPUT
commands in this file will be processed immediately.

## SRO0003

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0003 DMS ERROR '(&00)' WHEN OPENING FILE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

The file (&01) cannot be opened due to the DMS error (&00).
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Contact the system support to solve the problem
and try to initialize RSO again.

## SRO0004

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0004 GETKY ERROR ON THE '(&01)' FILE. DMS ERROR CODE '(&00)'. ERROR INFO IN SYSTEM MODE: /HELP DMS(&00)

### Meaning

Some records cannot be read from the file (&01) due to the DMS
error (&00).
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Contact the system support to solve the problem
and try to initialize RSO again.

## SRO0005

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0005 DISCREPANCY BETWEEN THE NUMBER OF PRINTERS SUPPORTABLE IN A SESSION AND THE NUMBER OF PRINTERS DECLARED IN THE SPOOL.PARAMETERS FILE

### Meaning

The number of printers declared in the SPOOL.PARAMETERS
file is too large for the generated system. The number of
printers which can be supported in the session is assumed.

### Response

Contact the system support to correct the device limit for the next
session using the controller in the SPOOL.PARAMETERS file in
accordance with the table in the RSO manual.

## SRO0006

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0006 INVALID NEW PARAMETER VALUE. CONTACT THE SYSTEM SUPPORT STAFF TO MIGRATE THE SPOOL.PARAMETERS FILE AND TO INITIALIZE RSO AGAIN

### Meaning

The present SPOOL.PARAMETERS file cannot be used with the
subsystem RSO V2.2.

### Response

Contact the system support to migrate the SPOOL.PARAMETERS file
using an SPSERVE run and try to initialize RSO again.

## SRO0007

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0007 CONTROLLER UPPER LIMIT REACHED. CONTACT THE SYSTEM SUPPORT

### Meaning

The upper limit for the controller as defined in the SPOOL.PARAMETERS file
by the system support has been reached for this RSO session.

### Response

Contact the system support :
- adjust the limit for the controller with regard to the defined network
for the following RSO session.
- release some unused devices by means of the /STOP-PRINTER-OUTPUT
command.

## SRO0008

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0008 INCONSISTENCY IN RSO TABLE

### Meaning

A discrepancy occurred in the RSO table:
- the RSO global table already contained the maximum permitted number of
entries when a new controller was initialized.
- no T3DTBL address in the RSO device table.

### Response

Contact the system support.

## SRO0009

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0009 CONTROLLER INITIALIZATION ERROR '(&00)'. INITIALIZATION ABORTED

### Meaning

Initialization of a new controller was aborted due to a DSSM problem.
(&00): return code.

### Response

Contact the system support.

## SRO0010

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0010 '(&00)': COMMAND REJECTED FOR DEVICE '(&01)'

### Meaning

Possible causes:
- the controller of the device is not initialized.
- SHUTDOWN being processed.
(&00): cause of the command being rejected
(&01): device name.

### Response

If the controller was not initialized, contact the system support.

## SRO0011

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SRO0011 SYSPAR.SYSTEM version '(&00)' not compatible with loaded RSO version '(&01)'. RSO aborted.

### Response

Use the correct SYSPAR.SYSTEM version.

## SRO0012

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SRO0012 IMON LOGICAL-ID '(&00)' UNKNOWN. '(&01)'

### Meaning

The logical-id (&00) not present in the SYSSII file .

### Response

Contact the system support.

## SRO0013

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0013 INTERNAL ERROR. NEW CONTROLLER INITIALIZATION ABORTED

### Meaning

Possible error cause:
- no memory available.
- error during the initialization of the SRAM task.

### Response

Contact the system support.

## SRO0014

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0014 WRONG INTERNAL TABLE INITIALIZED

### Meaning

Discrepancy between the fields of T3DTBL.

### Response

Contact the system support.

## SRO0015

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0015 DEVICE '(&00)' NOT ALLOCATED TO RSO. COMMAND REJECTED

## SRO0016

Destination: CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0016 ERROR IN '(&00)' FILE. USE THE COPY? REPLY (Y=YES; N=NO)

### Meaning

One of the following errors explained by a previous message has occurred:
- DMS error on file (&00)
- inconsistency in the file (&00) due to problems during a merge
processing.

### Response

Y: the copy of file (&00) is used
N: the loading of the RSO subsystem will be ended.

## SRO0017

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0017 FILE '(&00)' AND COPY '(&01)' CANNOT BE USED. RSO SESSION NOT POSSIBLE

### Meaning

The (&00) and (&01) files are inconsistent.

### Response

Restore a correct (&00) file and reload RSO subsystem.

## SRO0018

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0018 SPOOL BEING UNLOADED OR NOT LOADED. RSO INITIALIZATION ABORTED

### Meaning

The SPOOL subsystem is being unloaded or not loaded. No RSO subsystem may
be initialized without SPOOL. Command processing aborted.

### Response

Wait for SPOOL to be initialized and then reenter the command.

## SRO0019

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0019 '(&00)' FILE CANNOT BE UPDATED. RSO STARTUP CONTINUES

### Meaning

The original file is correctly being processed but an error occurred
during the update of its copy.

### Response

The system support must update the file (&00) from
the original file by means of the /COPY-FILE
command.

## SRO0020

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0020 TSN '(&00)' NOT FOUND. RECOVERY ABORTED

### Meaning

The driver of a controller has been terminated abnormally.
During recovery processing no trace was found in the RSO table for the
specified TSN.

### Response

Contact the system support.

## SRO0021

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0021 DMS ERROR '(&00)' WHILE OPENING '(&01)' FILE. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

An error has occurred during the attempt to open the file (&01)
in read mode.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Contact the system support.

## SRO0022

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0022 '(&00)' RECORD IS MISSING OR INVALID IN '(&01)' FILE

### Meaning

An invalid record has been detected or the expected record is missing.
(&00): type of record which is invalid or missing.

### Response

Check the contents of the file.

## SRO0023

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0023 INVALID '(&00)' RECORD IN '(&01)' FILE

### Meaning

The content of the received record is invalid.
Possible causes:
- A counter may contain the value zero.
- Zero is entered for the memory pool size.
- Some information is missing in the record.
(&00): type of record which is missing.

### Response

Check the contents of the file.

## SRO0024

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0024 DMS ERROR '(&00)' WHILE CLOSING '(&01)' FILE. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

An error has occurred during the attempt to close the (&01) file.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Contact the system support.

## SRO0025

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0025 RETURN CODE '(&00)' DURING '(&01)' MACRO PROCESSING FOR THE '(&02)'

### Meaning

(&00): return code
(&01): macro name
(&02): memory pool name.

## SRO0026

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0026 DMS ERROR '(&00)' ON INPUT FILE. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

An error has occurred during the processing.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## SRO0027

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0027 ENABLE ERROR '(&00)' DURING SRAM LOADING. LOADING ABORTED

### Meaning

An error has occurred when accessing the SRAM memory pool.
The SRAM memory pool contains various tables.

### Response

Contact the system support.

## SRO0028

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0028 '(&00)' RECORD FOR JOB WITH TSN '(&01)' INVALID OR MISSING IN '(&02)' FILE

### Meaning

An invalid record has been detected or the expected record is missing.
(&00): type of missing record.

### Response

Check the contents of the file.

## SRO0029

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0029 RSO INTERNAL ENVIRONMENT DESTROYED. LOADING ABORTED

### Meaning

While SRAM was being loaded, no controller entry was found in the
internal table.
Possible cause:
The SRAM loading was started without starting up the driver of the
controller.

### Response

Contact the system support.

## SRO0030

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0030 DMS ERROR '(&00)' WHILE PROCESSING MACRO '(&01)' ON FILE '(&02)'. MERGE FUNCTION ABORTED. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

The processing is immediately stopped.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Correct the problem corresponding to the DMS error code and resubmit the
the startup function.

## SRO0031

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0031 'L' OR/AND 'S' RECORDS MISSING IN PREVIOUS CORRECTION. PREVIOUS CORRECTION IGNORED, PROCESSING CONTINUED

### Meaning

A correction of type ADD or UPDATE has been encountered in the correction
file (logical id = SYSPAR.CORR) and the records of type 'L' or/and 'S'
are missing.
The record displayed with this message is the first record read after the
correction in which the error has been detected. It only serves to
localize the erroneous correction.

### Response

After the merge completion, complete the correction and after the deletion
of parameter file(SYSPAR.RSO) (if not done), resubmit the
startup function.

## SRO0032

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0032 INVALID DATA LENGTH. CORRECTION IGNORED, PROCESSING CONTINUED

### Meaning

Possible reasons:
- the length of the data of the records 'S' of the correction file
(logical id = SYSPAR.CORR) is incorrect (not a multiple of 2).
- The total length of the data given in the 'S' records does not
correspond
to the length specified in the 'L' record.
- The total length of the data is greater than the maximum length of the
record.
- the data moved at the given displacement will exceed the maximum length
of the record.

### Response

After the merge completion, complete the correction and after the deletion
of parameter file (SYSPAR.RSO) (if not done), resubmit the
startup function.

## SRO0033

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0033 UNEXPECTED CHARACTER(S) AT POSITION(S) '(&00)'. CORRECTION IGNORED, PROCESSING CONTINUED

### Meaning

Possible reasons:
- a field of the record types 'A', 'D', 'U', 'L' or 'S' contains
(an) unexpected character(s) at the position(s) (&00).
- the first position is different from ' ' or '*'.
- the second character is different from 'A', 'D', 'U', 'L' or 'S'.

### Response

After the merge completion, complete the correction and after the deletion
of parameter file (SYSPAR.RSO) (if not done), resubmit the
startup function.

## SRO0034

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0034 ERROR ENCOUNTERED WHILE PROCESSING CORRECTION ON KEY '(&00)' AT DISTANCE '(&01)' FOR PM# '(&02)/(&03)'. CORRECTION IGNORED, PROCESSING CONTINUED

### Meaning

This message is sent each time an error is encountered during the merge
function in order to identify the concerned correction.
This message is always followed by another message giving the cause of
the error.
(&00): key
(&01): displacement to apply the correction
(&02): problem message number (PM#)
(&03): julian date.

## SRO0035

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0035 PM# AND JULIAN DATE OF KEY DIFFERENT FROM PM# AND JULIAN DATE OF RECORD. CORRECTION IGNORED, PROCESSING CONTINUED

### Meaning

The key contained in the record of correction file (logical id = SYSPAR.
CORR)
is the key of a header record and the problem message number (PM#)
and/or the julian date of this key are(is) different from the one(s)
contained in the data record.

### Response

After the merge completion, complete the correction and after the deletion
of parameter file (SYSPAR.RSO) (if not done), resubmit the
startup function.

## SRO0036

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0036 UNEXPECTED RECORD SEQUENCE. CORRECTION IGNORED, PROCESSING CONTINUED

### Meaning

While processing correction file (logical id = SYSPAR.CORR), a record has
been found out of the correct sequence of the correction which is:
'D' alone, 'A' and 'U' following by one 'L' following by one or more 'S'.

### Response

After the merge completion, complete the correction and after the deletion
of parameter file (SYSPAR.RSO) (if not done), resubmit the
startup function.

## SRO0037

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0037 ERROR IN A PREVIOUS RECORD. RECORD REJECTED

### Meaning

Due to an error encountered in a previous record of the correction file
(logical id = SYSPAR.CORR), the other records concerning this correction
are rejected.

### Response

After the merge completion, complete the correction and after the deletion
of parameter file (SYSPAR.RSO) (if not done), resubmit the
startup function.

## SRO0038

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0038 FIELD '(&00)' IS NOT AN HEXADECIMAL REPRESENTATION. CORRECTION IGNORED, PROCESSING CONTINUED

### Meaning

While processing a record of correction file (logical id = SYSPAR.CORR),
a field has not the expected hexadecimal representation.

### Response

After the merge completion, complete the correction and after the deletion
of parameter file (SYSPAR.RSO) (if not done), resubmit the
startup function.

## SRO0039

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0039 DUPLICATE CORRECTION. CORRECTION IGNORED, PROCESSING CONTINUED

### Meaning

While processing the records of correction file (logical id = SYSPAR.
CORR),
a correction has been found for the same key and the same displacement.
A duplicate key is only accepted for two records 'U' when one record
inserts code and the other suppresses code.

### Response

After this merge completion, complete the correction and after the
deletion
of parameter file (SYSPAR.RSO) (if not done), resubmit the
startup function.

## SRO0040

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0040 'ADD' ASKED AND RECORD ALREADY EXISTS. CORRECTION IGNORED, PROCESSING CONTINUED

### Meaning

A correction of type 'A' has been introduced and the record already
exists in parameter file (logical id = SYSPAR.SYSTEM).

### Response

After this merge completion, complete the correction and after the
deletion
of parameter file (SYSPAR.RSO) (if not done), resubmit the
startup function.

## SRO0041

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0041 CORRECTION OVERLAPPING. CORRECTION IGNORED, PROCESSING CONTINUED

### Meaning

An overlapping problem has been encountered while inserting the correction
from correction file (logical id = SYSPAR.CORR).
The first correction is applied.

### Response

After this merge completion, complete the correction and after the
deletion
of parameter file (SYSPAR.RSO) (if not done), resubmit the
startup function.

## SRO0042

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0042 CORRECTION OUT OF RECORD LIMITS. CORRECTION IGNORED, PROCESSING CONTINUED

### Meaning

The displacement given in the correction is out of the limits of the
record of parameter file (logical id = SYSPAR.SYSTEM).

### Response

After this merge completion, complete the correction and after the
deletion
of parameter file (SYSPAR.RSO) (if not done), resubmit the
startup function.

## SRO0043

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0043 UPDATE OR DELETE ASKED AND RECORD NOT FOUND. CORRECTION IGNORED, PROCESSING CONTINUED

### Meaning

A correction of type 'U' or 'D' has been introduced and the record
does not exist in parameter file (logical id = SYSPAR.SYSTEM).

### Response

After this merge completion, complete the correction and after the
deletion
of parameter file (SYSPAR.RSO) (if not done), resubmit the
startup function.

## SRO0044

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0044 MERGE FUNCTION STARTED FOR FILE '(&00)'

### Meaning

This message is sent when the merge function is started.

## SRO0045

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0045 MERGE FUNCTION TERMINATED WITHOUT ERROR

## SRO0046

Destination: USER-TASK, CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0046 MERGE FUNCTION TERMINATED WITH ERROR(S). CONTINUE PROCESSING? REPLY (Y=CONTINUE; N=TERMINATE)

### Meaning

This message is sent when the merge function is terminated and
some corrections have been rejected.

### Response

Y: the processing continues but errors can occur due to an incoherent
status of the data.
N: the startup is terminated with error(s) and parameter file
(SYSPAR.RSO) is erased.

## SRO0047

Destination: USER-TASK, CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0047 FILE '(&00)' CAN BE INCONSISTENT. REGENERATE FILE? REPLY (Y=YES; N=TERMINATE PROCESSING)

### Meaning

The merge function in a previous startup has been terminated abnormally.

### Response

Y: parameter file (SYSPAR.RSO) is erased and the merge
function is started.
N: the processing is immediately terminated.

## SRO0048

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0048 INVALID DATA LENGTH IN THE PREVIOUS CORRECTION. PREVIOUS CORRECTION IGNORED, PROCESSING CONTINUED

### Meaning

The data given in the records 'S' of correction file
(logical id = SYSPAR.CORR) has a length different from the
length specified in the record 'L'.
The record displayed with this message is the first record read after the
correction in which the error has been detected. It only serves to
localize the erroneous correction.

### Response

After this merge completion, complete the correction and after the
deletion
of parameter file (SYSPAR.RSO) (if not done), resubmit the
startup function.

## SRO0049

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0049 FILE '(&00)' NOT A RSO PARAMETER FILE. NO MERGE FUNCTION REALIZED

### Meaning

The first record of parameter file (logical id = SYSPAR.SYSTEM) is
not the first global record.

### Response

After this merge completion, use the correct parameter file
(logical id = SYSPAR.SYSTEM) and resubmit the startup function.

## SRO0050

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0050 WRONG RECORD TYPE USED. CORRECTION IGNORED, PROCESSING CONTINUED

### Meaning

In correction file (logical id = SYSPAR.CORR), a wrong correction is
given for a header record. The first header record can only be updated
and the other header records can only be added.

### Response

After this merge completion, complete the correction and after the
deletion
of parameter file (SYSPAR.RSO) (if not done), resubmit the
startup function.

## SRO0051

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0051 'L' OR 'S' RECORDS MISSING IN CURRENT CORRECTION. CORRECTION IGNORED, PROCESSING CONTINUED

### Meaning

A correction of type ADD or UPDATE has been encountered in the
correction file (logical id = SYSPAR.CORR) and the records
of type 'L' or/and 'S' are missing.
The displayed record is this of which the records are missing.

### Response

After this merge completion, complete the correction and after the
deletion
of parameter file (SYSPAR.RSO) (if not done), resubmit the
startup function.

## SRO0052

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0052 NO MORE CLASS 4 MEMORY

### Meaning

The task waits until the system has released the class 4 memory.

## SRO0053

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0053 FILE '(&00)' DOES NOT EXIST. PROCESSING CONTINUES

### Meaning

As the correction file (logical id = SYSPAR.CORR) does not exist,
the parameter file with logical id SYSPAR.SYSTEM
becomes parameter file (SYSPAR.RSO).

## SRO0054

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SRO0054 Unexpected check byte(s) or EOR check. Correction ignored, processing continues.

### Meaning

While processing correction file (logical id = SYSPAR.CORR), a record
has been found with a wrong check byte(s) or EOR check.

### Response

After the merge completion, complete the correction and after the
deletion of parameter file (SYSPAR.RSO) (if not done), resubmit the
startup function.

## SRO0055

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0055 RSO SUBSYSTEM CANNOT BE STOPPED OR HELD FOR REASON '(&00)'. COMMAND ABORTED

### Meaning

(&00): reason:
01: RSO subsystem is not running.
02: RSO administration task cannot be performed.

### Response

Reason 02: try again to stop or held the RSO subsystem.
If this attempt also fails, take system dump.

## SRO0056

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SRO0056 DMS error '(&00)' during processing 'GET','FILE' or 'OPEN' macro for file '(&01)'. Startup aborted. In system mode: /HELP-MSG DMS(&00).

### Meaning

For more detailed information about the DMS error code enter
/HELP-MSG in system mode or see the BS2000 manual 'System Messages'.

### Response

Try to correct the DMS error and retry the startup.

## SRO0057

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SRO0057 Invalid specification in the '(&00)' parameter file. RSO subsystem startup aborted.

### Meaning

The (&00) file doesn't exist or
a wrong information has been introduced in the file.

### Response

Correct or restore the (&00) file and retry the startup.

## SRO0058

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SRO0058 Monitoring job variable error '(&01)' for device '(&00)'. Processing continues.

### Meaning

(&00): device name concerned by the monitoring job variable.
(&01): return code of the called interface composed as follows : XXYYZZZZ
XX : no meaning.
YY : subcode1 : X'01' : CATJV error.
X'02' : job variable doesn't exist.
X'04' : invalid password.
X'06' : invalid parameter list.
X'08' : STAJV error.
X'10' : SETJV error.
X'20' : GETJV error.
X'22' : ERAJV error.
X'24' : MONJV error.
X'25' : GETMEM error.
X'40' : incoherent job variable.
X'41' : parameter error.
X'80' : job variable service not available.
ZZZZ : main return code from the job variable service.
For more information see the BS2000 manual 'Job Variables'.

## SRO0059

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SRO0059 Warning : the key "XS" + access type '(&00)' (hexadecimal '(&01)') was not found in the RSO "CHK" record. Processing continues.

### Meaning

AS the RSO "CHK" record of the SYSPAR.RSO parameter file doesn't
contain the access type associated to the device type of the device
specified at the /START-PRINTER-OUTPUT command, it's not possible to
check the compatibility between the device and access type.

### Response

Correct the RSO "CHK" record of the SYSPAR.RSO parameter file
and restart the device.

## SRO0060

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SRO0060 Incompatibility between access type and printer type used for device '(&00)' during /START-PRINTER-OUTPUT command validation. Command rejected.

### Meaning

The specified access type is not supported by the printer type of the
specified device.

### Response

Correct the device definition in the SPOOL.PARAMETERS file and
restart the device.

## SRO0061

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SRO0061 The '(&00)' pathname is '(&01)'.

### Meaning

This message display the IMON static table that will be used by RSO
for the current session.
(&00): logical id.
(&01): current IMON pathname.

### Response

In case of issuing a new set-imon-path, the RSO sub-system must be
stopped and restarted in order to take the change into account.

## SRO0062

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SRO0062 Error '(&00)' for header / trailer customised page. Template file name : '(&01)'

### Meaning

(&00) : error code
00010001: wrong FCB type
00010002: unknown function
00010003: syntax error
00010004: IF misplacement
00010005: GTIME error
00010006: PBBIND error
00010007: BARCODE error
00010008: memory error
00010009: big letter error
0001000A: DMS error
0001000B: internal error
0001000C: FONT error
(&01) : filename

### Response

None

## SRO0100

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0100 TSN '(&01)': EXIT ROUTINE '(&00)' DOES NOT EXIST

## SRO0101

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0101 TSN '(&01)': EXIT ROUTINE '(&00)' NOT ACTIVE. JOB SUSPENDED

### Meaning

The SPOOL job is interrupted and will be restarted with TYPE=S.
(&00): EX090 or EX095.

## SRO0102

Destination: CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0102 TSN '(&01)': EXIT ROUTINE '(&00)' NOT ACTIVE. REPLY (R=RETRY (PREVIOUSLY THE EXIT ROUTINE MUST BE ACTIVATED); T=ABORT)

### Meaning

The operator has to activate the exit routine if the SPOOL job is desired.

### Response

R: start the job again with an active exit routine.
T: the exit routine will not be called; the SPOOL job is aborted.

## SRO0103

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0103 RSO RECEIVED UNKNOWN ERROR CODE '(&00)', TSN '(&01)'. JOB ENTERED IN KEEP QUEUE

### Meaning

RSO received an error code from SRAM which is not contained in its
internal tables.

### Response

Contact the system support to check the validity of the
parameter file (SYSPAR.RSO).

## SRO0104

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0104 (&00) DUPLICATE PAGE(S) POSSIBLE DUE TO SPOOLOUT INTERRUPTION(S)

### Meaning

During the spoolout of the job, RSO was interrupted at least one time.
The interruption was caused by specific hardware errors (end of paper,
printer stopped, ...) for which a special processing is implemented.
This processing may result in some pages being printed more than once.
(&00): number of the RSO interrupts.

### Response

Check the contents of the output which may contain
duplicate pages in (&00) different places.

## SRO0105

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0105 'SETL' ERROR ON FILE '(&00)'

### Meaning

Possible reasons:
- The positioning value specified for file (&00) destined for the device
is invalid or
- in a PLAM element all record types are > 159.
In the latter case the job cannot be printed by the RSO subsystem.

### Response

Correct the specified value via the /RESUME-PRINT-JOB command.

## SRO0106

Destination: USER-TASK, CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0106 TSN '(&01)': RESTART PAGE NUMBER '(&00)' GREATER THAN FILE CAPACITY. REPLY (T=ABORT; <NN>=NEW PAGE NUMBER)

### Meaning

The given restart page number is too high.

## SRO0107

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0107 SPOOLOUT INTERRUPTED. OUTPUT INCOMPLETE

### Meaning

The spoolout job has been interrupted by a /HOLD-PRINT-JOB command
and has been restarted.

## SRO0108

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0108 SPOOLOUT SUSPENDED

### Meaning

The spoolout job is temporarily suspended, i.e. it is put back into the
spoolout queue.

### Response

Subsequent messages will ask for a new priority and for the type
of restart for the suspended job.

## SRO0109

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0109 SPOOLOUT KEPT

### Meaning

The spoolout job is placed in the KEEP queue until it is restarted by
means of the /RESUME-PRINT-JOB command.

### Response

A subsequent message will ask for the type of restart.

## SRO0110

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0110 SPOOLOUT CANCELED BY MEANS OF /CANCEL-PRINT-JOB

## SRO0111

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0111 LINE TRUNCATION IN RECORD NUMBER (&00). PRINTOUT CONTINUES

## SRO0112

Destination: CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0112 TSN '(&01)', DEVICE '(&00)': ERROR DURING SPOOLOUT. REPLY (T=ABORT; D=DEFER; S=STANDARD; K=KEEP WITHOUT AUTOMATIC RESTART)

### Response

T: the spoolout job will be removed from the spoolout queue
and the file will be erased if requested.
D: the spoolout job will be returned to the spoolout queue.
Subsequent messages will query the new priority and the restart
type for the deferred job.
S: the spoolout job will be returned to the spoolout queue without
its priority being modified. The job will be restarted from
the previous checkpoint.
K: the spoolout job will be added to the KEEP queue until it is restarted
by means of a /RESUME-PRINT-JOB command.
A subsequent message will query the restart type.

## SRO0113

Destination: CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0113 TSN '(&00)', DEVICE '(&01)': NEW PRIORITY OF DEFERRED JOB DESIRED? REPLY (<NNN>=NEW PRIORITY 30 THROUGH 255; 'ETX'=NO CHANGE)

## SRO0114

Destination: CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0114 TSN '(&00)', DEVICE '(&01)': SPECIFY RESTART TYPE FOR DEFERRED JOB. REPLY (B=BEGINNING; P=PREVIOUS CHECKPOINT; S=START OF PAGE; <NN>= DECIMAL PAGE NUMBER)

### Meaning

The user is requested to specify where to restart the job that was
deferred on device (&01).

### Response

B: the job will be restarted from the very beginning.
P: the job will be restarted from the previous checkpoint.
S: not valid for card punches; the job will be restarted
from the beginning of the page currently being printed.
<NN>: not valid for card punches; decimal value specifying the
page number from which the job is to be restarted.
(must be lower than the current page number).

## SRO0115

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0115 TSN '(&00)', DEVICE '(&01)': ERROR DURING SPOOLOUT. JOB ADDED TO KEEP QUEUE

### Meaning

The job is placed in the KEEP queue with the last checkpoint value.

### Response

The spoolout job can be restarted by means of a /RESUME-PRINT-JOB command.

## SRO0116

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0116 TSN '(&01)', DEVICE '(&00)': JOB IS RESTARTED WITH 'TYPE=BEGINNING'

## SRO0117

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0117 CONNECTION FOR DEVICE '(&00)' NOT ALLOWED. DEVICE DETACHED

### Response

Request the system support to check the validation of
the SPOOL.PARAMETERS file.

## SRO0118

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0118 SPOOLOUT ENDED

### Meaning

- The file has been completely printed.
- The print request has been removed from the queue.
- The file is erased subsequent to the spoolout if requested by the user.

## SRO0119

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0119 TSN '(&02)', DEVICE '(&01)': LINE TRUNCATION FOR FILE '(&00)'

### Meaning

One or more lines of file (&00) printed on device (&01) have been
truncated.

## SRO0120

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0120 '(&00)': '(&01)' IN RECORD '(&02)'

### Meaning

(&00): WRONG SPACING CTRL BYTE: print control character error
WRONG CHANNEL VALUE : channel number skip greater than 12 or
channel number not defined in the loop
(&01): value of the invalid information
(&02): record number in the input file.

## SRO0121

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0121 USER ERROR: RECORD LENGTH GREATER THAN DCAM BUFFER SIZE

### Response

Redefine the DCAM buffer size via SPSERVE
(MODIFY-SPOOL-DEVICE) or
change the file record length definition.

## SRO0122

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0122 USER ERROR: PRINTER RECEIVED UNEXPECTED CLOSE DOCUMENT(S)

### Meaning

User data may contain unexpected close documents (\ ] ;).

### Response

Check the file.

## SRO0123

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0123 USER ERROR: INVALID CSI '(&00)'

### Meaning

Due to an invalid CSI (character set identifier) the job is terminated.

### Response

Modify the input file and start the job again.

## SRO0124

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0124 DMS ERROR CODE '(&00)' FOR FILE '(&01)'. THE CHARACTER-IMAGE '(&03)' FOR DEVICE '(&02)' CANNOT BE READ. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

An error occurs during the read of the CHARACTER-IMAGE (&03) when the
/START-PRINTER-OUTPUT command is processed for the device (&02).
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Correct the DMS error and repeat the command.

## SRO0125

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0125 FILE TO BE PRINTED IS EMPTY

## SRO0126

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0126 SPOOLOUT JOB SUSPENDED IN KEEP QUEUE. DEVICE DETACHED

### Meaning

The spoolout job has been kept because the device where the job was
active, has been detached by the operator or the RSO device administration
by means of the /STOP-PRINTER-OUTPUT command with operand STOP=IMMEDIATE.

## SRO0127

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0127 TSN '(&01)': 'SETL' ERROR ON FILE '(&00)'

### Meaning

The specified positioning value for the file (&00) is invalid.

### Response

Correct the specified value by means of the /RESUME-PRINT-JOB command.

## SRO0128

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0128 DMS ERROR CODE '(&00)' FOR FILE '(&01)', TSN '(&02)'. IN SYSTEM MODE /HELP-MSG DMS(&00)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Correct the DMS error and release the job by means of the
/RESUME-PRINT-JOB
command (exception: DMS error DMS0D33: file not cataloged).

## SRO0129

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0129 TSN '(&01)': INVALID CHANNEL 1 POSITION IN 'LOOP' OPERAND '(&00)'

### Meaning

There is not enough space left between the channel 1 position (first line
of the printout and the end of the printer page to enable printing with
the
specified PRINT operand.
(&00): - LOOP name
- SPACING if '*SPACING' was specified for the vertical control or
rotation control value in the SPOOL.PARAMETERS file for
the form used.

### Response

User loop: correct the channel 1 position.
In all other cases, contact the system support to have the
correction made.

## SRO0130

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0130 TSN '(&02)', DEVICE '(&00)': RECORDING DENSITY ERROR USING FORM OPERAND '(&01)'. JOB SUSPENDED

### Meaning

The recording density specified in the FORM operand is invalid.
The spoolout job is placed in the KEEP queue.

### Response

Correct the form definition in the SPOOL.PARAMETERS file and
release the spoolout job by means of a /RESUME-PRINT-JOB command.

## SRO0131

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0131 TSN '(&01)': FILE NOT FOUND FOR DIA '(&00)'

### Meaning

The DIA (forms overlay) file is not defined with the standard file name
either under the PRINT user ID or under the device administration user ID
or in the device itself.

### Response

The DIA must be defined by the user or by the device administration.

## SRO0132

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0132 INCONSISTENCY BETWEEN OPERAND 'LEFT-MARGIN' AND PAPER FORMAT OR RECORDING DENSITY

### Meaning

The value of the LEFT-MARGIN operand in the PRINT-FILE/PRINT-DOC command
or the corresponding default value defined in the SPOOL.PARAMETERS
file is too large.

### Response

Contact the system support to correct the paper format or
recording density before releasing the TSN.

## SRO0133

Destination: CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0133 TSN '(&01)', DEVICE '(&00)': SAMPLE PRINTOUT REQUIRED FOR SPOOLOUT-NAME '(&02)'? REPLY (Y=YES; N=NO; <N>=NUMBER OF PAGES 1 THROUGH 9)

### Meaning

The operand PRINT-SAMPLE was specified in a previous /START-PRINTER-OUTPUT
command. The operator is therefore asked every time the form is changed
whether a sample printout is desired for this form.

### Response

Y : sample printout of one page required
N : no sample printout required
<N>: sample printout of n pages required (n = 1 to 9).

## SRO0134

Destination: CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0134 TSN '(&01)': SAMPLE PRINTOUT FOR '(&00)' CORRECT? REPLY (Y=YES; N=NO)

### Meaning

The sample printout for form (&00) has been printed. The result should be
checked for errors.

### Response

Y: the form alignment is correct; regular spoolout will begin.
N: the form alignment must be corrected before entering the reply.
The sample printout is repeated.

## SRO0135

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0135 INVALID VALUE SPECIFIED IN 'FIRST-RECORD' OPERAND. NO OUTPUT

### Meaning

The values specified in the FIRST-RECORD operand of the PRINT-FILE/
PRINT-DOC command are not contained in the file to be printed.

## SRO0136

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0136 JVS ERROR '(&00)' DURING JV PROCESSING. IN SYSTEM MODE: /HELP-MSG JVS(&00)

### Meaning

For more detailed information about the JVS error code, enter /HELP-MSG
in system mode or see BS2000 manual 'System Messages'.
JV: job variable
(&00): JVS error code.

## SRO0137

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0137 WRONG POSITION OF THE CONTROL CHARACTER

### Meaning

The position of the control character is outside of the record.

## SRO0138

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0138 BEGINNING OF THE SECTION TO BE PRINTED NOT FOUND

### Meaning

The record corresponding to the FIRST-RECORD operand of the SECTION
cannot be found in the file.

### Response

Correct the PRINT-FILE/PRINT-DOC command and try again or modify the file.

## SRO0139

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0139 VFB LENGTH DEFINED IN OPERAND '(&00)' IS NOT SUPPORTED ON THE DEVICE. COMMAND REJECTED

### Meaning

The length of the vertical format buffer (VFB) used in the operand (&00)
is greater than the maximum physical page size supported by the device.

### Response

Correct the concerned operand and start the job again.

## SRO0140

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0140 FAMILY LOCK ERROR. COMMAND NOT PROCESSED FOR TSN '(&00)'

### Meaning

During the redirection of one family, an internal error occurred.
The system cannot lock this family to avoid other actions (delete job,
change priority etc.).

## SRO0141

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0141 DMS ERROR WHILE PRINTING A 'PRE-DATA' OR 'POST-DATA' FILE

### Meaning

More detailed information about the DMS error (DMS error code and file
name) are given on the trailer page of the print job.

## SRO0142

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0142 USER ERROR: INVALID CPI IN CHARACTER SET '(&00)'. CORRECT SPOOL.PARAMETERS FILE

### Meaning

In the SPOOL.PARAMETERS file the character density defined in the
character set (&00) for the form is not allowed for the device type
of the printer.
CPI: character per inch = print density.

### Response

Correct the character set record in the SPOOL.PARAMETERS file and
start the job again.

## SRO0143

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0143 USER ERROR: INVALID CPI IN CSI '(&00)'

### Meaning

The character density (CPI) defined in the character set via the
CSI (&00) is invalid for the device type associated with the printer.
CPI: character per inch = print density.
CSI: Character Set Identifier.

### Response

Correct the character set record in the SPOOL.PARAMETERS file and
start the job again.

## SRO0144

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0144 FILE NOT FOUND OR PROTECTED FOR DIA '(&00)'

### Meaning

The DIA file (FORMS-OVERLAY) is not defined with the standard file name
or is protected.
The file can exist on three possible locations:
- on the user ID that issues the print.
- on the user ID of the RSO device administration (private device)
or on the user ID $SYSSPOOL (public device).
- in the memory of the device.

## SRO0145

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0145 INVALID VERTICAL DENSITY USED FOR DEVICE '(&00)'. COMMAND REJECTED. CORRECT SPOOL.PARAMETERS FILE

### Meaning

Possible reasons:
- invalid LPI value in the character set, which is specified in the
LOOP-NAME operand of the PRINT-FILE/PRINT-DOC command.
- invalid LPI value in the LOOP record, which is attached to the form.
- invalid LPI value specified in the vertical spacing of the form.
LPI: Lines Per Inch.

### Response

Correct the form definition in the SPOOL.PARAMETERS file and start the job
again.

## SRO0146

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SRO0146 INVALID CPI IN CHARACTER SET '(&00)' FOR DEVICE '(&01)'. COMMAND REJECTED

### Meaning

Possible reasons:
- invalid CPI value in the character set, which is specified in the
operand CHARACTER-SETS of the PRINT-FILE/PRINT-DOC command.
- invalid CPI value in the character set, which is attached to the form.
CPI: character per inch.

### Response

Correct the character set record in the SPOOL.PARAMETERS file and start
the job again.

## SRO0147

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0147 TSN '(&01)': VFB LENGTH DEFINED IN OPERAND '(&00)' EXCEEDS THE MAXIMUM PHYSICAL PAGE SIZE SUPPORTED BY THE DEVICE

### Meaning

VFB: vertical format buffer.

### Response

Correct operand and run job again.

## SRO0148

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0148 MAXIMUM VALUE FOR REPEAT-MESSAGE RETRY TIME REACHED. JOB SUSPENDED

### Meaning

The value specified in the device record of the SPOOL.PARAMETERS file is
reached.

## SRO0149

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0149 MAXIMUM VALUE FOR RESTART-ACTION RETRY TIME REACHED. JOB SUSPENDED

### Meaning

The value specified in the device record of the SPOOL.PARAMETERS file is
reached.

## SRO0150

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SRO0150 REMOTE FILE ACCESS NOT SUPPORTED BY RSO. FILES OR CAT ID '(&00)' NOT ACCESSIBLE. COMMAND REJECTED

### Meaning

(&00): cat ID or file name.

## SRO0151

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0151 TSN '(&00)': SUBSYSTEM '(&02)' NOT LOADED WHEN PROCESSING FILE '(&01)'. JOB SUSPENDED

### Meaning

DSEM: Dynamic Spool Extension Management
XHCS: Extended Host Code Support.

## SRO0152

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0152 TSN '(&00)': SUBSYSTEM 'XHCS' NOT DEFINED IN DSSM CATALOG WHEN PROCESSING FILE '(&01)'. JOB SUSPENDED

### Meaning

XHCS: Extended Host Code Support.

## SRO0153

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0153 TSN '(&00)': CCSN '(&02)' UNKNOWN TO XHCS WHEN PROCESSING FILE '(&01)'. JOB SUSPENDED

### Meaning

CCSN: Coded Character Set Name
XHCS: Extended Host Code Support.

## SRO0154

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0154 TSN '(&00)': XHCS ERROR '(&02)' WHEN PROCESSING FILE '(&01)'. JOB SUSPENDED

### Meaning

For more detailed information about the error code, see the BS2000
manual 'XHCS'.
XHCS: Extended Host Code Support.

### Response

Contact the system support.

## SRO0155

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0155 Warning: at least one character contained in '(&00)' file has no equivalence XHCS unicode table.

### Meaning

(&00) : USER, PROLOG, EPILOG oder DIA
At least one character could not be converted. The XHCS default
character has been used.

## SRO0156

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0156 WARNING: NO CONVERSION APPLIED ON '(&00)' FILE

### Meaning

(&00): USER, PROLOG, EPILOG or DIA
- A coded character set name (CCSNAME) is attached to the file and a
translation table has been specified in the PRINT-FILE/PRINT-DOC command
or
- the CCSNAME attached to the file has been assumed of type EBCDIC
because of the non availability of XHCS

## SRO0157

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0157 INCONSISTENCY IN RECOVERY FILE '(&00)' FOR DEVICE '(&01)'. PROCESSING CONTINUES WITH DEFAULT RECOVERY RULES

### Meaning

One of the following errors has been detected when
validating the recovery rules file (&00) for the device (&01) :
1. an invalid "generic" action code has been specified
2. an invalid "generic" printer error code has been specified

### Response

Contact the system support.

## SRO0158

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0158 JOB IN AUTOMATIC RESTART PROCESSING

### Meaning

The job will retry the open connection after an interval time
specified in the SPOOL.PARAMETERS file.

## SRO0159

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0159 DMS ERROR '(&00)' IN RECOVERY FILE '(&01)' FOR DEVICE '(&02)'. PROCESSING CONTINUES WITH DEFAULT RECOVERY FILE

### Meaning

For more detailed information about the DMS error code enter
/HELP-MSG DMS(&00) in system mode or see the BS2000 manual
'System Messages'.
(&00): specific error code
(&01): file name

## SRO0160

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0160 ACCESS TO S1/S2 STORAGE LEVEL. PLEASE WAIT.

### Meaning

The current file has been migrated to the S1 or S2 storage level.
The recall of the migrated data may take some time.
Please wait.

## SRO0161

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0161 MIGRATED FILE '(&00)' CANNOT BE RECALLED. COMMAND REJECTED

### Meaning

The file (&00) has been migrated to the S1 or S2 storage level.
The recall issued by the print processing does not succeed.
The spoolout request is rejected for this file.

## SRO0162

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0162 TSN '(&01)': FILE '(&00)' HAS BEEN MIGRATED.

### Meaning

The file (&00) has been migrated and thus is not available.
Recall the file and repeat the spoolout job.

## SRO0163

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0163 FILE FOR '(&00)' HAS BEEN MIGRATED.

### Meaning

The file has been migrated and thus is not available.
Recall the file or contact the device administrator

## SRO0164

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0164 REQUESTED RECOVERY ACTION CODE CANNOT BE CARRIED OUT.

### Meaning

A problem has been detected during printing but its corresponding
recovery action code (e.g. REPEAT) cannot be carried out (e.g. not
possible
to perform the REPEAT action code when a TACLAN-connected printer is
defined with SYNCHRO=NETWORK). The recovery action code defined for
the 'InvalidAction' general error code (STOP by default) is then carried
out.

### Response

Contact the system support or the device administration.

## SRO0165

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0165 SYNTAX ERROR IN LINE'(&00)' DURING ANALYSIS OF CAPABILITY FILE '(&01)' FOR DEVICE '(&02)', REASON '(&03)'.

### Meaning

The capability file contains syntax errors with reason
(01) : wrong control characters (beginning with '\' or '^')
(02) : missing delimiter (',') at end of capability
(03) : unexpected characters after the terminating comma
(04) : missing delimiter ('#') in numeric capability
(05) : missing numeric value
(06) : string length/numeric value too large or invalid printer name
(07) : missing mandatory unit in numeric capability
(08) : unit not supported in numeric capability
(09) : capability defined twice
(10) : missing delimiter ('=') in string capability
(11) : missing capability name or printer name in LikeString
(12) : not supported capability
(13) : missing delimiter ('like:') in LikeString capability
(14) : missing delimiter ('%') in KeyStringList capability
(15) : missing delimiter (':') in KeyStringList capability
Processing continues without taking into account the capability
file content.

## SRO0166

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0166 OUT OF MEMORY DURING PROCESSING OF CAPABILITY FILE '(&00)' FOR DEVICE '(&01)'.

### Meaning

All information contained in the capability file cannot
be stored into memory. Processing continues without
taking into account the capability file content.

## SRO0167

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0167 TSN '(&00)' : INCONSISTENCY BETWEEN INPUT-TRAY VALUE AND PAGE/LINE SIZE VALUE. JOB SUSPENDED.

### Meaning

The INPUT-TRAY value is incorrect in function of the used form.
The value doesn't match the PAGE/LINE SIZE value.

## SRO0168

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SRO0168 Remote predata/postdata file access not supported.

## SRO0169

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SRO0169 Predata/postdata file is empty.

## SRO0170

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0170 User error: No ippuri available for the IPP printer '(&00)'.

### Meaning

(&00) : device name
No ippuri has been defined in the printer parameter file associated
to the selected IPP printer.

### Response

Check and correct the associated printer parameter file.

## SRO0171

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0171 Standard device record in the SPOOL PARAMETERS file mandatory for specified RSO device type. Command/macro rejected.

### Meaning

No standard device record in the SPOOL PARAMETERS file for the
specified RSO device type.

### Response

Add the standard device to the SPOOL.PARAMETERS file by means of
the //ADD-SPOOL-DEVICE statement of SPSERVE.

## SRO0172

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0172 Internal error during system device allocation. Command/macro rejected.

### Meaning

Possible error cause:
- no memory available
- error during the initialisation of the SROSDIP task
- error during the initialisation of the system device

### Response

Contact the system support.

## SRO0173

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0173 INCONSISTENCY BETWEEN OPERANDS IN THE COMMAND. COMMAND REJECTED

### Meaning

Possible reasons:
- incorrect syntax of operands
- combination of operands not permitted.

### Response

Correct the operands and try the command again.

## SRO0174

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0174 SYSTEM INTERFACE ERROR. CONTACT THE SYSTEM SUPPORT STAFF

### Meaning

An error occurred during the command processing.

## SRO0175

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0175 USER NOT AUTHORIZED TO QUERY INFORMATION OR TO ISSUE COMMAND. COMMAND REJECTED

## SRO0176

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0176 LOGICAL VALIDATION PROBLEM DURING COMMAND PROCESSING

### Meaning

Possible cause:
- missing definition in the SPOOL parameters or in the SPOOL files
- DMS error (except system error) occurred
- device not available.

## SRO0177

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0177 REDIRECTION NOT AUTHORIZED FOR AT LEAST ONE TSN

### Meaning

The user is not authorized to redirect the TSN or at least one TSN of
the list which has been specified in the /REDIRECT-PRINT-JOB command.

## SRO0178

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0178 TSN '(&01)': IMON LOGICAL ID '(&00)' UNKNOWN. JOB SUSPENDED.

## SRO0179

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0179 TSN '(&00)': ROTATION VALUE INCORRECT. JOB SUSPENDED.

### Meaning

Rotation has been requested but no rotation loop or rotation
spacing value has been specified.

## SRO0180

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0180 TSN '(&00)': The ccsname '(&02)' is incompatible with the device '(&01)'. Job Suspended.

### Meaning

(&00) : job
(&01) : device name
(&02) : coded character set name
Some resources or the file to be printed are encoded in an
incompatible way with the selected device.

### Response

Use correct resources or redirect the job to a device compatible
with the ccsname.

## SRO0181

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0181 TSN '(&00)': Warning: conversion applied on '(&01)' file.

### Meaning

(&00) : job
(&01) : USER, PROLOG, EPILOG oder DIA
The coded character set name (CCSNAME) attached to the file is
incompatible with the RSO process and a conversion to EDF041 or
UTFE has been applied.

## SRO0182

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0182 Warning: conversion applied on '(&00)' file.

### Meaning

(&00) : USER, PROLOG, EPILOG oder DIA
The coded character set name (CCSNAME) attached to the file is
incompatible with the RSO process and a conversion to EDF041 or
UTFE has been applied.

## SRO0183

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0183 User error: No sutf8/rutf8 available for the printer '(&00)'.

### Meaning

(&00) : device name
No sutf8/rutf8 has been defined in the printer parameter file associated
to the selected printer.

### Response

Check and correct the associated printer parameter file.

## SRO0184

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0184 User error: Invalid escape sequence used for the printer '(&00)'.

### Meaning

(&00) : device name
An invalid escape sequence is used in the file printed
on the selected printer.

### Response

Check and correct the print file.

## SRO0185

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0185 User error: UTFE/UTF8 conversion error during the printing of the file '(&00)'. Job suspended.

### Meaning

(&00) : file name
An UTFE/UTF8 conversion error occurs during the printing of the file
on the selected printer.

### Response

Check and correct the print file.

## SRO0186

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0186 User error: No Escape table defined for this unicode printer '(&00)'.

### Meaning

(&00) : device name
This printer cannot support Unicode feature

### Response

Check and correct the device printer.

## SRO0187

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0187 Predata error: Remote buffer size too small.

### Meaning

The Remote Buffer is too small to contain the Predata record

### Response

Increase the Remote Buffer size in the SPOOL.PARAMETERS file

## SRO0300

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0300 SYSTEM ERROR: RSO ADMINISTRATOR BOURSE DESTROYED. COMMAND NOT PROCESSED

### Meaning

The bourse mechanism has detected an error and was therefore aborted.

## SRO0301

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0301 ERROR WHEN ACCESSING THE SPOOL.PARAMETERS FILE. COMMAND PROCESSING ABORTED

## SRO0302

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0302 ERROR WHEN ACCESSING THE SLOT MANAGER. COMMAND PROCESSING ABORTED

## SRO0303

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0303 SAMPLE FUNCTION NOT ALLOWED FOR PRIVATE DEVICE OR SINGLE-SHEET PRINTER

## SRO0304

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : YES

SRO0304 POOL NAME '(&00)' NOT DEFINED IN THE SPOOL.PARAMETERS FILE. COMMAND REJECTED

### Meaning

In the PRINT-FILE/PRINT-DOC command, the destination name can be either
a device name or a pool name defined in the SPOOL.PARAMETERS file.
In the /START-PRINTER-OUTPUT command, the destination name must
be a pool name defined in the SPOOL.PARAMETERS file.

## SRO0305

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0305 COMMAND IS RESTRICTED TO THE SYSTEM SUPPORT STAFF OR RSO DEVICE ADMINISTRATOR. COMMAND REJECTED

### Meaning

Only the system support or the RSO device administration may issue
the /REDIRECT-PRINT-JOB command or the /STATUS R command without the
DEVICE operand.

## SRO0306

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0306 SYSTEM ERROR: EQUISAMQ FILE CORRUPTED. COMMAND ABORTED

### Meaning

The EQUISAMQ file has been corrupted and one of the
following commands has been aborted.
/RESUME-PRINT-JOB
/REDIRECT-PRINT-JOB.

## SRO0307

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0307 NO MORE CLASS (&00) MEMORY AVAILABLE. COMMAND NOT PROCESSED

### Meaning

An error occurred when trying to request memory.

## SRO0308

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : YES

SRO0308 DMS ERROR '(&00)' DURING RSO ACCESS TO FILE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## SRO0309

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0309 INTERNAL SYSTEM ERROR. RETRY COMMAND

## SRO0310

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0310 INCOHERENCE BETWEEN '(&00)' AND SPOOL.PARAMETERS FILE VERSIONS. COMMAND REJECTED

### Meaning

The SPOOL.PARAMETERS file does not contain enough RSO information to
process the command.

### Response

Contact the system support to migrate the SPOOL.PARAMETERS file
by a run of SPSERVE and retry the RSO creation.

## SRO0311

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0311 WARNING: PRINTS AUTOMATICALLY REDIRECTED TO DEVICE '(&00)'

### Meaning

The RSO or SPOOL jobs are automatically redirected on the specified
device.

## SRO0312

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SRO0312 TSN '(&02): REDIRECTION FROM DEVICE '(&00)' TO DEVICE '(&01)' NOT ACCEPTED. COMMAND NOT PROCESSED

### Meaning

Possible reasons:
- the specified mode of redirection is not supported.
- the redirection is not processed for the specified TSN or for each
remaining TSN ((&02)=*ALL).

## SRO0313

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SRO0313 TSN '(&01)': POOL OR DEVICE NAME '(&00)' NOT DEFINED IN SPOOL.PARAMETERS FILE. COMMAND NOT PROCESSED

### Meaning

The redirection is not processed for the specified TSN or for each
remaining TSN ((&01)=*ALL).

## SRO0314

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SRO0314 USER NOT AUTHORIZED TO REDIRECT TSN '(&00)'. COMMAND NOT PROCESSED

### Meaning

The redirection is not processed for the specified TSN or for each
remaining TSN ((&00)=*ALL).

## SRO0315

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0315 TSN '(&00)': ERROR DURING EQUISAMQ FILE ACCESS. COMMAND NOT PROCESSED

### Meaning

The redirection is not processed for the specified TSN or for each
remaining TSN ((&00)=*ALL).

## SRO0316

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0316 TSN '(&00)': SPOOL SLOT MANAGER ACCESS ERROR. COMMAND NOT PROCESSED

### Meaning

An error has been reported by the SPOOL slot manager.
The redirection is not processed for the specified TSN or for each
remaining TSN ((&00)=*ALL).

## SRO0317

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SRO0317 JOB WITH TSN '(&00)' NOT FOUND

### Meaning

The specified TSN cannot be found in the system.

## SRO0318

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0318 DEVICE SPECIFIED AS REDIRECTION IS NOT A RSO DEVICE. COMMAND REJECTED.

### Meaning

The redirection device specified in the device record is not
a device supported by RSO. Contact the device
administrator or the spool administrator

## SRO0320

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0320 CONFLICT BETWEEN '(&00)' AND '(&01)' OPERANDS. CORRECT COMMAND OR MACRO

### Meaning

These two operands cannot be specified together in the
PRINT-FILE/PRINT-DOC
command or the PRNT/PRNTDOC macro.
(&00), (&01): names of operands.

## SRO0321

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0321 INCONSISTENCY BETWEEN RSO '(&00)' OPERAND AND A 'LOCAL' OPERAND. CORRECT COMMAND OR MACRO

### Meaning

The RSO operand (&00) cannot be specified together with a LOCAL operand
such as CHARS-MODIFICATION etc.
(&00): name of the RSO operand.

## SRO0322

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0322 DEVICE '(&00)' NOT ENTERED IN SPOOL.PARAMETERS FILE. TSN '(&01)' CANNOT BE PROCESSED

### Meaning

The RSO job with TSN (&01) entered in a previous RSO session for the
device
(&00) cannot be processed because this device is no longer contained in
the
SPOOL.PARAMETERS file.

### Response

Contact the system support to redirect this job to another printer
or to the same one after it has been added to the SPOOL.PARAMETERS file.
.

## SRO0323

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0323 INCONSISTENCY BETWEEN '(&00)' OPERAND AND SPECIFIED RSO DEVICE TYPE(S). CORRECT COMMAND OR MACRO

### Meaning

The use of some operands of the PRINT-FILE/PRINT-DOC command (e.g.
FORMS-OVERLAY,PAGE-COPIES) depends on the device type(s) on which
the print request could be issued.

## SRO0324

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0324 INVALID 'TRAY-NUMBER' OPERAND. COMMAND OR MACRO REJECTED

### Meaning

- Value doesn't match the PAGE/LINE SIZE value in the used form.
The PRINT-FILE/PRINT-DOC command or the PRNT/PRNTDOC macro is rejected.

## SRO0325

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0325 SPECIFIED 'TRAY-NUMBER' OPERAND VALUE NOT IN PERMISSIBLE RANGE FROM 1 THROUGH 9. COMMAND OR MACRO REJECTED

### Meaning

The PRINT-FILE/PRINT-DOC command or the PRNT/PRNTDOC macro is rejected.

### Response

Correct the TRAY-NUMBER operand value and retry the command.

## SRO0326

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0326 VALIDATION RECORDS NOT PRESENT IN '(&00)' FILE. COMMAND REJECTED

### Meaning

Records which enable the dynamic validation of some operands
(e.g. FORMS-OVERLAY) according to the device types are not
present in the (&00) file.

### Response

Contact the system support.

## SRO0327

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : YES

SRO0327 CHARACTER SET '(&00)' NOT DEFINED IN SPOOL.PARAMETERS FILE. COMMAND REJECTED

### Response

Correct the CHARACTER-SETS operand and enter the command again.

## SRO0328

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : YES

SRO0328 TRANSLATION TABLE '(&00)' DOES NOT EXIST IN FILE '(&01)'. COMMAND OR MACRO REJECTED

### Meaning

(&01): $TSOS.RSOFILE or
$userid.yyyy.RSOFILE or
$TSOS.yyyy.RSOFILE
(yyyy: value (up to 28 characters) given in the second operand of
the TRANSLATION-TABLE operand).

## SRO0329

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : YES

SRO0329 VFB RECORD WITH KEY '(&00)' MISSING IN FILE '(&01)'. COMMAND OR MACRO REJECTED

### Meaning

VFB: vertical format buffer.
(&00): key of the missing record
(&01): file name.

### Response

- Create the VFB record in file (&01) or
- or retry the command with another FORM-NAME or LOOP-NAME operand value.

## SRO0330

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : YES

SRO0330 VFB OF LOOP '(&00)' DEFINED IN FILE '(&01)' INCOMPATIBLE WITH DEFAULT VFB OF 'FORM-NAME' OPERAND. COMMAND REJECTED

### Meaning

The length of the default VFB must be equal to
the length of the VFB given with the LOOP-NAME operand.
VFB: vertical format buffer.

### Response

Select compatible VFB.

## SRO0331

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : YES

SRO0331 WRONG CHANNEL 1 POSITION IN THE VFB BUILT FROM THE 'LINE-SPACING' VALUE OF THE FORM '(&00)'. COMMAND (MACRO) REJECTED

### Meaning

There is not enough space left between the channel 1 position (first
line of output) and the end of the printer page to allow printout with
the specified print operand values.

### Response

- Contact the system support to correct the channel 1 position
defined in the form (&00) or
- correct the operand values in the PRINT-FILE/PRINT-DOC command.

## SRO0332

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : YES

SRO0332 WRONG CHANNEL 1 POSITION IN THE VFB BUILT FROM THE LOOP '(&00)' DEFINED IN FILE '(&01)'. COMMAND REJECTED

### Meaning

There is not enough space left between the channel 1 position (first line
of output) and the end of the printer page to allow printout with the
operand value specified in the PRINT-FILE/PRINT-DOC command.

### Response

- Contact the system support to correct the VFB (vertical format
buffer) in the system RSOFILE or
- correct the user RSOFILE or
- correct the operands or operand values in the PRINT-FILE/PRINT-DOC
command.

## SRO0333

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : YES

SRO0333 FORM '(&00)': SPOOLOUT PROHIBITED DUE TO MISSING OR INCOMPLETE DEFINITION IN SPOOL.PARAMETERS FILE OR INCOMPLETE SPECIFICATION IN PRINT-FILE/PRINT-DOC. COMMAND (MACRO) REJECTED

### Meaning

Possible causes:
- There is no printer name specified in the PRINT-FILE/PRINT-DOC command.
- The form is not defined in the SPOOL.PARAMETERS file. Therefore the form
cannot be assigned to a printer type.

### Response

- Correct the PRINT-FILE/PRINT-DOC command or
- ask the system support to create the form in the SPOOL.PARAMETERS
file or to add it for the desired printer type(s).

## SRO0334

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0334 WRONG CHANNEL 1 POSITION IN THE 'LOOP' OPERAND '(&00)'

### Meaning

There is not enough space left between the channel 1 position (first line
of the output) and the end of the printer page to allow the printout with
the operand specified in the PRINT-FILE/PRINT-DOC command.
PRINT operand.
(&00): LOOP name
SPACING if the vertical control or the rotation control is equal to
'*SPACING' in the SPOOL.PARAMETERS file for the form
specified in the FORM-NAME operand.

### Response

User loop: correct the channel 1 position.
In all other cases, contact the system support to have the
correction made.

## SRO0335

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0335 INCOMPATIBILITIES BETWEEN DEVICE TYPE OF THE POOL '(&00)' AND OPERAND VALUES. COMMAND OR MACRO REJECTED

### Meaning

The print request cannot be forwarded to any printer belonging to the
pool (&00) due to incompatibilities between the printer type belonging to
the pool and some operands (e.g. FORMS-OVERLAY, PAGE-COPIES, FORM-NAME) of
the PRINT-FILE/PRINT-DOC command or the PRNT/PRNTDOC macro.

## SRO0336

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0336 OPERAND '(&00)' IS MANDATORY WITH OPERAND '(&01)'. CORRECT COMMAND OR MACRO

## SRO0337

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0337 'ROTATION' MODE DEFINED IN FORM '(&00)' NOT SUPPORTED BY THE PRINTER. COMMAND OR MACRO REJECTED

### Meaning

According to the form definition, the file must be printed in the
ROTATION mode but the device does not support this feature.

## SRO0338

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0338 SYNTACTICAL ERROR IN OPERAND '(&00)'. CORRECT COMMAND (MACRO)

## SRO0339

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : YES

SRO0339 RSO JOB '(&00)' HAS BEEN PUT IN 'KEEP' BY AN EXCAT COMMAND AND CANNOT BE RESUMED. COMMAND REJECTED

### Meaning

The /FORCE-CATALOG-EXPORT command has caused the pubset required for
processing the RSO job (&00) to be exported, thus placing the job
in the KEEP state.
The /RESUME-PRINT-JOB command is rejected.

### Response

Import the relevant pubset by means of the /IMPORT-PUBLIC-VOLUME-SET
command.

## SRO0340

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0340 RSO REQUEST WITH INVALID OR INCOMPLETE CONTROL INFORMATION. COMMAND REJECTED

### Meaning

The specified request cannot be properly processed by any of the defined
SPOOL devices. Possible reasons are explained by the preceding messages
(SRO0308 and/or SRO0796).

### Response

Check the specifications in the SPOOL administration files, i.e the
files $SYSSPOOL.SPOOL.PARAMETERS and/or $TSOS.RSOFILE or the user RSOFILE.

## SRO0341

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0341 INVALID 'ROTATION' OPERAND. COMMAND OR MACRO REJECTED.

### Meaning

Rotation has been requested but no rotation loop or rotation
spacing value has been specified in :
- the PRINT-FILE/PRINT-DOC command or
- the PRNT/PRNTDOC macro or
- the FORM

## SRO0342

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0342 VALIDATION RECORDS NOT PRESENT. COMMAND REJECTED.

### Meaning

Records which enable the dynamic validation of some operands
(e.g. FORMS-OVERLAY) are not present.

### Response

Contact the system support.

## SRO0343

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0343 Incompatibility between file ccsname '(&00)' and the device '(&01)'. Command rejected.

### Meaning

(&00) : coded character set name
(&01) : device name
The ccsname of the file is incompatible with the selected
device.

### Response

Select a device compatible with the file ccsname.

## SRO0344

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0344 Incompatibility between file ccsname '(&00)' and control mode. Command or macro rejected.

### Meaning

Ccsname : Coded Character Set Name.

## SRO0345

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0345 Incompatibility between file ccsname '(&00)' and specified RSO device type(s). Command or macro rejected.

### Meaning

Ccsname : Coded Character Set Name.

## SRO0348

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0348 DEVICE '(&00)': INVALID SYNCHRONIZATION

## SRO0349

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0349 DEVICE '(&00)': INVALID 'ESCAPE-CHARACTER'

### Meaning

The ESCAPE-CHARACTER specified in the device record of
the SPOOL.PARAMETERS file is not supported.

## SRO0350

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : YES

SRO0350 SPOOLOUT COMMAND PROCESSING COMPLETED FOR DEVICE '(&00)'

### Meaning

One of the following commands is executed correctly for the device (&00):
/START-PRINTER-OUTPUT
/STOP-PRINTER-OUTPUT
/HOLD-PRINT-JOB

## SRO0351

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0351 TSN '(&00)': SPOOLOUT COMMAND PROCESSING COMPLETED

### Meaning

The /RESUME-PRINT-JOB command has been executed correctly for TSN (&00).

## SRO0352

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0352 SYNTAX ERROR. CORRECT COMMAND

### Meaning

A syntactical error has been encountered in an operand in one of the
following commands:
/START-PRINTER-OUTPUT
/STOP-PRINTER-OUTPUT
/HOLD-PRINT-JOB
/RESUME-PRINT-JOB

### Response

Correct the command and try again.

## SRO0353

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : YES

SRO0353 DEVICE NAME '(&00)' NOT ACCEPTED. COMMAND REJECTED

### Meaning

- The specified device name is not the name of an RSO device.
- The specified device name is not defined in the SPOOL.PARAMETERS file.
One of the following commands is rejected:
/START-PRINTER-OUTPUT
/STOP-PRINTER-OUTPUT

### Response

Verify the device name.

## SRO0354

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : YES

SRO0354 'DESTINATION' NAME '(&00)' INVALID FOR DEVICE '(&01)'. COMMAND REJECTED

### Meaning

Possible reasons:
- device (&01) does not belong to the pool in the SPOOL.PARAMETERS file;
- pool (&00) does not exist in the SPOOL.PARAMETERS file.
The /START-PRINTER-OUTPUT command is rejected for device (&01).

## SRO0355

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0355 TOO MANY VALUES SPECIFIED IN 'DESTINATION' OPERAND. COMMAND REJECTED FOR DEVICE '(&00)'

### Meaning

A maximum of 100 pools can be activated for one device.
The /START-PRINTER-OUTPUT command is rejected.

### Response

- Specify fewer values and/or
- remove the required number of values before adding new ones.

## SRO0356

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0356 'DESTINATION' VALUE TO BE REMOVED WAS NOT ACTIVATED FOR DEVICE '(&00)'. COMMAND REJECTED FOR DEVICE '(&00)'

### Meaning

One pool of the 'to-be-removed' list (DESTINATION=*REMOVE operand) has not
been previously activated for the device (&00) by a /START-PRINTER-OUTPUT
or /MODIFY-PRINTER-OUTPUT command. As a result the /MODIFY-PRINTER-OUTPUT
command is rejected for this device.

## SRO0357

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0357 WARNING: ONLY THE FIRST 100 POOLS ASSIGNED TO DEVICE '(&00)' IN THE SPOOL. PARAMETERS FILE ARE ACTIVATED

### Meaning

Device (&00) belongs to more than 100 pools in the SPOOL.PARAMETERS file
and only the first 100 are activated via the /START-PRINTER-OUTPUT
command.

## SRO0358

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0358 PAGE NUMBER TOO HIGH. COMMAND REJECTED

### Meaning

The page number given in one of the
following commands is higher than 10**7.
/HOLD-PRINT-JOB
/RESUME-PRINT-JOB.

## SRO0359

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0359 PRIORITY NOT ACCEPTED. COMMAND REJECTED

### Meaning

The priority given in one of the following commands is invalid:
/HOLD-PRINT-JOB
/RESUME-PRINT-JOB.

## SRO0360

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0360 PREVIOUS /HOLD-PRINT-JOB NOT COMPLETED FOR DEVICE '(&00)'. TRY COMMAND LATER

### Meaning

The operator tried to do a respool or to defer the spoolout job on
device (&00) by means of a /HOLD-PRINT-JOB command. This attempt failed
because of a running sample process or a previous /HOLD-PRINT-JOB command
for this device which has not yet been completed.
As a result a new command cannot be accepted at present.

## SRO0361

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0361 RSO JOB '(&00)' NOT INTERRUPTED BY KEEP OPTION. COMMAND REJECTED

### Meaning

The RSO job (&00) was not interrupted by a previous KEEP option.
The /RESUME-PRINT-JOB command is rejected.

## SRO0362

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0362 USER NOT AUTHORIZED TO RELEASE THE INTERRUPTED PRINT JOB. COMMAND REJECTED

### Meaning

The print request which is to be moved from the KEEP queue to the
WAIT queue has a pool as a destination.
Thus only the system support or the user who issued the print job
is allowed to enter a /RESUME-PRINT-JOB command.

### Response

Ask the system support to release the print job.

## SRO0363

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : YES

SRO0363 DEVICE '(&00)' DOES NOT BELONG TO ANY POOL IN THE SPOOL.PARAMETERS FILE. COMMAND REJECTED

### Meaning

No pool is assigned to the printer (&00) in the SPOOL.PARAMETERS file.

### Response

Printer (&00) must be activated with the operand DEST=*NONE of the
/START-PRINTER-OUTPUT command.

## SRO0364

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : YES

SRO0364 WARNING: FORM '(&00)' NOT DEFINED IN SPOOL.PARAMETERS FILE. THUS NOT ACCEPTED ON DEVICE '(&01)'

### Meaning

The default form (&00) specified in the device record for the device
(&01) is not defined in the SPOOL.PARAMETERS file. Thus, this form cannot
be used.

### Response

Ask the system support to correct the SPOOL.PARAMETERS file.

## SRO0365

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0365 NO DEFAULT FORM(S) DEFINED FOR PRINTER '(&00)'

### Meaning

There is no list of default forms in the SPOOL.PARAMETERS file for
the printer. *STD has no meaning in this case.

### Response

Ask the system support to define a list of default forms for
the printer or issue a /START-PRINTER-OUTPUT command with a form name.

## SRO0366

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0366 ERROR IN RSO INTERNAL TABLE. COMMAND REJECTED

### Meaning

The RSO table containing the different printer types
supported by this session is erroneous.

### Response

Request the system support to produce diagnostic documentation.

## SRO0367

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0367 PRINTER TYPE '(&00)' OF DEVICE '(&01)' NOT SUPPORTED BY LOADED RSO VERSION. COMMAND NOT PROCESSED

### Response

Contact the system support.

## SRO0368

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0368 TRACE FILE FOR PRINTER CAN ONLY BE CREATED BY THE SYSTEM SUPPORT STAFF. COMMAND REJECTED

### Response

Contact the system support.

## SRO0369

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0369 SUBSYSTEM '(&00)' NOT PRESENT. COMMAND REJECTED

### Meaning

The subsystem (&00) must be created to execute the command.

### Response

Retry later or contact the system support.

## SRO0370

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0370 UNKNOWN USER ID '(&00)'. COMMAND REJECTED

### Meaning

The user ID given in the command does not exist in the JOIN file.

## SRO0371

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0371 SYNTACTICAL ERROR IN VALUE '(&00)' OF OPERAND '(&01)'. CORRECT OPERAND VALUE

## SRO0372

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0372 INVALID OR UNKNOWN OPERAND IN COMMAND. CORRECT COMMAND

## SRO0373

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0373 RSO DEVICE(S) NOT YET STARTED OR NOT DEFINED

### Meaning

The device(s) about which the user is requesting information
- has (have) not been activated via a previous /START-PRINTER-OUTPUT
command or
- has (have) not been defined in the SPOOL.PARAMETERS file by means of
the /ADD-SPOOL-DEVICE command.

## SRO0374

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0374 ADMINISTERED DEVICES NOT YET STARTED

### Meaning

The devices administered by the caller have not yet been activated via a
/START-PRINTER-OUTPUT command.

## SRO0375

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0375 USER NOT AUTHORIZED TO QUERY INFORMATION. COMMAND REJECTED

### Meaning

The user does not have the privilege to obtain the status information
about
RSO jobs issued by a user ID other than his own.

## SRO0376

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0376 NO RSO JOB OF TYPE 'T7' PRESENT

## SRO0377

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0377 DEVICE RECORD CONTAINS A REDIRECTION NAME. COMMAND REJECTED.

### Meaning

A redirection name is not allowed for an active device.

## SRO0378

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0378 USE OF THE PRINTER BY UTM IS NOT ALLOWED DUE TO THE ACTIVATION TYPE OF THE CONTROLLER TASK. COMMAND REJECTED

### Meaning

UTM may only use printers with a controller task activated
at START-PRINTER command.
Contact the device administrator or the system support staff to change
the controller activation in the SPOOL.PARAMETERS file.

## SRO0379

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0379 VALUE '(&00)' GIVEN IN ALLOWED-ACCESS OPERAND IS NOT SUPPORTED. COMMAND REJECTED.

### Meaning

Up to now, the values supported are 'RSO' or 'UTM'.

## SRO0380

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0380 Encryption required for printing on a device declared with ENCRYPTION=NO. Command rejected.

### Meaning

The specified device (or the devices contained in the specified
printer pool) is declared with ENCRYPTION=NO. The job cannot be
treated in a secure way.

## SRO0381

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0381 Encryption not required for printing on a device declared with ENCRYPTION=YES. Command rejected.

### Meaning

The specified device (or the devices contained in the specified
printer-pool) is declared with ENCRYPTION=YES. The job would be
processed with an additional useless CPU time.

## SRO0391

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SRO0391 '(&00)' PRINT REQUESTS REDIRECTED TO DEVICE '(&01)'

### Meaning

With the /REDIRECT-PRINT-JOB command, the printouts are redirected
to the second device (or *CENTRAL with the default value).
(&00): number of prints redirected.

## SRO0392

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : YES

SRO0392 NO RSO PRINT REQUEST FOR DEVICE OR POOL '(&00)'. COMMAND REJECTED

### Meaning

There is no RSO print request waiting for printout on device or pool
(&00).

## SRO0393

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0393 INVALID OPERAND '(&00)'. COMMAND NOT PROCESSED FOR TSN '(&01)'

### Meaning

The RSO or the SPOOL job is not redirected as the print requirements
are not available for central or remote processing.

## SRO0394

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SRO0394 DEVICE '(&00)' NOT A RSO DEVICE. COMMAND NOT PROCESSED FOR TSN '(&01)'

### Meaning

The device name entered in the /REDIRECT-PRINT-JOB command is not an
RSO device.

### Response

Enter the correct RSO device name.

## SRO0700

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0700 USER NOT THE DEVICE ADMINISTRATOR FOR DEVICE '(&00)' AND/OR TERMINAL NOT AN ADMINISTRATION TERMINAL

### Meaning

The user is not the administrator of device (&00).
Either the user identification is not assigned to the system support
or device administration or the terminal is not authorized to perform
administration tasks.

### Response

Request the authorization from the system support to administrate
the device or use an authorized terminal.

## SRO0701

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0701 'FORM-NAME' OPERAND VALUE '(&00)' NOT PERMITTED FOR DEVICE '(&01)'. COMMAND REJECTED

### Meaning

The specified value for the FORM-NAME operand
- does not match any form in the SPOOL parameter file or
- has not been defined as a form for the specified printer.

### Response

For detailed information about the forms or printers defined in the
SPOOL.PARAMETERS file enter the /SHOW-SPOOL-FORMS or /SHOW-SPOOL-DEVICE
command and correct the FORM-NAME operand using this information.

## SRO0702

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0702 WARNING: CHARS ('(&00)',...) NOT IN THE '(&01)' FILE

### Meaning

Some character sets given in the CHARACTER-SETS operand of the PRINT-FILE/
PRINT-DOC command are not defined in the (&01) file.
The subsequent print processing may therefore be erroneous.
(&00): list of non-defined character sets (maximum 7).

### Response

- Correct the value of the CHARACTER-SETS operand and try the PRINT-FILE/
PRINT-DOC command again or
- include the missing character sets into the (&01) file.

## SRO0703

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO0703 RSO TASK '(&00)' CURRENTLY NOT AVAILABLE. RETRY COMMAND LATER

### Meaning

Possible reasons:
- RSO recovery in progress
- communication not possible because of SRAM crash.

## SRO0704

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0704 RSO SUBSYSTEM CANNOT CURRENTLY BE ACCESSED. RETRY COMMAND LATER

### Meaning

The RSO devices cannot currently be accessed because
- the RSO subsystem is being recovered.
- no communication is possible due to a SRAM crash.

## SRO0705

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0705 RSO DEVICE '(&00)' RELEASED BY DEVICE ADMINISTRATOR ID '(&01)'

### Meaning

A /STOP-PRINTER-OUTPUT command has been executed for a RSO device.
(&01): user ID of the device administration.

## SRO0706

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0706 LIMIT VALUE FOR PRIVATE ONLINE RSO DEVICES REACHED. RETRY COMMAND LATER

### Meaning

The limit value for private online RSO devices defined in the
SPOOL.PARAMETERS file has been reached. A new /START-PRINTER-OUTPUT
command
is not permitted for private RSO devices.

### Response

If this device is essential, ask the system support to modify the
REMOTE-DEVICE-LIMIT value of the SPOOL.PARAMETERS file.

## SRO0707

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0707 RSO VERSION '(&00)' NOT COMPATIBLE WITH LOADED SPOOL VERSION '(&01)'. RSO ABORTED

### Response

Use the appropriate RSO version.

## SRO0708

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0708 DEVICE '(&00)' HAS BEEN REMOVED FROM THE CONFIGURATION TABLE OR THE IPP PRINTER NAME PREFIX HAS BEEN CHANGED. SPOOL JOB REMAINS IN 'KEEP' STATE.

### Meaning

The device was removed from the configuration table before the
/RESUME-PRINT-JOB command was executed.
Or the IPP printer name prefix has been changed.
The SPOOL job remains in the KEEP queue.

### Response

Request the system support to add the device to the configuration
table again using an /ADD-SPOOL-DEVICE command.
In case of a print-job scheduled on a system device, either cancel
the concerned print-jobs or reinstall the old prefix temporarily
in order to print out these jobs.

## SRO0709

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0709 INTERNAL ERROR DURING SPOOL PARAMETER FILE ACCESS. COMMAND PROCESSING ABORTED

### Response

Check the validity of the SPOOL.PARAMETERS file and, if it is valid,
retry the command. If the error persists, inform the system support.

## SRO0710

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0710 TSN '(&00)': INCONSISTENCY BETWEEN 'LEFT-MARGIN' OPERAND IN PRINT-FILE/PRINT-DOC AND PAPER FORMAT OR CHARACTER DENSITY. OUTPUT SUSPENDED

### Meaning

The value of the LEFT-MARGIN operand in the PRINT-FILE/PRINT-DOC command
or its default defined in the SPOOL.PARAMETERS file is too large.

### Response

Ask the system support to change the paper format or character
density before releasing the TSN.

## SRO0711

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0711 TSN '(&00)': READ ERROR WHEN ACCESSING SPOOL.PARAMETERS FILE. CHECK FILE

## SRO0712

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0712 TSN '(&02)': CHARACTER SET C'(&00)', X'(&01)' DOES NOT EXIST IN SPOOL. PARAMETERS FILE. JOB SUSPENDED

### Meaning

(&00): alphanumeric character set
(&01): hexadecimal character set.

### Response

Include the missing character set in the SPOOL.PARAMETERS file and,
if necessary, also in the RSOFILE or the RSO PARAMETER file.
Then release the TSN.

## SRO0713

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0713 TSN '(&02)': FORM '(&00)' DEFINED FOR DEVICE TYPE '(&01)' DOES NOT EXIST IN SPOOL.PARAMETERS FILE. JOB SUSPENDED

### Meaning

(&00): form name
(&01): device type.

### Response

Include the missing form for this device type in the SPOOL.PARAMETERS
file.
Then release the TSN.

## SRO0714

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0714 TSN '(&01)': DEVICE '(&00)' NOT DEFINED IN SPOOL.PARAMETERS FILE

### Meaning

The definition of the RSO printer is not or no longer present in the
SPOOL.PARAMETERS file.

### Response

If necessary, request the system support to add the specified
RSO device to the SPOOL.PARAMETERS file.

## SRO0715

Destination: CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0715 DCAM APPLICATION 'OPEN' REQUEST FROM SRAM ABORTED WITH DCAM RETURNCODE FDB=X'(&00)'. REPLY (R=RETRY; T=TERMINATE).

### Meaning

FDB: the relevant bytes of the DCAM returncode.

### Response

Inform the network administration if necessary.

## SRO0716

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0716 TSN '(&00)': BOURSE FOR RSO MESSAGE OUTPUT CANNOT BE CREATED. JOB SUSPENDED

### Meaning

The macro $NBCREA returns an error code: it is impossible to establish
a communication between the message task and the controller task.

### Response

Contact the system support.

## SRO0717

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0717 TSN '(&00)': RSO MESSAGE OUTPUT TASK CANNOT BE CREATED. JOB SUSPENDED

### Response

Once that a message output task can be created, the suspended print jobs
should be released.

## SRO0718

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0718 TSN '(&00)': MEMORY POOL FOR RSO MESSAGE OUTPUT CANNOT BE REQUESTED. JOB SUSPENDED

### Meaning

The macro $ENAMP returns an error code: the connection to the memory pool
of the controller task is refused to the message task.

### Response

Contact the system support.

## SRO0719

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0719 TSN '(&00)': MESSAGE TASK UPPER LIMIT REACHED. JOB SUSPENDED

### Response

Contact the system support.

## SRO0720

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0720 *** MEMORY POOL NOT AVAILABLE. RSO SESSION NOT POSSIBLE ***

### Meaning

The macro $ENAMP returns an error code: the required memory pool could not
be generated by the controller task.

### Response

Contact the system support.

## SRO0721

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0721 *** RSO SUBSYSTEM NO LONGER AVAILABLE IN THIS BS2000 SESSION. CONTACT THE SYSTEM SUPPORT STAFF ***

## SRO0722

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0722 *** NO CLASS (&00) MEMORY AVAILABLE. RSO SUBSYSTEM ABORTED. CONTACT THE SYSTEM SUPPORT STAFF ***

## SRO0723

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0723 RSO DEVICE '(&00)' NOT AVAILABLE DUE TO SHORTAGE OF CLASS 5 MEMORY SPACE

### Response

Contact the system support or try again later.

## SRO0724

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0724 SHORTAGE OF CLASS 5 MEMORY SPACE

### Response

When the memory allocation problem is solved, the operator or
the system support can restart the job with a /RESUME-PRINT-JOB
command or re-activate the device with a /START-PRINTER-OUTPUT command.

## SRO0725

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0725 WARNING: 'CHAR-IMAGE=(&00)' NOT DEFINED IN TRANSLATION TABLE FOR DEVICE '(&01)'. SPOOLOUT CONTINUES

### Response

Request the system support to add the translation table
with RSOSERVE or to modify the value of the CHARACTER-IMAGE operand.

## SRO0726

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0726 TSN '(&02)': SPOOLOUT COMPLETED ON DEVICE '(&00)' FOR FILE '(&01)'

## SRO0727

Destination: CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0727 ERROR DURING SPOOLOUT ON DEVICE '(&00)'. REPLY (T=TERMINATE; D=DEFER; K=KEEP)

### Response

T: the spoolout job will be removed from the spoolout queue
and the file will be erased if requested.
D: the spoolout job will be returned to the spoolout queue.
Subsequent messages will query the new priority and the restart
type for the deferred job.
K: the spoolout job will be added to the KEEP queue until the operator
restarts it by means of a /RESUME-PRINT-JOB command.
A subsequent message will query the restart type.

## SRO0728

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0728 ERROR DURING SPOOLOUT ON DEVICE '(&00)'

### Response

When the error cause has been removed, restart the job by means of the
/RESUME-PRINT-JOB command.

## SRO0729

Destination: CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0729 '(&00)' ERROR DURING SPOOLOUT ON DEVICE '(&01)'. REPLY (T=TERMINATE; D=DEFER; K=KEEP)

### Meaning

An error occurred when loading the buffer of the specified printer.
(&00): BUFFER or VFB or DMS.

### Response

T: the spoolout job will be removed from the spoolout queue
and the file will be erased if requested.
D: the spoolout job will be returned to the spoolout queue.
Subsequent messages will query the new priority and the restart
type for the deferred job.
K: the spoolout job will be added to the KEEP queue until the operator
restarts it by means of a /RESUME-PRINT-JOB command.
A subsequent message will query the restart type.

## SRO0730

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0730 TSN '(&02)': '(&00)' ERROR ON DEVICE '(&01)' DURING SPOOLOUT

### Meaning

An error occurred when loading the buffer of the specified printer.
(&00): BUFFER or VFB or DMS.

### Response

When the error cause has been removed, restart the job by means of the
/RESUME-PRINT-JOB command.

## SRO0731

Destination: CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0731 SPECIFY NEW PRIORITY FOR DEFERRED JOB ON DEVICE '(&00)'. REPLY (<NNN>=NEW PRIORITY 30 THROUGH 255)

## SRO0732

Destination: CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0732 SPECIFY RESTART TYPE FOR DEFERRED JOB, DEVICE '(&00)'. REPLY (B=BEGINNING; P=PREVIOUS CHECKPOINT; S=START OF PAGE; <NN>= DECIMAL PAGE NUMBER)

### Meaning

The operator is requested to specify where to restart the job that was
deferred on device (&00).

### Response

B: the job will be restarted from the very beginning.
P: the job will be restarted from the previous spoolout checkpoint.
S: the job will be restarted from the beginning of the page currently
being printed.
<NN>: decimal value specifying the page number from which the job is to
be restarted (must be lower than the current page number).

## SRO0733

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0733 TSN '(&02)': DMS ERROR '(&01)' WHEN OPENING FILE '(&00)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

The spoolout job (&00) resulted in OPEN error code (&01).
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

When the error cause has been removed, restart the job by means of the
/RESUME-PRINT-JOB command.

## SRO0734

Destination: CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0734 DMS ERROR '(&00)' WHEN PROCESSING FILE '(&01)'. REPLY (T=TERMINATE; D=DEFER; K=KEEP)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

T: The spoolout job is terminated.
D: the spoolout job will be returned to the spoolout queue.
Subsequent messages will query the new priority and the restart
type for the deferred job.
K: the spoolout job will be added to the KEEP queue until the operator
restarts it by means of a /RESUME-PRINT-JOB command. A subsequent
message
will query the restart type.

## SRO0735

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0735 (&00) ERROR '(&01)' FOR FILE '(&02)'

### Meaning

For more detailed information about the DMS or PLAM error code enter
/HELP-MSG DMS(&01) or /HELP-MSG PLA(&01) in system mode or see the
BS2000 manual 'System Messages'.
(&00): DMS / PLAM
(&01): specific error code
(&02): file name.

### Response

Correct the PLAM or DMS error and restart the job by means of the
/RESUME-PRINT-JOB command.
In the case of the error key DMS0D33 check and if necessary correct the
file name.

## SRO0736

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0736 TSN '(&02)': USER ERROR WHEN SPOOLOUT OF FILE '(&00)' ON DEVICE '(&01)'. VFB OVERFLOW

### Meaning

The user wants to print more lines per page than permitted by the VFB
(Vertical Format Buffer) used for the RSO printer indicated by the device
name (&01).

### Response

After the input file has been modified, start the job again. In the event
of an invalid LOOP-NAME operand in the PRINT-FILE/PRINT-DOC command, the
job has to be cancelled by means of a /CANCEL-PRINT-JOB command and a
corrected PRINT-FILE/PRINT-DOC command has to be entered.

## SRO0737

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0737 TSN '(&02)', DEVICE '(&01)': USER ERROR WHEN PRINTING FILE '(&00)'. INVALID CONTROL BYTE

### Response

Correct the input file and start the job again.

## SRO0738

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0738 USER ERROR FOR FILE '(&00)' ON DEVICE '(&01)'. VFB CHANNEL NOT FOUND

### Meaning

The user uses a skip to a channel which does not exist in the VFB
(Vertical Format Buffer) used for the RSO printer (&01).

### Response

Modify the input file and start the job again.

## SRO0739

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0739 TSN '(&03)', DEVICE '(&01)': USER ERROR WHEN PRINTING FILE '(&00)'. INVALID CSI '(&02)'

### Meaning

CSI: Character Set Identifier.

### Response

Correct the input file and start the job again.

## SRO0740

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0740 SYSTEM ERROR. JOB WITH TSN '(&01)' DEFERRED ON DEVICE '(&00)' CANNOT BE ACTIVATED. JOB ADDED TO SPOOL SHUTDOWN QUEUE

### Meaning

The suspended spoolout job could not be entered into the ACTIVE queue due
to an error in the defer operation.
The spoolout job will stay in the SHUTDOWN queue until the next warm
start.
In the case of a cold start the spoolout job is lost.
(&00): mnemonic or logical name of the device on which the operator
deferred the task.

## SRO0741

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0741 TSN '(&00)', DEVICE '(&01)': RSO JOB SUSPENDED

### Meaning

The RSO job is suspended, i.e. it is put back into the spoolout queue.

## SRO0742

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0742 CANNOT RELEASE CLASS 5 MEMORY. SPOOLOUT CONTINUES. CONTACT THE SYSTEM SUPPORT STAFF

### Meaning

RSO received an error code while class 5 memory (RELM) was being released.

## SRO0744

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0744 SYSTEM FAILED ON DEVICE '(&00)'. IMPOSSIBLE TO UPDATE CHECKPOINT INFORMATION FOR JOB WITH TSN '(&01)'

### Meaning

Due to a system error it is not possible to write the job back into the
shutdown queue in order to include the last checkpoint.
The spoolout continues normally but some positioning problems
(e.g. too many reprinted pages) can occur if there is a crash.
(&00): RSO printer name.

## SRO0746

Destination: CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO0746 ENTER PROCESSING OF 'SRAM' TASK FOR CONTROLLER (TSN: (&00)) ABORTED WITH ERROR. REPLY (R=RETRY; T=TERMINATE)

### Response

Check the ENTER file.

## SRO0747

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0747 CONFIGURATION TABLE ERROR. CONTACT THE SYSTEM SUPPORT STAFF

### Meaning

The RSO items in the SPOOL.PARAMETERS file contain at least one error.
The spoolout job will be added to the KEEP queue.

### Response

Contact the device administration or the system support.
As soon as the error is corrected, restart the job by means of a
/RESUME-PRINT-JOB command.

## SRO0748

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0748 RECOVERY PROCESSING FOR RSO TASK '(&00)' STARTED. WAIT FOR COMPLETION

### Meaning

The RSO control task and/or the SRAM task were/was destroyed as a result
of
a serious error.
Recovery processing has been started to check the status of the RSO memory
pool and to generate the RSO control task and/or the SRAM task again.

## SRO0749

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0749 END OF RECOVERY PROCESSING. RSO AVAILABLE

## SRO0750

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0750 RECORDING DENSITY ERROR IN 'FORM-NAME' OPERAND '(&00)'

### Meaning

(&00): name of the form.

### Response

Correct the form definition in the SPOOL.PARAMETERS file.

## SRO0751

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0751 RSO SUBSYSTEM CANNOT BE LOADED WITHOUT SPOOL SUBSYSTEM

### Response

Load the SPOOL subsystem by means of the /START-SUBSYSTEM command.
Subsequent load the RSO subsystem.

## SRO0752

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0752 BOURSE CREATION ERROR '(&00)'.

### Meaning

The $NBCREA interface has returned an error code : (&00).

### Response

Contact the system support.

## SRO0753

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SRO0753 Invalid value in subsystem-parameter operand of '(&00)' , command.

### Meaning

(&00) : command name :
/START-SUBSYSTEM or /STOP-SUBSYSTEM or
/RESUME-SUBSYSTEM or /HOLD-SUBSYSTEM.

### Response

Correct command and retry.

## SRO0788

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0788 TSN '(&01)': NO DEVICE RECORD SPECIFIED IN '(&02)' FILE FOR DEVICE '(&00)'

### Response

Request the device administration to add all the default values on the
control panel of device (&00) to a device record of the (&02) file.

## SRO0789

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0789 FILE NOT FOUND FOR DIA '(&00)'

### Meaning

The DIA file is not defined with the standard file name either under the
PRINT user ID or under the device administration user ID or in the
device itself.

### Response

The DIA must be defined by the user or by the device administration.

## SRO0790

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0790 TSN '(&02)': CHARACTER SET '(&00)' NOT DEFINED IN '(&03)' FILE FOR DEVICE TYPE '(&01)'

### Response

Use a different character set or ask the device administration to enter
the character set (&00) in the file (&03) for device type (&01).

## SRO0791

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0791 LENGTH OF DEFAULT VFB DOES NOT CORRESPOND TO THAT SPECIFIED IN OPERAND 'FORM-NAME'. COMMAND REJECTED

### Meaning

The form length calculated from the default VFB is different from the form
length in the SPOOL.PARAMETERS file for the specified FORM-NAME operand.

### Response

Ask the device administration to correct the SPOOL.PARAMETERS file.

## SRO0792

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0792 INCONSISTENCY BETWEEN OPERAND 'FORMS-OVERLAY' AND SPECIFIED RSO DEVICE TYPE. CORRECT COMMAND

### Meaning

The FORMS-OVERLAY operand in the PRINT-FILE/PRINT-DOC command may be
specified only for 9025 or 9026-RENO RSO printer.

## SRO0793

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0793 VALUE OF OPERAND 'FROM' OR 'TO' CANNOT BE EXPRESSED IN LINES IF 'CONTROL-CHARACTER=LINE-MODE' IS SPECIFIED. CORRECT COMMAND

### Meaning

With 'CONTROL-CHARACTER=LINE-MODE', the operand FROM or TO must be
expressed in pages (DIMENSION=PAGES operand).

## SRO0794

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0794 USER ERROR '(&00)' WHEN PRINTING FILE '(&01)' ON DEVICE '(&02)'. JOB SUSPENDED

### Meaning

The spoolout job will be added to the KEEP queue.
(&00): 9025 or 9026-RENO error code.

### Response

Modify the input file and release the job by means of the
/RESUME-PRINT-JOB
command.

## SRO0795

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0795 PAGE COPIES CANNOT BE PRINTED ON THE SPECIFIED DEVICE. CORRECT COMMAND.

## SRO0796

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0796 PRINTER NOT DEFINED IN SPOOL.PARAMETERS FILE

### Meaning

The specified device has not been previously defined by means of
the command /ADD-SPOOL-DEVICE.

### Response

Check this SPOOL parameter with the /SHOW-SPOOL-DEVICES command.

## SRO0798

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0798 RESTART PAGE NUMBER '(&00)' FOR JOB WITH TSN '(&01)' IS GREATER THAN FILE CAPACITY. JOB SUSPENDED

### Meaning

The page number specified for restarting the printout is too high.
The job is added to the KEEP queue. After the file has been released
by means of a /RESUME-PRINT-JOB command, the printout is restarted from
the beginning of the file.

## SRO0799

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0799 CHARACTER SET '(&00)' NOT DEFINED IN '(&01)' FILE

### Response

Use a different character set or ask the device administration to enter
the character set in the file (&01).

## SRO0892

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0892 PARITY ERROR DETECTED BY THE PRINTER

### Response

Contact a device administrator or the system support.

## SRO0893

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0893 PRINTER IS WARMING UP

### Meaning

The printer has just been switched on and may need
some time to warm up.

### Response

Retry later.

## SRO0894

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0894 PRINTER TONER IS EMPTY

### Response

Ask a device administrator or the system support
to replenish the printer toner container.

## SRO0895

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0895 PAPER JAM DETECTED BY THE PRINTER

### Meaning

An input or internal or output paper jam occurred.

## SRO0896

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0896 INVALID PAPER SIZE DETECTED BY THE PRINTER

### Meaning

The programmed form length exceeds the maximum form length
permitted by the paper used.

### Response

Check the LOOP or the FORM definition or the installed paper size.

## SRO0897

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0897 INVALID PRINTER ESCAPE SEQUENCE DETECTED BY THE PRINTER

### Meaning

The printer did not recognize a printer escape sequence.

### Response

Check the contents of your file.

## SRO0898

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0898 LINE OVERFLOW DETECTED BY THE PRINTER

### Meaning

The printer has detected a line overflow. Forced "carriage return"
and "line feed" are automatically performed by some printer types.

### Response

Check the contents of your file.

## SRO0899

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0899 PRINTER SERVICING REQUIRED

### Meaning

Maintenance is required on the printer.

### Response

Contact a device administrator or the system support.

## SRO0900

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0900 WARNING: DCAM CALL TERMINATED WITH ERROR CODE '(&00)'

### Meaning

If one of the following commands is entered, the complete DCAM return code
is contained in the ERCOD field of the command output.
/SHOW-SYSTEM-STATUS
/SHOW-JOB-STATUS
/SHOW-USER-STATUS JOB-TYPE=RSO-SPOOLOUT

### Response

Contact the network administrator, if necessary.

## SRO0901

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0901 DCAM CALL DOES NOT CORRESPOND TO CURRENT APPLICATION STATUS. DCAM RETURN CODE '(&00)'

### Meaning

If one of the following commands is entered, the complete DCAM return code
is contained in the ERCOD field of the command output.
/SHOW-SYSTEM-STATUS
/SHOW-JOB-STATUS
/SHOW-USER-STATUS JOB-TYPE=RSO-SPOOLOUT

### Response

Contact the network administrator, if necessary.

## SRO0902

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0902 DCAM CALL DOES NOT CORRESPOND TO CURRENT PARTNER STATUS. DCAM RETURN CODE '(&00)'

### Meaning

If one of the following commands is entered, the complete DCAM return code
is contained in the ERCOD field of the command output.
/SHOW-SYSTEM-STATUS
/SHOW-JOB-STATUS
/SHOW-USER-STATUS JOB-TYPE=RSO-SPOOLOUT

### Response

Contact the network administrator, if necessary.

## SRO0903

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0903 DCM ERROR: DCAM RETURN CODE '(&00)'

### Meaning

If one of the following commands is entered, the complete DCAM return code
is contained in the ERCOD field of the command output.
/SHOW-SYSTEM-STATUS
/SHOW-JOB-STATUS
/SHOW-USER-STATUS JOB-TYPE=RSO-SPOOLOUT

### Response

Contact the network administrator, if necessary.

## SRO0904

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0904 SYSTEM ERROR. INVALID DCAM MACRO CALL: DCAM RETURN CODE '(&00)'

### Meaning

If one of the following commands is entered, the complete DCAM return code
is contained in the ERCOD field of the command output.
/SHOW-SYSTEM-STATUS
/SHOW-JOB-STATUS
/SHOW-USER-STATUS JOB-TYPE=RSO-SPOOLOUT

### Response

Contact the network administrator, if necessary.

## SRO0905

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0905 NEGATIVE ACKNOWLEDGMENT FROM PRINTER. RETURN CODE '(&00)'

### Meaning

If one of the following commands is entered, the complete DCAM return code
is contained in the ERCOD field of the command output.
/SHOW-SYSTEM-STATUS
/SHOW-JOB-STATUS
/SHOW-USER-STATUS JOB-TYPE=RSO-SPOOLOUT

### Response

Contact the network administrator, if necessary.

## SRO0906

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0906 NEGATIVE RETURN CODE OF PDN '(&00)' FOR 9645 PRINTER

### Meaning

The complete PDN return code '(&00)' is contained in the ERCOD field
of the /STATUS R and /STATUS <tsn> command output.
(&00): 4 digits, 1.byte: NBZ
2.byte: letter for the definition of the PDN DMS macro
O: open connection error
L: open library error
M: open member error
R: read member error
A: administration error
W: write error.
3.byte: register R
4.byte: PDN register T .

### Response

Contact the network administrator, if requested.

## SRO0907

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0907 ERROR MESSAGE '(&00)' FROM 9025 PRINTER OR 9026-RENO PRINTER

### Meaning

The 9025/9026-RENO error message number (&00) is contained in the
ERCOD field of the /STATUS R and /STATUS <tsn> command output.

### Response

Contact the system support or the printer administration,
if necessary.

## SRO0908

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0908 9025 PRINTER OR 9026-RENO PRINTER NO LONGER OPERABLE DUE TO OPERATOR ACTION. ERROR MESSAGE '(&00)'

### Meaning

The 9025/9026-RENO error message number (&00) is contained in the
ERCOD field of the /STATUS R and /STATUS <tsn> command output.

### Response

Contact the system support or the printer administration,
if necessary.

## SRO0909

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0909 DCAM APPLICATION NOT OPENED BY CALLING TASK (AID INVALID). DCAM RETURN CODE FDB=X'0804....'

### Meaning

FDB: Relevant bytes of the DCAM return code (FDB1 to FDB4).

### Response

Contact the network administrator, if necessary.

## SRO0911

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0911 PRINTER ERROR (EXCEPT END OF PAPER OR OFFLINE)

## SRO0912

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0912 END OF PAPER OR OFFLINE

## SRO0913

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0913 NO PRINT ACKNOWLEDGMENT FROM 9025/9026-RENO PRINTER

### Meaning

RSO received no print acknowledgment for the printout on the
9025/9026-RENO
printer.

### Response

Check the printer.

## SRO0914

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0914 NETWORK ERROR: 'LOSCON' RECEIVED FOR PRINTER. DCAM RETURN CODE '(&00)'

### Meaning

If one of the following commands is entered, the complete DCAM return code
is contained in the ERCOD field of the command output. The return code
corresponds to the register 6 of the LOSCON contingency.
/SHOW-SYSTEM-STATUS
/SHOW-JOB-STATUS
/SHOW-USER-STATUS JOB-TYPE=RSO-SPOOLOUT

### Response

Contact the network administrator, if necessary.

## SRO0915

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0915 NETWORK ERROR: 'COMEND' RECEIVED. DCAM RETURN CODE '(&00)'

### Meaning

If one of the following commands is entered, the complete DCAM return code
is contained in the ERCOD field of the command output. The return code
corresponds to the register 4 of the COMEND contingency.
/SHOW-SYSTEM-STATUS
/SHOW-JOB-STATUS
/SHOW-USER-STATUS JOB-TYPE=RSO-SPOOLOUT

### Response

Contact the network administrator, if necessary.

## SRO0916

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0916 DCAM APPLICATION ABORTED. DCAM RETURN CODE FDB=X'0824....'

### Meaning

The BCAM connection is terminated by the operator by means of the /DASC
command.
FDB: Relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if necessary.

## SRO0917

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0917 DCAM APPLICATION ABORTED DUE TO DCAM ERROR. DCAM RETURN CODE FDB=X'0828.... '

### Meaning

The BCAM connection is terminated by the operator by means of the /DASC
command.
FDB: Relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if necessary.

## SRO0919

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0919 INVALID OR MISSING PRINT ACKNOWLEDGMENT

### Response

Contact the network administrator, if necessary.

## SRO0920

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0920 SRAM VERSION '(&00)' NOT COMPATIBLE WITH LOADED RSO VERSION '(&01)'. RSO ABORTED.

### Response

Use the correct SRAM version.

## SRO0921

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0921 SRAM CANNOT BE LOADED. RETURN CODE=X'(&00)' FOR DYNAMIC LINKAGE

### Meaning

The cause is a DLL error.
Refer to previous console messages.

### Response

Reload RSO.

## SRO0922

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0922 SRAM RECEIVED NO OPEN ACKNOWLEDGMENT FROM PDN OR DCAM. PLEASE CONTACT THE SYSTEM SUPPORT STAFF

### Meaning

If SRAM does not receive an open acknowledgment within a specified period,
it assumes that the acknowledgment has been lost.

## SRO0930

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0930 SOCKETS : THE REQUESTED SOCKET IS NOT CONNECTED

### Meaning

The connection to the printer has been lost. Check whether the port

### Response

name (see device definition) is still active. Check also the
cable interfacing the printer with the TACLAN or the PC-DOS
running SPPCS.
Contact the network administration.

## SRO0931

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0931 SOCKETS : INVALID ADDRESS

### Meaning

The printer you wish to gain access to is probably wrongly defined.

### Response

Check the internet address and the port name.
Contact the network administration.

## SRO0932

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0932 PARTNER NOT LINKED WITH DCAM APPLICATION (INVALID CID). DCAM RETURN CODE FDB=X'0C04....'

### Meaning

FDB: Relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if necessary.

## SRO0933

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0933 PARTNER ALREADY LINKED WITH DCAM APPLICATION. DCAM RETURN CODE FDB=X'0C08.. ..'

### Meaning

FDB: Relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if necessary.

## SRO0934

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0934 SOCKETS : THE REQUESTED SOCKET IS ALREADY CONNECTED

### Meaning

The printer you wish to gain access to is already connected.

### Response

Contact the network administration.

## SRO0935

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0935 SOCKETS : ADDRESS ALREADY IN USE

### Meaning

The printer you wish to gain access to is being used by someone else.

### Response

Retry later or contact the network administration.

## SRO0946

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0946 SOCKETS : CONNECTION TIMEOUT

### Meaning

The connection to the printer cannot be set up within the system
interval of time.

### Response

Retry later or contact the network administration.

## SRO0947

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0947 SYSTEM TIMEOUT FOR CONNECTION REQUEST. DCAM RETURN CODE FDB=X'0C48....'

### Meaning

FDB: Relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if necessary.

## SRO0948

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0948 PARTNER NOT ACCESSIBLE WITHOUT OPENING DCAM APPLICATION. DCAM RETURN CODE FDB=X'0C4C....'

### Meaning

Possible reasons:
- printer not correctly defined
- printer already being used.
FDB: relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if necessary to start the
DCAM application computers or make the printer operable (CC61 at console).

## SRO0949

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0949 PARTNER DOES NOT PROCESS CONNECTION REQUESTS. DCAM APPLICATION IN STOP STATE. DCAM RETURN CODE FDB=X'0C50....'

### Meaning

FDB: Relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if necessary.

## SRO0951

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0951 SOCKETS : CONNECTION REJECTED

### Meaning

The connection to the printer has been rejected.
Probably the required service was not available at that time.

### Response

Check the availability of the printer. Check the validity
of the internet address. Check whether the line (internet
address) has been activated from BS2000 side.
Retry later or contact the network administration.

## SRO0952

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0952 CONNECTION REQUEST REJECTED BY PARTNER (E.G. 'REJLOG' MACRO CALL). DCAM RETURN CODE FDB=X'0C5C....'

### Meaning

FDB: Relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if necessary.

## SRO0953

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0953 PARTNER BELONGS TO ANOTHER DCAM APPLICATION. DCAM RETURN CODE FDB=X'0C70... .'

### Meaning

FDB: Relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if necessary.

## SRO0957

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0957 SOCKETS : NOT ENOUGH STORAGE SPACE TO CREATE A SOCKET. RETRY LATER

### Meaning

Not enough memory available to create a socket.

### Response

Retry later or contact the network administration.

## SRO0958

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0958 SOCKETS : TOO MANY OPEN DESCRIPTORS TO CREATE A SOCKET

### Meaning

The limit for the number of socket descriptors which can be processed
simultaneously has been reached.

### Response

Retry later or contact the system support.

## SRO0959

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0959 DCAM: NOT ENOUGH STORAGE SPACE. BCAM: RETRY INPUT/OUTPUT LATER. DCAM RETURN CODE FDB=X'100404..'

### Meaning

FDB: Relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if necessary.

## SRO0960

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0960 DCAM: NOT ENOUGH STORAGE SPACE. BCAM: NOT ENOUGH STORAGE SPACE. DCAM RETURN CODE FDB=X'100408..'

### Meaning

FDB: Relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if necessary.

## SRO0961

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0961 DCAM: NOT ENOUGH STORAGE SPACE, THEREFORE NO CONTROL BLOCK AVAILABLE. DCAM RETURN CODE FDB=X'100420..'

### Meaning

FDB: Relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if necessary.

## SRO0962

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0962 DCAM: NOT ENOUGH STORAGE SPACE, THEREFORE NO ID ENTRY AVAILABLE. DCAM RETURN CODE FDB=X'100424..'

### Meaning

FDB: Relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if necessary.

## SRO0963

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0963 DCAM: NOT ENOUGH STORAGE SPACE. DCAM: NO STORAGE SPACE AVAILABLE ($REQM). DCAM RETURN CODE FDB=X'100428..'

### Meaning

FDB: Relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if requested

## SRO0965

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0965 DCM TERMINATION. DCAM RETURN CODE FDB=X'1008....' OR X'100C....'

### Meaning

FDB: Relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if necessary.

## SRO0966

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0966 DCM NOT ACTIVE. DCAM RETURN CODE FDB=X'1010....'

### Meaning

FDB: Relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if necessary.

## SRO0967

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0967 DCM ERROR. DCAM RETURN CODE FDB=X'1014....'

### Meaning

FDB: Relevant bytes of the DCAM return code.

### Response

Contact the network administrator, if necessary.

## SRO0968

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0968 PRINTER DEVICE ERROR

### Response

Check the printer.

## SRO0969

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0969 END OF PAPER OR PAPER SIZE ERROR

### Meaning

Depending on the printer type (check printer manual),
either the printer has run out of paper or an invalid
paper size was requested.

## SRO0970

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0970 PRINTER IN STOP STATUS

## SRO0971

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0971 END OF PAPER AND PRINTER IN STOP STATE

## SRO0972

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0972 DATA OVERFLOW

### Response

Check the file, if necessary.

## SRO0973

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0973 CARRIAGE SHIELD OPENED

## SRO0974

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0974 CARRIAGE SHIELD OPENED AND PRINTER IN STOP STATE

## SRO0975

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0975 DEVICE ERROR AND FORMAT ERROR

### Response

Check the printer and the file.

## SRO0976

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0976 END OF PAPER AND FORMAT ERROR

### Response

Supply paper and check the printer.

## SRO0977

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0977 PRINTER IN STOP STATE AND FORMAT ERROR

## SRO0978

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0978 END OF PAPER, PRINTER IN STOP STATE AND FORMAT ERROR

## SRO0979

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0979 DATA OVERFLOW AND FORMAT ERROR

## SRO0980

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0980 CARRIAGE SHIELD OPENED AND FORMAT ERROR

## SRO0981

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0981 CARRIAGE SHIELD OPENED, PRINTER IN STOP STATE AND FORMAT ERROR

## SRO0982

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0982 NETWORK BREAK.

## SRO0983

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0983 INTERNAL 'SRAM' ERROR

### Meaning

Possible causes:
- last entry in the SRAM printer table
- no DCAM application free
- format error for YSEND, but connection is still available.

## SRO0984

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0984 JOB WHICH CAUSED ABORTION OF CONTROLLER TASK IS SUSPENDED

### Response

Restart the job with a /RESUME-PRINT-JOB command.

## SRO0985

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0985 PROCESSOR NAME UNKNOWN

### Meaning

Possible reasons:
1. The processor name given when defining the printer is invalid.
2. The processor is not connected to the host.

### Response

Case 1: Request the device administrator or the system support
to check the printer definition.
Case 2: Request the operator to connect the processor.

## SRO0986

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0986 RSO PRINTER NOT AVAILABLE OR CANNOT BE SUPPORTED BY 'PDN'

### Response

Either set the remote printer in an operable state or request the system
support to modify the PDN generation for this printer.

## SRO0987

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0987 SRAM DID NOT RECEIVE PRINT ACKNOWLEDGMENT FOR DEVICE '(&00)'. CONTACT THE SYSTEM SUPPORT STAFF.

### Meaning

Possible reasons:
- The printer is unable to send a print acknowledgment.
- The printer was stopped too long while printing a block.
- The print acknowledgment has been lost.
- The open connection has been lost by the network.
(&00) : device name

### Response

Contact the system support or if necessary maintenance staff.

## SRO0988

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0988 FORMAT ERROR

### Meaning

The message contained one or more format error(s), but has
nevertheless been printed.

## SRO0989

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0989 CONNECTION WITH RSO PRINTER HAS BEEN SEVERED

### Meaning

Possible reason:
One of the following commands has been entered:
/BCLOSE
/BCEND
/DADM DAS,<printer name>

### Response

Contact the system support or the operator to reestablish the
connection.

## SRO0990

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0990 SOCKETS : I/O ERROR

### Meaning

The message could not be transmitted to the transport system.

### Response

Contact the network administration.

## SRO0991

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0991 SOCKETS : INACTIVE NETWORK

### Meaning

A socket operation was attempted on an inactive network.

### Response

Contact the network administration.

## SRO0992

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0992 SOCKETS : NETWORK CURRENTLY INACTIVE. RETRY LATER

### Meaning

The network dropped connection on reset and is currently inactive.

### Response

Check whether the LAN has been started and switched on
your system.
Retry later or contact the network administration.

## SRO0993

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0993 PRINT JOB ABORTED BY LPD-SERVER.

### Meaning

The Lpd-server (managing the printer) has aborted the print job
due to one of the following reasons depending on the rightmost
value of ERCOD field :
01 : -lpd-printer-name (specified in RSO printer definition) doesn't
exist in BSD/LPD server's printcap file or
-spoolin/queuing not enabled for the lpd-printer-name (specified
in RSO printer definition) or
-local port (specified in RSO printer definition) invalid for the
BSD/LPD server
02 : -lack of memory on the BSD/LPD server
Ask the network administrator to check the lpd-server
configuration and lpd-printer status.

## SRO0994

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO0994 Print Job scheduled on IPP printer has been aborted.

### Meaning

The Ipp server (managing the printer) has aborted the print job
due to one of the following reasons depending on the leftmost
value of ERCOD field:
FC: Error reported by the HTTP server
FD: Error reported by the IPP server.
The status code is in the two rightmost bytes.
A full description of the meaning of the status code is
available in the corresponding RFCs.

### Response

Ask the network administrator to check the IPP printer configuration.

## SRO1000

Destination: USER-TASK, CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO1000 DCAM APPLICATION 'OPEN' REQUESTED BY SRAM ABORTED WITH DCAM RETURN CODE FDB=X'(&00)'. REPLY (R=RETRY; T=TERMINATE)

### Meaning

(&00): the relevant bytes of the DCAM return code.

### Response

R: try again
T: terminate.
Contact the network administrator if required.

## SRO1001

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO1001 POSSIBILITY OF DOUBLE PRINTING

### Meaning

This message is sent due to the printer status.
Possibly RSO must repeat the printout.
Possible reasons:
- the printer was in the STOP state when printing began, i.e.
the printout has not actually been duplicated
- the printer was in the STOP state during printing or at 'end of paper',
i.e. the printout has been duplicated
- the task was cancelled in the STOP state or there was no more paper, i.
e.
the printout has not actually been duplicated.

### Response

Check the printout.

## SRO1002

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO1002 RETURN CODE '(&01)' FOR '(&02)' WHILE PROCESSING MACRO '(&00)'. PROCESSING ABORTED. TAKE DUMP

### Meaning

A macro call (&00) failed with the return code (&01).
(&02): last parameter processed by the macro.

## SRO1003

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO1003 RETURN CODE '(&01)' FOR MODULE OR PRINTER NAME '(&02)' WHILE PROCESSING MACRO '(&00)'. PROCESSING CONTINUES

### Meaning

A macro call (&00) failed with the return code (&01).
(&02): module or printer name

## SRO1004

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO1004 At least one RSO system device not activated. The IPP printer name prefix has been changed.

### Meaning

The IPP printer name prefix has been changed between the two RSO
sessions. Because of the warm start-up, the remaining jobs are kept
but will not be scheduled.

### Response

Either cancel the concerned print-jobs or reinstall the old prefix
temporarily in order to print out these jobs.

## SRO1007

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO1007 ERROR X'(&00)' DURING (&01) FOR (&02)

### Meaning

An error occurred during macro processing for the specified memory pool.
(&00): return code
(&01): macro name
(&02): memory pool name.

## SRO1008

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO1008 ERROR RETURN CODE X'(&00)' DURING '(&01)' PROCESSING FOR '(&02)'

### Meaning

An error occurred when processing the macro for the given event item.
(&00): return code
(&01): macro name
(&02): event item name.

## SRO1009

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO1009 Sockets error '(&00)' during a sockets function call.

### Meaning

Sockets error '(&00)' occurred when performing a sockets function.

### Response

Contact the network administration.

## SRO1010

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO1010 ERROR RETURN CODE X'(&00)' DURING INTERNAL RSO PROCESSING

### Meaning

An error has occurred during the processing of the TMODE or VSVI1 macro.

### Response

Contact the system support.

## SRO1011

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO1011 OpenSSL error '(&00)'during an OpenSSL function call.

### Meaning

OpenSSL error '(&00)' occurred when performing an OpenSSL function.

### Response

Ask the network administrator to check the IPP printer configuration.

## SRO2000

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2000 'ACTION' TERMINATED SUCCESSFULLY

### Meaning

This message indicates successful execution of the ACTION when no further
screen is to be displayed.

## SRO2001

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2001 SELECTED ACTION ILLEGAL

### Meaning

The selected ACTION is not in the list displayed on the screen.

### Response

Select a valid ACTION.

## SRO2002

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2002 SELECTED DEVICE TYPE '(&00)' NOT MANAGED

### Response

Select another device type.

## SRO2003

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2003 NO DEVICE OF TYPE '(&00)' EXISTS FOR THE ADMINISTRATOR

### Meaning

You are not device administrator of at least one device
of type (&00).

### Response

Select another device type.

## SRO2004

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2004 ERROR WHEN ACCESSING SPOOL.PARAMETERS FILE'

### Response

Terminate RSOSERVE and verify the existence, the structure or
the access rights of SPOOL.PARAMETERS file.

## SRO2005

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2005 ERROR WHEN ACCESSING FILE '(&00)'

### Meaning

Terminate RSOSERVE and verify the existence of the structure
of parameter file (SYSPAR.RSO).

### Response

Terminate RSOSERVE and verify the existence of the structure of
parameter file (logical id = SYSPAR).

## SRO2006

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2006 TO ENTER THE 'REMOVE' 'ACTION': HIT THE <F1> KEY

### Response

To enter the 'REMOVE' 'ACTION' you must hit the <F1> key and not the
<DUE1> key.

## SRO2007

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2007 FILE '(&00)' IS PASSWORD-PROTECTED

### Meaning

Possible reasons:
- the user has tried to open a file protected by a password
- the specified password is invalid.
(&00): name of the file being processed.

### Response

Enter another file name or correct the PASSWORD.

## SRO2008

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2008 INSUFFICIENT PRIVILEGE FOR SELECTED 'ACTION'

### Meaning

Either the user is not authorized to execute the selected
ACTION or he has tried to use restricted operands connected
with the selected ACTION.

### Response

In interactive mode, select another ACTION or withdraw the restricted
operands.

## SRO2009

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2009 DEVICE RELEASE FORCED BY A DEVICE ADMINISTRATOR

### Response

Restart the device or select another one.

## SRO2010

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2010 DMS ERROR '(&00)' OF TYPE '(&01)' ON FILE '(&03)' WHILE PROCESSING THE MACRO '(&02)'. IN SYSTEM MODE: HELP-MSG DMS(&00).

### Meaning

For more detailed information about the DMS error enter the command
/HELP-MSG in system mode or see the BS2000 manual 'System Messages'.
(&00): DMS return code
(&01): DMS error type
(&02): DMS macro type.
(&03): name of the file being processed.

### Response

React in accordance with the DMS return code.

## SRO2011

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2011 DMS ERROR '(&00)' ON FILE '(&02)' WHILE PROCESSING THE MACRO '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.
(&00): DMS return code
(&01): DMS macro type
(&02): name of the file being processed.

## SRO2012

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2012 NO MEMBERS DEFINED FOR FORM '(&00)'. 'ACTION' REJECTED

### Meaning

(&00): form name.

### Response

Correct the form name.

## SRO2014

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2014 NO CLASS 5 MEMORY AVAILABLE. PROCESSING NOT POSSIBLE

### Meaning

The error was returned during the request memory.

### Response

Terminate RSOSERVE.

## SRO2016

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2016 FILE DOES NOT CONTAIN ANY DATA OF THE SPECIFIED DATA TYPE

### Meaning

The RSOFILE file, the parameter file (logical id = SYSPAR.USER)
or the DSR library contains no data of the selected data type.

## SRO2017

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2017 PRINTER SEQUENCE NUMBER OUT OF RANGE.

### Meaning

The specified sequence number is not contained in the
column "#" displayed on the screen.

### Response

Enter one of the numbers displayed in the column "#".

## SRO2018

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2018 INVALID PASSWORD VALUE FOR PRINTER. REPLY (<N>=1 THROUGH 64000)

## SRO2019

Destination: USER-TASK, CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO2019 '(&00)' FIELD VALUES MAY ONLY BE 'Y'=YES; 'N'=NO

### Meaning

The value for the (&00) field is either 'Y' or 'N'.
(&00): OVERWRITE, ERASE or ALL.

### Response

OVERWRITE = Y: duplicate records are overwritten.
N: duplicate records are not overwritten.
ERASE = Y: the specified file is cleared before use.
N: it is not cleared.
ALL = Y: all the records of the specified type are treated.
N: only some records are treated.

## SRO2020

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2020 SPECIFIED FONT NAME NOT DEFINED

### Response

Either select an existing font name
or define the font name before character set creation.

## SRO2021

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2021 DEVICE ERROR '(&00)': '(&01)'

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one is
displayed.
(&00): device error code
(&01): short explanatory text.

## SRO2023

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2023 (&00) FILE NAME DOES NOT FOLLOW THE CONSTRUCTION RULE OF (&01) FILES

### Meaning

The specified file name is invalid.
Correct file name: $userid.xxxx.RSOFILE or
$userid.xxxx.NDFILE.
(&00): type of file (INPUT or OUTPUT)
(&01): sort of file (NDFILE or RSOFILE).

### Response

Correct the file name.

## SRO2024

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2024 INVALID DIRECTORY NAME '(&00)'. 'ACTION' REJECTED

### Meaning

The directory name
- contains the character ',' ';' '\' or ' '
- begins with the character '-'
- is longer than 24 characters.
(&00): invalid directory name.

### Response

Enter a valid directory name.

## SRO2025

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2025 INVALID '(&00)' FILE NAME '(&01)'. STATEMENT REJECTED

### Meaning

The FILE NAME contains the character ',' ';' '\' '-' or ' '.
(&00): file type: INPUT or OUTPUT or PRINTER or BS2000 or NEW
(&01): name of the file being processed.

### Response

Correct the FILE NAME and try again.

## SRO2026

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2026 AT LEAST ONE MEMBER NAME IS NOT ALPHANUMERIC

### Response

Correct the member name(s).

## SRO2027

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2027 SAME MEMBER NAME SPECIFIED MORE THAN ONCE. CORRECT MEMBER NAME(S)

## SRO2028

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2028 LIST OF MEMBER NAMES IS EMPTY

### Response

Enter at least one member name or select another action.

## SRO2030

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2030 WARNING: AT LEAST ONE FONT NO LONGER DEFINED IN FILE '(&00)'

### Meaning

The font names represented by '??????????' are no longer defined in the
file (&00). This may cause problems in subsequent print operations.

### Response

Possible measures:
- Change the name of the font associated with the concerned character set,
- define the font again in file (&00) or
- remove the character set.

## SRO2031

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2031 ENTERED FILE TYPE IS NOT SAM OR ISAM

### Meaning

The specified input file type is invalid.

### Response

Enter 'S' or 'I'.

## SRO2032

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2032 FILE '(&00)' DOES NOT EXIST

### Meaning

(&00): file name.

### Response

In interactive mode, enter another file name or select another 'ACTION'.

## SRO2033

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2033 FILE '(&00)' NOT SAM OR ISAM

### Meaning

(&00): file name.

### Response

Enter another file name or select another 'ACTION'.

## SRO2034

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2034 BLOCK SIZE OF FILE '(&00)' NOT '(STD,1)'

### Meaning

(&00): file name.

### Response

Enter another file name or select another 'ACTION'.

## SRO2035

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2035 FILE '(&00)' DOES NOT HAVE VARIABLE RECORD LENGTH

### Meaning

(&00): file name.

### Response

Enter another file name or select another 'ACTION'.

## SRO2036

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2036 KEY LENGTH OF FILE '(&00)' NOT '8'

### Meaning

(&00): file name.

### Response

Enter another file name or select another 'ACTION'.

## SRO2037

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2037 KEY POSITION OF FILE '(&00)' NOT '5'

### Meaning

(&00): file name.

### Response

Enter another file name or select another 'ACTION'.

## SRO2038

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2038 BS2000 FILE '(&00)' EMPTY

### Meaning

(&00): file name.

### Response

Enter another file name or select another 'ACTION'.

## SRO2039

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2039 <K1> <LZE> <EM> <AM> <DU2> FORBIDDEN

### Meaning

One of the specified keys has been pressed but is not
recognized by the program; the input data is not processed.

### Response

Reenter the lost data and press the data transmission key.

## SRO2040

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2040 RSO ERROR. DEVICE MANAGEMENT NOT POSSIBLE

### Meaning

A RSO error has occurred during the selected device management function.

### Response

Contact the system support for further information.
Select another device or terminate RSOSERVE.

## SRO2041

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2041 DUE TO DCAM ERROR '(&00)' NO MANAGEMENT POSSIBLE

### Meaning

A DCAM return code was received during a printer operation.
(&00): DCAM return code.

### Response

React in accordance with the DCAM return code.

## SRO2042

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2042 INTERNAL ERROR TYPE '(&00)' '(&01)'

### Meaning

An error was returned by the device access interface.
(&00): type of the error (LEVCO, SOLSIG, POSSIG, RSO SVC)
(&01): additional return code, if any.

### Response

Contact the system support.

## SRO2043

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2043 CURRENT DEVICE STATE IS '(&00)'. MANAGEMENT NOT POSSIBLE

### Meaning

The current device state does not permit a connection to be set up.
(&00): device state (D, S, A, T, M, I, W).

### Response

React in accordance with the device state.

## SRO2044

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2044 PRINTER NOT STARTED. MANAGEMENT NOT POSSIBLE

### Meaning

The selected device has not been started.

### Response

Enter a start command for the device.

## SRO2045

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2045 MEMORY POOL FULL. RETRY LATER

### Meaning

The maximum number of simultaneous users has been reached.

## SRO2046

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2046 DEVICE ACCESS ERROR '(&00)'

### Meaning

A system error has occurred during a printer operation.
(&00): Complementary information, if available.

### Response

Contact the system support.

## SRO2047

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2047 SELECTED '(&00)' NAME '(&01)' DOES NOT EXIST. ACTION REJECTED

### Meaning

The name selected for the DELETE/RENAME/COPY/SHOW ACTION
does not exist.
(&00): data type
(&01): data name.

### Response

Correct the name.

## SRO2048

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2048 SELECTED '(&00)' NAME '(&01)' ALREADY EXISTS. ACTION REJECTED

### Meaning

The name selected for the ADD ACTION already exists.
(&00): data type
(&01): data name.

### Response

Correct the name.

## SRO2049

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2049 NON-HEXADECIMAL CHARACTER AT LINE '(&00)', COLUMN '(&01)'

### Meaning

The table must contain hexadecimal codes ( X'00' -> X'FF' ).
(&00): table line number ( 0 -> F )
(&01): table column number ( 0 -> F ).

### Response

Correct the input.

## SRO2050

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2050 INVALID TABLE STRUCTURE IN LINE '(&00)', COLUMN '(&01)'

### Meaning

The table must contain codes separated by a blank character.
At line (&00) and column (&01), the separation character is not a blank.
(&00): table line number ( 0 -> F )
(&01): table column number ( 0 -> F ).

### Response

Correct the input.

## SRO2051

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2051 REQUIRED '(&00)' NAME FIELD NOT FILLED IN

### Meaning

The required name has not been specified but, for this specified ACTION,
the data selection can only be done by filling in this area.
(&00): data type.

### Response

Enter a name.

## SRO2052

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2052 SELECTED '(&00)' NAME '(&01)' INVALID

### Meaning

The selected name does not match the expected type
(alphanumeric, alphabetic, numeric).
(&00): data type
(&01): data name.

### Response

Correct the name.

## SRO2053

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2053 SPECIFIED ESCAPE VALUE INVALID

### Meaning

Possible causes:
- The frame number is not in the range 1 through 7 or
- the device configuration number is not 1, 2 or 3.

### Response

Correct the erroneous value(s).

## SRO2054

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2054 EMPTY STRING

### Meaning

The data string to be sent to the printer is empty.

### Response

Enter appropriate text/command in the string or select a different action.

## SRO2055

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2055 SYSTEM ERROR DURING IMPORT OR EXPORT PROCESSING

### Response

Contact the system support.

## SRO2056

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2056 BS2000 FILE '(&00)' ALREADY EXISTS AND 'OVERWRITE=N' IS SPECIFIED

### Meaning

The user has tried to export a file to BS2000. The attempt failed because
- the OVERWRITE field in the mask is set to NO and
- the specified file name already exists in the BS2000.
(&00): file name.

### Response

Enter a different file name for the file to be exported or
set the OVERWRITE field to YES.

## SRO2057

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2057 SELECTED NAME IS NOT A DIRECTORY NAME

### Meaning

The required ACTION is LIST directory, but the specified
file name is not the name of a directory.

### Response

Enter another file name.

## SRO2058

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2058 REQUIRED ACTION ONLY POSSIBLE FOR DIA/PROLOG/EPILOG/SYMBOL

### Response

Select another action.

## SRO2059

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2059 INVALID FILE STRUCTURE FOR FILE '(&00)'

### Meaning

The header of the file to be imported does not match
the standard header of the selected data type.
(&00): name of the file being processed.

### Response

Correct the file header or select another data type.

## SRO2060

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2060 INVALID CODE '(&00)' IN ESCAPE SEQUENCE

### Meaning

A non-hexadecimal character was encountered in an escape sequence.

### Response

Correct the escape sequence.

## SRO2061

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2061 INVALID OR AMBIGUOUS PASSWORD

### Meaning

The specified password is
- invalid (hexadecimal password contains a non-hexadecimal character)
- ambiguous (both password types are filled in: hexadecimal and
non-hexadecimal).

### Response

Correct the password.

## SRO2062

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2062 SPECIFIED ESCAPE SEQUENCE ALREADY IN USE

### Meaning

The escape sequence associated with the font to be
added or modified is already being used for another font.

### Response

Modify the escape sequence.

## SRO2063

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2063 RSO NOT AVAILABLE. MANAGEMENT NOT POSSIBLE

### Meaning

The RSO subsystem is not initialized or has been deleted.

### Response

Create the RSO subsystem.

## SRO2065

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2065 NO RESPONSE FROM DEVICE

### Meaning

Within the predefined wait time no response has been received from the
managed device.

### Response

Contact the system support.

## SRO2066

Destination: USER-TASK, CONSOLE Routing code: N Weight: 98

Warranty : NO

SRO2066 TERMINATE MIGRATION? REPLY (Y=YES; N=NO)

### Meaning

The K2 interrupt key was hit during the migration processing.
The user is asked whether migration should be terminated or resumed.

### Response

Y: migration processing will be terminated
N: migration processing will be continued.

## SRO2067

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2067 END OF LIST REACHED

### Meaning

This message is output after a NEXT ACTION. The message informs the
user that he has already reached the end of the list.

## SRO2068

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2068 BEGINNING OF FILE REACHED

### Meaning

This message is output after a PREVIOUS ACTION. The message informs the
the user that he has already reached the beginning of the file.

## SRO2069

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2069 INVALID VALUE FOR FIELD NAME '(&00)'

### Meaning

(&00): field name: LINE NUMBER or CHANNEL or LPI

## SRO2071

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2071 ERROR DURING CONTINGENCY PROCESSING

### Meaning

An error occurred during the enabling or disabling
of the migration interrupt contingency.

### Response

Contact the maintenance staff.

## SRO2075

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2075 SPECIFIED LEVEL ALREADY REACHED

### Meaning

A Lx command was entered when the user was already at level x.

## SRO2076

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2076 SPECIFIED MODEL '(&00)' DOES NOT EXIST. 'ACTION' REJECTED

### Meaning

(&00): name of the MODEL.

## SRO2077

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2077 SELECT ONE RECORD TYPE

### Meaning

This message is output in the SYSTEM RSOFILES MANAGEMENT (RSOFILES merge)
when no record type has been selected and the user does not want to treat
all the record types (ALL field = N).

## SRO2078

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2078 SELECT ONLY ONE RECORD TYPE

### Meaning

This message is output in the SYSTEM RSOFILES MANAGEMENT (RSOFILES merge)
when several record types have been selected and the user does not want
to treat all the record types (ALL field = N).

## SRO2079

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2079 NAME OF INPUT FILE MUST BE DIFFERENT FROM NAME OF OUTPUT FILE

## SRO2080

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2080 FHS OR MASK OML ACCESS ERROR

### Meaning

An error occurred during the access to the RSOSERVE FHS masks.
OML: Object Module Library
FHS: Format Handling System.

### Response

Make sure RSOSERVE IFG OML is present. If it is present contact the
maintenance staff.
IFG: Interactive Format Generator.

## SRO2081

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2081 NO RECORD OF TYPE '(&00)' MARKED

### Meaning

There are two types of record selection: either by specifying a value to
the field SELECTED NAME or by marking an element in a record list with
'X'.
If, in a processing, these two types of selection are possible, precedence
is given to the field SELECTED NAME. If this field is not filled in, at
least one record must be marked.
(&00): data type.

## SRO2082

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2082 SEVERAL '(&00)' RECORDS HAVE BEEN MARKED

### Meaning

This message is output in device management when the ACTION is
MODIFY or SHOW a FONT record. The selection can be done by
giving a name or by entering the 'X' character in front of
the FONT name. For these two ACTIONs, only one record can be selected.
(&00): data type: FONT.

## SRO2083

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2083 INVALID DEVICE SUBTYPE SPECIFIED

## SRO2084

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2084 'LOOP' LENGTH NOT EQUAL TO 'TOTAL LENGTH'

### Meaning

The loop length resulting from the LINE and LPI specification is different
from the loop length given in the TOTAL LENGTH field.

### Response

Correct LINE and LPI specifications.

## SRO2085

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2085 'LOOP' LENGTH OUT OF RANGE

### Meaning

The loop length resulting from the LINE and LPI specifications is not
within the range: 1 inch <= loop length <= 32 inches.

### Response

Correct LINE and LPI specifications.

## SRO2086

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2086 'TOTAL LENGTH' OUT OF RANGE

### Meaning

The TOTAL LENGTH value is not within the range:
1 inch <= loop length < 32 inches.

### Response

Correct TOTAL LENGTH value.

## SRO2087

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2087 FOR RECORD OF TYPE '(&00)' SELECTED NAME '(&01)' DOES NOT EXIST. (&02) RECORD(S) TREATED. PROCESSING ABORTED

### Meaning

This message is issued when several records are treated one after
the other, which have been marked with the 'X' character in a record list.
(&00): data type
(&01): name of the record
(&02): number of successfully treated records.

## SRO2088

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2088 FOR RECORD OF TYPE '(&00)' SELECTED NAME '(&01)' ALREADY EXISTS. (&02) RECORD(S) TREATED. PROCESSING ABORTED

### Meaning

This message is issued when several records are treated one after
the other, which have been marked with the 'X' character in a record list.
(&00): data type
(&01): name of the record
(&02): number of records treated successfully.

## SRO2099

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2099 RSOSERVE ENDED

## SRO2100

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2100 I/O ERROR OR EOF ON SYSDTA. PROCESSING ABORTED

### Meaning

An error occurred during the processing of the RDATA macro.

## SRO2101

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2101 STATEMENT SEQUENCE ERROR

### Meaning

An unexpected statement was encountered.

## SRO2102

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2102 FOR RECORD TYPE '(&00)' SPECIFIED NAME '(&01)' IS INVALID

### Meaning

Possible causes:
- the specified name does not match the expected type (alphanumeric,
numeric, alphabetic) or the name is too long.
- the name is too long. Maximum name length for the record type
LOOP, CHARACTER-IMAGE and IDENTIFIER: 3 characters
BAND-ID : 4 characters
TRANSLATION-TABLE: 8 characters.
(&01): name of the record.

### Response

Correct the name.

## SRO2103

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2103 OPERAND(S) IN STATEMENT SPECIFIED MORE THAN ONCE

### Meaning

At least one operand in the statement is duplicated.

### Response

Correct the statement.

## SRO2104

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2104 OPERAND '(&00)' MISSING IN STATEMENT

## SRO2105

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2105 RECORD OF TYPE '(&00)' WITH NAME '(&01)' ALREADY EXISTS IN THE FILE. RECORD NOT OVERWRITTEN

### Meaning

(&00): type of the record: LOOP, CHARACTER-IMAGE, BAND-ID,
TRANSLATION-TABLE
(&01): name of the record.

## SRO2106

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2106 SOME RECORDS NOT COPIED DUE TO DUPLICATION

### Meaning

Some records of the INPUT file already exist in the OUTPUT file.
These records are not overwritten.

## SRO2107

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2107 INVALID STATEMENT

### Meaning

An unknown statement was entered.

## SRO2108

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2108 INVALID HEXADECIMAL CODE

### Meaning

The CODE operand does not contain an hexadecimal character.

## SRO2109

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2109 'LOOP' GENERATION MODE TERMINATED

### Meaning

GENLOOP has been terminated by means of a BACK or HALT statement.

## SRO2111

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2111 BEFORE THIS 'ACTION' ENTER A 'LIST-INPUT ACTION'

### Meaning

For this ACTION, the record selection must be done by marking the elements
in the list describing the contents of the input file.
This message is issued when it is the output file contents which is
displayed.

## SRO2112

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2112 BEFORE THIS 'ACTION' ENTER A 'LIST-OUTPUT ACTION'

### Meaning

For this ACTION, the record selection must be done by marking the elements
in the list describing the contents of the output file.
This message is issued when it is the input file contents which is
displayed.

## SRO2113

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2113 RECORD TYPE '(&00)' WITH NAME '(&01)' WRITTEN

### Meaning

(&00): record type: TRANSLATION-TABLE, BAND-ID, CHARACTER-IMAGE
(&01): record name.

## SRO2114

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2114 RECORD TYPE '(&00)' DOES NOT EXIST

### Meaning

(&00): record type: LOOP, CHARACTER-IMAGE, BAND-ID, TRANSLATION-TABLE.

## SRO2115

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2115 SYNTAX ERROR IN FILE NAME '(&00)'

### Meaning

Error in the file name format.

## SRO2116

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2116 INVALID HEXADECIMAL CODE AT POSITION '(&00)'

### Response

Correct the input.

## SRO2117

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2117 MISSING EBCDIC STRING TERMINATOR

### Meaning

An EBCDIC string in the data is not terminated with the ')' character.

### Response

Correct the input.

## SRO2118

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2118 INVALID ESCAPE SEQUENCE LENGTH

### Meaning

The length of the entered ESCAPE SEQUENCE - after conversion
to hexadecimal format - is equal to zero or greater than 256 characters.

### Response

Correct the input.

## SRO2119

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2119 UNEXPECTED DATA FOLLOWS THE ESCAPE SEQUENCE TERMINATING CHARACTER

### Meaning

The ESCAPE SEQUENCE terminating character (a blank or an underscore not
enclosed in parentheses) is followed by more data.

### Response

Correct the input.

## SRO2120

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2120 UNEXPECTED DATA READ

### Meaning

Data was read although the preceding data was not terminated with the '-'
continuation character.

## SRO2121

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2121 INVALID IGNORE SYNTAX

### Meaning

To ensure that an ML5GLOOP screen line is ignored by the processing,
all of its fields must be filled with zeros.

### Response

Correct the input.

## SRO2124

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2124 UNSPECIFIED LINE INTERVALS

### Meaning

The description of the LOOP on the ML5GLOOP screen is incomplete.
Some line intervals are not specified.

### Response

Correct the input.

## SRO2125

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2125 'ACTION' TERMINATED SUCCESSFULLY. (&00) RECORD(S) TREATED

### Meaning

(&00): the number of records which were treated.

## SRO2126

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO2126 ERROR OCCURRED DURING 'XMCLP' MACRO ACCESS TO SPOOL PARAMETERS

### Meaning

An error occurred while performing the /SHOW-SPOOL-FORM or
/SHOW-SPOOL-CHARACTER-SETS command through the XMCLP macro call.

### Response

Contact the system support.

## SRO2127

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO2127 'FORM-NAME' AND 'CHARACTER-SET-NAME' FIELDS CANNOT BE FILLED TOGETHER FOR THIS 'ACTION'

### Response

Correct the input.

## SRO2128

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO2128 EITHER 'FORM-NAME' OR 'CHARACTER-SET-NAME' FIELD MUST BE FILLED FOR THIS 'ACTION'

### Response

Correct the input.

## SRO2129

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO2129 '(&00)' WITH NAME '(&01)' NOT FOUND IN SPOOL.PARAMETERS FILE

### Meaning

(&00): record type
(&01): record name.

## SRO2130

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO2130 '(&00)' ERROR WHEN PROCESSING THE 'SPSINFO' MACRO

### Meaning

For more detailed information about the error code see BS2000 manual
'SPSERVE'.
(&00): error code of macro SPSINFO.

### Response

Contact the system support.

## SRO2131

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO2131 '(&00)' NOT SUPPORTED BY SPECIFIED DEVICE TYPE

### Meaning

(&00): - horizontal density
- vertical control density
- rotational control density
- vertical and rotational control density.

## SRO2132

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO2132 NO ROTATIONAL CHARACTER SET ASSOCIATED WITH FORM

## SRO2133

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO2133 'ACTION' NOT PERMITTED FOR SPECIFIED DEVICE TYPE

## SRO2134

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SRO2134 INVALID KEY PRESSED

### Response

Press the F1 key in the case of a REMOVE action or DUE1 in other cases.

## SRO2201

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2201 GENERATION OF 'LOOPS' NOW IN EFFECT

### Meaning

GENLOOP mode was called.

## SRO2202

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2202 GENERATION OF TRANSLATION TABLES NOW IN EFFECT

### Meaning

Translation table generation mode was called.

## SRO2204

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2204 NO FILES ASSIGNED

### Meaning

The HELP-FILE statement was issued and no files were assigned.

## SRO2206

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2206 INVALID OPERAND IN STATEMENT 'HELP'

### Meaning

This operand must be a statement name (to obtain information about a
statement) or the FILE keyword (to know which files are assigned).

### Response

Correct the statement.

## SRO2207

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2207 KEYWORD OPERAND 'LOOP' MISSING IN SPECIFIED STATEMENT

### Response

Correct the statement.

## SRO2208

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2208 OPERAND 'NEWNAME' MISSING IN SPECIFIED STATEMENT 'RENAME'

### Response

Correct the statement.

## SRO2211

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2211 NO '(&00)' FILE ASSIGNED

### Meaning

No file of the specified type has been assigned.
(&00): file type, INPUT, OUTPUT or WORK.

## SRO2212

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2212 INVALID NAME OF 'MODEL' OPERAND IN STATEMENT 'LOOP'

## SRO2214

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2214 SYNTACTICAL ERROR IN KEYWORD '(&00)'

### Meaning

(&00): invalid keyword.

## SRO2216

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2216 (&00) 'LOOPS' PRINTED TO SYSLST

### Meaning

The statement PRINTWORK or PRINTIN or PRINTOUT has been completed.
(&00): number of loops printed on SYSLST.

## SRO2217

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2217 SPECIFIED 'LOOP' PRINTED TO SYSLST

### Meaning

The statement PRINTWORK or PRINTIN or PRINTOUT has been completed.

## SRO2218

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2218 SYNTACTICAL ERROR IN OPERAND 'CLEAR'

## SRO2222

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2222 SPECIFIED 'LOOP' NOT DEFINED IN WORK FILE

### Response

Use a defined loop.

## SRO2223

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2223 FILE DOES NOT EXIST

### Meaning

A statement that implies the presence of a particular
file was entered when this file was not yet assigned.

## SRO2224

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2224 OPERAND 'FILE' ILLEGAL WITHOUT OPERAND 'MODEL'

### Meaning

In statement LOOP the operand FILE is specified but not the operand MODEL.

### Response

Correct the statement.

## SRO2225

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2225 CHANNEL 1 NOT DEFINED

### Meaning

Channel 1 was not set in any line.
As channel 1 is the criterion for starting a new page for SPOOL (if SPACE
not equal to E), it must be specified at least once in every loop record.

## SRO2226

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2226 LAST LINE RESERVED FOR CHANNEL 12

### Meaning

No channel can be defined on the last line of the loop because SPOOL sets
the channel 12 on this line at loading time.

## SRO2227

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2227 'LOOP' AND 'NEWNAME' MUST BE DIFFERENT IN STATEMENT 'RENAME'

### Meaning

The same name is used to define loop name and new loop name in the RENAME
statement.

### Response

Use different names.

## SRO2228

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2228 SPECIFIED LINE SPACING FOR OPERAND 'D' MUST BE 3, 4, 6, 8, 10, 12, 15 OR 20 LPI

### Meaning

LPI: Lines Per Inch.

## SRO2229

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2229 OPERAND 'D' INCOMPATIBLE WITH OPERAND 'MODEL' IN STATEMENT 'LOOP'

### Meaning

Both the operands MODEL and D were specified in statement LOOP.

## SRO2230

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2230 LINE DENSITY SELECTED IN 'LINE' STATEMENT CAUSES VIOLATION OF 'LOOP' BOUNDARY

### Response

Correct the D operand in the LINE statement.

## SRO2231

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2231 SPECIFIED CHANNEL NOT IN PERMISSIBLE RANGE FROM 1 THROUGH 11

## SRO2232

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2232 SPECIFIED LINE NUMBER NOT IN PERMISSIBLE RANGE FROM 1 THROUGH 500

## SRO2233

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2233 'NEWNAME' OPERAND MISSING IN 'RENAME' STATEMENT

### Meaning

No new loop name is given in statement RENAME.

### Response

Correct the RENAME statement.

## SRO2234

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2234 'LENGTH' OR 'MODEL' OPERAND MISSING IN 'LOOP' STATEMENT

### Response

Correct the LOOP statement.

## SRO2235

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2235 'LENGTH' AND/OR 'FR' OPERAND NOT IN PERMISSIBLE RANGE

### Meaning

The value of the LENGTH operand in the LOOP statement was not in the
range 1 to 25 and/or that of the FR operand was not in the range 0 to 5
(units of 1/6 inch).

## SRO2236

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2236 SPECIFIED LINE NUMBER GREATER THAN 'LOOP' LENGTH. LAST LINE: (&00)

### Meaning

The line number specified in the LINE statement is greater than the LOOP
length.
(&00): number of the last line of the loop.

### Response

Correct the statement.

## SRO2237

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2237 SPECIFIED LENGTH FOR 'LOOP': (&00) INCHES, FR=(&01). 'LOOP' LENGTH IN LAST LINE EXCEEDED BY (&02)/120 INCH

### Meaning

The length of the loop resulting from loop creation is different from the
length calculated from the LENGTH and FRACTION values specified at the
beginning of the loop creation.
(&00): specified loop LENGTH
(&01): specified loop FRACTION
(&02): difference between specified loop length and final loop length.

### Response

Correct the loop.

## SRO2238

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2238 FINAL 'LOOP' LENGTH DIFFERENT FROM INITIAL 'LOOP' LENGTH

### Meaning

The length of the loop calculated from the ML5GLOOP screen is different
from the initial length i.e.
- the LENGTH specified in the ML4GLOOP screen (loop creation) or
- the length of the specified MODEL or
- the length of the loop before modification.

### Response

Correct the input.

## SRO2239

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2239 RECORD TYPE '(&00)' NOT SAVED

### Meaning

This message is displayed after a BACK or HALT statement and indicates
that the record type (&00) has been generated but not saved.
(&00): record type: LOOP, CHARACTER-IMAGE, BAND-ID, TRANSLATION-TABLE.

## SRO2241

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2241 'LOOP' COPIED

### Meaning

A confirmation of a COPY statement.

## SRO2242

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2242 'LOOP' RECORD WRITTEN TO '(&00)' FILE

### Meaning

A STORE or COPY statement has been processed successfully.
(&00): WORK or OUTPUT file.

## SRO2243

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2243 'LOOP' RECORD WRITTEN TO OUTPUT FILE

### Meaning

A STORE statement has been processed successfully.

## SRO2244

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2244 FILE '(&00)' CLOSED

## SRO2245

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2245 NORMAL END OF WORK FILE REACHED

### Meaning

A GENALL statement has been processed successfully.

## SRO2246

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2246 FILE NOT OPENED. 'CLOSE' STATEMENT REJECTED

### Meaning

A CLOSE statement was entered for a file that had not been opened.

## SRO2247

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2247 INVALID VALUE FOR 'NEWNAME' OPERAND

### Meaning

Possible reasons:
- The name of the new loop does not match the expected type
(alphanumeric, numeric, alphabetic).
- The value of the NEWNAME operand is too long.

### Response

Correct the NEWNAME operand if necessary.

## SRO2252

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2252 ERROR IN /SHOW-FILE-ATTRIBUTES COMMAND PROCESSING: FILE NOT ASSIGNED

### Meaning

System error.

## SRO2253

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2253 FILE CRITERIA NOT: ISAM, KEYPOS=5, KEYLEN=(&00)

### Meaning

The work or output file assigned by means of ASSIGN cannot be processed.

## SRO2254

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2254 RECORD OF TYPE '(&00)' WITH NAME '(&01)' ALREADY EXISTS IN THE FILE. RECORD WAS OVERWRITTEN

### Meaning

(&00): record type: LOOP
(&01): record name.

## SRO2255

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2255 READ ERROR ON WORK FILE. STATEMENT ABORTED

## SRO2256

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2256 RECORD OF TYPE '(&00)' WITH NAME '(&01)' STORED AS NEW RECORD

### Meaning

The record of type (&00) and with the name (&01) did not exist in
the file. This record has been added to the file.
(&00): record type: LOOP
(&01): record name.

## SRO2257

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2257 KEYWORD MISSING IN STATEMENT

## SRO2258

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2258 HIGHEST LINE REFERENCED WAS (&00) BUT (&01) IS THE LAST LINE

### Meaning

This message is displayed only when, in a LINE statement,
a change in line spacing from 8LPI to 6LPI, causes another
line, previously defined in another LINE statement,
to have a number greater than the last line number.
(&00): referenced line number: 1 -> 500
(&01): loop last line number: 1 -> 500.

## SRO2259

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2259 INVALID 'MODEL' NAME SPECIFIED

## SRO2299

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2299 END OF TRANSLATION TABLE GENERATION MODE

### Meaning

The translation table generation mode was terminated by means of a BACK or
HALT statement.

## SRO2300

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO2300 THERE IS NO DEVICE OF TYPE '(&00)' IN SPOOL.PARAMETERS FILE

### Response

Define a device in the SPOOL.PARAMETERS file with the SPSERVE product.

## SRO3140

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3140 DEVICE ERROR 140: COMMAND SYNTAX ERROR

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3141

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3141 DEVICE ERROR 141: ARGUMENT OUT OF RANGE OR INVALID

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3142

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3142 DEVICE ERROR 142: INTEGER OVERFLOW

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3143

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3143 DEVICE ERROR 143: ACCESS ERROR: STACK UNDERFLOW FOR \POP \END OR \UNTIL

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3144

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3144 DEVICE ERROR 144 : STACK OVERFLOW FOR \PUSH \IF OR \REPEAT

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3145

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3145 DEVICE ERROR 145: TOO MANY REPEAT LOOPS

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3146

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3146 DEVICE ERROR 146: OVERFLOW ON OVERLAP STACK

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3147

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3147 DEVICE ERROR 147: REPEAT UNTIL BLOCK RANGE OVERFLOW

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3148

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3148 DEVICE ERROR 148: INVALID TABLIST

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3150

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3150 DEVICE ERROR 150: FONT NOT AVAILABLE

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3151

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3151 DEVICE ERROR 151: CHARACTER NOT DEFINED IN FONT

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3152

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3152 DEVICE ERROR 152 : NEGATIVE CHARACTER SPACING IN 'PORTRAIT' MODE

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3153

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3153 DEVICE ERROR 153: NEGATIVE CHARACTER SPACING IN LANDSCAPE MODE

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3154

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3154 DEVICE ERROR 154: 'PSEUDO BOLD' REQUESTED WHILE PRINTING IN 'LANDSCAPE' MODE

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3155

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3155 DEVICE ERROR 155: 'PSEUDO ITALIC' REQUESTED WHILE PRINTING IN 'LANDSCAPE' MODE

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3156

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3156 DEVICE ERROR 156: INVALID LANGUAGE TABLE SELECTION

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3157

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3157 DEVICE ERROR 157: FONT OR LANGUAGE TABLE CHECKSUM ERROR

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3158

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3158 DEVICE ERROR 158: TOO MANY FONTS IN MEM-SUBDEVICE

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3159

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3159 DEVICE ERROR 159 : SYMBOL LOAD CHECKSUM ERROR

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3160

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3160 DEVICE ERROR 160: HARDWARE CHARACTER GENERATOR NOT EQUIPPED FOR COLOURS OR LINES

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3170

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3170 DEVICE ERROR 170: OVERLAPPING TEXT SEGMENTS

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3171

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3171 DEVICE ERROR 171: TEXT SEGMENT OUTSIDE OF PAGE BOUNDARIES

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3172

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3172 DEVICE ERROR 172: TOO MANY TEXT SEGMENTS

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3173

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3173 DEVICE ERROR 173: TOO MANY NESTED SEGMENTS

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3174

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3174 DEVICE ERROR 174: INVALID CLOSE SEGMENT

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3175

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3175 DEVICE ERROR 175: ALIGNMENT ERROR

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3176

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3176 DEVICE ERROR 176: UNIT CONVERSION OVERFLOW ERROR

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3180

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3180 DEVICE ERROR 180: MEM-SUBDEVICE IS FULL

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3181

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3181 DEVICE ERROR 181: TOO MANY FILES IN MEM-SUBDEVICE (MAX. 80)

### Meaning

During an operation the printer has detected more than 80 allowed files in
the MEM-subdevice. Eventual the printer has detected further errors but
these errors are not displayed. Only the most serious error is displayed,
in this case the device error 181.

## SRO3182

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3182 DEVICE ERROR 182: FILE IN MEM-SUBDEVICE NOT ACTIVATED (WRONG FILE TYPE OR FILE STATUS)

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3183

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3183 DEVICE ERROR 183: MEM-SUBDEVICE NOT ACTIVATED (WRONG FILE STATUS)

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3184

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3184 DEVICE ERROR 184: FILE NOT FOUND IN MEM-SUBDEVICE (WRONG FILE STATUS)

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3185

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3185 DEVICE ERROR 185: PROTECTED FONT

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3190

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3190 DEVICE ERROR 190: 'COPY' OR 'INCLUDE' SOURCE FILE NOT FOUND

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3191

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3191 DEVICE ERROR 191: COPY DESTINATION FILE ALREADY EXISTS

### Meaning

- An error has been detected by the printer during an operation.
- This message is also displayed when trying to activate a non-existent
file (font, symbol, language table etc.). The activation introduces the
printer to copy the file from the disk storage to the subdevice.
An error has been detected by the printer during this operation.
When more than one error is detected, only the most serious one
is displayed, in this case the device error 191.

## SRO3193

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3193 DEVICE ERROR 193: NO MEM FILE CREATED (INPUT FILE EMPTY OR INVALID FORMAT)

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3195

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3195 DEVICE ERROR 195: USER HAS INSUFFICIENT PRIVILEGE FOR ATTEMPTED OPERATION

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3200

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3200 DEVICE ERROR 200: NO VIC-CARD PRESENT

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3201

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3201 DEVICE ERROR 201: NO PRIVILEGE FOR ATTEMPTED OPERATION

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3204

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3204 DEVICE ERROR 204: DIRECT MEMORY ACCESS ERROR

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3205

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3205 DEVICE ERROR 205: SUBDEVICE NOT AVAILABLE

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3206

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3206 DEVICE ERROR 206: FILE NOT FOUND

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3207

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3207 DEVICE ERROR 207: DISK FULL

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3208

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3208 DEVICE ERROR 208: DUPLICATE FILENAME

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3209

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3209 DEVICE ERROR 209: DISK DATA ERROR, SOURCE FILE NOT FOUND

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3210

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3210 DEVICE ERROR 210: PROCESSING DATA ERROR

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3211

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3211 DEVICE ERROR 211: LAST DIRECTORY NOT FOUND

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3212

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3212 DEVICE ERROR 212: NO DIRECTORY SPECIFICATION FOUND

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3213

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3213 DEVICE ERROR 213: DISK WRITE PROTECTED, FILE NOT CREATED

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3214

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3214 DEVICE ERROR 214: FILE CANNOT BE OPENED

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3215

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3215 DEVICE ERROR 215: FILE CLOSE ERROR

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3216

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3216 DEVICE ERROR 216: FILE ACCESS ERROR

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3217

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3217 DEVICE ERROR 217: BLOCK NOT FOUND

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3218

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3218 DEVICE ERROR 218: EMPTY FILE, NOT CREATED

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3219

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3219 DEVICE ERROR 219: DISK SURFACE ERROR

### Meaning

An error has been detected by the printer during an operation.
When more than one error is detected, only the most serious one
is displayed.

## SRO3999

Destination: USER-TASK, CONSOLE Routing code: N Weight: 99

Warranty : NO

SRO3999 UNDEFINED DEVICE ERROR

### Meaning

When more than one error is detected, only the most
serious one is displayed.

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages