## SDVCOPY

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SDVCOPY Copyright (C) '(&00)' '(&01)' All Rights Reserved

## SDVLOAD

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SDVLOAD Program '(&00)',Version '(&01)' of '(&02)' loaded

## SDV0001

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDV0001 ERROR '(&00)' FROM INTERFACE'(&01)'

### Meaning

(&00) : return code from interface standard header
(&01) : interface name

## SDV0002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDV0002 System interface error. Command rejected. Contact System Support Staff

### Meaning

An error occurred in a system interface and the command can not be
processed.

## SDV0003

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDV0003 ERROR '(&00)' FROM INTERFACE'(&01)'. ERROR LOGGING SEQUENCE NUMBER IS '(&02)'

### Meaning

(&00) : return code from interface standard header
(&01) : interface name
(&02) : error logging sequence number

## SDV0101

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDV0101 CLASS '(&00)' MEMORY REQUEST ERROR

### Meaning

(&00) : memory class

## SDV0102

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDV0102 CLASS '(&00)' MEMORY RELEASE ERROR

### Meaning

(&00) : memory class

## SDV0203

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDV0203 DPRINTSV SUBSYSTEM CAN NOT BE CREATED. SPOOL PARAMETERS INTERNAL VERSION '(&00)' NOT SUPPORTED

### Meaning

(&00) : spool parameters internal version

### Response

Use SPSERVE to migrate the spool parameters up to the supported version.

## SDV0210

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDV0210 DPRINTSV SUBSYSTEM CAN NOT BE STOPPED OR HELD. '(&00)' TASK NOT ACCESSIBLE

### Meaning

The distributed printers can not be stopped.
(&00) : tsn of the task

## SDV0300

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SDV0300 DMS ERROR '(&00)' FROM INTERFACE '(&01)' FOR FILE '(&02)'. FURTHER INFORMATION : /HELP-MSG DMS(&00)

### Meaning

(&00) : DMS error code
(&01) : DMS interface name
(&02) : filename

## SDV0700

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDV0700 SPOOL '(&00)' TASK NOT ACCESSIBLE

### Meaning

Due to a communication problem with a SPOOL task, the SPOOL request is
unsuccessfully terminated.
(&00) : tsn of the task

## SDV2001

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDV2001 INTERNAL ERROR DURING DPRINT CONFIGURATION ACCESS

## SDV9000

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SDV9000 INVALID VALUE IN SUBSYSTEM-PARAMETER OPERAND OF (&00) DPRINTSV COMMAND

### Meaning

Either the subsystem-parameter operand may not be specified or a wrong
value has been specified
(&00) : command name : /START-SUBSYSTEM or /STOP-SUBSYSTEM or
/RESUME-SUBSYSTEM or /HOLD-SUBSYSTEM

### Response

Correct command and retry.

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages