## NBC0001

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0001 IPL CONSOLE NOT DEFINED IN BS2000 - WRONG PATH

### Meaning

CIO-Initialisation fails, due to wrong system generation
Systemcrash is initiated.

## NBC0003

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0003 IPL CONSOLE CANNOT BE DETERMINED - CIO-INITIALISIATION FAILED

### Meaning

$NKBINF reports wrong macro usage after
being called in module NBCUNPD.
Systemcrash is initiated.

## NBC0004

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0004 SYSTEM-INFORMATIONS NOT AVAILABLE FOR CONSOLE-DEVICE - CIO-INITIALIZATION FAILED

### Meaning

A call to system information services terminates with error.
Thus channel-type and CCW-format of at least one console device
cannot be determined.
Systemcrash is initiated.

### Response

Check console configuration.

## NBC0007

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0007 IPL CONSOLE DEVICE NOT GENERATED - CIO-INITIALIZATION FAILED

### Meaning

The IPL Consoledevice cannot be found in BS2000 console configuration
(TIO table). Systemcrash is initiated.

## NBC0008

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0008 SUPPORT OF IPL CONSOLE NOT POSSIBLE - CIO-INITIALIZATION FAILED

### Meaning

Given IPL-console is not defined in BS2000-console-
configuration (TPK-table) and no free (dummy) table-entry
is available to correct the situation, as all dummy-entries
have been already used up via parameterservice.
Wrong input at systemgeneration or at parameterservice.
Systemcrash is initiated.

## NBC0009

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0009 THE IPL CONSOLE CANNOT FIND CORRESPONDING BS2000-SCREEN-IMAGE-BUFFER - CIO-INITIALIZATION FAILED

### Meaning

For the IPL Console (Type 0A = FJ) exists no link to the
corresponding BS2000-Screen-Image-Buffer (SIB).
The IPL-SIB cannot be transfered to the console-SIB.
Systemcrash is initiated.

### Response

This consoletype is no longer supported.

## NBC0010

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0010 OVERFLOW OF THE CIO-RESIDENT-PROGRAM-STACK

### Meaning

Due to a systemerror, overflow of the resident programstack in module
NBSTACK has occurred.
Systemcrash is initiated.

## NBC0011

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0011 KTT-BOURSE-ERROR - (RDATA < SDATA)

### Meaning

Error during reading at the KTT-bourse ( read data < sent data )
KTT takes SNAP-SHOT-DUMP and repeats.

## NBC0012

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0012 KTT-BOURSE-ERROR - INKONSISTENT PARAMETERS AGAIN

### Meaning

The KTT-Bourse-Parameter are inconsistent for the second time.
Systemcrash is initiated.

## NBC0013

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0013 KTT-BOURSE-ERROR - FIRST INCONSISTENCY OF PARAMETERS

### Meaning

KTT takes SNAP-SHOT-DUMP and repeats.

## NBC0014

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0014 KTT-BOURSE-ERROR - WRONG UNIT- OR FUNCTION-NUMBER

### Meaning

Reading at the KTT-bourse is tried with wrong UNIT- or
FUNCTION-number of the macro $NBRSIG.
Systemcrash is initiated.

## NBC0015

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0015 KTT-BOURSE-ERROR - VERSION NOT SUPPORTED

### Meaning

The version of the $NBRSIG-macro used in KTT-task is not supported.
Systemcrash is initiated.

## NBC0016

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0016 KTT-BOURSE-ERROR - ERROR IN BOURSE-DATA-STRUCTURE

### Meaning

This error happens during receiving data at the KTT-bourse.
KTT takes SNAP-SHOT-DUMP and repeats.

## NBC0017

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0017 KTT-BOURSE-ERROR - WRONG BOURSE-ID AGAIN

### Meaning

Due to wrong bourse-ID KTT-task cannot receive data the second time.
Systemcrcash is initiated.

## NBC0018

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0018 KTT-BOURSE-ERROR - WRONG BOURSE-ID

### Meaning

For the first time receiving data at the KTT-bourse is rejected
due to wrong bourse-ID
KTT takes SNAP-SHOT-DUMP and repeats.

## NBC0019

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0019 ORDER FOR KTT-TASK CANNOT BE IDENTIFIED

### Meaning

KTT receives an order with invalid opcode.
KTT takes SNAP-SHOT-DUMP.

## NBC0020

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0020 SYSTEM-ERROR IN KTT ( REGISTER 12 DESTROYED )

### Meaning

Register 12 (Program-manager-entry) is zero due to a system error.
Systemcrash is initiated.

## NBC0021

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0021 CREATION OF KTT-BOURSE FAILED - INCONSISTENT PARAMETERS

### Meaning

The KTT-bourse cannot be created due to inconsistent parameter
at the $NBCREA-call.
Systemcrash is initiated.

## NBC0022

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0022 CREATION OF KTT-BOURSE FAILED - WRONG UNIT- OR FUNCTION-NUMBER

### Meaning

The KTT-bourse cannot be created due to $NBCREA-call
with wrong UNIT- or FUNCTION-number.
Systemcrash is initiated.

## NBC0023

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0023 CREATION OF KTT-BOURSE FAILED - WRONG VERSION

### Meaning

The KTT-bourse cannot be created because the used
version of the $NBCREA-macro is not supported.
Systemcrash is initiated.

## NBC0024

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0024 ENTRY NBRBRSE UNRESOLVED - CIO-INITIALIZATION FAILED

### Meaning

The entry NBRBRSE is unresolved.
So CIO cannot send data to OPERATING.
Systemcrash is initiated.

## NBC0025

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0025 ENTRY NBMBRSE UNRESOLVED - CIO-INITIALIZATION FAILED

### Meaning

The entry NBMBRSE is unresolved.
So CIO cannot send data to EMERGENCY-HANDLER.
Systemcrash is initiated.

## NBC0026

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0026 NO IPL-CONSOLEDEVICE MARKED - CIO-INITIALIZATION FAILED

### Meaning

In BS2000 console device configuration (TIO-table)
no entry marked as IPL console device is found.
Systemcrash is initiated.

### Response

Check in module NBCUNPD supplying the table.

## NBC0027

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0027 ERROR IN BS2000 CONSOLE TABLES DUE TO SYSTEMGENERATION - CIO-INITIALIZATION FAILED

### Meaning

1. Coupling between a TPK-table-entry and the corresponding TIO-table-
entry is not possible, as this entry cannot be found.
Check at systemgeneration for mismatch between TPK- and TIO-tables.
Systemcrash is initiated.
2. At least one entry of the KTT initialization table GENKTT contains an
erroneous device type.
Systemcrash is initiated.

### Response

Only virtual consoles (type Siemens) are affected.

## NBC0028

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0028 BS2000 CONSOLE CONFIGURATION NOT CORRECTLY GENERATED - CIO-INITIALIZATION FAILED

### Meaning

The requested coupling of two console devices (type 64 SKP2) using the
TIO-table entries is not possible, as only one entry is generated.
Systemcrash is initiated.

### Response

Check console configuration data used as input for system generation.

## NBC0029

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0029 DATA-ERROR IN DATA SENT TO OPERATING OR EMERGENCY-HANDLER BY CIO

### Meaning

The data sent to OPERATING or to EMERGENCY-HANDLER by CIO are incorrect
(wrong recipient- or senderfield, or wrong return-codes sent to
EMERGENCY-HANDLER).
CIO takes SNAP-SHOT-DUMP.

## NBC0030

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0030 KTT-TABLE-ERROR - NO MEMORY SPACE

### Meaning

Important configuration tables of KTT task could not be generated, as a
$REQM call has failed.
Systemcrash is initiated.

## NBC0031

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0031 IPL CONSOLE UNKNOWN TO KTT - CIO-INITIALISATION FAILED

### Meaning

The mnemonic for the physical IPL console is not available to KTT
(NO TKP-Table entry with IPL flag found).
The MN should have been transmitted to EMERGENCY-HANDLER.
Systemcrash is initiated.

## NBC0032

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NBC0032 ERROR IN ADDRESSCONVERSION FOR KTT-I/OS

### Meaning

KTT-I/Os are not possible. Systemcrash is initiated.

## NBC0036

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0036 ERROR AT $NKBINF-CALL - CHANNEL TYPE COULD NOT BE UPDATED

### Meaning

A $NKBINF call ended with system error. Thus CIO is not able to update
the channeltype of a console device (type 64, SKP2), which is going to
be attached. Systemcrash is initiated.

## NBC0037

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0037 CHANNEL TYPE CHECK FOR CONSOLE DEVICE PAIR REPORTS MIXED TYPES

### Meaning

After updating the channeltype of a console device pair (type 64, SKP2)
different channel types are reported.
Systemcrash is initiated.

### Response

Serious error at generation of the BS2000 device configuration.

## NBC0038

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0038 TOO MANY CONSOLE DEVICES GENERATED

### Meaning

The BS2000 device configuration consists of more than 224 consol devices
(all console device types as generated in TIO-Table are counted).
Systemcrash is initiated.

### Response

Reduce the number of console devices.

## NBC0050

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0050 CONSOLE-ERROR - TRY AGAIN

### Meaning

LAST CONSOLE INPUT IS TERMINATED WITH ERROR.
INPUT IS IGNORED.

## NBC0051

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0051 TIME-OUT - INPUT IGNORED

### Meaning

LAST CONSOLE-INPUT IS TERMINATED WITH 'TIME-OUT'.
INPUT IS IGNORED.

## NBC0052

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0052 INPUT NULL - IGNORED

### Meaning

LAST CONSOLE-INPUT IS AN EMPTY STRING.
INPUT IS IGNORED.

## NBC0053

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0053 RECIPIENT NOT AVAILABLE - INPUT IGNORED

### Meaning

THE INPUT CANNOT BE GIVEN TO THE RECIPIENT.
INPUT IS IGNORED.

## NBC0054

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0054 UCON NOT ACTIVE - INPUT IGNORED

### Meaning

THE RECIPIENT OF LAST INPUT - UCON - IS NOT ACTIVE.
INPUT IS IGNORED.

## NBC0055

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0055 INVALID PREFIX ENTERED - NO SUCH ANSWER EXPECTED

### Meaning

AN INPUT TO EMERGENCY-HANDLER IS NEEDED, BUT INPUT FOR UCON IS GIVEN
AND UCON IS NOT ACTIVE, OR
AN INPUT TO EMERGENCY-HANDLER IS GIVEN, ALTHOUGH IT IS NOT EXPECTED.
INPUT IS IGNORED.

## NBC0056

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0056 HARDCOPY INOPERABLE

### Meaning

THE HARDCOPY COUPLED TO THE DISPLAY CANNOT BE SERVED.
DEPENDING ON THE KIND OF COUPLING THE DISPLAY IS NO LONGER AVAILABLE, TOO.

### Response

This devicetype is no longer supported.

## NBC0057

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0057 INPUT IGNORED - HARDCOPY DEFECTIVE

### Meaning

DUE TO HARD COUPLING BETWEEN DISPLAY AND HARDCOPY NO INPUT CAN
BE ACCEPTED AS LONG AS THE HARDCOPY IS DEFECIVE.
INPUT IS IGNORED.

## NBC0058

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0058 UCON BUSY - INPUT IGNORED

### Meaning

AN INPUT FOR UCON ARRIVES CIO DURING CIO IS WAITING FOR THE ACKNOWLEDGE-
MENT OF UCON TO THE PREVIOUS INPUT.
INPUT IS IGNORED.

## NBC0059

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0059 NO PF1-, PF2- OR ENTER-KEY USED - INPUT IGNORED

### Meaning

NEITHER PF1-, PF2- NOR 'ENTER'-KEY WAS USED FOR INPUT.
INPUT IS IGNORED.

## NBC0060

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NBC0060 INPUT TEXT NOT RECOGNIZED - UCON REJECTS INPUT

### Meaning

Both UCON reject buffers in use. KTT outputs own reject message.

## NBC0070

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NBC0070 CIO TESTS THIS CONSOLE

### Meaning

ALL CONSOLES ARE INOPERABLE AND CIO TESTS THEM IN A CYCLE.
THE FIRST CONSOLE WHICH GETS OPERABLE AGAIN ISSUES THIS
MESSAGE TEXT

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages