## IRMCOPY

Destination: USER-TASK Routing code: Weight: 20

Warranty : NO

IRMCOPY Copyright (C) (&01) (&00). All rights reserved

## IRMLOAD

Destination: USER-TASK Routing code: Weight: 20

Warranty : NO

IRMLOAD Program '(&00)', Version '(&01)' of '(&02)' loaded from file '(&03)'

## IRM0001

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IRM0001 SUBSYSTEM IORM NOT ACTIVE

### Meaning

Subsystem IORM not loaded or in HOLD state.

## IRM0002

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IRM0002 INTERNAL ERROR '(&00)'

### Meaning

Initialisation error of IORM resources.
(01) - (06): System error.
(07): Memory saturation.

### Response

(01) - (06): Call system administration.
(07): Wait and retry.

## IRM0003

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IRM0003 WRONG INPUT : '(&00)'

### Meaning

Wrong input.

### Response

Correct and retry.

## IRM0004

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IRM0004 WRONG DEVICE RANGE

### Meaning

Wrong device range.

### Response

Correct and retry.

## IRM0005

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IRM0005 (&00) NOT ALLOWED IN GUEST SYSTEM

### Meaning

(&00) is not allowed in guest system.

### Response

Retry in monitor system.

## IRM0006

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IRM0006 USER NOT PRIVILEGED FOR IORM

### Meaning

Required IORM privileges missing.

## IRM0007

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IRM0007 IORM NOT INITIALIZED

### Meaning

IORM already started but not yet initialized.

### Response

Wait and retry.

## IRM0008

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IRM0008 IORM NO LONGER ACTIVE

### Meaning

IORM no longer active after HOLD-SS.

### Response

Stop subsystem IORM and restart it again, then start program
IORM.

## IRM0020

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

IRM0020 DYNAMIC PAV NOT SUPPORTED BY DEVICE '(&00)'

### Meaning

DPAV not executed by device.

### Response

DPAV setting in control unit missing ?

## IRM0021

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

IRM0021 DYNAMIC PAV: DETACH ALIAS DEVICE '(&00)'

### Meaning

ALIAS device (&00) detached by IORM/DPAV.

## IRM0022

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

IRM0022 DYNAMIC PAV: ATTACH ALIAS DEVICE '(&00)'

### Meaning

ALIAS device (&00) attached by IORM/DPAV.

## IRM0023

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

IRM0023 DYNAMIC PAV: SWITCH ALIAS DEVICE '(&00)'

### Meaning

ALIAS device (&00) switched to other BASE device by IORM/DPAV.

## IRM0024

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

IRM0024 DYNAMIC PAV: ALIAS DEVICE '(&00)' CANNOT BE ASSIGNED

### Meaning

ALIAS device (&00) cannot be assigned to system.
VM2000: Device attached to other guest system ?

### Response

If the alias device is attached to other guest system:
1) IORM: DPAV_DEV_REM=D-R(&00,&00)
2) BS2000: /DETACH &00
3) IORM: DPAV_DEV_ADD=D-R(&00,&00)

## IRM0025

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IRM0025 DPAV SUPPORT ONLY FOR DEVICES AT CHANNELS OF TYPE FC

## IRM0026

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

IRM0026 DYNAMIC PAV: ALIAS DEVICE '(&00)' LOST

### Meaning

ALIAS device (&00) removed from I/O configuration.

### Response

Add ALIAS device again with /ADD-IO-UNIT.

## IRM0030

Destination: USER-TASK Routing code: Weight:

Warranty : NO

IRM0030 FUNCTION NOT SUPPORTED

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages