## DRVCOPY

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRVCOPY Copyright (C) '(&00)' '(&01)' All Rights Reserved

## DRVLOAD

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRVLOAD Program '(&00)',Version '(&01)' of '(&02)' loaded from file '(&03)'

## DRV0001

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0001 OPERATOR ACTION OR DECISION NEEDED FOR ALLOCATION OF DRV DISK '(&00)'. REASON: (&01). REPLY (&02)

### Meaning

No complete or unambiguously logical volume with the volume serial number
(&00) corresponding to the recording mode specified in the command has
been mounted.
(&01): previous message explaining the reason for the present situation
(&02): possible operator responses
R = RETRY: repeat mount operation
D = DUAL: mount disk in DUAL mode
M = MONO: mount disk in MONO mode
S = SRV: mount disk in SRV mode
T = TERM: abort mount operation
F = FORCE: confirm mount suggestion
<mn> = the requested disk has been mounted on device <mn>.

### Response

Take appropriate action in accordance with (&02).

## DRV0002

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0002 SYNTAX ERROR IN REPLY TO MESSAGE 'DRV0001' FOR DISK '(&00)'.REPLY '(&01)' NOT IN CURRENT REPLY SET '(&02)'

### Meaning

Message DRV0001 is displayed again.

## DRV0003

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0003 LABEL UPDATE FOR DISK '(&00)' ON '(&01)' ABORTED. ALLOCATION RESTART

### Meaning

The attempt to update the volume label or, in the case of private disks,
possibly to equalize the F5 labels has been aborted due to an input/output
error.
The last successfully reached stage in setting up the logical disk is
used and message DRV0001, which requires a response, is issued.

## DRV0004

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0004 DISK '(&00)' ON DEVICE '(&01)' HAS CURRENT TIME STAMP BUT IS NOT COMPLETE LOGICAL DRV DISK

### Meaning

An attempt to restore or equalize the specified disk has been aborted. It
can form a complete logical DRV disk only in conjunction with the
associated consistent read disk.
Possible reasons:
- 'N' has been entered in response to mount message NKVD013.
- At least two disks with the VSN (&00) have already been mounted, but
no READ disk.
TIME STAMP: date and time of day of the most recent allocation.

### Response

An appropriate response must be entered to the subsequent DRV0001 message.

## DRV0005

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0005 DISK '(&00)' ON DEVICE '(&01)' HAS CURRENT TIME STAMP BUT IS INCONSISTENT

### Meaning

A VOLIN or FDDRL run for the specified disk has been aborted, thus causing
disk (&00) to be inconsistent. DRV can use this disk only as a second disk
which has to be restored.
Possible reasons:
- 'N' was entered in response to mount message NKVD013.
- At least two disks with the VSN (&00) have already been mounted, but
none of them can be used.
TIME STAMP: date and time of day of the most recent allocation.

### Response

An appropriate response must be entered to the subsequent DRV0001 message.

## DRV0007

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0007 DRV CANNOT IDENTIFY RECORDING MODE FOR VSN '(&00)'

### Meaning

The specification FROM-DISK or DRV set for the recording mode by means of
the /SET-DRV-PARAMETER command is not specific enough for the mounted
disks, as allocation is possible in both DRV DUAL mode and DRV MONO mode.

### Response

The recording mode is set by the response to the subsequent DRV0001
message. It cannot be set right now by means of the /SET-DRV-PARAMETER
command.

## DRV0008

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0008 MORE THAN TWO EQUIVALENT DISKS MOUNTED ON DEVICES '(&01)' FOR VSN '(&00)'. LOGICAL DRV DISK NOT UNIQUE

### Meaning

The logical DRV disk cannot be set up without operator intervention.

### Response

First the desired recording mode DRV MONO or DRV DUAL must be set by
the response to the subsequent DRV0001 message; then the desired device(s)
must be selected by the following DRV0001 message(s).
If recording mode DRV DUAL is selected, the subsequent DRV0001 message
has to be answered twice by <mn>.
Another way of ensuring that the disk is unique is to use the /DETACH
command to make all disks that are not be used inaccessible.

## DRV0009

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0009 TWO IDENTICAL DISKS MOUNTED ON DEVICES '(&01)' FOR VSN '(&00)'. LOGICAL 'DRV-MONO' DISK NOT UNIQUE. 'RECORDING-MODE DRV-DUAL' IS POSSIBLE

### Meaning

The logical DRV disk cannot be set up without assistance from the operator
as it is not unique.

### Response

The recording mode is set by entering the appropriate response to the
subsequent DRV0001 message:
<mn> = recording mode DRV MONO
D = recording mode DRV DUAL

## DRV0010

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0010 LAST USE OF DISK '(&00)' ON DEVICE '(&01)' CRASHED. CONFIRMATION FOR USE OF DISK IN RECORDING-MODE DRV-MONO REQUIRED

### Meaning

Since the DRV-MONO recording mode has been set, the mounted disk can be
used accordingly.
However, if the specified disk has been removed (/STOP-DRV-DUAL-MODE),
a more recent MONO disk still exists.
Since DRV does not have enough information to determine which of the above
cases applies, the operator has to confirm the correctness of disk (&00)
in DRV MONO recording mode.

### Response

The DRV MONO recording mode is confirmed for the disk by entering 'F' in
response to the subsequent DRV0001 message.

## DRV0011

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0011 DISK '(&00)' ON DEVICE '(&01)' IS SRV DISK WITH MORE RECENT TIME STAMP THAN MOUNTED DRV DISK. CONFIRMATION OF USE OF SRV DISK FOR RECORDING-MODE DRV REQUIRED

### Meaning

The current disk is an SRV disk and thus also the current logical DRV
disk. In addition, at least one DRV disk has been mounted. This message
is intended as a safeguard in the case of simultaneous SPECIAL operation
to prevent any SRV disks produced in SPECIAL mode which may
intermittently have more recent time stamps from being allocated as
DRV disks without the possibility of operator intervention.
TIME STAMP: date and time of day of the most recent allocation.

### Response

Possible responses:
- Entering 'F' in response to the subsequent DRV0001 message forces
recording mode DRV-MONO to be set for the disk.
- The uniqueness of the disk can be ensured with the aid of the /DETACH
command before a fresh allocation attempt is made by entering 'R'.

## DRV0012

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0012 THE LOGICAL VOLUME '(&01)' FOR VSN '(&00)' ESTABLISHED BY OPERATOR ANSWER IS NOT CORRECT

### Meaning

No valid logical volume can be established by the MN given by the response
to the DRV0001 message.
The disks selected must have the most current TIME STAMP and a fitting
SVL DRV MODE (cf. the output of /SHOW-DRV-STATUS ).
Disk pairs must have identical TIME STAMPs SVL DRV MODEs, configuration
paths and disk topologies (VOLIN).

## DRV0013

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0013 DISK '(&00)' ON '(&01)' IS NOT COMPLETE DRV DISK

### Meaning

The specified disk has not been completely defined in the recording mode
by the preceding command.
Reason: either 'N' has been entered in response to mount message NKVD013
or at least two disks with VSN (&00) have been mounted and they
do not match.

### Response

Enter an appropriate response to the subsequent DRV0001 message.

## DRV0014

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0014 TYPE OF VOLIN INITIALIZATION FOR DISKS '(&00)' ON DEVICES '(&01)' NOT IDENTICAL OR FASTDISKS WITH DIFFERENT SIZE

### Meaning

The two specified disks do not form a valid DRV disk pair as the
corresponding VOLIN runs were not performed with the same operands.
If FASTDISKs (type D3409) are used, they must be configurated to have
the same capacity.

## DRV0015

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0015 TYPE OF CONFIGURATION PATH FOR DISKS '(&00)' ON DEVICES '(&01)' NOT IDENTICAL

### Meaning

The two specified disks do not form a valid DRV disk pair. The channel,
controller and device types must be identical.

## DRV0016

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0016 DRV ALLOCATION FOR DISK '(&00)' ON DEVICE '(&01)' CLASHES WITH SPECIAL ALLOCATION

### Meaning

The disk or disks cannot be used for a DRV allocation because of an
already existing SPECIAL allocation (e.g. VOLIN, FDDRL or SIR).

## DRV0019

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0019 ALLOCATION OF DISK '(&00)' ON DEVICE '(&01)' COMPLETED

### Meaning

This message is issued after a response has been entered to message
DRV0001
and confirms that the disk has been successfully allocated.

## DRV0030

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0030 SYNTAX ERROR IN '(&00)' COMMAND. COMMAND NOT PROCCESSED

### Meaning

This message is issued if the combination of the specified operand
values are not allowed for a DRV command.
Command /SET-DRV-PARAMETER:
UNIT=*VOLUME and EQUALIZE=*OPEN-FILES
UNIT=*PUBSET/*VOLUME-SET and RECORDING-MODE=DRV-MONO/DRV-DUAL
DUAL-STOP=*AT-ERROR and wait time exceeds 32000 seconds
Command /START-DRV-DUAL-MODE:
FROM-PUBSET and TO-PUBSET have different length
Command /STOP-DRV-DUAL-MODE:
PUBSET and NEW-NAME-OF-REMOVED have different length
NEW-NAME-OF-REMOVED=PUB not allowed

## DRV0031

Destination: CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0031 COMMAND '(&00)' FOR DISK '(&01)' CANNOT CURRENTLY BE PROCESSED

### Response

Reenter the command later.

## DRV0032

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0032 NO INFORMATION AVAILABLE FOR 'ALLOCATION-PHASE=(&00)', 'ALLOCATION-TYPE=(&01)', 'RECOVER=(&02)', 'RECORDING-MODE=(&03)' AND 'INFORMATION=(&04)'

## DRV0033

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0033 NO INFORMATION AVAILABLE FOR 'VOLUME=(&01)' AND 'INFORMATION=(&00)'

## DRV0034

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0034 NO INFORMATION AVAILABLE FOR 'UNIT=*ALL-DRV' AND 'INFORMATION=(&00)'

## DRV0040

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0040 COMMAND '(&00)': NO SUITABLE DISK MOUNTED ON DEVICE '(&01)' FOR RECORDING MODE DRV DUAL OR DEVICE INOPERABLE

### Meaning

Device (&01): the mounted disk is not suitable for the recording mode
DRV DUAL, the mnemonic device name is invalid or the device is inoperable.

### Response

Correct the error and reenter the command, or ready the device.

## DRV0041

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0041 COMMAND '(&00)': DISKS WITH DIFFERENT VSN'S ARE MOUNTED ON DEVICES '(&01)' AND '(&02)'

## DRV0042

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0042 COMMAND '(&00)': '(&03) (&01)' AND '(&04) (&02)' ARE IDENTICAL

## DRV0043

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0043 COMMAND '(&00)': DISK '(&01)' ON DEVICE PAIR ('(&02)','(&03)') IS ALREADY LOGICAL 'DRV-DUAL DISK'. COMMAND IGNORED

## DRV0044

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0044 COMMAND '(&00)': NO TWO DISKS WITH VSN '(&01)' MOUNTED

## DRV0045

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0045 COMMAND '(&00)': SPECIFICATION OF VSN '(&01)' IS NOT SUFFICIENT

### Response

Reenter the command in the form
/START-DRV-DUAL-MODE VOLUME=*BY-UNIT(FROM-UNIT=<mn>,TO-UNIT=<mn>).

## DRV0046

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0046 COMMAND '(&00)': 'RECOVER' OPERATION ALREADY RUNNING FOR DRV DUAL DISK '(&01)' ON DEVICE PAIR ('(&02)','(&03)')

### Response

If necessary, reenter the (&00) command following completion of the
recover operation.

## DRV0047

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0047 COMMAND '(&00)': DISK '(&01)' ON DEVICE '(&02)' ALREADY ALLOCATED IN 'RECORDING-MODE DRV-MONO'. COMMAND IGNORED

## DRV0048

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0048 COMMAND '(&00)' FOR DISK '(&01)' NOT PROCESSED

## DRV0049

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0049 COMMAND '(&00)' PROCESSED FOR DISK '(&01)'

### Meaning

The (&00) command contained no syntax errors and was processed. However,
it is possible that the entire processing sequence initiated by the
command has not been completed; e.g. a reconstruction or equalization
operation may still be running.

## DRV0050

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0050 COMMAND '(&00)': DISK '(&01)' DEFINED AS PUBLIC. USE SYNTAX : /SET-DRV-PAR PUBSET=... OR VOLUME-SET=...

### Meaning

The disk specified by VOLUME=(&01) in the (&00) command is part of a
pubset that has to be referenced via the pubset ID.

### Response

Reenter the command, specifying PUBSET=<pubset-ID> resp. VOLUME-SET=
<pubset-ID>.

## DRV0051

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0051 COMMAND '(&00)': DISK '(&01)' ALREADY DEFINED AS SRV DISK

### Meaning

The specified volume (&01) has already been defined as an SRV disk in an
earlier /SET-DRV-PARAMETER command. This clashes with the attempt to use
this disk implicitly as a DRV DUAL disk by the START-DRV-DUAL command.
SRV: Single Recording by Volume
DRV: Dual Recording by Volume.

## DRV0052

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0052 COMMAND '(&00)': DISK '(&01)' RESP. SOME DISKS OF CORRESPONDING PUBSET ALREADY ALLOCATED

### Meaning

The specified volume (&01) has already been allocated. It is not possible
to switch from SRV to DRV and vice versa as long as this allocation is
in effect.
For pubsets one or more disk volumes may be allocated, for instance by
PAGING.
SRV: Single Recording by Volume
DRV: Dual Recording by Volume.

## DRV0053

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0053 COMMAND '(&00)': DISK '(&01)' ALREADY DEFINED AS PPD OR SPD DISK

### Meaning

A PPD or SPD disk cannot be used as a DRV disk.
PPD: Protected Private Disk
SPD: Shared Private Disk
DRV: Dual Recording by Volume.

## DRV0054

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0054 COMMAND '(&00)' CANNOT BE PERFORMED WHILE ALLOCATION OF DISK '(&01)' IS IN PROGRESS

## DRV0055

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0055 COMMAND '(&00)': DISK '(&01)' CANNOT BE ALLOCATED IN 'RECORDING-MODE DRV-DUAL' WITHOUT OPERATOR ASSISTANCE. REASON: '(&02)'

### Meaning

The (&00) command cannot be processed unless the mount status of the disks
permits allocation without operator intervention.
The reason for operator intervention is given in message (&02).
Further information on this message can be requested by entering the
/HELP-MESS command.

### Response

Ensure that all the prerequisites for setting up a logical disk have
been met and then reenter the command.

## DRV0057

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0057 COMMAND '(&00)': DISK '(&01)' IS NO DRV DISK

## DRV0058

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0058 COMMAND '(&00)' FOR DISK '(&01)' NOT PROCESSED: SPECIFICATION OF VSN NOT SUFFICIENT RESP. UNIT MAY CURRENTLY NOT BE REMOVED

### Meaning

For command STOP-DRV-DUAL-MODE with syntax VOLUME=vsn:
As currently no DRV action is running, DRV is not able to determine
which disk should be removed if only the VSN is given.
For command STOP-DRV-DUAL-MODE with syntax UNIT-TO-REMOVE=mn:
The disk specified may currently not be removed as it is used as read
disk for a reconstruction or equalization.

### Response

For command STOP-DRV-DUAL-MODE with syntax VOLUME=vsn:
Specifiy the UNIT-TO-REMOVE by using the relevant syntax.
For command STOP-DRV-DUAL-MODE with syntax UNIT-TO-REMOVE=mn:
Wait until the reconstruction resp. equalization is completed.

## DRV0059

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0059 COMMAND '(&00)': DEVICE '(&01)' CANNOT BE USED AS DEVICE '(&02)' IS STILL USED FOR PAGING

### Meaning

On device '(&02)' a PAGING area is still used. The device is no longer
used by DRV because of a disk error or a command.
To resume DRV-DUAL mode, the device '(&01)' cannot be used as long as
the PAGING area is still used.

### Response

Retry the command specifying FROM-MN='(&02)' or
stop the use of the PAGING area via /REDUCE-PAGING-AREA and retry the
command with the same operands.

## DRV0060

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0060 DUAL START FOR DISK '(&00)' ON DEVICE PAIR '(&01)' COMPLETED. RECONSTRUCTION FROM DEVICE '(&02)' TO DEVICE '(&03)'. COPY MODE: '(&04)'

### Meaning

By means of a copy operation the MONO disk (&00) on device (&02) has been
converted into a DUAL disk on device pair (&01). The data is now
available twice.
Copy mode:
ALL-BLOCKS: All blocks of the disk have been copied.
ALLOCATED-BLOCKS: All blocks indicated as allocated in the F5 label
have been copied.
MODIFIED-FILES: All blocks of currently open or modified files since
the allocation of the original disk have been copied.
LABEL: Only the standard volume label (SVL) has been
equalized.

## DRV0061

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0061 DUAL STOP FOR DISK '(&00)' ON DEVICE PAIR '(&01)' COMPLETED. 'DRV-MONO' DISK CREATED ON DEVICE '(&02)'

### Meaning

DUAL disk (&00) on device pair (&01) has been converted into a MONO disk
on device (&02). The data is now available once only.

## DRV0062

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0062 EQUALIZATION OF DISK '(&00)' ON DEVICE PAIR '(&01)' COMPLETED. DATA COPIED FROM DEVICE '(&02)' TO DEVICE '(&03)'. COPY MODE: '(&04)'

### Meaning

The equalization operation for disk (&00) on device pair (&01) has been
successfully completed. The data on the disk is now available twice again.
Copy Mode:
ALL-BLOCKS: All blocks of the disk have been copied.
ALLOCATED-BLOCKS: All blocks indicated as allocated in the F5 label
have been copied.
OPEN-FILES: All blocks of open files have been copied.

## DRV0064

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0064 DRV ALLOCATION FOR DISK '(&00)' ON DEVICE '(&01)' CANCELLED

### Meaning

User access to logical disk (&00) has been cancelled by the system or the
operator. The disk does not become available for use again until all users
have released it. For SPECIAL allocations, however, the individual disks
are available immediately.

## DRV0065

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0065 DUAL START FOR DISK '(&00)' ON DEVICE PAIR '(&01)' ABORTED

### Meaning

The dual start of the disk is aborted either because an unrecoverable
I/O error has occurred or because a dual stop has been initiated.

## DRV0066

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0066 DUAL STOP FOR DISK '(&00)' ON DEVICE PAIR '(&01)' FOR 'DRV-MONO' DISK ON DEVICE '(&02)' ABORTED

### Meaning

The dual stop is aborted because cancellation of the allocation for
logical disk (&00) has been initiated by the system or the operator.

## DRV0067

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0067 EQUALIZATION FOR DISK '(&00)' ON DEVICE PAIR '(&01)' ABORTED

### Meaning

The equalization of the disk is aborted either because an unrecoverable
I/O error has occurred or because a dual stop has been initiated.

## DRV0068

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0068 DEVICE '(&01)' IS STILL USED BY PAGING FOR DISK '(&00)'

### Meaning

This message is preceeded by message DRV0061 (DUAL STOP COMPLETED).
Device '(&01)' is no longer used by DRV but still used by PAGING.
It cannot be repaired by physical replacement or VOLIN.
If possible, the usage of the PAGING area on the disk should be
terminated.

## DRV0069

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0069 CANCELLATION OF DRV ALLOCATION FOR DISK '(&00)' ON DEVICE '(&01)' ABORTED

### Meaning

The attempt by the system or the operator to cancel the allocation of
logical disk (&00) could not be completely processed. The user can no
longer access the disk, which does not become available for use again
until all users have released it.
The individual disks are not available for SPECIAL allocations.

## DRV0070

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0070 DUAL STOP FOR DISK '(&00)' ON DEVICE '(&01)' NOT POSSIBLE

### Meaning

By means of the /CHANGE-DISK-MOUNT command or by entering a negative
response to remount message NKVD014 the operator has initiated
cancellation of the allocation of a logical disk.
Disk (&00) is part of a DRV DUAL disk whose operation has been
interrupted. The allocation of a logical disk can only be cancelled at
this time if it is subsequently possible to resume the resulting MONO
operation without any delay.

## DRV0071

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0071 I/O ERROR DURING LABEL UPDATE FOR DISK '(&00)' ON DEVICE '(&01)'. 'DRV-RECOVER' CONTINUES

### Meaning

The abortive attempt to update the labels is repeated on completion of
the recover operation, this time with the I/O error facility activated.

## DRV0072

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0072 ALLOCATION OF DISK '(&00)' ON DEVICE '(&01)' FAILED. 'DRV-RECOVER' CANCELLED

### Meaning

The attempt by the RECOVER task to allocate disk (&00), which is necessary
to execute the recover operation, was rejected, thus causing the
original status to be restored.

## DRV0073

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0073 'DRV-RECOVER' FOR DISK '(&00)' ON DEVICE '(&01)' FAILED. REASON : '(&02)'. ERROR CODE : '(&03)'. ACTION '(&04)' WILL BE INITIATED

### Meaning

A DRV recover action failed. The error reason indicates what type of
action returned an error condition as presented in error code.
The action indicated may be switching to MONO use or cancellation of the
access to the disk.

## DRV0074

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0074 COPYING OF DISK '(&00)' FROM DEVICE '(&01)' TO DEVICE '(&02)' STARTED

### Meaning

The copying of logical disk (&00) has been initiated.
Successful or unsuccessful completion of copying will be indicated
by an appropriate message.

## DRV0075

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0075 COPYING OF DISK '(&00)' COULD NOT BE STARTED

### Meaning

A recover operation is already in progress. For this reason the copy
operation could not be started.

## DRV0076

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0076 TWO IDENTICAL DISKS MOUNTED ON DEVICES '(&02)' AND '(&03)' FOR LOGICAL DRV DISK '(&01)' IN COMMAND '(&00)'. SPECIFY DEVICE TO BE DETACHED

### Response

As both disks are currently identical, one of the two devices (&02) and
(&03) must be detached by means of the command /UNIT-TO-REMOVE=<mn>.

## DRV0077

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0077 FOR DISK '(&00)' ON DEVICE '(&01)' EVENT '(&02)' WITH ERROR CODE '(&03)' OCCURED

### Meaning

Possible Values for 'EVENT':
PV_CANCEL_REQUEST, LV_CANCEL_REQUEST : a /CHANGE-DISK ACTION=CANCEL
command issued by the operator was relayed to DRV.
PV= CANCEL for a unit, LV= CANCEL for the volume.
PV_CANCEL_EVENT, LV_CANCEL_EVENT : DRV is informed about the
cancellation of the user access to one unit (PV) or the volume (LV).
PV_CANCEL_EVENT_PCA : same as PV_CANCEL_EVENT, caller was PCA .
PCA : PP5 cache assist.
DRER_PPAM_ABNORMAL_TT : Due to a task termination an I/O could not be
processed completely. The contents of the disks could differ.
REMOUNT_START : The disk monitor informs about the suspension of the
access to the disk.
REMOUNT_END : The disk monitor informs about the reestablishment of
the access to the disk.
TIMER_EVENT : The wait time specified by means of /SET-DRV-PARAMETER
before an automatic switch to mono mode in case of an error ran out.

## DRV0078

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV0078 REQUEST FOR DISK '(&00)' ON DEVICE '(&01)' NOT PROCESSED AS IT WOULD CANCEL A DISK OF THE HOME PVS

### Meaning

By means of the /CHANGE-DISK-MOUNT command or by entering a negative
response to remount message NKVD014 the operator has initiated
cancellation of the allocation of a logical disk.
The allocation of the disk cannot be cancelled as it is part of
the HOME public volume set.

## DRV0079

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

DRV0079 COMMAND: '(&00)': WRONG PUBSET TYPE SPECIFIED FOR PUBSET/VOLUME SEt '(&01)'

### Meaning

The command '&00' has been called with UNIT=*PUBSET or UNIT=*VOLUME-SET.
The CATID specified has the wrong type:
For UNIT=*PUBSET it must be a SF pubset (single feature, traditional
pubset),
for UNIT=*VOLUME-SET it must be volume set of SM pubset (system managed
pubset).
The specification of a CATID of a SM pubset is not possible; DRV can
only be used for single volume sets of a given SM pubset.
The type of a pubset can be checked with /SHOW-MASTER-CATALOG-ENTRY.

## DRV0080

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0080 COMMAND '(&00)' SUCESSFULLY PROCESSED

### Meaning

Final message of a DRV command for which all parts have been
successfully processed.

## DRV0081

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0081 COMMAND '(&00)' PARTIALLY SUCCESSFULLY COMPLETED

### Meaning

Final message of a DRV command for which some parts have been
successfully processed.

## DRV0082

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0082 COMMAND '(&00)' NOT SUCCESSFULLY PROCESSED

### Meaning

Final message of a DRV command for which no part has been successfully
processed.

## DRV0083

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0083 COMMAND '(&00)' CANNOT CURRENTLY BE PROCESSED

### Meaning

Final message of a DRV command for which no part could currently be
processed

## DRV0084

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV0084 COMMAND '(&00)' ABORTED

### Meaning

Final message of a DRV command that has been aborted due to internal
errors.

## DRV0085

Destination: USER-TASK Routing code: Weight:

Warranty : YES

DRV0085 COMMAND '(&00)': REQUIREMENTS FOR VOLUME '(&01)' NOT MET. REASON: '(&02)'

### Meaning

The command '(&00)' with syntax PUBSET=<catid>,COPY-PUBSET=<catid> cannot
be processed. The reason is given in the 2nd insert and is valid (at
least) for the VSN '(&01)'.
Meaning of Insert 2 at command /START-DRV-DUAL-MODE:
NOT SINGLE FEATURE PUBSET wrong pubset type
LV NOT FREE allocation exists (poss. cancel situation)
ALLOCATED OR NOT DUAL still allocated or wrong DRV mode
ONLINE disks of the pubset to create are online
CATALOG INCONSISTENT file catalog $TSOS.TSOSCAT is inconsistent
STOP-DRV NOT FINISHED transition to MONO not successful/completed
Meaning of Insert 2 at command /STOP-DRV-DUAL-MODE:
NOT SINGLE FEATURE PUBSET wrong pubset type
NOT ALLOCATED OR NOT MONO not imported or wrong DRV mode
COPY-PUBSET DOES NOT MATCH disk pairs not created by /STOP-DRV
*BY-PUBSET or different number of volumes
VOLUME NOT MONITORED disk(s) of original pubset not monitored
(not created by /STOP-DRV *BY-PUBSET
or situation after system crash)
NOT ORIGINAL PUBSET FROM-PUBSET is not original pubset
CANNOT OCCUPY PUBSET pubset occupation not successful
VOLUMES DO NOT MATCH cf. COPY-PUBSET DOES NOT MATCH
EXCAT NOT FINISHED /EXPORT-PUBSET not successful/terminated
Meaning of Insert 2 for command /STOP-DRV-DUAL-MODE with operand
NEW-NAME-OF-REMOVED *SAME or /START-DRV-DUAL-MODE with operand
FROM-PUBSET=*CURRENT:
NOT FOUND OR WRONG ALLOCATION pubset not found or wrong allocation
NOT SF PUBSET / VOLSET only single feature pubsets or volume sets
of system managed pubsets are allowed
CANNOT EVALUATE PUBSET MEMBERS pubset in use and members cannot
be determined

### Response

Correct errenous situation and retry command for reasons:
LV NOT FREE, ONLINE, ALLOCATED OR NOT DUAL, NOT ALLOCATED OR NOT MONO,
CANNOUT OCCUPY PUBSET, EXCAT NOT FINISHED
For all other reasons at command /START-DRV-DUAL-MODE no fast
reconstruction is possible.
Export the mirror pubset, re-initialize the disks with VOLIN (FMT=NO)
and start the (full) reconstruction with command:
/START-DRV VOLUME=*BY-PUBSET(FROM-PUBSET=*CURRENT,TO-PUBSET=<catid>).

## DRV0086

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV0086 PROCESSING ERROR FOR DISK '(&00)' ON DEVICE '(&01)' AT OPERATION '(&02)'. ERROR CODE : '(&03)'

## DRV0087

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV0087 FILE '(&01)' MODIFIED ON DISK '(&00)', WILL BE RECONSTRUCTED

### Meaning

This message is issued during the processing of /START-DRV-DUAL-MODE if
a copy pubset is to be reconstructed by copying all modified blocks resp.
all modified files from the original pubset. The message indicates the
files that will be copied. If the copy pubset has been monitored by DRV,
all modified blocks, otherwise all blocks of the file will be restored
by copying the current content of the file from the original pubset.

## DRV1004

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV1004 SYSTEM ERROR DURING INITIALISATION OF SUBSYSTEM DRV

### Response

Take NDMDAMP and stop subsystem DRV.

## DRV1005

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV1005 SYSTEM ERROR IN DRV: DRVT LOCK REQUESTED BUT ALREADY HELD

### Response

Take requested system dump.

## DRV1006

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV1006 SYSTEM ERROR IN DRV: DRVT LOCK NOT HELD

### Response

Take requested system dump.

## DRV1010

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

DRV1010 FILE '(&00)' IS USED AS DRV CONFIGURATION FILE.

### Meaning

Displays the used configuration file

## DRV1011

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

DRV1011 DMS-Error '(&00)' during processing of file '(&01)'

### Meaning

DMS-Error during processing of the configuration file.

## DRV1012

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

DRV1012 Syntax-Error in line '(&00)' of file '(&01)'

### Meaning

Error during processing of the configuration file. Processing aborted.

## DRV1013

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

DRV1013 Error during command processing in line '(&00)' of file '(&01)'

### Meaning

Error during processing of a command in the DRV configuration file.
Processing continues.

## DRV1014

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

DRV1014 Configuration file not valid. Defaults used.

### Meaning

Configuration file does not exist or
contains no valid command.

### Response

Specify a correct configuration file.

## DRV1015

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

DRV1015 Syntaxerror in subsystem parameters

### Meaning

Error in subsystem parameters of command START-SUBSYSTEM. Loading aborted.

## DRV2000

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV2000 ACTIVATE MIGRATION FOR SOURCE DEVICE '(&00)' AND TARGET DEVICE '(&01)' SUCCESSFUL

## DRV2001

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : NO

DRV2001 DEACTIVATE MIGRATION FOR SOURCE DEVICE '(&00)' AND TARGET DEVICE '(&01)' SUCCESSFUL

## DRV2002

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

DRV2002 ACTIVATE MIGRATION FOR SOURCE DEVICE '(&00)' AND TARGET DEVICE '(&01)' REJECTED

## DRV2003

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

DRV2003 DEACTIVATE MIGRATION FOR SOURCE DEVICE '(&00)' AND TARGET DEVICE '(&01)' REJECTED

## DRV2004

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

DRV2004 SYSTEM ERROR '(&00)'

### Meaning

Error at system interface:
(&00) = LOCK : $LOCK-Error
(&00) = GETM : $GETMEM-Error
(&00) = CONV : $IOCONV-Error
(&00) = VTEN : $VTENPR-Error

## DRV2005

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

DRV2005 SOURCE DEVICE '(&00)' AND TARGET DEVICE '(&01)' IDENTICAL

## DRV2006

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

DRV2006 MIGRATION FOR DEVICE '(&00)' ALREADY ACTIVE WITH DEVICE '(&01)'

## DRV2007

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

DRV2007 MIGRATION NOT ACTIVE FOR DEVICE '(&00)' AND DEVICE '(&01)'

## DRV2008

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

DRV2008 DEVICE '(&00)' NOT AVAILABLE

## DRV2009

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

DRV2009 I/O ERROR FOR DEVICE '(&00)'

## DRV2010

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

DRV2010 STANDARD VOLUME LABEL OF DEVICE '(&00)' NOT SUPPORTED

## DRV2011

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

DRV2011 DISK FORMAT FOR SOURCE DEVICE '(&00)' AND TARGET DEVICE '(&01)' NOT IDENTICAL

## DRV2012

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

DRV2012 TYPE OF DEVICE '(&00)' NOT SUPPORTED

## DRV2013

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

DRV2013 INSUFFICIENT SPACE ON TARGET DEVICE '(&00)'

## DRV2014

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

DRV2014 DEVICE '(&00)' CONNECTED TO NOT SUPPORTED CHANNEL TYPE

## DRV2015

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

DRV2015 MIGRATION NOT SUPPORTED

## DRV2100

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

DRV2100 Command not fully processed

### Meaning

At least some parts of the command could not be processed

### Response

see previous messages DRV2nnn

## DRV2101

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV2101 NO TWO DISKS WITH VSN '(&00)' MOUNTED

## DRV2102

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV2102 THE DISKS WITH VSN '(&00)' HAVE INVALID TYP FOR MIGRATION

## DRV2103

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV2103 NO VOLUMES AVAILABLE FOR PUBSET '(&00)'

## DRV2104

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV2104 DRV-DUAL STILL ACTIVE FOR PUBSET '(&00)', MIGRATION COULD NOT BE FINALIZED

### Response

EXECUTE STOP-DRV-DUAL-MODE FOR THE PUBSET

## DRV2105

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : YES

DRV2105 PROBLEMS DURING TARGET UPDATE FOR PUBSET '(&00)', ABORT-PUBSET-MIGRATION WILL BE EXECUTED

## DRV2500

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV2500 BEGIN OF PUBSET-MIGRATION: FUNCTION = (&00)

### Meaning

The DRV disk migration with function (&00) has been started.

## DRV2501

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV2501 PUBSET-MIGRATION, FUNCTION = (&00), for PUBSET (&01) successful

## DRV2502

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV2502 PUBSET-MIGRATION, FUNCTION = (&00), for PUBSET (&01) aborted. PROCEDURE-TRACE: (&02)

### Meaning

Prozedure EXECUTE-PUBSET-MIGRATION has been terminated with an error.
Procedure trace was saved under (&02).

## DRV2503

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV2503 Following parameters for PUBSET-MIGRATION not or wrong specified: (&00)

## DRV2505

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV2505 MIGRATION-STATE '(&00)' of volume (&01) not valid

### Meaning

MIGRATION-STATE (&00) of volume (&01) does not allow
PUBSET-MIGRATION for the pubset

## DRV2506

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV2506 No logic volume assigned to PUBSET (&00)

### Meaning

PUBSET-MIGRATION not possible, PUBSET (&00) invalid

## DRV2507

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV2507 Disk (&00) still in use

### Meaning

PUBSET-MIGRATION not possible as disk (&00) is in use

### Response

Export Pubset.

## DRV2508

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV2508 COMMAND (&00) NOT SUCCESSFULLY COMPLETED. ERROR: (&01)

## DRV2509

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV2509 (&00) for PUBSET (&01) not successfully completed. ERROR: (&02)

### Meaning

For PUBSET (&01), the function (&00) could not
be realized successfully.

### Response

Check pubset (&00).

## DRV2510

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV2510 (&00) for one or more devices not successfully completed. ERROR: (&01)

### Meaning

For at least one device, the function (&00) could not
be realized successfully.

## DRV2511

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV2511 Pubset (&00) is of invalid type (&01)

## DRV2520

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV2520 PROP-XT not ready

### Meaning

PROP-XT is not available.

## DRV2522

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV2522 ACCESS TO CONSOLE VIA PROP-XT FAILED. ERROR: (&00)

### Meaning

While accessing the console via PROP-XT, the error
(&00) occured.

### Response

Check status of PROP-XT.

## DRV2523

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV2523 PROP-XT-WAIT FAILED WITH ERROR (&00)

### Meaning

Waiting with PROP-XT was aborted with error (&00)

## DRV3000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3000 ***** P V S R E N VERSION '(&00)' *****

## DRV3100

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3100 PVSREN NOT EXECUTABLE IN PRESENT BS2000 VERSION. PVSREN NOT LOADED

### Response

Use a PVSREN version which supports the BS2000 version.

## DRV3114

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3114 'INCONSISTENCY' BIT SET FOR DISK WITH VSN '(&00)'. PROCESSING ABORTED

### Meaning

The NKDINF macro reports that the INCONSISTENCY bit is set in the
system volume label of the disk.

### Response

Cancel the bit setting for the disk.

## DRV3115

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3115 PUBSET OR VOLUME-SET WITH CATALOG ID '(&00)' AVAILABLE. PROCESSING ABORTED

### Meaning

The pubset or volume-set must not be available when this statement is
executed, otherwise other users could make unwanted changes to the
file catalog during program execution.

### Response

Export the pubset from the catalog using the /EXPORT-PUBSET command and
repeat the statement.

## DRV3116

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3116 VOLUME '(&00)' OF PUBSET OR VOLUME-SET NOT ONLINE. PROCESSING ABORTED

### Meaning

The terminal of the specified volume has not been attached to
the installation.

### Response

Attach the volume terminal by means of the command /ATTACH <mn>
and initiate conversion again.

## DRV3120

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3120 ERROR IN MACRO '(&00)'. RETURN CODE: '(&01)'. PROCESSING ABORTED

### Response

Take appropriate action in accordance with the return code.

## DRV3124

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3124 ERROR WHEN OPENING VOLUME '(&00)'. RETURN CODE: '(&01)'. PROCESSING ABORTED

### Response

Take appropriate action in accordance with the return code.

## DRV3125

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3125 ERROR WHEN READING BLOCK. RETURN CODE: '(&00)'. PROCESSING ABORTED

### Response

Take appropriate action in accordance with the return code.

## DRV3126

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3126 ERROR WHEN WRITING BLOCK. RETURN CODE: '(&00)'. PROCESSING ABORTED. PUBSET OR VOLUME-SET INCONSISTENT

### Response

See message DRV3129.
Take appropriate action in accordance with the return code.

## DRV3127

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3127 ERROR WHEN CLOSING VOLUME '(&00)'. RETURN CODE: '(&01)'

### Response

Take appropriate action in accordance with the return code.

## DRV3129

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3129 PUBSET OR VOLUME-SET INCONSISTENT. STATEMENT PROCESSING ABORTED

### Meaning

The program terminated abnormally during an earlier conversion of
the pubset or volume-set. VSN-ENTRIES in SVL/OLC of PUBRES incorrect.

### Response

The pubset or volume-set can only be converted if the operands are
given the same values as they had before the abnormal program
termination. Please correct the wrong entries written into the
SVL/OLC of the PUBRES during the last conversion of the pubset.

## DRV3136

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3136 FILE CATALOG 'TSOSCAT' SUCCESSFULLY UPDATED

### Meaning

The file catalog of the pubset or volume-set was successfully updated.

## DRV3137

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3137 VOL1 LABELS SUCCESSFULLY UPDATED

### Meaning

The VOl1 labels of the pubset or volume-set were successfully updated.

## DRV3139

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3139 PUBSET OR VOLUME-SET '(&00)' HAS BEEN RENAMED TO THE NEW NAME '(&01)'

### Meaning

The pubset or volume set was successfully renamed.

## DRV3144

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3144 PVSREN TERMINATED ABNORMALLY

### Response

The appropriate action is indicated in the previous PVR message.

## DRV3145

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3145 PVSREN TERMINATED NORMALLY

### Meaning

The program was terminated normally via the END statement.

## DRV3146

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3146 CAT-ID '(&00)' is invalid.

### Meaning

There is no pubset or volume set with this cat-id.

### Response

Response
- none

## DRV3147

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3147 An error occurred while the device type of the target discs was updated.

### Meaning

More detailed information on the detected errror(s) may be found in the
preceding messages.

### Response

Response
- none

## DRV3153

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV3153 INFORMATIONS IN THE MRSCAT-ENTRY '(&00)' DO NOT AGREE WITH THE INFORMATIONS IN THE SVL OF DISK '(&01)'.

### Meaning

Pubset type, CATID of the Control-Volume-Set or CATID of the SM-Pubset
in the MRSCAT-Entry &00 does not agree with the information in the
SVL of the disk &01.

### Response

Check MRSCAT-Entry and corresponding disk. Remove the conflict and
repeat the renaming.

## DRV3154

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV3154 PUBSET '(&00)' IS LOCKED. RENAMING IS NOT POSSIBLE AT THE TIME.

### Meaning

The SF-Pubset or SM-Pubset &00 is locked through an active PVSREN run
or a PVSREN run, that has been terminated abnormally.
A volume-set, that belongs to a SM-Pubset, can only be renamed, if
the SM-Pubset is not locked.
A SM-Pubset is locked, if the SM-Pubset or a volume-Set, that belongs
to the SM-Pubset, is renamed.

### Response

In case of an active PVSREN run, wait until the run has been finished.
In case of an abnormal terminated PVSREN run, use the statement
'RESTART-RENAMING', to remove the lock. This statement requires the
logging file SYSLOG.PVSREN.<catid-old>.<catid-new>, that is created
by PVSREN.

## DRV3155

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV3155 VOLUME-SET '(&00)' IS DEFECT OR DEFINED ONLY. RENAMING IS NOT PROCESSED.

### Meaning

It is not possible to rename a defect volume set.
If a SM-pubset contains a defect volume set, it is not possible to
rename the SM-pubset or the control-volume-set.
For a defined only volume set there is only an entry in the
configuration file of the pubset.

### Response

Remove the defect volume set from the pubset. All files of this
volume set will be lost.
For a defined only volume set the Configuration can be changed with
the command 'MODIFY-PUBSET-PROCESSING'.

## DRV3156

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV3156 THE CATID OF THE SM-PUBSET IN THE SVL OR IN THE PUBSET CONFIGURATION FILE FOR THE VOLUME SET '(&00)' IS NOT CORRECT.

### Meaning

The configuration of the SM-pubset is inconsistent.
The CATID of the SM-Pubset, to which the volume set belongs, is stored
in the pubset configuration file. This information does not agree with
the information that ist stored in the SVL of the volume set.

### Response

Check and correct the configuration. Repeat the PVSREN run.

## DRV3157

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV3157 EXCLUSIVE ALLOCATION NOT POSSIBLE FOR DISK '(&00)'. RETURNCODE '(&01)'. PROCESSING ABORTED.

### Meaning

Returncode &01 comes from the interface $NKAADS.

### Response

Check the returncode. Repeat the run.

## DRV3161

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV3161 STATEMENT 'CHECK-FILENAME-LENGTH' IS NOT ALLOWED FOR VOLUME-SETS.

### Meaning

The renaming of a volume-set has no effect to the length of the
filenames placed on this volume-set, because files are adressed
with the pubset-ID. Therefore the statement CHECK-FILENAME-LENGHT
is not allowed for volume-sets.

### Response

Use statement CHECK-FILENAME-LENGTH with the SM-pubset, that includes
this volume-set.

## DRV3162

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV3162 DISK CONFIGURATION FOR VSN '(&00)' IS NOT CORRECT.

### Meaning

Possible reasons:
- There are more than two disks with the same VSN.
- There are two disks with the same VSN that do not belong to a
DRV-pubset or DRV-volume-set.
- The discs do not have the same DRV state.
- The pubset or volume set is not running in DRV-DUAL mode.

### Response

Check and corret the disc configuration and repeat the PVSREN run.

## DRV3167

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV3167 INFORMATIONS IN PUBSET CONFIGURATION FILE OF SM-PUBSET '(&00)' DO NOT AGREE WITH THE ALREADY EXISTING INFORMATIONS

### Meaning

One of the following informations in the pubset configuration file does
not agree with the informations in the MRSCAT entry or in the SVL of the
disc:
CATID of the SM-pubset
CATID of the control volume set
Device code of the control volume set

### Response

Check configuration of the SM-pubset.

## DRV3169

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV3169 CONTROL VOLUME SET '(&00)' DOES NOT BELONG TO SM-PUBSET '(&01)'.

### Meaning

The catid of the SM pubset in the SVL of the control volume set does not
agree with already available information. The catid of the control volume
set comes from the MRSCAT entry of the SM pubset or from the SVL of the
volume set.

### Response

Check the MRSCAT entry of the SM pubset or the SVL of the volume set.

## DRV3174

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3174 Volume '(&00)' is not mounted on emulated target disk of disk emulation. Command rejectd.

### Meaning

During processing of the command /FINISH-DISK-EMULATION certain data
structures on the target device are adapted to the new (native) device
type. Onyl the target device maust be on-line.

### Response

Make sure the target discs are on-line:
- Check status of target discs with command /SHO-DISC-STATUS
- If necessary attach target discs with command /ATTACH-DEVICE
- If necessary detach source disks with command /DETACH-DEVICE

## DRV3175

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DRV3175 Check of volume '(&00)' returned error code '(&01)'. Processing aborted.

### Meaning

During processing of the command /FINISH-DISK-EMULATION a check of a
volume with interface NKLMCAL resulted in a negative error code.

### Response

- Check status of target discs with command /SHOW-DISC-STATUS
- Contact system administrator

## DRV3193

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV3193 CONVERSION OF CATALOG '(&00)' TO EXTRA-LARGE FORMAT HAS NOT BEEN COMPLETED. PROCESSING IS ABORTED.

### Meaning

(&00): Pubset id oder volume set id

### Response

Import pubset; conversion of catalog to extra-large format is completed
as part of import processing. After exporting the pubset repeat aborted
DRV processing.

## DRV3199

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DRV3199 INTERNAL PROGRAM ERROR '(&00)'. PROCESSING ABORTED.

### Meaning

The parameter &00 marks the place, where the error has been occured.

### Response

Compile error documents and send them to the systems engineer.

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages