## SPS0B01

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0B01 SPOOLOUT FOR USER FILE '(&00)' ACCEPTED. TSN: '(&01)', SPOOLOUT-NAME: '(&02)'

### Meaning

Printing is initiated by entering the user's
request in the spoolout queue.
(&00): name of the user file
(&01): spoolout TSN
(&02): name of the print job
(NONE): no SPOOLOUT-NAME specified.

## SPS0B02

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0B02 WRITE-DISKETTE FOR USER FILE '(&00)' ACCEPTED. TSN: '(&01)', SPOOLOUT-NAME: '(&02)'

### Meaning

Output to floppy disk is initiated by entering the user's
request in the spoolout queue.
(&00): name of the user file
(&01): spoolout TSN
(&02): name of the spoolout job
(NONE): no SPOOLOUT-NAME specified.

## SPS0B03

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0B03 '(&00)' ERROR CODE '(&01)'. SPOOLOUT REQUEST ABORTED

### Meaning

An error occurred during spoolout request processing.
(&00): Type of error:
= EAM: EAM error;
= REQ: User request error;
= PUTQ: Put queue error;
= REQM: Request memory error;
= DMS: DMS error; (&01) is the corresponding DMS error code
= CAT: Catalog error; (&01) is the corresponding DMS error code.
For more detailed information about the DMS error code, enter
/HELP-MSG in system mode or see BS2000 manual 'System Messages'.
(&01): Error code for (&00):
= 04: Queue routine error;
= 0C: Catalog error;
= 10: EAM processing error;
= 18: Password validation error;
= 1C: Request memory error (LOGOFF only);
= 20: Release memory error (LOGOFF only);
= 24: Parameter validation error;
= 28: Cannot erase foreign file;
= 2C: Nonshareable file;
= 30: Record size and block size are zero;
= 34: Creation date, expiration date or last page used is 0;
= 38: File not SAM, PAM or ISAM;
= 3C: Invalid parameter address;
= 40: EAM OMF (object module file) is nonexistent;
= 44: EAM file contains no data;
= 48: Invalid DELETE-FILE option (FGG (file generation group) file);
= 54: RFA mode not supported in SPOOL;
= 58: DEVIN for a non-SAM tape file;
= 60: Tape without STD labels;
= 64: System file is not PRIMARY;
= 68: System file does not exist;
= 6C: FLUSH/CLOSE error on system file;
= 70: File currently in use.

### Response

None.

## SPS0B04

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0B04 SYNTAX ERROR. COMMAND REJECTED

### Meaning

A syntax error occurred in one of the following commands:
/START-DISKETTE-INPUT
/START-DISKETTE-OUTPUT
/START-PRINTER-OUTPUT
/START-TAPE-OUTPUT
/START-TAPE-REPLAY
/STOP-DISKETTE-INPUT
/STOP-DISKETTE-OUTPUT
/STOP-PRINTER-OUTPUT
/STOP-TAPE-OUTPUT
/STOP-TAPE-REPLAY
/HOLD-SPOOLOUT
/RESUME-SPOOLOUT .

### Response

Correct the command and retry.

## SPS0B05

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0B05 PREVIOUS '(&00)' COMMAND PROCESSING NOT YET COMPLETED. RETRY COMMAND LATER

### Response

The command may be reentered at a later time when spoolout
processing of command (&00) has been completed.

## SPS0B06

Destination: USER-TASK, CONSOLE Routing code: V Weight: 99

Warranty : YES

SPS0B06 SPOOLOUT COMMAND PROCESSING COMPLETED FOR DEVICE '(&00)'

## SPS0B07

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0B07 COMMAND RESTRICTED TO OPERATOR OR SYSTEM SUPPORT STAFF

### Meaning

One of the following privileged commands was given by the user:
/START-DISKETTE-INPUT
/START-DISKETTE-OUTPUT
/START-PRINTER-OUTPUT
/START-TAPE-OUTPUT
/START-TAPE-REPLAY
/STOP-DISKETTE-INPUT
/STOP-DISKETTE-OUTPUT
/STOP-PRINTER-OUTPUT
/STOP-TAPE-OUTPUT
/STOP-TAPE-REPLAY
/HOLD-SPOOLOUT
/RESUME-SPOOLOUT .

## SPS0B08

Destination: USER-TASK, CONSOLE Routing code: V Weight: 99

Warranty : NO

SPS0B08 SPOOLIN COMMAND PROCESSING COMPLETED FOR DEVICE '(&00)'

## SPS0002

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0002 *** NEW SPOOL MASTER TASK READY ***

### Meaning

Following abnormal termination of the SPOOL master task, a new one has
been set up. SPOOL requests can thus be processed again.

## SPS0003

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0003 *** NO RECOVERY POSSIBLE FOR RSO CONTROLLER TASK. RSO NO LONGER AVAILABLE ***

### Meaning

Task creation problem during recovery of RSO controller task.
Spoolout on RSO devices no longer possible.

### Response

Contact the system support staff.

## SPS0004

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0004 *** RSO STARTUP PROBLEM, SPOOL STARTUP CONTINUES ***

### Meaning

The spoolout of RSO requests cannot be
scheduled in this session due to:
- memory allocation problem with the RSO device list or
- RSO task creation problem.

### Response

When RSO is mandatory, dump the BS2000 system for
diagnosis and reload after correction.

## SPS0005

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0005 INVALID INITIALIZATION OF RSO DEVICE TABLE FOR DEVICE '(&00)'

### Meaning

Discrepancy between the fields of the
T3DTBL associated with the (&00) device.
Diagnostic information is available in the error logging file.

### Response

Contact the SPOOL administrator.

## SPS0007

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0007 NO SPOOL REQUESTS FOR FILES STORED ON PVS '(&00)' COULD BE PUT INTO SPOOL WAIT QUEUE

### Meaning

During processing of the /IMCAT command, the
EQUISAMQ file cannot be accessed properly. Diagnostic
information is available in the error logging file.

## SPS0008

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0008 NO SPOOL REQUESTS FOR FILES STORED ON PVS '(&00)' COULD BE SET INTO SPOOL KEEP QUEUE

### Meaning

During processing of the /EXCAT command, the
EQUISAMQ file cannot be accessed properly. Diagnostic
information is available in the error logging file.

## SPS0009

Destination: CONSOLE Routing code: S Weight: 98

Warranty : NO

SPS0009 ERROR '(&01)' WHILE LOCKING FILE '(&00)'. REPLY (R=RETRY; C=CONTINUE)

### Meaning

A /PRINT-FILE command with LOCK-FILE=YES was entered for file (&00) in a
previous session. This file protection would normally apply in the new
session also, but could not be set up during current SPOOL startup.
(&00): name of the file to be locked
(&01): $DCALOCK error code.

### Response

R: the attempt to lock the file is repeated.
Before input, the operator must check whether the volumes are
available.
C: the job can be processed without lock protection.

## SPS0010

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0010 COMMAND NOT AVAILABLE BEFORE SPOOL V3. COMMAND REJECTED

### Meaning

When a SPOOL V3 command is recognized
by an earlier SPOOL version, this message is sent
to explain that the command is not available
until SPOOL V3.

## SPS0011

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0011 SPOOL MEMORY POOL MANAGEMENT INTERNAL ERROR '(&00)'. ABNORMAL TASK TERMINATION INITIATED

### Meaning

(&00): 0020: Bourse mechanism failure (send or receive signal)
0021: Bourse mechanism failure (bourse creation - $NCREBO).

## SPS0012

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0012 DEVICE '(&00)' NOT DEFINED IN SYSTEM

### Meaning

Spoolout cannot continue until the device has been defined.

## SPS0013

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0013 Error '(&00)' during processing of template '(&01)'

### Meaning

&00 : error code:
01: template is not a SAM file
02: unknown function
03: syntax error
04: IF misplaced
05: GTIME error
06: PBBIND error
07: BARCODE error
08: memory error
09: character not supported in BIGLETTER function
10: DMS error
11: internal error
&01 : template filename

## SPS0050

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0050 TASK CANNOT BE DISCONNECTED FROM SPOOL SUBSYSTEM (DSSM PROBLEM). TASK TERMINATED

## SPS0100

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0100 CANNOT OBTAIN CLASS 3 MEMORY. SPOOLOUT TASK ABORTED

## SPS0101

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0101 CANNOT OBTAIN CLASS 4 MEMORY. SPOOLOUT TASK ABORTED

## SPS0102

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0102 SPOOLOUT OF '*SYSOUT' NOT ALLOWED FOR INTERACTIVE TASK. COMMAND REJECTED

## SPS0103

Destination: USER-TASK, CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0103 CARD READER '(&00)' ALREADY IN USE. COMMAND REJECTED

### Meaning

A /START-CARD-INPUT command without REPEAT-INPUT operand has been given
for the card reader (&00) which is already in use.

## SPS0104

Destination: CONSOLE Routing code: S Weight: 98

Warranty : NO

SPS0104 ERROR ON DEVICE '(&00)', FILE '(&02), TSN '(&04)': NO OR INCOMPLETE '(&01)'. CLEAR STACKER. '(&03)' WILL CONTINUE AFTER RESPONSE. REPLY (Y=CONTINUE)

### Meaning

(&00): mnemonic device name
(&01): HEADER PAGE or TRAILER PAGE
(&02): file name
(&03): spoolout.

### Response

Before printing of the incomplete listing is resumed in accordance with
the
appropriate reply, the operator can remove the listings that have already
been completed.

## SPS0105

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0105 LASER PRINTER SPOOLOUT REDIRECTION ONLY ALLOWED FOR PRINTERS. COMMAND REJECTED

### Meaning

The /START-PRINTER-OUTPUT command with the operand
PAGE-PRINTER-OUTPUT=ALLOWED is only allowed for printers. The purpose of
this command is to permit a laser printer spoolout on line printers also.

## SPS0110

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0110 CANNOT RELEASE CLASS 3 MEMORY. SPOOLOUT CONTINUES

## SPS0111

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0111 CANNOT RELEASE CLASS 4 MEMORY. SPOOLOUT CONTINUES

## SPS0112

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0112 '(&00)' PROBLEM, REGISTER CONTENTS '(&01)', MSG ID '(&02)'

### Meaning

An error occurred during internal system calls in SSVADM.
(&00): macro or module name
(&01): contents of registers 0 through 15
(&02): related console message number or blank.

### Response

Ask the system support staff to check the diagnostic data in the
SERSLOG file.

## SPS0113

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0113 INTERNAL ERROR. COMMAND REJECTED

### Meaning

An internal SPOOL error has occurred in the $SPSINF, $SQMGR, $DCTI,
$GTLOCK, $EZST4P or $TANC macro.

### Response

Contact the SPOOL administrator.

## SPS0120

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0120 TSN '(&02)', DEVICE '(&00)': SPOOLOUT COMPLETED FOR FILE '(&01)'

## SPS0121

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0121 SPOOLOUT COMPLETED. DEVICE: '(&00)', TAPE: '(&01)', FILE: '(&02)'

### Meaning

The file (&02) has been written to a replay tape with VSN (&01).
(&00): tape device.

## SPS0122

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0122 SPOOLOUT ABORTED. DEVICE: '(&00)', FILE: '(&01)', TSN: '(&02)'

## SPS0129

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0129 FORM-NAME '(&00)': FORM LENGTH VALUE SET ON PRINTER '(&01)' FOR TSN '(&02)' CONTRADICTS SPOOL PARAMETER FILE

### Meaning

The form length for form name (&00) defined in the SPOOL parameter file
does not match the length specified on the printer panel.
This error leads to a 'LOOP load error'.

### Response

Set the correct form length on the printer panel.

## SPS0130

Destination: CONSOLE Routing code: O Weight: 98

Warranty : NO

SPS0130 TSN '(&01)', DEVICE '(&00)': ERROR DURING SPOOLOUT. REPLY (T=TERMINATE; S=STANDARD; D=DEFER; K=KEEP WITHOUT AUTOMATIC RESTART)

### Response

T: the spoolout job will be removed from the spoolout queue
and the file will be erased if requested.
S: the spoolout job will be returned to the spoolout queue without
its priority being modified. The job will be restarted from
the previous checkpoint.
D: the spoolout job will be returned to the spoolout queue.
Subsequent messages will query the new priority and the restart
type for the deferred job.
K: the spoolout job will be added to the KEEP queue until the operator
restarts it by means of a /RESUME-PRINT-JOB command.
A subsequent message will query the restart type.

## SPS0131

Destination: CONSOLE Routing code: O Weight: 98

Warranty : NO

SPS0131 TSN '(&02)', DEVICE '(&01)': '(&00)' ERROR DURING SPOOLOUT. REPLY (T=TERMINATE; S=STANDARD; D=DEFER; K=KEEP WITHOUT AUTOMATIC RESTART)

### Meaning

(&00): BUFFER LOADING: error while loading a character set (CTB or MXM)
FCB LOADING : error while loading a FORM CONTROL BUFFER
VFB LOADING : error while loading a LOOP
FOB LOADING:
error while loading a FORMS OVERLAY BUFFER
ROT SELECTION : error while selecting a ROTATION value
ROT/TWO-UP SELECTION:
error while selecting a ROTATION value or
a TWO-UP mode value or an HP90-PRINTER
BUFFER FILE COHERENCE:
inconsistency between the number of character sets
in the pool when the command is processed and when
the buffer is loaded
FOB COHERENCE:
inconsistency between the FORMS OVERLAY BUFFER size
when the command is processed and when the buffer
is loaded
PRFILE :
DMS error while trying to access the specified file
LOADING : other error while loading printer buffer
(&01): mnemonic device name.

### Response

T: the spoolout job will be removed from the spoolout queue
and the file will be erased if requested.
S: the spoolout job will be returned to the spoolout queue without
its priority being modified. The job will be restarted from
the previous checkpoint.
D: the spoolout job will be returned to the spoolout queue.
Subsequent messages will query the new priority and the restart
type for the deferred job.
K: the spoolout job will be added to the KEEP queue until the operator
restarts it by means of a /RESUME-PRINT-JOB command.
A subsequent message will query the restart type.

## SPS0132

Destination: CONSOLE Routing code: O Weight: 98

Warranty : NO

SPS0132 TSN '(&01)', DEVICE '(&00)': NEW PRIORITY OF DEFERRED JOB DESIRED? REPLY (<NNN>=NEW PRIORITY 30 THROUGH 255; 'ETX'=NO CHANGE)

## SPS0133

Destination: CONSOLE Routing code: O Weight: 98

Warranty : NO

SPS0133 TSN '(&01)': SPECIFY RESTART TYPE FOR DEFERRED JOB, DEVICE '(&00)'. REPLY (B=BEGINNING; P=PREVIOUS CHECKPOINT; S=START OF PAGE; <NN>= DECIMAL PAGE NUMBER)

### Meaning

The operator is requested to specify where to restart the job that was
deferred on device (&00).

### Response

B: the job will be restarted from the very beginning.
P: the job will be restarted from the previous checkpoint.
S: not valid for card punches; the job will be restarted
from the beginning of the page currently being printed.
<NN>: not valid for card punches; decimal value specifying the
page number from which the job is to be restarted.

## SPS0134

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0134 '(&00)' ERROR IN SPOOLOUT JOB FOR DEVICE '(&01)'

### Meaning

(&00): BUFFER LOADING: error while loading a character set (CTB or MXM)
FCB LOADING : error while loading a FORM CONTROL BUFFER
FORM-OVERLAY-BUFFER LOADING:
error while loading a FORMS OVERLAY BUFFER
ROT SELECTION : error while selecting a ROTATION value
VFB LOADING : error while loading a LOOP
PRFILE :
DMS error while trying to access the specified file
LOADING : other error while loading printer buffer
(&01): logical device name or mnemonic.

## SPS0140

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0140 TSN '(&02)': (&00) OPEN ERROR '(&01)' WHEN OPENING FILE '(&03)'. IN SYSTEM MODE: /HELP-MSG (&00)(&01)

### Meaning

If the error which occurred is OPEN error DMS0D93, DMS0DA9 or PLAxxxx
(except PLA0201 and PLA0205), the job is returned to the KEEP queue in
KEEP mode. For all other codes, the job will be aborted.
For more detailed information about the DMS or PLAM error code enter
/HELP-MSG in system mode or see the BS2000 manual 'System Messages'.

### Response

If the error code is DMS0D93, DMS0DA9 or PLAxxxx (except PLA0201 and
PLA0205), release the TSN (&02) by means of the /RESUME-PRINT-JOB command
if the job can be restarted (e.g. if a tape device is available).

## SPS0145

Destination: CONSOLE Routing code: O Weight: 98

Warranty : NO

SPS0145 TSN '(&03)', DRIVE '(&02)': MOUNT FLOPPY DISK TYPE '(&00)' WITH SECTOR LENGTH '(&01)' FOR SPOOLOUT. REPLY (Y=MOUNTED; N=ABORT)

### Meaning

(&00): floppy disk type: scratch; 3170
one side, single density
two sides, single density
two sides, double density
(&01): sector length: 128, 256, 512, 1024, 2048 bytes
(&02): mnemonic device name
(&03): TSN.

### Response

Y: the operator has mounted the requested floppy disk; task processing
continues.
N: the spoolout of this task will be aborted.

## SPS0146

Destination: CONSOLE Routing code: O Weight: 98

Warranty : NO

SPS0146 TSN '(&03)', DRIVE '(&00)': INVALID FLOPPY DISK TYPE '(&01)'. MOUNT FLOPPY DISK '(&02)'. REPLY (R=RETRY; T=TERMINATE; D=DEFER; K=KEEP; A=ACCEPT)

### Meaning

(&00): mnemonic device name
(&01): type of floppy disk: scratch
one side, single density
two sides, single density
two sides, double density + sector length
(&02): requested floppy disk (type + sector length).

### Response

R: retry with the requested floppy disk
T: abort spoolout
D: defer the job
K: keep the job without automatic restart
A: accept the invalid type of floppy disk (&01).

## SPS0150

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0150 '(&00)' MACRO ERROR. RETURN CODE '(&01)' FOR DEVICE '(&02)'

### Meaning

(&00): (ENAMP or REQMP) macro error.

## SPS0151

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0151 TSN '(&01)': SYSTEM EXIT ROUTINE '(&00)' DOES NOT EXIST

### Meaning

The exit routine requested by the job with the TSN (&01) does not exist.

## SPS0152

Destination: CONSOLE Routing code: S Weight: 98

Warranty : NO

SPS0152 TSN '(&01)': SYSTEM EXIT ROUTINE '(&00)' NOT ACTIVE. REPLY (R=RETRY; T=ABORT)

### Meaning

The SPOOL task is waiting for a reply, allowing the operator to activate
the exit routine in the meantime.

### Response

R: try again with the exit routine activated by the operator.
T: the exit routine will not be called; the job will be aborted.

## SPS0153

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0153 EXIT ROUTINE '(&00)' NOT ACTIVE. JOB IS SUSPENDED

### Meaning

(&00): EX090 or EX095

### Response

The SPOOL job can be restarted with the /RESUME-PRINT-JOB command.
The RESTART-POSITION operand defines the point from which the spoolout
file
is to be output again.

## SPS0154

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0154 SPOOLOUT RESTARTED WITH 'RESTART-POSITION=CURRENT-PAGE'

### Meaning

Spoolout is restarted from the beginning of the page being printed.

## SPS0155

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0155 INCOMPATIBLE CODED CHARACTER SET '(&00)' REPORTED BY XHCS FOR FILE '(&01)' ON DEVICE '(&02)'

### Meaning

XHCS is not able to convert the coded character set '(&00)'.
Job is kept.
(&00): Coded Character Set Name
(&01): file name
(&02): device name

### Response

Contact the system support staff

## SPS0156

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0156 WARNING: NO XHCS CONVERSION HAS BEEN PERFORMED

### Meaning

A Coded Character Set Name (CCSN) different from EDF03IRV is
associated to the printed file and
- either the CONTROL-CHARACTER operand of the /PRINT-FILE
command is different to NO
- or a translation table has been specified.

## SPS0160

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0160 '(&00)' ERROR CODE '(&01)' FOR TSN '(&02)'. INPUT OR TAPE OUTPUT FILE COULD NOT BE CLOSED OR DELETED

### Meaning

Information for diagnostic purposes only.

## SPS0165

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0165 INPUT I/O ERROR. USER ERROR FILE WILL BE OUTPUT ON DEVICE '(&00)'

### Meaning

If the user has specified ERROR=ACCEPT, the operator is notified of the
occurrence of the I/O error and a record is written to the USER-ERROR file
which is output at the end of the job upon the device (&00).

## SPS0166

Destination: CONSOLE Routing code: S Weight: 98

Warranty : NO

SPS0166 TSN '(&03)': '(&00)' ERROR '(&01)' DURING SPOOLOUT OF FILE '(&02)'. REPLY (T=TERMINATE; S=STANDARD; D=DEFER; K=KEEP WITHOUT AUTOMATIC RESTART)

### Meaning

For more detailed information about the error code (&00)(&01) enter
/HELP-MSG in system mode or see the BS2000 manual 'System Messages'.

### Response

T: the spoolout job will be removed from the spoolout queue
and the file will be erased if requested.
S: the spoolout job will be returned to the spoolout queue without
its priority being modified. The job will be restarted from
the previous checkpoint.
D: the spoolout job will be returned to the spoolout queue.
Subsequent messages will query the new priority and the restart
type for the deferred job.
K: the spoolout job will be added to the KEEP queue until the operator
restarts it by means of a /RESUME-PRINT-JOB command.
A subsequent message will query the restart type.

## SPS0167

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0167 ERROR IN JOIN FILE ACCESS FOR USER ID VALIDATION. COMMAND REJECTED

### Response

Inform the system support staff.

## SPS0168

Destination: USER-TASK, CONSOLE Routing code: I Weight: 99

Warranty : YES

SPS0168 UNKNOWN USERID '(&00)'. COMMAND REJECTED

### Response

Verify the user ID given in the command or ask the operator to do so.

## SPS0169

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0169 MOUNT FLOPPY DISK '(&01)' IN DRIVE '(&00)'

## SPS0170

Destination: USER-TASK, CONSOLE Routing code: S Weight: 98

Warranty : NO

SPS0170 TSN '(&01)': RESTART PAGE NUMBER '(&00)' GREATER THAN FILE CAPACITY. REPLY (T=ABORT; <NN>=NEW PAGE NUMBER)

### Meaning

The page number entered in response to message SPS0133 is too high.

### Response

T: the spoolout job will be removed from the spoolout queue.
<NN>: decimal value specifying the page number from which the job is to be
restarted.

## SPS0171

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0171 NO LOCAL SPOOLOUT JOB PRESENT

### Meaning

At the moment no spoolout job of the requested type 4, 5 or 6 is present.

## SPS0173

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0173 TSN '(&04)', DEVICE '(&03)': USER WITH ID '(&00)' WRITES FILE '(&01)' TO FLOPPY DISK WITH VOLUME '(&02)'

### Meaning

(&00): user ID
(&01): file name
(&02): VOLUME or, if the floppy disk has no VOLUME, 'XXXXXX'
(&03): mnemonic device name.

### Response

Allocate the floppy disk to the appropriate user ID wherever necessary
(e.g. in the accounting documents).

## SPS0174

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0174 TSN '(&02)', PRINTER '(&01)': ONLY '(&00)' FORM NAMES WILL BE ACCEPTED

### Meaning

Only the form names specified for printer (&01) in one of the following
commands can be entered in response to message SPS0200.
/START-PRINTER-OUTPUT
/START-TAPE-OUTPUT
/START-TAPE-REPLAY .

## SPS0175

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0175 TSN '(&02)', DEVICE '(&01)': ONLY '(&00)' FORMS OVERLAY NAMES WILL BE ACCEPTED

### Meaning

Only forms overlay names specified in the FORMS-OVERLAY operand of the
/START-PRINTER-OUTPUT command for device (&01) are accepted as valid
responses to message SPS0232.

## SPS0176

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0176 FILE '(&00)' NOT FOUND. SPOOL CANNOT BE LOADED. RETRY IS STILL POSSIBLE

### Meaning

The file containing the SPOOL OML is not found.

### Response

Verify the name of the SPOOL OML file. If necessary, import the file to
user ID $TSOS. Retry SPOOL startup using the /START-SPOOL command.

## SPS0177

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

SPS0177 SPOOLIN STARTED FOR FILE '(&00)' ON FLOPPY DISK '(&01)' IN DRIVE '(&02)'

## SPS0178

Destination: USER-TASK, CONSOLE Routing code: P Weight: 99

Warranty : YES

SPS0178 FILE '(&00)' COULD NOT BE UNLOCKED WHEN CANCELING TSN '(&01)'. COMMAND COMPLETED

### Meaning

The file (&00) was being printed with the LOCK-FILE=YES operand when a
/CANCEL-JOB or /CANCEL-PRINT-JOB command was issued for TSN (&01).
Although unlock processing was unsuccessful, the /CANCEL-JOB or ,
the /CANCEL-PRINT-JOB command was executed completely.

## SPS0179

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0179 TSN '(&03)': USER ERROR '(&00)' FOR FILE '(&02)' ON PRINTER '(&01)'

### Response

Correct the error and retry the /PRINT-FILE command.

## SPS0180

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0180 TSN '(&02)': USER ERROR WHILE PRINTING FILE '(&00)' ON PRINTER '(&01)'. NUMBER OF LINES PER PAGE GREATER THAN PERMITTED IN 'LOOP'

### Meaning

The user attempted to print more lines than permitted by the LOOP
loaded on printer (&01).
After this message the job will be aborted and message SPS0345 will be
printed on the trailer page.

## SPS0184

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0184 TSN '(&02)', DRIVE '(&01)': FLOPPY DISK WITH VOLUME '(&00)' IS NOT A SCRATCH FLOPPY DISK

### Meaning

The (further) spoolout will be made on a scratch floppy disk because
- no VOLUME has been specified or
- the VOLUME list is full.
Scratch floppy disks have the following attributes:
- no owner ID,
- volume is accessible,
- no write protection,
- file is accessible,
- expiration date reached.
(&01): mnemonic device name.

### Response

Insert a scratch floppy disk into the drive.

## SPS0185

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0185 USER ERROR WHILE PRINTING FILE '(&00)' ON DEVICE '(&01)', TSN '(&02)'. INVALID CONTROL BYTE. JOB ABORTED. CONTACT USER

### Meaning

The error occurred when loading the control byte on printer (&01).
Possible reasons:
- an invalid control byte,
- an invalid control byte number at the top of the page for a file
to be printed with CONTROL-CHARACTERS=PHYSICAL.
After this message the job will be aborted and message SPS0345 will be
printed on the trailer page.
(&01): mnemonic or logical device name.

## SPS0186

Destination: CONSOLE Routing code: I Weight: 98

Warranty : NO

SPS0186 TSN '(&02)': FLOPPY DISK(S) '(&00)' MOUNTED IN DRIVE '(&01)' FOR SPOOLOUT? REPLY (Y=YES; N=NO)

### Meaning

One or more floppy disks are requested for spoolout.
(&00): list of VOLUMEs
(&01): mnemonic device name.

### Response

Y: the requested floppy disk(s) is/are mounted.
N: terminate spoolout for this TSN.

## SPS0187

Destination: CONSOLE Routing code: I Weight: 98

Warranty : NO

SPS0187 WRONG FLOPPY DISK '(&00)' IN DRIVE '(&01)'. MOUNT CORRECT FLOPPY DISK '(&02)'. REPLY (R=RETRY; T=TERMINATE)

### Meaning

The operator is requested to insert the correct floppy disk (&02) and to
either continue or terminate the job as appropriate.
(&00): VOLUME of the invalid floppy disk
(&01): mnemonic device name of the floppy disk drive
(&02): VOLUME of the correct floppy disk.

### Response

R: the correct floppy disk has been mounted; retry the job.
T: the correct floppy disk is not available; abort the job.

## SPS0188

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0188 LIST OF SPECIFIED VOLUMES FOR TSN '(&00)' EXHAUSTED. OUTPUT CONTINUED ON SCRATCH FLOPPY DISK(S)

### Meaning

Scratch floppy disks have the following attributes:
- no owner ID,
- volume is accessible,
- no write protection,
- file is accessible,
- expiration date reached.

## SPS0189

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0189 TSN '(&03)': PROCESSING OF FILE '(&00)' ON FLOPPY DISK '(&01)' IN DRIVE '(&02)' COMPLETED

## SPS0190

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0190 FILE '(&00)' READ FROM FLOPPY DISK '(&01)' IN DRIVE '(&02)'

## SPS0191

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0191 TSN '(&03)': CONTINUE FILE '(&00)' ON NEXT FLOPPY DISK. OUTPUT TO FLOPPY DISK '(&01)' IN DRIVE '(&02)' COMPLETED

### Meaning

The end of floppy disk (&01) has been reached while writing
file (&00). The file is continued on the next floppy disk in the drive
with
mnemonic device name (&02).

## SPS0192

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0192 TSN '(&03)': RECORD TRUNCATION FOR FILE '(&00)' ON FLOPPY DISK WITH VOLUME '(&01)' IN DRIVE '(&02)'

### Meaning

Some of the records in the input file are longer than the record size
specified in the /WRITE-DISKETTE command (OUTPUT-RECORD-SIZE operand)
or the corresponding default value.
The appropriate records have been truncated accordingly.

## SPS0193

Destination: CONSOLE Routing code: O Weight: 99

Warranty : NO

SPS0193 GIVEN RESTART POSITION NOT VALID FOR FLOPPY DISK. COMMAND REJECTED

### Meaning

For floppy disk devices, only RESTART-POSITION=BEGIN-OF-SPOOLOUT or
RESTART-POSITION=CURRENT-PAGE is allowed in the /HOLD-PRINT-JOB command.

### Response

Correct the command and try again.

## SPS0194

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0194 DRIVE '(&00)' ALREADY ALLOCATED TO FLOPPY DISK '(&01)'. COMMAND REJECTED

## SPS0195

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0195 DEVICE '(&00)' NOT ASSIGNED TO '(&01)'. COMMAND REJECTED

### Meaning

One of the following commands is rejected:
/STOP-DISKETTE-OUTPUT
/STOP-DISKETTE-INPUT
/STOP-PRINTER-OUTPUT
/STOP-TAPE-OUTPUT
/STOP-TAPE-REPLAY .
(&00): device mnemonic or printer logical name.
(&01): SPOOL, SPOOLIN or SPOOLOUT.

## SPS0196

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0196 TSN '(&04)': ERROR ON TRACK AND SECTOR '(&00)' ON FLOPPY DISK WITH VOLUME '(&02)' IN DRIVE '(&01)', FILE '(&03)'

### Meaning

A defective sector has been discovered on the floppy disk in drive (&01)
during the session.
(&00): track and sector in the format 'nnnnn'.

### Response

If there are too many defective sectors on the floppy disk, the job
can be either repeated or suspended.

## SPS0197

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0197 TSN '(&03)': USER '(&00)' NOT AUTHORIZED TO WRITE TO FLOPPY DISK WITH VOLUME '(&01)' IN DRIVE '(&02)'

### Meaning

The floppy disk does not belong to the user and is not a scratch
floppy disk.

## SPS0198

Destination: USER-TASK, CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0198 FLOPPY DISK DEVICE '(&00)' IS ASSIGNED AS INPUT DEVICE

## SPS0199

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0199 ALL FLOPPY DISK DEVICES ARE IN USE OR DETACHED. TRY COMMAND LATER

## SPS0200

Destination: CONSOLE Routing code: S Weight: 98

Warranty : NO

SPS0200 TSN '(&02)': FORM '(&00)' MOUNTED ON PRINTER '(&01)'? REPLY (Y=YES; N=NO; C,<FORMNAME>=NEW FORM)

### Meaning

The operator has to mount the required form (&00) on printer (&01).
If this form is not available, the operator may choose another one
out of the set selected (perhaps implicitly) in a previous
/START-PRINTER-OUTPUT command.

### Response

Y: the form has been mounted, printing will start
N: release the printer
C,<formname>: another form (identified by <formname>) has been
mounted on printer (&01).

## SPS0201

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0201 DEVICE '(&00)' NOT ASSIGNED TO SYSTEM

### Meaning

Device acquire failed. Possible reasons :
- the device is not defined in the
system device configuration;
- the device is not attached to the system;
- the device is attached but not accessible;

### Response

Contact operator to make the device accessible.

## SPS0202

Destination: USER-TASK, CONSOLE Routing code: S Weight: 98

Warranty : NO

SPS0202 USER ID IN /START-DISKETTE-INPUT DIFFERENT FROM USER ID '(&00)' ON FLOPPY DISK '(&01)' ON DEVICE '(&02)'. REPLY (I=IGNORE; T=TERMINATE; R=RETRY)

### Meaning

Possible reasons:
Spoolin without JCL: The user ID specified in
the /START-DISKETTE-INPUT command is not
the same as that stored on the FD.
Multivolume file: The FDs have different IDs.

### Response

I: Ignore the error, continue floppy disk processing
T: Terminate spoolin processing
R: Retry spoolin processing with the next floppy disk.

## SPS0203

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0203 DEVICE '(&00)' IS NOT BUSY. CANNOT RESPOOL OR SUSPEND

### Meaning

Operator tries to do a respool or a suspend on a device
which is not running. No effect

## SPS0204

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0204 SYSTEM ERROR. SPOOLOUT TASK SUSPENDED INDEFINITELY ON '(&00)'. /HOLD-PRINT-JOB NOT PROCESSED

### Meaning

A spoolout task using an output device has been suspended indefinitely.
The operator tried to do a respool or to defer the spoolout, but this
attempt failed.

## SPS0206

Destination: CONSOLE Routing code: T Weight: 98

Warranty : NO

SPS0206 TSN '(&00)' REQUESTING TAPE DEVICE. REPLY (<MN>=MNEMONIC DEVICE NAME; NO=NO TAPE AVAILABLE)

### Meaning

The user with the TSN (&00) has issued a spoolout command or macro with
the
specification TAPE=YES or a /LOGOFF TAPE command.

### Response

MN: mnemonic name of the device to which spoolout is to be directed.
NO: no tape device is available at present.
The message will be displayed again later.

## SPS0207

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0207 '(&00)' PROCESSING COMPLETED ON DEVICE '(&01)'

### Meaning

If device (&01) is available, or at the end of the current output, the
device is deallocated after entering one of the following commands:
/STOP-DISKETTE-INPUT
/STOP-DISKETTE-OUTPUT
/STOP-PRINTER-OUTPUT
/STOP-TAPE-OUTPUT
/STOP-TAPE-REPLAY.
(&00): SPOOLIN / SPOOLOUT / REPLAY.

## SPS0209

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0209 FILE '(&00)' DOES NOT HAVE VARIABLE-LENGTH RECORDS. SPOOL TASK ABORTED. FILE ERASED

### Meaning

The user has requested spoolout of an EAM file named (&00)
with fixed-length records.

## SPS0210

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0210 '(&00)'-ERROR: DMS ERROR '(&01)' IN '(&02)' DURING SPOOLOUT OF TSN '(&03)'. IN SYSTEM MODE: /HELP-MSG DMS(&01). CONTACT SYSTEM SUPPORT STAFF

### Meaning

A DMS error has been detected during SPOOL file processing.
This means that spoolout cannot be continued on a 3343 or 3337 printer.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.
(&00): 'OPEN' : the error occurred when opening the file
'CLOSE': the error occurred when closing the file
'DMS' : the error occurred when processing the file
(&02): name of the SPOOL file
(&03): TSN allocated.

### Response

Ask the system support staff to recover file (&02).

## SPS0211

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0211 '(&00)' RECORD WITH KEY '(&01)' NOT FOUND IN FILE '(&02)', TSN '(&03)'. CONTACT SYSTEM SUPPORT STAFF

### Meaning

During the loading phase, no record of type (&00) with key (&01)
has been found in the SPOOL system file.
(&00): CHAR = character set
POOL = character set pool
FOB = form overlay buffer
LOOP = FCB or LOOP
IMAGE = image (user file which includes a LOOP record and
character)
FORM = form
B-ID = Band-id
PREFORM = preform
(&01) : printable form of the record key
(&02) : name of the file : PRFILE
(&03) : TSN

## SPS0212

Destination: CONSOLE Routing code: O Weight: 98

Warranty : NO

SPS0212 TSN '(&01)': PRESS PAPER HOMING KEY ON PRINTER '(&00)'. THEN REPLY (TSN. =CONTINUE)

### Meaning

- Invalid I/O operation after pressing the paper homing key:
LOOP not loaded.
- Invalid I/O operation after loading the LOOP: paper homing suppressed.
(&00): mnemonic device name.

## SPS0215

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0215 SYSTEM ERROR. DEFERRED JOB '(&01)' ON DEVICE '(&00)' CANNOT BE ACTIVATED. JOB ADDED TO SHUTDOWN QUEUE

### Meaning

The suspended spoolout job could not be entered into the ACTIVE queue due
to an error in the defer operation.
The spoolout job will stay in the SHUTDOWN queue until the next warm
start.
In the case of a cold start the spoolout job is lost.
(&00): mnemonic or logical name of the device on which the operator
deferred the task.

## SPS0216

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0216 DEFERRED SPOOLOUT JOB ON DEVICE '(&00)' WILL REMAIN IN SHUTDOWN QUEUE

### Meaning

Device = *FILTER means that the job has been deferred
by a filter controller

### Response

The next startup must be a warm start.
In the case of a cold start the deferred spoolout job will be lost.

## SPS0217

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0217 TSN '(&00)' DEFERRED

## SPS0218

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0218 RESPOOL OR SUSPEND REQUEST NOT POSSIBLE FOR DEVICE '(&00)'AT THE MOMENT

### Meaning

Operator tries to respool or suspend a job active on
a device for which a previous /HOLD-PRINT-JOB command has not
yet been completed.
or the operator tries to respool or suspend an active job
for which the header or the trailer page is currently printed
and so, cannot be interrupted
and so, cannot be interrupted

## SPS0221

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0221 /HOLD-PRINT-JOB REJECTED FOR TAPE DEVICE '(&00)'

### Meaning

On a tape device in output mode it is not permitted to defer or to
respool the spoolout. The /HOLD-PRINT-JOB command is rejected.

## SPS0224

Destination: CONSOLE Routing code: O Weight: 98

Warranty : NO

SPS0224 TSN '(&02)': SAMPLE PRINTOUT REQUIRED ON PRINTER '(&00)' OR SPOOLOUT-NAME '(&01)' WITH FORM '(&03)'? REPLY (Y=YES; N=NO; <N>=NUMBER OF PAGES 1 THROUGH 9)

### Meaning

The operand PRINT-SAMPLE was specified in a previous /START-PRINTER-OUTPUT
command. The operator is therefore asked every time the form is changed
whether a sample printout is desired for this form.

### Response

Y : sample printout of one page required
N : no sample printout required
<N>: sample printout of n pages required (n = 1 to 9).

## SPS0225

Destination: CONSOLE Routing code: O Weight: 98

Warranty : NO

SPS0225 TSN '(&01)': SAMPLE PRINTOUT FOR '(&00)' CORRECT? REPLY (Y=YES; N=NO)

### Meaning

The sample printout for form (&00) has been printed. The operator has
to check the result for errors.

### Response

Y: the form alignment is correct; regular spoolout will begin.
N: the form alignment must be corrected before entering the reply.
The sample printout is repeated.

## SPS0226

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0226 DMS ERROR '(&00)' WHEN ACCESSING FILE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## SPS0227

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0227 '(&03)' '(&00)' MISSING IN FILE '(&01)' FOR DEVICE TYPE '(&02)'

### Meaning

(&00): key of the missing record.
(&01): file name.
(&02): device type.
(&03): object type.
The SPOOLOUT of the /PRINT-FILE or /PRINT-DOCUMENT can not be directed to
HP or HP90 or
or 2050-APA or 2090-APA or 2090-TWIN or LP-EMUL or LP devices.

## SPS0228

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0228 PREFORM, FORM, VFB, CROSS VFB, FOB, CHARS POOL, CTB, TTB, MXM, FORMDEF OR PAGEDEF RECORD WITH KEY '(&00)' MISSING IN FILE '(&01)'

### Meaning

(&00): key of the missing record.
(&01): file name.
The SPOOLOUT of the /PRINT-FILE or /PRINT-DOCUMENT can not be directed to
HP or HP90 or
or 2050-APA or 2090-APA or 2090-TWIN or LP-EMUL or LP devices.

## SPS0229

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0229 TSN '(&01)': NO CHAIN CORRESPONDS TO BAND ID RECORD '(&00)'

### Meaning

The band ID record (&00) defined in the SPOOL file has no corresponding
print chain for the 3337 Printer.

## SPS0230

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0230 INVALID 'CHARACTER-SETS' OPERAND '(&00)' FOR FILE '(&01)'. COMMAND REJECTED

### Meaning

(&00): name of the invalid character set
(&01): name of the file containing the invalid character set.

### Response

Correct the CHARACTER-SETS operand and retry the command.

## SPS0231

Destination: CONSOLE Routing code: S Weight: 98

Warranty : NO

SPS0231 TSN '(&02)': PRINTER '(&00)' REQUIRES PRINT CHAIN FOR BAND ID '(&01)'. CHAIN MOUNTED? REPLY (Y=YES; N=NO; I=IGNORE)

### Meaning

The appropriate chain for band ID (&01) has not been mounted in the 3337
printer (&00).
(&00): mnemonic device name of the printer.

### Response

Y: the print chain has been mounted.
N: the print chain cannot be mounted.
I: the message is ignored. Spoolout processing continues with the print
chain which is mounted on the printer at the moment.

## SPS0232

Destination: CONSOLE Routing code: O Weight: 98

Warranty : NO

SPS0232 MOUNT FORMS OVERLAY '(&00)' ON PRINTER '(&01)' FOR TSN '(&02)'. REPLY (Y=YES; N=NO; C,<OVERLAYNAME>=MODIFY)

### Meaning

The required forms overlay (&00) must be mounted on the laser printer.
If this forms overlay is not available, the operator may select another
one, provided it is included in the set specified (perhaps implicitly)
in a previous /START-PRINTER-OUTPUT command.

### Response

Y: the forms overlay has been mounted.
N: release the printer.
C,<overlayname>: another forms overlay (identified by <overlayname>)
has been mounted on printer (&01).

## SPS0233

Destination: CONSOLE Routing code: O Weight: 98

Warranty : NO

SPS0233 PRESS 'TEST PRINT' KEY FOR SAMPLE PRINTOUT ON PRINTER '(&00)'. THEN REPLY (TSN.=JOB CONTINUES)

### Meaning

SPOOLOUT has loaded a page of the sample file for the 3352 laser printer
identified by (&00). The operator can have this page printed and modify
the paper alignment if necessary.

### Response

The operator must take the following steps:
1) Press the 'TEST PRINT' key
2) Press the 'START' key as often as required
3) When finished, press the 'STOP' key
4) Press the 'TEST PRINT' key again
5) When finished, press 'ETX'.

## SPS0235

Destination: CONSOLE Routing code: O Weight: 98

Warranty : NO

SPS0235 ENTER NUMBER OF LINES FOR SAMPLE PRINTOUT ON DEVICE '(&00)' FOR SPOOLOUT-NAME '(&01)'. REPLY (<NNN>=NUMBER OF LINES FROM 1 THROUGH 255)

## SPS0236

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0236 SYSTEM ERROR. SPOOLOUT ADMINISTRATOR BOURSE DESTROYED. TAKE DUMP

### Meaning

The bourse mechanism used for spoolout or scheduler interface has detected
an error and has crashed. Therefore it is impossible to continue spoolout.

### Response

Take a dump for future analysis.

## SPS0238

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0238 TSN '(&02)': DMS ERROR '(&00)' DURING SPOOL PROCESSING OF FILE '(&01)'. SPOOLOUT JOB ABORTED. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

An error has occurred either when cataloging an input replay tape file
(via a FILE macro) or when opening an input replay tape file or a user
tape file.
For more detailed information about the DMS error code enter /HELP-MSG
in system mode or see the BS2000 manual 'System Messages'.

## SPS0242

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0242 NO SPOOLOUT JOB IN REPLAY QUEUE

## SPS0243

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0243 NO RBP PRINTER ACTIVE

## SPS0244

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0244 FILE '(&00)' IS NOT REQUESTED, HENCE IT CANNOT BE EXCEPTED. COMMAND REJECTED

### Meaning

Contradiction in command /START-DISKETTE-INPUT.
A nonselected file is to be excepted.

## SPS0245

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0245 BYPASS INDICATOR ON FLOPPY DISK POSITIONED FOR FILE '(&00)'

### Meaning

A hardware problem was detected on a floppy disk for file (&00),
which cannot be read.

## SPS0246

Destination: USER-TASK, CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0246 SYSTEM ERROR. CANNOT OBTAIN CLASS 4 MEMORY. COMMAND REJECTED

### Meaning

The module SCPIPTO cannot get class 4 memory for its work area because
the system has no more resources.

## SPS0247

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0247 DMS ERROR '(&00)' DURING SPOOLIN FROM FILE '(&01)' ON FD DEVICE '(&02)'

### Meaning

A DMS or REQM error occurred during spoolin processing.
The spoolin task is continued if possible or terminated.
For more detailed information about any DMS error code enter
/HELP-MSG in system mode or see the BS2000 manual 'System Messages'.
(&00): DMS error code or 'REQUEST MEMORY'.

## SPS0248

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0248 SPOOLIN FROM FLOPPY DISK '(&00)' COMPLETED FOR FILE '(&01)'

### Meaning

The spoolin of the floppy disk file has been successfully completed.

## SPS0249

Destination: CONSOLE Routing code: I Weight: 98

Warranty : NO

SPS0249 HDR1 LABEL MISSING FOR CONTINUATION OF FILE '(&00)' ON FLOPPY DISK DRIVE '(&01)'. REPLY (R=RETRY; T=CLOSE FILE)

### Meaning

The floppy disk required for spoolin does not contain the continuation
of file (&00).
Possible error causes:
- The record length in the HDR1 label does not match that of the previous
floppy disk.
- The multivolume indicator or the volume sequence is invalid.

### Response

R: Continue spoolin with a different, valid floppy disk.
T: The file is closed. SPOOLIN regards this file as complete and
continues processing with the current volume.

## SPS0250

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0250 INVALID LABEL (VOL1, HDR1, DDR1) ON FD DEVICE '(&00)'. PROCESSING CONTINUES WITH NEXT FLOPPY DISK

## SPS0252

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0252 HDR1 LABEL ERROR FOR FILE '(&00)' ON FD DEVICE '(&01)'. FILE IS SKIPPED

### Meaning

There is an error in the HDR1 label at the BOE (beginning of extent),
EOE (end of extent) or EOD (end of data) address.

## SPS0253

Destination: CONSOLE Routing code: I Weight: 98

Warranty : NO

SPS0253 CONTINUATION OF FILE '(&00)' NOT FOUND ON FLOPPY DISK DRIVE '(&01)'. REPLY (R=RETRY, T=CLOSE FILE)

### Meaning

The floppy disk required for spoolin does not contain the continuation
of file (&00).
Possible error cause:
- New file name does not match the old file name.
- The user IDs do not match.

### Response

R: Continue spoolin with a different, valid floppy disk.
T: The file is closed. SPOOLIN regards this file as complete and
continues processing with the current volume.

## SPS0254

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0254 HDR1 LABEL ERROR FOR FIRST EXTENT OF FILE '(&00)' ON FD DEVICE '(&01)'. FILE IS SKIPPED

### Meaning

Possible error causes:
- The multivolume indicator is invalid.
- The volume sequence number contained in the HDR1 label of the first
extent of a floppy disk file is invalid.

## SPS0255

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0255 UNRECOVERABLE I/O ERROR ON FD DEVICE '(&00)'. SPOOLIN TASK ABORTED

## SPS0256

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

SPS0256 INVALID FILE NAME SPECIFIED IN /DATA OF FILE '(&00)' ON FD DEVICE '(&01)'. DATA BELONGING TO THIS NAME IS SKIPPED

### Meaning

(&00) is the file where SPOOLIN has detected a record containing
a /DATA command specifying an invalid file name.

## SPS0257

Destination: CONSOLE Routing code: J Weight: 30

Warranty : NO

SPS0257 FIRST RECORD OF FILE '(&00)' ON FD DEVICE '(&01)' NOT A VALID /SET-LOGON-PAR. FILE IS SKIPPED

## SPS0258

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0258 FILE '(&00)' NOT PRESENT ON FD VOLUME '(&01)' ON FD DEVICE '(&02)'. TASK TERMINATED

### Meaning

The file specified in the /START-DISKETTE-INPUT command cannot be found
on the floppy disk.

## SPS0259

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0259 I/O ERROR WHEN PROCESSING 'CLOSE DEVICE' OF A FD IN DEVICE '(&00)'

## SPS0260

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0260 'OPEN VOLUME' ERROR ON FD DEVICE '(&00)'. SPOOLIN TASK ABORTED

### Meaning

An error occurred during the OPEN VOLUME processing of a floppy disk.
This error is likely to be an I/O error.

## SPS0261

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0261 HOPPER OF FD DEVICE '(&00)' EMPTY. FEED THE HOPPER

### Meaning

The hopper of the floppy disk station 3170 is empty.

### Response

Continue spoolin by inserting new floppy disks.
If no more floppy disks are available, stop the spoolin process.

## SPS0262

Destination: CONSOLE Routing code: I Weight: 98

Warranty : NO

SPS0262 PROCESSING TERMINATED FOR FLOPPY DISK ON DRIVE '(&00)'. INSERT NEW FLOPPY DISK. REPLY (Y=CONTINUE; N=ABORT)

### Meaning

A new floppy disk is required for spoolin/spoolout.
(&00): device mnemonic

### Response

Y: a floppy disk has been mounted; continue processing.
N: the job is aborted and lost.

## SPS0263

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0263 TSN '(&02)': USER ERROR FOR FILE '(&00)' ON PRINTER '(&01)'. LOOP CHANNEL NOT FOUND. CONTACT USER

### Meaning

SPOOLOUT has detected a user error while printing user file (&00).
A channel feed has been specified for a channel on printer (&01) but
does not exist in the vertical format buffer.
The job is aborted following this message.
Message SPS0345 is printed on the trailer page.

## SPS0264

Destination: CONSOLE Routing code: J Weight: 50

Warranty : NO

SPS0264 JOB REJECTED: '(&00)', FOR FILE '(&01)', ON VOLUME '(&02)', DEVICE '(&03)'

### Meaning

The spoolin job is rejected by job management. The reason is indicated
by a message from job management.
(&00): message from job management
(&01): floppy disk file name
(&02): volume ID
(&03): device mnemonic.

### Response

The file is skipped and the next one is opened.

## SPS0265

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0265 SPOOLOUT FAMILY FOR JOB WITH TSN '(&00)' NOT ENTIRELY IN QUEUE. COMMAND REJECTED

### Meaning

The user or operator is not allowed
- to change the priority of a spoolout job
- to cancel a spoolout job
if the spoolout family in question is not yet completely in the queue.

## SPS0266

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0266 SPOOL MASTER TASK DID NOT REPLY WITHIN TIME LIMIT

### Meaning

Due to a communication problem with the SPOOL master task, the SPOOL
request is terminated unsuccessfully.

### Response

Retry the command later.

## SPS0267

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0267 /START-SUBSYSTEM (&00) OR /RESUME-SUBSYSTEM (&00) HAS ALREADY BEEN ISSUED. COMMAND REJECTED

### Meaning

A /START-SUBSYSTEM or /RESUME-SUBSYSTEM command is currently not allowed
because:
- the subsystem is already loaded and coexistence is not allowed.
- the subsystem is in create/resume but the action is not yet completed.
(&00): subsystem name.

## SPS0268

Destination: CONSOLE Routing code: I Weight: 98

Warranty : NO

SPS0268 USER ID '(&00)' REQUESTS FLOPPY DISK(S) '(&01)' IN DRIVE '(&02)' FOR SYSDTA ASSIGNMENT. REPLY (Y=YES; N=NO)

### Response

Y: the requested floppy disk has been mounted
N: no SYSDTA assignment is made.

## SPS0269

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0269 'LOCK-FILE=YES' IS NOT ALLOWED FOR TAPE FILES. COMMAND REJECTED

## SPS0270

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0270 SPOOL CANNOT BE LOADED

### Meaning

Possible reason:
- Incomplete SPOOL OML
- DLL error (refer to previous console messages).

### Response

Reload SPOOL after a new system startup.

## SPS0271

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0271 SPOOL TASK CANNOT BE CREATED. RETRY STARTUP

### Meaning

Creation of the SPOOL task has failed during execution of the
SPOOL startup procedure.

## SPS0272

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0272 *** SPOOL (VERSION (&00)) READY ***

## SPS0273

Destination: CONSOLE Routing code: S Weight: 98

Warranty : NO

SPS0273 FLOPPY DISK '(&00)' REQUESTED ON DRIVE '(&01)' FOR SPOOLIN. REPLY (Y=YES; N=NO)

### Meaning

A floppy disk has been requested for /START-DISKETTE-INPUT processing.

### Response

Y: the requested floppy disk has been mounted; continue spoolin
N: reject /START-DISKETTE-INPUT processing; suspend spoolin.

## SPS0274

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0274 DEVICE '(&00)' NOT ACCESSIBLE. SPOOLOUT TASK ABORTED

### Meaning

The first access to device (&00) has failed.

### Response

Contact hardware maintenance.

## SPS0275

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0275 SPOOLOUT JOB '(&00)' CANNOT BE RELEASED BY /RESUME-PRINT-JOB AT THE MOMENT. COMMAND REJECTED

### Meaning

The SPOOLOUT job has not previously been suspended by the /HOLD-PRINT-JOB
command (operand RESUME-CONDITION=BY-OPERATOR) or processing of this
command is still in progress.
The /RESUME-PRINT-JOB command is therefore rejected.

### Response

If processing of the /HOLD-PRINT-JOB command is still in progress,
repeat the /RESUME-PRINT-JOB command later.

## SPS0276

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0276 TAPE DEVICE '(&00)' ALREADY ASSIGNED TO SPOOL. COMMAND REJECTED

### Meaning

The /START-TAPE-REPLAY command is rejected.

## SPS0277

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0277 TAPE DEVICE '(&00)' ALREADY ASSIGNED TO SPOOL IN INPUT MODE. COMMAND REJECTED

### Meaning

The /START-TAPE-OUTPUT command is rejected.

## SPS0280

Destination: CONSOLE Routing code: S Weight: 98

Warranty : NO

SPS0280 TSN '(&03)': I/O ERROR ON PRINTER '(&00)'; (&01) PAGES WILL BE REPRINTED AS OF PAGE (&02). PLEASE CONFIRM. REPLY (Y=YES; <NN>=NUMBER OF PAGES (1 THROUGH 63))

### Meaning

While printing the file an I/O error has been detected by the printer.

### Response

Before reply check the form alignment on the printer.
Y : the operator agrees with the proposed number of pages.
<NN>: number of pages that are to be reprinted (not more than 63).
In this case the message requesting confirmation is displayed again.
As it is not possible to pinpoint the exact error location, some
pages may be lost or printed twice.

## SPS0281

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0281 ABNORMAL I/O ON DEVICE '(&00)'. REPRINT FROM BEGIN OF FILE. CHECK OUTPUT

### Meaning

The 3352 laser printer hardware detected that some pages have not been
fixed. SPOOL will reprint the current file from the beginning.

### Response

Check the output for unfixed or duplicate pages.

## SPS0282

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0282 OPERAND 'FORMS-OVERLAY' ONLY ALLOWED FOR LASER PRINTER AND TAPE DEVICE. COMMAND REJECTED

## SPS0283

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0283 TAPE DRIVE '(&00)' ACQUIRED BY SPOOL REPLAY SESSION

### Meaning

SPOOL will use the tape drive (&00) for the processing of a replay tape
which was started by a /START-TAPE-REPLAY command (creation of a
replay tape or spoolout from a previously created replay tape).

## SPS0284

Destination: USER-TASK, CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0284 TSN '(&01)': FLOPPY DISK '(&00)' IS NO LONGER USABLE, SECTOR DEFECTIVE

### Meaning

A defective sector could not be marked as being defective.

## SPS0285

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0285 TSN '(&03)': I/O ERROR ON PRINTER '(&00)'; (&01) PAGES WILL BE REPRINTED AS OF PAGE (&02). CHECK OUTPUT

### Meaning

The hardware of the laser printer with mnemonic device name (&00) has
detected an error during offline printing. SPOOL will reprint up to
(&01) pages. As it is not possible to pinpoint the exact location of
the error, some pages may be lost or printed twice.

### Response

Check the form alignment on the printer.
Check the output for missing or duplicate pages.

## SPS0286

Destination: USER-TASK, CONSOLE Routing code: S Weight: 70

Warranty : NO

SPS0286 TSN '(&02)': FILE '(&00)' PRINTED ON PRINTER '(&01)' WITH TRUNCATED LINES

### Meaning

While printing user file (&00) on printer (&01) it was discovered that
one or more records contain more characters than can be accommodated
in a print line. SPOOL has truncated the records accordingly. In the
case of HP printers (3351 or 3353), SPOOL does not truncate the
records because of the proportional spacing option. If truncation is
necessary it will be performed by the printer hardware.
If truncation is not desired, specify the LAST-CHARACTER operand
in the /PRINT-FILE command.

## SPS0287

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0287 USER ERROR FOR FILE '(&00)' ON DEVICE '(&01)'. LINE TRUNCATION. JOB SUSPENDED

### Meaning

Specification of the LEFT-MARGIN operand in the /PRINT-FILE command
caused an excessive line length during printing of file (&00) on
device (&01). The job will be put in the KEEP queue.

### Response

Contact the user or the device administrator.
Modify the /PRINT-FILE command.
For information about the default value of the LEFT-MARGIN operand, enter
the SPSERVE statement SHOW-SPOOL-PARAMETERS. If necessary, modify the
default value in the SPOOL.PARAMETERS file.

## SPS0288

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0288 PRIORITY NOT ACCEPTED. COMMAND REJECTED

### Meaning

The priority given in one of the following commands is invalid:
/HOLD-PRINT-JOB
/START-TAPE-OUTPUT
/START-TAPE-REPLAY.

### Response

Correct the command and try again.

## SPS0289

Destination: USER-TASK, CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0289 INVALID ACCOUNT NUMBER. COMMAND REJECTED

### Meaning

The account number given in the /START-DISKETTE-INPUT command is invalid
for the user ID specified via the USER-ID operand.

### Response

The operator should verify the account number.

## SPS0292

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0292 DEVICE '(&00)' ALREADY OCCUPIED BY OTHER TASK. COMMAND REJECTED

### Response

Retry with a different device.

## SPS0293

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0293 'PRINT-SAMPLE' OPERAND NOT VALID FOR DEVICE TYPE (&00)'. COMMAND REJECTED

### Meaning

The /START-PRINTER-OUTPUT command with PRINT-SAMPLE=YES may only be
issued for printers (except LP65, 2090-APA and 2050-APA printers).
(&00): device type (LP65, 2090-APA, 2050-APA, TAPE or DISKETTE).

## SPS0294

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0294 DEVICE NAME '(&00)' NOT ACCEPTED. COMMAND REJECTED

### Meaning

Possible cause:
The device name is
- invalid
- not allocated to SPOOL
- assigned to a device not supported by SPOOL
- assigned to a tape device for which /HOLD-PRINT-JOB is illegal
- not defined with the /ADD-SPOOL-DEVICE command
- assigned to a device whose type differs from that of the first device
in the list. All devices contained in a list must be either local or
remote, but not mixed.

### Response

Verify the device name.

## SPS0295

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0295 REPLAY PROCESSING ONLY ALLOWED FOR TAPES. COMMAND REJECTED

### Meaning

The device name given in the /START-TAPE-REPLAY command is not the name of
a tape device.

### Response

Verify the device name.

## SPS0296

Destination: USER-TASK, CONSOLE Routing code: O Weight: 99

Warranty : NO

SPS0296 PAGE NUMBER IS TOO HIGH. COMMAND REJECTED

### Meaning

The page number given in one of the following commands
is higher than 10**7.
/HOLD-PRINT-JOB
/RESUME-PRINT-JOB.

## SPS0298

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

SPS0298 WORK TAPE '(&00)' NOT ALLOWED FOR THIS COMMAND. COMMAND REJECTED

### Meaning

Work tapes are not allowed in the following commands:
/START-TAPE-REPLAY
/START-TAPE-OUTPUT.

### Response

Try the command with another mnemonic.

## SPS0300

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0300 /REDIRECT-REMOTE-OUTPUT RESERVED FOR SPOOL ADMINISTRATOR. COMMAND REJECTED

### Meaning

The user having issued the /REDIRECT-PRINT-JOB command is not allowed
to redirect jobs to another printer. The command is reserved for the
SPOOL administrator or the device administrator.

## SPS0301

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0301 NO OUTPUT FOR STATION '(&00)'. /REDIRECT-PRINT-JOB REJECTED

## SPS0302

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0302 SYSTEM ERROR. EQUISAMQ FILE CORRUPTED

### Meaning

The spoolout requests cannot be redirected to the central printer.

## SPS0303

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0303 /REDIRECT-PRINT-JOB ACCEPTED. (&00) SPOOLOUT REQUESTS DESTINED FOR '(&01)' ARE REDIRECTED TO '(&02)'

### Meaning

RSO printouts destined for the printer (&01) are redirected to the
printer (&02) (default: central printer) if the requisite forms have
been defined for printer (&02) in the SPOOL.PARAMETERS file.
Spoolouts already being processed will not be redirected.
(&00): number of redirected printouts
(&01): name of printer whose RSO jobs are redirected to printer (&02)
(&02): name of printer on which the redirected jobs are to be spooled out.
If *CENTRAL or nothing was specified for the TO-REMOTE-PRINTER
operand, the RSO jobs are redirected to the local printer.

## SPS0304

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0304 DEVICE ADMINISTRATORS FOR DEVICES IN /REDIRECT-PRINT-JOB ARE NOT THE SAME. COMMAND REJECTED

### Meaning

The two remote printers specified in the command do not have the same
administrator in the device declaration in the SPOOL.PARAMETERS file.

### Response

Try the command again with two remote printers which have the same device
administrator.

## SPS0305

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0305 INTERNAL ERROR DURING SPOOL PARAMETER FILE ACCESS. /REDIRECT-PRINT-JOB TERMINATED

### Response

Check the validity of the SPOOL.PARAMETERS file and, if it is valid,
retry the command. If the error persists, inform the system support staff.

## SPS0306

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : YES

SPS0306 DEVICE/POOL IDENTIFICATION '(&00)' NOT DEFINED. /REDIRECT-PRINT-JOB COMMAND REJECTED

### Meaning

The station name or POOL name (&00) is not defined in the
SPOOL PARAMETER file or in the BSET.

## SPS0307

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0307 RSO NOT AVAILABLE. /REDIRECT-PRINT-JOB REJECTED

### Response

Retry the command when the RSO subsystem is loaded.

## SPS0308

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0308 SYNTAX ERROR IN DEVICE NAME. /REDIRECT-PRINT-JOB REJECTED

### Response

Reenter the command with a valid device name.

## SPS0309

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0309 MEMORY ALLOCATION ERROR FOR CLASS (&00) MEMORY IN MODULE '(&01)'

## SPS0310

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0310 TSN '(&00)': INCONSISTENCY BETWEEN 'LEFT-MARGIN' OPERAND IN /PRINT-FILE AND PAPER FORMAT OR CHARACTER DENSITY. OUTPUT SUSPENDED

### Meaning

The value of the LEFT-MARGIN operand in the /PRINT-FILE command or
its default defined in the SPOOL.PARAMETERS file is too large.

### Response

Ask the SPOOL administrator to change the paper format or
character density before releasing the TSN.

## SPS0311

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0311 READ ERROR ON SPOOL.PARAMETERS FILE. CHECK THE FILE

## SPS0312

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0312 CHARACTER SET C'(&00)', X'(&01)' DOES NOT EXIST IN SPOOL.PARAMETERS FILE. JOB SUSPENDED

### Meaning

(&00): alphanumeric character set
(&01): hexadecimal character set.

### Response

Include the missing character set in the SPOOL.PARAMETERS file and, if
- required, also in the PRFILE.
Then release the TSN.

## SPS0313

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0313 INFORMATION CONCERNING FORM NAME '(&00)' FOR DEVICE TYPE '(&01)' NOT AVAILABLE IN SPOOL.PARAMETERS FILE. JOB SUSPENDED

### Response

Include the missing form for this device type in the SPOOL parameter file.
Then release the TSN.

## SPS0314

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0314 LASER PRINTER JOBS CANNOT BE PRINTED ON DEVICE '(&00)'. JOB SUSPENDED

### Meaning

The operator has redirected a print job intended for a laser printer to
printer (&00). However, because of the information in the SPOOL.PARAMETERS
file and/or the PRFILE, the current job cannot be printed on this
device.

### Response

The SPOOL administrator should check the contents of the
SPOOL.PARAMETERS file and/or PRFILE and possibly correct the
data in these files. Otherwise the job has to stay in the KEEP
queue until a laser printer can be assigned.

## SPS0320

Destination: USER-TASK, CONSOLE Routing code: S Weight: 70

Warranty : NO

SPS0320 SUBSYSTEM '(&00)' CANNOT BE INITIALIZED. '(&01)' COMMAND ABORTED

### Meaning

An error occurred in the initialization subroutine of the subsystem.
(&00) subsystem name
(&01) product name.

### Response

Retry the command or take a dump.

## SPS0321

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0321 USER ERROR: DSSM COMMAND NOT ALLOWED IN SUBSYSTEM '(&00)'. SPECIFY '(&01)' AS SUBSYSTEM

### Meaning

(&00): name of the subsystem not available to the user
(&01): name of the subsystem which the user may handle with DSSM commands

### Response

Retry command with subsystem indicated by (&01).

## SPS0322

Destination: USER-TASK, CONSOLE Routing code: S Weight: 70

Warranty : NO

SPS0322 INVALID VALUE IN SUBSYSTEM-PARAMETER OPERAND OF '(&00)' SPOOL COMMAND

### Meaning

(&00) : command name :
/START-SUBSYSTEM or /STOP-SUBSYSTEM
or /RESUME-SUBSYSTEM or /HOLD-SUBSYSTEM

### Response

Correct command and retry

## SPS0323

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0323 SUBSYSTEM '(&01)' STILL IN INIT PHASE. '(&00)' SUBSYSTEM DELETE/HOLD IMPOSSIBLE. RETRY COMMAND LATER

### Meaning

A slave subsystem is still in initialization phase and thus prevent
the master one to be deleted.
(&00): master subsystem name
(&01): slave subsystem name

### Response

Try again the command. If unsuccessful, take a system dump.

## SPS0324

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0324 '(&00)' operand in /RESUME-SUBSYSTEM command will be ignored

### Meaning

The RSO or SPS version number may not be specified.
The RSO or SPS number expected in the /RESUME-SUBSYSTEM command
is the version of the subsystem currently in HOLD status
(&00): subsystem name RSO or SPS.

## SPS0325

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0325 INTERNAL ERROR '(&02)' DURING '(&00)'-SUBSYSTEM '(&01)' COMMAND. COMMAND NOT PROCESSED

### Meaning

An internal error occurs during the START/RESUME or STOP/DELETE of a
subsystem.Diagnose information are available in the SERSLOG file under
the number (&02).
(&00): requested action on the subsystem: START or STOP or RESUME or HOLD
(&01): subsystem name
(&02): error logging sequence number

## SPS0339

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0339 DMS ERROR '(&00)' ON INPUT FILE

### Meaning

Generation of the user tape is aborted, unless the error occurred when
releasing the lock.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## SPS0340

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0340 SPOOLOUT ENDED

### Meaning

- The file has been completely printed.
- The print request has been removed from the queue.
- The file is erased subsequent to the spoolout if requested by the user.

## SPS0341

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0341 SPOOLOUT DEFERRED

### Meaning

The spoolout job is suspended, i.e. it is put back into the
spoolout queue.

### Response

Subsequent messages will ask for a new priority and for the type
of restart for the suspended job.

## SPS0342

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0342 PRINT KEPT

### Meaning

The spoolout job is placed in the KEEP queue until it is restarted by
means of the /RESUME-PRINT-JOB command.

### Response

A subsequent message will ask for the type of restart.

## SPS0343

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0343 SPOOLOUT CANCELLED

### Meaning

Spoolout has been cancelled by means of a /CANCEL-JOB
or a /CANCEL-PRINT-JOB command

## SPS0344

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0344 TAPE ERROR. SPOOLOUT CANNOT BE PERFORMED

## SPS0345

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0345 SPOOLOUT STOPPED. USER ERROR IN THE INPUT FILE

### Meaning

SPOOLOUT has discovered a user error while printing the user's file.
Three types of error can cause this message:
- The user wanted to print more lines than allowed by the VFB
(vertical format buffer).
- The user wanted to skip to a channel which is not defined in the VFB.
- The user specified a control byte which SPOOLOUT does not know.

## SPS0346

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0346 WARNING: LINE TRUNCATION

### Meaning

The amount of characters in one or several records is greater
than allowed in the print line; SPOOL has truncated the print lines
concerned. The records in these lines are therefore incomplete.

### Response

If truncation is not desired, use the LAST-CHARACTER operand in the
/PRINT-FILE command.

## SPS0347

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0347 SPOOLOUT STOPPED. DMS ERROR CODE '(&00)' IN INPUT FILE

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## SPS0348

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0348 DMS ERROR '(&00)' IN OUTPUT TAPE FILE. JOB ABORTED. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

DMS error (&00) occurred when opening or closing the output tape file.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## SPS0349

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0349 SPOOL QUEUE ERROR '(&00)' FOR '(&01)' OPERATION

### Meaning

Message for diagnostic purposes only.
(&00): return code from EQS
(&01): operation INSERT, MODIFY, MODIFYKEY, DELETE, GETKEY, GETPARKEY,
GETBYTSN, GETNXTREC, GETCOUNT or shutdown error on EQS.

## SPS0350

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0350 WARNING: ERROR '(&00)' FOR A '(&01)' OF CLASS-'(&02)' MEMORY IN MODULE '(&03)' AT '(&04)'

### Meaning

This information is given for diagnostic purposes only.
Error code (&00) is returned by a memory allocation or release macro
(indicated by (&01)) for class (&02) memory.
If the error occurred in SSVRIS, control is returned to SSVADM.
(&01): REQM or RELM
(&03): module name
(&04): mnemonic or address for the macro call

## SPS0351

Destination: CONSOLE Routing code: S Weight: 98

Warranty : NO

SPS0351 *** REPLAY SESSION ABORTED. ACKNOWLEDGMENT REQUIRED. REPLY (TSN.=ABORTION REGISTERED)

### Meaning

A serious error has occurred.
The cause of this error was described in a previous message.

### Response

TSN.: The replay session abortion message has been taken account of.

## SPS0352

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0352 REPLAY TAPE SESSION NEEDS MORE THAN 16 VOLUMES. SESSION ABORTED

### Meaning

The replay tape session must not use more than 16 volumes
(system restriction).

## SPS0353

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0353 *** 'FSTAT' MACRO ERROR. DMS ERROR '(&00)' FOR FILE '(&01)'. REPLAY SESSION ABORTED. IN SYSTEM MODE: /HELP-MSG DMS(&00) ***

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## SPS0354

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0354 MNEMONIC '(&00)' IS INVALID. COMMAND REJECTED

### Meaning

The mnemonic given in one of the following commands is invalid:
/STOP-DISKETTE-OUTPUT
/STOP-TAPE-OUTPUT.

### Response

Correct the command and try again.

## SPS0355

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0355 REPLAY TAPE SESSION '(&00)' ALREADY IN PROCESS. COMMAND REJECTED

### Meaning

One of the following commands is rejected:
/START-TAPE-OUTPUT
/START-TAPE-REPLAY.

## SPS0356

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SPS0356 TAPE NOT A REPLAY TAPE. COMMAND REJECTED

### Meaning

One of the following commands is rejected:
/STOP-TAPE-OUTPUT
/STOP-TAPE-REPLAY.

## SPS0357

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0357 VOLUME LIST UPDATE NOT ALLOWED FOR REPLAY TAPE OUTPUT ON DEVICE '(&00)'. COMMAND REJECTED

### Meaning

It is not allowed to give a volume list to change the characteristics of a
replay tape output.
The /START-TAPE-OUTPUT command is rejected.

## SPS0358

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0358 NO JOB FOR REPLAY SESSION '(&00)'. COMMAND REJECTED

### Meaning

The SRD file contains no job for the replay session (&00).
Consequently, no job is put into the replay queue and the
/START-TAPE-REPLAY command is rejected.

## SPS0359

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0359 TSN '(&02)': SPOOLOUT OF FILE '(&01)' ON TAPE WITH VOLUME '(&00)' COMPLETED

## SPS0360

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0360 SESSION COMPLETED. SRD FILE '(&00)' ERASED

### Meaning

All the files contained in the SRD file (&00) have been processed.

## SPS0361

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0361 SESSION COMPLETED. JOB(S) REMAINING IN SRD FILE '(&00)'. SRD FILE KEPT

### Meaning

During the input processing of a replay tape, certain jobs were
not processed for one of the following reasons:
- a selection has been made in the START-TAPE-REPLAY command;
- the printer(s) to be used for the job are not supported any more;
- the replay session has been abnormally terminated.

## SPS0362

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0362 'ERASE' MACRO ERROR. DMS-ERROR-CODE '(&00)' AT ADDRESS '(&01)'. REPLAY TAPE PROCESSING CONTINUES. IN SYSTEM-MODE: /HELP-MSG DMS(&00)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## SPS0363

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0363 WARNING: REQM, RELM, BOURSE OR SSVINH ERROR AT ADDRESS '(&00)'

### Meaning

This message is given for diagnostic purposes only.
An error occurred at address (&00) in module SLOCTPI.
Depending on the type of error, processing is continued or aborted.

### Response

Inform the system support staff.

## SPS0364

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0364 SRD FILE SAVED ON TAPE '(&00)'

## SPS0365

Destination: CONSOLE Routing code: S Weight: 98

Warranty : NO

SPS0365 SRD FILE '(&00)' ALREADY EXISTS. OVERWRITE? REPLY (Y=YES; N=NO)

### Meaning

A new SRD file is to be created at the start of a replay session (read
or write), but the file name is already assigned to another file.

### Response

Y: process the replay session; the existing file is overwritten
N: abort the replay session; the existing file will be preserved.

## SPS0366

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0366 WARNING: ERROR IN SRD FILE '(&00)'; OPTION BYTE '(&01)'. ERROR BYTE AND DMS CODE '(&02)' AT ADDRESS '(&03)'

### Meaning

This message is given for diagnostic purposes only.

### Response

Inform the system support staff.

## SPS0367

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0367 WARNING: SSVINH ERROR. OPTION BYTE '(&00)', FLAG BYTE '(&01)', DMS ERROR CODE '(&02)', FILE SEQUENCE NO. '(&03)' AT ADDRESS '(&04)'

### Meaning

This message is given for diagnostic purposes only.
An error has occurred when trying to perform operation (&00) on the
tape file with file sequence number (FSEQ) (&03).
(&04): address in SLOCTPI.

## SPS0368

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0368 'FILE' MACRO ERROR. DMS ERROR '(&00)' FOR FILE '(&01)' AT ADDRESS '(&02)'. NO JOB CREATED FOR FILE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

This file cannot be extracted from the tape, due to the indicated
DMS error code. No job is created for this file.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.
(&01): tape file name
(&02): address in the module SLOCTPI.

### Response

Inform the system support staff.

## SPS0370

Destination: USER-TASK, CONSOLE Routing code: S Weight: 30

Warranty : NO

SPS0370 DENSITY NOT AVAILABLE FOR MNEMONIC '(&00)'. COMMAND REJECTED

### Meaning

The density given in one of the following commands does not exist in this
system configuration.
/START-TAPE-OUTPUT
/START-TAPE-REPLAY.

## SPS0371

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0371 ERROR ON VOLUME '(&00)'. REMAINING FILES ON THIS TAPE WILL BE IGNORED

## SPS0373

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0373 *** EAM ERROR. OPTION BYTE + LBN + FILE# '(&00)', ERROR BYTE + SDB + SENSE BYTES + EXECUTIVE FLAG '(&01)' AT ADDRESS '(&02)' ***

### Response

Contact system support staff.

## SPS0374

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0374 WARNING: SCB RECORD TOO LONG. RECORD TRUNCATED

### Meaning

When reading an SCB record from a replay tape, the record length exceeded
the limit. The record is truncated to the maximum SCB record length.

## SPS0377

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0377 FILE '(&00)' CREATED FOR TSN '(&01)'

### Meaning

The file to be printed has been created successfully in file (&00)
for TSN (&01).

## SPS0378

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0378 'FILE' MACRO ERROR '(&00)' FOR REPLAY SESSION '(&01)', USER ID '(&02)', TSN '(&03)'. SPOOL JOB WITH TSN '(&04)' ABORTED. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

Due to the DMS error code (&00) the file access for output to the printer
or punch for replay session (&01) with TSN (&03) and user ID (&02) is
not possible.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.
(&01): session ID
(&03): TSN of the user job
(&04): TSN of the SPOOL job.

### Response

Contact the user.

## SPS0379

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0379 SYNTACTICAL ERROR. CORRECT /SPARAM COMMAND

## SPS0380

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0380 /SPARAM COMMAND ACCEPTED

## SPS0381

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0381 SPOOL DID NOT ACQUIRE TAPE DRIVE OF SPECIFIED DENSITY. SPOOL PROCESSING CONTINUES

## SPS0382

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0382 DEVICE '(&00)' CANNOT CURRENTLY BE ASSIGNED TO SPOOL SUBSYSTEM

### Meaning

Physical device cannot be acquired by SPOOL subsystem
or controller task cannot be created
(&00) : device mnemonic for physical device
or *V for virtual device
Possible cause: the needed subsystem is not loaded or not ready.

## SPS0383

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0383 SPOOL NOT AVAILABLE. COMMAND REJECTED

### Meaning

A SPOOL command has been given while the SPOOL administrator task
was crashed.

### Response

Restart the SPOOL administrator task with a /START-SPOOL command.
When the message SPS0002 is given, the command can be repeated.

## SPS0384

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0384 PRESENTLY NO TAPE DRIVE FOR TSN '(&00)' AVAILABLE. SPOOL PROCESSING CONTINUES

## SPS0387

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0387 WARNING: ERROR '(&00)' IN EQS GET QUEUE OPERATION

### Meaning

Information for diagnostic purposes only.

### Response

Inform the SPOOL administrator.

## SPS039A

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS039A KEY '(&00)' ((&01)) OR HEXADECIMAL KEY '(&02)' NOT FOUND IN FILE '(&03)'

## SPS0390

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0390 SPOOL MASTER TASK ABNORMAL TERMINATION. SPOOL SHUTDOWN IN PROCESS

### Meaning

Since the SPOOL-MASTER task has crashed, a SPOOL shutdown is
initiated to allow further creation of a new SPOOL task.
To speed up this SPOOL shutdown, it is recommended to the
operator to answer to all SPOOL messages as soon as possible.

### Response

None.

## SPS0391

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

SPS0391 WARNING: ENQUEUE ERROR '(&00)' ON CONTROLLER BOURSE

### Meaning

Information for diagnostic purposes only.
(&00): ENQUEUE return code value.

### Response

Contact the system support staff.

## SPS0392

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

SPS0392 RELM ERROR '(&00)' AT ADDRESS '(&01)'

### Meaning

(&00): RELM error code.

### Response

Inform the system support staff.

## SPS0393

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0393 AT LEAST ONE REPLAY JOB COULD NOT BE SCHEDULED FROM DEVICE '(&00)'

### Meaning

During input processing of a replay tape, at least one job is not
processed
for one of the following reasons:
- the printer(s) to be used for the job is/are no longer supported;
- the printer(s) to be used for the job is/are currently not available.

## SPS0395

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

SPS0395 SPECIFY RESTART TYPE ON DEVICE '(&00)' FOR TSN '(&01)'. REPLY (B=BEGINNING, S=START AT FIRST RECORD)

### Meaning

(&00): mnemonic device name of the printer.

### Response

B: the spoolout job will be restarted from the very beginning.
S: the spoolout job will be restarted from the first record written on
the current volume.

## SPS0397

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0397 'EXIT-ROUTINE' OPERAND ONLY ALLOWED ON PRINTER AND TAPE DRIVE. COMMAND REJECTED

### Meaning

An EXIT-ROUTINE operand has been given for a device other than a printer
or a tape drive.

## SPS0398

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0398 RECOVERY FROM MEMORY POOL NOT POSSIBLE, ADDRESSES HAVE BEEN DESTROYED AFTER ABNORMAL TASK TERMINATION

### Response

Contact the system support staff.

## SPS0399

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0399 FILE '(&00)' STILL IN MEMORY POOL FOR DEVICE '(&01)' AFTER ABNORMAL TASK TERMINATION. LISTING MAY HAVE BEEN PRINTED TWICE

## SPS0401

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0401 DEVICE '(&00)' ACTIVATED. FOB SIZE: (&01); CHARACTER SETS (&02); ROTATION: '(&03)'; FO-OV: '(&04)'; R-P-M: '(&05)'

### Meaning

(&00): device mnemonic
(&01): FORMS OVERLAY BUFFER size
(&02): number of character sets
(&03): ANY / YES / NO / MANUAL
(&04): forms overlay: ALL / NONE / ONLY / <list>.
(&05): raster pattern memory size

## SPS0402

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0402 SPOOLOUT COMMAND PROCESSING COMPLETED FOR TSN '(&00)'

### Meaning

The /RESUME-PRINT-JOB command has been completed for TSN (&00).

## SPS0403

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0403 SPOOLOUT RESPOOLED. OUTPUT INCOMPLETE

### Meaning

The current spoolout job has been interrupted by a
/HOLD-PRINT-JOB RESUME-CONDITION=IMMEDIATE operator command.
Spoolout will be repeated immediately.

## SPS0404

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0404 DEVICE '(&00)' ACTIVATED. FOB SIZE: (&01); CHARACTER SETS (&02); ROTATION: '(&03)'; FO-OV: '(&04)'

### Meaning

(&00): device mnemonic
(&01): forms overlay buffer size
(&02): number of character sets
(&03): ANY / YES / NO / MANUAL
(&04): forms overlay: ALL / NONE / ONLY / <list>.

## SPS0405

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0405 VALUES SPECIFIED FOR '(&00)' ON '(&01)' ARE IN CONTRADICTION TO THE PHYSICAL VALUES. DEVICE WILL BE RELEASED

### Meaning

Possible reason:
- the lower limit of the FOB size exceeds the physical value on the
printer;
- the lower limit of the character set number exceeds the physical
value on the printer;
- ROTATION has been specified but is not supported on the device;
- the device does not support forms overlays.
No job could be scheduled on this device.
(&00): FOB (FORMS OVERLAY BUFFER) / CHARS / ROTATION / FO-OV
(&01): device mnemonic.

## SPS0406

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0406 TSN '(&00)' LOCKED. /CANCEL-JOB OR /CANCEL-PRINT-JOB REJECTED. RETRY COMMAND LATER

### Meaning

The /CANCEL-JOB or /CANCEL-PRINT-JOB command has been issued
for a TSN which is locked.

## SPS0407

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0407 TSN '(&02)': DMS ERROR '(&00)' DURING READ ACCESS TO FILE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

DMS error (&00) occurred during spoolout access to file (&01) initiated by
TSN (&02).
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.
(&01): name of the PRFILE currently used.

## SPS0408

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0408 SET SOFTWARE ROTATION MODE ON DEVICE '(&00)'? REPLY (Y=YES; N=NO)

### Meaning

(&00): device mnemonic.

### Response

Y: software rotation mode is set
N: software rotation mode is not set; the device will be released.

## SPS0409

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0409 '(&00)': '(&01)' IN REC# '(&02)'

### Meaning

(&00): WRONG DEN/FONT CTRL BYTE : character density or font error
WRONG FORM-OVERLAY CTRL BYTE: mechanical forms overlay error
WRONG LEFT-MARGIN CTRL BYTE : shift error
WRONG DATMODI CTRL BYTE : data modification error
WRONG ROTATION CTRL BYTE : page rotation error
WRONG TYPE0 HP CTRL BYTE : wide/inverse/underscore/density error
WRONG TYPE1 HP CTRL BYTE : font selection error
WRONG TYPE3 HP CTRL BYTE : FOB control error
TYPE3 HP UNALLOWED : control character of type 3
at illegal location
WRONG CHANNEL VALUE : feed to channel number > 12
CHANNEL NOT DEFINED : channel is missing in loop
AT END OF REC, TYPE3 HP : escape sequence truncated
AT END OF REC, TYPE2 HP : escape sequence truncated
ESCAPE CHAR AT END OF RECORD: escape sequence truncated
TOP OF PAGE RECORD TOO SHORT: control byte sequence incomplete
LINE TRUNCATION : line incomplete
WRONG PCC DISPLACEMENT : no valid print-control-char pos.
found
at displacement given in /PRINT-FILE.
(&01): value of the invalid control byte; 'POSSIBLE' only in conjunction
with LINE TRUNCATION
(&02): record number in the input file.

## SPS0410

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0410 WARNING: 'ROTATION' NOT SUPPORTED ON DEVICE '(&00)'. SPOOLOUT CONTINUES

### Meaning

The value ANY has been given for the operand ROTATION. Since rotations
are not supported by this device, only the jobs which do not use
this function will be scheduled.
(&00): device mnemonic.

## SPS0411

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0411 SPECIFIED LOWER LIMIT FOR FOB SIZE, NUMBER OF CHARACTER SETS, FILE SIZE OR PRIORITY EXCEEDS UPPER LIMIT. COMMAND REJECTED

### Meaning

FOB: FORMS OVERLAY BUFFER.

## SPS0412

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0412 'FORMS-OVERLAY-BUFFER', 'CHARACTER-SET-NUMBER' AND 'ROTATION' OPERANDS ARE ONLY SUPPORTED ON HP PRINTERS. COMMAND REJECTED

## SPS0413

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

SPS0413 WARNING: LINE TRUNCATION POSSIBLE

### Meaning

The amount of characters in one or more records is greater than allowed
in the print line. Due to the proportional spacing option, SPOOL does not
truncate the records. If truncation is necessary it will be performed by
the printer hardware.
If truncation is not desired, specify the LAST-CHARACTER operand in the
/PRINT-FILE command.

## SPS0414

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0414 PARAMETERS FOR '(&00)' SCHEDULING COULD NOT BE READ. DEFAULT VALUES ARE USED

### Meaning

The values specified for DEVICE-WEIGHT, JOB-SEQUENCE or JOB-PRIORITY could
not be read from the SPOOL.PARAMETERS file.
(&00): LOCAL or RSO.

## SPS0415

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0415 '(&00)' DURING BUFFER LOADING

### Meaning

The relevant error occurred when loading the buffer after header
processing.
If a DMS error code is output, for more detailed information about this
error code enter /HELP-MSG in system mode or see the
BS2000 manual 'System Messages'.
(&00): INCOHERENT CHAR#(POOL-PRINT)
DMS ERROR
I/O ERROR FOR ROTATION
I/O ERROR ON LOAD LOOP
I/O ERROR ON LOAD CHAR SET
POOL NOT FOUND
LOOP NOT FOUND
CHAR NOT FOUND.

## SPS0416

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0416 FILE TO BE PRINTED IS EMPTY

## SPS0417

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0417 NOTHING WILL BE PRINTED

### Meaning

The values specified in the FIRST-RECORD operand of the /PRINT-FILE
command
are not contained in the file to be printed.

## SPS0418

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0418 HARDWARE ERROR: '(&00)'

### Meaning

This message appears on the trailer page of the printout.
(&00): description of the hardware error which occurred during printing.

## SPS0419

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0419 SPOOLOUT PROCESSING ABORTED

### Meaning

This message appears on the trailer page of the printout.
The error in question is identified in the preceding SPS0418 message.

## SPS0420

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0420 RSO WARNING : SOME RSO PRINT-JOBS CANNOT BE DISPLAYED

### Meaning

RSO subsystem is not started.

### Response

Start RSO subsystem and retry
Please contact system support staff

## SPS0421

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0421 DMS ERROR '(&00)' DURING ACCESS TO FILE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

A DMS error occurred during the spoolout access to file (&01).
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.
(&01): PRFILE.

## SPS0422

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0422 SPOOL SCHEDULER CANNOT BE STARTED. RETRY STARTUP

### Meaning

The scheduler task did not reply in due time. SPOOL startup is aborted.

### Response

Retry SPOOL startup. If the error persists, contact the system diagnostics
staff.

## SPS0424

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0424 $VALID ERROR FOR SPOOL REQUEST P/L

### Meaning

The parameter list address is not correct.

## SPS0425

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0425 TSN '(&03)': (&00) ERROR '(&01)' DURING ACCESS TO FILE '(&02)'

### Meaning

A DMS or PLAM error occurred during the spoolout access to file (&02).
For more detailed information about the DMS or PLAM error code enter
/HELP-MSG DMS(&01) or /HELP-MSG PLA(&01) in system mode or see the
BS2000 manual 'System Messages'.
(&00): DMS / PLAM
(&01): error code.

## SPS0426

Destination: CONSOLE Routing code: I Weight: 98

Warranty : NO

SPS0426 TSN '(&03)': INVALID FLOPPY DISK '(&00)' INSERTED IN DRIVE '(&01)'. INSERT CORRECT FLOPPY DISK '(&02)'. REPLY (R=RETRY; T=TERMINATE)

### Meaning

The operator is requested to insert the correct floppy disk (&02) and to
either continue or terminate the job as appropriate.
(&00): VOLUME of the invalid floppy disk
(&01): mnemonic device name of the floppy disk drive
(&02): VOLUME of the correct floppy disk.

### Response

R: the correct floppy disk has been mounted; continue the job.
T: the correct floppy disk is not available; abort the job.

## SPS0427

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0427 TSN '(&01)': INVALID LABEL (VOL1, HDR1, DDR1) ON FLOPPY DISK IN DRIVE '(&00)'. PROCESSING CONTINUES WITH NEXT FLOPPY DISK

### Meaning

(&00): mnemonic device name of the floppy disk drive.

## SPS0429

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0429 TSN '(&00)': CLASS 3 MEMORY REQUEST REJECTED. SPOOLOUT TASK ABORTED

## SPS0430

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0430 TSN '(&00)': CLASS 4 MEMORY REQUEST REJECTED. SPOOLOUT TASK ABORTED

## SPS0431

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

SPS0431 INITIALIZATION OF VOLUME '(&00)' COMPLETED

### Meaning

The volume (&00) may now be used in BS2000.

## SPS0432

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

SPS0432 VOLUME '(&00)' CANNOT BE USED DUE TO ERROR(S). INITIALIZATION TERMINATED ABNORMALLY

### Meaning

This message is preceded by more detailed error messages.
The volume cannot be used in BS2000 for the time being.

## SPS0433

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

SPS0433 INITIALIZATION OF VOLUME '(&00)' STARTED

## SPS0434

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0434 UNRECOVERABLE ERROR DURING /REDIRECT-PRINT-JOB PROCESSING. PROCESSING ABORTED

## SPS0435

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0435 NO VALID JOB ON TAPE WITH VOLUME '(&00)'. REPLAY TAPE PROCESSING ABORTED

## SPS0436

Destination: CONSOLE Routing code: N Weight: 98

Warranty : NO

SPS0436 PRINTER '(&00)': 'STANDARD LINE PRINTER' MODE FOR SPOOL SWITCHED ON AT THE DEVICE? REPLY (Y=YES; N=NO)

### Meaning

The printer is not in the required mode for the support of SPOOL control
characters. The standard line printer mode must be switched on at
the printer panel.

### Response

Y: the printer has been initialized in the mode required by SPOOL.
N: the printer has not been initialized; the device will be released.

## SPS0437

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SPS0437 DMS ERROR '(&00)' FOR FILE '(&01)'. CHARACTER-IMAGE '(&03)' FOR DEVICE '(&02)' CANNOT BE READ. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

A DMS error occurred while reading the CHARACTER-IMAGE (&03) for
device (&02).
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Correct the DMS error and repeat the command.

## SPS0438

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0438 PRM error '(&00)' for file '(&01)'. Character-image '(&03)' for device '(&02)' cannot be read. In system mode: /HELP-MSG DMS'(&00)'

### Meaning

A PRM error occurred while reading the CHARACTER-IMAGE (&03) for
device (&02).
For more detailed information about the PRM error code enter /HELP-MSG in
system mode.

## SPS0439

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0439 SPOOL JOB '(&00)' CANNOT BE PROCESSED ON ANY SUPPORTED DEVICE TYPE. JOB IGNORED

### Meaning

A job contained in a replay tape created in a previous version
is only validated for device types which are no longer supported
by the present version.

## SPS0440

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0440 WARNING: DEVICE INFORMATION FOR DEVICE '(&00)' IN SPOOL PARAMETERS DOES NOT CORRESPOND TO REAL DEVICE

### Meaning

- if HP printer :
The FOB size, number of character sets, ROTATION, RPM or FORMS-OVERLAY
contained in the SPOOL.PARAMETERS file for device (&00) is invalid.
- If LP65 printer :
The form feed contained in the SPOOL PARAMETERS file
for device (&00) is invalid
The correct values are given in a subsequent message.
The second device name eventually displayed in parenthesis references
the associated distributed printer name which has been specified in
the /START-PRINTER-OUTPUT command

## SPS0441

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0441 NO BAND ID AVAILABLE IN SPOOL PARAMETER FILE FOR DEVICE '(&00)'. DEVICE IS RELEASED

### Meaning

The necessary band ID is not defined either in the FORM record or
in the device record in the SPOOL parameter file.
(&00): mnemonic or logical device name.

### Response

Ask the SPOOL administrator to correct the
SPOOL.PARAMETERS file, then try again.

## SPS0442

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0442 TSN '(&02)': SPOOLOUT COMPLETED ON DEVICE '(&00)' FOR FILE '(&01)'

### Meaning

(&00): mnemonic device name.

## SPS0443

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0443 PLAM ERROR CODE '(&00)' FOR INPUT FILE. SPOOLOUT ABORTED

### Meaning

For more detailed information about the PLAM error code enter the
SDF command /HELP-MSG PLA(&00) in system mode or see the BS2000 manual
'System Messages'.

## SPS0444

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0444 MORE THAN TWO OPERANDS IN /REDIRECT-PRINT-JOB. COMMAND REJECTED

## SPS0445

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0445 DEVICE RECORD '(&00)' OF SPOOL PARAMETER FILE CANNOT BE READ. SPOOLOUT ABORTED

## SPS0446

Destination: CONSOLE Routing code: O Weight: 98

Warranty : NO

SPS0446 TSN '(&01)', DEVICE '(&00)': CSS ERROR DURING SPOOLOUT. REPLY (T=TERMINATE; S=STANDARD; D=DEFER; K=KEEP WITHOUT AUTOM. RESTART)

### Response

T: the spoolout job will be removed from the spoolout queue and the file
will be erased if requested.
S: the spoolout job will be returned to the spoolout queue.
Its priority will be unchanged.
The job will be restarted from the previous checkpoint.
D: the spoolout job will be returned to the spoolout queue.
Subsequent messages will query the new priority and the restart
type for the deferred job.
K: the spoolout job will be added to the KEEP queue until the operator
restarts it by means of a /RESUME-PRINT-JOB command.
A subsequent message will query the restart type.

## SPS0447

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0447 BEGINNING OF 'SECTION' TO BE PRINTED NOT FOUND

### Meaning

The front-end processor has discovered one of the following errors in the
SECTION parameters:
- SECTION-ID not found
- FIRST-RECORD not found because LAST-RECORD was found first
- FIRST-RECORD does not exist.

### Response

Enter a correct /PRINT-FILE command or modify the file.

## SPS0448

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0448 TSN '(&02)', PRINTER '(&01)': '(&00)' FORM NAMES NOT ACCEPTED

### Meaning

The form names specified for printer (&01) in one of the following
commands must not be entered in response to message SPS0200.
/START-PRINTER-OUTPUT
/START-TAPE-OUTPUT
/START-TAPE-REPLAY .

## SPS0449

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0449 TSN '(&02)', DEVICE '(&01)': '(&00)' FORMS OVERLAY NAMES NOT ACCEPTED

### Meaning

The forms overlay names specified in the FORMS-OVERLAY operand of the
/START-PRINTER-OUTPUT command for device (&01) are not permissible
as responses to message SPS0232.

## SPS0450

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0450 JVS ERROR '(&00)' DURING JV PROCESSING

### Meaning

For more detailed information about the JVS error code, enter /HELP-MSG
in system mode or see BS2000 manual 'System Messages'.
JV: job variable
(&00): JVS error code.

## SPS0451

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0451 DMS SETL ERROR WHEN POSITIONING TO START OF 'SECTION'

### Meaning

A DMS error occurred during SETL processing.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## SPS0452

Destination: CONSOLE Routing code: O Weight: 98

Warranty : NO

SPS0452 TSN '(&02)', DEVICE '(&01)': USER ERROR WHILE STARTING PCL '(&00)'. REPLY (R=RETRY; T=TERMINATE)

### Meaning

A data check error occurred while starting the PCL due to an incorrect PCL
command.
(&00): PCL number (PAGE-DEFINITION)
(&01): mnemonic device name.

### Response

R: the spoolout job will be restarted. The operator must first modify the
panel settings or change the floppy disk.
T: the spoolout job will be terminated.
Subsequent messages will ask what action should be taken for the job
(abort or keep).

## SPS0453

Destination: CONSOLE Routing code: N Weight: 99

Warranty : NO

SPS0453 DMS ERROR '(&00)' FOR FILE '(&01)'. TRANSLATION-TABLE '(&03)' FOR DEVICE '(&02)' CANNOT BE READ. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

A DMS error occurred while reading the TRANSLATION-TABLE (&03) for
device (&02).
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Correct the DMS error and repeat the command.

## SPS0454

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0454 POSSIBLE FOB TRUNCATION

### Meaning

The forms overlay buffer size is greater than the FORM-SIZE defined in the
SPOOL.PARAMETERS file.

## SPS0455

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SPS0455 JVS ERROR '(&00)' ON SPOOL MONJV '(&01)' FOR TSN '(&02)'. IN SYSTEM MODE: /HELP-MSG JVS(&00)

### Meaning

For more detailed information about the JVS error code, enter
/HELP-MSG JVS(&00) in system mode or refer to the BS2000 manuals
'System Messages' or 'Job Variables'.
(&00): JVS error code
(&01): MONJV name
(&02): TSN of the job.

## SPS0456

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0456 SECTION CONTROLLER STARTED WITH TSN '(&00)'

## SPS0457

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0457 WARNING: REQUIRED SRDFILE '(&00)' NOT CATALOGED IN SYSTEM

### Response

Catalog SRDFILE (&00) and retry input.

## SPS0458

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0458 PLAM ERROR '(&00)' FOR INPUT FILE. IN SYSTEM MODE: /HELP-MSG PLA(&00)

### Meaning

Generation of the user tape is aborted, unless the error occurred when
releasing the lock.
For more detailed information about the PLAM error code enter
/HELP-MSG PLA(&00) in system mode or see the BS2000 manual
'System Messages'.

## SPS0459

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0459 '(&00)' CANNOT BE CREATED WITHOUT '(&01)' SUBSYSTEM

### Meaning

Subsystem (&01) must be loaded before subsystem (&00).

## SPS0460

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0460 SPS VERSION '(&00)' NOT COMPATIBLE WITH SPOOL VERSION '(&01)'. SPS LOADING IS ABORTED

## SPS0461

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0461 '/STOP-SUBSYSTEM SPS' OR '/DELETE-SUBSYSTEM SPS' ALREADY PROCESSED

## SPS0462

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0462 SPS NOT LOADED OR NOT READY

## SPS0463

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0463 SPECIFIED RESTART POSITION NOT ALLOWED FOR APA DEVICE. COMMAND REJECTED

### Meaning

- The RESTART-POSITION=PAGE or BACK operand in the
/HOLD-PRINT-JOB command is illegal for APA devices.
- The RESTART-POSITION=PAGE or BACK operand in the
/RESUME-PRINT-JOB command is illegal for a job submitted
via /PRINT-FILE with the PRINTER-RESOURCES=APA operand.

### Response

Correct the command and retry.

## SPS0464

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0464 JV SUBSYSTEM NOT LOADED OR NOT READY

### Meaning

Commands via which job variables are addressed cannot be (completely)
processed.

### Response

Ask the system support staff to load the JV subsystem.

## SPS0465

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0465 DMS ERROR '(&00)' WHEN ACCESSING EQUISAMQ FILE: EQS PROCESSING ABORTED. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## SPS0466

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0466 I/O ERROR '(&00)' IN EQUISAMQ FILE

## SPS0467

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0467 TASK '(&00)' CANNOT BE CREATED OR INITIALIZED. SPOOL STARTUP ABORTED

### Meaning

A SPOOL task management cannot be created during the SPOOL startup.
No SPOOL session is thus possible.
(&00): SPMG (SPOOL Parameter Manager) task.
EQS (equisamq file manager) task.
S (spool administrator) task.

## SPS0468

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0468 '(&00)' SYSTEM ERROR DURING EQS STARTUP. SPOOL INITIALIZATION ABORTED

### Meaning

Message for diagnostic purposes only.
(&00): system interface name (e.g. $NBCREA).

## SPS0469

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SPS0469 JV '(&00)' ALREADY IN USE OR CORRUPTED. COMMAND REJECTED

### Meaning

The job variable has been assigned to another SPOOL job
or is a monitoring JV or its status has been altered by someone.
(&00): JV name.

## SPS0470

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0470 WARNING: CONTROL CHARS NOT INTERPRETED IN REC# '(&00)'

### Meaning

The control characters are not interpreted because the record is
not the first output on the printed page.
(&00): record number in the input file.

## SPS0471

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0471 DMS ERROR '(&00)' DURING PROCESSING 'GET','FILE' OR 'OPEN' MACRO FOR FILE '(&01)'. SPOOL SUBSYSTEM STARTUP ABORTED. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

For more detailed information about the DMS error code enter
/HELP-MSG in system mode

### Response

Try to correct the DMS error and retry the startup

## SPS0472

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0472 INVALID SPECIFICATION IN THE '(&00)' PARAMETER FILE. SPOOL SUBSYSTEM ABORTED

### Meaning

The '(&00)' file does not exist or
a wrong information has been introduced in the file

### Response

Correct or restore the '(&00)' file and retry the startup

## SPS0473

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0473 Connection has been established between supervisor task and the user application '(&00)'

### Meaning

A virtual printer created successfully the user application (&00)
and established the connection

## SPS0474

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0474 Connection cannot be established between supervisor task and the user application '(&00)'

### Meaning

Possible reasons :
- the file name specified in the SPOOL parameter file device record
is wrong
- the procedure identified by the file name specified in the SPOOL
parameter file device record does not start the user application
correctly
- the user application did not perform the SPVDINI in order to
create the communication interface
- the SPVDINI action failed. More information about the error
is displayed by the previously sent message SPS0876

### Response

Correct the start procedure or the user application and retry

## SPS0475

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0475 Filter controller started with TSN '(&00)'

## SPS0476

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0476 Document format conversion not possible. Reason : '(&00)'

### Meaning

Reason : 00 : Initialization of the filter controller interrupted
because the SPCONV subsystem is not present or not
ready
01 : The SPCONV subsystem has been unloaded during the
job processing. The job is suspended
02 : Internal job conversion before or after the
filtering was unsuccessful. The job is suspended
03 : An incoherence of the new job characteristics has
been detected. The job is suspended
04 : The subsystem RSO has been unloaded during the RSO
job processing. The job is suspended
05 : The target printer is not recognized. The job is
suspended
06 : Memory allocation error.

### Response

- For reasons 00, 01, 04, check the status of the requested
subsystems. Reload them if necessary and resume the print
job
- For reason 03, correct the converter and resume the print job
- For reason 05, check the definitions of the target printer in
the spool parameter file, correct them and resume the print
job
- For reason 02 and 06, call the system support staff

## SPS0477

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0477 PRM error '(&00)' for file '(&01)'. TRANSLATION TABLE '(&03)' for device '(&02)' cannot be read. In system mode: /HELP-MSG SPR0014

### Meaning

A PRM error occurred while reading the TRANSLATION TABLE (&03)
for the device (&02).
For more detailed information about the PRM error code, enter
/HELP-MSG SPR0014 in system mode

## SPS0479

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0479 EQS error '(&00)' for TSN '(&01)'. No further job modification possible

### Meaning

An error occurred when the document format converter tries to
save the original Spool Control Block in the EQUISAMQ file
A MODIFY-PRINT-JOB-ATTRIBUTES command on the corresponding job
is no longer possible. The converted job will be processed
anyway

## SPS0480

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0480 Job with TSN '(&00)' has been intercepted by the virtual device '(&01)'

### Meaning

A print job has been intercepted by a virtual device and
transmitted to the associated application

## SPS0500

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0500 Access to Spool Notification Task with tsn '(&00)' failed

### Meaning

An error occurred while accessing the Spool Notification
system task. Following message SPS0876 provides more
information

### Response

Please contact your system administrator

## SPS0501

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0501 Print job information for notification not available for TSN '(&00)'

### Meaning

Print job information is not accessible. Notifications
will be sent with minimum information.

## SPS0502

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0502 SCB with key '(&00)' '(&01)' '(&02)' not found for notification

### Meaning

Error when building print job information for notification.
SCB was not found. If previous information is found, this
one will be used.

## SPS0503

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0503 Raise Event '(&00)' for object class '(&01)' failed. Reason: '(&02)'

### Meaning

(&00) : Event name
(&01) : Object Class name
(&02) : Reason of the error:
01: Object Class not found
02: Event not found

## SPS0856

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

SPS0856 'DER' INFO (DISK/FLOPPY DISK) FOR TSN '(&01)': '(&00)'

### Meaning

Via this message the DER (device error recovery) routine provides
information on the status of the disks and floppy disks.
For further information enter /HELP-MSG SPS0857 in system mode.

## SPS0857

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

SPS0857 'DER' INFO (DISK/FLOPPY DISK) FOR TSN '(&01)': '(&00)'

### Meaning

Via this message the DER (device error recovery) routine provides
information on disk/floppy disk I/O errors.
(&00): list with the format 'X1X2X3 AAAA TTTTTTTT ADDITIONAL-INFORMATION'
X1X2X3 (2 characters each):
X1: mnemonic name of the channel as specified in the configuration
record of $DSTATUS;
X2: mnemonic name of the physical controller as specified in the
configuration record of $DSTATUS, or blank
(X1X2 = ???? if mnemonic names are not available);
X3: mnemonic name of the device as specified in the DAR record of
$DSTATUS.
AAAA: mnemonic error code (up to 4 characters):
= BOPE: Bus Out Parity Error;
= BUSY: device busy for a prolonged period or reserved by another
channel;
= CDPE: 'channel data error' bit set in CSB;
= CHCE: error in the channel program;
= CORR: too many recoverable data errors in an I/O job;
= CRIN: command retry prohibited;
= CSBE: Channel Status Byte Error: channel control error, save error
or program error;
= CTRM: controller malfunction;
= DFCH: illegal operation, see 'define operations' command;
= DTSP: error in track overflow blocks;
= EBM: error bits missing; neither 'device end condition' nor
'device inop' is set in the SDB, or secondary indicator
is set but no OSBs (operational status bytes);
= EDPM: statistics counter overflow;
= EOCY: end of cylinder reached;
= EQCH: equipment check bit set, i.e. hardware error;
= FLUS: floppy disk not usable;
= FPRT: access to an unassigned disk area;
= HE: no floppy disk inserted (hopper empty);
= HEAD: error in automatic address incrementation;
= HOLD: STOP key has been pressed;
= ICBL: invalid block length;
= ILOP: illegal operation;
= INOP: device inoperable or path not available;
= IOER: IOE bit of CCRII is set (P4 error);
= IVAD: error in SEEK command;
= IVCH: the scanned CCW chain or the address used by TIC CCW is not
aligned on a doubleword boundary, or the invalid CCW cannot
be identified, or TIC CCW is the first CCW in the chain;
= IVSQ: invalid sequence of commands;
= JAM: card jam;
= LPOS: positioning error;
= MTOP: message to the operator advising him/her to contact the
service technician;
= NINT: no termination interrupt detected;
= NOSK: no SEEK command detected in that part of the CCW chain
which has been processed;
= NTFC: data block not found;
= PARY: channel status byte error transferred as special record, or
internal parity error, or parity error during transfer;
= PERR: permanent read/write error;
= PGER: permanent error in conjunction with paging I/O; system run
continues;
= PROT: attempt to write data despite write protection;
= RCLE: the number of data items modified (as indicated by the counter)
is greater than the number of data field length bytes or
the key-field length byte in the identification field of
the block;
= READ: error on system page, see 'READ ERROR ON SYSTEM PAGE' below;
= SBME: sense bytes missing;
= SEEK: SEEK error;
= SEQ: illegal sequence of commands;
= SRNH: service request not honored;
= TPER: parity error during transfer;
= TROV: track overflow, end of track reached;
= UNRC: unrecoverable device error;
= WRSW: 'write inhibit' switch set to 'on'.
TTTTTTTT: identifier of device error recovery call.
ADDITIONAL-INFORMATION (self-explanatory texts are not listed here):
-CC=3, CHECK CONFIGURATION !- :
IOP, channel or controller is inoperable or not available,
see CC=0.
-CC=0, CHECK CONFIGURATION !- :
the specified disk drive or device string is disabled; the
power supply for the device interface controller has been
switched off; the selected device has not been installed
or is in wait mode.
Warning: Bring the system tables into line with the current
hardware installation either by means of a /REMOVE
command or by attaching the appropriate hardware
component(s).
-INOPERABLE CC=V, DEV.ADDR.=XYZZ- :
V=3: IOP, channel or controller inoperable or not available;
V=2: hardware malfunction or software error;
X: IOC/IOP number of device status register;
Y: channel number of device status register;
ZZ: device address of channel address register.
-INOPERABLE CC=V- DDEEFFGGGGGGHHLL :
V=0: device became inoperable during processing;
V=1: device was inoperable right from the start;
DD: channel status byte (CSB);
EE: standard device byte 2 (SDB2);
FF: standard device byte 1 (SDB1);
GGGGGG: operational status bytes (OSB) 1-3;
HH: executive flag byte;
LL: operation code of the errored CCW.
-ENVIRONMENTAL DATA PRESENT-:
the statistics or error counter indicator could not be reset
in the controller.
-PERMANENT READ ERROR AFTER WRITE-:
a permanent read-after-write check error has occurred. No
alternate track could be assigned because the CCB
extension is missing. This indicates a channel program
error or a save error.
-SECTOR NOT FLAGGED- :
A defective sector could not be correctly flagged.
-SYSTEM ERROR-:
'unconditional device reservation' impossible due to resource
bottleneck.
-UNCONDITIONAL RESERVE ?-:
a disk drive is busy for more than 2 minutes or is
reserved for another channel.
'tsn.0' causes an 'unconditional device reservation' in order
to start the I/O operation via an alternative route.
'tsn.1' terminates the I/O operation without an 'unconditional
device reservation'.
-UNCONDITIONAL RESERVE UNSUCCESSFUL-:
I/O error in 'unconditional device reservation'.
-UNCONDITIONAL RELEASE UNSUCCESSFUL-:
the attempt to release a device unconditionally was
unsuccessful because of a permanent I/O error.
-C...CCCHHH- or -CCCC.HHH or -****.***-:
C...CCC: decimal cylinder number for disks, or track number for
floppy disks.
HHH: decimal head number for disks, or sector number for floppy
disks.
****.***: Both not available.
DDEEFFGGGGGGHHLL MM...MM :
DD: channel status byte (CSB);
EE: standard device byte 2 (SDB2);
FF: standard device byte 1 (SDB1) or unit status byte;
GGGGGG: operational status bytes (OSB) 1-3;
HH: executive flag byte;
LL: operation code of the errored CCW;
MM...MM: diagnostic status bytes.
Additional message relating to paging device error recovery:
READ ERROR ON SYSTEM PAGE - DANGER OF SYSTEM CRASH; READ MANUAL BEFORE ANY
CONSOLE INPUT
A system page could not be read without errors. Do not enter any system
commands. Try to make the hardware components (IOP, controller or
device)
operable. Analyze the last PGER message and contact the service
technician if necessary. In the case of devices with interchangeable
disk packs and the same controller, swapping the disks and the
address plug to another drive may prove successful. Following input of
EOT, another attempt is made to read the page. If the error persists,
an imminent system crash is likely.

### Response

Depending on the mnemonic error code (AAAA) and the condition code (CC=V):
tsn.0: restart all or part of the user CCW chain, if necessary after
issuing a /CHANGE-DISK-MOUNT command.
tsn.1: terminate the DER (Device Error Recovery) routine and continue
the user program.

## SPS0858

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0858 'DER' INFO (CARD READER) FOR TSN '(&01)': '(&00)'

### Meaning

Via this message the DER (Device Error Recovery) routine provides
information on card punches and card readers.

### Response

For further information enter /HELP-MSG SPS0859 in system mode.

## SPS0859

Destination: CONSOLE Routing code: I Weight: 99

Warranty : NO

SPS0859 'DER' INFO (CARD READER) FOR TSN '(&01)': '(&00)'

### Meaning

Via this message the DER (Device Error Recovery) routine provides
information on card punches and card readers.
(&00): list with the format 'X1X2X3 AAAA TTTTTTTT ADDITIONAL-INFORMATION'
X1X2X3 (2 characters each):
X1: mnemonic name of the channel as specified in the configuration
record of $DSTATUS;
X2: mnemonic name of the physical controller as specified in the
configuration record of $DSTATUS, or blank
(X1X2 = ???? if mnemonic names are not available);
X3: mnemonic name of the device as specified in the DAR record of
$DSTATUS.
AAAA: mnemonic error code (up to 4 characters):
= ABFR: FORMAT could not be reset to NONFORMAT;
= BOPE: Bus Out Parity Error during initialization;
= BUSY: device busy;
= CCPE: 'channel control error' bit set in CSB;
= CCWE: 'program error' bit set in CSB;
= CDPE: 'channel data error' bit set in CSB;
= CODE: illegal punch combination;
= CSBE: Channel Status Byte Error;
= EBM : Error Bits Missing; neither 'device end condition' nor
'device inop' is set in the SDB, or secondary indicator
is set but no OSBs (Operational Status Bytes);
= EQCH: EQuipment CHeck, hardware error (see additional information);
= FORM: format error;
= HOLD: STOP key has been pressed;
= ILOP: illegal operation;
= INOP: device inoperable;
= IOER: IOE bit of CCRII is set (P4 error);
= IVCH: incomplete CCW chain detected by software, or address of first
CCW is 0 or not aligned on doubleword boundary, or errored CCW
cannot be pinpointed, or TIC CCW is first command in chain,
or too many CCWs in CCW chain, or illegal address field in
TIC command;
= IVRQ: manual operator intervention required;
= JAM: card jam;
= MOMA: motion malfunction / transport error;
= NAIN: no attention interrupt detected;
= NINT: no termination interrupt detected;
= PCER: punch error;
= PEER: 'PERMANENT ERROR' key has been pressed;
= PKEY: 'memory protect error' bit set in channel status byte (CSB);
= PMPE: parity error(s) in hardware punch memory;
= READ: read error;
= SRNH: Service Request Not Honored;
= SSEL: stacker selection too late;
= TPER: parity error during transfer;
= UNRC: unrecoverable device error.
TTTTTTTT: identifier of the device error recovery request.
ADDITIONAL-INFORMATION (self-explanatory texts are not listed here):
-INOPERABLE CC=V, DEV.ADDR.=XYZZ- :
V=3: IOP, channel or controller inoperable or not available;
V=2: hardware malfunction or software error;
X: IOC number of device status register;
Y: channel number of device status register;
ZZ: device number of channel address register.
-DEVICE DETACHED BY RECONFIGURATION: CC=3, DEV.ADDR.=XYZZ- :
no path to specified device available;
X: IOC number of device status register;
Y: channel number of device status register;
ZZ: device number of channel address register.
-INOPERABLE CC=V- DDEEFFGGGGGGHHLL :
V=0: device became inoperable during processing;
V=1: device inoperable right from the start;
DD: channel status byte (CSB);
EE: standard device byte 2 (SDB2);
FF: standard device byte 1 (SDB1);
GGGGGG: operational status bytes (OSB) 1-3;
HH: executive flag byte;
LL: operation code of the errored CCW.
DDEEFFGGGGGGHHLL MM...MM :
DD: channel status byte (CSB);
EE: standard device byte 2 (SDB2);
FF: standard device byte 1 (SDB1);
GGGGGG: operational status bytes 1-3 (OSB);
HH: executive flag byte;
LL: operation code of the errored CCW;
MM...MM: diagnostic status bytes.

### Response

Depending on the mnemonic error code (AAAA) and the condition code (CC=V):
tsn.0: restart all or part of the user CCW chain.
tsn.1: terminate DER and continue the user program.

## SPS0860

Destination: CONSOLE Routing code: O Weight: 99

Warranty : NO

SPS0860 'DER' INFO (PRINTER) FOR TSN '(&01)': '(&00)'

### Meaning

Via this message the DER (Device Error Recovery) routine provides
information on printers.

### Response

For further information enter /HELP-MESS SPS0861 in system mode.

## SPS0861

Destination: CONSOLE Routing code: O Weight: 99

Warranty : NO

SPS0861 'DER' INFO. (PRINTER) FOR TSN '(&01)': '(&00)'

### Meaning

NB : The CHANNEL-TYPE of the device defined in the SPOOL.PARAMETERS
file must be correct for a good interpretation of the error
code.
Via this message the DER (Device Error Recovery) routine provides
information on printers.
(&00): List with the format 'X1X2X3 AAAA TTTTTTTT ADDITIONAL INFORMATION'.
X1X2X3: 2 characters each.
X1: mnemonic name of the channel as specified in the configuration
record of $DSTATUS.
X2: mnemonic name of the physical controller as specified in the
configuration record of $DSTATUS, or blank
(X1X2 = ???? if the mnemonic names could not be found).
X3: mnemonic name of the device as specified in the DAR record of
$DSTATUS.
AAAA: mnemonic error code of up to 4 characters.
= BOPE: Bus Out Parity Error.
= BUSY: device off-line or subchannel busy.
= CCPE: 'channel control error' bit set in the CSB.
= CCWE: 'channel program error' bit set in the CSB.
= CDPE: 'channel data parity error' bit set in the CSB.
= CSBE: Channel Status Byte Error: channel control error, save error,
data error or program error.
= CTBE: error in CTB.
= DACK: error in the data of the command that just been transferred.
= DMSE: DMS cannot work on the file containing the user's vertical
format buffer or blocks with the core image. This message is
accompanied by the additional information
UNABLE TO READ FROM LOOP/IM FILE.
This message applies only to the following printers:
3331, 3341, 3342, 3343, 3337, 3338.
= EBM: Error Bits Missing; neither 'end condition in device' nor
'device inop' is set in the SDB, or 'secondary indicator' is
set but no operation status bytes.
= EQCH: EQuipment CHeck; hardware error.
= FORM: error in form position.
= HOLD: STOP key has been pressed.
= ILOP: illegal operation, illegal character frame or character
density.
= IMER: error in image memory. This message applies only to the
following printers: 3341, 3341, 3342, 3343, 3337, 3338.
Error recovery attempts to reload the buffer. If the attempt is
successful, a message requesting a response is issued;
otherwise a message not requiring a response is issued.
= INOP: device inoperable.
= IOER: IOE bit of CCRII is set (P4 error).
= IVCH: the CCW chain or the address used by TIC CCW is not aligned
on a double word boundary, or the errored CCW cannot be
identified, or the TIC CCW is the first CCW in the chain.
= IVRQ: manual operator intervention required.
= LDCK: an illegal load command has been rejected.
= MXME: matrix memory overflow.
= NAIN: no attention interrupt detected.
= NINT: no termination interrupt detected.
= PAPR: paper has run through (3350/2) or paper supply is used up.
= PARY: print buffer parity error or transmission parity error.
= PEND: paper supply used up.
= PKEY: 'memory protect error' bit set in CSB.
= PRER: parity error in the page buffer or matrix memory (3350/2), or
last printed line is invalid or incomplete; it is advisable
to check the line (except for 3350/2 printers).
= PRTY: parity error in format or code table buffer.
= PRUN: paper has run through. Either the user has specified
the line spacing in an illegal channel or there is
a device malfunction.
= TPER: transmission error.
= UNRC: unrecoverable device error.
= USER: line or page too long, or overprint error, or specified
character set too large, or unknown character detected.
= VFBE: invalid VFB (Vertical Format Buffer).
TTTTTTTT: Identifier of the device error recovery request.
ADDITIONAL INFORMATION:
Self-explanatory texts are not listed here.
-INOPERABLE CC=V, DEV.ADDR.=XYZZ- :
V=3: IOP, channel or controller inoperable or not available.
V=2: hardware malfunction or software error.
X: IOC / IOP number of device status register.
Y: channel number of device status register.
ZZ: device number of channel address register.
-INOPERABLE CC=V- DDEEFFGGGGGGHHLL :
V=0: device became inoperable during execution.
V=1: device inoperable right from the start.
DD: channel status byte (CSB).
EE: standard device byte 2 (SDB2).
FF: standard device byte 1 (SDB1) or unit status byte.
GGGGGG: operational status bytes 1-3 (OSB).
HH: executive flag byte.
LL: operation code of the errored CCW.
-CHECK PRINTOUT F.RESTART- :
The printer is inoperable. Parts of the paging memory have been
deleted. Once the printer error has been removed, a check
should be carried out as to whether the number of pages
specified in the subsequent SPOOL message is sufficient
to ensure an error-free restart.
-ILLEGAL PAPER ADVANCE CC=1- :
The paper advance command does not match the
vertical format buffer.
-ILLEGAL PRINT INHIBIT SWITCH ON- :
The two switches for print inhibit mode do not match.
-TAPE READER INSTALLED- :
An attempt was made to load the vertical format buffer but the
paper feed is controlled by the tape reader.
-n-: error code in the UNRC message of the laser printer.
n = 2: error in sense command.
3: command rejected with load command.
5: synchronization lost during A.I. (attention interrupt)
analysis.
6: invalid device address with asynchronous A.I..
7: illegal hardware condition.
8: error in bourse calls.
9: unrecoverable error after attaching the printer.
A: more than 255 errors while waiting for last page to be printed.
DDEEFFGGGGGGHHLL MM...MM :
DD: channel status byte (CSB).
EE: standard device byte 2 (SDB2).
FF: standard device byte 1 (SDB1).
GGGGGG: operational status bytes 1-3 (OSB).
HH: executive flag byte.
LL: operation code of the errored CCW; = FF / 00, if not available.
MM...MM: diagnostic status bytes.

### Response

Depending on the mnemonic error code (AAAA) and the condition code (CC=V):
tsn.0: restart all or part of the user CCW chain.
tsn.1: terminate DER and continue the user program.

## SPS0862

Destination: CONSOLE Routing code: S Weight: 98

Warranty : NO

SPS0862 MANUAL INTERVENTION REQUIRED ON DEVICE '(&00)'. REPLY (R=RETRY; T=TERMINATE)

### Response

R: the intervention has been completed; spoolout is resumed.
T: the intervention has not been effected; the device is released.

## SPS0863

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0863 DEVICE '(&00)' NOT ACCESSIBLE. SPOOLOUT TASK ABORTED

### Meaning

The device (&00) could not be acquired by SPOOL.

### Response

Contact hardware maintenance.

## SPS0864

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0864 THE LOCAL SPOOL I/O TRACE FILE NAME IS '(&00)'

## SPS0865

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0865 LOCAL SPOOL I/O TRACE TRANSLATION ERROR; TRACE PROCESSING TERMINATED

## SPS0866

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0866 LOCAL SPOOL I/O TRACE DMS ERROR CODE '(&00)'; TRACE PROCESSING TERMINATED

## SPS0867

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0867 LOCAL SPOOL I/O TRACE CANNOT ACQUIRE CLASS 5 MEMORY; TRACE PROCESSING TERMINATED

## SPS0868

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0868 THE TRACE FILE '(&00)' IS CLOSED

## SPS0870

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0870 INTERNAL INCOHERENCE BETWEEN EQUISAMQ FILE AND SLOT DESCRIPTION FOR TSN '(&00)'

### Meaning

(&00) : TSN in error
The SCB corresponding to the slot does not exist anymore

## SPS0871

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0871 SUBSYSTEM 'XHCS' NOT LOADED AND REQUIRED FOR FILE '(&00)' ON DEVICE '(&01)'

### Meaning

Due to the Coded Character Set Name of the file, the
XHCS subsystem must be used but it is not loaded.
Job is kept.
(&00): file name
(&01): device name

### Response

Start the XHCS subsystem and use the /RESUME-PRINT-JOB
command to restart the kept job.

## SPS0872

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0872 CCSN '(&00)' UNKNOWN TO XHCS AND USED ,FOR FILE '(&01)' ON DEVICE '(&02)'

### Meaning

The Coded Character Set Name (CCSN) '(&00)' is used for
file '(&01)' and is not known by the XHCS subsystem.
Job is kept
(&00): Coded Character Set Name
(&01): file name
(&02): device name

### Response

Define the CCSN in XHCS and use the /RESUME-PRINT-JOB
command to restart the kept job.

## SPS0873

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0873 XHCS ERROR '(&00)' FOR FILE '(&01)' ON DEVICE '(&02)'

### Meaning

The XHCS subsystem reports the error code '(&00)'
Job is kept.
(&00): XHCS error code
(&01): file name
(&02): device name

### Response

Contact the system support staff

## SPS0874

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0874 THE PROCESSING FOR THE TSN '(&00)' HAS BEEN ABORTED DUE TO AN ACCESS PROBLEM OF THE EQUISAMQ FILE

### Meaning

During the IMCAT processing of the TSN '(&00)', the
EQUISAMQ file cannot be accessed properly.
Diagnostic information is available in the
error logging file.

## SPS0875

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0875 DEVICE '(&00)' NOT AVAILABLE. ACQUIRE REJECTED

### Meaning

The device has already been assigned to another task
Give SHOW-DEVICE command for more information

## SPS0876

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0876 ERROR '(&00)' FROM INTERFACE '(&01)'

### Meaning

NO FURTHER INFORMATION

## SPS0877

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0877 SPOOL subsystem cannot be created '(&01)' Subsystem creation rejected with '(&00)' return code

### Meaning

(&00) : Return code from $ESMCREI interface
Either (&01) subsystem is not defined in the system catalog
or coexistence is not allowed for the subsystem.

### Response

Define (&01) subsystem in the system catalog
or take care that the default subsystem version (STD)
is the version that must be created with SPOOL

## SPS0878

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0878 PRM ERROR '(&00)' ON RESOURCE FILE '(&01)' FOR TSN '(&02)'. IN SYSTEM MODE : /HELP-MSG SPR0014

### Meaning

(&00) = Print Resources Management error code
(&01) = Resource file name
(&02) = TSN of the print job

## SPS0879

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0879 INTERNAL ERROR '(&00)' IN '(&01)'

### Meaning

(&00) : internal error number or concerned interface name
(&01) : module which detected the failure

## SPS0880

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0880 TSN '(&00)' : SUBSYSTEM DSEM NOT LOADED OR NOT READY. JOB SUSPENDED

### Meaning

DSEM : Dynamic Spool Extension Management

## SPS0881

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS0881 PROBLEM DETECTED BY DSEM PROCESSING

### Meaning

DSEM : Dynamic Spool Extension Management
An error occurred during DSEM processing
More detailed message has been sent to the console

### Response

Contact SPOOL administrator

## SPS0882

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0882 UNABLE TO DELETE THE UFS FILE OR DMS WORK FILE FOR TSN '(&00)'

## SPS0883

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0883 PROBLEM WITH IMON RELEASE ITEM FOR SUBSYSTEM '(&00)'; LOGICAL ID '(&01)'; FILE NAME '(&02)'; SPOOL STARTUP ABORTED. PLEASE CONTACT SYSTEM SUPPORT STAFF

### Meaning

An error occurred while accessing IMON facilities

## SPS0884

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0884 '(&00)'-ERROR: PRM ERROR '(&01)' IN '(&02)' DURING SPOOLOUT OF TSN '(&03)'. IN SYSTEM MODE: /HELP-MSG SPR0014. CONTACT SYSTEM SUPPORT STAFF

### Meaning

A PRM error has been detected during SPOOL file processing.
The spoolout cannot be continued on a 3343 or 3337 printer.
For more detailed information about the PRM error code enter
/HELP-MSG in system mode.
(&00): 'OPEN' : the error occurred when opening the file
'CLOSE': the error occurred when closing the file
'DMS' : the error occurred when processing the file
(&02): name of the SPOOL file
(&03): TSN allocated.

### Response

Ask the system administrator to recover file (&02).

## SPS0886

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0886 FSTAT error '(&00)' for file '(&01)'

### Meaning

An error (&00) occurred when accessing the catalog entry
of the work file (&01) produced by a document format
converter

### Response

Check the work file (&01) and eventually the converter
application producing it

## SPS0887

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0887 File format for output filter file '(&00)' not supported

### Meaning

The format of the work file produced by the document
format converter is not supported. Only the SAM format
is supported

### Response

Modify the converter application and retry

## SPS0888

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0888 Spoolout stopped. User error in the input file for TSN '(&00)'

### Meaning

SPOOLOUT has discovered a user error while printing the user's file.
Three types of error can cause this message:
- The user wanted to print more lines than allowed by the VFB
(vertical format buffer).
- The user wanted to skip to a channel which is not defined in the VFB.
- The user specified a control byte which SPOOLOUT does not know.
(&00) : TSN of the spoolout job

## SPS0889

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPS0889 '(&00)': '(&01)' in REC# '(&02)' for TSN '(&03)'

### Meaning

(&00): WRONG DEN/FONT CTRL BYTE : character density or font error
WRONG FORM-OVERLAY CTRL BYTE: mechanical forms overlay error
WRONG LEFT-MARGIN CTRL BYTE : shift error
WRONG DATMODI CTRL BYTE : data modification error
WRONG ROTATION CTRL BYTE : page rotation error
WRONG TYPE0 HP CTRL BYTE : wide/inverse/underscore/density error
WRONG TYPE1 HP CTRL BYTE : font selection error
WRONG TYPE3 HP CTRL BYTE : FOB control error
TYPE3 HP UNALLOWED : control character of type 3
at illegal location
WRONG CHANNEL VALUE : feed to channel number > 12
CHANNEL NOT DEFINED : channel is missing in loop
AT END OF REC, TYPE3 HP : escape sequence truncated
AT END OF REC, TYPE2 HP : escape sequence truncated
ESCAPE CHAR AT END OF RECORD: escape sequence truncated
TOP OF PAGE RECORD TOO SHORT: control byte sequence incomplete
LINE TRUNCATION : line incomplete
WRONG PCC DISPLACEMENT : no valid print-control-char pos.
found. at displacement given in
/PRINT-FILE.
(&01): value of the invalid control byte; 'POSSIBLE' only in conjunction
with LINE TRUNCATION
(&02): record number in the input file.
(&03): TSN of the spoolout job

## SPS0890

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0890 Warning: STOP-PRINTER-OUTPUT command processed but controller task is waiting for operator reply

### Meaning

A STOP-PRINTER-OUTPUT FORCE=YES or a STOP-SUBSYSTEM SPOOL FORCE=YES
has been given but the printer controller task is waiting for
operator message reply. The stop of the printer or of the
subsystem will be completed after the message reply. The console
message is repeated until the reply

## SPS0891

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0891 Print job recovery processed. Job with TSN '(&00)' has been updated

### Meaning

An incoherence has been detected between SCB and SLOT. The slot
has been updated according to the status of the SCB. If the SCB
was active, the slot has been put in KEEP status

## SPS0892

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0892 '(&00)' error '(&01)' on output file '(&02)'. Spoolout job '(&03)' aborted

### Meaning

An error occurred during open of the data file received by the
application associated to the virtual device. The spoolout
job is terminated.
(&00): PLAM or DMS
(&01): error code
(&02): input data file name
(&03): spoolout job TSN
For more detailed information about the PLAM/DMS error code, enter
/HELP-MSG PLA<error code> / DMS<error code> in system mode

## SPS0893

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0893 DMS error '(&00)' on normalized file '(&01)'. Spoolout job '(&02)' aborted

### Meaning

An error occurred during creation of normalized data file
received by the application associated to the virtual device.
The spoolout job is terminated.
(&00): DMS error code
(&01): data file name
(&02): spoolout job TSN
For more detailed information about the DMS error code, enter
/HELP-MSG DMS<error code> in system mode

## SPS0894

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0894 IDOM subsystem not loaded. Start device aborted

### Meaning

The start of a virtual device dedicated to IDOM is not allowed
while IDOM subsystem is not loaded.

### Response

Execute /START-SUBSYSTEM IDOM command and retry

## SPS0895

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0895 Communication between user application task '(&00)' and virtual device '(&01)' failed. Reason '(&02)'

### Meaning

(&00) : user application task tsn
(&01) : virtual device name
(&02) : error reason
01 : The user application task has been aborted or cancelled
without termination of the virtual device
02 : The user application task aborted the communication

## SPS0896

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0896 DMS error code '(&00)' while creating procedure file '(&01)' for virtual device '(&02)'. Spoolout processing aborted. In system mode: /HELP-MSG '(&00)'

### Meaning

(&00) : DMS error code
(&01) : procedure file name
(&02) : virtual device name
A DMS error code occurred at creation of the procedure file in charge
of starting the user application. The spoolout processing is aborted

## SPS0897

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPS0897 Input file not supported by IDOM light entry process

### Meaning

File is not SAM,
File is temporary
CODED-CHARACTER-SET is not EBCDIC
XHCS not available to evaluate CODED-CHARACTER-SET

## SPS8000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8000 ACTION SUCCESSFULLY TERMINATED

### Meaning

No further screens will be displayed.

## SPS8001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8001 SELECTED ACTION INVALID

### Meaning

The selected action is not in the list displayed on the screen.

### Response

Select a valid action.

## SPS8006

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8006 FILE TO BE OPENED DOES NOT EXIST

### Response

Correct the file name.

## SPS8007

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8007 FILE TO BE OPENED IS PASSWORD-PROTECTED

### Meaning

Possible cause:
- the user tried to open a file protected by a password or
- the specified password is invalid.

### Response

Correct the password or select a different file.

## SPS8008

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8008 INSUFFICIENT PRIVILEGE FOR SELECTED ACTION

### Meaning

Either the user is not authorized to execute the selected action or he has
tried to use privileged operands in connection with the selected action.

### Response

Select another action or do not use the privileged operand fields.

## SPS8010

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8010 DMS ERROR '(&00)' OF TYPE '(&01)' OCCURRED DURING PROCESSING OF '(&02)' MACRO IN FILE '(&03)'. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.
(&00): DMS error code
(&01): SPLDMS error type
(&02): DMS macro
(&03): name of the file being processed.

## SPS8014

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8014 NO CLASS 5 MEMORY AVAILABLE. PROCESSING NOT POSSIBLE

### Meaning

An error has occurred when requesting memory space.

### Response

Terminate SPOOLSERVE.

## SPS8016

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8016 SPOOL FILE CONTAINS NO DATA OF SPECIFIED RECORD TYPE

## SPS8023

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8023 '(&00)' FILE NOT OF TYPE '(&01)'

### Meaning

(&00): file open mode INPUT or OUTPUT
(&01): file type PRFILE.

## SPS8025

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8025 INVALID '(&00)' FILE NAME. STATEMENT REJECTED

### Meaning

The following characters are not permitted for file names:
',', ';', '/', '-', ' ' .
(&00): INPUT or OUTPUT.

### Response

Correct the file name and reenter the statement.

## SPS8046

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8046 SPECIFIED 'MODEL' DOES NOT EXIST. ACTION REJECTED

## SPS8047

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8047 SELECTED NAME DOES NOT EXIST. ACTION REJECTED

### Meaning

The name selected for the DELETE or RENAME or COPY or SHOW action does
not exist.

### Response

Correct the name.

## SPS8048

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8048 SELECTED NAME ALREADY EXISTS. ACTION REJECTED

### Meaning

The name selected for the ADD action already exists.

### Response

Correct the name.

## SPS8049

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8049 NONHEXADECIMAL CHARACTER IN LINE (&00), COLUMN (&01)

### Response

Correct the input.

## SPS8050

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8050 INVALID TABLE STRUCTURE IN LINE '(&00)', COLUMN '(&01)'

### Meaning

The table must contain codes separated by a blank.
In column (&01) of line (&00) the separator is not a blank.
(&00): table line number ( 0 -> F )
(&01): table column number ( 0 -> F ).

### Response

Correct the input.

## SPS8051

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8051 REQUIRED NAME NOT SPECIFIED

### Response

Enter a name.

## SPS8052

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8052 SELECTED NAME INVALID

### Meaning

The selected name does not match the expected type
(alphanumeric, alphabetic, numeric).

### Response

Correct the name.

## SPS8061

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8061 INVALID OR AMBIGUOUS PASSWORD

### Meaning

The specified password is either invalid (hexadecimal password contains
one
or more nonhexadecimal characters) or ambiguous (both password types, i.e.
character and hexadecimal are present).

### Response

Correct the password.

## SPS8064

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8064 INVALID VALUE FOR '(&00)' OPERAND. COMMAND REJECTED

### Meaning

An invalid operand value was specified for the operand.

## SPS8066

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

SPS8066 TERMINATE MIGRATION? REPLY (Y=YES; N=NO)

### Meaning

The K2 interrupt key was hit during migration processing.
The user is asked whether migration is to be terminated or resumed.

### Response

Y: migration processing will be terminated.
N: migration processing will be continued.

## SPS8067

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8067 END OF LIST REACHED

### Meaning

This message is issued after a //NEXT statement if the end of
the list has been reached.

## SPS8068

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8068 BEGINNING OF LIST REACHED

### Meaning

This message is issued after a //PREVIOUS statement if the
beginning of the list has been reached.

## SPS8069

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8069 INVALID '(&00)' OPERAND IN SCREEN LINE (&01)

### Meaning

(&00): LINE NUMBER, CHANNEL or LPI operand
(&01): screen line number, value from 1 through 11.

## SPS8071

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8071 ERROR DURING CONTINGENCY PROCESSING

### Meaning

An error occurred during the enabling or disabling of the migration
interrupt contingency.

### Response

Contact the maintenance staff.

## SPS8073

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8073 SOME BAND ID'S WERE GENERATED WITHOUT ASSOCIATED CODE

### Meaning

-During the migration from a PRFILE to a PRFILE , bandIDs were
created in the SPOOL file without the associated code.

### Response

The user must modify these band IDs, specifying the appropriate code.

## SPS8074

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8074 INVALID VALUE FOR '(&00)' OPERAND. STATEMENT REJECTED

### Meaning

(&00): operand name.

## SPS8075

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8075 SPECIFIED LEVEL ALREADY REACHED

### Meaning

An Lx statement was entered when the user was already at level x.

## SPS8080

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8080 FHS MASK ERROR DURING LIBRARY ACCESS

### Meaning

An error occurred while accessing the SPOOLSERVE FHS masks.

### Response

Make sure that the SPOOLSERVE IFG object module library actually exists.
If it does, contact the maintenance staff.

## SPS8082

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8082 ILLEGAL DEVICE TYPE SPECIFIED

## SPS8083

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8083 ILLEGAL DEVICE SUBTYPE SPECIFIED

## SPS8084

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8084 'LOOP' LENGTH NOT EQUAL TO SPECIFIED TOTAL LENGTH

### Meaning

The LOOP length derived from the LINE and LPI specifications is
different from the LOOP length given in the LENGTH field.

### Response

Correct the LINE and LPI specifications.

## SPS8085

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8085 INVALID 'LOOP' LENGTH

### Meaning

The LOOP length derived from the LINE and LPI specifications is not
within the range: 1 inch <= LOOP length < 32 inches.

### Response

Correct the LINE and LPI specifications.

## SPS8086

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8086 TOTAL LOOP LENGTH OUT OF RANGE

### Meaning

The LENGTH value is not within the range
1 inch <= LOOP length < 32 inches.

### Response

Correct the value in the LENGTH field.

## SPS8089

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8089 SPECIFIED TOTAL LENGTH OF 'LOOP' NOT MULTIPLE OF SPECIFIED LINE DENSITY

### Meaning

The total LOOP length must be a multiple of the line density as it is not
possible to change the line density within a LOOP.

### Response

Correct the value in the LENGTH field.

## SPS8099

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8099 SPOOLSERVE TERMINATED

## SPS8100

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8100 I/O ERROR OR EOF ON SYSDTA

### Meaning

An error occurred during processing of the RDATA macro.

## SPS8101

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8101 STATEMENT SEQUENCE ERROR

### Meaning

An unexpected statement has been encountered.

## SPS8102

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8102 ILLEGAL '(&00)' NAME

### Meaning

The specified name does not match the expected type
(alphanumeric, alphabetic, numeric).
(&00): record type.

### Response

Correct the name.

## SPS8103

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8103 OPERAND DUPLICATION IN STATEMENT. CORRECT STATEMENT

### Meaning

At least one operand in the statement has been specified more than once.

## SPS8104

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8104 '(&00)' OPERAND MISSING IN STATEMENT. CORRECT STATEMENT

### Meaning

(&00): name of the missing operand.

## SPS8105

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8105 RECORD OF TYPE '(&00)' WITH NAME '(&01)' NOT OVERWRITTEN DUE TO DUPLICATION

### Meaning

Possible cause:
- The record is already contained in the file.
- The name of the record has already been specified.

## SPS8107

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8107 INVALID STATEMENT

### Meaning

An unknown statement was entered.

## SPS8108

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8108 INVALID HEXADECIMAL CODE

### Meaning

The CODE operand does not contain a hexadecimal character.

## SPS8109

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8109 TERMINATION OF LOOP GENERATION MODE

### Meaning

GENLOOP has been terminated by means of a //BACK or //HALT statement.

## SPS8113

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8113 RECORD '(&00)' '(&01)' WRITTEN

### Meaning

(&00): record type
(&01): record name.

## SPS8114

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8114 RECORD WITH RECORD TYPE '(&00)' DOES NOT EXIST

## SPS8115

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8115 SYNTAX ERROR IN FILE NAME

## SPS8116

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8116 INVALID HEXADECIMAL CODE AT POSITION '(&00)'

### Response

Correct the input.

## SPS8117

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8117 MISSING EBCDIC STRING TERMINATOR ')'

### Meaning

An EBCDIC string in the data is not terminated with the ')' character.

### Response

Correct the input.

## SPS8118

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8118 INVALID 'PREFORM' DATA LENGTH

### Meaning

The length of the entered PREFORM - after conversion to the hexadecimal
format - is equal to zero or greater than 256 characters.

### Response

Correct the input.

## SPS8119

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8119 UNEXPECTED DATA FOLLOWS THE 'PREFORM' DATA TERMINATOR

### Meaning

The PREFORM data terminating character (a blank or - in interactive mode
only - an underscore not enclosed in parentheses) is followed by more
PREFORM data.

### Response

Correct the input.

## SPS8120

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8120 UNEXPECTED DATA READ

### Meaning

In batch mode, a data line was read which was not terminated with the
'-' continuation character. Any subsequent data lines will be ignored
until a //STORE statement is encountered.

## SPS8121

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8121 INVALID IGNORE SYNTAX

### Meaning

All fields of the SP3GLOOP screen line must be filled with zeros.

### Response

Correct the input.

## SPS8122

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8122 MODIFICATION OF DENSITY NOT PERMITTED

### Meaning

Only LOOPs with an invariable line density can be created.

### Response

Correct the input.

## SPS8123

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8123 'LOOP' FRACTION MUST BE '0' OR '3'

### Meaning

The length of the LOOPs with a line density of 8 lpi must be a multiple of
half an inch.

### Response

Correct the input.

## SPS8124

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8124 UNSPECIFIED LINE INTERVALS

### Meaning

The description of the LOOP on the SP3GLOOP screen is incomplete.
Some line intervals have not been specified.

### Response

Correct the input.

## SPS8201

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8201 GENERATION OF LOOPS IN PROGRESS

### Meaning

GENLOOP mode was called.

## SPS8204

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8204 NO FILES OPENED

### Meaning

The //HELP-FILE statement was issued and no files were assigned.

## SPS8206

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8206 INVALID OPERAND IN //HELP

### Meaning

An invalid operand has been detected in the //HELP statement.

### Response

Correct the statement.

## SPS8207

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8207 KEYWORD OPERAND 'LOOP' MISSING

## SPS8211

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8211 NO INPUT FILE ASSIGNED

## SPS8212

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8212 INVALID NAME OF 'MODEL' OPERAND

### Meaning

The name of the MODEL operand in the //LOOP statement is invalid.

## SPS8214

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8214 SYNTAX ERROR IN KEYWORD

## SPS8216

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8216 (&00) 'LOOPS' PRINTED ON SYSLST

### Meaning

The //PRINTIN, //PRINTOUT or //PRINTWORK statement has been processed.
(&00): number of LOOPs that have been printed on SYSLST.

## SPS8217

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8217 'LOOP' PRINTED ON SYSLST

### Meaning

The //PRINTIN, //PRINTOUT or //PRINTWORK statement has been processed.
The specified LOOP has been output to SYSLST.

## SPS8218

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8218 SYNTAX ERROR IN 'CLEAR' OPERAND

## SPS8220

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8220 NO OUTPUT FILE ASSIGNED

## SPS8221

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8221 NO WORK FILE ASSIGNED

## SPS8222

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8222 SPECIFIED 'LOOP' NOT DEFINED IN WORK FILE

### Response

Use a defined LOOP.

## SPS8223

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8223 FILE DOES NOT EXIST

### Meaning

A statement that implies the presence of a particular file was entered,
but
this file has not yet been assigned.

## SPS8224

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8224 'FILE' OPERAND ILLEGAL WITHOUT 'MODEL' OPERAND

### Meaning

In the //LOOP statement, the FILE operand has been specified but not the
MODEL operand.

### Response

Correct the statement.

## SPS8225

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8225 CHANNEL 1 NOT SET

### Meaning

Channel 1 was not set in any line. As channel 1 is the criterion for
starting a new page, it must be specified at least once in every
LOOP record (exception: CONTROL-CHARACTERS=EBCDIC).

## SPS8226

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8226 LAST LINE RESERVED FOR CHANNEL 12

### Meaning

A channel cannot be set to the last line of a LOOP record because SPOOL
sets channel 12 to this line during loading.

## SPS8227

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8227 EXISTING LOOP NAME AND NEW LOOP NAME MUST BE DIFFERENT IN //RENAME STATEMENT

### Meaning

The same name has been used to define the old LOOP name and the new LOOP
name (NEWNAME operand) in the //RENAME statement.

### Response

Use different names.

## SPS8228

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8228 SPECIFIED LINE SPACING NOT 6 OR 8 LPI FOR OPERAND 'D'

### Meaning

The line density specified in the D operand must be 6 or 8 lines
per inch (lpi).

## SPS8229

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8229 '(&00)' OPERAND INCOMPATIBLE WITH '(&01)' OPERAND IN //LOOP STATEMENT

### Meaning

These two operands cannot be specified together in the //LOOP statement.
(&00), (&01): names of operands.

## SPS8230

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8230 LINE DENSITY SELECTED IN //LINE STATEMENT CAUSES VIOLATION OF 'LOOP' BOUNDARY

### Response

Correct the D operand in the //LINE statement.

## SPS8231

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8231 SPECIFIED CHANNEL NOT IN PERMISSIBLE RANGE FROM 1 THROUGH 11

## SPS8232

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8232 SPECIFIED LINE NUMBER NOT IN PERMISSIBLE RANGE FROM 1 THROUGH 1024

## SPS8234

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8234 'LENGTH' OR 'LINES' OR 'MODEL' OPERAND MISSING IN 'LOOP' STATEMENT

## SPS8235

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8235 'LENGTH' OR 'FR' OPERAND NOT IN PERMISSIBLE RANGE

### Meaning

The value of the LENGTH operand in the LOOP statement was not in the
range 2 to 31 and/or that of the FR operand was not in the range 0 to 5
(units of 1/6 inch).

## SPS8236

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8236 SPECIFIED LINE NUMBER GREATER THAN 'LOOP' LENGTH. LAST LINE: (&00)

### Meaning

The line number specified in the //LINE statement is greater than the LOOP
length.
(&00): number of the last line of the LOOP.

### Response

Correct the statement.

## SPS8237

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8237 SPECIFIED LENGTH FOR 'LOOP': (&00) INCHES, FR=(&01). 'LOOP' LENGTH IN LAST LINE EXCEEDED BY (&02)/120 INCH

### Meaning

The length of the LOOP resulting from LOOP creation is different from
that specified at the beginning of LOOP creation.
(&00): specified LOOP length
(&01): specified LOOP section
(&02): difference between specified LOOP length and final LOOP length.

### Response

Correct the LOOP statement.

## SPS8238

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8238 FINAL 'LOOP' LENGTH DIFFERENT FROM INITIAL 'LOOP' LENGTH

### Meaning

The length of the LOOP calculated from the SP3GLOOP screen is different
from the initial length (i.e. from the length specified in the SP2GLOOP
screen or the length of the MODEL or the length of the LOOP before
modification).

### Response

Correct the input.

## SPS8239

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8239 '(&00)' NOT SAVED

### Meaning

This message is displayed after a //BACK or //HALT statement and indicates
that the record type (&00) has been generated but not saved.

## SPS8240

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8240 SPECIFIED LINE NUMBER GREATER THAN 'LOOP' LINE NUMBER. LAST LINE: (&00)

### Meaning

The line number specified in the //LINE statement is greater than the
LOOP line number.
(&00): number of the last line of the LOOP.

### Response

Correct the statement.

## SPS8241

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8241 'LINES' OPERAND NOT IN PERMISSIBLE RANGE

### Meaning

The value of the LINES operand in the //LOOP statement was not in the
range 1 to 1024.

## SPS8242

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8242 'LOOP' RECORD WRITTEN TO WORK FILE

### Meaning

A //STORE or //COPY statement has been processed successfully.
A work file was open.

## SPS8243

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8243 'LOOP' RECORD WRITTEN TO OUTPUT FILE

### Meaning

A //STORE statement has been processed successfully.
No work file was open.

## SPS8244

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8244 FILE '(&00)' CLOSED

## SPS8245

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8245 NORMAL END OF WORK FILE REACHED

### Meaning

The //GENALL statement has been processed without errors.

## SPS8246

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8246 FILE NOT OPEN. //CLOSE STATEMENT REJECTED

### Meaning

A //CLOSE statement was entered for a file that had not been opened.

## SPS8247

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8247 INVALID VALUE FOR 'NEWNAME' OPERAND

### Meaning

Possible reason:
- The name of the new loop does not match the expected type
(alphanumeric, numeric, alphabetic).
- The NEWNAME operand is too long.

### Response

Correct the NEWNAME operand if necessary.

## SPS8252

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8252 ERROR IN //FSTAT PROCESSING

### Meaning

System error.

## SPS8253

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8253 FILE CRITERIA NOT: ISAM, KEYPOS=5, KEYLEN=(&00)

### Meaning

The work or output file assigned by means of //ASSIGN cannot be processed.

## SPS8254

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8254 RECORD '(&00)' '(&01)' OVERWRITES DUPLICATE

### Meaning

The record of type (&00) and with the name (&01) or whose name was
specified earlier existed already in the file.
The existing record has been overwritten.

## SPS8255

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8255 READ ERROR ON WORK FILE. STATEMENT ABORTED

## SPS8256

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8256 RECORD OF TYPE '(&00)' WITH NAME '(&01)' STORED AS NEW RECORD

### Meaning

The record of type (&00) and with the name (&01) or whose name
was specified earlier did not exist in the file.
This record has been added to the file.

## SPS8257

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8257 KEYWORD MISSING IN STATEMENT

## SPS8258

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8258 HIGHEST LINE REFERENCED WAS (&00) BUT (&01) IS THE LAST LINE

### Meaning

This message is displayed only when a change in the line spacing from
8 lpi to 6 lpi in a line with a higher line number has already been
specified in an earlier LINE statement due to a lack of space in the LOOP.
lpi: lines per inch.

## SPS8259

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPS8259 ILLEGAL 'MODEL' NAME SPECIFIED

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages