## NSD0900

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD0900 ONLINE SCAN ? REPLY (Y; N; IPL-CONF=I; GENERAL ONLINE SCAN=X; EOT=Y)

### Meaning

This message only appears in case of Non Standard SLED.
If the answer is 'Y' an Online Scan for all PVSs wich are
required by SLED is performed by IPL.
If the answer is 'X' an Online Scan for all devices
is performed by IPL.
If the answer is 'N', only the SLED IPL volume is available
for SLED.
If the answer is 'I', the configuration file
$TSOS.SYSDAT.IPL-CONF.vvv is evaluated.
(vvv = BS2000 version (200, 210, ...)). If this could
be done without errors, no Online-Scan is performed.
In this case the Home-PVS, the Paging-Disks and the
SLED IPL volume are available for SLED. If an error
occurs on evaluating IPL-CONF, an Online-Scan for
desired PVSs is performed.
In any case output to tape or private disk (via NSD3410)
is possible.

### Response

Y : Online Scan for PVSs required by SLED (default).
N : No Online Scan.
I : Evaluation of IPL-CONF.
X : Online Scan for all devices.

## NSD0901

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD0901 FORMAT MAIN MEMORY ? REPLY ( (PASSWORD); N; EOT=N)

### Meaning

This message only appears at Non Standard SLED
in SLED Test Mode.
If the user specifies the correct password,
the whole main memory excluding the last page
will be formatted by storing into each word
its address.
This function is password protected.

### Response

(PASSWORD) : Format main memory.
N : Continue SLED (default).

## NSD0903

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD0903 DATA COMPRESSION ? REPLY (Y; N; EOT=N)

### Meaning

This message only appears at Non Standard SLED
in SLED Test Mode.
If the answer is 'Y' data will be software-compressed
when output is written to tape.

### Response

Y : Data compression (default).
N : No data compression.

## NSD0905

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD0905 ZERO PAGE REDUCTION ? REPLY (Y; N; EOT=Y)

### Meaning

This message only appears at Non Standard SLED
in SLED Test Mode.
If the answer is 'Y' the halfpages containing but
hexadecimal zeroes are packed.

### Response

Y : Zero page reduction (default).
N : No zero page reduction.

## NSD0906

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD0906 SAVING IPL TRACE TABLE ? REPLY (Y; N; EOT=Y)

### Meaning

This message only appears at Non Standard SLED
in SLED Test Mode.
If the answer is 'Y' the IPL TRACE TABLE is
saved (only if output to tape).

### Response

Y : Saving IPL's trace table (default).
N : No saving of IPL's trace table.

## NSD0907

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD0907 DUMP OF COMPLETE MAIN MEMORY ? REPLY (Y; N; S; EOT=N)

### Meaning

This message only appears at Non Standard SLED
in SLED Test Mode.
If the answer is 'Y',
the whole main memory is dumped.

### Response

EOT : SLED decides whether page selection is done.
Y : Dump the whole main memory.
N : Selection of main memory pages requested.
S : (Skip) No main memory pages are dumped.

## NSD0908

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD0908 DUMP OF COMPLETE PAGING AREA ? REPLY (Y; N; S; EOT=N)

### Meaning

This message only appears at Non Standard SLED
in SLED Test mode.
If the answer is 'Y' the whole Paging Area is dumped.

### Response

Y : Dump the whole Paging Area.
N : Select Paging Area pages (default).
S : (skip) No dump of paging area pages.

## NSD0909

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD0909 SLED MODE ? (AUTO; STD; NSTD; EOT=STD)

### Meaning

This message only appears at Non Standard SLED
in SLED Test Mode.
If the answer is 'AUTO' SLED switches to automatic mode.
If the answer is 'NSTD' a Non Standard dialog is done again
(after completion of the current SLED run).
In all other cases SLED continues in manual mode
and the answers given up to now remain valid.

### Response

AUTO : Automatic SLED.
STD : Manual SLED (default).
NSTD : Manual SLED with Non Standard dialog.

## NSD0999

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD0999 SIZE OF MM: (&00) PA: (&01) NUMBER OF TASKS: (&02) SELECTED: (&03)

### Meaning

This message is written into the SLEDLOG.
(In SLED Test Mode to Console too.)
The data displayed are useful for
further development of SLED.
The size of main memory (MM), etc.
is given in units of 4 KB.
All numbers displayed are hexadecimal.
(&00): Size of Main Memory.
(&01): Size of Paging Area.
(&02): Number of Tasks in System.
(&03): Number of Tasks selected by SLED.

## NSD1000

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1000 SLED VERSION (&00) LOADED FROM (&01) TO (&02)

### Meaning

SLED with version (&00)
was loaded from disk with VSN (&01)
to real address (&02).
(&00): SLED version.
(&01): VSN of SLED's IPL volume.
(&02): Real load address of SLED.

## NSD1001

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1001 SLED TERMINATED

### Meaning

SLED terminated without errors.

## NSD1002

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1002 ABNORMAL TERMINATION OF SLED. TAKE DUMP OF SLED (MODE=REAL)

### Meaning

SLED detects an internal error
and terminates abnormally.

### Response

Take dump of SLED using MODE=REAL.
For a detailed description see the manual.

## NSD1003

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD1003 STANDARD SLED ? REPLY (Y; N; EOT=Y)

### Meaning

This message may only occur in manual mode.
If the answer is 'Y', the default values (STD)
are assumed for the parameters MODE and TASK.
If the answer is 'N', a supplementary operator dialog is done
to call special functions of SLED or to set
internal SLED-switches. The parameters MODE and TASK
have to be provided.

### Response

Y : Standard SLED (default)
N : Non Standard dialog (special SLED functions).

## NSD1005

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1005 ONLINE SCAN STARTED.

### Meaning

Online Scan is performed.
This message is displayed at the console only
when SLED runs in Test Mode, but is always
written into the SLEDLOG,
if an Online Scan is performed.

## NSD1100

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1100 WARNING: IPL VERSION (&00) NOT COMPATIBLE WITH SLED VERSION

### Meaning

Possibly SLED's IPL volume has been initialized incorrectly.
(&00): Version of loading IPL.

### Response

Load SLED from another volume.
Initialize the erroneous IPL volume.

## NSD1101

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1101 WARNING: XVT INCONSISTENT OR NO BS2000 WAS LOADED

### Meaning

No valid XVT has been found at real location X'1000'.
In NOEDIT mode SLED will save the whole main memory.
Generation of BS2000-specific dump information is restricted.
The following checks are performed:
EXVTVRSN = 'XVT'
EXVTIDL = X'80000000'
'01/01/00001' <= EXVTDATE <= '12/31/99366'

## NSD1102

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1102 WARNING: BS2000 VERSION (&00) NOT COMPATIBLE WITH SLED VERSION

### Meaning

The XVT field EXVTSGVR contains a version number not
supported by the current SLED.
In NOEDIT mode SLED will save the whole main memory.
BS2000-specific information may be dumped incompletely.
(&00): version of BS2000 to be dumped (from EXVTSGVR).

### Response

If necessary load SLED with appropriate version.

## NSD1103

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1103 WARNING: BS2000 VERSION CANNOT BE DETERMINED

### Meaning

No correct version number was found in the XVT.
(EXVTSGVR).
In NOEDIT mode SLED will save the whole main memory.
BS2000-specific information may be dumped incompletely.

## NSD1104

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1104 ERROR IN PRODUCT-ID OR DUMP-TESTAMENT

### Meaning

The Product-ID or the Dump-Testament of the system to dump
is erroneous.
In NOEDIT mode SLED will save the whole main memory.
SLED assumes location of XVT global part: X'1000' real for /390 and
x86 servers.

## NSD1106

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1106 SVL OF VOLUME (&00) INCONSISTENT

### Meaning

SVL version unknown to SLED.
(&00): VSN of disk.

## NSD1107

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1107 TASK-IN-CONTROL TRACE OF LM (&00) INCONSISTENT; TASK=ALL ASSUMED

### Meaning

The task in control (EXVTTIC) could not be determined or
the task in control (TIC) trace of the specified
Logical Machine (LM) was inconsistent
or could not be accessed by SLED.
SLED assumes all accessible tasks are traced in the TIC trace
(i.e. TASK=ALL).
(&00): Number of the Logical Machine (LM). 0 means undefined LM number.

## NSD1108

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1108 TASK-IN-CONTROL TRACE OF LM (&00) IS EMPTY.

### Meaning

The task in control (TIC) trace of the specified
Logical Machine (LM) is empty.
May be a spare CPU or a freshly dispatched LM and no task in control was
selected for this LM.
(&00): Number of the Logical Machine (LM). 0 means undefined LM number.

## NSD1109

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1109 NO TASK IN CONTROL (TIC) FOUND AMONG SELECTED TASKS. TASK=ALL ASSUMED.

### Meaning

SLED could not access (some/all) localXVTs. An evaluation
of EXVTTIC and task-in-control (TIC) traces was therefore not possible.
To prevent to loose these tasks, SLED assumes TASK=ALL.

## NSD1111

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1111 PRODUCT-ID OF DUMPED SYSTEM: (&00) (&01)

### Meaning

SLED displays the Product-ID of the system to be dumped.
(&00): Product name.
(&01): Product version.

## NSD1112

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1112 SLED RUNTIME LIMIT SET TO (&00) MINUTES

### Meaning

SLED runtime limit of (&00) minutes was chosen.

## NSD1113

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NSD1113 DO YOU WANT TO CHANGE CURRENT SLED RUNTIME LIMIT OF (&00) MINUTES ? REPLY (Y; N; EOT=N; - (BACKTRACK))

### Meaning

SLED terminates after runtime limit is exceeded.
A possible runtime exceeding is
checked after completion of each section. Exception : PAGEPHYS section;
check is performed after each 2 GB. MAINMEM-, SLEDMEM-
and SLEDLOG section are always present in SLEDFILE.

## NSD1114

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NSD1114 SET RUNTIME LIMIT. REPLY (1-999 (MINUTES); N (CURRENT LIMIT); EOT=N; - (BACKTRACK))

### Meaning

Set runtime limit in minutes.

## NSD1200

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1200 SLED FAILURE AT ADDRESS (&00) = (&01) + (&02)

### Meaning

SLED has detected an unrecoverable internal failure and
called its CRASH routine. This call is specified:
(&00): Absolute address of CRASH call.
(&01): Name of SLED module calling CRASH.
(&02): Module-relative address of CRASH call.

## NSD1202

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1202 SLED REGISTERS (&00): (&01)

### Meaning

This message will be issued 2 times following message
NSD1200.
(&00): Numbers of the 8 edited SLED registers.
(&01): Values of the 8 SLED registers when calling CRASH.

## NSD1400

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD1400 DISK WITH VSN (&00) NOT ONLINE

### Meaning

Disk (&00) is not online.
(&00): VSN of disk.

### Response

If data relevant to diagnosis are residing on the
disk specified, SLED must be loaded once again
after the disk has been made online.

## NSD1600

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1600 SVL OF THE FIRST SLED IPL VOLUME (&00) CANNOT BE READ

### Meaning

The SVL of the first SLED IPL volume cannot be read.
Thus the data saved in the SLEDSAVE are not accessible.
The data dumped by SLED will not be sufficient for diagnosis.
(&00): VSN of first SLED IPL volume.

## NSD1601

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1601 SVL OF PUBRES (&00) CANNOT BE READ

### Meaning

(a) If the PUBRES specified is the SYSRES of the
interrupted BS2000,
the correspondent system files cannot
be saved by SLED.
(b) If the PUBRES belongs to the PVS specified for the SLED
output file, this PVS is not usable.
(&00): VSN of PUBRES.

## NSD1602

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1602 WARNING: BLOCK (&00) OF SLEDSAVE ON VOLUME (&01) CANNOT BE READ

### Meaning

A block saved on the first SLED IPL volume cannot
be read.
The data dumped by SLED may be not sufficient for diagnosis.
(&00): VSN of first SLED IPL volume.

## NSD1603

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1603 WARNING: SLEDSAVE FILE NOT ACCESSIBLE

### Meaning

The SLEDSAVE on the first SLED IPL volume is
not accessible. All blocks overwritten by IPL and SLED
are invalid in the SLED output.
The data dumped by SLED may be not sufficient for diagnosis.

## NSD1604

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1604 WARNING: SLEDSAVE ON VOLUME (&00) TOO SMALL

### Meaning

The SLEDSAVE on the first SLED IPL volume was
too small to save all main memory blocks overwritten
while loading IPL and SLED.
The data dumped by SLED may be not sufficient for diagnosis.
(&00): VSN of first SLED IPL volume.

## NSD1605

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1605 WARNING: SVL DESCRIPTION OF SLEDSAVE INCONSISTENT

### Meaning

The SVL description of the SLEDSAVE on the first SLED
IPL volume is inconsistent.
The data dumped by SLED may be not sufficient for diagnosis.

## NSD1701

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1701 (&00) SECTION : PAGE SELECTION (&01). TIME = (&02)

### Meaning

For the SLEDFILE section (&00) a page selection is performed.
As this selection demands a great amount of computing,
several minutes may pass before output is started.
For section PAGEPHYS, this message may appear several
times.
(&00): Name of SLEDFILE section (MAINMEM or PAGEPHYS).
(&01): 'STARTED' or 'CONTINUED'.
(&02): Time.

## NSD1702

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1702 (&00) SECTION : DUMP (&01). TIME = (&02)

### Meaning

Dump of section (&00) is in process.
For section PAGEPHYS, this message may appear several
times.
(&00): Name of SLEDFILE section (MAINMEM or PAGEPHYS).
(&01): 'STARTED' or 'CONTINUED'.
(&02): Time.

## NSD1800

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1800 (&00) SECTION : TERMINATED. LAST BLOCK = (&01). TIME = (&02)

### Meaning

The output of section (&00) has been terminated.
(&00): name of terminated section:
MAINMEM, STATUS, ...
(&01): Logical PAM block number of the last block already
written to the SLED output file or output tape.
(&02): Time, when section was terminated.

## NSD1801

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1801 NO MORE SPACE AVAILABLE ON SLED OUTPUT FILE (&00)

### Meaning

The output file is too small. The output is aborted.
(&00): name of SLED output file.

### Response

If necessary, repeat output to larger file
or to tape.

## NSD1802

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1802 SLED OUTPUT COMPLETED

### Meaning

NOEDIT function of SLED completed without error.

## NSD1803

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1803 SLED OUTPUT INCOMPLETE BUT DUMP ANALYSIS POSSIBLE

### Meaning

The SLED output file is incomplete. All recorded sections
are nevertheless available for diagnosis.

## NSD1804

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1804 SLED OUTPUT STOPPED DUE TO RUNTIME LIMIT OVERFLOW

### Meaning

SLED output file was stopped due to runtime limit overflow. Not all
sections are written into SLEDFILE. At least MAINMEM-, SLEDMEM- and
SLEDLOG section are available within SLEDFILE. During writing the
PAGEPHYS section a possible runtime overflow is checked after every 2 GB.

## NSD1900

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1900 AUTOMATIC SLED WITHOUT PARAMETER FILE.

### Meaning

SLED runs in automatic mode without parameter file.
The output file used is the file
$TSOS.SLEDFILE on the Home-PVS.

## NSD1901

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1901 SLED OUTPUT FILE (&00) IS NOT EMPTY. NO DATA ARE DUMPED BY AUTOMATIC SLED TO THIS FILE

### Meaning

This message only appears if an automatic SLED is running.
The SLED output file (&00) may have been used by a
previous automatic SLED and may contain valid but not yet
evaluated dump data.
SLED immediately initiates the automatic system load process
if not working with a parameter file.
If working with a parameter file, SLED tries to
process the next parameter record.
(&00): Name of SLED output file.

## NSD1902

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1902 AUTOMATIC RESTART OF BS2000 INITIATED BY SLED

### Meaning

SLED has initiated the restart of BS2000.

## NSD1903

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD1903 AUTOMATIC RESTART FAILED. LOAD BS2000 MANUALLY

### Meaning

SLED cannot load the system automatically because the SVP
has not executed the IPL successfully.
If the reason is unclear, take a SLED from SLED.

### Response

Load the system manually.

## NSD3000

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3000 SPECIFY OUTPUT DEVICE. REPLY (DPUB; DPRIV; TAPE; EOT=DPUB; - (BACKTRACK))

### Meaning

Specification of the output device.

### Response

(OUTPUT=) DPUB : output to public disks (default)
(OUTPUT=) DPRIV : output to private disk
(OUTPUT=) TAPE : output to tape
(OUTPUT=) END : terminate SLED
- : backtrack
The following parameters may be entered in advance:
(OUTPUT=) DPUB (,FILE=filename)
(,MODE=STD / NSF / REAL / ALL)
(,TASK=STD / ALL / NONE )
(OUTPUT=) DPRIV (,VSN=vsn)
(,DEV=mn)
(,FILE=filename)
(,MODE=STD / NSF / REAL / ALL)
(,TASK=STD / ALL / NONE )
(OUTPUT=) TAPE (,VSN=vsn(*))
(,DEV=(dev# / mn)(-ALL))
(,MODE=STD / NSF / REAL / ALL)
(,TASK=STD / ALL / NONE )

## NSD3001

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3001 SPECIFY NOEDIT MODE. REPLY (STD; NSF; REAL; ALL; EOT=STD; - (BACKTRACK))

### Meaning

The amount of data to be dumped is determined.
This message is not issued when Standard SLED is running
(message NSD1003). In this case MODE=EOT is assumed
(if not specified in advance)

### Response

(MODE=) EOT : MODE=STD regardless of SETS
MODE=ALL only if problems (f.i. inconsistent system tables)
during processing occur
(MODE=) STD : Data dumped: (if accessible)
- System files
- CPU-Status
- HSA (Hardware Save Area)
- System address space (Class 1-4)
- Class 5 of tasks selected by NSD3002
- Class 6 of system- and SVC79-tasks
- Class 6 of tasks specified via TSN (NSD3002)
- resident class 6 pages of all tasks in
control of a CPU
- page 0 (if resident) of the tasks selected
(MODE=) NSF : As MODE=STD, but without system files
(MODE=) REAL : Data dumped: (if accessible)
- CPU-Status
- HSA
- Main Memory (complete)
(MODE=) ALL : In addition to the data dumped if MODE=STD,
the whole main memory is dumped.
- : Backtrack.

## NSD3002

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3002 SELECT TASKS. REPLY (STD; NONE; ALL; (TSN LIST); EOT=STD; - (BACKTRACK))

### Meaning

The tasks whose address space is to be saved are selected.
This message is not issued when Standard SLED is running
(message NSD1003). In this case TASK=EOT is assumed
(if not specified in advance).

### Response

(TASK=) EOT : TASK=STD regardless of SETS
(TASK=) NONE : Tasks In Control of all LMs.
(TASK=) STD : Following tasks are selected:
- Tasks In Control (of all LMs)
- System and SVC79-tasks
- CDUMP-in-progress tasks
- Tasks permanent pended in Q10
- Tasks traced in the Task-in-control-traces
(of all LMs)
(TASK=) ALL : All tasks are selected.
(TASK=) '('tsn1,...,tsnx')' : The tasks specified by their TSN
are selected in addition to the tasks which
would be selected by TASK=STD.
- : Backtrack.

## NSD3200

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3200 SPECIFY NAME OF SLED OUTPUT FILE. REPLY (FILENAME; EOT='$TSOS.SLEDFILE'; - (BACKTRACK))

### Response

(FILE=) filename : name of SLED output file
(FILE=) EOT : default filename is '$TSOS.SLEDFILE'
- : Backtrack.
The following parameters may be entered in advance:
(FILE=) filename (,MODE=STD / NSF / REAL / ALL)
(,TASK=STD / ALL / NONE )

## NSD3201

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3201 SLED OUTPUT FILE (&00) NOT FOUND

### Meaning

The specified SLED output file (&00) has not been found in
the catalog of the SLEDFILE-PVS (if output to PVS)
or in the F1-Label (if output to private disk).
(&00): Name of SLED output file.

## NSD3202

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3202 SLED OUTPUT FILE (&00) IS PASSWORD PROTECTED

### Meaning

(&00): Name of SLED output file.

## NSD3203

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3203 SLED OUTPUT FILE (&00) IS WRITE PROTECTED

### Meaning

The SLED output file (&00) does not have the attribute
'ACCESS=WRITE'.
(&00): name of SLED output file.

## NSD3204

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3204 SLED OUTPUT FILE (&00) IS NOT EMPTY. OVERWRITE ? REPLY (YES=Y; NO=N)

### Meaning

The SLED output file (&00) may have been used by a
previous SLED and may contain valid but not yet
evaluated dump data.
(&00): name of SLED output file.

### Response

Y: Overwrite output file.
N: Do not overwrite output file.
- SLED with parameter file:
processing of the next parameter record
SLED without parameter file:
backtrack to message NSD3200

## NSD3205

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3205 WARNING: SLED OUTPUT FILE (&00) MAY BE TOO SMALL

### Meaning

The SLED output file (&00) may be too small to receive
the complete main memory.
SLED continues.
(&00): name of SLED output file.

## NSD3206

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3206 EXPIRATION DATE OF SLED OUTPUT FILE (&00) NOT YET REACHED

### Meaning

(&00): name of SLED output file.

## NSD3207

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3207 SLEDFILE-PVS NOT ONLINE.

## NSD3208

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3208 SLED OUTPUT FILE MUST NOT BE ON NET STORAGE.

## NSD3300

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3300 UNRECOVERABLE I/O-ERROR DURING OUTPUT TO SLED OUTPUT FILE, DMS-RC = (&00), BLOCK = (&01)

### Meaning

An error occurred when writing to disk.
SLED terminates output.
(&00): return code from DMS (PAM-macro)
(&01): block number where the error occurred.
See also previous IPL message.

## NSD3302

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3302 ERROR DURING CLOSE OF SLED OUTPUT FILE; DMS-RC = (&00), MACRO-RC = (&01)

### Meaning

An error occurred during close of diskfile/tapefile.
SLED cannot close file correctly.
(&00): return code from DMS
(&01): return code from CLOSE-macro (IPL)
Diskfile:
Required automatic restart is executed only if DMS-RC=0.
Tapefile:
Error might be caused by a defective tape/MBK. If so repeat SLED with
another tape/MBK.

## NSD3400

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3400 SPECIFY VSN OF PRIVATE DISK. REPLY (VSN(&00); - (BACKTRACK))

### Meaning

The VSN of the private disk containing the
output file (SLEDFILE) has to be specified.
The given VSN is compared with the VSN from the
disk label.
The answer (VSN=) '*' or EOT is allowed;

### Response

(VSN=) vsn : VSN.
(VSN=) EOT / * : Device only specified by Mnemonic
or device number.
- : Backtrack.
The following parameters may be entered in advance:
(VSN=) vsn (,DEV=mn / dev#) (,FILE=filename)
(,MODE=STD / NSF / REAL / ALL)
(,TASK=STD / ALL / NONE)

## NSD3401

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3401 VSN (&00) ILLEGAL FOR PRIVATE DISK

### Meaning

The given VSN belongs to a public disk.
(&00): VSN (response to message NSD3400).

## NSD3402

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3402 CATID NOT ALLOWED FOR FILE ON PRIVATE DISK

### Meaning

Files residing on a private disk must be specified
without Catalog-Identification.

## NSD3403

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3403 NO USABLE F1-LABEL ON PRIVATE DISK (&00)

### Meaning

(&00): VSN of private disk.

## NSD3410

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3410 SPECIFY (&00) OF PRIVATE DISK. REPLY ((&01); - (BACKTRACK))

### Meaning

SLED does not know private discs, because no online scan
for these devices is done.
Specified VSN is not known to SLED up to now.
Depending on the HSI the mnemonic
or the device number of the disc
containing the complete output file (SLEDFILE)
has to be specified.
(&00): mnemonic / device number
(&01): MN / DEV#

### Response

(DEV=) : mnemonic / device number
- : backtrack.
The following parameters may be entered in advance:
(DEV=) mn/dev# (,FILE=filename)
(,MODE=STD / NSF / REAL / ALL)
(,TASK=STD / ALL / NONE)
(,TASK=STD / ALL / NONE)

## NSD3411

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3411 DISK WITH MNEMONIC (&00) NOT ONLINE

### Meaning

The device with the mnemonic specified is not
online or it is not a disk device.
(&00): Mnemonic .

## NSD3412

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3412 VSN (&00) OF DEVICE (&01) NOT EXPECTED

### Meaning

The VSN found does not match the VSN specified.
(&00): VSN of disk as found in SVL.
(&01): Device mnemonic.

### Response

Specify correct VSN resp.MN.

## NSD3600

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3600 SPECIFY CATID FOR FILE (&00). REPLY (CATID; - (BACKTRACK))

### Meaning

(a) SLED was loaded from a private disk and there are
several PVSs online. Without
CATID the SLED output file (&00) is not unambiguously
defined.
(b) SLED could not determine the Home-PVSID of the dumped
system. Without CATID the SLED parameter file (&00) is
not unambiguously defined.

### Response

catid : Catalog identification.
- : Backtrack.

## NSD3601

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3601 NO USABLE CATALOG FOR FILE (&00)

### Meaning

The CATID of the catalog to be used for the
file (&00) either has been given with the file name,
or has been determined via default rules. But there
is no usable catalog with this CATID; thus the usage
of the specified file is not possible.
(&00): Name of the concerned file including CATID.

## NSD3603

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3603 SLED OUTPUT FILE (&00) NOT ON PVS

### Meaning

Although output to PVS has been demanded, the
specified SLED output file resides on a private disk.
(&00): Name of SLED output file.

## NSD3800

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3800 SPECIFY VSN OF SLED OUTPUT TAPE. REPLY (VSN; VSN*; - (BACKTRACK))

### Meaning

This message is issued to request the first
SLED output tape or a continuation tape.

### Response

(VSN=) vsn(*) : VSN of SLED output tape.
If a VSN ending with the
character '*' is specified, SLED will accept
any tape with a VSN beginning
with the string preceding this character.
In this case the VSN of continuation tapes
will not be demanded.
- : Backtrack.
If a continuation tape is to be specified,
no Backtrack is possible.
The following parameters may be entered in advance:
- If the first SLED output tape is to be specified
(VSN=) vsn(*) (,DEV=(dev# / mn)(-ALL))
(,MODE=STD / NSF / REAL / ALL)
(,TASK=STD / ALL / NONE)
- If a continuation tape is to be specified
(VSN=) vsn(*) (,DEV=(dev# / mn)(-ALL))

## NSD3803

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3803 NO STANDARD VOLUME LABELS FOR TAPE (&00) ON DEVICE (&01)

### Meaning

The labels VOL1, HDR1 and HDR2 must exist.
(&00): VSN of tape.
(&01): Device number or mnemonic.

### Response

Use a newly initialized tape.

## NSD3804

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3804 WRONG VOLUME (&00) MOUNTED ON DEVICE (&01)

### Meaning

The VSN found does not match the VSN specified.
(&00): VSN of tape as found in the VOL1 label.
(&01): Device number or mnemonic.

### Response

Mount tape with specified VSN or specify another one.

## NSD3805

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3805 EXPIRATION DATE OF TAPE (&00) NOT YET REACHED

### Meaning

(&00): VSN of tape.

### Response

Use another output tape.

## NSD3806

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3806 TAPE (&00) HAS ALREADY BEEN USED DURING CURRENT SLED OUTPUT

### Meaning

The specified tape has already been used
for the current output file and must not
be overwritten.
(&00): VSN of tape.

### Response

Mount another tape.

## NSD3808

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3808 MOUNT NEXT TAPE

### Meaning

This message is issued, if end-of-tape was reached or
if SLED is able to continue after an unrecoverable tape error.

## NSD3809

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3809 TAPE (&00) ON DEVICE (&01) INITIALISED WITH DENSITY (&02)

### Meaning

(&00): VSN of tape.
(&01): Device number or mnemonic.
(&02): Used density.

## NSD3810

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3810 TAPE (&00) ON DEVICE (&01) INITIALISED AS (&02)

### Meaning

(&00): VSN of tape.
(&01): Device number or mnemonic.
(&02): Used tape recording technique.

## NSD3811

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3811 SPECIFY DEVICE NUMBER OF SLED OUTPUT TAPE (&00). REPLY (DEV#; DEV#-ALL; - (BACKTRACK))

### Meaning

(&00): VSN of SLED output tape.

### Response

(DEV=) dev#(-ALL) : Device number, hexadecimal, 4 digits.
If you want to use a device with
automatic cartridge loader, you may
specify the device number with the
suffix '-ALL'. SLED tries to load
continuation cartridges without
operator dialog.
- : Backtrack.
The following parameters may be entered in advance,
when the first SLED output tape is to be specified:
(DEV=) dev#(-ALL) (,MODE=STD / NSF / REAL / ALL)
(,TASK=STD / ALL / NONE)

## NSD3812

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3812 NO OPERABLE DEVICE/SUBCHANNEL AT (&00)

### Meaning

At the specified address no operable tape device has
been found.
Possible cause:
- A wrong device number or
device mnemonic was entered.
- Tape unit or subchannel not clear.
(&00): Device number or mnemonic.

## NSD3813

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3813 CHANNEL-, CONTROLLER- OR DEVICE-TYPE UNKNOWN ( (&00) )

### Meaning

Possible cause:
- A wrong device number or
device mnemonic was entered.
- Tape unit not clear.
(&00): Device number or mnemonic.

## NSD3814

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3814 UNRECOVERABLE I/O ERROR OCCURRED ( (&00) )

### Meaning

Possible cause:
- Tape unit not clear.
(&00): Device number or mnemonic.

## NSD3817

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3817 FIX WRITE RING FOR SLED OUTPUT TAPE (&00) ON DEVICE (&01). REPLY (READY=EOT; OTHER DEVICE=DEV# OR DEV#-ALL; - (BACKTRACK))

### Meaning

(&00): VSN of SLED output tape
(&01): Device number, hexadecimal, with 4 digits.

### Response

Fix write ring.
EOT : Tape mounted with writering,
continue with same tape at same device
dev#(-ALL) : Tape mounted with writering,
continue with same tape on device with
number DEV# (4 hexadecimal characters).
When the suffix '-ALL' is entered, SLED tries
to load continuation cartridges without operator
dialog from the device with stacker at the
specified device number.
If another tape is to be used instead, enter the
BACKTRACK command:
- : Backtrack.

## NSD3821

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3821 SPECIFY MN OF SLED OUTPUT TAPE (&00). REPLY (MN; MN-ALL; - (BACKTRACK))

### Meaning

(&00): VSN of SLED output tape.

### Response

(DEV=) mn(-ALL) : Specify device mnemonic.
If you want to use a device with automatic
cartridge loader, you may specify the device
mnemonic with the suffix '-ALL'. SLED tries
to load continuation cartridges without
operator dialog.
- : Backtrack.
The following parameters may be entered in advance,
when the first SLED output tape is to be specified:
(DEV=) mn(-ALL) (,MODE=STD / NSF / REAL /ALL)
(,TASK=STD / ALL / NONE)

## NSD3822

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3822 SPECIFY MN OF SLED OUTPUT TAPE (&00). REPLY (MN; - (BACKTRACK))

### Meaning

(&00): VSN of SLED output tape.

### Response

(DEV=) mn : Specify device mnemonic.
- : Backtrack.
The following parameters may be entered in advance,
when the first SLED output tape is to be specified:
(DEV=) mn (,MODE=STD / NSF / REAL /ALL)
(,TASK=STD / ALL / NONE)

## NSD3823

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3823 TAPE WITH VSN (&00) HAS BEEN SELECTED. OKAY? REPLY (N; Y)

### Meaning

The selected tape has been mounted on device.
Confirmation is necessary in case of wildcards.

### Response

Please answer accordingly!

## NSD3824

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3824 SELECTED TAPE (&00) DOES NOT MATCH MOUNTED TAPE (&01)

### Meaning

VSN of mounted tape does not match wildcard vsn.

### Response

Please select another VSN (with wildcard)!

## NSD3827

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3827 LIFT TAPE WRITE PROTECTION FOR SLED OUTPUT TAPE (&00) ON MN (&01). REPLY (READY=EOT; OTHER DEVICE=MN OR MN-ALL; - (BACKTRACK))

### Meaning

(&00): VSN of SLED output tape
(&01): Device mnemonic

### Response

Lift tape write protection.
EOT : Tape mounted without write protection,
continue with same tape at same device
mn(-ALL) : Tape mounted without writeprotection,
continue with same tape on device with
mnemonic MN.
When the suffix '-ALL' is entered, SLED tries to
load continuation cartridges without operator
dialog from the device with stacker at the
specified device mnemonic.
If another tape is to be used instead, enter the
BACKTRACK command:
- : Backtrack.

## NSD3828

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3828 LIFT TAPE WRITE PROTECTION FOR SLED OUTPUT TAPE (&00) ON MN (&01). REPLY (READY=EOT; OTHER DEVICE=MN; - (BACKTRACK))

### Meaning

(&00): VSN of SLED output tape
(&01): Device mnemonic

### Response

Lift tape write protection.
EOT : Tape mounted without write protection,
continue with same tape at same device
mn : Tape mounted without writeprotection,
continue with same tape on device with
mnemonic MN.
If another tape is to be used instead, enter the
BACKTRACK command:
- : Backtrack.

## NSD3829

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3829 DEVICE (&00) REPORTS "COMMAND REJECT".

### Meaning

No work possible with device (&00).
Possible cause:
- For device (&00) "Stand-alone-mode" is adjusted.
SLED does not support library 3594 in Stand-alone-mode.
SLED only supports "manual mode" or "automatic mode".

## NSD3830

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3830 LIFT TAPE WRITE PROTECTION FOR SLED OUTPUT TAPE (&00) ON MN (&01). REPLY (READY=EOT; - (BACKTRACK))

### Meaning

(&00): VSN of SLED output tape
(&01): Device mnemonic

### Response

Lift tape write protection.
EOT : Tape mounted without write protection,
continue with same tape at same device
If another tape is to be used instead, enter the
BACKTRACK command:
- : Backtrack.

## NSD3831

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3831 FIX WRITE RING FOR SLED OUTPUT TAPE (&00) ON MN (&01). REPLY (READY=EOT; OTHER DEVICE=MN; - (BACKTRACK))

### Meaning

(&00): VSN of SLED output tape
(&01): Device mnemonic

### Response

Lift tape write protection.
EOT : Tape mounted with writering,
continue with same tape at same device
mn : Tape mounted with writering,
continue with same tape on device with
mnemonic MN.
If another tape is to be used instead, enter the
BACKTRACK command:
- : Backtrack.

## NSD3832

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3832 FIX WRITE RING FOR SLED OUTPUT TAPE (&00) ON MN (&01). REPLY (READY=EOT; - (BACKTRACK))

### Meaning

(&00): VSN of SLED output tape.

### Response

Lift tape write protection.
EOT : Tape mounted with writering,
continue with same tape at same device.
If another tape is to be used instead, enter the
BACKTRACK command:
- : Backtrack.

## NSD3840

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3840 NSIAQIR REPORTS ERROR CODE ( (&00) )

### Meaning

Call of NSIAQIR function not successfully completed.
(&00): NSIAQIR error code.

## NSD3841

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3841 BTAM-OPEN REPORTS ERROR CODE ( (&00) )

### Meaning

Call of BTAM-OPEN not successfully completed.
(&00): BTAM-OPEN error code.

## NSD3900

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3900 UNRECOVERABLE I/O ERROR DURING INITIALISATION OF TAPE (&00)

### Meaning

See also previous IPL message, if there is any.
(&00): VSN of tape.

## NSD3901

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3901 UNRECOVERABLE I/O ERROR DURING OUTPUT TO TAPE (&00) WHILE WRITING I/O BLOCK (&01)

### Meaning

(&00): VSN of tape
(&01): number of I/O block which could not be written.
See also previous IPL message.
If the error didn't occur on the first output volume
and if the MAINMEM section was already terminated on
a previous volume, SLED is able to continue after
mounting a new volume.

## NSD3902

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3902 REQUIRED DENSITY OR RECORDING TECHNIQUE FOR VOLUME (&00) NOT SUPPORTED BY DEVICE (&01)

### Meaning

While initialising a SLED output tape it is
recognized, that the density or recording technique of the
first output volume is not available on the used device.
SLED continues with message NSD3800.
(&00): VSN of tape.
(&01): Device number or mnemonic.

## NSD3903

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3903 DEVICE (&00) RESERVED ELSEWHERE

### Meaning

SLED continues with message NSD3800.
(&00): Device number or mnemonic.

## NSD3904

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3904 WRITE RING MISSING FOR TAPE (&00) ON DEVICE (&01)

### Meaning

The tape is not used for output.
(&00): VSN of tape.
(&01): Device number or mnemonic.

## NSD3905

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3905 TAPE (&00) ON DEVICE (&01) IGNORED

### Meaning

The previous messages specify the reason why.
SLED continues with message NSD3800.
(&00): VSN of tape.
(&01): Device number or mnemonic.

## NSD3906

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3906 REMOVE TAPE (&00) FROM CURRENT SLED OUTPUT

### Meaning

After an hard tape error, SLED has determined a restart
point. Doing this SLED has recognized, that the data on
the specified tape has to be rewritten. Therefore this
tape does no longer belong to the multi volume output file.
(&00): VSN of tape.

## NSD3907

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3907 DO NOT MIX TAPE AND CARTRIDGE

### Meaning

The output device type must be the same for all volumes.

## NSD3908

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3908 DO NOT MIX BUS AND CHANNEL TAPE DEVICES

## NSD3909

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3909 CARTRIDGE DEVICE TYPE NOT SUPPORTED BY SLED

### Meaning

SLED does not support the type of the device specified.

## NSD3910

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3910 DEVICE RESERVED ELSEWHERE

### Meaning

The tape device used by SLED for current output is reserved
by another instance. On tape initialization the device
was reserved by SLED.

## NSD3920

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3920 WRITE INHIBITED FOR CARTRIDGE (&00) ON DEVICE (&01)

### Meaning

On the current device with library system
the file protection mode is set.
The cartridge is not used for output.
(&00): VSN of cartridge.
(&01): Device number or mnemonic.

## NSD3922

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3922 FOR THE GIVEN VSN (&00) THERE IS NO FURTHER SUITABLE VOLUME IN THE TAPE LIBRARY.

### Meaning

On the current library system
no more cartridges exist in the pool
which VSN correspond to the given VSN.
(If a VSN with * was given, all SLED
conformable VSNs were checked.)
(&00): VSN of cartridge.

## NSD3924

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3924 MBK WITH VSN (&00) COULD NOT BE MOUNTED FROM LIBRARY SYSTEM.

### Meaning

On the current library system
the cartridge with VSN (&00) could not be mounted
(because it could not be found).
(&00): VSN of cartridge.

## NSD3926

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3926 LOGICAL VOLUMES ARE NOT SUPPORTED. VSN (&00) IS A LOGICAL VOLUME.

### Meaning

VSN (&00) is defined as logical volume.
Logical volumes are not supported by SLED.
This VSN is treated as a not existing cartridge.

## NSD3928

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3928 DEVICE (&00) IS IN RANDOM MODE. RANDOM MODE IS NOT SUPPORTED BY SLED.

### Meaning

For device (&00) "random mode" is adjusted.
SLED does not support cartridge devices in random mode.
SLED only supports "manual mode" or "automatic mode".

## NSD3930

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3930 DEVICE (&00) IS NOT IN AUTOMATIC OR MANUAL MODE. SLED ONLY SUPPORTS AUTOMATIC OR MANUAL MODE.

### Meaning

For device (&00) neither "automatic mode" nor "manual mode" is adjusted.
SLED does not support cartridge devices in other modes.

## NSD3932

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD3932 VOLUME (&00) IS ENCRYPTED. SLED DOES NOT SUPPORT ENCRYPTED VOLUMES.

### Meaning

Encrypted tapes are not supported by SLED.

### Response

Please select another tape.

## NSD3940

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD3940 VOLUME TYPE NOT SUPPORTED BY CARTRIDGE DEVICE

### Meaning

On the current device only volumes of type
TAPE-C1 or TAPE-C2 can be processed.

## NSD5000

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5000 DEFAULT TAKEN: (&00)=(&01)

### Meaning

The previous message has been answered with EOT (empty input).
SLED provides the default value (&01) for parameter (&00).
(&00): Keyword.
(&01): Default value.

## NSD5001

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5001 PARAMETER WITH UNDEFINED OR MISSING KEYWORD IGNORED: (&00)=(&01)

### Meaning

A parameter has been entered in advance, whose keyword is
missing or not defined. This part of input will be ignored.
(&00): Keyword or '?' .
(&01): Parameter value.

## NSD5002

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5002 UNEXPECTED KEYWORD PARAMETER IGNORED: (&00)=(&01)

### Meaning

A parameter has been entered in advance which is not expected
as response of the previous message. This part of input will
be ignored.
(&00): Keyword.
(&01): Parameter value.

## NSD5003

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5003 REDUNDANT KEYWORD PARAMETER IGNORED: (&00)=(&01)

### Meaning

A parameter has been entered in advance. During further
processing it turned out that the information of this
parameter was not used.
This part of input will be ignored, the parameter value will
not be checked.
(&00): Keyword.
(&01): Parameter value.

## NSD5004

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5004 KEYWORD PARAMETER (&00)=(&01) OVERWRITTEN BY (&00)=(&02)

### Meaning

A parameter already entered in advance has been entered
again. The last value entered is valid.
(&00): Keyword.
(&01): Old parameter value
(&02): New parameter value.

## NSD5005

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5005 ILLEGAL PARAMETER VALUE: (&00)=(&01)

### Meaning

This part of input will be ignored.
(&00): Keyword.
(&01): Parameter value.

## NSD5006

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5006 PARAMETER : (&00)=(&01) NOT SUPPORTED FOR THIS HSI

### Meaning

Parameter not supported for this HSI
(&00): Keyword.
(&01): Parameter value.

## NSD5100

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5100 RESTART OF BS2000 ? REPLY (YES=Y; NO=N; EOT=N)

### Meaning

An automatic SLED was interrupted by an error and continued
in manual mode.
BS2000 may be reloaded and restarted as foreseen in the
automatic mode. If not, SLED continues in manual mode.

### Response

Y : BS2000 is restarted.
N : SLED continues in manual mode (default).

## NSD5200

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5200 SPECIFY NAME OF SLED PARAMETER FILE. REPLY (NO FILE=EOT; FILENAME; STANDARD NAME=STD; END)

### Meaning

SLED uses the specified file as control input
for the following run.

### Response

(PARFILE=) EOT : No parameter file (default)
(PARFILE=) filename : Parameter file name (fully qualified)
(PARFILE=) STD : default parameter file name is
$TSOS.SYSPAR.SLED.vvv of home PVS,
with vvv = BS2000 version (e.g. vvv = 210)
(PARFILE=) END : terminate SLED

## NSD5201

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5201 PARAMETER FILE (&00) IN PROCESS

### Meaning

The file (&00) was opened by SLED in INPUT-mode. It is inter-
preted as a SLED parameter file, of which each record controls
one SLED run completely - in sense of 'input in advance'
for message NSD3000.
(&00): Fully qualified name of SLED parameter file.

## NSD5202

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5202 PARAMETER RECORD (&00): (&01)

### Meaning

From the current parameter file (see message NSD5201) SLED
processes the record (&00) with the contents (&01).
(&00): Record number of the current parameter file
(&01): Contents of the record

## NSD5203

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5203 END OF PARAMETER FILE (&00) REACHED

### Meaning

SLED has reached the end of the parameter file but
no record was found with 'OUTPUT=END'.
(&00): fully qualified name of SLED parameter file.

## NSD5210

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5210 PARAMETER FILE (&00) NOT FOUND

### Meaning

The specified SLED parameter file (&00) has not been found in
the catalog of the Home-PVS or of the PVS, which was specified
explicitly by the CATID.
(&00): Fully qualified name of SLED parameter file.

## NSD5213

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5213 PARAMETER FILE (&00) NOT ON PVS

### Meaning

(&00): Fully qualified name of SLED parameter file.

## NSD5214

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5214 UNEXPECTED FSTAT ERROR FOR PARAMETER FILE (&00), DMS-RC=(&01)

### Meaning

(&00): Fully qualified name of SLED parameter file.
(&01): Return code from DMS (FSTAT-macro)
See also previous IPL message.

## NSD5220

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5220 PARAMETER FILE (&00) IS EMPTY

### Meaning

(&00): Fully qualified name of SLED parameter file.

## NSD5221

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5221 PARAMETER FILE (&00) IS NOT A SAM-FILE

### Meaning

The parameter file does not have the attribute FCBTYPE=SAM.
(&00): Fully qualified name of SLED parameter file.

## NSD5222

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5222 PARAMETER FILE (&00) DOES NOT HAVE STANDARD BLOCK SIZE

### Meaning

The parameter file must have the attribute
FCBTYPE=(STD,1) or FCBTYPE=(STD,2).
(&00): Fully qualified name of SLED parameter file.

## NSD5223

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5223 PARAMETER FILE (&00) DOES NOT HAVE VARIABLE RECORD FORMAT

### Meaning

The parameter file must have the attribute RECFORM=V .
(&00): Fully qualified name of SLED parameter file.

## NSD5224

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5224 ERROR IN SAM STRUCTURE OF PARAMETER FILE (&00)

### Meaning

The parameter file is not accessible via SAM.
(&00): Fully qualified name of SLED parameter file.

## NSD5225

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5225 RECORD SIZE OF PARAMETER FILE (&00) TOO LARGE

### Meaning

The parameter file contains records longer than 256 byte.
(&00): Fully qualified name of SLED parameter file.

## NSD5226

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5226 PARAMETER RECORD (&00) REJECTED BECAUSE OF INVALID SIZE

### Meaning

(&00): Record number of the current parameter file.

## NSD5230

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5230 ERROR DURING OPEN OF PARAMETER FILE (&00), DMS-RC=(&01)

### Meaning

(&00): Fully qualified name of SLED parameter file.
(&01): Return code from DMS (OPEN-macro)
See also previous IPL message.

## NSD5231

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5231 ERROR ON READING PARAMETER FILE (&00), DMS-RC=(&01), BLOCK=(&02)

### Meaning

(&00): Fully qualified name of SLED parameter file.
(&01): Return code from DMS (PAM-macro).
(&02): Block number where the error occurred.
See also previous IPL message.

## NSD5240

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5240 PARAMETER RECORD (&00) REJECTED BECAUSE OF INVALID CHARACTERS

### Meaning

A parameter record contains lower case letters,
or invalid or non printable characters.
(&00): Record number of the current parameter file.

## NSD5241

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5241 PARAMETER RECORD (&00) EMPTY

### Meaning

(&00): Record number of the current parameter file.

## NSD5245

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD5245 PROCESSING OF CURRENT PARAMETER FILE TO BE TERMINATED? REPLY (Y; N; EOT=Y)

### Response

Y : processing of current parameter file is terminated.
N : processing of current parameter file is continued.
The erroneous parameter record is ignored.

## NSD5500

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5500 ILLEGAL REPLY: (&00)

### Meaning

The message answered incorrectly will be issued again.
(&00): Reply to previous message.

## NSD5600

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5600 COMMAND IGNORED

### Meaning

An asynchronous input (command) was not allowed
in this situation.

## NSD5601

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5601 ILLEGAL INPUT: (&00)

### Meaning

An asynchronous input (command) could not be treated.
(&00): input of the operator.

## NSD5602

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5602 CURRENT PRINT STOPPED BY OPERATOR

### Meaning

The command /BREAK has been executed.
SLED continues with message NSD9002.

## NSD5603

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5603 LAST BLOCK WRITTEN: (&00)

### Meaning

This message is the reply of SLED, if the /STATUS-
command is executed during the NOEDIT function.
(&00): logical block number of the last block already
written to the SLED output file or output tape.

## NSD5604

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD5604 CURRENT MEMORY ADDRESS PRINTED: (&00)

### Meaning

This message is the reply of SLED, if the /STATUS-
command is executed during the EDIT function.
(&00): Address of the 4K page currently printed.

## NSD7200

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7200 MAIN MEMORY ERROR: FSA = (&00) MCIC = (&01) (&02)

### Meaning

This message is displayed if a Machine Check has
occurred when accessing main memory.
(&00): Failing Storage Address (FSA).
(&01): 1st word of Machine Check Interruption Code
(&02): 2nd word of Machine Check Interruption Code

## NSD7201

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7201 NUMBER OF DETECTED MAIN MEMORY ERRORS: (&00)

### Meaning

This message is displayed after dump of main memory,
if at least one memory error has been detected.
SLED continues.
(&00): number of errors.

## NSD7311

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7311 MAXIMUM NUMBER OF HSA MEMORY ERRORS HAS BEEN REACHED IN CURRENT AREA

### Meaning

This message is displayed after dump of HSA,
if the maximum of memory errors has been reached.
SLED continues with the next section.

## NSD7312

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7312 HSA CANNOT BE SAVED : "READ HSA" GIVES CC=3

### Meaning

The HSA cannot be saved, because the OSF-Call READ HSA has
not been installed.
SLED continues with the next section.

## NSD7313

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7313 HSA CANNOT BE SAVED : HSA DESCRIPTION IS INVALID

### Meaning

The HSA cannot be saved, because the HSA description
delivered by IPL is not correct.
SLED continues with the next section.
(When dumping a VM2000 guest system the HSA cannot be saved.)

## NSD7314

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7314 END OF HSA REACHED, "READ HSA" GIVES CC=1 AT ADDRESS (&00)

### Meaning

The saving for the HSA has been ended. OSF-Call READ HSA
gives CC=1 (address out of HSA)
SLED continues with the next section.
(&00): Address, which has caused CC=1

## NSD7315

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7315 SAVING OF HSA ABORTED : UNRECOVERABLE MEMORY ERROR

### Meaning

Saving of the HSA has been aborted due to an
unrecoverable memory error (FSA not valid).
SLED continues with the next section.

## NSD7316

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7316 IOHIOSDP section : SVP error: (&00). Use /HELP-MSG (&01) for more information.

### Meaning

$HSVP read-HSA reports error during constructing the IOHIOSDP section.
(&00): SVP response.
(&01): MSG-ID.

## NSD7317

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7317 IOHIOSDP section : no output possible. $HSVP error: (&00).

### Meaning

Due to $HSVP error (&00) IOHIOSDP section could not be written.
SLED continues with the next section.

## NSD7413

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7413 PSA CANNOT BE SAVED : PSA DESCRIPTION IS INVALID

### Meaning

The PSA cannot be saved, because the PSA description
delivered by IPL is not correct.
SLED continues with the next section.

## NSD7600

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD7600 SPECIFY HOME-PVSID OF SYSTEM TO BE DUMPED. REPLY (PVSID; IGNORE=EOT)

### Meaning

SLED cannot determine the PVSID of the interrupted system run.
This PVSID is necessary if system files are to be dumped.

### Response

pvsid = enter identifier
1 to 4 characters from (A..Z, 0..9)
EOT = Ignore. SLED continues, but system files cannot be
dumped.

## NSD7601

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7601 PUBRES OF HOME-PVS NOT ACCESSIBLE. NO OUTPUT OF SYSTEM FILES

### Meaning

SLED could not determine the Home-PVSID
of the dumped system, or the PUBRES of the Home-PVS
is not online.
Hence the system catalog is not available and no system files
can be saved.

## NSD7602

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7602 NO USABLE CATALOG OF SYSTEM TO BE DUMPED. NO OUTPUT OF SYSTEM FILES

## NSD7603

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7603 SYSTEM FILE (&00) NOT FOUND: DMS-RC = (&01)

### Meaning

System file (&00) not found. The corresponding section of
the SLED output file is skipped.
(&00): Name of system file
(&01): Return code from DMS (FSTAT-macro).

## NSD7604

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7604 DUE TO READ ERROR (I/O ERROR, DISK NOT ONLINE) SYSTEMFILE IS NOT OR PARTIALLY WRITTEN INTO SLEDFILE.

### Meaning

SYSTEMFILE NOT OR PARTIALLY WITHIN SLEDFILE.

### Response

IF NEEDED HAND OVER SYSTEMFILE LATER.

## NSD7800

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7800 INVALID SYSTEM TABLE ADDRESS. PAGING AREA NOT ACCESSIBLE

### Meaning

The address of a system table needed for the output of
the virtual memory areas is invalid or a system table is
overwritten by SLED/IPL code.
No data which reside on the Paging Area are saved
in the SLEDFILE.

## NSD7801

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7801 NO DATA FROM PAGING AREA ARE SAVED

### Meaning

No data which reside on the Paging Area are saved
in the SLEDFILE.

## NSD7802

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7802 BVDT INCONSISTENT. ACCESS TO PAGING AREA MAY BE NOT POSSIBLE.

### Meaning

The end of BVDT-entries is not the same as indicated by SVMT.
Pages to be read from paging area might be incorrect or
missing.

## NSD7900

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7900 NAME OF THE CORRESPONDING IOHDUMP : (&00)

### Meaning

Parallel to this Sledfile a IOHDUMP was generated
It can be found under the given name.

## NSD7901

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD7901 NAME OF THE CORRESPONDING IOSDUMP : (&00)

### Meaning

Parallel to this Sledfile a IOSDUMP was generated
It can be found under the given name.

## NSD9001

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD9001 SPECIFY EDIT MODE. REPLY (STD; NHW; EOT=STD; - (BACKTRACK))

### Meaning

The amount of SLED print output is to be defined.

### Response

(MODE=) STD : maximum amount (default)
(MODE=) NHW : no hardware, only specified memory areas
- : Backtrack.
The following parameters may be entered in advance:
(MODE=) mode (,LIMITS=(V)a / (V)a-b / (V)ALL)

## NSD9002

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD9002 SPECIFY MEMORY LIMITS OR END. REPLY (A; A-B; ALL; - (BACKTRACK); END)

### Meaning

Specification of the memory area (real or virtual)
to be edited.
A and B stand for hexadecimal addresses.
Leading zeroes may be omitted.
If END is specified the EDIT function is terminated.

### Response

(LIMITS=) V... : The area is to be printed in virtual mode.
The limits are to be specified as below.
(LIMITS=) a : Output of the 4K page, which
contains the specified address.
(LIMITS=) a-b : Output from address <a> to address <b>
(LIMITS=) ALL : Output of the whole main memory or
of the virtual address space
(LIMITS=) END : The EDIT-function is terminated;
back to message NSD3000.
- : Backtrack.

## NSD9010

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD9010 SPECIFY DEVICE NUMBER OF SLED OUTPUT PRINTER. REPLY (DEV#; - (BACKTRACK))

### Response

(DEV=) dev# : Device number (hexadecimal, 4 digits).
- : Backtrack.
The following parameters may be entered in advance:
(DEV=) dev# (,MODE=STD / NTT / NHW)
(,LIMITS=(V)a / (V)a-b / (V)ALL)

## NSD9020

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

NSD9020 SPECIFY MN OF SLED OUTPUT PRINTER. REPLY (MN; - (BACKTRACK))

### Response

(DEV=) mn : Device mnemonic, 2 alphanumeric characters
- : Backtrack.
The following parameters may be entered in advance:
(DEV=) mn (,MODE=STD / NTT / NHW)
(,LIMITS=(V)a / (V)a-b / (V)ALL)

## NSD9200

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD9200 UNRECOVERABLE I/O ERROR DURING OUTPUT TO PRINTER (&00)

### Meaning

(&00): Device number or
device mnemonic of line printer.
The next message will be:
- NSD9010/20, if the printer is no longer usable
- NSD9002, if the operator is able to fix the
lineprinter.
See also previous IPL message.

## NSD9201

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD9201 NO OPERABLE PRINTER FOUND ON DEVICE (&00)

### Meaning

Message NSD9010/20 will be issued again.
Possible reasons:
- typing error with (&00)
- print request terminates with error
(for example because of ROTATION mode)
(&00): Device number
or device mnemonic of line printer.

## NSD9202

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD9202 PRINTER ON DEVICE (&00) RESERVED ELSEWHERE

### Meaning

SLED continues with message NSD9010/NSD9020
(&00): specified device number or
device mnemonic.

## NSD9400

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD9400 AVAILABLE MAIN MEMORY: (&00)

### Meaning

(&00): size of main memory (hexadecimal digits).

## NSD9401

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD9401 OUTPUT OF MEMORY STARTED: LIMITS = (&00) - (&01)

### Meaning

(&00): lower memory limit
(&01): upper memory limit.

## NSD9402

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD9402 ILLEGAL MEMORY LIMIT: (&00)

### Meaning

(&00): illegal memory limit
SLED continues with message NSD9002.

## NSD9403

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD9403 MEMORY LIMIT OUT OF RANGE: (&00)

### Meaning

The specified address is outside the real main memory
or outside the virtual address space.
(&00): value in error
SLED continues with message NSD9002.

## NSD9404

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSD9404 NO PRINT OUTPUT OF VIRTUAL MEMORY POSSIBLE

### Meaning

It was not possible to determine valid system segment
tables. SLED continues with message NSD9002.

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages