## RFA0001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0001 SYSAFR. DATE '(&00)'

### Meaning

(&00): creation date in the form YYYY/MM/DD.

## RFA0002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0002 COMMAND PROCESSING COMPLETED

### Meaning

The command /SET-RFA-CONNECTION or
/REMOVE-RFA-CONNECTION or
/SHOW-RFA-CONNECTIONS has been executed successfully.

## RFA0003

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0003 ERROR '(&00)'. COMMAND PROCESSING ABORTED

### Meaning

Error (&00) occurred during the processing of the
/SET-RFA-CONNECTION or /REMOVE-RFA-CONNECTION command.
In a procedure all commands are rejected until /SET-JOB-STEP
or /LOGOFF.
(&00): error code.
01: possible reasons:
- incomplete MRSCAT entry.
- invalid MRSCAT entry.
- the remote MRSCAT status is INACCESSIBLE.
Contact the system administrator.
02: catalog identifier not found in MRSCAT.
The system administrator has to create the MRSCAT entry.
03: /SET-RFA-CONNECTION with the cat ID of the user default pubset is
not possible if the user default pubset is a shared pubset.
04: the /REMOVE-RFA-CONNECTION command is rejected because no
/SET-RFA-CONNECTION command has been issued before.
05: error during creation of RFA bourses and contingencies.
06: RFA connection inoperable.
Terminate the connection with the /REMOVE-RFA-CONNECTION command and
create a new one with the /SET-RFA-CONNECTION command.
07: BCAM did not answer within a specified time limit.
08: the /SET-RFA-CONNECTION command cannot be executed because the user
already has established the maximum number of 16 RFA connections.
09: insufficient class 5 memory for RFA tables.
Repeat the /SET-RFA-CONNECTION command later.
0A: shortage of BCAM.
Possible reasons:
- limit of BCAM applications,
- limit of BCAM connections,
- BCAM requests to try the action later.
Possible reason:
- the remote processor does not run.
- The local host is not known to BCAM in the partner system.
Cases 1 and 2: contact the system administrator.
0B: BCAM shutdown warning.
0C: BCAM shutdown finished.
0D: BCAM not active.
Contact the system administrator.
0E: unknown partner or unknown application $DIALOG on partner.
The host name found in the MRSCAT entry is not known to BCAM,
or the application $DIALOG on partner is not known to BCAM.
Contact the system administrator.
0F: request of connection has been rejected.
Contact the system administrator.
10: the operator disconnects BCAM.
Contact the system administrator.
11: error during creation of the partner task.
Possible reasons:
- error in the protocol.
- File $SYSAFR missing, not share or not cataloged on the
default user ID.
- The versions of $SYSAFR and the remote BS2000 do not fit together.
- User ID or account number unknown to the remote system.
- Invalid password.
Contact the system administrator
to install the (correct) file $SYSAFR or
to make file $SYSAFR share or
to establish the missing user ID and account number in the remote
system or
correct the command.
12: the /REMOVE-RFA-CONNECTION command is rejected while a program
is loaded.
Terminate the program and try the command again.
13: BCAM buffer too small.
BCAM has been generated with a buffer size which is not big enough
for RFA.
Contact the system administrator.
14: error during a read from a terminal:
a hardware error or the terminal is disconnected.
Try the command again.
15: for shared pubsets the user IDs of /SET-RFA-CONNECTION,
/SET-LOGON-PARAMETERS and the AFR partner task have to be the same.
Contact the system administrator to give a
/MODIFY-MASTER-CATALOG-ENTRY with SHARED-PUBSET=NO
for this catalog identifier.

## RFA0004

Destination: USER-TASK, CONSOLE Routing code: R Weight: 70

Warranty : NO

RFA0004 RFA BCAM CONNECTION ERROR '(&00)'

### Meaning

BCAM has detected an error.
This message is sent to the console for diagnostic purposes.
(&00): BCAM information word.

## RFA0005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0005 WARNING: COMMAND REJECTED FOR IMPORTED CATALOG

### Meaning

The user issued a /SET-RFA-CONNECTION command for an imported catalog.
Files on public volumes are not accessible.

## RFA0006

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

RFA0006 RFA PROTOCOL ERROR. RFA PARTNER TASK TERMINATED WITH DUMP

### Meaning

The partner task SYSAFR detected an error in the RFA protocol.

## RFA0007

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

RFA0007 CATALOG NOT AVAILABLE. INVALID HOST NAME

### Meaning

The MRS catalog entry with the catalog identifier specified
in the /SET-RFA-CONNECTION command contains an invalid host name.

### Response

Contact the system administrator to correct the host name.

## RFA0008

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

RFA0008 SPECIFY CATALOG IDENTIFIER

### Meaning

The mandatory operand <catalog identifier> in the
/SET-RFA-CONNECTION or /REMOVE-RFA-CONNECTION has not been specified.

### Response

Repeat the command with a catalog identifier.

## RFA0009

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

RFA0009 UNKNOWN OPERAND

### Meaning

The /SET-RFA-CONNECTION or /REMOVE-RFA-CONNECTION command contains
an unknown operand.

### Response

Compare the command with the description in the manual and correct it.

## RFA0010

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

RFA0010 INVALID KEYWORD

### Meaning

The /SET-RFA-CONNECTION or /REMOVE-RFA-CONNECTION command contains
an invalid keyword.

### Response

Compare the command with the description in the manual and correct it.

## RFA0011

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

RFA0011 INVALID OPERAND '(&00)'

### Meaning

The displayed operand in the /SET-RFA-CONNECTION or
/REMOVE-RFA-CONNECTION command has an invalid value.
(&00): Name of operand
CATALOG-ID
USER-IDENTIFICATION
ACCOUNT
PASSWORD
CONNECTION
ANSWER.

### Response

Compare the operand with the description in the manual and correct it.

## RFA0012

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0012 ERROR IN RFA OR IN TASK TABLES OR MEMORY MANAGEMENT

### Meaning

Possible reasons:
- A software error was detected during RFA processing.
- A request or release memory was terminated with system error.
- When trying to get a task specific or job specific information
an error was detected.

### Response

Contact system diagnosis if the reason of this error is unexplainable.

## RFA0013

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0013 NO REMOTE PARTNER. SYSAFR ABORTED

### Meaning

RDATA has been rejected with operand error.
This indicates that SYSAFR has been executed by a local user, which
cannot be done successfully. SYSAFR must be executed by a partner system.

## RFA0014

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0014 COMMAND NOT KNOWN IN REMOTE SYSTEM

### Meaning

A command, which was transmitted by RFA, is not known in the
remote system on account of the SDF system syntax file or on account
of the SDF user syntax file belonging to the user ID specified in the
/SET-RFA-CONNECTION command.

## RFA0015

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0015 PLEASE ENTER REPLY TO MESSAGE FROM '(&00)'

### Meaning

RFA asks the user to enter his answer to the message from
the remote system, which has just been displayed.
(&00): catalog identifier of the remote system.

### Response

Enter reply.

## RFA0016

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0016 VERSION OF REMOTE SYSTEM IS NOT SUPPORTED

### Meaning

A connection to the remote BS2000 version by RFA is not supported.

## RFA0017

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0017 NO ACTIVE RFA CONNECTIONS

### Meaning

There are no active RFA connections for this user identification.

## RFA0018

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0018 NO RFA CONNECTION

### Meaning

There does not exist any RFA connection to the given catalog identifier.

## RFA0019

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0019 WARNING: OUTPUT CUT

### Meaning

The output to SYSOUT is not complete.

## RFA0020

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0020 OUTPUT ERROR

### Meaning

An error occurred when giving the output to SYSOUT.

## RFA0021

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0021 NO BCAM NAME

### Meaning

The own (local) BCAM name could not be found out.

## RFA0022

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0022 SYSAFR (&00) NEEDS BS2000 (&01). BS2000 (&02) ACTIVE. SYSAFR ABORTED

### Response

Contact the system administrator to install the right SYSAFR.

## RFA0023

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0023 RFA CONNECTION INOPERABLE.

### Meaning

The RFA connection is not established correctly; it is inoperable.

### Response

Terminate the connection with /REMOVE-RFA-CONNECTION and create a new
one with /SET-RFA-CONNECTION.

## RFA0024

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0024 NO ADDITIONAL RFA CONNECTION POSSIBLE.

### Meaning

The maximum number of RFA connections is already established.

## RFA0025

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0025 PROGRAM LOADED. COMMAND PROCESSING ABORTED.

### Meaning

The command /REMOVE-RFA-CONNECTION is rejected while a program is
loaded.

### Response

Terminate the program and try the command again.

## RFA0026

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0026 COMMAND REJECTED FOR A SHARED PUBSET.

### Meaning

The SET-RFA-CONNNECTION command is rejected when the catalog identifier
specifies a shared pubset and
- the catalog identifier specifies the user default pubset or
- the userids of /SET-RFA-CONNECTION, /SET-LOGON-PARAMETERS and the
AFR partnertask are not the same.

## RFA0027

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

RFA0027 RFA CONFIGURATION ERROR.

### Meaning

During the command processing an error occurred in the RFA configuration.
For example
- the host name is missing in the MRSCAT entry or
- the partner host is unknown to BCAM.

### Response

For more detail look at the obtained message RFA0003 and
contact the system or network administrator if necessary.

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages