## SEMREVI

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SEMREVI COMP=SEMMF,VERS=91A,DATE=201215

## SEM1001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1001 INCORRECT KEY PRESSED FOR DATA TRANSFER

### Response

Press the DUE key to transfer data from the form. Press the K2 key to
interrupt the monitor.

## SEM1002

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1002 INVALID CONFIGURATION NAME

### Response

Enter a valid configuration name. In interactive mode, letters, digits and
blank may be entered. In batch mode, letters, digits and '*BLANK' are
permitted.

## SEM1003

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1003 INVALID INPUT FOR FILE

### Response

Enter 'x' or 'X'.

## SEM1004

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1004 INVALID INPUT FOR SCREEN

### Response

Enter 'x' or 'X' or 'r' or 'R' or 'c' or 'C'.

## SEM1005

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1005 INVALID INPUT FOR SYSLST

### Response

Enter 'x' or 'X'.

## SEM1006

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1006 INVALID INPUT FOR SELECTION OF OUTPUT FORM

### Response

Enter 'x' or 'X'.

## SEM1007

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1007 NO DESTINATION SPECIFIED

### Response

At least one of the possible destinations ('SCREEN', 'SYSLST' or 'FILE')
must be specified.

## SEM1008

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1008 CONTINUATION OF COUNTER RESET IMPOSSIBLE WITHOUT RESET!

### Meaning

To continue the output (input 'C') relative to a reset there has to be
a reset (input 'R') before.

### Response

First type in 'R' (RESET) for Output Medium 'SCREEN' to initialize a
Counter Reset. After that you can keep the Reset by typing 'C'
(Continuation) with an appropriate new selection of output.

## SEM1009

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1009 A CONTINUATION CAN NOT EXTEND SELECTION OF THE RESET!

### Meaning

A continuation of a counter reset is possible only if there is a backup
of the counters at reset time! Therefore the new configuration selection
needs to have been part of the selection at reset time.

### Response

Have a new reset with the new selection

## SEM1011

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1011 INVALID 'SESAM-DBH' 'NAM' SPECIFICATION

### Response

Enter a valid 'SESAM-DBH' 'NAM' identifier. In interactive mode, letters,
digits and blank may be entered. In batch mode, letters, digits, '*BLANK'
and '*NONE' are permitted.

## SEM1012

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1012 'SESAM-DBH' SPECIFIED, BUT NO 'SESAM-DBH' OUTPUT SCREEN SELECTED.

### Meaning

This message only appears if 'SCREEN"" and/or 'SYSLST' was selected for
output.

### Response

At least one of the 'SESAM-DBH' output screens must be selected.

## SEM1013

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1013 OUTPUT TO FILE IN PROGRESS

### Meaning

This message is only displayed if output to 'SCREEN' has not been
requested.

## SEM1014

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1014 OUTPUT TO SYSLST AND FILE IN PROGRESS

### Meaning

This message is only displayed if output to 'SCREEN' has not been
requested.

## SEM1015

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1015 OUTPUT TO SYSLST IN PROGRESS

### Meaning

This message is only displayed if output to 'SCREEN' has not been
requested.

## SEM1016

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1016 NO OUTPUT TO SYSLST POSSIBLE

## SEM1017

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1017 NO OUTPUT TO FILE POSSIBLE

## SEM1018

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1018 ERROR IN THE 'SET-MONITOR-OPTIONS' STATEMENT

### Meaning

This message is only output in batch mode.

## SEM1019

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1019 'INFORM-PROGRAM' REJECTED. ONLY MESSAGE TEXT 'STOP' OR 'SEL' PERMITTED

### Meaning

The given command INFORM-PROGRAM MSG='message-text' or INTR 'message-text'
or SEND-MSG TO=PROGRAM, MSG='message-text' has been rejected. Only the
message text 'SEL' or 'STOP' is allowed.

### Response

Hit the K2 key again and type a correct command INFORM-PROGRAM
MSG='message-text'.

## SEM1020

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1020 SDF SYNTAX FILE DOES NOT EXIST.

### Meaning

'SESMON' cannot be started, since the SDF syntax file is not available.

### Response

Ask the system administrator to add the SDF syntax file

## SEM1021

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1021 ALL SELECTED TASKS HAVE BEEN TERMINATED

### Meaning

The monitor has finished its evaluation. In interactive mode, an
additional evaluation task may be entered in the SELECTION form. In batch
mode, the monitor is terminated.

## SEM1022

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1022 NO SESDCN AND NONE OF THE SPECIFIED SESAM DBHS EXIST IN THE CONFIGURATION

### Meaning

This message is only output in batch mode.

## SEM1023

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1023 INPUT OF REFRESH TIME WITHOUT SELECTION OF CORRESPONDING DESTINATION

## SEM1024

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1024 NO OUTPUT FORM SPECIFIED.

### Meaning

This message is only displayed if 'SCREEN' or 'SYSLST' was selected as the
destination.

### Response

At least one of the output forms must be selected.

## SEM1025

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1025 SESAM DBH OUTPUT FORM SPECIFIED, BUT NO SESAM DBH

## SEM1026

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1026 SPECIFIED SESAM DBH DOES NOT EXIST IN THE CONFIGURATION

### Meaning

This message is only output in interactive mode.

## SEM1027

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1027 NO SESDCN IN CONFIGURATION

### Meaning

This message is only output in interactive mode.

## SEM1028

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1028 ALL SESAM DBHS SPECIFIED IN THE CONFIGURATION HAVE BEEN TERMINATED.

## SEM1029

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1029 OUTPUT TO FILE STILL IN PROGRESS

## SEM1030

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1030 SPECIFIED SESAM DBH AND SESAM MONITOR HAVE DIFFERENT CORRECTION LEVELS.

### Meaning

This message is only output in interactive mode.
DBH and monitor were loaded from diffenrent libraries that are not
compatible.
Therefor it is impossible to present data from this DBH.

### Response

Use the same library for DBH and monitor.

## SEM1032

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1032 SCREEN REFRESHTIME SPECIFIED AS '0', BUT MORE THAN ONE SCREEN SELECTED.

### Response

Specify different SCREEN REFRESHTIME or select only one screen.

## SEM1033

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1033 SESAM DBH '(&00)' NOT IN SPECIFIED CONFIGURATION

### Meaning

This SESAM DBH is removed from the evaluation. All other tasks are
monitored normally.

### Response

This message is displayed only in batch mode.

## SEM1034

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1034 SESAM DBH '(&00)' HAS A DIFFERENT CORRECTION LEVEL AS THE SESAM MONITOR.

### Meaning

This SESAM DBH is removed from the evaluation. All other tasks are
monitored normally.

### Response

This message is displayed only in batch mode.

## SEM1036

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1036 ALL TASKS EXAMINED FOR THE SELECTED FORMS WERE TERMINATED

### Meaning

In interactive mode this message is displayed if "SCREEN" or SYSLST was
selected as the destination.

## SEM1037

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1037 INVALID MAXIMUM NUMBER OF TRANSACTIONS TO SYSLST

### Response

Enter a valid number of transactions. The values '0' or '10'
through '999' are permitted.

## SEM1038

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1038 MAX. NUMBER OF TRANSACTIONS ENTERED WITHOUT SELECTING TRANSACTIONS FORM

### Response

Select TRANSACTIONS form or enter "0" for maximum number
of transactions.

## SEM1039

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1039 MEMORY BOTTLENECK ON CREATING TABLE FOR THE TRANSACTIONS

### Response

Increase user address space in the join entry for the user ID
or
in interactive mode, reduce the maximum number of transactions to be
output to SYSLST; in batch mode restart the monitor with a lower number
of transactions to be output to SYSLST.

## SEM1050

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1050 THE USED BS2000 VERSION DOES NOT SUPPORT THE TRANSFER OF DB DATA TO OPENSM2.

### Meaning

The used BS2000 version does not support the transfer of db data
to openSM2. The BS2000 Version must be V8 or higher.

## SEM1051

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1051 SESAM-SQL MEASUREMENT PROGRAM IN SM2 NOT YET STARTED.

### Meaning

The SESAM-SQL measurement program in SM2 is not yet started.

### Response

Start measurement program with SM2 administration command
START-MEASUREMENT-PROGRAM=*SESAM-SQL.

## SEM1052

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1052 SM2 GATHERER TASK DOWN.

### Meaning

The SM2 gatherer task is not yet started or abnormal terminated.

### Response

After evaluating the reason and correcting restart SM2 (START-SM2)
and activate measurement program for SESAM/SQL.

## SEM1053

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1053 SUBSYSTEM SM2 NOT ACTIVE.

### Meaning

The subsystem is not started.

### Response

Start the subsystem SM2.

## SEM1054

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1054 OUTPUT SM2, BUT NO SESAM DBH SPECIFIED.

### Meaning

By specification of SM2 for OUTPUT you must specify at least one dbh
in the operand DBH-NAMES.

### Response

Correct the options and start SESMON again.

## SEM1055

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEM1055 INTERNAL ERROR IN SM2.

### Meaning

In SM2 a system error occurred. No dump was generated.

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages