## NVICOPY

Destination: USER-TASK Routing code: Weight: 20

Warranty : NO

NVICOPY Copyright (C) (&01) (&00). All rights reserved

## NVILOAD

Destination: USER-TASK Routing code: Weight: 20

Warranty : NO

NVILOAD Program '(&00)', Version '(&01)' of '(&02)' loaded from file '(&03)'

## NVIREVI

Destination: USER-TASK Routing code: Weight: 20

Warranty : NO

NVIREVI INIT message file, version 104

## NVISTRT

Destination: USER-TASK Routing code: Weight: 20

Warranty : NO

NVISTRT Procedure '(&00)', Version '(&01)' of '(&02)' started from file '(&03)'

## NVI0000

Destination: USER-TASK, CONSOLE Routing code: G Weight: 70

Warranty : NO

NVI0000 PROGRAM INIT READY

### Meaning

Program INIT is loaded and executable.

## NVI0001

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0001 ENTER COMMAND. (END = TERMINATE INIT)

### Meaning

An INIT command is requested.
INIT will be terminated by entering 'END'.

### Response

Enter command with appropriate operands or enter 'END'.

## NVI0002

Destination: USER-TASK, CONSOLE Routing code: G Weight: 70

Warranty : NO

NVI0002 ENTER ADDITIONAL OPERANDS

### Meaning

Further initialization operands are requested, a '-' character in the
previous statement line having indicated that the line is to be continued.

## NVI0003

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0003 VOLUME LABELS (&00):

### Meaning

The output of the read volume labels is announced.
(&00): (ISO7) : the labels are coded in 7-bit code
' ' : the labels are coded in EBCDIC code

## NVI0004

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0004 (&01) LABEL: '(&00)'

### Meaning

(&00): 80 bytes (printable), volume label
Trailing blanks are suppressed.
(&01): Label type (VOL1,VOL2,...HDR1,HDR2,...)

## NVI0005

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0005 FIRST BLOCK IS NO VOLUME LABEL

### Meaning

The first block on the volume does not begin with VOL1.

## NVI0007

Destination: USER-TASK, CONSOLE Routing code: T Weight: 98

Warranty : NO

NVI0007 OVERWRITE VOLUME ? REPLY (YES=YES N=NO)

### Meaning

This is the last opportunity to stop initialization of the volume,
e.g. if the wrong volume has been assigned.

### Response

YES: The volume will be overwritten.
For reasons of security no abbreviation is allowed as a response.
N : The volume assignment will be revoked.

## NVI0008

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0008 DATA SECURITY ERASE STARTED

### Meaning

This action may take from several minutes up to hours, depending on the
volume type.

## NVI0009

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0009 DATA SECURITY ERASE COMPLETED

## NVI0010

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0010 INITIALIZATION OF VOLUME '(&00)' ON DEVICE '(&01)' COMPLETED

### Meaning

The volume can now be used in BS2000.
(&00): VSN of the volume or
'*WTM' if only tape marks were written
(&01): Mnemonic device name

## NVI0011

Destination: USER-TASK, CONSOLE Routing code: G Weight: 70

Warranty : NO

NVI0011 PROGRAM INIT TERMINATED NORMALLY

## NVI0012

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0012 CONTINUE ? REPLY (Y = YES; N = NO)

## NVI0013

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0013 INIT-OPTIONS IN EFFECT: (&00)

### Meaning

The optional INIT functions, activated with the INIT command OPTION, are
displayed.
(&00): operand keywords of the INIT-operand OPTION

## NVI0100

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0100 RESTRICTED ACCESS '(&00)'

### Meaning

(&00): 'BYTE 11 IN VOL1' or 'BYTE 54 IN HDR1'.
Access to the volume or to the first file on the volume is restricted by
- a character not equal '0' or ' ' in byte 11 of VOL1-label
(access to the volume permitted only for the owner), or by
- a character not equal ' ' in byte 54 of HDR1-label
(access to the first file on the volume permitted only for the owner).

## NVI0101

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0101 EXPIRATION DATE OF FIRST FILE ON VOLUME NOT YET REACHED

### Meaning

The expiration date in the HDR1 label of the first file on the volume
is not yet reached.

## NVI0102

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0102 NO LABELS FOUND. VOLUME IS EMPTY

## NVI0103

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0103 NO LABELS FOUND. TAPE MARKS READ

## NVI0104

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0104 I/O-ERROR WHILE READING LABELS

### Meaning

A device error was reported while reading the labels. It is neither
'empty volume' nor 'tapemarks detected'. If the instruction 'INIT' with
the operand 'NEW' was given, but the volume is not empty, then, the
device error recovery was not in effect. In this case, the labels may
be readable with the error recovery in effect.

### Response

If the instruction 'INIT' was given with the operand 'NEW' retry 'INIT'
without 'NEW' or use 'LIST' to read the labels. In any other case see
preceding messages on console or HEL-file entries.

## NVI0105

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0105 FIRST FILE ON VOLUME IS PROTECTED BY PASSWORD

### Meaning

The HDR3-Label of the first file on the volume is containing a read
password and/or a write password.
- read password : Bytes 57-60
- write password : Bytes 61-64

## NVI0106

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0106 FIRST FILE ON VOLUME IS WRITE PROTECTED

### Meaning

In the HDR3-Label of the first file on the volume only read access is
permitted (Byte 69).
- '0' : read and write access
- '1' : only read access

## NVI0113

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0113 VOLUME LABELS (&00):

### Meaning

The output of the read volume labels is announced.
(&00): (ISO7) : the labels are coded in 7-bit code
' ' : the labels are coded in EBCDIC code

## NVI0114

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0114 (&01) LABEL: '(&00)'

### Meaning

(&00): 80 bytes (printable), volume label
Trailing blanks are suppressed.
(&01): Label type (VOL1,VOL2,...HDR1,HDR2,...)

## NVI0115

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0115 FIRST BLOCK IS NO VOLUME LABEL

### Meaning

The first block on the volume does not begin with VOL1.

## NVI0117

Destination: USER-TASK, CONSOLE Routing code: T Weight: 98

Warranty : NO

NVI0117 OVERWRITE VOLUME ? REPLY (YES=YES N=NO)

### Meaning

This is the last opportunity to stop initialization of the volume,
e.g. if the wrong volume has been assigned.

### Response

YES: The volume will be overwritten.
For reasons of security no abbreviation is allowed as a response.
N : The volume assignment will be revoked.

## NVI0200

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0200 INITIALIZATION ABORTED

### Meaning

The initialization request was aborted, because the query as to whether
the volume is to be overwritten was not answered with 'YES'.

## NVI0201

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0201 VOLUME IS PROTECTED. INITIALIZATION REQUEST REJECTED

### Meaning

Extended write protection (OPTION PROT) was set prior to the
initialization request and at least one of the following criteria is met:
- Volume access is permitted to the owner only
(Byte 11 in the VOL1 label is neither '0' nor ' ').
- Access to the first file on the volume is permitted to the owner
only (Byte 54 in the HDR1 label is neither '0' nor ' ').
- The retention period of the first file on the volume is not yet
expired (Byte 48-53 in the HDR1 label).
- The first file on the volume is protected by a read and/or by a
write password (Byte 57-64 in the HDR3 label).
- Only read access is permitted to the first file on the volume
(Byte 69 in the HDR3 label is '1').

### Response

If the volume is to be overwritten, extended write protection must
be revoked.

## NVI0202

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0202 FORMATTING STARTED ON DEVICE (&00)

### Meaning

Formatting of the volume has been started.
This action may take from several minutes up to hours.
(&00): mnemonic device name (MN)

## NVI0203

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0203 FORMATTING COMPLETED ON DEVICE (&00)

### Meaning

Formatting of the volume is completed.
(&00): mnemonic device name (MN)

## NVI0204

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0204 FORMATTING NOT POSSIBLE FOR VOLUME TYPE (&00). INITIALIZATION CONTINUES

### Meaning

Formatting of a volume of type (&00) has been requested with operand
'FORMAT', but the volume type doesn't offer the formatting feature.
The operand 'FORMAT' is ignored.
(&00): volume type

## NVI0205

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0205 FORMATTING NOT POSSIBLE ON DEVICE (&00). INITIALIZATION CONTINUES

### Meaning

Formatting of a volume has been requested with operand 'FORMAT'.
The device (&00) doesn't offer the formatting feature.
The operand 'FORMAT' is ignored.
(&00): mnemonic device type (MN)

## NVI0208

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0208 DATA SECURITY ERASE STARTED

### Meaning

This action may take from several minutes up to hours, depending on the
volume type.

## NVI0209

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0209 DATA SECURITY ERASE COMPLETED

## NVI0210

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0210 INITIALIZATION OF VOLUME '(&00)' ON DEVICE '(&01)' COMPLETED

### Meaning

The volume can now be used in BS2000.
(&00): VSN of the volume or
'*WTM' if only tape marks were written
(&01): Mnemonic device name

## NVI0211

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0211 DATA SECURITY ERASE NOT POSSIBLE FOR VOLUME TYPE "(&00)". INITIALIZATION CONTINUES WITHOUT ERASING

### Meaning

Data security erase has been requested for volume of type (&00)
by specifying operand 'ERASE', but erasing is not allowed for
this volume type because it is a WORM medium (Write Once, Read Many).
The operand 'ERASE' is ignored, initialization continues without
data security erase
(&00): volume type

## NVI0212

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0212 WRITING OF HDR LABELS NOT ALLOWED FOR VOLUME TYPE "(&00)". INITIALIZATION CONTINUES WITHOUT HDR LABELS

### Meaning

Writing of dummy HDR labels is not allowed for volume type (&00),
because it is a WORM medium (Write Once, Read Many).
Initialization continues, only the VOL1 label is written as if
option NOHDR has been specified.
By specifying option NOHDR with the initialization request, this
message will not been issued.
(&00): volume type

## NVI0300

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0300 REQUESTED INIT VERSION '(&00)' ONLY SUPPORTS BS2000 (&01)

### Meaning

(&00): INIT version number, e.g. Vnn.nann
(&01): BS2000 version number, e.g. Vnn.n

### Response

Start an INIT version which can run on the loaded BS2000 version.

## NVI0301

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0301 PRIVILEGE MISSING FOR REQUESTED INIT FUNCTION

### Meaning

The user task has not the necessary privilege (see manual) to execute
the requested INIT function.

### Response

Contact the system administrator.

## NVI0302

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0302 ERROR DURING SYSTEM CALL. INITIALIZATION PROCESSING ABORTED. DIAGNOSTIC INFORMATION: '(&00)'

### Meaning

(&00): Diagnostic information
(Interface name, function id, returncode, call id)

### Response

Contact system administrator.

## NVI0303

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0303 DEVICE DOES NOT SUPPORT SPECIFIED VOLUME TYPE

### Meaning

A volume of the specified volume type is not supported by the assigned
device.

### Response

Start initialization on a device which supports the specified volume
type.

## NVI0305

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0305 WRONG VOLUME

### Meaning

The allocated volume may not be used, because its VSN is different to the
VSN requested in the operand 'CHECK=vsn'.

### Response

Assign the correct volume or choose another CHECK-VSN.

## NVI0306

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0306 ERROR DURING ALLOCATION OF A DEVICE OR VOLUME, RC='(&00)'

### Meaning

The requested INIT function has been cancelled.
See return code for the reason.
(&00): Return code (n1n2) :
n1=04: Device cannot be reserved
n2=00: Device temporarily not available
04: Device permanently not available
08: Reservation not allowed
0C: Device not defined
n1=08: Volume cannot be reserved
n2=00: Volume temporarily not available
04: Volume permanently not available
08: Reservation not allowed
n1=0C: Illegal operand
n2=10: Invalid operation.

### Response

Change the device or volume or take other measures in accordance with
the return code.

## NVI0307

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0307 WRITTEN VOL1 LABEL IS INCORRECT

### Meaning

An error occurred when reading control of VOL1-Label after
initialization.

### Response

Use an other volume or device, or take other measures in accordance
with possible console messages of the device error recovery.

## NVI0308

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0308 I/O ERROR WHILE WRITING LABELS OR WHILE ERASING THE VOLUME

### Meaning

The device error recovery has detected an I/O error.

### Response

For further information see preceding messages on console (as far as
issued) or HEL-file entries (as far as written).

## NVI0309

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0309 VOLUME WITH VSN '(&00)' CANNOT BE USED. INITIALIZATION ABORTED

### Meaning

An error has been detected during initialization of the volume.
The preceding message describes the error in detail.

## NVI0311

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0311 INCORRECT VERSION OF MAGNETIC TAPE INITIALIZATION ROUTINE

### Meaning

The loaded magnetic tape initialization routine has an incorrect
version number.

### Response

Contact the system administrator.

## NVI0312

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0312 FLOPPY DISK INITIALIZATION ROUTINE COULD NOT BE LOADED

### Meaning

The loading of the floppy disk initialization routine by SPOOL has been
rejected.

### Response

Contact the system administrator.

## NVI0315

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0315 SUBSYSTEM 'SPOOL' DOES NOT EXIST. FLOPPY DISK INITIALIZATION ABORTED

### Response

Load subsystem SPOOL and repeat initialization request.

## NVI0316

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0316 ERROR WHEN ACCESSING THE INIT MODULE LIBRARY

### Meaning

An error occurred when DSSM attempted to access the INIT module
library.
Possible reasons :
- library does not exist
- library is read-protected
- incorrect version of the subsystem

### Response

Install INIT module library with correct version.
Library must not be read-protected.

## NVI0317

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0317 VOLUME CANNOT BE INITIALIZED

### Meaning

The operating system only permits read access to the volume.
Possible reason : magnetic tape cartridge and tape too short.

### Response

For further information see preceding messages on console or
HEL-file entries as far as issued.

## NVI0318

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0318 INIT > (&00)

### Meaning

An INIT information is issued.
(&00) : Self explaining, language-independent text

## NVI0319

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0319 Error during allocation of a device or volume: '(&00)'. Further information: /HELP-MSG (&01)

### Meaning

The allocation of a device or volume has been rejected.
The reason for the rejected allocation request is more precise explained
in additional information, gained from one of the called system functions.
The additional information is a message text of the called system
component. This text may be truncated, if it was too long to be inserted
into this message. This case is indicated by '...' at the end of the
additional information text.
If there are inserts in the additional information text, they are not
supplied!!
(&00): Additional information about the unsuccessful allocation request
(&01): Message id of the additional information

### Response

The measures to be taken are dependent on the additional information.

## NVI0320

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0320 NO DEVICE AVAILABLE FOR VOLUME-TYPE (&00)

### Meaning

No device is available for the requested volume type.
(&00): Requested volume type

### Response

Initialization of the requested volume type is not possible on this
installation.

## NVI0321

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0321 TEMPORARILY NO DEVICE AVAILABLE FOR VOLUME-TYPE (&00)

### Meaning

No device is available for the requested volume type at the moment.
(&00): Requested volume type

### Response

Repeat initialization request if a suitable device is available.

## NVI0322

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0322 DEVICE (&00) NOT AVAILABLE

### Meaning

The requested device is not available.
(&00): Device mnemonic (MN) of requested device

### Response

Use another device.

## NVI0323

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0323 DEVICE (&00) TEMPORARILY NOT AVAILABLE

### Meaning

The requested device is not available at the moment.
(&00): Device mnemonic (MN) of requested device.

### Response

Repeat initialization request if the device is free.

## NVI0324

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0324 NO VOLUME OF TYPE (&00) AVAILABLE

### Meaning

No volume of the requested volume type is available.
(&00): Requested volume type

### Response

Use another volume type.

## NVI0325

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0325 TEMPORARILY NO VOLUME OF TYPE (&00) AVAILABLE

### Meaning

No volume of the requested volume type is available at the moment.
(&00): Requested volume type

### Response

Repeat initialization request if a suitable volume is available.

## NVI0326

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0326 VOLUME WITH VSN (&00) NOT AVAILABLE

### Meaning

The requested volume is not available.
(&00): requested VSN

### Response

Use another volume (VSN).

## NVI0327

Destination: USER-TASK, CONSOLE Routing code: T Weight: 99

Warranty : NO

NVI0327 VOLUME WITH VSN (&00) TEMPORARILY NOT AVAILABLE

### Meaning

The requested volume is not available at the moment.
(&00): requested VSN

### Response

Repeat initialization request if the volume is free.

## NVI0328

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NVI0328 DEVICE CANCELLED (DAR permanently locked)

### Meaning

The access to the device used with this INIT run was inhibited by a
permanent locked device access right (DAR).
This may be caused by a tape library system after repeated occurrence
of device- or volume errors.

### Response

Find out the reason of potential device defects and repeat the
initialization request if the device is ready again.
Please notice the messages of the device error recovery (EXC0858,
NJTxxxx), of the device management (NKVTxxx) and of a tape library system,
that have probably been issued to the console and also possible messages
on a display of a tape library system.

## NVI0400

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0400 INVALID COMMAND

### Meaning

The entered INIT command does not begin with a valid operation
(e.g. INIT, LIST, OPTION, HELP).

### Response

Enter a valid command as described in the manual.

## NVI0401

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0401 VOLUME TYPE MISSING

### Meaning

The statement contains no information about the volume type.
The volume type is a mandatory operand.

### Response

Correct statement.

## NVI0402

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0402 THE OPERAND 'VSN' OR 'WTM' IS MISSING

### Meaning

The statement contains nether the oerand 'VSN' nor the operand 'WTM'.
One of these operands must be specified.

### Response

Correct statement.

## NVI0403

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0403 INVALID OPERAND '(&00)'

### Meaning

(&00) : Unknown or invalid operand in the statement, e.g.
- 'ERASE' with function LIST
- typing error 'VSB' instead of 'VSN'

### Response

Correct statement.

## NVI0404

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0404 INVALID CHARACTER '(&00)'

### Meaning

The character (&00) is not allowed for this statement.
Valid characters are :
A-Z , 0-9 , with OPTION DIN not set : #,$,@
for OWN additional : .(period),-(hyphen)

### Response

Use only the valid characters.

## NVI0405

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0405 INVALID OPERAND VALUE '(&00)'

### Meaning

(&00): 'xxx=xx', operand with invalid operand value.

### Response

Correct statement.

## NVI0406

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0406 '(&00)' PERMITTED IN BATCH MODE ONLY

### Meaning

(&00): OPTION CONS (or old format 'OPTION=($CONS)')
OPTION CONS is permitted in batch mode only, to enable the handling
of INIT in dialog mode via CONSOLE.

## NVI0407

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0407 Floppy Disk initialization no longer supported

### Meaning

Since BS2000 V13.0 (OSD V4.0) no floppy disk devices are supported.
Therefore INIT does'nt support floppy disk initialization any longer.

## NVI0408

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0408 ABBREVIATED KEYWORD '(&00)'IS AMBIGUOUS

### Meaning

(&00): ambiguous keyword as entered

### Response

Use unambiguous keyword.

## NVI0409

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NVI0409 ACTION "(&01)" IS NOT ALLOWED FOR VOLUME TYPE "(&00)"

### Meaning

The requested action (INIT / WTM / LIST) is not allowed with
volumes of type (&00).
Possible reasons:
- Action WTM is requested for a WORM-volume (Write Once, Read Many).
(&00): volume type
(&01): requested action

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages