## NSP0001

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP0001 MACHINE ERROR CODE X'(&00)' DURING SNAP, SNAP-ID: '(&01)'

### Meaning

(&01): SNAP-ID of SNAP caller.

### Response

Take SLED and reload system.

## NSP0002

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP0002 SNAP ERROR CODE '(&00)', SNAP-ID: '(&01)', '(&02)'

### Meaning

(&01): SNAP-ID of SNAP caller
(&02): Insert of SNAP caller, if it exists.

### Response

Take SLED and reload system.

## NSP1000

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP1000 SNAPFILE WRITTEN. SNAP-ID: '(&00)', '(&01)'

### Meaning

SNAP was called with SNAP-ID (&00) and insert (&01).
The file 'SNAPFILE' contains the SNAPSHOT dump.

## NSP1001

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP1001 SNAP ERROR. SNAP NOT WRITTEN. SNAP-ID: '(&00)', '(&01)'

### Meaning

During SNAP for SNAP ID (&00) an error occurred.
SNAP processing is aborted. The caller gets control with an error
return code.
No valid SNAPSHOT dump is in the SNAP file.
At /SHUTDOWN a message is displayed advising the operator to take a
SLED dump after /SHUTDOWN.
(&00): SNAP-ID of SNAP caller
(&01): Insert of SNAP caller, if existing.

### Response

After /SHUTDOWN the operator should take a SLED dump which should be
sent to the SNAP developers' department.

## NSP1002

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP1002 SNAPSHOT FUNCTION NOT AVAILABLE. SNAP-ID '(&00)' REJECTED

### Meaning

The SNAPSHOT function is not available on the running system.
(&00): SNAP-ID of SNAP caller.

### Response

See the manual SYSTEM OPERATOR'S GUIDE.

## NSP1010

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP1010 OUTPUT OF SNAPSHOT INCOMPLETE BECAUSE OF '(&02)'. SNAP ID: '(&00)'; '(&01)'

### Meaning

Because of '(&02)' it was impossible to save all data. The saved data are
not lost but will be processed.
(&00): SNAP-ID of SNAP caller
(&01): Insert of SNAP caller if exists
(&02): 1 = Lack of space (SNAPFILE too small)
2 = Lack of time (system parameter value SNAPTIME too small)
3 = I/O error
4 = Program error
5 = CCW error
6 = Conversion error
7 = Memory Management error

### Response

In case of lack of space: increase SNAPFILE size by means of
- command ACTIVATE-SNAPSHOT
- or product SIR
In case of lack of time : increase system parameter value SNAPTIME:
to maximum value (24 seconds), in case of less
These measures enable SNAPSHOT to save more diagnostic data in the
SNAPFILE.

## NSP2000

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP2000 SNAP FILE COPIED INTO FILE '(&00)'

### Meaning

SNAP File has been copied into file (&00).
The file name has been built as follows:
(&00) : $SYSSNAP.SNAP.<snap-id>.<date>.<time>,
<snap-id>: SNAP-ID of the SNAP caller,
<date> : YYYY.MM.DD date of SNAP call,
<time> : HH.MM.SS time of SNAP call.
File (&00) may be analyzed by means of DAMP.

## NSP2002

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP2002 SNAP FILE NOT YET COPIED

### Meaning

SHUTDOWN is in process. The copying of the SNAP file can no longer be
started by the SNAP task.

### Response

At next STARTUP the copying will be done if DRV is not activated.

## NSP2003

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP2003 SNAP FUNCTION ERROR DURING COPY INTO FILE '(&00)'

### Response

Analyze error logging file.

## NSP2005

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP2005 UNRECOVERABLE ERROR DURING COPY OF SNAPFILE CAUSED TERMINATION OF THE TASK SNAP('(&00)','(&01)')

### Meaning

During the copying of the file SNAPFILE an unrecoverable error has
occurred. Thus the task SNAP was terminated.

## NSP2007

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP2007 REQUESTED DISK SPACE FOR SNAP COPY FILE COULD NOT BE ALLOCATED. PLEASE CONTACT SYSTEM ADMINISTRATION FOR RECOVERY. REPLY (EOT = ACKNOWLEDGE)

### Meaning

Due to lack of disc space (DMS0541/DMS0546) the SNAP COPY FILE cannot
be allocated under userID SYSSNAP.
The SNAP dump function is deactivated.

### Response

After recovery of disc space by system administration the
SNAP dump function must be activeted again via command
ACTIVATE-SNAPSHOT.

## NSP2008

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP2008 REQUESTED DISK SPACE FOR SNAP FILES COULD NOT BE ALLOCATED. PLEASE CONTACT SYSTEM ADMINISTRATION FOR RECOVERY. REPLY (EOT = ACKNOWLEDGE)

### Meaning

Due to lack of disc space (DMS0541/DMS0546) the snapfiles cannot
be allocated under userID TSOS. Until recovery of disc space
SNAP dump function can not be activated.

### Response

Recovery of disc space by system administration.

## NSP3000

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3000 SNAP FILE '(&00)' NOT IN CATALOG. SNAPSHOT FUNCTION SUPPRESSED

### Meaning

File (&00) has not been created, despite option SNAPSHOT=ON.
Therefore, the SNAPSHOT function has been suppressed.

### Response

Generate the SNAP file by means of SIR.

## NSP3010

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3010 NO USABLE CATALOG FOR SNAP FILE '(&00)'. SNAPSHOT FUNCTION SUPPRESSED

### Meaning

There is no usable catalog for location of SNAP file (&00).
Therefore, the SNAPSHOT function has been suppressed.

## NSP3020

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3020 SNAP FILE '(&00)' NOT FOUND. DMS-RC '(&01)'. SNAPSHOT FUNCTION SUPPRESSED. /HELP DMS(&01),INF=D

### Meaning

An FSTAT call for file (&00) has been rejected by the DMS with
error code (&01).
Therefore, the SNAPSHOT function has been suppressed.
For more detailed information about the DMS error enter the /HELP command,
in system mode or see the manuals 'System Messages', 'DMS Disk Processing'
or 'DMS Tape Processing'.

### Response

Take appropriate actions, in accordance with DMS error code (&01).

## NSP3030

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3030 SNAP FILE '(&00)' NOT ON PUBLIC VOLUME. SNAPSHOT FUNCTION SUPPRESSED

### Response

Generate the SNAP file by means of SIR.

## NSP3040

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3040 SNAP FILE '(&00)' NOT CONTINUOUS. SNAPSHOT FUNCTION SUPPRESSED

### Response

Generate the SNAP file by means of SIR.

## NSP3050

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3050 SNAP FILE '(&00)' PASSWORD PROTECTED. SNAPSHOT FUNCTION SUPPRESSED

### Response

Reset password protection.

## NSP3060

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3060 SNAP FILE '(&00)' WRITE PROTECTED. SNAPSHOT FUNCTION SUPPRESSED

### Response

Reset write protection.

## NSP3070

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3070 SNAP FILE '(&00)' TOO SMALL. SNAPSHOT FUNCTION SUPPRESSED

### Meaning

The SNAP file (&00) is smaller than the class 1 memory.
Therefore, the SNAPSHOT function has been suppressed.

### Response

Erase file (&00) and generate a SNAP file by means of SIR.

## NSP3080

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3080 DISK WITH VSN '(&00)' FOR SNAP FILE '(&01)' NOT ONLINE. SNAPSHOT FUNCTION SUPPRESSED

## NSP3090

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3090 DISK WITH VSN '(&00)' FOR SNAP FILE '(&01)' NOT AVAILABLE. NSIAQIR-RC: '(&02)'. SNAPSHOT FUNCTION SUPPRESSED

### Meaning

The NSIAQIR call for disk (&00) containing file (&01) has been rejected
with error code (&02).

## NSP3091

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3091 DISK WITH VSN '(&00)' FOR FILE '(&01)' NOT SUPPORTED BY SNAPSHOT. SNAP FUNCTION SUPPRESSED

### Response

Generate SNAP file by means of SIR on a disk supported by SNAPSHOT.

## NSP3092

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3092 CPU HSI NOT SUPPORTED BY SNAPSHOT. SNAPSHOT FUNCTION SUPPRESSED

## NSP3100

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3100 OPEN ERROR FOR SNAP FILE '(&00)'. DMS-RC: '(&01)'. SNAPSHOT FUNCTION SUPPRESSED. /HELP DMS(&01),INF=D

### Meaning

For more detailed information about the DMS error enter the /HELP command,
in system mode or see the manuals 'System Messages', 'DMS Disk Processing'
or 'DMS Tape Processing'.

### Response

Analyze DMS error code (&01).

## NSP3110

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3110 WRITE ERROR FOR SNAP FILE '(&00)'. DMS-RC: '(&01)'. SNAPSHOT FUNCTION SUPPRESSED. /HELP DMS(&01),INF=D

### Meaning

For more detailed information about the DMS error enter the /HELP command,
in system mode or see the manuals 'System Messages', 'DMS Disk Processing'
or 'DMS Tape Processing'.

### Response

Analyze DMS error code (&01).

## NSP3120

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3120 CLOSE ERROR FOR SNAP FILE '(&00)'. DMS-RC: '(&01)'. SNAPSHOT FUNCTION SUPPRESSED. /HELP DMS(&01),INF=D

### Meaning

For more detailed information about the DMS error enter the /HELP command,
in system mode or see the manuals 'System Messages', 'DMS Disk Processing'
or 'DMS Tape Processing'.

### Response

Analyze DMS error code (&01).

## NSP3130

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3130 SNAP ERROR CODE '(&00)'. SNAPSHOT FUNCTION SUPPRESSED

### Meaning

Verification of SNAP file has been rejected with error code (&00).
Therefore, the SNAPSHOT function has been suppressed.

### Response

Analyze SNAP error code (&00).
&00: X'04' Last half page pointer of SNAP file differs from catalogue
entry

## NSP3131

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3131 SNAP ERROR CODE '(&00)' ON CREATING CHANNEL PROGRAM. SNAPSHOT FUNCTION SUPPRESSED

### Response

Analyze SNAP error code (&00).
&00: X'04' Function code incorrect
X'08' Invalid request of memory
X'14' Wrong function 'Get size of skeleton'
X'20' Wrong function 'Generate skeleton'

## NSP3140

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3140 ERROR ON CREATING SNAP TASK. $CREAT ERROR CODE: '(&00)'

### Meaning

The $CREAT call to create the SNAP task was rejected with $CREAT error
code (&00). If a SNAPSHOT dump has been written into the SNAP file,
it cannot be copied.

### Response

Analyze $CREAT error code (&00).

## NSP3141

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3141 BOURSE CREATION ERROR CODE '(&00)'. SNAP TASK TERMINATED

### Meaning

The $NCREBO call to built up the 'DMS READY' bourse interface between
SNAP task und DMS startup has been rejected with an error code (&00) and,
therefore the SNAP task has been terminated.

### Response

Analyze $NCREBO error code (&00).

## NSP3142

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3142 'NAME MANAGER' ERROR CODE '(&00)'. SNAP TASK TERMINATED

### Meaning

The NAME MANAGER call to save the 'DMS READY' bourse identification
for DMS startup has been rejected with error code (&00) and,
therefore the SNAP task has been terminated.

### Response

Analyze error code (&00).

## NSP3150

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3150 INFORMATION REQUEST HAS BEEN REJECTED WITH ERROR CODE '(&00)'. SNAPSHOT FUNCTION SUPPRESSED

### Meaning

A request for memory management to inform about the main memory size
and PPAT location supported by the system has been rejected with error
code (&00) and, therefore the SNAPSHOT function has been suppressed.

### Response

Analyze error code (&00).

## NSP3151

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3151 A RESIDENT MEMORY REQUEST HAS BEEN REJECTED. SNAPSHOT FUNCTION SUPPRESSED

### Meaning

A class 3 memory request has been rejected. There are no resident
work buffer for SNAPSHOT and, therefore the SNAPSHOT function has been
suppressed.

## NSP3152

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3152 TRANSLATION ERROR FOR ADDRESS X'(&00)'. SNAPSHOT FUNCTION SUPPRESSED

### Meaning

The translation of class 3 page address (&00) by means of $V2C has been
rejected with condition code and, therefore the SNAPSHOT function has
been suppressed.
(&00): Virtual page address.

## NSP3160

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

NSP3160 WRONG SNAP PARAMETER IN THE STARTUP PARAMETER FILE

### Meaning

The SNAP parameter 'SNAP-ACTIVE-SWITCH' in the parameter file is wrong.
Default value ON is used.

## NSP3161

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

NSP3161 ERROR (&00) WHEN CALLING THE STARTUP PARAMETER SERVICE

### Meaning

Startup parameter service returned RC=(&00). Please contact maintenance
if a STARTUP parameter file for SNAP is existing.
(&00): C'0000000C' = The datas has been truncated
C'00000010' = No (more) datas existing

## NSP3170

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

NSP3170 DURING COPY OF SNAPFILE ONE (OR MORE) FRAME WAS DETECTED TO BE ASSIGNED BOTH TO CL1/CL3 AND CL4 MEMORY. ASSIGNMENT IS MADE TO CL1/CL3 MEMORY

### Meaning

There are two bitmaps, one for CL1/CL3 memory the other for CL4 memory.
One (or more) frame is marked in both bitmaps.

### Response

NONE.

## NSP3180

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP3180 OPERATION NAME SHOW-SNAPSHOT-STATUS NOT PERMITTED WITH THE CURRENT PRIVILEGES

### Meaning

Current privileges do not permit operation SHOW-SNAPSHOT-STATUS.

## NSP3181

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NSP3181 (&00) ERROR. RETURNCODE : (&01)

## NSP4000

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NSP4000 FUNCTION '(&00)' STARTED FOR SNAP DUMP FUNCTION

### Meaning

(&00): Function ACTIVATE or DEACTIVATE

### Response

NONE.

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages