## GCFCOPY

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

GCFCOPY Copyright (C) (&01) (&00). All rights reserved

## GCF0001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

GCF0001 PARAMETER ERROR WHEN CALLING AN INTERNAL INTERFACE. SERSLOG ENTRY CREATED. CONTACT SYSTEM ADMINISTRATOR

### Meaning

An internal interface has been called with an invalid parameter list.
For a more detailed diagnosis an entry has been written into
the SERSLOG file.

### Response

The system administrator should analyze the SERSLOG entries GCF0001
and GCF0002.

## GCF0002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

GCF0002 INTERNAL ERROR. SERSLOG ENTRY CREATED. CONTACT SYSTEM ADMINISTRATOR

### Meaning

For a more detailed diagnosis an entry has been written into
the SERSLOG file.

### Response

The system administrator should analyze the SERSLOG entries GCF0001
and GCF0002.

## GCF1000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

GCF1000 INVALID VALUE FOR OPERAND '(&00)'. COMMAND REJECTED

### Meaning

The specified operand value does not lie in the permitted range.

### Response

Repeat the command or job using a valid operand value.

## GCF1001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

GCF1001 INTERNAL ERROR. SERSLOG ENTRY CREATED. CONTACT THE SYSTEM ADMINISTRATOR

### Meaning

An entry has been written in the SERSLOG file in order to enable
a more precise diagnosis of the error.
The function is not performed.

### Response

The system administrator should analyze SERSLOG entries GCF0001
and GCF0002.

## GCF1002

Destination: USER-TASK Routing code: Weight:

Warranty : NO

GCF1002 NO OPEN CATALOGS

## GCF1003

Destination: USER-TASK Routing code: Weight:

Warranty : NO

GCF1003 NO ACTIVE SERVER TASKS

## GCF1014

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

GCF1014 USER NOT AUTHORIZED TO PERFORM FUNCTION

## GCF1020

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

GCF1020 NO MEMORY AVAILABLE. FUNCTION NOT PROCESSED

### Meaning

All the available system memory space has been used up.

### Response

Contact the system administrator or reenter the command later.

## GCF1038

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

GCF1038 CATALOG '(&00)' LOCKED BY ARCHIVE. RETRY FUNCTION LATER

### Meaning

The catalog cannot be updated at the moment.

## GCF6000

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

GCF6000 CATALOG '(&00)' OPENED

## GCF6001

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

GCF6001 NEW CATALOG '(&00)' CREATED

## GCF6005

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

GCF6005 CATALOG '(&00)' CLOSED

## GCF6007

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

GCF6007 ERROR '(&00)' DURING INITIALIZATION OF SUBSYSTEM GCF. FUNCTION NOT PROCESSED

### Meaning

The source of the error can be identified by means of the error
class, and a precise description can be found in the corresponding
SERSLOG entry.
(&00): Error class.
01: Error when assigning the task lock ($CRELOCK interface).
02: Error when making the subsystem known to task management
($TERMRF interface).
03: Error when reading the catalog ID of the HOME pubset
($STAM interface).
04: Memory shortage.

## GCF6008

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

GCF6008 GCF: INTERNAL ERROR '(&00)' REPORTED FROM '(&01)'

### Meaning

An entry is written to the SERSLOG file for exact diagnosis.
If "error intolerance" was set, a diagnostic dump is offered.
(&00): brief designation of the relevant error.
(&01): function affected.

### Response

Contact the system administrator or diagnostics staff.

## GCF6009

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

GCF6009 ERROR WHEN CLOSING CATALOG OF TYPE NUMBER '(&00)' ON PUBSET '(&01)'

## GCF6011

Destination: CONSOLE Routing code: R Weight: 90

Warranty : NO

GCF6011 ERROR '(&00)' DURING START OF SERVER TASK '(&01)' OF SUBSYSTEM GCF

### Meaning

(&00): Error class.
01: Memory shortage.
02: Error when requesting the next free TSN GC** (interface $TSNNFR).
03: Error when creating the server task (interface $CREA).
04: Error when connecting to the server task via FITC
(interface CONNECT).
05: Error when enabling special privileged access to a pubset
(interface $DMSSTP).
06: Error when setting a privilege for the server task
(interface $SETPRV).
07: Error when creating an ISAM pool for the server task
(interface CREPOOL).
08: Error when assigning a link name to the ISAM pool of the
server task (interface ADDPLNK).
09: Error when setting up a FITC port (interface DEFPORT).
0A: Error when making a recovery routine known to task management
(interface $ENER).
(&01): TSN of the server task.

## GCF6012

Destination: CONSOLE Routing code: R Weight: 90

Warranty : NO

GCF6012 ERROR DURING TERMINATION OF SERVER TASK '(&00)' OF SUBSYSTEM GCF

### Meaning

An entry was written into the SERSLOG file for a more detailed diagnosis.
(&00): TSN of the server task.

## GCF6013

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

GCF6013 MANAGEMENT OF ALL CATALOGS IN SERVER TASK '(&00)' TERMINATED DUE TO AN ERROR

### Meaning

(&00): TSN of the server task.

### Response

Enter a /CHANGE-...-CATALOG for everyone of the catalogs or
enter an /EXPORT-PUBLIC-VOLUME-SET command, followed by
an /IMPORT-PUBLIC-VOLUME-SET command.

## GCF6666

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

GCF6666 '(&00)'

### Meaning

This message is displayed only when a diagnostic REP has been
activated.

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages