## BLP0002

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0002 DBL INTERNAL ERROR. PROCESSING ABORTED WITH DUMP

### Response

Contact the system administrator.

## BLP0003

Destination: CONSOLE Routing code: P Weight: 99

Warranty : NO

BLP0003 STARTUP ABORTED DUE TO INSUFFICIENT MEMORY OR SYSTEM ERROR

### Meaning

DBL cannot generate its global tables.

## BLP0004

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLP0004 DBL ERROR IN SYMBOLIC NAME PROCESSING. STARTUP ABORTED

### Meaning

A data element processed by DM (DBL data manager) is inconsistent.

## BLP0005

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0005 ERROR IN DBL CONTEXT VECTOR MANAGER. PROCESSING ABORTED WITH DUMP

### Meaning

An internal inconsistency has been detected in the context
vector manager.

### Response

Contact the system administrator.

## BLP0006

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0006 INTERNAL ERROR IN DBL MEMORY MANAGER. PROCESSING ABORTED WITH DUMP

### Meaning

An internal error is detected in the memory manager.

### Response

Contact the system administrator.

## BLP0007

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0007 ERROR DURING EXTERNAL SYSTEM CALL. PROCESSING ABORTED WITH DUMP

### Meaning

An external system call has returned an error to DBL.
The possible external calls are:
$GETMEM, REQMP, ENAMP,
$RETMEM, RELMP, $CSTAT, $NVYMPA
$NVYMPA, RDTFT, $CHKPRV, $SANC, $TANC.

### Response

Contact the system administrator.

## BLP0008

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0008 INTERNAL ERROR IN DBL INTERFACE HANDLER. PROCESSING ABORTED WITH DUMP

### Meaning

An internal error is detected in the interface handler.

### Response

Contact the system administrator.

## BLP0009

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0009 INTERNAL ERROR IN DBL DATA MANAGER. PROCESSING ABORTED WITH DUMP

### Meaning

An internal error is detected in the data manager.

### Response

Contact the system administrator.

## BLP0010

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0010 INTERNAL ERROR IN DBL DATA STRUCTURE MANAGER. PROCESSING ABORTED WITH DUMP

### Meaning

An internal error is detected in the data structure manager.
Possible reason: privileged memory area managed by DBL
has been overwritten.

### Response

Contact the system administrator.

## BLP0011

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0011 INTERNAL ERROR IN DBL BASIC INPUT MANAGER. PROCESSING ABORTED WITH DUMP

### Meaning

An internal error is detected in the basic input manager.

### Response

Contact the system administrator.

## BLP0012

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0012 INTERNAL ERROR IN DBL LINK-LOAD PROCESSOR. PROCESSING ABORTED WITH DUMP

### Meaning

An internal error is detected by the linking-loading processor.

### Response

Contact the system administrator.

## BLP0013

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0013 INTERNAL ERROR IN DBL ERROR HANDLER (ERROR-ID=(&00))

### Meaning

An internal error is detected by the DBL error handler:
the message corresponding to the given ERROR-ID (&00)
is not defined in the DBL message table.

### Response

Contact the system administrator.

## BLP0014

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0014 ERROR IN DBL SHARE PROCESSOR. PROCESSING ABORTED WITH DUMP

### Meaning

An internal error is detected by the SHARE processor.

### Response

Contact the system administrator.

## BLP0015

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLP0015 LIBRARY ERROR DURING LDSLICE PROCESSING

### Meaning

A call to PLAM during LDSLICE processing has failed.

## BLP0016

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0016 ERROR IN DBL POSIX-PROGRAM STARTER. PROCESSING ABORTED

### Meaning

An internal error has been detected by the POSIX-program starter.

### Response

Contact the system administrator.

## BLP0020

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLP0020 $GETMEM ERROR. TASK ABORTED WITH SYSTEM DUMP

### Meaning

The requested memory space could not be allocated.
Possible reason: system memory saturation at this moment.

### Response

Contact the system administrator or retry later.

## BLP0021

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLP0021 $RETMEM ERROR. TASK ABORTED WITH SYSTEM DUMP

### Meaning

The requested memory space could not be released.
Possible reason : system error.

### Response

Contact the system administrator.

## BLP0034

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0034 ERROR IN OBJECT MODULE '(&00)'. LOADING ABORTED WITH DUMP

### Meaning

An inconsistency in the input object module (&00) has been detected.
module name=C'?': no valid ESD-record in current module.

## BLP0035

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0035 ERROR '(&00)' IN DBL INTERNAL MEMORY MANAGEMENT. PROCESSING ABORTED

### Meaning

(&00): DBL memory management error code :
- '0B040188': invalid load address specified
- '0C080194': validation error, i.e. user has released or
changed
status of a class 6 memory page belonging to DBL.
- '0A0C0198': discrepancy error during allocation of vector
address space.
- '0B0C0198': saturation of vector address space.
- '0C0C0198': module too big or not enough space.
A dump is taken for diagnosis only in case of
error codes x'0B040188' and x'0C080194'.

### Response

Correct the program according to the return code
and try again.

## BLP0040

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0040 ERROR WHEN LOADING SYMBOLIC INFORMATION. LOADING ABORTED WITH DUMP

### Response

Correct object module.

## BLP0041

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0041 LSDA RECORD ERROR IN MODULE '(&00)'. LOADING ABORTED WITH DUMP

### Meaning

(&00): Module name.

### Response

Correct object module.

## BLP0053

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0053 ERROR IN CSECT '(&00)'. SYMBOLIC INFORMATION ABOUT CSECT IN MODULE '(&01)' NOT LOADED. DUMP TAKEN

### Meaning

(&00): CSECT name.
(&01): Module name.

### Response

Recreate object module.

## BLP0054

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0054 LOAD OF SYMBOLIC INFORMATION CONTINUES

### Meaning

Additional message to the preceding one.

## BLP0055

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0055 COMPILER OR LIBRARY ERROR. INVALID SYMBOLIC INFORMATION RECORD TYPE IN CSECT '(&00)' IN MODULE '(&01)'. DUMP TAKEN

### Meaning

(&00): CSECT name.
(&01): Module name.

### Response

Contact the system administrator.

## BLP0060

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0060 RESIDENCY OF (&00) '(&01)' INVALID IN THIS ENVIRONMENT. LOADING ABORTED

### Meaning

(&00): MODULE or COMMON.
(&01): name of the module or of the common.
Possible reasons for a MODULE:
1. The computed PSEUDO-RMODE of the module is 24 and the load unit
is loaded in the privileged memory.
2. The computed PSEUDO-RMODE of the module is 24 and the load unit
is loaded in a memory pool which is located above the 16 MB limit.
(How the PSEUDO-RMODE of a module is computed is explained in the
BS2000 "Dynamic Binder Loader / Starter" manual).
Possible reasons for a COMMON:
1. The COMMON is to be loaded below the 16 MB limit and the load unit
is loaded in a memory pool which is located above the 16 MB limit.
The COMMON is to be loaded below this limit because:
- its RMODE is 24 or
- the load unit PROGMODE is 24 or
- at least one MODULE of the load unit is loaded below the
16 MB limit.
2. The COMMON was already loaded in the same context (in a previous
load unit ) above the 16 MB limit and is to be loaded in the current
load unit below the 16 MB limit.
3. The COMMON is to be loaded below the 16 MB limit and the load
unit is to be loaded in the privileged memory.

### Response

Correct the program or module.

## BLP0061

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0061 AMODE OF SYMBOL '(&00)' INVALID IN THIS ENVIRONMENT. LOADING ABORTED

### Meaning

The load unit contains a symbol (CSECT, COMMON or ENTRY) (&00)
with AMODE=31. Either the system is not an XS one or
PROG-MOD=24 was specified or the loading concerns a privileged
sub-system.

### Response

Change the AMODE value (24 or ANY).

## BLP0100

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0100 NOT ENOUGH MEMORY. PROCESSING ABORTED

### Meaning

DBL receives the return code NOT ENOUGH MEMORY from the system
memory management. A memory class is saturated either by the program
code or the areas requested by the user or by the system
metadata in the privileged memory.
The saturation is often due to too big an amount of symbolic
information generated via the TEST-OPTIONS=AID or IDA parameter of the
command /START-PROGRAM or /LOAD-PROGRAM and the BIND macro.

### Response

Contact the system administrator for the saturation analysis (possibly
reduce the amount of symbolic information and try again).

## BLP0101

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0101 ERROR DURING VALIDATION OF CLASS 6 MEMORY BLOCK

### Meaning

The validation error occurs either
- if the user has released or changed status
of a class 6 memory block belonging to DBL or
- if the LLM to be loaded contains an empty slice or
- if the reference towards the server inside the user provided
indirection routine is only read accessible.

### Response

Correct the program and try again.

## BLP0102

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0102 SPECIFIED LOAD ADDRESS CAN NOT BE USED. PROCESSING ABORTED

### Meaning

1. The load address specified in the BIND call cannot be used.
The possible reasons are:
A. The address lies in a page previously requested and
OVERLAY=N is specified.
B. The address is not a class 6 address.
C. The address does not match the minimum alignment required by
the first module of the load unit (e.g. the address is not
page aligned and the first CSECT of the first module has the
attribute PAGE).
D. It is not allowed to load a LLM if a load address is specified
in the BIND call.
2. A not relocatable LLM cannot be loaded at the address specified
in the LLM, because the memory area in which the LLM should be
placed is not free.

### Response

Correct program and try again.

## BLP0104

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0104 LLM '(&00)' CANNOT BE LOADED. REASON '(&01)'. PROCESSING ABORTED

### Meaning

DBL cannot load LLM for reason (&01) :
- '01' : The LLM can only be loaded on a higher BS2000/OSD resp.
- BLSSERV version or it has an invalid LLM-Format.
- '02' : LLM sliced "BY-USER" cannot be loaded in POSIX environment.
- '03' : Only 1 LLM sliced "BY-USER" can be loaded at a time in a given
context and there already exists one.
- '04' : LLM cannot be loaded in standard RUN MODE.
- '05' : LLM is not compatible with the pre-loading feature.
- '06' : LLM not loadable. Such a LLM can only be processed by BINDER
and LLMAM.
- '07' : LLM with CSECT AMODE=31 cannot be loaded in a unit loaded with
PROG-MOD=24.
- '08' : System options do not allow to load a LLM in standard RUN MODE.

### Response

Correct the LLM.

## BLP0105

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLP0105 CONNECTION TO MEMORY POOL '(&00)' WITH SCOPE '(&01)' IS NOT POSSIBLE. PROCESSING ABORTED

### Meaning

A memory pool which holds "user shared code" referenced by the
current load unit cannot be enabled by the task because the
memory block used by the memory pool is not free.

### Response

Ensure that memory block(s) occupied by memory pool(s) holding
"user shared code" are free.

## BLP0136

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

BLP0136 FUNKTION SCHON VERARBEITET

### Meaning

Die gewuenschte Funktion wurde schon frueher verarbeitet.

## BLP0139

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0139 (&00) '(&01)' IN (&02) '(&03)' IS DUPLICATE. PROCESSING ABORTED

### Meaning

A name collision is detected inside a context and the user has
specified NAME-COLLISION=ABORT.
(&00): 'ENTRY', 'COMMON' or 'CSECT'.
(&01): ENTRY, COMMON or CSECT name.
(&02): 'MODULE' or 'LLM'.
(&03): Module or LLM name.

### Response

Erase the name collision or make the symbol invisible in the specified
module or specify NAME-COLLISION=STD.

## BLP0140

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0140 WRONG '(&00)' RECORD TYPE IN MODULE '(&01)'. LOADING ABORTED WITH DUMP

### Meaning

(&00): Invalid record type.
(&01): Module name.

### Response

Compiler or library error.
Compile and try again.

## BLP0142

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0142 TYPE CODE '(&00)' IN ESD RECORD IN MODULE '(&01)' INCORRECT. LOADING ABORTED

### Meaning

(&00): Invalid type code.
(&01): Module name.
For the meaning of type code see the manual "System conventions".

### Response

Compile and try again.

## BLP0150

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0150 BLS-WARNING DURING LOADING

### Meaning

A warning has been issued by BLS during the loading.

## BLP0151

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0151 USER IS NOT AUTHORIZED TO ISSUE THIS COMMAND. COMMAND REJECTED

### Meaning

The command is rejected according to the task privileges.

## BLP0152

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0152 SYSTEM ERROR DURING LOADING. COMMAND NOT EXECUTED

### Meaning

A system error has been detected by BLS during loading.

## BLP0153

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0153 UNRECOVERABLE ERROR DURING LOADING. COMMAND NOT EXECUTED

### Meaning

An unrecoverable error has been detected by BLS during loading.

## BLP0160

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0160 COMMAND INPUT RESERVED FOR THE ADMINISTRATOR ONLY

### Meaning

Only the system administrator may enter an
/ADD-SHARED-PROGRAM command.

## BLP0162

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0162 PRODUCT NAME '(&00)' ALREADY IN SHARE TABLE. CMD NOT PROCESSED

### Meaning

The current product name (&00) already exists in the share table.
The command /ADD-SHARED-PROGRAM is rejected.

## BLP0163

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0163 INVALID OPERAND. CORRECT COMMAND

### Meaning

The format of the command /ADD-SHARED-PROGRAM is invalid
The command is not processed.

### Response

Correct rejected command and try again.

## BLP0165

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0165 INVALID FILENAME. COMMAND REJECTED

### Meaning

Invalid file name in the command /ADD-SHARED-PROGRAM.
The specified CATID is not local.

### Response

Repeat command with correct operand.

## BLP0166

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0166 ### SPECIFIED RESOLUTION SCOPE NOT PROCESSED BY DSSM

### Meaning

DBL receives a return code from "Select Subsystem Version"
function of DSSM.
The DSSM version is not correct (function not yet supported).

### Response

Retry with correct version of DSSM.

## BLP0167

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0167 ### PRODUCT '(&00)' NOT FOUND IN '(&01)' SCOPE TABLE. COMMAND NOT PROCESSED

### Meaning

The deletion of the product '&00' is not performed because
this product cannot be found in the given product table ('&01').
'&00': product name
'&01': table scope

## BLP0168

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0168 ### NO MEMORY AVAILABLE FOR PRODUCT TABLE. COMMAND NOT PROCESSED

### Meaning

The product entry cannot be created because no memory
can be requested for the product table.

## BLP0170

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0170 OPTION '(&00)' MAY NOT BE SPECIFIED IN COMBINATION WITH "OPTION-PRIORITY=FORCED". COMMAND NOT PROCESSED

### Meaning

An invalid option (&00) has been specified together with
OPTION-PRIORITY=FORCED.
(&00): LIBRARY
PROGRAM-VERSION
CONTEXT
CONTEXT-STATE

### Response

Correct rejected command and try again.

## BLP0171

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0171 INVALID CONTEXT NAME '(&00)' SPECIFIED. COMMAND NOT PROCESSED

### Meaning

The context name must begin with a letter.
(&00): Given context name

### Response

Correct the context name and try again.

## BLP0230

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0230 INVALID FORMAT IN STATEMENT '(&00)(&01)'. CONTINUE PROCESSING? REPLY (Y=YES; N=NO)

### Meaning

Message only for dialog process.
(&00): first part of REP or INCLUDE statement.
(&01): second part of REP or INCLUDE statement.

### Response

Enter appropriate reply.

## BLP0231

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0231 ### INVALID FORMAT IN STATEMENT '(&00)(&01)'. PROCESSING CONTINUES

### Meaning

Message only for batch process.
(&00): first part of REP or INCLUDE statement
(&01): second part of REP or INCLUDE statement.

## BLP0232

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0232 MODULE '(&00)' NOT IN THE LIBRARY. CONTINUE PROCESSING? REPLY (Y=YES; N=NO)

### Meaning

(&00): Module name.

### Response

Enter appropriate reply.

## BLP0233

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0233 ### MODULE '(&00)' NOT IN THE LIBRARY. PROCESSING CONTINUES

### Meaning

Message only for batch process.
(&00): module name.

## BLP0234

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

BLP0234 MODULE '(&00)' NOT IN CURRENT LOAD UNIT. REP STATEMENT IGNORED. CONTINUE PROCESSING? REPLY (Y=YES; N=NO)

### Meaning

(&00): module name.

### Response

Enter appropriate reply.

## BLP0235

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0235 ### MODULE '(&00)' NOT IN CURRENT LOAD UNIT. REP STATEMENT IGNORED. PROCESSING CONTINUES

### Meaning

Message only for batch process.
(&00): The module name which appears on the REP card.

## BLP0310

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0310 ERROR DURING MAP OUTPUT. SYSOUT MAP GENERATION ABORTED

### Meaning

The YTIEWOUT call returns an error. The map generation on SYSOUT
cannot be continued.

## BLP0311

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0311 WRLST ERROR DURING MAP OUTPUT. SYSLST MAP GENERATION ABORTED

### Meaning

The WRLST call returns an error. The SYSLST map generation cannot
be continued.

## BLP0330

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0330 ### INVALID RECORD '(&00)' IN MODULE '(&01)' IGNORED. PROCESSING CONTINUES

### Meaning

Error in object module.
(&00): Invalid record number.
(&01): Module name.

### Response

Compile and try again.

## BLP0331

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0331 ### CSECT '(&00)' ALREADY LOADED. CURRENT MODULE '(&01)' IGNORED

### Meaning

Duplicate CSECT names are not allowed in standard RUN MODE.
(&00): CSECT name.
(&01): Module name.

## BLP0332

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0332 ERROR DETECTED WHILE LOADING ELEMENT '(&00)', VERSION '(&01)' FROM LIBRARY '(&02)'. LOADING ABORTED

### Meaning

An error is detected while loading LLM (&00) with version (&01)
from library (&02). The private part of this BY-ATTRIBUTE
PRIVATE/PUBLIC LLM refers to a non-visible symbol of the public
part. The loading of the current load unit is aborted.

### Response

Make the related symbol visible or suppress the reference.

## BLP0333

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0333 RESOLUTION BETWEEN PRIVATE AND PUBLIC SLICES OF LLM '(&00)' FAILED. LOADING ABORTED

### Meaning

The resolution of the references from the PRIVATE to the PUBLIC slices
of the LLM (&00) has failed.
Possible reasons :
- A reference could not be solved because of programming mode
incompatibility.
- A reference could not be solved because no corresponding definition was
found.

### Response

Please contact the responsible for loading the LLM PUBLIC slices
to adapt the programming mode(s) or to correct the LLM.

## BLP0334

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0334 SYMBOL '(&00)' CANNOT BE FOUND. LOADING ABORTED

### Meaning

The symbol specified in the command
/START-PROGRAM or /LOAD-PROGRAM or in MEXEC-MLOAD-LINK-BIND
cannot be found in the assigned library(ies).

### Response

Correct the symbol name and try again.

## BLP0335

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0335 UNRESOLVED EXTERNAL REFERENCES '(&00)'

### Meaning

The specified EXTRN or VCON symbol(s) (&00) cannot be found in any
library. In batch process loading will be processed as far as possible.
In dialog process it can be decided in the following message (BLP0336)
whether loading should be continued or not.

## BLP0336

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLP0336 CONTINUE PROCESSING? REPLY (Y=YES; N=NO)

### Meaning

External references specified in the BLP0335 message cannot be
found in any library.

### Response

Enter appropriate reply.

## BLP0337

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0337 ### DUPLICATE SYMBOL '(&00)' SPECIFIED IN TABLE MACRO. PROCESSING CONTINUES

### Meaning

The user specifies a symbol (&00) which is already known in the
BLS tables. BLS accepts this duplicate symbol but some problems
could arise later.

## BLP0338

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0338 ### ATTRIBUTE (&00) OF CSECT '(&01)' IN MODULE '(&02)' IGNORED

### Meaning

Due to some internal consistency rules or to some system limitation
DBL cannot take account of the attribute (&00) of the CSECT (&01)
in module (&02). Nevertheless, this module is loaded.

## BLP0339

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0339 ### (&00) '(&01)' IN (&02) '(&03)' IS DUPLICATE

### Meaning

A name collision is detected in the context.
The processing continues.
(&00): ENTRY, COMMON or CSECT.
(&01): ENTRY, COMMON or CSECT name.
(&02): MODULE or LLM.
(&03): Module or LLM name.

## BLP0340

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0340 UNRESOLVED EXTERNAL REFERENCES

### Meaning

The list of the unresolved external references follows in the
message BLP0342.
In interactive mode the list is followed by the message BLP0350
which asks the user if he wants to continue the link-load
processing or not.
In batch mode the processing continues.
This message concerns the unresolved EXTRNs and V-CONs only
(the unresolved WXTRNs are not shown and the unresolved
XDSEC-References follow in the message BLP0341).

## BLP0341

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0341 UNRESOLVED XDSEC REFERENCES

### Meaning

The list of the unresolved XDSEC references follows in the message
BLP0342.
In interactive mode the list is followed by the message BLP0350
which asks the user if he wants to continue the link-load
processing or not.
In batch mode, the processing continues.

## BLP0342

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0342 ### '(&00)'

### Meaning

(&00) is a list of up to 7 unresolved symbol names.
The message BLP0342 follows the message BLP0340 or the
message BLP0341.

## BLP0343

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

BLP0343 RELOCATION TRUNCATED. PROCESSING CONTINUES

### Meaning

At least one address resulting from the computation of a relocation
has been truncated.

## BLP0344

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLP0344 ADDRESS IN A MIPS INSTRUCTION OUTSIDE THE CURRENT SEGMENT. PROCESSING ABORTED

### Meaning

The resulting address of a relocation computation, for a "JUMP" or
"JUMP and LINK" instruction, is outside the current segment :
this is forbidden for such instructions.

### Response

- Instead of "direct JUMP" instructions, use the corresponding "register"
instructions, or
- load the symbol referenced by the "JUMP" instruction in the same segment
as the instruction itself.

## BLP0345

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0345 SYMBOL '(&00)' ALREADY IN LINK CONTEXT. LOADING ABORTED

### Meaning

As the specified symbol is already loaded in the link context, a new
loading of this symbol is rejected, in order to avoid duplicate symbols
in a same context.

## BLP0346

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

BLP0346 INCOMPATIBILITY BETWEEN SERVER HSI CODE AND ILE HSI CODE

### Meaning

In the current load unit, a symbol usable as server of ILE has an HSI
code which doesn't match the HSI code of the corresponding ILE

## BLP0347

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

BLP0347 EOLDTAB IS FULL. PROCESSING CONTINUES

### Meaning

No additional CSECT or ENTRY can be added in EOLDTAB.

## BLP0348

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

BLP0348 SYMBOL '(&00)' NOT YET INITIALIZED IN "SHARED CODE" FOR THE CURRENT TASK

### Meaning

Symbol (&00) belongs to a subsystem not yet initialized for the current
task.

### Response

Make /LOGOFF followed by /SET-LOGON-PARAMETERS in order to initialize
the subsystem for a new task and retry in this task.

## BLP0349

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

BLP0349 THE COMMAND MODIFY-DBL-OPTIONS IST ONLY SUPPORTED UP TO VERSION V12.0Q AND V12.1P

### Meaning

The command is replaced by the MODIFY-DBL-PARAMETERS one.

## BLP0350

Destination: USER-TASK Routing code: Weight: 90

Warranty : NO

BLP0350 CONTINUE LINK-LOAD PROCESSING ? REPLY (Y=YES; N=NO)

### Meaning

This message is issued in interactive mode and asks the user if he
wants to continue the link-load processing after DBL has detected
an event explained in the previous message.
If the reply is Y, the processing continues.
If the reply is N, the processing is aborted, i.e. nothing is loaded.

## BLP0405

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLP0405 UNRECOVERABLE ERROR DURING MESSAGE OUTPUT BY MSG7-MACRO. PROCESSING CONTINUES

## BLP0420

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0420 ERROR WHEN OPENING EAM FILE (*- OR OMF FILE). LOADING ABORTED

## BLP0421

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0421 EAM FILE (*- OR OMF FILE) DOES NOT EXIST. LOADING ABORTED

## BLP0422

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0422 NON-PRIVILEGED PROGRAM NOT ALLOWED TO ACCESS PRIVILEGED EAM FILE (*- OR OMF-FILE). LOADING ABORTED

## BLP0424

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0424 I/O-ERROR WHEN READING EAM FILE (*- OR OMF-FILE). LOADING ABORTED

## BLP0425

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0425 ERROR WHEN CLOSING EAM FILE (*- OR OMF-FILE). PROCESSING CONTINUES

### Response

Contact the system administrator.

## BLP0450

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0450 ERROR WHEN ACCESSING FILE '(&00)'

### Meaning

(&00): Filename.
Error description in the next message.

## BLP0451

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0451 I/O ERROR WHEN ACCESSING OBJECT MODULE LIBRARY. DMS ERROR '(&00)'. IN SYSTEM MODE /HELP-MSG DMS(&00)

### Meaning

For more detailed information about DMS error code enter
/HELP-MSG in system mode or see the DMS manual.

## BLP0452

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0452 FILE IS NOT A VALID LIBRARY

### Meaning

The specified file is neither a program library (PL) nor
an object module library (OML).

### Response

Specify an object module library or a program library.

## BLP0453

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0453 SIZE FIELD ERROR IN OML DIRECTORY

### Response

Send an error message to diagnosis.

## BLP0454

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0454 READ ERROR ON LIBRARY '(&00)'. PROCESSING ABORTED

### Meaning

A read error has occurred on the specified library (&00).
The current linking-loading processing cannot be
continued.

## BLP0456

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0456 ERROR WHILE ACCESSING FILE '(&00)'. DMS ERROR CODE '(&01)'. USE /HELP-MSG DMS(&01)

### Meaning

(&00): Filename.
(&01): DMS error code.
For more detailed information about the DMS error code enter
/HELP-MSG DMS(&01) in system mode or see the DMS manual.

## BLP0457

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0457 EXTERNAL REFERENCE '(&00)' CANNOT BE RESOLVED. MODULE NAME IN LIBRARY '(&01)' TOO LONG

### Meaning

(&00): ENTRY name.
(&01): Filename.
A module containing the ENTRY (&00) has a name longer than
8 characters (RUN-MODE=STD) or 32 characters (RUN-MODE=ADV).

### Response

Use module names shorter or equal to 8 characters (RUN-MODE=STD)
or 32 characters (RUN-MODE=ADV).

## BLP0460

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

BLP0460 LOCK ERROR ON ELEMENT '(&00)' OF LIBRARY '(&01)'. PLAM ERROR CODE '(&02)'. IN SYSTEM MODE /HELP-MSG PLA(&02)

### Meaning

The element '(&00)' of the program library '(&01)'
can not be processed because it is currently locked
(PLAM return code '(&02)').
For more detailed information about PLAM return code
enter /HELP-MSG PLA(&02) in system mode.

### Response

Retry later.

## BLP0461

Destination: USER-TASK Routing code: Weight: 98

Warranty : YES

BLP0461 FILE '(&00)' IS LOCKED. DO YOU WANT TO RETRY ? REPLY (Y=YES, N=NO)

### Meaning

The specified file is currently locked (the DMS error code '0D99' is
received).
Reply = Y : DBL retries to open the file.
If the retry is not successful, the message is sent again
with a maximum of 10 attempts. If the last attempt fails,
the processing is aborted with a further error message.
Reply = N : no retry is performed. The processing is aborted with a
further error message.

### Response

Unlock the file, if it is possible, before the reply "Y".

## BLP0462

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0462 FILE '(&00)' IS LOCKED. RETRY IN PROGRESS

### Meaning

The specified file is currently locked (the DMS error code '0D99' is
received).
The message is sent only in batch mode. DBL retries to open the file;
up to 10 attempts are performed with a waiting time of 20 seconds.
If the last attempt fails, the processing is aborted with a further
error message.

## BLP0464

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0464 PLAM IS NOT AVAILABLE. LOADING ABORTED

### Meaning

PLAM is not linked to the operating system.

### Response

Contact the system administrator.

## BLP0467

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0467 ERROR WHEN ACCESSING FILE '(&00)'. PLAM AMCB ERROR CODE '(&01)'. IN SYSTEM MODE /HELP-MSG PLA(&01)

### Meaning

(&00): Filename.
(&01): PLAM return code.
For more detailed information about PLAM return code
enter /HELP-MSG PLA(&01) in system mode.

### Response

Retry later.

## BLP0468

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0468 SYSTEM SERVICE ERROR CODE '(&00)'

### Meaning

(&00): System service error code (PLAM output).
(Continuation of message BLP0467).

## BLP0469

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0469 LINK NAME '(&00)' NOT FOUND. PROCESSING ABORTED

### Meaning

The specified link name '(&00)' does not exist.

### Response

Correct the link name or assign another one and try again.

## BLP0470

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0470 CATID OF FILE '(&00)' IS NOT LOCAL. PROCESSING ABORTED

### Meaning

The cat ID of the specified file is not local. The linking-
loading is rejected by DBL.

## BLP0500

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

BLP0500 PROGRAM '(&00)', VERSION '(&01)' OF '(&02)' LOADED

### Meaning

The program with name (&00), version (&01) and
creation date (&02) is loaded.
This message is always sent to the terminal (exception: the task
switch 4 is set) and, additionally, to the operator console if the
CPG-option EACTETYP is set to '2' or '3'.

## BLP0501

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0501 OPERAND ERROR IN MONJV (MONITORING JOB VARIABLE). COMMAND REJECTED

### Response

See previous MONJV message.

## BLP0502

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0502 ERROR WHEN READING PROGRAM FILE. LOADING ABORTED

## BLP0505

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0505 AT THE MOMENT INSUFFICIENT MEMORY TO EXECUTE PROGRAM

### Meaning

- Parameter "RESIDENT-PAGES" in /START-PROGRAM command is in conflict
with the attributes of the current task, or
- Total number of pages (resident + pageable) for the program execution
is in conflict with the attributes of the current task, or
- Paging saturation.

## BLP0506

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0506 INVALID CONTEXT INFORMATION. PROGRAM NOT LOADABLE

### Meaning

Context information has been wrongly generated by PBELDE or
error occurred during BLS data structure initialization.

### Response

Contact the system administrator.

## BLP0507

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0507 LOADER FOUND INVALID TEXT MODIFIER RECORD. PROGRAM NOT LOADABLE

### Response

Correct the OML (object module library) and retry loading.

## BLP0508

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0508 NAME OF TEXT MODIFIER RECORD DOES NOT CORRESPOND TO PROGRAM NAME. PROGRAM NOT LOADABLE

### Response

Correct the OML (object module library) and retry loading.

## BLP0509

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0509 ERROR WHEN LOADING PROGRAM. COMMAND NOT PROCESSED

## BLP0510

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0510 FOR STATIC LOADER NO MEMORY AVAILABLE FOR LOADING PROGRAM

### Meaning

Either not enough space is available in the system or the load
point is not in the user address space.

## BLP0511

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0511 I/O ERROR WHEN READING PAM FILE. DMS ERROR '(&00)'. IN SYSTEM MODE /HELP-MSG DMS(&00)

### Meaning

An error corresponding to the specified DMS error code (&00) occurred
when loading the program by the static loader.
For more detailed information about DMS error code enter
/HELP-MSG DMS(&00) in system mode or see the DMS manual.

### Response

Contact the system administrator.

## BLP0512

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0512 INVALID FILE OR MODULE NAME. COMMAND REJECTED

### Meaning

File or module name is invalid in the command /LOAD-PROGRAM resp.
/START-PROGRAM or the filename references a non imported pubset.

### Response

Repeat the command with correct operand.

## BLP0513

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0513 PROGRAM ERROR FLAG SET. ALL COMMANDS WILL BE IGNORED UNTIL /SET-JOB-STEP OR /LOGOFF INTERCEPTED

### Meaning

User program has detected an error flag.

## BLP0514

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0514 ERROR WHEN OPENING FILE '(&01)'. DMS ERROR '(&00)'. IN SYSTEM MODE /HELP-MSG DMS(&00)

### Meaning

For more detailed information about DMS error code enter
/HELP-MSG DMS(&00) in system mode or see the DMS manual.

## BLP0515

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0515 INVALID OPERAND IN COMMAND FOR LOADING PROGRAM. CORRECT COMMAND

### Meaning

User attempted to issue a command /START-PROGRAM or
/LOAD-PROGRAM with an invalid format.

### Response

Correct rejected command and try again.

## BLP0516

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0516 AUDIT MODE SWITCHED ON. PROCESSING CONTINUES

### Meaning

The TU-AUDIT is switched on. The loading time will be increased.

### Response

Switch off TU-AUDIT to decrease the loading time.

## BLP0517

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

BLP0517 MODULE '(&00)' LOADED

### Meaning

The dynamic bind and load is done.
(&00): First module name (if the first module is an object module). This
message is always sent to the terminal (exception: the switch 4 is
set) and, additionally, to the operator console when the CPG option
EACTETYP is set to '2' or '3'.

## BLP0518

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0518 INVALID FORMAT OF LOAD MODULE. COMMAND REJECTED

### Response

Generate the load module again.

## BLP0519

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 30

Warranty : NO

BLP0519 PROGRAM '(&00)' LOADED

### Meaning

When the CPG-option EACTETYP is set to '1' or '2', the name of the
loaded program (&00) is sent to the operator console.

## BLP0520

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0520 ACCESS ERROR ON PROGRAM LIBRARY. PLAM AMCB ERROR CODE '(&00)' AND SYSTEM ERROR CODE '(&01)'. IN SYSTEM MODE /HELP-MSG PLA(&00)

### Meaning

An error has been detected by PLAM.
(&00) : PLAM AMCB error code (see manual LMS).
(&01) : System service error code.
For more detailed information about the PLAM AMCB error code
enter /HELP-MSG PLA(&00) in system mode.

### Response

If necessary take DUMP.

## BLP0521

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0521 LOADING OF CLASS-1 PROGRAM NOT PERMITTED. COMMAND REJECTED

## BLP0522

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0522 INPUT FILE NOT PAM FILE

### Meaning

The user tried to load a file which is not a PAM file.

## BLP0523

Destination: USER-TASK Routing code: Weight: 30

Warranty : YES

BLP0523 ELEMENT '(&00)', VERSION '(&01)' FROM LIBRARY '(&02)' IN PROCESS

### Meaning

External identification of a LLM (Link and Load Module) if the first
loaded module is a LLM. The type L element with the name (&00) and the
version (&01) from the library (&02) is processed by DBL.

## BLP0524

Destination: USER-TASK Routing code: Weight: 30

Warranty : YES

BLP0524 LLM '(&00)', VERSION '(&01)' OF '(&02)' LOADED

### Meaning

Internal identification of a LLM (Link and Load Module) if the first
loaded module is a LLM: LLM with internal name(&00), internal
version (&01) and creation date and time (&02) was loaded.
This message is always sent to terminal (exception : the task switch 4
is set) and, additionally, to the operator console if the CPG-option
EACTETYP is set to '2' or '3'.

## BLP0529

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0529 ERROR IN BLS STARTER. PROCESSING ABORTED

### Meaning

An internal error has been detected by the starter ECEXECUT:
the parameter list of $CPROG is incorrect.

### Response

Contact the system administrator.

## BLP0530

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0530 I/O ERROR WHEN READING PROGRAM LIBRARY : PLAM AMCB ERROR CODE '(&00)' AND SYSTEM ERROR CODE '(&01)'. IN SYSTEM MODE /HELP-MSG PLA(&00)

### Meaning

(&00): PLAM-AMCB error code.
(&01): System error code.
The error occurred during static loading.
For more detailed information about PLAM-AMCB error
code enter /HELP-MSG PLA(&00) in system mode.

### Response

Retry later.

## BLP0532

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0532 ERROR WHEN LOADING PROGRAM

### Meaning

Further information about the error is generally specified in a preceding
BLS message.
If there is no preceding message, an inconsistency has been detected
by the dynamic loader between the load unit to be processed and the
command /START-PROGRAM or /LOAD-PROGRAM of DBL.
Example : a subsystem is loaded above 16 MB and a command /START-PROGRAM
or /LOAD-PROGRAM is specified with the same entry point name and without
PROG-MOD=ANY on an XS machine.

### Response

See the preceding BLS message if there is any.

## BLP0533

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0533 SYSTEM ERROR

### Meaning

Error code for $TERM after system error.

### Response

Contact the system administrator.

## BLP0534

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0534 NO MEMORY SPACE AVAILABLE. PROGRAM NOT LOADED

### Meaning

Class 5 memory saturation. There is not enough space to satisfy the
system request.

### Response

Contact the system administrator.

## BLP0536

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0536 INTERNAL ERROR IN STATIC LOADER. PROCESSING ABORTED WITH DUMP

### Meaning

An internal error has been detected while reading the program phase.

### Response

Contact the system administrator.

## BLP0540

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0540 DATA SECURITY CHECK FAILURE. LOADING ABORTED

### Meaning

Error during library or element check. Possible reasons :
the relocation items (RLD) or the OML directory (1 or 2) or the
input (LLM or OM) is corrupted.

### Response

Correct input and try again.

## BLP0541

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

BLP0541 THE SYMBOLIC INFORMATION (LSD) IS ONLY PARTIALLY LOADED

### Meaning

A discrepancy between the real LSD size and the corresponding information
in the LSDA records has been detected.

## BLP0550

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0550 DISCREPANCY BETWEEN LAST PAGE NUMBER IN CATALOG ENTRY OF PROGRAM FILE AND PROGRAM HEADER

### Meaning

The number of the last page in catalog entry of the program file is
not equal to the page number written by TSOSLNK.

## BLP0551

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

BLP0551 Copyright (C) (&01) (&00). All rights reserved

### Meaning

(&00): copyright text.
(&01): copyright year, if specified.
This message is issued when the copyright is available. This message is
always sent to the terminal (exception: the task switch 4 is set) and,
additionally, to the operator console if the CPG-option EACTETYP is
set to '2' or '3'.

## BLP0552

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

BLP0552 Copyright (C) (&00) Fujitsu Technology Solutions GmbH. All rights reserved

### Meaning

(&00): copyright year, if specified.
This message is always sent to the terminal (exception: the task switch 4
is set), and, additionally, to the operator console if the CPG-option is
set to '2' or '3'.

## BLP0553

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0553 IN THIS PROCEDURE IT IS NOT PERMITTED TO UNLOAD AN ALREADY LOADED PROGRAM. COMMAND REJECTED

### Meaning

The operand UNLOAD=NO was given in the command /CALL-PROCEDURE.
So it is not permitted to unload a program which has already been
loaded at this moment.
This case is an error, SPINOFF is activated.

## BLP0554

Destination: USER-TASK Routing code: Weight: 30

Warranty : YES

BLP0554 NO PROGRAM TO UNLOAD

### Meaning

A command /CANCEL-PROGRAM was issued when no program had been loaded.

## BLP0555

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0555 PROGRAM FILE NOT COMPLETE. LOADING ABORTED

### Meaning

The number of the last page in the catalog entry of the program file
written by TSOSLNK does not correspond to the number in the program
header. Part of the program file has been destroyed.

## BLP0560

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

BLP0560 INVALID 'CFID' DETECTED DURING PROGRAM LOADING

### Meaning

The CFID of the page is not equal to the CFID in the catalog entry.
Either this page has not been written by TSOSLNK during the program
generation or it has been overwritten before the command /START-PROGRAM
or /LOAD-PROGRAM.

## BLP0565

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

BLP0565 ### INCOMPATIBLE OPERAND VALUES. OPERAND IGNORED. PROCESSING CONTINUES

### Meaning

There is an incompatibility between operand values of the /START- or
/LOAD-PROGRAM command.
Possible reasons:
- ALTERNATE-LIBRARIES=NO and AUTOLINK=ALTERNATE-LIBRARIES: AUTOLINK=NO
assumed.

## BLP0570

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0570 TEST AND DIAGNOSTIC INFORMATION NOT LOADED

### Meaning

A 'CFID' error has been detected when loading the test and diagnostic
information.

## BLP0977

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0977 ### REPFILE '(&00)' DOES NOT EXIST. REP PROCESSING ABORTED

### Meaning

The specified repfile (&00) does not exist. The module is loaded
without REP correction.

### Response

Retry with the correct repfile name.

## BLP0978

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

BLP0978 PROBLEM DURING REPLOG TASK INITIALIZATION. NO REP LOGGING ON THIS SESSION

### Meaning

A problem occurs during REPLOG task initialization, no REP
logging will be active on current session.

### Response

Contact the system administrator.

## BLP0979

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0979 ### NO ACTIVE REP LOGGING FILE ON THIS SESSION. NO READ MARK SET

### Meaning

On this session, no REP logging file is currently open.
The /SET-REPLOG-READ-MARK command is thus aimless.

## BLP0980

Destination: CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

BLP0980 REP COMMENT: '(&00)'

### Meaning

The REP comment (&00) from the REP file is displayed.

## BLP0981

Destination: CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

BLP0981 LOCK FOR REP LOGGING HELD BY TASK WITH ID '(&00)'. PROCESSING CONTINUES WITHOUT REP LOGGING

### Meaning

Accesses to the REP logging information in memory cannot be done,
because the task with Id (&00) holds the necessary lock.

### Response

Contact the system administrator.

## BLP0990

Destination: CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

BLP0990 PROCESSING OF REP FILE '(&00)' STARTED

### Meaning

(&00): REP file name.

## BLP0991

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

BLP0991 $GETMEM ERROR. PROCESSING OF REP FILE '(&00)' NOT EXECUTED

### Meaning

The REP loader routine cannot obtain memory space.

## BLP0992

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

BLP0992 DMS ERROR CODE '(&00)'. PROCESSING OF REP FILE '(&01)' ABORTED. IN SYSTEM MODE /HELP-MSG DMS(&00)

### Meaning

(&00): DMS error code
(&01): REP file name
The REPs read before the DMS error are applied.
For more detailed information about the DMS error code enter
/HELP-MSG DMS(&00) in system mode or see the DMS manual.

### Response

Correct the file before the next loading.

## BLP0993

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

BLP0993 REP '(&00)'-ERROR. REPFILE '(&02)'. REP PROCESSING CONTINUES. (&01)

### Meaning

An error of the type (&00) has been detected when processing the REP
record (&01) that has last been read from the file (&02).
This REP is not applied.
(&00) = FORMAT : format error
= PARITY : parity error
= CHECK : data check error
= NAME : invalid module name or module not found
= LENGTH : address not in module
= VERSION : invalid version number.
= RELOC : - relocation truncated (type H or L) or
- relocation range error (type I)
(&01): invalid REP record.

### Response

Correct the invalid REP before the next loading.

## BLP0994

Destination: USER-TASK Routing code: Weight: 50

Warranty : YES

BLP0994 ERROR WHILE SETTING READ MARK ON CURRENT REP LOGGING FILE. COMMAND NOT PROCESSED

### Meaning

The CLTF CLOSE function (called with type = PSEUDO) has reported
an error to BLS. The command is not processed.

## BLP0995

Destination: CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

BLP0995 NOREF FILE IS '(&00)'

### Meaning

(&00) NOREF file name.

## BLP0996

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

BLP0996 DMS ERROR CODE '(&00)'. PROCESSING OF NOREF FILE '(&01)' ABORTED. IN SYSTEM MODE /HELP-MSG DMS(&00)

### Meaning

(&00): DMS error code.
(&01): NOREF file name.
For more detailed information about the DMS error code enter
/HELP-MSG DMS(&00) in system mode or see the DMS manual.

### Response

Correct the file before the next loading of the concerned program.

## BLP0997

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : YES

BLP0997 $GETMEM ERROR. PROCESSING FOR NOREF FILE '(&00)' ABORTED

### Meaning

The REP loader routine cannot obtain a
work area. The NOREF file (&00) cannot be used.

## BLP0998

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

BLP0998 DMS ERROR '(&00)' WHEN OPENING FILE '(&01)'. RETRY ? REPLY (Y=YES; N=NO). IN SYSTEM MODE /HELP-MSG DMS(&00)

### Meaning

The REP file cannot be opened.

### Response

Correct the error and retry (answer: Y),
or abort the REP processing (answer: N).
Only one retry is allowed and if it is not successful
the REP processing is aborted with message BLP0992.
When the REP processing is aborted the program remains
loaded but without REP correction(s).

## BLP0999

Destination: CONSOLE Routing code: * (main console) Weight: 50

Warranty : NO

BLP0999 ERROR IN REPLOG TASK. REP LOGGING SUPPRESSED. DUMP TAKEN, PROCESSING CONTINUES

### Meaning

An external call has reported to DBL an error in the REPLOG task.
The possible external calls are :
- $RETMEM
- CLTF(Common-Log-Task-Facility) call
- $TSKID
- $SYSINF.
System dump taken and REP logging suppressed, but the normal REP
processing continues.

### Response

Contact the system administrator.

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages