## SMRREVI

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SMRREVI COMP=SMRMF,VER=001,DATE=940922,COMPNR=00000001

### Meaning

MEANING : NO FURTHER INFORMATION

### Response

RESPONSE : NONE

## SMR0001

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SMR0001 NO STRING IS POSSIBLE FOR THE COMMANDS /START-SUBSYSTEM AND /STOP-SUBSYSTEM

### Meaning

MEANING : NO FURTHER INFORMATION
CLASS : E
KEYWORD : SUBSYSTEM,COMMANDS

### Response

RESPONSE : NONE

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages