## NRTC500

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC500 TERM-REQ FOR TSN=(&00),EC=(&01),NIA=(&02)

### Meaning

A termination request for the preallocated task with the task sequence
number (&00) has been initiated with event code (&01) at location (&02)
before the end of class-2-STARTUP.

### Response

Take SLED.

## NRTC501

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC501 TERM-REQ FOR TSN=(&00),EC=(&01),NIA=(&02) (&03)

### Meaning

A termination request for the preallocated task with the task sequence
number (&00) has been initiated with event code (&01) at location (&02).
If possible, additionally (&03) the termination code is given.

### Response

Take SLED.

## NRTC502

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC502 TERM-ORDER INIT FAILED AND CDUMP NOT POSSIBLE.

### Meaning

In the module NRTINIT, it was not possible to process a termination
request in spite of several retries. Additionally a system dump could
not be taken.

### Response

As this is a diagnostic crash, take SLED.

## NRTC503

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC503 TERMINATION ORDER OVERFLOW AND CDUMP NOT POSSIBLE

### Meaning

In the module NRTINIT more than 4 recursive termination requests have
occurred. Additionally a system dump could not be taken.

### Response

As this is a diagnostic crash, take SLED.

## NRTC504

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC504 NEITHER SERSLOG NOR CDUMP POSSIBLE

### Meaning

The module NRTINIT has received a recursive termination order during
SERSLOG processing. Additionally a system dump could not be taken.

### Response

As this is a diagnostic crash, take SLED

## NRTC505

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC505 REPETITIVE TERMINATION ERROR AND CDUMP NOT POSSIBLE

### Meaning

The module NRTINIT has detected repetitive errors in the module NRTCTRL.
Additionally a system dump could not be taken.

### Response

As this is a diagnostic crash, take SLED.

## NRTC506

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC506 ERROR DURING TASK DESTROY AND CDUMP NOT POSSIBLE

### Meaning

The module NRTINIT has received a termination order after task
destruction was initiated for the task (the indicator ETCBLTST is set
in the switch ETCBRTSW). Additionally a system dump could not be taken.

### Response

As this is a diagnostic crash, take SLED.

## NRTC507

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC507 NO TERMINATION WORK AREA AVAILABLE

### Meaning

In the module NRTINIT it was not possible to obtain a Termination Work
Area.

### Response

As this is a diagnostic crash, take SLED.

## NRTC508

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC508 TERMINATION WORK AREA NOT ACCESSIBLE AND CDUMP NOT POSSIBLE.

### Meaning

In the module NRTINIT it was not possible to access the Termination Work
Area addressed in the TCB. Additionally a system dump could not be taken.

### Response

As this is a diagnostic crash, take SLED.

## NRTC509

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC509 TERM-REQ FOR TSN=(&00),NIA=(&01)

### Meaning

A termination request for the preallocated task with the task
sequence number (&00) has been initiated at location (&01)
before the end of class-2-STARTUP.

### Response

Take SLED.

## NRTC510

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC510 SYSTEM DUMP REQUESTED FOR A SYSTEM TASK DURING SHUTDOWN. CDUMP NOT POSSIBLE

### Meaning

The processing of a system task leads to an error which causes an
abnormal task termination with request for a system dump.
If this occurs during SHUTDOWN(-END)-processing, an abnormal system
termination ("crash") is initiated if system is in fault intolerant
mode.
When an analogous error is caused by a user task, the task is set
to permanent wait state "Pended indefinitely".
When the system is in tolerant mode, any task which leads to the
analogous error will be terminated. Any diagnostic information is lost.

### Response

Take SLED.

## NRTC511

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC511 RECURSION DURING TERMINATION FOR UNALLOWED INTERRUPTS

### Meaning

An error within the central error handling routine of Termination
Processing has led to a recursive call of this (central error
handling) routine.
The following actions are necessary in order to avoid an endless loop:
If the switch NRTRECSW is set to X'FF',
an abnormal system termination ("crash") is initiated.
If the switch is not set, the affected task is put into
permanent wait state "Pended indefinitely".
Diagnostic information remains available.

### Response

Take SLED.

## NRTC512

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC512 DIAGNOSTIC REP AT (&00)

### Meaning

A diagnostic rep at location (&00) caused the system crash.

### Response

As this is a diagnostic crash, take SLED.

## NRTC513

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC513 SYSTEM DUMP REQUESTED FOR A SYSTEM TASK WHILE RESTART OPTION WITH DUMP IS ON. CDUMP NOT POSSIBLE

### Meaning

The processing of a system task leads to an error which causes an
abnormal task termination with request for a system dump.
If this occurs while Restart Option is switched on with DUMP
an abnormal termination ("crash") is initiated with automatic SLED
if system is in fault intolerant mode.
When an analogous error is caused by a user task, the task is set
to permanent wait state "Pended indefinitely".
When the system is in tolerant mode, any task which leads to the
analogous error will be terminated. Any diagnostic information is lost.

## NRTC514

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC514 MER ERROR AT NIA (&00); EVENT CODE (&01)

### Meaning

An illegal interrupt with event code (&01) of class 'M' (machine error)
has been detected at address (&00) in SIH.
Processing was terminated in order to avoid further possible problems.

### Response

Take SLED.

## NRTC515

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC515 SVC ERROR AT NIA (&00)

### Meaning

An interrupt of class 'S' (SVC) has been detected in SIH.
Processing was terminated in order to avoid further possible problems.

### Response

Take SLED.

## NRTC516

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC516 PRG-INT ERROR AT NIA (&00); EVENT CODE (&01)

### Meaning

An illegal interrupt with event code (&01) of class 'P' (program
interrupt) has been detected at address (&00) in SIH.
Processing was terminated in order to avoid further possible problems.

### Response

Take SLED.

## NRTC517

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC517 SYSTEM DUMP REQUESTED FOR A SYSTEM TASK WHILE DMS NOT YET READY. CDUMP NOT POSSIBLE

### Meaning

The processing of a system task leads to an error which causes an
abnormal task termination with request for a system dump.
If this occurs within startup while DMS not yet ready an abnormal
system termination ("crash") is initiated is system is in fault
intolerant mode.
When an analogous error is caused by a user task, the task is set
to permanent wait state "Pended indefinitely".
When the system is in tolerant mode, any task which leads to the
analogous error will be terminated. Any diagnostic information is lost.

## NRTC550

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTC550 ONE OR MORE TASKS PERMANENTLY PENDED. TAKE SLED

### Meaning

One or more tasks were put into the permanent wait state
"Pended Indefinitely" during the session.

### Response

As this is a diagnostic crash, take SLED.

## NRTKILL

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTKILL TASK TERMINATED BY /CANCEL ...,KILL

### Meaning

The operator or system administrator issued the command
/CANCEL ...,KILL for this task.

### Response

NONE

## NRTK100

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTK100 RELEASE OF PCB NOT POSSIBLE DUE TO MISSING ADF

### Meaning

The dsl processing routine gave a bad return code, i.e.
it was not possible to return to automatic storage area.
"Function detach" of the actual PCB was not possible,
therefore the task had to be abnormally terminated.

## NRTK101

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTK101 ERROR AT CANCEL RELEASE ROUTINE

### Meaning

The reasons for this error can be:
1. The Command Processor was called incorrectly.
2. The Command Processor calls incorrectly the cancel release routine.
3. The PCB link mechanism is inconsistent.
4. The indicator "CANCEL REQUESTED" was set wrongly.

## NRTK109

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTK109 THIS TASK WITH USERID (&00), JOBNAME (&01) ISSUED A CANCEL COMMAND FROM THE TERMINAL (&02) FOR TASK (&03)

### Meaning

This task with the USERID (&00) and the jobname (&01) has cancelled the
the task with the Task Sequence Number (&03).
If the canceller is a dialog task, the terminal (&02) is named;
otherwise the terminal is given as BATCH.

### Response

NONE

## NRTK201

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTK201 SHUTDOWN SOON (&00)

### Meaning

The terminal user is informed that the session will be terminated by
the /SHUTDOWN command soon. The operator can specify an explaining
text (&00).
No further jobs will be started in this session.

### Response

Terminate processing as soon as possible.

## NRTP200

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTP200 ABNORMAL TASK TERMINATION DUE TO USE OF AN ENVIRONMENT NOT SUPPORTED BY THE PROGRAM MANAGER

### Meaning

The task was terminated abnormally because the called routine
requests an environment that is not supported by the Program Manager.

### Response

Take dump to determine the erroneous routine.

## NRTP201

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTP201 ABNORMAL TASK TERMINATION DUE TO OVERFLOW OF A NON-EXPANDABLE STACK

### Meaning

The task was abnormally terminated because the requested amount of
dynamic storage exceeds the size of the program stack and it is not
possible to expand the stack (resident or real time stack).

### Response

Take dump to determine the reason for the stack overflow.

## NRTP202

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTP202 ABNORMAL TASK TERMINATION DUE TO STACK UNDERFLOW

### Meaning

The task was abnormally terminated because more dynamic storage
within the program stack was to be returned than had been requested
(one @EXIT to many).

### Response

Take dump to determine the reason for the stack underflow.

## NRTP203

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTP203 ABNORMAL TASK TERMINATION BECAUSE REQUESTED ADF LENGTH EXCEEDS EXTENT LENGTH

### Meaning

The Program Manager was called to provide an ADF that is longer than
the maximal extent length. Therefore the task was abnormally
terminated.

### Response

Take dump to determine the erroneous routine.

## NRTP204

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTP204 ABNORMAL TASK TERMINATION BECAUSE GIVEN EXTENT LENGTH IS TOO SHORT

### Meaning

The minimal length of a stack extent must be 400 bytes. When calling
the Program Manager, a smaller extent length was given.

### Response

Take dump to determine the caller of the Program Manager.

## NRTP205

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTP205 ABNORMAL TASK TERMINATION DUE TO $REQM ERROR WHEN REQUESTING A STACK EXTENT

### Meaning

It was not possible for the Program Manager to obtain a new stack extent.

## NRTP206

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTP206 ABNORMAL TASK TERMINATION DUE TO INVALID NON-LOCAL-GOTO DESTINATION

### Meaning

The ADF given as destination of a non-local goto was not requested on
the current PCB level but on a PCB on a lower level.

### Response

Take dump to determine the caller of the non-local goto function.

## NRTP207

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTP207 ABNORMAL TASK TERMINATION DUE TO A NON-LOCAL-GOTO TO AN ADF THAT DOES NOT EXIST

### Meaning

The ADF given as destination of a non-local goto does not exist.

### Response

Take dump to determine the caller of the non-local goto.

## NRTP208

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTP208 ABNORMAL TASK TERMINATION DUE TO THE OVERWRITING OF THE STACK

### Meaning

The task was terminated because stack management data in the stack
has been overwritten.

### Response

Take dump to determine the overwriter. The overwriter can probably
be found in the uppermost ADF, which is addressed by the TCB field
ETCBPMSP. The overwriting is detected when the ADF is to be released.

## NRTSHUT

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTSHUT TASK TERMINATED BY /SHUTDOWN

### Meaning

The operator has initiated system termination with the command /SHUTDOWN.
Therefore the task was aborted.

### Response

NONE

## NRTT101

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTT101 ABNORMAL JOBSTEP TERMINATION (&00)

### Meaning

The jobstep was abnormally terminated.
The cause is documented by the termination code (&00), which is a
message code and can be issued with the /HELP command.

### Response

NONE

## NRTT201

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTT201 TASK TERMINATION DUE TO /(&00) COMMAND

### Meaning

The task termination was caused by a /CANCEL-JOB resp. /CANCEL or a
/SHUTDOWN command.

### Response

NONE

## NRTT501

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTT501 SETS. (&00) (&01)

### Meaning

The abbreviation "SETS" stands for "SYSTEM ERROR TERMINATED SESSION".
The running session is aborted. (&00) specifies the identifier of
a message that explains the cause for system termination. (&01) is an
insert to be interpreted together with the message specified by (&00).

### Response

see manual "Operating"

## NRTT502

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRTT502 SETS. (&00) (&01)

### Meaning

The abbreviation "SETS" stands for "SERIOUS ERROR TERMINATED SESSION".
The running session is aborted. (&00) specifies the identifier of
a message that explains the cause for the system termination. (&01) is
an insert to be interpreted together with the message specified by (&00).

### Response

see the Manual "Operating".

## NRTV001

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRTV001 MONITOR SYSTEM FAILED

### Meaning

The monitor system failed because of a system error.

### Response

NONE

## NRTV002

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRTV002 MONITOR SYSTEM NOT READY. RESTART HAS BEEN INITIATED

### Meaning

Possible reasons:
- An automatic RESTART has been initiated after a system error in the
monitor system
- SHUTDOWN with RESTART initiated in the monitor system
- SVP-RESTART initiated in the monitor system

### Response

NONE

## NRTV003

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRTV003 MONITOR SYSTEM READY AGAIN

## NRT0001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0001 ABNORMAL PROGRAM TERMINATION DUE TO TERM MODE=ABNORMAL

### Meaning

Termination of the program has been requested by the program with the
help of the macro
TERM UNIT=PRGR,MODE=ABNORMAL

### Response

NONE

## NRT0002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0002 NON-PRIVILEGED CALL OF TERM-INTERFACE FROM PRIVILEGED PROCESS

### Meaning

The non-privileged TERM-interface was called from a privileged process
(TPR-PCB).
The Generative Components TERM, TERMD and TERMI are concerned as far
as they mean the Program and not the Jobstep termination.

### Response

The call of the non-privileged TERM-interface must be replaced by
the call of the privileged $TERM-interface.

## NRT0101

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0101 ABNORMAL PROGRAM TERMINATION DUE TO TERM UNIT=STEP,MODE=ABNORMAL

### Meaning

Termination of the program has been requested by the program with the
help of the macro
TERM UNIT=STEP,MODE=ABNORMAL

### Response

NONE

## NRT0200

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0200 HARDWARE-DETECTED SOFTWARE ERROR FROM TPR

### Meaning

An interrupt with one of the following interrupt weights has occurred
while executing TPR coding:
48, 54, 58, 5C, 60, 64, 68, 6C, 70, 74, 78.

### Response

Take dump.

## NRT0202

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0202 SYSTEM ERROR IN /LOGOFF PROCESSING

### Meaning

The module NRTLGOF has been called for a system task or for a task
without a Termination work area.

### Response

Take dump.

## NRT0203

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0203 PAGING ERROR DUE TO HARDWARE ERROR IN TPR

### Meaning

An interrupt with the event code 94 (paging error due to hardware error)
has occurred while executing task privileged (TPR) coding.
The console hardcopy should be checked to determine if a message EXC0857
with the insert "PGER" has occurred shortly beforehand, as the error
may be a disk error.

### Response

NONE

## NRT0204

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0204 TASK TERMINATED DUE TO SUSPECTED DEADLOCK

### Meaning

The task was terminated, because it is presumably in a deadlock
situation.

### Response

Take dump.

## NRT0205

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0205 HARDWARE ERROR IN TPR

### Meaning

An interrupt with the event code 5E (Hardware Error) has occurred while
executing task privileged (TPR) coding.

### Response

NONE

## NRT0206

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0206 TASK RESTART IN TEST MODE NOT POSSIBLE DUE TO MISSING ADF

### Meaning

The task had been enabled for task restart in test mode.
It was not possible to return to the automatic storage area active
at enable time. Therefore the task had to be abnormally terminated.

### Response

NONE

## NRT0207

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0207 ABNORMAL TASK TERMINATION BECAUSE THE TASK VECTOR COULD NOT BE OBTAINED

### Meaning

It was not possible to obtain the task vector needed to activate
system exits. Therefore the task is terminated abnormally.

### Response

NONE

## NRT0208

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0208 ABNORMAL TASK TERMINATION BECAUSE THE SYSTEM VECTOR WAS NOT OBTAINED

### Meaning

It was not possible to obtain the system vector to call system exits.
Therefore the task was terminated abnormally.

### Response

NONE

## NRT0601

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0601 INVALID TERM PARAMETER LIST

### Meaning

The parameter list of the TERM macro issued by the program is either
inaccessible or contains one or more invalid parameter values.
Following TERM is executed instead:
TERM UNIT=PRGR,MODE=ABNORMAL,DUMP=Y

### Response

Call TERM with a valid parameter list.

## NRT0602

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0602 INVALID $TERMSPL PARAMETERLIST

### Meaning

The entry NRTISPL to the module NRTINIT has been called with one or more
invalid parameters.

### Response

Take dump.

## NRT0603

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0603 INVALID $TERM PARAMETER LIST

### Meaning

The given $TERM parameter list could not be interpreted by the module
NRTINIT.

### Response

Take dump.

## NRT0605

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0605 NRTINIT ERROR

### Meaning

An error has occurred in the module NRTINIT or in a routine called by it:
- during the initialization of the termination work area
- during the initialization of the termination order
- during SERSLOG processing

### Response

Take dump.

## NRT0606

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0606 SYSTEM DUMP RETRY

### Meaning

A system error occurred during the system dump called by termination.
The CDUMP function is retried.

### Response

NONE

## NRT0607

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0607 ERROR DURING TERMINATION

### Meaning

During Termination a called function returned a bad return code or was
aborted.
The corresponding diagnostic information can be found within the Soft-
ware-Error-Logging-File under the respective Rectype.
There are the following error cases:
1. Rectype NRT0101: Function gave a bad return code.
2. Rectype NRT0102: Repetitive calls during Termination.
3. Rectype NRTTRM1: Error during the STXIT-processing.

### Response

NONE

## NRT0608

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NRT0608 SYSTEM TASK RECOVERY WITH EXIT INSTEAD OF $TERM

### Meaning

A Systemtaskrecovery-Routine may not terminate with EXIT. If a
continuation of termination is wanted, a new $TERM must be called.

## NRT0610

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0610 TERMINATION CODE WAS NOT GIVEN CORRECTLY

### Meaning

The pointer to termination code given within a general register
was an invalid address. This result was indicated by hard validation.
This message is the replacement for the non-accessible original
termination code of the $TERM-call.

## NRT0611

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT0611 DEFAULT TERMINATIONCODE.

### Meaning

For an abnormal task termination the termination code is not
supplied. Therefore a default termination code is used.

### Response

NONE

## NRT0700

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT0700 TSN (&00): ERROR AT TASK INIT ROUTINE (&01). TASK CREATION ABORTED

### Meaning

(&00) : Task Sequence Number of the corresponding task.
(&01) : Name of the task initialization routine,
which gave a bad return code to Creation.
Creation issues this Emergency-Message and initiates subsequently
the termination of this task.

### Response

Partner for further diagnose is the responsible of the given
task initialization routine. He can give information about the reason
why the present bad return code was delivered.

## NRT1200

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1200 SHUTDOWN WITH RUNTIME LIMIT REQUESTED BY '(&00)'. REMAINING RUNTIME: '(&01)'

### Meaning

(&00) SHUTDOWN requester.
(&01) Remaining runtime in the form hh:mm.
After lapse of the given runtime the machine is stopped.

### Response

NONE

## NRT1201

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1201 SHUTDOWN REQUESTED BY '(&00)'

### Meaning

(&00) SHUTDOWN requester.

### Response

NONE

## NRT1202

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1202 SHUTDOWN WITH AUTOMATIC RESTART INITIATED

### Meaning

An Automatic Restart was specified with the SHUTDOWN request, i.e.
after system termination a system restart should be initiated.

### Response

NONE

## NRT1203

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1203 SHUTDOWN WITH AUTOMATIC RESTART WITHDRAWN. DYNAMIC I/O CONFIGURATION CHANGES ARE STARTED

### Response

An Automatic Restart was specified with the SHUTDOWN request, i.e. after
system termination a system restart should be initiated.
The command is rejected because dynamic I/O configuration changes are
started which may prevent a system restart.

## NRT1204

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1204 SHUTDOWN END ALREADY BEING PROCESSED. REQUEST REJECTED

### Meaning

NO FURTHER INFORMATION

### Response

NONE

## NRT1205

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1205 SHUTDOWN WITH AUTOMATIC RESTART AND IPL DEVICE CHANGE WITHDRAWN. SVP-FUNCTIONS NOT SUPPORTED

### Meaning

An Automatic Restart with IPL device change was specified with the
SHUTDOWN request, i.e. after system termination a system restart with
a new IPL device should be initiated.
The request is rejected because the necessary SVP functions (GET/MODIFY
IPL DEVICE LIST) are not supported.

## NRT1206

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1206 SHUTDOWN WITH AUTOMATIC RESTART AND IPL-DEVICE CHANGE WITHDRAWN. INTERNAL $HSVP ERROR

### Meaning

An Automatic Restart with IPL device change was specified with the
SHUTDOWN request, i.e. after system termination a system restart with
a new IPL device should be initiated.
The request is rejected because an internal error occurred at $HSVP call.

## NRT1207

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1207 SHUTDOWN WITH AUTOMATIC RESTART AND IPL DEVICE CHANGE WITHDRAWN. IPL DEVICE UNKNOWN

### Meaning

An Automatic Restart with IPL device change was specified with the
SHUTDOWN request, i.e. after system termination a system restart with
a new IPL device should be initiated.
The request is rejected because the given IPL device is unknown to the
system.

## NRT1208

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1208 SHUTDOWN WITH AUTOMATIC RESTART AND IPL DEVICE CHANGE WITHDRAWN. INTERNAL $NKBINF ERROR

### Meaning

An Automatic Restart with IPL device change was specified with the
SHUTDOWN request, i.e. after system termination a system restart with
a new IPL device should be initiated.
The request is rejected because an internal error ocurred at $NKBINF call.

## NRT1209

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

NRT1209 AUTOMATIC RESTART INHIBITED BECAUSE IPL DEVICE WAS REMOVED BY DRV

### Meaning

Automatic Restart cannot be switched on or is switched off because the
IPL device is removed by DRV.

## NRT1210

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1210 SHUTDOWN WITH AUTOMATIC RESTART AND IPL DEVICE CHANGE WITHDRAWN. IPL DEVICE IS NOT A VALID DISK

### Meaning

An Automatic Restart with IPL device change was specified with the
SHUTDOWN request, i.e. after system termination a system restart with
a new IPL device should be initiated.
The request is rejected because the given IPL device either is not a disk
or else is invalid.

## NRT1211

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1211 SHUTDOWN WITH AUTOMATIC RESTART AND IPL DEVICE CHANGE WITHDRAWN. IPL DEVICE IS NOT INSTALLED OR NOT ASSIGNED TO SYSTEM

### Meaning

An Automatic Restart with IPL device change was specified with the
SHUTDOWN request, i.e. after system termination a system restart with
a new IPL device should be initiated.
The request is rejected because the given IPL device is not installed or
else not assigned to system (virtual machine).

### Response

If needed, first assign IPL device by means of ADD-VM-DEVICES.

## NRT1212

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1212 SHUTDOWN WITH AUTOMATIC RESTART AND CHANGE OF IPL DEVICE WITHDRAWN: IPL DEVICE NOT ASSIGNED EXCLUSIVELY TO THE VM BY COMMAND.

## NRT1213

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1213 SHUTDOWN WITH AUTOMATIC RESTART AND CHANGE OF IPL DEVICE WITHDRAWN: IPL DEVICE NOT ACCEPTED.

### Meaning

Repeat SHUTDOWN: either choose now another IPL Device or initiate
an automatic Restart with the actual IPL Device.

## NRT1215

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1215 SHUTDOWN REQUEST WITHDRAWN. ARCHIVE-TASKS ARE STILL ACTIVE

## NRT1216

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1216 RUNNINIG ARCHIVE TASKS IGNORED. SHUTDOWN PROCESSING CONTINUES

## NRT1219

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1219 INVALID VALUE '(&00)' FOUND IN SYSTEM PARAMETER SHUTPROC. DEFAULT VALUE 'BY-SHUTDOWN-CMD' ASSUMED

### Meaning

(&00) Actual invalid value.
Valid values are 'BY-SHUTDOWN-CMD' or 'BY-ENTER-JOB'.

### Response

Correct System Parameter SHUTPROC

## NRT1220

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT1220 SHUTDOWN REQUEST BY '(&00)' ABORTED WITH ERROR '(&01)'

### Meaning

(&00) SHUTDOWN caller.
(&01) Error cause with possible values
1,2,..9: Internal Error (for System Diagnosis only)
CMDxxxx: CMD-RC of /ENTER-JOB Command

### Response

In case of Error-Code CMDxxxx check Command-File SYSENT.SHUTDOWN

## NRT5001

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NRT5001 NO SLOTPOOL FOR TASK-CREATION AVAILABLE

### Meaning

No slot pool can be installed during task creation for building
a Task Control Block (TCB). Therefore it is not possible to
create dynamically any task during session.

### Response

Take SLED.

## NRT9005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT9005 BOURSE PROBLEMS WITHIN THE COMMON LOG TASK.

### Meaning

A bourse call within the Common Log Task received an unexpected
returncode.

### Response

Take dump.

## NRT9008

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NRT9008 SYSTEM ERROR IN SERSLOG PROCESSING

### Meaning

One of the system functions $RELM, $MSG, $SINF or "Complete Filename"
called by NRTELOG could not be executed correctly.

### Response

Take dump.

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages