## NTF0C0C

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0C0C NO VALID USER ID COULD BE ASSIGNED AS OWNER OF PORT NAME

### Meaning

No valid user ID could be assigned as the owner of the port
name to be protected by a SUPPORT profile.

## NTF0C04

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0C04 SPECIFIED STANDARD CONNECTION ID OUTSIDE PERMISSIBLE VALUE RANGE

### Meaning

The specified standard connection ID is not contained within
the permissible value range.

## NTF0C10

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0C10 CALLER NOT AUTHORIZED TO MODIFY REQUEST PROFILE

### Meaning

The caller does not comply with the SUPPORT authorization
profile of the protected name or the testing module
(GUARDS) is not active.

## NTF0018

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0018 FITC NOT AVAILABLE. FUNCTION NOT POSSIBLE

### Meaning

FITC is not available in the system.

## NTF0100

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0100 INTERNAL FITC ERROR

## NTF0101

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0101 UNEXPECTED PKSTXIT ERROR

## NTF0102

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0102 LOOP COUNTER RUN DOWN; PRESUMED ENDLESS LOOP ABORTED

## NTF0103

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0103 CIP LOCK INCONSISTENCY

## NTF0104

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0104 MEMORY BOTTLENECK FOR FITC SLOT POOL

## NTF020A

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF020A ERROR IN CREATING TASK

## NTF020B

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF020B ERROR IN TRACE MANAGEMENT

## NTF0201

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0201 ERROR OF NEW CMF

## NTF0202

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0202 ERROR IN NAME MANAGER

## NTF0203

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0203 ERROR IN MEMORY MANAGEMENT

## NTF0204

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0204 ERROR IN SLOT MANAGEMENT

## NTF0205

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0205 ERROR IN VALIDATION

## NTF0206

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0206 ERROR IN DATA SPACE MANAGEMENT

## NTF0207

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0207 ERROR IN CONTINGENCY MANAGEMENT

## NTF0208

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0208 ERROR IN GUARDS MANAGEMENT

## NTF0209

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0209 ERROR IN SAT MANAGEMENT

## NTF040C

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF040C SPECIFIED PORT NAME ALREADY ASSIGNED

### Meaning

No SUPPORT GUARD name or standard port name can be assigned.

## NTF0404

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0404 ILLEGAL PARAMETER COMBINATION

### Meaning

Abortion owing to incorrect parameter list. This may be caused by
incorrect parameter block alignment, an unknown function code,
a missing parameter or an illegal link to another parameter block.

## NTF0418

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0418 FUNCTION CANNOT BE PERFORMED AT PRESENT DUE TO LACK OF MEMORY SPACE

### Meaning

No internal FITC tables can currently be set up because there is
not sufficient memory available.

## NTF080C

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF080C SPECIFIED STANDARD CONNECTION ID ALREADY ASSIGNED

### Meaning

The value specified as the standard connection ID has already
been assigned.

## NTF0804

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF0804 SPECIFIED APPLICATION NAME (PORT NAME) NOT PERMITTED

### Meaning

The port name specified is illegal.

## NTF100C

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF100C SPECIFIED GUARD NAME(S) CANNOT BE COMPLETED

### Meaning

The specified GUARD name(s) could not be completed because
the syntax was not correct.

## NTF1010

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF1010 SUPPORT PROFILE ASSIGNED TO PORT NAME CANNOT BE ACCESSED

### Meaning

The SUPPORT profile assigned to the port name cannot be accessed.
Execution is rejected because no check can be made.

## NTF140C

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF140C REQUEST PROFILE CAN ONLY BE ALLOCATED TOGETHER WITH SUPPORT PROFILE OR IF LATTER EXISTS

### Meaning

A REQUEST profile can only be assigned together with the SUPPORT
profile or if the latter exists (in which case the caller's SUPPORT
authorization is requested).

## NTF1418

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF1418 FUNCTION ABORTED OWING TO INTERNAL FITC ERROR

### Meaning

An internal FITC error has occurred. It can no longer be
guaranteed that FITC will operate without error.

## NTF400C

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

NTF400C REDEFINITION OF SPECIFIED ATTRIBUTES NOT PERMITTED

### Meaning

The specified attributes cannot be redefined.

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages