## JPM0202

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JPM0202 REMOTE JOB MANAGEMENT NOT AVAILABLE. COMMAND REJECTED

### Meaning

When the command was processed, the remote job management facility
was inactive.

### Response

Ask the operator to set up the MSCF (multi system control facility)
environment and repeat the command once this has been done.

## JPM0204

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

JPM0204 SYSTEM ERROR ON PROCESSOR '(&00)'. ERROR CODE: '(&01)'. COMMAND PROCESSING TERMINATED

### Meaning

An internal system error occurred during command processing on the
remote processor, causing processing to be aborted.
(&00): BCAM name of the remote processor, taken from the MONJV operand.
(&01): error code:
x'04': request memory error for MCLP (macro command
language processor).
x'08': request memory error for the response.
x'0C': invalid caller code.
x'10': error in MCLP call.
x'1C': error when sending the request.

### Response

Retry the command later.

## JPM0205

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

JPM0205 USER NOT AUTHORIZED TO WORK WITH REMOTE PROCESSOR '(&00)'. COMMAND REJECTED

### Meaning

The user is not authorized to execute the command on the specified
remote processor.
(&00): BCAM name of the remote processor.

### Response

Ask the system administrator to create a JOIN entry for the remote
processor analogous to the one for the home processor, and then
repeat the command.

## JPM0208

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

JPM0208 SYSTEM ERROR ON THIS PROCESSOR WHILE SENDING REPLY TO USER '(&00)' ON PROCESSOR '(&01)'. MRSSEND RETURN CODE IS '(&02)'

### Meaning

A system error occurred during command processing, making it impossible
to respond to the request from user (&00) on remote processor (&01).
Command processing is aborted and, after a timeout, the user is
informed that the connection between the processors has been severed.
(&00): user ID on the remote processor.
(&01): BCAM name of the remote processor.
(&02): MRSSEND return code:
x'04': invalid action code (correct: REPLY).
x'08': message too long.
x'12': BCAM name unknown.
x'16': remote processor not connected.
x'20': error in MRSSEND processing.
x'28': MC or BCAM not active.
x'32': attempt to send to own processor.

### Response

Contact the system administrator.

## JPM0209

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JPM0209 REQUEST MEMORY ERROR ON THIS PROCESSOR. COMMAND REJECTED

### Meaning

A request memory error occurred during command processing. This prevents
further processing.

### Response

Retry the command later.

## JPM0500

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

JPM0500 MESSAGE(S) OR OUTPUT FROM REMOTE PROCESSOR '(&00)':

### Meaning

This message is displayed as a result of a command which has been
issued via MSCF for execution on the specified remote processor.
Any resulting messages or other output on the remote system will
subsequently be displayed on SYSOUT or the operator console.
(&00): BCAM name of the remote processor.

### Response

Take appropriate action in accordance with the following
message(s) or output.

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages