## SSM0001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM0001 CYCLE IN SYSLST'S INDIRECTIONS. CORRECT COMMAND

### Meaning

User attempts to assign a 'SYSLSTn' system file to another
'SYSLSTm', provoking a cycle in the assignments.
'n' and 'm' are two numbers included between 01 and 99.

## SSM0002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM0002 System error during PCB access. Program terminated abnormally

## SSM0003

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM0003 TERMINAL DISPLAY INTERRUPTED BY K2 AT 'PLEASE ACKNOWLEDGE'

### Meaning

During the display at terminal, the K2 key has been pressed at
'PLEASE ACKNOWLEDGE'. Only the part of the message really
displayed is logged onto SYSLST followed by this message.

## SSM0004

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM0004 The asked sysfile function is not available for a RLOGIN task

### Meaning

A RLOGIN task can not use some specified functions as RDATA, WRTRD, etc.
Read/write a message on terminal using TIAM macros is not allowed except
for a MIP message or the SYSDTA/SYSIPT assignmenty to SYSCMD is rejected.

## SSM0005

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM0005 Unexpected return code received from system interface. SERSLOG entry written

## SSM0006

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM0006 Output to file with MODE=PHYS cancelled

### Meaning

A WROUT or WRTRD of a text containing physical control characters has
been done when SYSOUT is not assigned to the terminal
(file, library element, S-variable, etc.). This message replaces the text
that should be output. This also occurs on SYSLST when the logging has
been requested by /MODIFY-JOB-OPTIONS LOGGING=*PARAM(LISTING=*YES).

## SSM0301

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM0301 24 BIT SVC USED IN STATE 'P2'. TASK ABNORMALLY TERMINATED

## SSM1000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1000 INPUT FILE '(&00)' CANNOT BE CLOSED. DMS ERROR CODE '(&01)'. DMS ERROR: /HELP-MSG-INFORMATION DMS(&01)

### Meaning

In case of failure during close processing of an input file,
the DMS error code shows the error which occured.
For more detailed information about the DMS error enter
/HELP-MSG-INFORMATION command.

## SSM1001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1001 DCM ERROR 'I/O OUTSTANDING' DURING TERMINAL PROCESSING

## SSM1002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1002 SYSTEM ERROR DURING DMS OPERATION ON FILE '(&00)'. DMS ERROR CODE '(&01)'. DMS ERROR: /HELP-MSG-INFORMATION DMS(&01)

### Meaning

For more detailed information about the DMS error enter
/HELP-MSG-INFORMATION command.

## SSM1004

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1004 RELEASE MEMORY ERROR DURING SYSFILE ASSIGNMENT ON AN INPUT FILE

## SSM1005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1005 SYSTEM ERROR DURING ERASE PROCESSING ON FILE '(&00)'. DMS ERROR CODE '(&01)'. DMS ERROR: /HELP-MSG-INFORMATION DMS(&01)

### Meaning

For more detailed information about the DMS error enter
/HELP-MSG-INFORMATION command.

## SSM1006

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1006 SYSTEM ERROR DURING RELEASE OF FILE '(&00)'. DMS ERROR CODE '(&01)'. DMS ERROR: /HELP-MSG-INFORMATION DMS(&01)

### Meaning

For more detailed information about the DMS error enter
/HELP-MSG-INFORMATION command or refer to DMS manual.

## SSM1007

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1007 SYSTEM ERROR DURING SYSFILE ASSIGNMENT ON AN INPUT FILE

## SSM1008

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1008 SYSTEM ERROR DURING COMMAND EXIT PROCESSING

## SSM1009

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1009 NO MORE CLASS 5 MEMORY AVAILABLE DURING SYSFILE PROCESSING

## SSM1010

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1010 ABNORMAL PROGRAM TERMINATION DUE TO A WRONG ERROR ROUTINE ADDRESS

### Response

Correct error routine address and restart program.

## SSM1012

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1012 SYSTEM ERROR DURING RELEASE OF MEMORY IN COMMAND PROCESSING

## SSM1013

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1013 SYSTEM ERROR DURING COMMAND PROCESSING

## SSM1015

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1015 TERMINAL DISCONNECTED

### Meaning

Processing aborted.

### Response

Inform the system administrator.

## SSM1016

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1016 SYSTEM ERROR DURING 'GET' PROCESSING. FILE '(&00)' NOT OPENED. DMS ERROR CODE '(&01)'. DMS ERROR : /HELP-MSG-INFORMATION DMS(&01)

### Meaning

For more detailed information about the DMS error enter
/HELP-MSG-INFORMATION command.

## SSM1017

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1017 SYSTEM ERROR DURING 'MSG' PROCESSING

## SSM1021

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1021 SYSTEM ERROR DURING SWITCHING DISK TO TAPE

## SSM1024

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1024 USER ERROR DURING 'RDCRD' PROCESSING. USER DUMP CREATED

### Meaning

Due to a user error in RDCRD macro (p/l error, ...),
the user program terminates abnormally.

### Response

Diagnose the error.

## SSM1025

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1025 NO FD I/O DEVICE AVAILABLE. COMMAND REJECTED

### Meaning

A user has asked to read from a FD, but there is no
FD I/O device available.

### Response

The user may wait and re-enter the command.

## SSM1026

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1026 NO FD DEVICE AVAILABLE OR THE OPERATOR WAS UNABLE TO MOUNT THE SPECIFIED VSN'S. COMMAND REJECTED

### Response

Ask the operator for the reason and eventually correct the list of VSN's,
if there is any error and re-enter the command.

## SSM1027

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1027 ACCESS TO FD WITH VSN '(&00)' PROTECTED. COMMAND REJECTED

### Meaning

The volume VSN (&00) mounted is protected with the accessibility byte
not blank.

### Response

Give another VSN, or remove the accessibility byte.

## SSM1028

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1028 OPEN ERROR ON FD WITH VSN '(&00)' ON FD I/O DEVICE '(&01)'. COMMAND REJECTED

### Meaning

The track 0 cannot be read, or there is a wrong VOL1 label.

### Response

Look at the floppy disk, modify when possible the error
and re-enter the command.

## SSM1029

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1029 FILE '(&00)' NOT FOUND ON FLOPPY DISK WITH VSN '(&01)'. COMMAND REJECTED

### Response

Look for the right file name on the floppy disk and re-enter the command.

## SSM1030

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1030 OPEN ERROR FOR FILE '(&00)' ON FD DEVICE '(&01)'. COMMAND REJECTED

### Meaning

An error, such as: error during the read of the file's
label, or a wrong 'HDR1' label, has occurred during the
processing of OPEN of the file '(&00)'.

### Response

If possible, correct the floppy disk and re-enter the command.

## SSM1031

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1031 UNEXPECTED RETURN CODE (RC) SENT BACK BY TIAM TO SYSFILE CONVERTED TO AN UNRECOVERABLE ERROR

## SSM1100

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SSM1100 SYSFILE SUBSYSTEM NOT ACTIVE. TASK ABNORMALLY TERMINATED

### Meaning

A SYSFILE service is requested prior to system ready.

## SSM1101

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SSM1101 SYSFILE SUBSYSTEM IS NOT COMPATIBLE WITH SYSTEM VERSION

### Meaning

Integration error, SYSFILE cannot be initialized.

### Response

Reload system with correct SYSFILE version.

## SSM1201

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM1201 An internal error occurs during the pseudo close of either the syslst or the sysout file

## SSM1202

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM1202 System file is empty or not assigned

### Meaning

A read mark can't be set in an empty system file

## SSM1203

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM1203 Bad MONJV given in the /SET-<sysfile>-READ-MARK command

### Meaning

The specified JV is not monitoring a job

## SSM1204

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM1204 System file '(&00)' pseudo closed successfully

## SSM1205

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM1205 Waiting time for pseudo close operation expires, processing continues

## SSM1206

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM1206 TSN not found or command processing illegal. Command terminated

### Meaning

Possible reasons:
- the task does not exist
- the task does not allow information to be displayed

## SSM1207

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM1207 The system file is assigned to a library element or a S-variable

## SSM1208

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM1208 The MONJV given in the /SET-<sysfile>-READ-MARK command points to a task on a foreign system

## SSM1209

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM1209 Waiting time expires, processing continues

### Meaning

The command has probably been executed for a task that cannot be
interrupted

## SSM1210

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM1210 The system file is already closed

## SSM1211

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM1211 SYSTEM FILE ON TAPE, PSEUDO CLOSE OPERATION NOT POSSIBLE.

## SSM2000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2000 SYSLST SWITCHED FROM DISK TO TAPE. SPOOLOUT BEFORE CLOSE FUNCTION SUPPRESSED

## SSM2001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2001 DMS ERROR CODE '(&00)' DURING OPEN OF '*DUMMY' FILE. REASSIGNMENT OF SYSTEM FILE TO 'PRIMARY'. DMS ERROR: /HELP-MSG-INFORMATION DMS(&00)

### Meaning

For more detailed information about DMS error enter
/HELP-MSG-INFORMATION command.

## SSM2002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2002 DMS ERROR CODE '(&00)' DURING OPEN OF A CATALOGED SYSTEM FILE. REASSIGNMENT OF SYSTEM FILE TO 'PRIMARY'. DMS ERROR: /HELP-MSG-INFORMATION DMS(&00)

### Meaning

For more detailed information about DMS error enter
/HELP-MSG-INFORMATION command.

## SSM2003

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2003 SYNTACTICAL ERROR IN MEMBER NAME '(&00)' OF LIBRARY '(&01)'. COMMAND TERMINATED

### Meaning

The member name doesn't begin by an alphabetic character or is too long.

### Response

Re-enter the command with the correct member name.

## SSM2004

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2004 DMS ERROR '(&00)' ON LIBRARY '(&01)'. COMMAND TERMINATED. DMS ERROR: /HELP-MSG-INFORMATION DMS(&00)

### Meaning

A DMS error has occurred during the processing of a library file.
For more detailed information about DMS error enter
/HELP-MSG-INFORMATION command.

### Response

Analyse error code.

## SSM2005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2005 DMS ERROR '(&00)' ON FILE '(&01)'. COMMAND TERMINATED. DMS ERROR: /HELP DMS(&00)

### Meaning

A DMS error has occurred during the processing of the
temporary copy of a library member.
For more detailed information about DMS error enter /HELP command.

### Response

Analyse the error.

## SSM2006

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2006 FILE '(&00)' IS NOT A VALID SOURCE LIBRARY. COMMAND TERMINATED

### Meaning

The specified file is not a library file, or it's not a
source library, or it contains inconsistencies in its directory.

### Response

Analyse the error and take appropriate action.

## SSM2007

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2007 LIBRARY '(&00)' IS EMPTY. COMMAND TERMINATED

## SSM2008

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2008 MEMBER '(&00)' NOT FOUND IN LIBRARY '(&01)'. COMMAND TERMINATED

## SSM2009

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2009 SYSTEM ERROR DURING ASSIGNMENT OF THE PRIMARY SYSOUT FILE

### Meaning

An error has occurred during the CATAL, FILE or OPEN of the primary SYSOUT
file.

### Response

See the DMS return code in the SERSLOG entry.

## SSM2010

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2010 SYSTEM ERROR DURING ASSIGNMENT OF THE PRIMARY SYSLST FILE

### Meaning

An error has occurred during the CATAL, FILE or OPEN of the primary SYSLST
file.

### Response

See the DMS return code in the SERSLOG entry.

## SSM2011

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2011 SYSTEM ERROR DURING ASSIGNMENT OF THE PRIMARY SYSOPT FILE

### Meaning

An error has occurred during the CATAL, FILE or OPEN of the primary SYSOPT
file.

### Response

See the DMS return code in the SERSLOG entry.

## SSM2012

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SSM2012 UNABLE TO ASSIGN '(&00)' TO FILE '(&01)' DUE TO DMS ERROR CODE '(&02)'. PREVIOUS ASSIGNMENT KEPT. DMS ERROR: /HELP-MSG-INFORMATION DMS(&02)

### Meaning

The assignment is impossible due to the DMS error during
the FILE, CATAL or OPEN of the file.
For more detailed information about the DMS error enter
/HELP-MSG-INFORMATION command.
(&00): SYSOUT, SYSLST or SYSOPT

### Response

User error:
- Retry the command with a correct file.
System error:
- Contact the system administrator.

## SSM2013

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2013 NO MORE PROGRAM LOADED. TO RESUME THE PROCEDURE, ENTER COMMAND AGAIN WITH 'MODE=COMMAND'

### Meaning

No program is loaded and the user issued a /RESUME-PROCEDURE
command to return to a procedure which was interrupted in
program mode. o return to the interrupted procedure.

### Response

Re-enter command with MODE=COMMAND.

## SSM2014

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2014 TASK IN ESCAPE MODE AT LEVEL NUMBER '(&00)'

### Meaning

The message is displayed if either an /HOLD-PROCEDURE command is
encountered, or the answer to MSG EXC0613 is YES, or the escape mode
is downward propagated, due to an /END-PROCEDURE or /DO command
issued in escape mode.

## SSM2015

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2015 /HOLD-PROCEDURE COMMAND NOT ALLOWED IN BATCH. COMMAND IGNORED

## SSM2016

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2016 /HOLD-PROCEDURE COMMAND MAY NOT BE ENTERED FROM TERMINAL. COMMAND IGNORED

### Meaning

A command /HOLD-PROCEDURE may not be entered from the terminal, i.e. when
the task is not in procedure mode, or when the task is already in
interrupted state.

## SSM2017

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2017 SYNTACTICAL ERROR IN /RESUME-PROCEDURE COMMAND. RE-ENTER COMMAND

## SSM2018

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2018 /RESUME-PROCEDURE MAY ONLY BE ENTERED FROM TERMINAL

## SSM2019

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2019 NO PROCEDURE IN INTERRUPTED STATE. /RESUME-PROCEDURE COMMAND IGNORED

## SSM2020

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2020 NO PROGRAM LOADED. RE-ENTER COMMAND WITHOUT 'MODE=PROGRAM'

### Meaning

No program is loaded and a user issued command /RESUME-PROCEDURE
command with MODE=PROGRAM to return to an interrupted procedure.

### Response

Re-enter command without MODE=PROGRAM.

## SSM2021

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2021 INPUT EXCEEDS LOGON BUFFER SIZE. INCREASE BUFFER SIZE BY MEANS OF 'BUFFER' OPERAND IN /SET-LOGON-PARAMETERS COMMAND

### Meaning

The user entered an operand value which exceeds the buffer limits
defined at SET-LOGON-PARAMETERS.

### Response

Enter new value or issue a 'HOLD-PROGRAM'.

## SSM2022

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2022 INPUT OPERAND VALUE LONGER THAN 255 BYTES

### Response

Enter new value or a 'HOLD-PROGRAM'.

## SSM2023

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2023 STRING DELIMITER IS MISSING

### Meaning

User entered a string of alphanumerics which does not end with an
apostrophe.

### Response

Enter a new string or a 'HOLD-PROGRAM'.

## SSM2024

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2024 STRING SYNTAX ERROR

### Meaning

User entered an invalid string of alphanumerics due to the string
separator (space) being absent.

### Response

Enter a different string or a 'HOLD-PROGRAM'.

## SSM2025

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2025 OPERAND ERROR. RE-ENTER THE CORRECT OPERAND VALUE

### Response

Enter a new operand or a 'HOLD-PROGRAM'.

## SSM2029

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2029 SYSTEM ERROR DURING 'ALLOCATE/DEALLOCATE' PROCESSING

## SSM2031

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2031 WARNING: FILE GROUP '(&00)' CANNOT BE DECLARED IN OUTPUT MODE ON DISKS

### Meaning

The user cannot direct the system cataloged file SYSLST/SYSOPT/SYSOUT to
a file group, defined on private or public disks. Only a file group
on tape in output mode is allowed.

## SSM2032

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2032 DMS ERROR '(&00)' WHILE SWITCHING FROM DISK TO TAPE. DMS ERROR: /HELP-MSG-INFORMATION DMS(&00)

### Meaning

For more detailed information about the DMS error enter
/HELP-MSG-INFORMATION command.

## SSM2033

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

SSM2033 USER ID '(&00)', TSN: (&01) REQUESTED TAPE/MBK FOR CATALOGED SPOOL FILE

### Meaning

In interactive or batch mode a user requests a tape/MBK for his
cataloged file.

## SSM2034

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2034 NO MORE SPACE AVAILABLE ON DISK. SPOOL FILE '(&00)' WILL BE WRITTEN ON TAPE

### Meaning

Batch usage - no space for cataloged SPOOL file on disk store.

## SSM2035

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

SSM2035 NO MORE SPACE AVAILABLE ON DISK FOR SPOOL FILE '(&00)'. DO YOU WANT TO COPY AND EXTEND THE FILE ON A TAPE/(&01) OR TO CONTINUE ON *PRIMARY ? REPLY (T=TAPE; M=(&01);P=*PRIMARY;N=NO)

### Meaning

Terminal usage - it is determined that no space is available on disk store
for the cataloged SPOOL file (&00).

### Response

T: A tape is desired.
M: A (&01) is desired.
P: The system file is reassigned to *PRIMARY.
N: The system file is reassigned to *DUMMY.

## SSM2036

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2036 INVALID OPERAND IN COMMAND. COMMAND REJECTED

### Response

Correct the error and re-enter the command.

## SSM2037

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM2037 Unable to process a SYSFILE procedure called by 'DO' in a S-Procedure with SYSTEM-FILE-CONTEXT=*SAME-AS-CALLER

### Response

Transform the SYSFILE procedure into a S-Procedure or use CALL or
CALL-PROCEDURE command instead of DO command.

## SSM2038

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM2038 Coded-Character-Set not allowed

### Meaning

A coded character set can not be specified with the parameter OPEN-MODE=
*EXTEND or with the parameter TO=*VARIABLE/*PRIMARY/*DUMMY

## SSM2039

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SSM2039 DMS ERROR '(&00)' WHILE CLOSING A SYSOUT/OPT/LST (DMS ERROR: /HELP-MSG-INFORMATION DMS(&00)). EITHER PROCESSING CONTINUES (SYSOUT/OPT) OR PROCESSING IS ABORTED (SYSLST)

### Meaning

A DMS error has been detected while closing SYSOUT, SYSOPT or a SYSLST.
For more information about DMS error enter /HELP-MSG-INFORMATION
command.

## SSM2041

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2041 INCOMPATIBLE OPERATION MODE WITH /RESTART-PROGRAM COMMAND. COMMAND PROCESSING ABORTED

### Meaning

The SYSFILE environment of a task, saved by the CHKPT macro in a
specified mode of operation (batch or interactive), is reconstructed,
by the /RESTART-PROGRAM command, in the other mode (interactive or
batch). This construction is stopped because specific conditions
connected with the operation mode have been found; (redirection of
SYSOUT in batch, and procedure interruption is interactive).

## SSM2042

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2042 /RESTART-PROGRAM COMMAND MAY NOT BE ISSUED WITHIN A PROCEDURE MODE

## SSM2043

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2043 THE INPUT COMMAND OR DATA EXCEEDS THE CONTINUATION AREA. INPUT IGNORED

### Meaning

The length of the resulting input command or data
can be maximum 2040 bytes, including the V-field's
length. This input is ignored and is not displayed.
However, this error message is not sent, when the
erroneous input is skipped by a /SKIP-COMMANDS command,
or by SPIN-OFF mechanism.

### Response

The user is advised to reduce the contents of the
concerned input data or command.

## SSM2044

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2044 COMMAND REJECTED BY THE SYSTEM ADMINISTRATOR

### Meaning

The command was rejected by the exit routine for SYSCMD.

## SSM2045

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2045 DATA RECORD READ WHEN COMMAND WAS EXPECTED

### Meaning

A data record was read when a command was expected.
This data is displayed only when the protocol allows it.
This error message is not sent when the erroneous input is skipped
by a /SKIP-COMMANDS command, or by the SPIN-OFF mechanism.

### Response

Correct the JCL procedure and retry.

## SSM2046

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2046 'SYSDTA' IS STILL ASSIGNED. RESET ASSIGNMENT WITH /ASSIGN-SYSDTA TO-FILE=*PRIMARY AND RE-ENTER /RESTART-PROGRAM COMMAND

### Response

Retry after releasing it by a /ASSIGN-SYSDTA command.

## SSM2047

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2047 'SYSIPT' IS STILL ASSIGNED. RESET ASSIGNMENT WITH /ASSIGN-SYSIPT TO-FILE=*PRIMARY AND RE-ENTER /RESTART-PROGRAM COMMAND

### Response

Retry after releasing it by a /ASSIGN-SYSIPT command.

## SSM2048

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM2048 Coded-Character-Set not supported by XHCS

## SSM2049

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2049 'SYSOPT' IS STILL ASSIGNED. RESET ASSIGNMENT WITH /ASSIGN-SYSOPT TO-FILE=*PRIMARY AND RE-ENTER /RESTART-PROGRAM COMMAND

### Response

Retry after releasing it by a /ASSIGN-SYSOPT command.

## SSM2050

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2050 EXPLICIT '(&00)' ASSIGNMENT STILL IN EFFECT. COMMAND PROCESSING ABORTED

### Meaning

SYSLST or a SYSLSTnn system file is reassigned explicitly when issued
a /RESTART-PROGRAM command.
'nn' is a number included between 01 and 99.
(&00): SYSLST or SYSLSTnn system file.

### Response

Reassign the corresponding system file
to its primary value and re-enter the /RESTART-PROGRAM command.

## SSM2051

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2051 EXPLICIT 'SYSOUT' ASSIGNMENT STILL IN EFFECT

### Meaning

SYSOUT still assigned in batch when issuing a /RESTART-PROGRAM command.

## SSM2052

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SSM2052 PROCEDURE FILE '(&00)' CANNOT BE OPENED. DMS ERROR CODE '(&01)'. COMMAND TERMINATED. DMS ERROR: /HELP-MSG-INFORMATION DMS(&01)

### Meaning

Procedure file referenced by a /DO or /CALL-PROCEDURE cannot be
opened. For more detailed information about DMS error enter
/HELP-MSG-INFORMATION command.

### Response

Analyse error code and re-enter the command.

## SSM2053

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SSM2053 FILE '(&00)' IS NOT A PROCEDURE FILE. COMMAND REJECTED

### Meaning

The file is not a SAM or ISAM file, or does not begin with
a /BEGIN-PROCEDURE command.

## SSM2054

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2054 SYMBOLIC OPERAND ERROR IN COMMAND. COMMAND IGNORED

### Response

Re-enter a corrected command.

## SSM2055

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2055 SYMBOLIC OPERAND ERROR IN /BEGIN-PROCEDURE COMMAND. PROCEDURE ABORTED

### Meaning

A syntactical error has been found at symbolic operand level.
An /END-PROCEDURE command is simulated.

### Response

Correct the error and re-enter the procedure file.

## SSM2056

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2056 SYMBOLIC OPERAND INCONSISTENCY BETWEEN /BEGIN-PROCEDURE COMMAND AND CALLING COMMAND. PROCEDURE TERMINATED

### Meaning

The symbolic operands specified in the calling command (/DO or
/CALL-PROCEDURE) doesn't correspond with those declared in the
/BEGIN-PROCEDURE command. The procedure file is terminated: an
/END-PROCEDURE command is simulated.

### Response

Re-enter the procedure file with the correct operand.

## SSM2057

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2057 INVALID /BEGIN-PROCEDURE COMMAND. IT MUST BE THE FIRST COMMAND OF A PROCEDURE FILE. COMMAND IGNORED

## SSM2058

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2058 THE PROTOCOL OPTION IS INVALID IN /BEGIN-PROCEDURE COMMAND. NO LOGGING WILL BE DONE. PROCEDURE CONTINUES

### Response

Modify the PROTOCOL option in the /BEGIN-PROCEDURE command.

## SSM2059

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2059 INVALID DATA SUBSTITUTION OPTION IN /BEGIN-PROCEDURE COMMAND. NO DATA SUBSTITUTION WILL BE DONE

### Meaning

The value assigned to the ESCAPE-CHARACTER operand in the
/BEGIN-PROCEDURE command is invalid. Procedure continues but no
data substitution will be done.

## SSM2060

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2060 DO YOU WANT TO ABORT ALL ACTIVATED PROCEDURES ? REPLY (Y=YES; N=NO)

### Meaning

During terminal procedure parameter prompting K2 occurs
Y : All the currently activated procedures are aborted.
N : Procedure continues, preceding prompting is repeated.

## SSM2061

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2061 ERROR DURING THE ACCESS TO A LIBRARY ELEMENT

### Meaning

Syntactical error in member name,
DMS error during library access,
the file isn't a valid library,
the library is empty,
the member doesn't exist in the library,
error during PLAM operation (ATTACH,OPEN,GET,CLOSE,DETACH),
PLAM isn't available.

## SSM2062

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM2062 Command too long for SYSFILE internal area

## SSM2063

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2063 THE REQUEST OF MEMORY FOR SYSFILE PROCESSING IS UNSUCCESSFUL. COMMAND NOT PROCESSED

### Response

Check the reason why user's memory limit is reached
or contact the system administrator.

## SSM2064

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2064 THE FILE REFERENCED IN THE COMMAND CANNOT BE PROCESSED IN RFA MODE. COMMAND TERMINATED

### Meaning

These commands cannot be executed for remote files:
/CALL-PROCEDURE
/ENTER-JOB
/ASSIGN-SYSxxx.

## SSM2065

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2065 END OF FILE REACHED DURING PROCESSING OF PROCEDURE FILE

### Meaning

EOF reached during procedure file processing without
an /END-PROCEDURE command being encountered.

## SSM2066

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

SSM2066 SPOOLOUT REQUESTED FOR '(&00)'. SPOOL NOT AVAILABLE. DO YOU WANT TO WAIT FOR 'SPOOL READY'? REPLY (Y=YES; N=NO)

### Meaning

(&00): SYSOUT, SYSLST or SYSOPT.

### Response

Y: The processing waits for 'SPOOL READY' (the terminal is
not available until the request has been accepted by SPOOL).
N: The SPOOLOUT is lost and the processing continues.

## SSM2067

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2067 SPOOL NOT AVAILABLE. THE SPOOLOUT REQUEST IS DEFERRED UNTIL 'SPOOL READY'

## SSM2068

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2068 TASK NOT IN PROCEDURE MODE. COMMAND TERMINATED

## SSM2074

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SSM2074 SPOOL NOT LOADED OR NOT READY. COMMAND TERMINATED

## SSM2075

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

SSM2075 SPOOLOUT REQUESTED FOR FILE '(&00)'? REPLY (Y=YES; N=NO)

### Meaning

(&00): SYSLST, SYSOUT or SYSOPT.

### Response

Y: The SPOOLOUT request is scheduled and the processing continues.
N: The SPOOLOUT is lost and the processing continues.

## SSM2076

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM2076 WRITING TO FILE '(&00)' FAILED ON CURRENT DEVICE '(&01)'. SWITCHING TO DEVICE '(&02)'.

## SSM2077

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM2077 ALL $SSMXXXX LINK NAMES IN USE. FURTHER PROCESSING NOT POSSIBLE.

## SSM2078

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SSM2078 NO MORE SPACE AVAILABLE ON DISK FOR FILE '(&00)'. DO YOU WANT TO COPY AND EXTEND THE FILE ON A TAPE/(&01) ? REPLY (T=TAPE; M=(&01) ;N=NO)

### Meaning

Terminal usage - it is determined that no space is available on disk store
for the cataloged SPOOL file (&00).

### Response

T: A tape is desired.
M: A (&01) is desired.
N: The system file is reassigned to *DUMMY.

## SSM2221

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2221 PROGRAM/TASK TERMINATED: 'MAXOPT' REACHED

### Meaning

The maximum value of SYSOPT is reached and,
the user does not want to continue the processing.
The program (WRTOT records) is terminated without dump.

### Response

Program error (e.g. loop):
- Correct the program and retry.
MAXOPT limit too low:
- Increase the MAXOPT limit and retry.

## SSM2222

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

SSM2222 SPECIFIED MAXLST LIMIT REACHED. CONTINUE? REPLY (Y=YES; N=NO)

### Response

Y: The user decides to continue. The MAXLST counter is reset
to zero and the previously defined limit remains unchanged.
N: The user decides to abort. The program is terminated
without dump (termination code SSM2223).

## SSM2223

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2223 PROGRAM/TASK TERMINATED: 'MAXLST' REACHED

### Meaning

The maximum value of SYSLST is reached and,
the user does not want to continue the processing.
The program (WRLST records) is terminated without dump.

### Response

Program error (e.g. loop):
- Correct the program and retry.
MAXLST limit too low :
- Increase the MAXLST limit and retry.

## SSM2224

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

SSM2224 SPECIFIED MAXLST LIMIT FOR SYSOUT REACHED. CONTINUE? REPLY (Y=YES; N=NO)

### Response

Y: The user decides to continue. The MAXOUT counter is reset
to zero and the previously defined limit remains unchanged.
N: The user decides to abort. The program is terminated
without dump (termination code SSM2228).

## SSM2225

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2225 CLOSE ERROR ON SYSTEM FILE. JOB CONTINUES

### Meaning

An error has been detected during closing
of a cataloged system file (SYSOUT,SYSLST,SYSOPT).

## SSM2226

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

SSM2226 SPECIFIED MAXOPT LIMIT REACHED. CONTINUE? REPLY (Y=YES; N=NO)

### Response

Y: The user decides to continue. The MAXOPT counter is reset
to zero and the previously defined limit remains unchanged.
N: The user decides to abort. The program is terminated without dump
(termination code SSM2021.

## SSM2227

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2227 SYSTEM ERROR DURING 'DCTI' PROCESSING IN TIAM

### Meaning

ERRLOG entry created.

## SSM2228

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2228 PROGRAM/TASK TERMINATED: 'MAXLST' FOR SYSOUT REACHED

### Meaning

The maximum value of SYSOUT is reached and,
the user does not want to continue the processing.
The program (WROUT records) is terminated without dump.

### Response

Program error (e.g. loop):
- Correct the program and retry.
MAXLST limit too low :
- Increase the MAXLST limit and retry.

## SSM2250

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM2250 INCONSISTENT LOGGING LINE SIZE, 132 IS ASSUMED

### Meaning

The range of LOGGING-LINE-SIZE is 16..2044, 132 is the standard value.

### Response

None, the command is accepted

## SSM3000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3000 PLAM '(&00)' ERROR '(&01)'/'(&02)' ON LIBRARY '(&03)'. COMMAND NOT PROCESSED. CHECK ERROR CODE

### Meaning

(&00): ATTACH/OPEN/GET/CLOSE/DETACH
(&01): First PLAM error code
(&02): Second PLAM error code
(&03): Library name

## SSM3001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3001 PLAM NOT IN SYSTEM. COMMAND NOT PROCESSED. CONTACT SYSTEM ADMINISTRATOR

## SSM3005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3005 SYSTEM ERROR DURING '$SINF' PROCESSING. TASK TERMINATED ABNORMALLY. CONTACT SYSTEM ADMINISTRATOR

### Meaning

System error during CLASS2OP access processing.

## SSM3015

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3015 ABNORMAL PROGRAM TERMINATION DUE TO A WRONG ADDRESS OF THE ERROR ROUTINE. PROGRAM ABORTED

### Meaning

The error code is indicated in user register 15.

### Response

Correct and retry the user program.

## SSM3016

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3016 SYSTEM ERROR DURING 'TIAM' PROCESSING

### Meaning

ERRLOG entry created.

## SSM3017

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3017 PARAMETER LIST NOT ACCESSIBLE FOR SVC39. PROGRAM TERMINATED WITH DUMP

### Response

Correct and retry the user program.

## SSM3018

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3018 PARAMETER LIST NOT ACCESSIBLE FOR OLD SYSFILE SVC (NOT 39). PROGRAM TERMINATED WITH DUMP

### Meaning

Correct the program and retry.

## SSM3019

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3019 'YTIOUT' ISSUED FROM NON-PRIVILEGED PROGRAM. PROGRAM TERMINATED ABNORMALLY

### Response

Correct the program and retry.

## SSM3026

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3026 FILE NAME MISSING. COMMAND REJECTED

### Meaning

The operand 'NAME=' is missing, when '(DISKETTE)' or
'(MN)' and 'VOLUME=' are specified.

### Response

Correct the command and re-enter.

## SSM3027

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3027 'VOLUME' OPERAND MISSING. COMMAND REJECTED

### Meaning

The operand 'VOLUME=' is missing, while '(DISKETTE)'
or '(MN)' and 'NAME=' are specified.

### Response

Correct the command and re-enter.

## SSM3028

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3028 '(&00)' IS NO FD I/O DEVICE. COMMAND REJECTED

### Meaning

The user has specified 'TO-FILE=*DISKETTE(UNIT,...)', and
the unit (&00) does not correspond to a FD I/O device.
(&00): Mnemonic of the device.

### Response

Get the correct mnemonic of the FD I/O device from the
operator, correct the command and re-enter.

## SSM3029

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3029 'SYSIPT' IS NOT ALLOWED FOR FLOPPY DISK. COMMAND REJECTED

### Meaning

The user has specified 'TO-FILE=*DISKETTE(UNIT=,...)'.

### Response

The system file SYSIPT, with macro RDCRD cannot be
directed to a floppy disk device. The user may use the macro RDATA and
can direct the system file SYSDTA to a FD.

## SSM3030

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3030 A FD I/O DEVICE IS ALREADY ASSIGNED. PROCESSING CONTINUES

### Meaning

The user has specified the direction of the 'SYSDTA' to
a FD I/O device, with new or same values, which are
ignored, while 'SYSDTA' is already directed to the device.

## SSM3031

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3031 VALIDATION OPERANDS ERROR. COMMAND REJECTED

### Meaning

A command '/ASSIGN-SYSLST' is specified with:
1) a ND2 operand.
The NDFILE exists and the values specified do not
exist in that file (MXM or LOOP records)
2) a 'LOOP' operand but no NDFILE or no SPOOLFILE exists.
3) an invalid value (>31) for the 'SHIFT' operand has been given.

### Response

Correct the command with appropriate values and re-enter the command.

## SSM3034

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3034 ASSIGNMENT IS ALREADY PRIMARY. PROCESSING CONTINUES

### Meaning

User issued /ASSIGN-SYSxxx command to change
SYSIPT or SYSDTA to its primary assignment
and the system file had already been in primary assignment.

## SSM3035

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3035 ASSIGNMENT ALREADY THE SAME AS '(&00)'. PROCESSING CONTINUES

### Meaning

The specified system file is already correctly assigned.
The command will be ignored.
(&00): 'SYSCMD' or 'SYSDTA'.

## SSM3036

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3036 'SYSIPT' CANNOT BE ASSIGNED TO A TERMINAL

### Response

Assign SYSIPT to an appropriate device.

## SSM3039

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3039 NO PRIMARY ASSIGNMENT EXISTS FOR FILE REASSIGNMENT

### Meaning

User attempted to reassign a system file back to its primary assignment
when no primary assignment for the file has been designated.

### Response

Assign file and retry.

## SSM3042

Destination: CONSOLE Routing code: J Weight: 99

Warranty : NO

SSM3042 DMS ERROR '(&00)' ON FILE '(&01)'. JOB ABORTED. DMS ERROR: /HELP-MSG-INFORMATION DMS(&00)

### Meaning

An OPEN error has been detected on the SYSCMD file during the task
initialization. For more detailed information about DMS error enter
/HELP-MSG-INFORMATION command.

### Response

Check the status of the file and respool in or re-enter the job.

## SSM3052

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3052 'SYSDTA' OR 'SYSIPT' REASSIGNED TO PRIMARY. PROCESSING CONTINUES

### Meaning

At checkpoint time, SYSDTA or SYSIPT had been assigned.
This assignment is lost. SYSDTA or SYSIPT is reassigned to PRIMARY.
Command continues.

## SSM3053

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3053 INVALID OPERAND OR COMBINATION OF OPERANDS. COMMAND REJECTED

## SSM3054

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3054 ILLEGAL UNIT NUMBER FOR SVC39. PROGRAM TERMINATED ABNORMALLY

### Meaning

The unit number used in header of the SVC39 parameter list is incorrect
or not supported.

### Response

Correct the program and retry.

## SSM3055

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3055 USER SPECIFIED INCORRECT 'RECFORM' FOR THE FILE

### Meaning

A SAM or ISAM file contains an invalid record format.

## SSM3056

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SSM3056 FILE '(&00)' COULD NOT BE OPENED, DUE TO DMS ERROR: '(&01)'. DMS ERROR: /HELP-MSG-INFORMATION DMS(&01)

### Meaning

A /ASSIGN-SYSxxx command is being processed, but one of following errors
occurs:
- For SYSDTA or SYSIPT TO=< file name > is specified, but the
specified file does not exist.
- For SYSLST or SYSOPT or SYSOUT TO= < file name > is specified,
and the specified file already exists.
For more detailed information about DMS error enter
/HELP-MSG-INFORMATION command.

### Response

Look for the meaning of the error code, correct and
re-enter the command.

## SSM3057

Destination: CONSOLE Routing code: E Weight: 70

Warranty : NO

SSM3057 UNRECOVERABLE ERROR ON LINE '(&00)'. TERMINAL STATUS : '(&01)'

### Meaning

An unrecoverable communication error has occurred on line (&00).
(&00): Processor/station name.
(&01) : Terminal status : X'00' - terminal failed, but is now OK
X'80' - disconnected
X'40' - waits for an entry (dialog)
X'20' - break/escape mode
X'10' - IO busy
X'08' - OMNIS emulation.

## SSM3058

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3058 24-BIT SVC USED IN 31-BIT ADDRESSING MODE. PROGRAM TERMINATED ABNORMALLY

### Meaning

The SYSFILE macros with PARMOD=24 are not authorized in XS mode.

### Response

Use the macros with PARMOD=31 or load the program in no-XS mode.

## SSM3059

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3059 NEW RETURN CODE NOT PROVIDED TO OLD 24-BIT SVC CALLER. PROGRAM TERMINATED ABNORMALLY

### Meaning

A return code only supported by PARMOD=31 macros has been detected,
while PARMOD=24 macros were used. For compatibility reason,
(new return codes are not supported by old interface),
the program is terminated abnormally.

### Response

Correct and retry the program.

## SSM3060

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

SSM3060 NO DEVICE AVAILABLE FOR SWITCHING FILE FROM DISK TO TAPE/CARTRIDGE. CONTINUE? REPLY (R=RETRY (TAPE); T=TERMINATE; M=(&00))

### Response

R: The processing retries to obtain a free tape device.
T: The system file is reassigned to 'PRIMARY' or in case of
already primary file to 'DUMMY'
M: The processing (re)tries to obtain a free (&00)

## SSM3061

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3061 ILLOGICAL CONDITION ENCOUNTERED DURING ERASE OR SPOOLOUT OF SYSTEM FILES. TASK TERMINATED ABNORMALLY. CONTACT SYSTEM ADMINISTRATOR

### Meaning

The parameter list provided to SYSFILE processing is incorrect.

## SSM3063

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3063 SYSTEM ERROR DURING RESTART PROCESSING

## SSM3064

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SSM3064 SYSTEM ERROR DURING ASSIGNMENT OF A PRIMARY OUTPUT FILE (SYSOUT,SYSLST, SYSOPT)

## SSM3100

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SSM3100 S-VARIABLE '(&00)' DOESN'T EXIST

### Meaning

The Variable must be declared with the DECLARE-VARIABLE command.

## SSM3101

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SSM3101 INVALID TYPE FOR S-VARIABLE '(&00)'

### Meaning

Change type of variable or use another list variable.

## SSM3102

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3102 THE SUBSYSTEM SDF-P IS NOT AVAILABLE

## SSM3103

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3103 UNRECOVERABLE ERROR ON S-VARIABLE. SYSTEM FILE REASSIGNED TO *PRIMARY

## SSM3104

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3104 DATA-ESCAPE-CHARACTER specification other than *COMPATIBLE not allowed when SYSDTA is assigned to SYSCMD or *PRIMARY

## SSM3105

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3105 DATA-ESCAPE-CHARACTER value invalid in current software configuration

## SSM3106

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3106 Reading from SYSDTA with DATA-ESCAPE-CHARACTER specification other than *COMPATIBLE only allowed in S-procedures.

### Meaning

A previous SYSDTA assignment with DATA-ESCAPE-CHAR other than
*COMPATIBLE has been made. With this type of assignment, a RDATA
is not allowed in old-context procedures (Non-S-procedures or
batch-0)

## SSM3107

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3107 SYNTAX ERROR DURING ESCAPE CHARACTER REPLACEMENT

## SSM3108

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3108 SEMANTIC ERROR DURING ESCAPE CHARACTER REPLACEMENT

## SSM3200

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3200 AN ERROR OCCURRED DURING THE SYSFILE PLAM PROCESSING

## SSM3210

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3210 THE *LIB-ELEM(L=(&00),E=(&01)(V=(&02)),T=(&03)) CANNOT BE OPENED DUE TO PLAM ERROR (PLA(&04))

### Meaning

(&00):library name
(&01):element name
(&02):version of the element
(&03):type of the element
(&04):PLAM error code
The library-element cannot be opened.
The previous assignment is kept.
For more detailed information about the PLAM error,
enter /HELP-MSG-INFORMATION command.

## SSM3215

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3215 LIBRARY '(&00)' NOT FOUND

### Meaning

(&00):library name
The library doesn't exist.
The previous assignment is kept.

## SSM3220

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3220 THE SPECIFIED LIBRARY (&00) IS NOT A PLAM LIBRARY

### Meaning

(&00):library name
The type of the library must be PLAM.
The previous assignment is kept.

## SSM3225

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3225 THE *LIB-ELEM(L=(&00),E=(&01)(V=(&02)),T=(&03)) CANNOT BE OPENED DUE TO DMS ERROR (DMS(&04))

### Meaning

(&00):library name
(&01):element name
(&02):version of the element
(&03):type of the element
(&04):DMS error code
The library-element cannot be opened.
The previous assignment is kept.
For more detailed information about the DMS error,
enter /HELP-MSG-INFORMATION command.

## SSM3230

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3230 ELEMENT '(&01)(VERSION=(&02)),TYPE=(&03)' NOT FOUND IN LIBRARY '(&00)'

### Meaning

(&00):library name
(&01):element name
(&02):version of the element
(&03):type of the element
The element doesn't exist in the library.
The previous assignment is kept.

## SSM3235

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3235 THE *LIB-ELEM(L=(&00),E=(&01)(V=(&02)),T=(&03)) IS LOCKED

### Meaning

(&00):library name
(&01):element name
(&02):version of the element
(&03):type of the element
The library-element is locked.
The previous assignment is kept.

### Response

Retry later.

## SSM3240

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3240 THE *LIB-ELEM(L=(&00),E=(&01)(V=(&02)),T=(&03)) CANNOT BE CLOSED DUE TO DMS ERROR (DMS(&04))

### Meaning

(&00):library name
(&01):element name
(&02):version of the element
(&03):type of the element
(&04):DMS error code
The library-element cannot be closed.
For more detailed information about the DMS error,
enter /HELP-MSG-INFORMATION command.

## SSM3245

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3245 *LIB-ELEM(L=(&00),E=(&01)(V=(&02)),T=(&03)) CANNOT BE CLOSED DUE TO PLAM ERROR (PLA(&04))

### Meaning

(&00):library name
(&01):element name
(&02):version of the element
(&03):type of the element
(&04):PLAM error code
The library-element cannot be closed.
For more detailed information about the PLAM error,
enter /HELP-MSG-INFORMATION command.

## SSM3250

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3250 THE SWITCHING FROM DISK TO TAPE CANNOT BE DONE DUE TO PLAM ERROR (PLA(&00)). THE SYSTEM FILE IS REASSIGNED TO *PRIMARY

### Meaning

For more information about the PLAM error,
enter /HELP-MSG-INFORMATION command.

## SSM3252

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3252 SYSTEM ERROR DURING THE ASSIGNMENT OF THE FILE ON TAPE

## SSM3254

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3254 INSUFFICIENT SPACE ON DISK FOR THE *LIB-ELEM(L=(&00),E=(&01)(V=(&02)), T=(&03))

### Meaning

(&00):library name
(&01):element name
(&02):version of the element
(&03):type of the element
Disk saturation.

## SSM3255

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3255 THE LIBRARY-ELEMENT WILL BE COPIED AND EXTENDED ON TAPE UNDER THE NAME '(&00)'

### Meaning

(&00):tape file name
The library-element is saved on a tape file.

## SSM3256

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3256 DO YOU WANT TO COPY AND EXTEND THE LIBRARY-ELEMENT ON TAPE UNDER THE NAME '(&00)' OR TO CONTINUE ON *PRIMARY ? REPLY (T=TAPE,M=MBK,P=*PRIMARY,N=NO)

### Meaning

(&00):tape file name.
The library-element can be saved on a tape file.

### Response

T : A tape is desired.
M : A MBK is desired.
P : The system file is reassigned to *PRIMARY.
N : The system file is reassigned to *DUMMY.

## SSM3260

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3260 'FILE' PARAMETER ONLY AVAILABLE FOR DMS FILES

## SSM3280

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3280 AN ERROR OCCURRED DURING THE /COPY-SYSTEM-FILE COMMAND PROCESSING

## SSM3282

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3282 THE SYSTEM FILE IS NOT *PRIMARY. COMMAND REJECTED

### Meaning

Only a primary system file can be copied with
the /COPY-SYSTEM-FILE command.

## SSM3283

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM3283 SYSTEM FILE IS EMPTY. COMMAND IGNORED

### Meaning

A /COPY-SYSTEM-FILE command has been entered for a system
file which is currently empty.

## SSM3284

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

SSM3284 DMS ERROR (DMS(&00)) DURING PROCESSING ON FILE (&01)

### Meaning

(&00) : DMS error code
(&01) : file name on which error occurred
An error occurred during /COPY-SYSTEM-FILE
command processing.
If possible, the system file involved in the command
is reused.
Otherwise, a new primary system file is created.

## SSM4000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM4000 ENTER OR PROCEDURE FILE IS NOT OF TYPE SAM OR ISAM. COMMAND REJECTED

### Meaning

The enter or procedure file has to be a SAM or ISAM file. If not so the
command will
be rejected.

## SSM4001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM4001 ENTER OR PROCEDURE FILE RECORD FORMAT IS NOT OF VARIABLE LENGTH. COMMAND REJECTED

### Meaning

The record type of the enter or procedure file is not of variable length,
and
therefore the command is rejected.

## SSM4002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM4002 DELETE OPTION IGNORED FOR MEMBER OF LMS-LIBRARY. COMMAND PROCESSING CONTINUED

### Meaning

LMS library members cannot be deleted with option DELETE=YES of the
/ENTER-JOB command. The operand will be ignored and the processing
of the command continues.

## SSM4003

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM4003 INVALID LENGTH OF THE FIRST COMMAND IN ENTER OR PROCEDURE FILE. COMMAND REJECTED

### Meaning

The length of the first command in the specified file is too long due to
the restriction of command continuation or record contains nothing but
the isam key.

## SSM4005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM4005 INVALID FORMAT OF THE FIRST COMMAND IN ENTER OR PROCEDURE FILE. COMMAND REJECTED

### Meaning

The leading slash in a continuation record of the first command is
missing in the specified file.

## SSM4006

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SSM4006 ACCESS TO ENTER OR PROCEDURE FILE '(&00)' IN ERROR. DMS ERROR CODE '(&01)'. COMMAND REJECTED. DMS ERROR: /HELP-MSG-INFORMATION DMS(&01)

### Meaning

The data management system has detected an error when accessing
the enter or procedure file.
Therefore the command will be rejected.
&00 : Name of the enter or procedure file.
&01 : DMS error code.

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages