## DSP0001

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DSP0001 Internal error in command server

### Meaning

This message is only used as command returncode and SERSLOG ID
after preceding error message DSPFORM or DSP00RC

### Response

See preceding message

## DSP0002

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DSP0002 Internal error. Dump requested for diagnosis

### Response

Save dump file and contact your customer service

## DSP0003

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DSP0003 Command name '(&00)' invalid for DISPLAY mechanism

### Meaning

The syntax file of the subsystem DISPLAY may contain only copies of
commands starting with 'SHOW-'. Delete-display-cmd may only delete
commands starting with 'DISPLAY-'.
SHOW-USER-ATTRIBUTES is prohibited as well

## DSP0004

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DSP0004 Error when resetting privileges. Task must be terminated for security reasons

### Meaning

While executing a DISPLAY command, temporarily requested privileges could
not be returned again. To prevent misuse of this privileges, the task had
to be terminated.

## DSP0005

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DSP0005 Warning: DISPLAY command name shortened to '(&00)'. Processing continues

### Meaning

The command name resulting from replacing 'SHOW' by 'DISPLAY'
exceeds the maximum length of 30 characters and was cut therefore

### Response

Recognize the shortened name of the DISPLAY command

## DSP0006

Destination: USER-TASK Routing code: Weight:

Warranty : YES

DSP0006 Invalid format of DISPLAY command. Processing aborted

### Meaning

The DISPLAY command server was not able to find the name of the
DISPLAY command in the given SDF transfer area
Possible reasons:
- The INVARIANT-INPUT form is not given.
- The command name does not start with 'DISPLAY-'

### Response

Check syntax file of subsystem DISPLAY

## DSP0007

Destination: USER-TASK Routing code: Weight:

Warranty : YES

DSP0007 Internal error in macro call. Conmmand processing aborted

### Meaning

During execution of a DISPLAY command, an error occurred when
calling a macro

### Response

Save SERSLOG entry and inform your customer service

## DSP0008

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DSP0008 The file '(&00)' does not exist

## DSP0009

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DSP0009 Subsystem SDF-A not loaded

## DSP0010

Destination: USER-TASK Routing code: Weight:

Warranty : NO

DSP0010 The display mechanism is not applicable for commands defined with cmd-allowed=*no or commands defined with unload=*yes.

©2023 Fujitsu Technology Solutions GmbH | BS2000 System Messages