## TCP2000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP2000 (&00)-command for (&01)-server successfully completed.

### Meaning

ftp/telnet-server successfully started/stopped.

### Response

None.

## TCP2001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP2001 stop-command for (&00) SERVER has no effect.

### Meaning

no servers existing.

### Response

None.

## TCP2003

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP2003 No (&00)-server for the given Portnumber.

### Meaning

no server existing.

### Response

None.

## TCP2004

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP2004 Was not able to start procedure for (&00): (&01).

### Meaning

could not start procedure (&01) for (&00)-server

### Response

None.

## TCP5100

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP5100 (&00) SERVER VERSION (&01) STARTED.

### Meaning

TCP-IP server was started.

### Response

None.

## TCP5101

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP5101 (&00) SERVER STOPPED. REASON: '(&01)'.

### Meaning

TCP-IP server stopped.

### Response

None.

## TCP5102

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP5102 (&00) SERVER RESTARTED. REASON: '(&01)'.

### Meaning

TCP-IP server restarted.
...

### Response

None.

## TCP5103

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP5103 (&00) SERVER RESTARTED.

### Meaning

TCP-IP server restarted.

### Response

None.

## TCP5104

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP5104 OPEN ERROR ON APPLICATION '(&00)'. REASON: '(&01)'.

### Meaning

The server could not open the application.

### Response

None.

## TCP5108

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP5108 (&00)

### Response

None.

## TCP5109

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP5109 (&00),(&01): (&02)

### Response

None.

## TCP5110

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP5110 PARAMETER FILE (&00) COULD NOT BE OPENED.

### Meaning

parameterfile (&00) could not be opened.

### Response

None.

## TCP5111

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP5111 ILLEGAL COMMAND IN LINE (&00).

### Response

Correct the error and try again.

## TCP5112

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP5112 UNEXPECTED END OF FILE.

### Meaning

Missing command(s) in parameter file.

### Response

Correct the error and try again.

## TCP5113

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP5113 MEMORY ALLOCATION ERROR AT LINE (&00).

### Meaning

Memory allocation in line (&00) could not be performed.
Possible consequences:
program abortion
lost connection.

### Response

Check maximum user address space for this task and increase if
necessary.

## TCP5114

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP5114 BAD PARAMETER (&00) IN LINE (&01).

### Meaning

Incorrect parameter (&00) detected in line (&01) of parameter file.

### Response

Correct the parameter and try again.

## TCP5115

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP5115 CONFIGURATION ERROR IN LINE (&00). REASON: '(&01)'.

### Response

Correct the error and try again.

## TCP5120

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP5120 INVALID INTR COMMAND (&00).

### Response

Try again, entering the command correctly.

## TCP9000

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9000 INSTALLATION HAS BEEN COMPLETED SUCCESSFULLY

### Response

none.

## TCP9001

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9001 SELECT FUNCTION USING <MAR> AND <SEND>

### Response

Try again, selecting the function correctly.

## TCP9002

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9002 INVALID FILE NAME: (&00)

### Response

Enter correct file name and try again.

## TCP9003

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9003 INVALID PASSWORD: (&00)

### Response

Try again using the correct password.

## TCP9004

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9004 INVALID INSTALLATION KEY: (&00)

### Meaning

The installation key used was not alphanumeric.

### Response

Try again, entering a valid installation key.

## TCP9005

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9005 INVALID USER ID: (&00)

### Meaning

The specified user ID does not conform to BS2000 conventions.

### Response

Try again, entering a valid user ID.

## TCP9006

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9006 INVALID BS2000 VERSION: (&00)

### Meaning

The following BS2000 versions are permitted: 120,130.

### Response

Try again, specifying a valid BS2000 version.

## TCP9007

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9007 INVALID LOGON NAME: (&00)

### Meaning

The specified logon name was not alphanumeric.

### Response

Try again using a valid logon name.

## TCP9008

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP9008 MAXIMUM NUMBER OF CONNECTIONS SPECIFIED (&00) OUTSIDE RANGE.

### Meaning

The maximum number of connections must be between 0 and 128.

### Response

Try again using a valid number.

## TCP9009

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9009 INVALID (&01) PARAMETER: (&00)

### Meaning

For trace parameters, only values 0 through 9 are permitted.

### Response

Try again, specifying a valid number.

## TCP9010

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9010 INVALID JOB CLASS: (&00)

### Meaning

The specified job class does not conform to BS2000 conventions.

### Response

Try again using a valid job class.

## TCP9011

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9011 INVALID CPU TIME LIMIT: (&00)

### Meaning

The specified CPU time limit does not conform to BS2000 conventions.

### Response

Try again, entering a permissible value.

## TCP9012

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9012 INSERT (&00) PARAMETER(S).

### Response

Correct the error and try again.

## TCP9014

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9014 INVALID PRIORITY (&00).

### Meaning

The priority does not conform to BS2000 conventions.

### Response

Try again, specifying a valid priority.

## TCP9015

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9015 INVALID DCAM APPLICATION NAME (&00).

### Meaning

The DCAM application name does not conform to BS2000 conventions.

### Response

Try again, entering a valid name.

## TCP9016

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9016 INVALID PORT NUMBER (&00).

### Meaning

The specified port number does not conform to TCP conventions.
The number must be between 32767 and 1024.

### Response

Try again, entering a valid number.

## TCP9017

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9017 VALUE (&00) FOR MOUNT CHECK IS NOT CORRECT.

### Meaning

For the mount check, either "yes" or "no" must be entered.

### Response

Try again, entering the correct value.

## TCP9018

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9018 VALUE (&00) FOR AUTHORIZATION SERVICE IS NOT CORRECT.

### Meaning

For the authorization service, either "yes" or "no" must be entered.

### Response

Try again using a correct entry.

## TCP9020

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9020 NUMBER OF FIGURES FOR BUILDING DCAM APPLICATIONNAME (&00) IS INVALID.

### Meaning

none.

### Response

correct and retry.

## TCP9021

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9021 DEFAULT ASCII CODETABLE (&00) IS INVALID.

### Meaning

none.

### Response

correct and retry.

## TCP9022

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9022 DEFAULT EBCDIC CODETABLE (&00) IS INVALID.

### Meaning

none.

### Response

correct and retry.

## TCP9023

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9023 SDF-ERROR WHEN READING THE INSTRUCTION.

### Meaning

none.

### Response

CALL SYSTEMADMINISTRATOR.

## TCP9200

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9200 OPEN ERROR ON FILE: (&00) (DMS: (&01)).

### Meaning

The DMS error code is (&01).
The file (&00) could not be opened.

### Response

Correct the error and try again.

## TCP9201

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9201 WRITE ERROR ON INSTALLATION FILE: DMS: (&00).

### Meaning

The DMS error code is (&00).

### Response

Correct the error and try again.

## TCP9202

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9202 INSTALLATION PROGRAM AND PARAMETER FILE HAVE DIFFERENT VERSION NUMBERS.

### Meaning

The installation program and parameter file must have the same
version number.

### Response

Try again using a program and file with the same version number.

## TCP9203

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9203 FILE COMMAND NOT EXECUTED.

### Response

Correct the error and try again.

## TCP9205

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9205 INSTALLATION (&00) NOT FOUND: DMS (&01).

### Meaning

No installation has yet been stored under this key.

### Response

Try again, specifying the correct installation.

## TCP9206

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9206 ENTER FILE (&00) NOT CREATED. DMS: (&01)

### Response

Correct the error and try again.

## TCP9207

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9207 CLOSE ERROR ON INSTALLATION FILE (&00): DMS: (&01).

### Response

Correct the error and try again.

## TCP9208

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9208 MSG-Group TCP could not be initialized. Code (&00)

### Meaning

none.

### Response

CALL SYSTEMADMINISTRATOR.

## TCP9209

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9209 READ ERROR ON INSTALLATION FILE: (&00).

### Meaning

none.

### Response

Correct the error and try again.

## TCP9240

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP9240 Command SHOW-FTP-TELNET-STATUS successfully completed.

### Meaning

Command SHOW-FTP-TELNET-STATUS successfully completed.

### Response

None.

## TCP9241

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP9241 Error DMS(&00) during execution of FSTAT.

### Meaning

Possibly no Server active.

### Response

None.

## TCP9242

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP9242 Could not open configuration file (&00).

### Meaning

Desired server not active or configuration file (&00) locked.

### Response

None.

## TCP9243

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP9243 Could not read configuration file (&00).

### Meaning

File (&00) locked or empty etc.

### Response

None.

## TCP9244

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP9244 ENCRYPTION KEY is obligatory.

### Meaning

ENCRYPTION KEY is obligatory.

### Response

Type in the encryption key.

## TCP9250

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

TCP9250 VALUE "(&00)" NOT PERMITTED FOR "(&01)-(&02)".

### Response

Try again, specifying a correct value.

## TCP9260

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

TCP9260 VALUE (&00) FOR PAM-ACCOUNTING IS NOT CORRECT.

### Meaning

The value for PAM-accounting must be between 0 and 128.

### Response

Try again using a valid number.

## TCP9999

Destination: USER-TASK Routing code: Weight: 09

Warranty : NO

TCP9999 ENGLISH

### Meaning

Identifier for selected message language in BS2000.

©2024 Fujitsu | BS2000 System Messages