## SAT0000

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

SAT0000 UNRECOVERABLE ERROR IN SATCP

### Meaning

An unrecoverable error occurred when calling a system interface.
SATCP may be in an inconsistent state.

### Response

Check the SERSLOG record and contact the maintenance staff, if necessary.

## SAT0010

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

SAT0010 SATCP LOCKED BECAUSE NO SYSTEM RESOURCES AVAILABLE. TO RESUME WAITING TASKS, FOLLOW PROCEDURE FROM MESSAGE HELP TEXT. REPLY(ANY INPUT)

### Meaning

No system resources (disk space, memory) are available for storing
security relevant events.
Tasks with data records to be protocolled are placed into
a wait state. Excepted from this are tasks of the security
administrator, of the auditor and of the operator.

### Response

To lift the wait states :
1. Stop SAT logging by entering /HOLD-SAT-LOGGING
command under the user ID of the security administrator.
2. Free resources under the user ID of the SAT file
administrator or the system administrator, e.g. by
deleting files.
3. Resume SAT logging by entering
/RESUME-SAT-LOGGING command under the user ID of security
administrator. This will allow final processing of all
SAT events created already before switching off SATLOG
in Step 1.
4. If lack of disk space had been the result of
large(too big) SATLOG files, the scope of SAT logging
should be checked.

## SAT0011

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

SAT0011 TASK IN WAIT STATE DUE TO SATCP LOGGING STATE 'HOLD'. REPLY (ANY INPUT)

### Meaning

The task is just terminating, but still has data records to be
protocolled. The task termination is not continued until SATCP changes
into the protocol state and the protocol data records can be written.
Only the security administrator is allowed to take remedial action.

### Response

Security administrator: command /RESUME-SAT-LOGGING.

## SAT0012

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

SAT0012 WARNING: SAT SLOT POOL SATURATED. PROCESSING CONTINUES

### Meaning

The global memory area used for buffering events to be written
into the SATLOG file is full. Events are now buffered in task-local
memory instead.

### Response

- If this message occurs during normal ongoing operation, the number
of SAT events to be logged is too high. Please reconsider logging
selection for events, files, and users.
- If this message occurs in a specific, temporary state (e.g. while
an application accidentally loops, or while I/Os to SATLOG file
are held because splitting of mirror disks is taking place)
you may ignore it. SAT will resume logging automatically.

## SAT0013

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

SAT0013 WARNING: SAT EVENTS IN TASK-SPECIFIC BUFFERS WILL INHIBIT TERMINATION OF AFFECTED TASKS. PROCESSING CONTINUES

### Meaning

Due to a temporary shortage of memory in the past, at least one task
is still keeping SAT events in task-specific areas not accessible for
central SAT management. Termination of such tasks while SAT logging
is in hold state will issue message SAT0011 and wait until the events
can be recorded again.

### Response

Resume SAT logging as soon as possible

## SAT0040

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

SAT0040 ERROR DURING SATCP INITIALIZATION. SATCP LOGGING STATE: 'HOLD'.

### Meaning

Due to a DMS error during initialization SATCP has automatically been
placed in the logging state HOLD.
Only the security administrator and the auditor are allowed to take
remedial action.

### Response

Check the SERSLOG record and contact the maintenance staff, if necessary.

## SAT1000

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1000 USER NOT PRIVILEGED FOR COMMAND

### Meaning

The command has not been executed.

### Response

Contact the security administrator.

## SAT1010

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1010 ANOTHER SATCP COMMAND IS CURRENTLY BEING PROCESSED. RETRY COMMAND LATER

### Meaning

The SATCP commands are processed sequentially. No command may
be issued as long as another one is still being processed.

## SAT1011

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1011 TERMINATION OF SERVER TASK SATT NOT YET FINISHED. RETRY COMMAND LATER

### Meaning

A preceding HOLD-SAT-LOGGING command has initiated the termination
of the SATCP server task SATT. This process has not yet finished.
The RESUME-SAT-LOGGING command can be processed only after the
complete termination of this server task.

## SAT1012

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1012 SUBSYSTEM SATCP MUST NEITHER BE HOLD NOR STOPPED

## SAT1020

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT1020 EVENT '(&00)' ALREADY IN EVENT LIST. COMMAND REJECTED

### Meaning

Duplicate entries are not permitted in the event list.

### Response

Correct the command and try again.

## SAT1021

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT1021 ALARM '(&00)' ALREADY IN ALARM LIST. COMMAND REJECTED

### Meaning

Duplicate entries are not permitted in the alarm list.

### Response

Correct the command and try again.

## SAT1022

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT1022 FIELD '(&00)' ALREADY IN FIELD LIST. COMMAND REJECTED

### Meaning

Duplicate entries are not permitted in the field list.

### Response

Correct the command and try again.

## SAT1023

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT1023 FIELD '(&00)' CONTAINS DUPLICATE VALUES. COMMAND REJECTED

### Meaning

Duplicate entries are not permitted in the values list.

### Response

Correct the command and try again.

## SAT1024

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT1024 FIELD '(&00)' CONTAINS DUPLICATE PATTERN. COMMAND REJECTED

### Meaning

Duplicate entries are not permitted in the pattern list.

### Response

Correct the command and try again.

## SAT1025

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1025 SPECIFIED PERIOD INVALID

### Meaning

The period must be different from zero.

### Response

Correct the command and try again.

## SAT1026

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1026 SPECIFIED TIME LIMIT INVALID

### Meaning

The time limit must be different from zero.

### Response

Correct the command and try again.

## SAT1027

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT1027 ALARM '(&00)' ALREADY EXISTS. COMMAND REJECTED

### Meaning

An alarm cannot be added if it already exists.

### Response

Correct the command and try again.

## SAT1028

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT1028 ALARM '(&00)' UNKNOWN. COMMAND REJECTED

### Meaning

An alarm cannot be processed if it is unknown.

### Response

Correct the command and try again.

## SAT1029

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT1029 EVENT '(&00)' UNKNOWN. COMMAND REJECTED

### Meaning

An event cannot be processed if it is unknown.

### Response

Correct the command and try again.

## SAT1030

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT1030 USER '(&00)' ALREADY IN USER LIST. COMMAND REJECTED

### Meaning

Duplicate entries are not permitted in the user list.

### Response

Correct the command and try it again.

## SAT1031

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT1031 FILTER '(&00)' ALREADY IN FILTER LIST. COMMAND REJECTED

### Meaning

Duplicate entries are not permitted in the filter list.

### Response

Correct the command and try again.

## SAT1032

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT1032 FILTER '(&00)' ALREADY EXISTS. COMMAND REJECTED

### Meaning

An filter cannot be added if it already exists.

### Response

Correct the command and try again.

## SAT1033

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT1033 FILTER '(&00)' UNKNOWN. COMMAND REJECTED

### Meaning

An filter cannot be processed if it is unknown.

### Response

Correct the command and try again.

## SAT1034

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT1034 PATTERN '(&00)' IS WRONG. COMMAND REJECTED

### Meaning

Pattern for value contains wrong wildcard characters.

### Response

Correct the command and try it again.

## SAT1035

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT1035 INVALID VALUE FOR FIELD '(&00)'. COMMAND REJECTED

### Meaning

Dependent on the operand UNIT the following boundary conditions
are effective for the value of the field (&00):
UNIT=*BYTES: the specified value must be a multiple of 512,
UNIT=*KB : the maximum allowed for the value is 2**30 - 1,
UNIT=*MB : the maximum allowed for the value is 2**20 - 1,
UNIT=*GB : the maximum allowed for the value is 2**10 - 1.

### Response

Correct the command and try it again.

## SAT1040

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT1040 INFORMATION '(&00)' ALREADY IN INFORMATION LIST. COMMAND REJECTED

### Meaning

Duplicate entries are not permitted in the information list.

### Response

Correct the command and try it again.

## SAT1050

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1050 COMMAND PERMITTED ONLY IF SAT LOGGING FUNCTION IS ACTIVATED

### Meaning

The command cannot be executed unless the SAT logging file is open
and SATCP has the necessary resources.

### Response

Open a SAT logging file and retry the command.

## SAT1060

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1060 LIST OF INFORMATION TO BE DISPLAYED IS EMPTY

### Response

Correct the command and try it again.

## SAT1070

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1070 ALARMS TABLE EMPTY. COMMAND REJECTED

### Meaning

Only alarms written in the alarm table can be processed.

## SAT1071

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1071 ALARMS TABLE FULL. COMMAND REJECTED

### Meaning

A new alarm cannot be added if the alarm table is full.

## SAT1072

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1072 FILTER TABLE EMPTY. COMMAND REJECTED

### Meaning

Only filter written in the filter table can be processed.

## SAT1073

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1073 FILTER TABLE FULL. COMMAND REJECTED

### Meaning

A new filter cannot be added if the filter table is full.

## SAT1074

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1074 NO ALARM DEFINED PER DEFAULT. COMMAND REJECTED

## SAT1075

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1075 NO ALARM DEFINED IN SAT PARAMETER FILE. COMMAND REJECTED

## SAT1076

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1076 NO FILTER DEFINED PER DEFAULT. COMMAND REJECTED

## SAT1077

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1077 NO FILTER DEFINED IN SAT PARAMETER FILE. COMMAND REJECTED

## SAT1078

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1078 Pubset for SATLOG file must be imported exclusively. Shared pubset '(&00)' ignored

## SAT1080

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1080 A SATCP EXCHANGE IS CURRENTLY BEING PROCESSED. RETRY COMMAND LATER

### Meaning

No command may be issued as long as a SATCP exchange is being
processed.

## SAT1081

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1081 SATCP ERROR '(&00)' DURING SUBSYSTEM EXCHANGE. COMMAND REJECTED. FURTHER INFORMATION: /HELP-MSG (&00)

### Meaning

The currently running SATCP rejects an exchange because
an error occured.
For more detailed information about the SAT error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages' or one of the
BS2000 SECOS manuals.

## SAT1082

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT1082 EXCHANGE REJECTED BECAUSE NEW SATCP VERSION IS NOT COMPATIBLE WITH CURRENT ONE

### Meaning

The currently running SATCP rejects an exchange because
the new subsystem version is not compatible with the current one.

## SAT2000

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT2000 SATCP LOGGING FUNCTION ALREADY ACTIVATED

## SAT2010

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT2010 SATCP LOGGING FUNCTION ALREADY IN HOLD STATE

## SAT2030

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

SAT2030 DMS ERROR '(&00)' WHEN OPENING FILE '(&01)'. FURTHER INFORMATION: /HELP-MSG DMS(&00)

### Meaning

A DMS error prevents a new file from being opened.
Logging continues in the currently opened file.
For more detailed information about the DMS error code enter /HELP-MSG
or see the BS2000 manual 'System Messages' or one of the
BS2000 DMS manuals.

### Response

Take the appropriate action in accordance with the DMS error code and
then try again.

## SAT2031

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT2031 DMS ERROR '(&00)' WHEN CLOSING FILE '(&01)'. FURTHER INFORMATION: /HELP-MSG DMS(&00)

### Meaning

Due to a DMS error at least one of the following actions
could not be performed:
- The SATLOG file could not be closed.
- No release of storage space could be performed for the closed file.
- The closed file could not be set to ACCESS=READ.
For more detailed information about the DMS error code enter /HELP-MSG
or see the BS2000 manual 'System Messages' or one of the
BS2000 DMS manuals.

### Response

Take the appropriate action in accordance with the DMS error code.

## SAT2040

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

SAT2040 DMS ERROR '(&00)' WHEN CREATING CATALOG ENTRY FOR FILE '(&01)'. FURTHER INFORMATION: /HELP-MSG DMS(&00)

### Meaning

A DMS error prevents a new SATLOG file from being catalogued on the
pubset specified in the filename (&01).
This may happen if either the pubset specified in the SAT parameter
file or the default pubset of SYSAUDIT user ID is different from the
home pubset (and this pubset e.g. is not yet imported).
SAT will try to create a SATLOG file on the home pubset instead.
For more detailed information about the DMS error code enter /HELP-MSG
or see the BS2000 manual 'System Messages' or one of the
BS2000 DMS manuals.

### Response

Take the appropriate action in accordance with the DMS error code and
then try again.

## SAT2100

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 80

Warranty : YES

SAT2100 SAT LOGGING FILE = '(&00)' OPENED

### Meaning

A new SAT logging file has been opened by means of the /CHANGE-SAT-FILE
command or as a result of an automatic switch.

## SAT2110

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 80

Warranty : YES

SAT2110 SAT LOGGING FILE = '(&00)' CLOSED

### Meaning

The command has been successfully processed.

## SAT2200

Destination: CONSOLE Routing code: * (main console) Weight: 98

Warranty : NO

SAT2200 ALARM '(&00)' TRIGGERED OFF FOR EVENT '(&01)' AND USER '(&02)'

### Meaning

An alarm is currently triggered off.

### Response

Contact the security administrator.
The security administrator must analyse the reason
of the alarm and decide whether the task may continue

## SAT3021

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT3021 WARNING: EVENT '(&00)' NOT PROCESSED BECAUSE UNKNOWN

## SAT3022

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT3022 WARNING: EVENT '(&00)' NOT PROCESSED BECAUSE NOT SWITCHABLE

### Meaning

Preselection of the specified event cannot be changed.

## SAT3023

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT3023 TOO MANY INVALID EVENTS FOR WARNING LIST

### Meaning

The number of warnings exceeds the maximum area available to accommodate
them, with the result that the list of warnings is incomplete.

## SAT3031

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT3031 WARNING: USERID '(&00)' NOT PROCESSED BECAUSE UNKNOWN

## SAT3032

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT3032 WARNING: USERID '(&00)' NOT PROCESSED BECAUSE NOT SWITCHABLE

### Meaning

Preselection of the specified user cannot be changed.

## SAT3033

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT3033 TOO MANY INVALID USERIDS FOR WARNING LIST

### Meaning

The number of warnings exceeds the maximum area available to accommodate
them, with the result that the list of warnings is incomplete.

## SAT3034

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT3034 WARNING: USERID '(&00)' UNKNOWN

### Meaning

The userid is normally processed.

## SAT3035

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT3035 WARNING: ALARM WILL NEVER TRIGGER OFF ANY ACTION

### Meaning

The alarm can never be triggered off.

### Response

Correct the command and try it again.

## SAT3036

Destination: USER-TASK Routing code: Weight:

Warranty : YES

SAT3036 WARNING: FILTER WILL NEVER TRIGGER OFF ANY ACTION

### Meaning

The filter can never be triggered off.

### Response

Correct the command and try it again.

## SAT3040

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 80

Warranty : YES

SAT3040 WARNING: INTERNAL ERROR. SPECIFIED PERIOD NOT PROCESSED

### Meaning

The specified period cannot be changed.

### Response

Check the SERSLOG record and contact the maintenance staff, if necessary,
or try again.

## SAT4000

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 80

Warranty : NO

SAT4000 UNRECOVERABLE ERROR WHEN SAVING OR RESTORING THE SAT PARAMETERS

### Meaning

An unrecoverable error occurred when calling a system interface.
The function 'save/restore of SAT parameters' is not available
at the moment.
For a more detailed diagnosis an entry has been written into
the SERSLOG file.
The SAT logging is not concerned by this error.

## SAT4010

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SAT4010 SAT PARAMETER FILE NOT AVAILABLE AT THE MOMENT

### Meaning

Due to a problem during the start or the exchange of the subsystem
SATCP the SAT parameter file is not available.

### Response

Contact the system administration to find out the reason of the problem
concerning the SAT parameter file.

## SAT4030

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

SAT4030 WARNING: VERIFICATION OF THE SAT ALARM AND FILTER CONDITIONS NECESSARY BY THE SECURITY ADMINISTRATOR

### Meaning

The SAT alarm and filter conditions should be checked for the occurrence
of the SAT data fields FILPOS, CURLIM and MAXLIM.
Reason:
- The field FILPOS has changed its unit since SATCP 4.0B.
It contains now multiple of 512.
A SAT alarm or filter condition in the SAT parameter file
contained a specification for FILPOS, which is not exactly
divisible by 512. This value was converted to the next
multiple of 512 less than the original value.
- Since SATCP 4.0B the new fields CURLIM2 and MAXLIM2 are protocolled
instead of CURLIM and MAXLIM whenever the event XSR occurs and
the field RESOURC has the value FILE-SIZE.
Unlike CURLIM and MAXLIM the fields CURLIM2 and MAXLIM2 contain
multiple of 512.
A SAT alarm or filter condition in the SAT parameter file
contains a specification for CURLIM and/or MAXLIM.
This specification has been taken over unchanged, because the system
cannot decide whether a conversion has to be performed.

### Response

Verify the alarm resp. filter conditions and modify them, if necessary

## SAT4040

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 80

Warranty : YES

SAT4040 DMS ERROR '(&00)' IN FILE '(&01)'. FURTHER INFORMATION: /HELP-MSG DMS(&00)

### Meaning

Due to a DMS error on the SAT parameter file the desired function
cannot be executed.
The function 'save/restore of SAT parameters' is not available
at the moment.
For more detailed information about the DMS error code enter /HELP-MSG
or see the BS2000 manual 'System Messages'.
For a more detailed diagnosis an entry has been written into
the SERSLOG file.
The SAT logging is not concerned by this error.

### Response

Take the appropriate action in accordance with the DMS error code and
then try again.
If necessary, catalogue the defective SAT parameter file under another
name and make it available to the maintenance staff.

## SAT4042

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 80

Warranty : NO

SAT4042 SAT PARAMETER FILE INVALID

### Meaning

A check error occurred on the SAT parameter file.
The function 'save/restore of SAT parameters' is not available
at the moment.
For a more detailed diagnosis an entry has been written into
the SERSLOG file.
The SAT logging is not concerned by this error.

### Response

If necessary, catalogue the defective SAT parameter file under another
name and make it available to the maintenance staff.

## SAT4043

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 80

Warranty : NO

SAT4043 ABNORMAL TERMINATION OF SATP TASK

### Meaning

The system task SATP performs the access to the SAT parameter file.
The function 'save/restore of SAT parameters' is not available
at the moment.
For a more detailed diagnosis an entry has been written into
the SERSLOG file.
The SAT logging is not concerned by this error.

## SAT4044

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 80

Warranty : NO

SAT4044 ERROR DURING INITIALIZATION OF SATP TASK

### Meaning

The system task SATP performs the access to the SAT parameter file.
The function 'save/restore of SAT parameters' is not available
at the moment.
For a more detailed diagnosis an entry has been written into
the SERSLOG file.
The SAT logging is not concerned by this error.

## SAT4045

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 80

Warranty : NO

SAT4045 RESTART OF SYSTEM TASK SATP IMPOSSIBLE AT THE MOMENT

### Meaning

The system task SATP performs the access to the SAT parameter file.
At an exchange of the subsystem SATCP the system task SATP is terminated
during the deactivation of the subsystem version to be replaced;
at the start of the subsystem version to be activated this task is newly
created again.
The creation of a new SATP task was impossible, because the termination
of the old SATP task initiated before had not yet been finished.
The function 'save/restore of SAT parameters' is not available
at the moment.
The SAT logging is not concerned by this error.

### Response

Enter the command /SAVE-SAT-PARAMETERS with at least one operand
under the userid of the security administrator to initiate in that way
implicitly a restart of the SATP task.

## SAT4100

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

SAT4100 SAT PARAMETER FILE OPENED

### Meaning

The SAT parameter file is successfully opened.

## SAT4110

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

SAT4110 SAT PARAMETER FILE CLOSED

### Meaning

The SAT parameter file is successfully closed.

## SAT4200

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 80

Warranty : YES

SAT4200 WARNING: CHECK ERROR ON 'NEXT-SESSION' VALUE OF PARAMETER '(&00)'

### Meaning

An inconsistency has been found in the SAT parameter file,
concerning the NEXT-SESSION value of the given parameter.
The standard value for this parameter is taken as NEXT-SESSION value.

## SAT4220

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 80

Warranty : YES

SAT4220 ERROR AT RESTORING OF PREVIOUSLY SAVED VALUES. STANDARD VALUES TAKEN FOR PARAMETER '(&00)'

## SAT4300

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 80

Warranty : NO

SAT4300 ERROR DURING INITIALIZATION OF FUNCTION 'SAVE/RESTORE OF SAT PARAMETERS'

### Meaning

An error occurred preventing the successful initialization of the
function 'save/restore of SAT parameters'.
The function 'save/restore of SAT parameters' is not available
at the moment.
The SAT logging is not concerned by this error.

## SAT5000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SAT5000 INTERNAL ERROR. SERSLOG ENTRY CREATED. CONTACT SYSTEM ADMINISTRATOR

### Meaning

For a more detailed diagnosis an entry has been written into
the SERSLOG file.

### Response

The system administrator should analyze the SERSLOG entries SAT0000.

## SAT5001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SAT5001 INSUFFICIENT SPACE FOR SYSLST FILE

### Meaning

SYSLST is assigned to a cataloged file the PRIMARY-ALLOCATION of which
is exhausted and the SECONDARY-ALLOCATION of which is set to 0.

### Response

Increase the value of either the PRIMARY-ALLOCATION or
the SECONDARY-ALLOCATION.

©2024 Fujitsu | BS2000 System Messages