## MCS0001

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS0001 Subsystem 'MSCF' does not exist in 'DSSM' subsystem catalog. Command not processed

### Response

If desired, enter the declaration of the subsystem MSCF in the subsystem
catalog and prepare the subsystem configuration.

## MCS0002

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS0002 Subsystem 'MSCF' not loaded. Command rejected

### Response

At first, create the MSCF subsystem by means of the command
START-SUBSYSTEM SUBSYS=MSCF and then try the command again.

## MCS0003

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS0003 Subsystem 'MSCF' is being loaded. Try command later

### Response

Wait until the message "MCS0011 Subsystem 'MSCF' loaded ........" is
displayed on the console.

## MCS0004

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS0004 Subsystem 'MSCF' is being unloaded. Try command later

### Response

Wait until the message "MCS0012 Subsystem 'MSCF' unloaded ........" is
displayed on the console.
Then try command START-SUBSYSTEM SUBSYS=MSCF again.

## MCS0006

Destination: USER-TASK, CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS0006 Syntax error. Command '(&00)' not processed

### Meaning

(&00): definition of command.
Syntactical invalid option in command MRSSTART, MRSMOD, MRSEND, MRSSTA
or in the STRING operand of command START-SUBSYSTEM SUBSYS=MSCF or
STOP-SUBSYSTEM SUBSYS=MSCF.

### Response

Try the command again with the correct syntax.

## MCS0007

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0007 MSCF communication not initialized successfully. Error code '(&00)'

### Meaning

(&00): 01: Error when reading the system ID (e.g. dummy sys ID 250) or the
BS2000 version number.
03: Error when creating the SERVER bourse.
04: Error when creating the REPLY bourse.
05: Error when collecting BCAM requests.
06: Error when opening BCAM applications $MRSAPP/$MRSAPPS.
07: Error when creating the MSCF host table.
08: Error when rejecting BCAM requests.
09: The MSCF configuration file is incorrect:
- file is empty or
- file contains more entries than the maximum value allows or
- there is an entry with invalid syntax.
10: The MSCF configuration file is incorrect:
Double definition of entries.
11: The MSCF configuration file is incorrect:
No valid entry for local host.
12: Error when creating an MSCF host table entry.
13: Error when creating an MSCF server task.
14: Error when calling MSCF connection control.
15: Internal error.
16: Internal error.
17: Internal error.
18: Internal error.
19: XCS not allowed.
DMS error: Error in the processing of the MSCF configuration file.
The DMS error is identified by the 4-character DMS error code.
For more detailed information about the DMS error code, enter
/HELP-MSG DMS(&00) in system mode or see the BS2000 manual
'System Messages'.

### Response

01, 03, 04, 05, 07, 08:
contact the system administrator.
09, 10, 11, 12, DMS error:
retry the command START-SUBSYSTEM SUBSYS=MSCF with the correct
MSCF configuration file or take appropriate steps in accordance with
the DMS error code.
06:
if the message 'MCS0008' appears on the console, activate BCAM and try
the command START-SUBSYSTEM SUBSYS=MSCF again else contact the
BS2000 system administrator.
13, 14, 15, 16, 17, 18, 19:
contact the BS2000 system administrator.

## MCS0008

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0008 BCAM not yet started for MSCF communication

### Response

Start BCAM and try the command START-SUBSYSTEM SUBSYS=MSCF again.

## MCS0009

Destination: CONSOLE Routing code: R Weight: 99

Warranty : YES

MCS0009 MSCF CONNECTION TO HOST '(&00)' NOT ACCEPTED, ERROR CODE '(&01)'

### Meaning

The attempt to establish an MSCF connection to host (&00) is not accepted.
(&00): Processor name of remote host
(&01): reasons for the rejection:
01: MSCF not active on host (&00) (cf. remark).
02: MSCF on host (&00) does not know the Processor name of the
local host.
03: Host (&00) unknown in BCAM network or there is no BCAM
connection to host (&00) (cf. remark).
04: BCAM timeout because of fault in connection to host (&00)
(cf. remark).
05: An attempt is made to set up a connection to the local host.
08: The same system ID occurs more than once in a planned network.
09: Internal error (cf. remark). Possibly the BCMAP command was
not performed.
10: The request to include host (&00) in a closely or loosely
coupled system is rejected. Reason: there is an inconsistency
in using different coupling types or the password comparison
is negative or passwords were given for a loosely coupled
connection.
11: The request to include host (&00) in a closely coupled system
is rejected. Reason: given password for local host is invalid.
12: The minimum message length to be supported by BCAM is
insufficient. 8 kB are required.
13: There is an inconsistency concerning BCAM network (cf. remark).
14: Internal error from remote host (&00).
15: MSCF of the remote host (&00) has a version < V10.0
(cf. remark).
16: MSCF of the remote host (&00) cannot be coupled with the local
version of MSCF.
17: The host (&00) is not longer known on local host.
18: Inconsistent MSCF connection.
19: BCAM connection request pending.
20: The same host name occurs more than once in a planned network.
21: An MSCF connection to a CCS partner is not allowed
during XCS start.
The command will be executed by MSCF internally as soon as
possible.
22: The BCAM route, which is used for the MSCF connection to the
host (&00), does not support the required functionality in its
entirety.
23: Connection request rejected by configuration management of
local host. The reason is indicated in message MCS1005.
24: Connection request rejected by configuration management of
host (&00). The reason is indicated in message MCS1005
on host (&00).
25: The remote host (&00) too tries to establish the MSCF
connection.
26: Wrong REMOTE-PASSWORD in command /START-MSCF-CONNECTION on
local host or remote host (&00).
27: Error during initial internal communication.
28: Configuration error. The reason is indicated in message MCS1005
on host (&00).
Remark: In the case of reasons marked with '(cf. remark)' possibly the
remote host as well tries to establish an MSCF connection.

### Response

01: Load subsystem MSCF on host (&00).
02: Enter START-MSCF-CONNECTION PROCESSOR-NAME=<local>
on host (&00)
(<local> means the processor name of the local host).
03: Enter the command again with the correct processor name or
enter the appropriate /BCIN commands.
04, 13, 14:
Continue with the attempt to establish an MSCF connection.
If it is unsuccessful, contact the network administrator.
05: Enter the command again with the correct processor name.
08, 16, 20, 27:
Contact the system administrator.
09: Check whether correct BCMAP commands were entered at the local host
and at host (&00) for all MSCF applications. If necessary, enter
corrected BCMAP commands and repeat command /START-MSCF-CONNECTION.
If message MCS0050 has occurred, destroy connection by call of
/BCCONN command and repeat command /START-MSCF-CONNECTION.
If not successful, contact the network administrator.
10, 26:
Enter the command again with correct data, if necessary also on
remote host (&00).
11: Enter the command again with correct data.
12: Contact the network administrator.
17: Enter START-MSCF-CONNECTION on local host.
18: Continue with the attempt to set up an MSCF connection.
19: Continue with the attempt to set up an MSCF connection after waiting
for timeout of BCAM.
22: Enter command BCMAP for the MSCF applications on the local host
and on host (&00) and try command again.
25: If the MSCF connection is not established by the remote host enter
the command again.

## MCS0010

Destination: CONSOLE Routing code: R Weight: 99

Warranty : YES

MCS0010 MSCF connection to host '(&00)' accepted

### Meaning

(&00): Processor name of remote host.

## MCS0011

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0011 Subsystem MSCF loaded and MSCF communication activated. (&00) server tasks created

### Meaning

(&00): number of created MSCF server tasks.

## MCS0012

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0012 Subsystem MSCF unloaded and MSCF communication terminated on local host

## MCS0013

Destination: CONSOLE Routing code: R Weight: 99

Warranty : YES

MCS0013 MSCF connection request from host '(&00)' accepted

### Meaning

The request from host (&00) to establish an MSCF connection to the local
host has been accepted.
(&00): Processor name of remote host.

## MCS0014

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0014 MSCF connection with host '(&00)' no longer available

### Meaning

Possible reasons:
- command STOP-MSCF-CONNECTION PROCESSOR-NAME=<local> or
STOP-SUBSYSTEM SUBSYS=MSCF has been entered on host (&00)
(<local> stands for the processor name of the local host).
- the BCAM connection to host (&00) has been closed by BCAM command BCOUT
or BCEND.
- Unrecoverable network disruption.
(&00): Processor name of remote host.

## MCS0015

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0015 MSCF connection with host '(&00)' disconnected

### Meaning

(&00): Processor name of remote host.

## MCS0016

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0016 Host '(&00)' not connected

### Meaning

(&00): Processor name of remote host.

## MCS0017

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0017 Host '(&00)' already connected. Command rejected

### Meaning

(&00): Processor name of remote host.

## MCS0018

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0018 Connection interrupted with host '(&00)', but recovered, initiated by '(&01)'

### Meaning

A connection interrupt occurred but was recovered.
MSCF messages sent during the connection interrupt may be lost.
(&00): Processor name of remote host.
(&01): 01: initiated by local host
02: initiated by remote host

## MCS0019

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0019 Number of created MSCF server tasks increased to '(&00)'

### Meaning

The number of MSCF server tasks has been increased to &00 to avoid a
deadlock situation. Possible reasons:
- Excessive load on a slave partner.
- System error (MSCF user).

### Response

Contact the BS2000 system administrator.

## MCS0021

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0021 LOCAL host belongs to shared pubset or XCS configuration. Command '(&00)' rejected

### Response

To force execution of the command, reenter the command
STOP-MSCF-CONNECTION with operand FORCED=YES or the command
STOP-SUBSYSTEM MSCF with operand SUBSYSTEM-PARAMETER='FORCED=YES'.
However, this may have repercussions on applications on another host in
the shared pubset or XCS configuration.
(&00): command STOP-MSCF-CONNECTION or STOP-SUBSYSTEM SUBSYS=MSCF.

## MCS0022

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0022 SYSID '(&00)' not in permissible range. Command not processed

### Meaning

The system identifier specified in MSCF command SHOW-MRS-CONNECTIONS
is not in the range A,...,Z,0,....,9,65,...,192.
(&00): system identifier.

### Response

Reenter command SHOW-MRS-CONNECTIONS with a valid system identifier.

## MCS0023

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0023 Warning: Number of server tasks requested by /START-SUBSYSTEM not in range 2 through (&00). Value from configuration file or default value '4' will be assumed

## MCS0024

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0024 (&00) entries written to serslog file during recent MSCF session

### Meaning

Due to internal errors in the MSCF communication,
(&00) error records have been written to the SERSLOG file
during the recent MSCF session.

### Response

For error diagnosis, consult the SERSLOG file.

## MCS0025

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0025 Error during processing of command '(&00)'. Processing of command aborted

### Meaning

An error occurred during processing of command (&00). Further hints in
Serslog file.

### Response

Contact the system administrator.

## MCS0027

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

MCS0027 Internal MSCF error. MSCF communication terminated. Serslog entry written

### Response

If the error persists, contact the BS2000 system administrator.

## MCS0029

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

MCS0029 File '(&00)' will be used as MSCF configuration file

## MCS0030

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

MCS0030 File '(&00)' is used as MSCF trace file

## MCS0031

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

MCS0031 File '(&00)' is no longer used as MSCF trace file

## MCS0032

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

MCS0032 The command /SET-MSCF-ENVIRONMENT is only allowed in an MSCF configuration file

## MCS0033

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

MCS0033 Operand RECOVERY-START ignored for partner '(&00)'

### Meaning

Operand RECOVERY-START of command START-MSCF-CONNECTION is not defined for
partners with an MSCF version less than V12.0.
(&00): Processor name of partner.

## MCS0035

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0035 Command '(&00)' for host '(&01)' is still processed, command '(&02)' rejected

### Meaning

(&00): START-MSCF-CONNECTION or STOP-MSCF-CONNECTION
(&01): Processor name of the remote host
(&02): START-MSCF-CONNECTION or STOP-MSCF-CONNECTION

## MCS0036

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0036 Command '(&00)' not allowed for subsystem MSCF. Use command '(&01)' instead

### Meaning

(&00): HOLD-SUBSYSTEM
(&01): STOP-SUBSYSTEM

## MCS0037

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0037 Error in management of trace file '(&00)', reason '(&01)'

### Meaning

(&00): Name of the MSCF trace file.
(&01): Error reason:
01: The assigned user id is unknown.
02: The assigned pubset
- has no MRSCAT entry or
- is not imported exclusively.
03: Internal error when checking user id.
04: Internal error when checking MRSCAT entry.
05: MSCF task not ready to perform this task.
DMS0XXX: DMS error code. For more detailed information enter command
/HELP-MSG (&01).

### Response

01, 02: Correct and reenter the command resp. import the pubset
exclusively.
03, 04, 05: Contact the system administrator.

## MCS0038

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0038 Command 'MODIFY-MSCF-CONNECTION PROCESSOR-NAME=(&00) ...' rejected, reason '(&01)'

### Meaning

Command MODIFY-MSCF-CONNECTION for host (&00) rejected.
(&00): Processor name of the remote host.
(&01): Reason:
01: Specification of local host is not allowed.
02: Remote host is unknown.
03: Remote host is not connected.
04: Connection type is not CCS.
05: MSCF version of remote host is less than V14.0.
06: Internal error.

### Response

03: Use command /START-MSCF-CONNECTION instead.

## MCS0039

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0039 Second control connection noted for host '(&00)'

### Meaning

The second MSCF control connection will be established, as soon as it is
requested by the remote host.
(&00): Processor name of the remote host.

## MCS0040

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0040 Application '(&00)' established MSCF control connection to host '(&01)'. Control connections: '(&02)'

### Meaning

The local host established a MSCF control connection to a remote host.
(&00): Application name of control connection.
(&01): Processor name of the remote host.
(&02): Number of active control connections including the new connection:

## MCS0043

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0043 Application '(&00)' accepted MSCF control connection by host '(&01)'. Control connections: '(&02)'

### Meaning

A remote host established a MSCF control connection to the local host.
(&00): Application name of control connection.
(&01): Processor name of the remote host.
(&02): Number of active control connections including the new connection.

## MCS0044

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0044 Application '(&00)' lost MSCF control connection to host '(&01)'. Control connections: '(&02)'

### Meaning

A MSCF control connection has been closed or was lost.
(&00): Application name of control connection.
(&01): Processor name of the remote host.
(&02): Number of active control connections after the current loss.

## MCS0048

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS0048 MSCF control connection '(&00)' interrupted with host '(&01)', but recovered, initiated by '(&02)'

### Meaning

A temporarily interrupted control connection has recovered.
(&00): Application name of control connection.
(&01): Processor name of remote host.
(&02): 01: initiated by local host
02: initiated by remote host

## MCS0049

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS0049 MSCF connection with host '(&00)' interrupted, recovery started

### Meaning

An attempt is made to re-establish interrupted MSCF connection.
(&00): Processor name of remote host.

## MCS0050

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS0050 BCAM connection to host '(&00)' already established

### Meaning

BCAM connection to remote host already established.
(&00): Processor name of remote host.

### Response

Destroy BCAM connection with BCAM command (/BCCONN) and
re-establish MSCF connection with command /START-MSCF-CONNECTION.

## MCS0059

Destination: CONSOLE Routing code: R Weight: 99

Warranty : YES

MCS0059 MSCF connection from host '(&00)' not accepted, Error code '(&01)'

### Meaning

The attempt to establish an MSCF connection from host (&00) is not
accepted.
(&00): Processor name of remote host
(&01): reasons for the rejection:
02: MSCF on local host does not know the processor name of the
remote host (&00).
08: The same system ID occurs more than once in a planned network.
09: Internal error.
10: The request of host (&00) to include the local host in a
closely or loosely coupled system is rejected. Reason: there
is an inconsistency in using different coupling types or the
password comparison is negative or passwords were given for a
loosely coupled connection.
12: The minimum message length to be supported by BCAM is
insufficient. 8 kB are required.
14: Internal error in remote host (&00).
16: MSCF of the remote host (&00) cannot be coupled with the local
version of MSCF.
18: Inconsistent MSCF connection.
20: The same host name occurs more than once in a planned network.
21: An MSCF connection to a CCS partner is not allowed
during XCS start.
The command will be executed by MSCF internally as soon as
possible.
23: Connection request rejected by configuration management of
host (&00). The reason is indicated in message MCS1005
on host (&00).
24: Connection request from Host (&00) rejected by configuration
management of local host. The reason is indicated in message
MCS1005.
26: Wrong REMOTE-PASSWORD in command /START-MSCF-CONNECTION on
local host or remote host (&00).
27: Error during initial internal communication.
28: Configuration error. The reason is indicated in message
MCS1005.

### Response

02: Enter START-MSCF-CONNECTION PROCESSOR-NAME=(&00)
at local host.
08, 16, 20, 27:
Contact the system administrator.
09: Continue with the attempt to establish an MSCF connection.
If not successful, contact the network administrator.
10, 26:
Enter the command again with correct data, if necessary also on
remote host (&00).
12: Contact the network administrator.
14: Continue with the attempt to establish an MSCF connection.
If it is unsuccessful, contact the network administrator.
18: Continue with the attempt to set up an MSCF connection.

## MCS0999

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS0999 Unexpected situation in MSCF-C processing, error logged in SERSLOG file

## MCS1001

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1001 Local MSCF configuration parameter '(&00)' changed from '(&01)' to '(&02)'

### Meaning

A local MSCF configuration parameter has been modified via command
/MODIFY-MSCF-ENVIRONMENT.
(&00): Name of the modified parameter.
(&01): Old value.
(&02): New value.

## MCS1002

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1002 Global MSCF configuration parameter '(&00)' changed from '(&01)' to '(&02)'

### Meaning

A globally effective MSCF configuration parameter has been modified via
command /MODIFY-MSCF-ENVIRONMENT. The modification came into effect on the
local host and all connected partners.
(&00): Name of the modified parameter.
(&01): Old value.
(&02): New value.

## MCS1003

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1003 Abort of MSCF. Error code: '(&00)'

### Meaning

The host aborts MSCF. The error code (&00) classifies the possible
reasons. More detailed information about the reason of the abort can be
obtained through analysis of the CONSLOG and SERSLOG files.
(&00): Meaning of the error codes.
1: A CCS or XCS partner has been detected mistakenly as crashed.
Cf. message MCS1004.
2: Internal error: Invalid flow of control.
3: Internal error: Invalid control data.
4: Internal error: Error in monitoring protocol.
5: Total loss of communication.
6: Total loss of disk monitoring.
7: Error when requesting necessary resources (e.g. shortage of
memory or mandatory registered function not available).
8: Internal error: Program error.
9: Error in registered function or its interface. Cf. messages
MCS1007 or MCS1008 in CONSLOG.
10: Error in XCS occupation management: USER TERM LIMIT elapsed or
internal error.
11: The current XCS reconfiguration is terminated abnormally because
XCS is interrupted.
12: The partner named in message MCS1009 realized the interruption
of XCS quicker than the host and initiated the abort of the
current XCS reconfiguration.
13: Internal error. XCS configuration inconsistent.
14: The start of the leave reconfiguration was blocked for more
than 10 minutes by another reconfiguration. The leave is
therefore replaced by an abort.
15: Partners with identical names in different XCS' with the same
name.
16: LEAVE LIMIT elapsed. The leave is replaced by an abort.
17: XCS interrupted by loss of connection. In order to get rid of
the interruption, the XCS member with the lower HOST PRIORITY is
aborted.
99: Abort requested by operator.

### Response

1: After the abort of MSCF has been finished reload subsystem MSCF and
restart affected applications using a consistent database.
2, 3, 4, 8, 13:
Inform system administrator.
5, 6, 7, 11, 12, 13, 15, 17:
After elimination of the cause of the error, reload subsystem MSCF.
9: Look for messages of the registered function referred to by a
preceding message MCS1007 or MCS1008. Use these messages to narrow
down the cause of the error. After elimination of the cause of the
error reload subsystem MSCF. If not successful, inform the system
administrator.
10: In case USER TERM LIMIT has elapsed this is a normal reaction.
In other cases, inform system administrator.
14, 16:
These are normal reactions, no response required.
16: If necessary adjust the parameter LEAVE-LIMIT by means of command
SET-MSCF-ENVIRONMENT in the MSCF configuration file.

## MCS1004

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1004 Erroneous crash detection of partner '(&00)'. Data inconsistencies must be assumed

### Meaning

The remote partner is considered as crashed and the remaining XCS or
shared pubset configuration is reconfigured. The partner became active
again within the same MSCF session revealing the crash detection as
erroneous. An abort of subsystem MSCF is initiated. Data inconsistencies
within XCS or shared pubset applications must be taken into account.
(&00): Host name of the remote partner.
Possible reasons:
- Wrong MSCF configuration parameter settings.
- Faulty operating.

### Response

After abort of MSCF has been finished, reload subsystem MSCF and restart
affected applications using a consistent database.

## MCS1005

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1005 Configuration failure. Partner '(&00)' is rejected, reason: '(&01)'

### Meaning

(&00): Processor name of rejected partner.
(&01): Reason for rejection of partner:
1: During join of host to XCS connections to CCS partners cannot be
established.
2: Two partners have the same host name.
3: Partner declared as crashed.
4: Internal Error.
5: Shortage of memory.
6: Two different XCS are using the same XCS name.
7: Invalid control protocol sequence.
8: FAIL DETECTION LIMIT not compatible.
9: RECOVERY START not compatible.
11: SYSID already used by another partner.

## MCS1006

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1006 Reconfiguration time limit exceeded by registered function '(&00)'. Reconfiguration: '(&01)'

### Meaning

Reconfiguration of a registered function lasts longer than expected.
(&00): Registered function.
NSM Node Synchronization Manager.
XTS XCS Time Synchronization.
XPM XCS Pubset Management.
GSM Global Storage Manager.
NSG Node Synchronization - Global storage part.
GSV Global Storage Volume emulation.
CPM CCS Pubset Management.
DAB Disk Access Buffer.
SHC Symmetrix Host Component.
(&01): identification of reconfiguration.
*INIT: Local initialization.
*START: Global initialization.
*TERM-LOCAL: Local termination.
*TERM-GLOBAL: Global termination.
*ABORT-LOCAL: Local termination when aborting.
*ABORT-GLOBAL: Global termination when aborting.
PARTNER=<host name>: Abort of partner <host name> (CCS).
#<number>: <number> = reconfiguration number of destination
reconfiguration (XCS).
Possible reasons:
- The setting of fail detection interval is too small.
- Because of an extraordinary situation reconfiguration takes longer
than usual.
- Undetected protocol failure.

### Response

- Correct the setting of fail detection interval.
- Follow the suggestions made by the registered function.
- Terminate subsystem MSCF.

## MCS1007

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1007 Error when reconfiguring registered function '(&00)'

### Meaning

An error occurred at start or reconfiguration of a registered function.
(&00): Registered function.
NSM Node Synchronization Manager.
XTS XCS Time Synchronization.
XPM XCS Pubset Management.
GSM Global Storage Manager.
NSG Node Synchronization - Global storage part.
GSV Global Storage Volume emulation.
CPM CCS Pubset Management.
DAB Disk Access Buffer.
SHC Symmetrix Host Component.
Possible reasons:
- error when calling function bourse.
- protocol error.
Further hints in serslog entry.

## MCS1008

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1008 Abort requested by registered function '(&00)'

### Meaning

Abort initiated by a registered function.
(&00): Registered function.
NSM Node Synchronization Manager.
XTS XCS Time Synchronization.
XPM XCS Pubset Management.
GSM Global Storage Manager.
NSG Node Synchronization - Global storage part.
GSV Global Storage Volume emulation.
CPM CCS Pubset Management.
DAB Disk Access Buffer.
SHC Symmetrix Host Component.
Possible reasons:
- Registered function unable to initialize,
- registered function unable to reconfigure,
- registered function operational error.

## MCS1009

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1009 Abort requested by partner '(&00)'

### Meaning

This message complements error code '12' of message MCS1003
(&00): Host name of partner.

## MCS1010

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1010 MSCF termination failure. Subsystem MSCF is terminated at system shutdown

### Meaning

Termination of subsystem MSCF failed. MSCF is terminated in system
shutdown and cannot be started again in the current BS2000 session.
Possible reasons:
- Error in termination of a registered function. Use command
/SHOW-MSCF-CONFIGURATION to determine the state of the registered
functions.
- Error during reduction of XCS usage.

## MCS1011

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1011 System termination started. Fail-reconfiguration on partner may be started after shutdown end

### Meaning

The host could not leave an XCS properly. Shutdown has been initiated.
XCS reconfiguration is not started automatically.

### Response

After completion of shutdown answer message
'MCS1100 ... START FAIL-RECONFIGURATION?' displayed at a partner host
remaining in the XCS with 'CRASH'.

## MCS1012

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1012 Partner '(&00)' with SYSID '(&01)' crashed, reconfiguration follows

### Meaning

Partner (&00) is recognized as crashed. An XCS or CCS reconfiguration
will be initiated.
(&00): Host name of partner.
(&01): SYSID of partner.
Possible reasons:
- If recovery-start option is set to AUTOMATIC, a failure of connection
control and disk control has been detected within the time interval
set for automatic failure detection by all active hosts of the XCS.
- The operator has confirmed the crash of the partner.

## MCS1013

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1013 Partner '(&00)' abnormally terminated

### Meaning

Partner (&00) has finished abnormal termination.
(&00): Host name of partner.

## MCS1014

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1014 XCS not allowed in this session

### Meaning

Possible reasons:
- Class 2 option prohibits XCS (MCXSPXCS=N).
- Subsystem MSCF has been started earlier in this session providing
XCS functionality locally.

## MCS1015

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1015 Fail detection limit too short for snapshot dump

### Meaning

Creation of a SNAPSHOT dump takes longer than a fail detection interval.
If automatic failure recovery is activated, the host may be erroneously
considered as crashed by the partner hosts when a SNAPSHOT is created.
This erroneous crash detection is avoided, if local host and partner
hosts have installed BS2000 versions and MSCF versions V14 or greater
and working disk control paths (XCS pubset or shared pubset) exist
between local host and partner hosts.

### Response

Deactivate automatic failure recovery or correct the setting for the fail
detection interval.

## MCS1016

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1016 (&00) user tasks will be terminated

### Meaning

On termination of subsystem MSCF user tasks holding global locks
will be terminated.
(&00): Number of user tasks.

## MCS1017

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1017 Active XCS partner '(&00)' unknown

### Meaning

The active XCS partner (&00) is not noted in the local XCS configuration.
The configuration files may be inconsistent.
(&00): Host name of partner.

### Response

Eliminate the cause of the error and restart subsystem MSCF.

## MCS1018

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1018 Partner '(&00)' does not reply

### Meaning

Partner (&00) did not respond to a message denoting a change of the XCS
configuration. The message is sent again.
(&00): Host name of partner.

## MCS1019

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1019 No XCS defined

## MCS1020

Destination: CONSOLE Routing code: R Weight: 98

Warranty : NO

MCS1020 Not enough memory to process command '(&00)'

### Meaning

More main memory is needed to process the command than is available at the
moment.

### Response

Reenter the command.

## MCS1021

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1021 MSCF termination blocked by (&00) tasks

### Meaning

Termination of (&00) tasks using XCS functionality is not yet completed.
Subsystem MSCF may only be terminated after release of all XCS resources.

### Response

Wait until all tasks that use XCS functionality are terminated or help
them to do so. You can determine these tasks by command
SHOW-XCS-OCCUPATION.

## MCS1022

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1022 Not connected XCS partner '(&00)' using same XCS name '(&01)'

### Meaning

Creation of XCS cluster with XCS name (&01) not possible, because
XCS partner (&00) using the same XCS name already exists; establishing
MSCF connection to XCS partner (&00) has been refused.

### Response

Clear configuration on XCS partner (&00), possibly remove messages
waiting for answer, and restart subsystem MSCF

## MCS1026

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1026 XCM task not ready to process command '(&00)'

### Response

Reenter the command.

## MCS1027

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1027 Running '(&00)' timer changed to '(&01)'

## MCS1028

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1028 Elapsed '(&00)' time must not be modified

## MCS1029

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1029 The undefined MSCF configuration parameter '(&00)' must not be modified

### Meaning

The MSCF configuration parameter (&00) has no meaning in current context.

## MCS1030

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1030 LEAVE-LIMIT '(&00)' elapsed, MSCF aborts

### Meaning

(&00): LEAVE-LIMIT as specified in command SET/MODIFY-MSCF-ENVIRONMENT.

## MCS1031

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1031 ABORT-LIMIT '(&00)' elapsed, system termination follows

### Meaning

(&00): ABORT-LIMIT as specified in command SET/MODIFY-MSCF-ENVIRONMENT.

## MCS1032

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1032 MSCF terminated on partner '(&00)' with SYSID '(&01)', reconfiguration follows

### Meaning

MSCF of partner (&00) is recognized as aborted. An XCS or CCS
reconfiguration will be initiated.
(&00): Host name of partner.
(&01): SYSID of partner.
Possible reasons:
- The termination of MSCF on partner (&00) was recognized by all active
hosts of the CCS- or XCS-network.
- The operator has confirmed the termination of MSCF on partner (&00).

## MCS1033

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1033 Partner '(&00)' prevents modification of HOST-PRIORITY

### Meaning

HOST-PRIORITY may be modified only, if all XCS partners have a XCS version
greater or equal 14.0A.
(&00): Host name of partner.

## MCS1034

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1034 Partner specific MSCF configuration parameter RECOVERY-START for partner '(&00)' not changed

### Meaning

RECOVERY-START setting of partner with MSCF version less than V14.0A
prohibits modification.
(&00): Host name of the remote partner.

## MCS1036

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1036 XCS member '(&00)' and remote host '(&01)' in different XCS using the same XCS name

### Meaning

XCS names must be unambiguous. A MSCF connection to host (&01) is
rejected.

## MCS1037

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1037 Answer '(&00)' for question MCS1103 rejected, reason: '(&01)'

### Meaning

Question MCS1103 was answered wrongly.
(&02): Reasons:
1: Partner (&00) does not exist.
2: (&00) is not offered as possible answer in question MCS1103.
3: Partner (&00) is blocking a fail reconfiguration. The blockade
must be removed only by reestablishing the connection or
terminating the partner.

## MCS1038

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1038 Partner '(&00)' prevents modification of RECOVERY-START

### Meaning

RECOVERY-START can be changed to *CONSISTENT-BY-OPERATOR only, when
partners with MSCF versions less than 14.0A have set RECOVERY-START to
*CONSISTENT-BY-OPERATOR.
(&00): Host name of partner.

## MCS1039

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1039 RECOVERY-START setting of partner '(&00)' prevents MSCF connection with '(&01)'

### Meaning

RECOVERY-START settings of hosts (&00) and (&01) with MSCF versions
less than 14.0A are not compatible.
(&00), (&01): Host names of remote hosts.

## MCS1040

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1040 Partner '(&00)' changed global MSCF configuration parameter '(&01)' from '(&02)' to '(&03)'

### Meaning

A globally effective MSCF configuration parameter has been modified by a
remote partner. The modification came into effect on the local host.
(&00): Host name of the remote partner.
(&01): Name of the modified parameter.
(&02): Old value.
(&03): New value.

## MCS1041

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1041 Partner specific MSCF configuration parameter '(&00)' for partner '(&01)' changed from '(&02)' to '(&03)'

### Meaning

A partner specific MSCF configuration parameter has been modified via
command /MODIFY-MSCF-CONNECTION. The modification came into effect on the
local host and on the partner.
(&00): Name of the modified parameter.
(&01): Host name of the remote partner.
(&02): Old value.
(&03): New value.

## MCS1042

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1042 Partner '(&00)' changes partner specific MSCF configuration parameter '(&01)' from '(&02)' to '(&03)'

### Meaning

A remote partner is modifying an MSCF configuration parameter that has
effects on the local host. The modification came into effect on the local
host.
(&00): Host name of the remote partner.
(&01): Name of the modified parameter.
(&02): Old value.
(&03): New value.

## MCS1043

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1043 XCS partner '(&00)' is assigned permanently to CONTROL-GROUP='1'

### Meaning

When an MSCF connection to an XCS partner is established for the first
time, the partner is assigned to CONTROL-GROUP=1. This assignment must
not be changed.
(&00): Processor name of the remote XCS partner.

## MCS1044

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1044 Answer '(&00)' for '(&01)' rejected

### Meaning

Answer (&00) is not allowed for question (&01)

## MCS1045

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1045 Partner '(&00)' erroneously announced crashed

### Meaning

The remote partner or MSCF of remote partner was announced crashed by
means of message MCS1012 or MCS1032 respectively. The partner became
active again within the same MSCF session revealing the crash announcement
erroneous. No pubset is shared with the remote partner. The MSCF session
continues.
(&00): Host name of the remote partner.
Possible reasons:
- Wrong MSCF configuration parameter settings.
- Faulty operating.

## MCS1046

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1046 Partner '(&00)' with SYSID '(&01)' in SHUTDOWN

## MCS1047

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1047 Partner '(&00)' reports abnormal termination of '(&01)'. Reason: '(&02)'

### Meaning

(&00): Host name of monitoring partner.
(&01): Host name of terminating partner.
(&02): Reasons. Remote operator answers are valid locally:
MTERM: MCS1100 was answered with MTERM.
CRASH: MCS1100 was answered with CRASH.
Possibly RECOVERY-START settings require intervention by operator:
LIVE-MONITOR: System termination confirmed by LIVE-MONITOR.
MSCF: At least two independent monitoring paths failed
simultaneously.

## MCS1048

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1048 System component '(&00)' requests Cluster Recovery Lock

### Meaning

This message logs only the CRL request. Allocation of CRL is logged by
message MCS1002 ...to 'LOCKED'.
(&00): ETMDR = Dynamic Reconfiguration
ETMRK = CPU-Reconfiguration
VM2000 = VM2000

## MCS1049

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1049 System component '(&00)' releases Cluster Recovery Lock

### Meaning

This message logs only the release request. The release of CRL is logged
by message MCS1002 ...from 'LOCKED' to...
(&00): ETMDR = Dynamic Reconfiguration
ETMRK = CPU-Reconfiguration
VM2000 = VM2000

## MCS1050

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1050 System component '(&00)' locks modification of RECOVERY-START

### Response

Modification of RECOVERY-START is possible only after system component
(&00) releases the Cluster Recovery Lock.
(&00): ETMDR = Dynamic Reconfiguration
ETMRK = CPU-Reconfiguration
VM2000 = VM2000

## MCS1051

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1051 Partner '(&00)' locks modification of RECOVERY-START

### Meaning

A system component of partner (&00) is holding the Cluster Recovery Lock.
(&00): Host name of the partner system.

### Response

Modification of RECOVERY-START is possible only after release of Cluster
Recovery Lock.

## MCS1052

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1052 Cluster Recovery Lock not assigned, command rejected

## MCS1053

Destination: CONSOLE Routing code: @ (conslog) Weight: 70

Warranty : NO

MCS1053 Cluster Recovery Lock held by system component '(&00)' will be released

### Meaning

This message logs only the release request by the operating. The release
of CRL is logged by message MCS1002 ...from 'LOCKED' to...
(&00): ETMDR = Dynamic Reconfiguration
ETMRK = CPU-Reconfiguration
VM2000 = VM2000

## MCS1054

Destination: USER-TASK, CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1054 Host '(&00)' not known on local system

### Meaning

(&00): Processor name of remote host.

## MCS1080

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1080 Partner '(&00)' with SYSID '(&01)' starts monitoring of local host, RECOVERY-START='(&02)'

### Meaning

(&00): Host name of the remote partner.
(&01): SYSID of the remote partner.
(&02): Consolidated RECOVERY-START value for monitoring of local host
by partner (&00), resulting from current local and remote, general
and partner specific settings.
Possible values in order of decreasing priority:
LOCKED: A system component of local or remote system holds the
Cluster Recovery Lock (cf. message MCS1048).
BY-OPERATOR: A local setting is *CONSISTENT-BY-OPERATOR or a remote
setting is *CONSISTENT-BY-OPERATOR or *BY-OPERATOR.
SECURE: A local or remote setting is *SECURE.
AUTOMATIC: None of the statements above is true.

## MCS1081

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1081 Partner '(&00)' with SYSID '(&01)' finished monitoring of local host

### Meaning

(&00): Host name of the remote partner.
(&01): SYSID of the remote partner.

## MCS1082

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1082 Partner '(&00)' with SYSID '(&01)' changed monitoring of local host, RECOVERY-START='(&02)'

### Meaning

(&00): Host name of the remote partner.
(&01): SYSID of the remote partner.
(&02): Consolidated RECOVERY-START value for monitoring of local host
by partner (&00), resulting from current local and remote, general
and partner specific settings.
Possible values in order of decreasing priority:
LOCKED: A system component of local or remote system holds the
Cluster Recovery Lock (cf. message MCS1048).
BY-OPERATOR: A local setting is *CONSISTENT-BY-OPERATOR or a remote
setting is *CONSISTENT-BY-OPERATOR or *BY-OPERATOR.
SECURE: A local or remote setting is *SECURE.
AUTOMATIC: None of the statements above is true.

## MCS1090

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1090 Monitoring of partner '(&00)' with SYSID '(&01)' started, RECOVERY-START='(&02)'

### Meaning

The partner is monitored by one or both of the monitoring mechanisms,
connection monitoring and disk monitoring. Inactivity of the partner is
signaled by a console message. Depending on the RECOVERY-START settings,
a fail-reconfiguration may be started automatically or by operator.
(&00): Host name of the remote partner.
(&01): SYSID of the remote partner.
(&02): Consolidated RECOVERY-START value for monitoring of partner (&00)
by local host, resulting from current local and remote, general
and partner specific settings.
Possible values in order of decreasing priority:
LOCKED: A system component of local or remote system holds the
Cluster Recovery Lock (cf. message MCS1048).
BY-OPERATOR: A local setting is *CONSISTENT-BY-OPERATOR or *BY-OPERATOR
or a remote setting is *CONSISTENT-BY-OPERATOR.
SECURE: A local or remote setting is *SECURE.
AUTOMATIC: None of the statements above is true.

## MCS1091

Destination: CONSOLE Routing code: R Weight: 70

Warranty : NO

MCS1091 Monitoring of partner '(&00)' with SYSID '(&01)' finished

### Meaning

(&00): Host name of the remote partner.
(&01): SYSID of the remote partner.

## MCS1092

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1092 Monitoring of partner '(&00)' with SYSID '(&01)' changed, RECOVERY-START='(&02)'

### Meaning

(&00): Host name of the remote partner.
(&01): SYSID of the remote partner.
(&02): Consolidated RECOVERY-START value for monitoring of partner (&00)
by local host, resulting from current local and remote, general
and partner specific settings.
Possible values in order of decreasing priority:
LOCKED: A system component of local or remote system holds the
Cluster Recovery Lock (cf. message MCS1048).
BY-OPERATOR: A local setting is *CONSISTENT-BY-OPERATOR or *BY-OPERATOR
or a remote setting is *CONSISTENT-BY-OPERATOR.
SECURE: A local or remote setting is *SECURE.
AUTOMATIC: None of the statements above is true.

## MCS1100

Destination: CONSOLE Routing code: R Weight: 98

Warranty : NO

MCS1100 No activity of partner '(&00)' detectable, reason: '(&01)'. Start fail-reconfiguration? Reply: (MTERM=MSCF of partner (&00) terminated; CRASH=partner (&00) has crashed or finished SHUTDOWN)

### Meaning

Both monitoring mechanisms, connection monitoring and disk monitoring
notice inactivity of partner (&00). The partner has possibly crashed.
The views of all XCS members coincide in this respect. Live Monitor did
not confirm the partner as crashed. To start the fail-reconfiguration
the failure must be confirmed by the operator.
(&00): Host name of partner.
(&01): Reason for outputting the question:
Three consecutive letters characterize an explicit inhibition of
automatic reconfiguration by RECOVERY-START settings:
L..: The first letter shows, whether this is a local (=L) or remote (=R)
R..: setting.
.G.: The second letter shows, whether this is a general (=G) or
.P.: partner specific (=P) setting.
The third letter shows the value of the setting characterized by
first two letters:
..C: *CONSISTENT-BY-OPERATOR
..O: *BY-OPERATOR
..S: *SECURE
..L: *LOCKED: A system component locks automatic start of recovery.
Single letters characterize other reasons:
D: DOWN: Partner (&00) aborts MSCF or is in SHUTDOWN.
L: LOCKED by a system component (e.g. SNAP, ...) of partner.
M: MODIFYING: The MSCF configuration parameter RECOVERY-START is being
modified.
S: SINGLE PATH: Partner is monitored by a single path only.

### Response

Make sure whether MSCF of the partner has terminated or the partner system
has crashed or finished SHUTDOWN. Answer 'MTERM' or 'CRASH' respectively
only if you are absolutely sure. Otherwise try to get rid of the
disruption. If not successful, terminate MSCF or the BS2000 session of
partner (&00) and answer 'MTERM' or 'CRASH' only after termination of
MSCF or end of SHUTDOWN.

## MCS1101

Destination: CONSOLE Routing code: R Weight: 98

Warranty : NO

MCS1101 MSCF connection to XCS-partner '(&00)' lost, reasons: '(&01)'. Re-establish connection or stop MSCF

### Meaning

XCS is interrupted by loss of connection to partner (&00).
(&00): Host name of partner.
(&01): Reasons for outputting the question:
Three consecutive letters characterize an explicit inhibition of
automatic reconfiguration by RECOVERY-START settings:
L..: The first letter shows, whether this is a local (=L) or remote (=R)
R..: setting.
.G.: The second letter shows, whether this is a general (=G) or
.P.: partner specific (=P) setting.
The third letter shows the value of the setting characterized by
first two letters:
..C: *CONSISTENT-BY-OPERATOR
..O: *BY-OPERATOR
..S: *SECURE
..L: *LOCKED: A system component locks automatic start of recovery.
Single letters characterize other reasons:
D: DOWN: Partner (&00) aborts MSCF or is in SHUTDOWN.
L: LOCKED by a system component (e.g. SNAP, ...) of partner.
M: MODIFYING: The MSCF configuration parameter RECOVERY-START or
HOST-PRIORITY is being modified.
O: OVERDUE: An expected MSCF abort of the partner according to the
current settings of HOST-PRIORITY is overdue.
U: UNCERTAIN: Partner (&00) was lost or considered crashed by all
XCS-members, but then one partner signaled partner (&00) as
alive.

### Response

Do one of the following:
- re-establish the lost MSCF connection, or, if not successful
- terminate subsystem MSCF at one of the affected hosts.

## MCS1102

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1102 MSCF termination failure. System termination required to allow XCS reconfiguration

### Meaning

Subsystem MSCF cannot be terminated because of a non recoverable error.
Reconfiguration of XCS on remaining hosts may only be started after
shutdown end of this host.

### Response

Do the following in the indicated order:
1. Initiate system shutdown.
2. After completion of shutdown, answer message
'MCS1100 ... START FAIL-RECONFIGURATION?' displayed at a partner
host remaining in the XCS by 'CRASH'.

## MCS1103

Destination: CONSOLE Routing code: R Weight: 98

Warranty : NO

MCS1103 Partners '(&00)' are blocking reconfiguration of partners '(&01)'

### Meaning

Partners named in lists &00 and &01 share at least one pubset with the
local host. Systems named in list &01 are SPVS-master of at least one of
the shared pubsets. Fail reconfiguration for SPVS-partners may be started
only, when all active SPVS-partners are connected properly.
(&00): List of host names of blocking partners.
(&01): List of host names of blocked partners.

### Response

To remove the blockades act as follows:
1. If there are questions MCS1100 open for partners in list &00, answer
them for partners that have crashed or terminated MSCF:
The names of these partners are removed from list &00.
2. If 1. does not apply, re-establish MSCF connections to partners in list
&00: The names of the corresponding partners are removed from list
&00.
3. If another system is backup master for a crashed system in list &01,
the concerned names are removed automatically from the lists &00 and
&01, as soon as the corresponding master change has finished.
Possibly one of the actions described in 1. and 2. is to be executed
at the remote backup master.
4. When list &00 becomes empty, MCS1103 is retracted and fail
reconfiguration is started.
Normally MCS1103 should not be answered directly. MCS1103 is retracted
automatically, as soon as all actions described in 1. to 3. have been
executed. Only when you are sure that neither the local system nor a
slave system in list &00 is backup master for any crashed system in list
&01 and relevant to all shared pubsets, you can shorten step 3. (with
effect for the local host only) by answering with the name of this slave
system. In this case, the name of the slave system is removed from list
&00 immediately, without waiting for the termination (or start) of the
master change.

## MCS1104

Destination: CONSOLE Routing code: R Weight: 98

Warranty : NO

MCS1104 Partner '(&00)' crashed. Reason: '(&01)'. Start fail-reconfiguration? Reply: (YES=start fail-reconfiguration)

### Meaning

Crash of partner (&00) has been confirmed. One or more reasons (&01)
inhibit automatic start of fail-reconfiguration.
(&00): Host name of partner.
(&01): Reason for outputting the question:
Three consecutive letters characterize an explicit inhibition of
automatic reconfiguration by RECOVERY-START settings:
L..: The first letter shows, whether this is a local (=L) or remote (=R)
R..: setting.
.G.: The second letter shows, whether this is a general (=G) or
.P.: partner specific (=P) setting.
The third letter shows the value of the setting characterized by
first two letters:
..C: *CONSISTENT-BY-OPERATOR
..O: *BY-OPERATOR
Single letters characterize other reason:
M: MODIFYING: The MSCF configuration parameter RECOVERY-START is being
modified.

### Response

Answer 'YES' to start fail-reconfiguration.

## MCS1110

Destination: CONSOLE Routing code: R Weight: 98

Warranty : NO

MCS1110 Current MSCF version does not support Cluster Recovery Lock. Request by '(&00)' cannot be honored

### Meaning

To perform an operator request, system component (&00) requires a Cluster
Recovery Lock, but the currently loaded MSCF version does not support CRL.
(&00): ETMDR = Dynamic Reconfiguration
ETMRK = CPU-Reconfiguration
VM2000 = VM2000

### Response

Terminate MSCF and repeat operator call to (&00).

## MCS1111

Destination: CONSOLE Routing code: R Weight: 98

Warranty : NO

MCS1111 MSCF partner '(&00)' prevent allocation of Cluster Recovery Lock. Request by '(&01)' cannot be honored

### Meaning

To perform an operator request, system component (&01) requires a Cluster
Recovery Lock. The MSCF-partners in list (&00) prevent allocation of CRL.
(&00): Host names of partners with MSCF V13 and RECOVERY-START setting
different from *CONSISTENT-BY-OPERATOR.
(&01): ETMDR = Dynamic Reconfiguration
ETMRK = CPU-Reconfiguration
VM2000 = VM2000

### Response

Terminate MSCF at local system or at systems (&00) and repeat operator
call to (&01).

## MCS1112

Destination: CONSOLE Routing code: R Weight: 98

Warranty : NO

MCS1112 System component '(&00)' holds Cluster Recovery Lock

### Meaning

System component (&00) holds Cluster Recovery Lock.
(&00): ETMDR = Dynamic Reconfiguration
ETMRK = CPU-Reconfiguration
VM2000 = VM2000

## MCS1200

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1200 Creation of XCS '(&00)' started

### Meaning

The Host is the first to join XCS (&00) thereby creating XCS (&00).
Creation of XCS is started.

## MCS1201

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1201 Creation of XCS '(&00)' finished, XCS ready

### Meaning

The Host is the first to join XCS (&00) thereby creating XCS (&00).
Creation of XCS is finished.

## MCS1202

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1202 Join to XCS '(&00)' started

### Meaning

The local host joins to the existing XCS (&00). Join reconfiguration has
just been started.

## MCS1203

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1203 Reconfiguration of XCS '(&00)' started. Join of host '(&01)'

### Meaning

Command '/START-SUBSYSTEM MSCF' has been entered at partner (&01)
The partner is joining to the XCS (&00). The message is displayed at all
hosts already participating in the XCS.
(&01): Host name of partner.

## MCS1204

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1204 Reconfiguration of XCS '(&00)' finished. XCS ready

### Meaning

Possible reasons for the reconfiguration:
- A partner joined to the XCS.
- A partner left the XCS normally.
- A partner left the XCS abnormally.
- A combination of these reasons.
(&00): Name of XCS.

## MCS1205

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1205 Join to XCS '(&00)' finished. XCS ready

### Meaning

The reconfiguration for joining the local host to XCS (&00) is finished.

## MCS1206

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1206 Reconfiguration of XCS '(&00)' started. Leave of host '(&01)'

### Meaning

Command '/STOP-SUBSYSTEM MSCF' has been entered at partner (&01).
Leave reconfiguration of XCS (&00) for partner (&00) is started.
The message is displayed at hosts remaining in the XCS.
(&01): Host name of partner.

## MCS1207

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1207 Leave from XCS '(&00)' started

### Meaning

command '/STOP-SUBSYSTEM MSCF' has been entered. The local host leaves
XCS (&00). The XCS remains in existence and is reconfigured.

## MCS1208

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1208 Termination of XCS '(&00)' started

### Meaning

The command '/STOP-SUBSYSTEM MSCF' has been entered. The local host is
the last member of XCS (&00). The XCS will be terminated.

## MCS1210

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1210 Leave from XCS '(&00)' finished. XCS not available

### Meaning

The local host has left XCS (&00). XCS reconfiguration of the remaining
partners is finished. No XCS functionality is available at the local host.

## MCS1211

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1211 XCS '(&00)' terminated, XCS not available

### Meaning

The local host has left XCS (&00) as the last member thereby terminating
the XCS. No XCS functionality is available.

## MCS1213

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1213 Reconfiguration of XCS '(&00)' started. Partner '(&01)' will be removed

### Meaning

Partner (&01) is going to be removed from XCS (&00). The reason is given
in a preceding message.
(&01): Host name of partner.

## MCS1214

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1214 Reconfiguration of control group '(&00)' started

## MCS1215

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1215 SPVS sharer '(&00)' for shared pubset(s) '(&01)' crashed

### Meaning

Possibly a master change for pubsets in list '(&01)' is pending.
(&00): Host name of the crashed system.

## MCS1216

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1216 Fail reconfiguration of SPVS-partner '(&00)' started

## MCS1300

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1300 System termination to prevent erroneous crash detection by partners

### Meaning

A write error on all pubsets shared by the local host and a controlling
partner occurred simultaneously with the loss of all MSCF connections to
this partner. Because the RECOVERY-START settings (general and partner
specific, local and partners settings) are all set to *AUTOMATIC, the
controlling partner may assume the local host to have crashed and start
fail reconfiguration. To grant consistency even in this case, the local
host is terminated by SETS.

## MCS1301

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1301 System termination to allow the reconfiguration at the MSCF partners

### Meaning

The general RECOVERY-START value of the local host is set to *AUTOMATIC.
When terminating XCS membership of this host not all global XCS resources
occupied by the host could be released successfully. To initiate a fail
reconfiguration of the hosts remaining in the XCS the system is
terminated automatically to enable abort reconfiguration at the remaining
hosts.
Possible reasons:
- Program error in configuration management.
- Termination request by a registered function.

## MCS1302

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1302 System termination because of irrecoverable error in configuration management

### Meaning

Error recovery of configuration management is unable to recover from an
error. To grant consistency the current system session is terminated
by SETS.

### Response

Forward the dump to system diagnosis and restart the system.

## MCS1303

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS1303 Unexpected situation in XCM processing, error logged in SERSLOG file

## MCS1304

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS1304 System termination because of expiration of ABORT-LIMIT time

## MCS2000

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS2000 MSCF connection from host '(&01)' with MSCF version '(&02)' for application '(&00)' not accepted

### Meaning

The remote host (&01) tries to open an MSCF connection to local host for
application (&00). However, BCAM does not fully support the functionality
required by MSCF on the remote host for the selected route.
(&00): name of application.
(&01): Host name of remote host.
(&02): MSCF version of remote host.

### Response

1. On remote host (&01) verify by means of command
BCSHOW whether command BCMAP has been entered to restrict the selection
of BCAM routes for application (&00) to ISO class4 or NEA routes.
If necessary, enter command BCMAP.
2. Verify whether BCAM routes for application (&00) were correctly
generated.

## MCS2001

Destination: CONSOLE Routing code: R Weight: 50

Warranty : NO

MCS2001 Unexpected situation in processing, error logged in SERSLOG file

## MCS3000

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS3000 No information found for specified selection

### Meaning

No information is available matching the selection criteria specified in
command /SHOW-MSCF-CONFIGURATION.

### Response

Reenter the command specifying a different selection criterion.

## MCS4120

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS4120 The watchdog mechanism is initialized

### Meaning

The watchdog task (TSN=WDGS) has been initialized successfully.
If the host is of type XCS, all XCS pubsets are imported.

## MCS4121

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS4121 The '(&00)' of the shared pubset '(&01)' is rejected. Reason '(&02)'

### Meaning

(&00): IMPORT: The import of the pubset is rejected.
EXPORT: The export of the pubset is rejected.
(&01): Pubset-ID
(&02): Possible reasons in case of IMPORT:
01: Memory management error.
02: MRSCAT error.
03: System error
04: Configuration error: Failure detection limits of master and
slave are set differently.
05: MSCF communication error.
06: There is no XCS pubset in the XCS network or the XCS hosts use
different XCS pubsets.
07: XCS configuration error at the master of the XCS pubset.
08: No XCS pubset is defined at the host.
09: Write error at master sharer.
10: A CCS slave must not import an XCS pubset.
11: The slave export at the master is not yet finished. Start the
slave import again.
Possible reasons in case of EXPORT:
01: An XCS pubset can only be exported on the master.
02: MRSCAT error.
04: DLM-lock error.
05: The last XCS pubset in the XCS network must not be exported.
06: An export with master change is not allowed for XCS pubsets.
07: Pubset must not be exported during conversion into XCS pubset.

## MCS4122

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS4122 '(&00)' of the shared pubset '(&01)' is not processed

### Meaning

The reconfiguration of the XCS network cannot be completed, because a
shared pubset operation of the shared pubset (&01) could not be
processed.
(&00): Shared pubset operation:
IMPORT: The import of the shared pubset could not be finished.
EXPORT: The export of the shared pubset or exclusively in shared GS
imported pubset could not be finished.
MASTER-CHANGE: The master change of the shared pubset could not be
finished.

## MCS4123

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS4123 Error during initialization of the watchdog mechanism. Reason '(&00)'

### Meaning

An error occurred during the initialization of the watchdog mechanism.
The start of subsystem MSCF is aborted.
(&00): Reason:
01: The previous watchdog session is not terminated completely
02: Error during MRSCAT-Access.
03: A shared pubset import has been started already.
04: System error.
05: Error in the task lock management.
06: Error in the bourse management.
07: Error at task creation of the WDGS task.
08: XPM startup error.
09: Error in memory management.

## MCS4124

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS4124 Error during initialization or termination of the watchdog mechanism. Reason '(&00)'

### Meaning

An error occurred during the initialization or termination of the
watchdog mechanism. The subsystem MSCF is aborted.
(&00): Possible reasons:
01: Memory management error.
02: Error during MRSCAT access.
03: System error.
04: Error in the distributed lock management.
05: Error in the MSCF communication.
06: Error in the XCS pubset management.
07: Error when importing an XCS pubset
08: No XCS pubset defined.
09: The XCS pubset master suffers a permanent write error.

## MCS4125

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS4125 The watchdog mechanism has been terminated

### Meaning

The watchdog mechanism has been terminated normally.
The local host is unable to access shared pubsets.

## MCS4126

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS4126 Configuration error, the shared pubset '(&00)' has been exported. Reason '(&01)'

### Meaning

A Shared pubset configuration error occurred. To preserve the
consistency of SPVS (&00) and host control, the pubset has been
force exported.
(&01): Possible reasons:
01: Control state inconsistent.
02: Invalid block in watchdog file.
03: SYSID inconsistent.
04: Version ID inconsistent.
05: SYSID multiply used.
06: Host name and SYSID indicate different partners.
07: Error when calling interface $GETMEM.
08: HOST-ID inconsistent.
09: Error when calling interface MCXPSJ. The reason is indicated in
message MCS1005.

## MCS4127

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS4127 /SET-XCS-PUBSET for pubset '(&00)' rejected. Reason '(&01)'

### Meaning

An error occurred during the processing of the /SET-XCS-PUBSET command
for pubset (&00).
(&01): Possible reasons:
01: The pubset is not imported as a shared pubset.
02: XCM error occurred.
03: Error in the watchdog mechanism.
04: The shared pubsets and XCS have different configurations.
05: DLM error.
06: Error in the command processing at the partner host.
07: MSCF communication error.
08: XCS is not in ready state.
09: Bourse error.
10: DLM-Bourse-Timeout.
11: Internal Error.
12: The host is not an XCS member.
13: MRSCAT access error.
14: The pubset is already an XCS pubset.
15: Improper state of MRSCAT entry.
16: Pubset includes a GS volume.

## MCS4128

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS4128 Export with master change of shared pubset '(&00)' started on host '(&01)'

### Meaning

On host (&01) the export with master change of the indicated shared
pubset (&00) has been started. The pubset is set to quiet state.
After completion of the export processing, processing of the master
change will be continued.

## MCS4129

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS4129 Import for pubset '(&00)' rejected. Reason '(&01)'

### Meaning

An error occurred during the processing of the /IMPORT-PUBSET command for
pubset (&00).
(&01): Possible reasons:
01: The subsystem MSCF is not in the proper state to import a shared
pubset.
02: The watchdog file cannot be allocated on the PUBRES.
03: The watchdog file information in the TSOSCAT and SVL are
inconsistent.
04: Error during access to the shared pubset MONJV.
05: The MRSCAT entry of the shared pubset is not in the proper state
to allow the import.

### Response

01: The subsystem MSCF must be loaded and the registered functions CPM
and XPM must be in an error free state.
02: There is no enough free space on the PUBRES, please delete some files.
03: Please delete the watchdog file.
04: Please delete the shared pubset MONJV.
05: Please consult the MSCF trace file.

## MCS4130

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS4130 Shared pubset '(&00)' changed to XCS pubset

### Meaning

The shared pubset (&00) has been changed successfully to an XCS pubset by
means of command /SET-XCS-PUBSET.

## MCS4131

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS4131 The watchdog mechanism will be terminated, all shared pubsets will be exported

### Meaning

The termination of the watchdog mechanism has been started.
The export of all XCS and shared pubsets and of all exclusively imported
pubsets with a volume set in the shared GS is initiated. Only after these
exports are successfully completed, the watchdog mechanism is
terminated and subsystem MSCF unloaded.

## MCS4132

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

MCS4132 Watch dog mechanism is running, shared pubsets are monitored again

### Meaning

The failure reported by message DMS03B7 has been fixed, all shared pubsets
are monitored again.

©2024 Fujitsu | BS2000 System Messages