## MSMDC00

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSMDC00 DMS ERROR '(&01)' DELETING RECORDS OF MESSAGE '(&00)' IN FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

The message is not correctly suppressed.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Check the message, eliminate the cause of the error and retry the
operation.

## MSMDC01

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMDC01 DMS ERROR '(&01)' READING DOCUMENTATION OF CLASS '(&00)' IN FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## MSMDC02

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMDC02 DMS ERROR '(&01)' DELETING DOCUMENTATION LINE '(&04)' IN FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

The documentation is not correctly suppressed.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Check the documentation, eliminate the cause of the error and retry the
operation.

## MSMDC03

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMDC03 DMS ERROR '(&01)' DELETING DOCUMENTATION OF CLASS '(&00)' IN FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

The documentation is not correctly suppressed.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Check the documentation, eliminate the cause of the error and retry the
operation.

## MSMDC04

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMDC04 DMS ERROR '(&01)' WRITING DOCUMENTATION LINE '(&04)' IN FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

The documentation is not correctly written.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Check the documentation, eliminate the cause of the error and retry the
operation. Allow overwriting in order to replace the corrupted
documentation by the new one.

## MSMDC05

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMDC05 DMS ERROR '(&01)' READING COMPONENT-ID OF CLASS '(&00)' IN FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## MSMDC06

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMDC06 DMS ERROR '(&01)' DELETING COMPONENT-ID OF CLASS '(&00)' IN FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

The component-id is not correctly suppressed.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Check the component-id, eliminate the cause of the error and retry the
operation.

## MSMDC07

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMDC07 DMS ERROR '(&01)' WRITING COMPONENT-ID OF CLASS '(&00)' IN FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

The component-id is not correctly written.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Check the component-id, eliminate the cause of the error and retry the
operation. Allow overwriting in order to replace the corrupted
component-id by the new one.

## MSMDC08

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMDC08 DMS ERROR '(&01)' READING DOCUMENTATION LINE '(&04)' IN FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## MSMDC23

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMDC23 In message '(&00)', the text in language '(&02)' plus its default insert values result in an overlong record. Processing aborted

### Meaning

In a message file, the maximum record length is limited to 512 (new file
format) or 256 (old file format) bytes.
The internal representation of the message text, plus the default values
of the inserts defined in the text, plus the message attributes, exceeds
this limit.

### Response

Shorten the message text or the default insert values.
Retry the operation.

## MSMDG00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMDG00 DMS ERROR '(&01)' READING MESSAGE '(&00)' IN FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Check the message, eliminate the cause of the error and retry
the operation.

## MSMDG01

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMDG01 DMS ERROR '(&01)' WRITING MESSAGE '(&00)' IN FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

The message is not correctly written.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Check the message, eliminate the cause of the error and retry the
operation. Allow overwriting in order to replace the corrupted message
by the new one.

## MSMDJ00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMDJ00 DMS ERROR '(&09)' DURING ACCESS '(&10)' ON FILE '(&05)': FUNCTION ABORTED. IN SYSTEM MODE: /HELP-MSG DMS(&09)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Eliminate the cause of the error and retry the operation.

## MSMDJ01

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMDJ01 DMS ERROR '(&01)' OPENING FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## MSMDM00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMDM00 DMS ERROR CODE '(&01)' READING CORRECTION-INFORMATION OF CLASS '(&00)' IN FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## MSMDM01

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMDM01 DMS ERROR CODE '(&01)' WRITING CORRECTION-INFORMATION OF CLASS '(&00)' IN FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

The correction information is not correctly written.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Check the correction information, eliminate the cause of the error and
retry the operation.

## MSMD001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMD001 DMS ERROR '(&01)' CLOSING FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## MSMD013

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMD013 INVALID FILE NAME '(&07)'

## MSMD020

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMD020 FILE '(&05)' DOES NOT HAVE VALID ATTRIBUTES FOR A MESSAGE FILE

### Meaning

Correct file attributes are: FCBTYPE=ISAM, RECFORM=V, KEYPOS=5, KEYLEN=10.

## MSMD029

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMD029 FILE '(&05)' ALREADY EXISTS

### Meaning

A message file to be opened in CREATE mode already exists.

### Response

Delete the file before creating a new one with the same name
or correct the file name.

## MSMD100

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMD100 DMS ERROR '(&01)' READING RANGES OF FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

A DMS error occurred when reading the directory (range definitions) of a
message file in old format (i.e. produced with MSGEDIT).
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## MSMD101

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMD101 DMS ERROR '(&01)' CREATING FILE '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## MSMD102

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMD102 DMS ERROR '(&01)' READING MESSAGE FILE ATTRIBUTES OF '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## MSMD103

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMD103 DMS ERROR '(&01)' MODIFYING MESSAGE FILE ATTRIBUTES OF '(&05)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## MSMD300

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMD300 DMS ERROR '(&01)' READING MESSAGE '(&00)' IN FILE '(&05)'. '(&09)' ABORTED. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## MSMD301

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMD301 DMS ERROR '(&01)' DELETING MESSAGE '(&00)' IN FILE '(&05)'. '(&09)' ABORTED. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

The message is not correctly suppressed.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Check the message, eliminate the cause of the error and retry the
operation.

## MSMD302

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMD302 DMS ERROR '(&01)' WRITING MESSAGE '(&00)' IN FILE '(&05)'. '(&09)' ABORTED. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

The message is not correctly written.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Check the message, eliminate the cause of the error and retry the
operation. Allow overwriting in order to replace the corrupted message
by the new one.

## MSMEA00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEA00 MEANING and RESPONSE lines must be limited to 74 characters maximum

### Meaning

A MEANING or RESPONSE line in one of the languages is longer than 74
characters.

### Response

The text may be formatted using the separator character '^' and the join
statement J of EDT.

## MSMEB00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEB00 AT LEAST 1 LANGUAGE MUST BE DEFINED FOR MESSAGE '(&00)'

## MSMEB01

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEB01 TEXT '(&09)' HAS NO LANGUAGE. ADD ONE OR CLEAR TEXT

## MSMEC00

Destination: USER-TASK Routing code: Weight:

Warranty : NO

MSMEC00 Invalid attribute in message '(&00)' from file '(&05)'. Operation aborted

### Meaning

An unknown message element (attribute, insert number, insert
attribute, ...) was read. The message was created with a newer
version of MSGMAKER or is corrupted. It can not be processed.
If the operation was applied to a set of messages:
- all messages before the one in error have been processed
- subsequent messages will not be processed.

### Response

Try with a newer version of MSGMAKER.

## MSMEF00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEF00 NO CURRENT MESSAGE FILE OPENED IN UPDATE MODE. PROCESSING OF REQUESTED FUNCTION NOT POSSIBLE

### Meaning

A work message file must first be opened (in MENU panel or with a
//OPEN-MSG-FILE statement) before processing the requested function.

## MSMEF01

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEF01 INVALID FILE NAME '(&05)': WILDCARDS ARE NOT SUPPORTED

### Meaning

Wildcards in file names are not supported in this version of MSGMAKER.

## MSMEF02

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEF02 '(&07)' NOT ALLOWED IN COMMAND LINE OF THIS PANEL

### Meaning

The text entered in command line is not a valid action for this panel.

## MSMEF03

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEF03 NO INFORMATION ITEM SELECTED

## MSMEF04

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEF04 LANGUAGE(S) GIVEN AND NO MESSAGE INFORMATION SELECTED

### Response

Specify no language or select a MESSAGE information.

## MSMEI00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEI00 OUTPUT FILE '(&05)' NOT EMPTY

### Meaning

The message file (&05) contains (at least) a message, documentation, ...
This is not allowed.

## MSMEJ00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEJ00 NO CURRENT MESSAGE FILE OPEN. A FILE MUST BE SPECIFIED

### Response

Open a work message file (in MENU panel or with a //OPEN-MSG-FILE
statement) or give a message file name in the operation to be processed.

## MSMEJ01

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSMEJ01 NO MESSAGE CLASS IN FILE '(&05)', OR MORE THAN ONE. SPECIFY ONE

### Meaning

MSG-CLASS=*CURRENT can not be interpreted because there is no message
class or more than one in the message file.

### Response

A message class must be specified.

## MSMEK00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEK00 NO OUTPUT DESTINATION. SELECT AT LEAST ONE

## MSMEL01

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEL01 DOCUMENTATION LINE '(&04)' ALREADY EXISTS. NOTHING PROCESSED

### Meaning

The DOCUMENTATION line already exists and, in batch or procedure mode,
the global OVERWRITE option is set to NO.

### Response

In batch or procedure mode, change the global OVERWRITE option by means of
the //MODIFY-OPTIONS statement or use the //MODIFY-DOCUMENTATION
statement.

## MSMEL02

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEL02 DOCUMENTATION LINE '(&04)' DOES NOT EXIST

### Response

Use the ADD-DOCUMENTATION operation to add a new documentation line.

## MSMEM01

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEM01 NO PM-NUMBER ADDED TO CLASS '(&00)': IT ALREADY CONTAINS (&09) PM-NUMBERS

### Meaning

The maximum number of PM's for a message class is exceeded.
Nothing has been modified in the correction information of the message
class.

## MSMEM02

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEM02 LAST PM-NUMBERS NOT ADDED TO CLASS '(&00)'. ONLY (&09) MAY BE STORED WITHIN

### Meaning

The maximum number of PM's for a message class has been exceeded.
The PM-numbers specified beyond this limit are lost.

## MSMEN02

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEN02 MULTIPLE CLASSES NOT ALLOWED. NOTHING PROCESSED

### Meaning

The list of message identifiers may not extend beyond a class.

## MSMEN04

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEN04 FILE '(&05)' ALREADY EXISTS. NOTHING PROCESSED

### Meaning

The output file is already cataloged and is not empty.

## MSMEO00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEO00 MISSING OWNER INFORMATION

### Meaning

The owner name and team are mandatory information.

## MSMEO01

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSMEO01 NO COMPONENT-ID IN CLASS '(&00)(&04)'

### Response

Use the ADD-COMPONENT-ID operation to define a new component-id.

## MSMEO02

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMEO02 MULTIPLE COMPONENT-ID'S IN CLASS '(&00)'. 'ADD' AND 'MODIFY' OPERATIONS NOT ALLOWED

### Meaning

It is not allowed to add or modify a component-id in a message class which
already contains several ones.

### Response

Only the DELETE-COMPONENT-ID operation is allowed on multiple
component-id's.
Multiple component-id's for a same message class must be stored in
different message files.

## MSMEO03

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSMEO03 CLASS '(&00)' ALREADY CONTAINS A COMPONENT-ID (NAME='(&09)', VERSION='(&10)', DATE='(&11)'). OPERATION ABORTED

### Response

To allow overwriting, set the global OVERWRITE option to YES
(//MODIFY-OPTIONS statement).

## MSME000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME000 FILE '(&05)' IS ALREADY OPEN IN 'READ' MODE

### Meaning

A work message file currently open in READ mode (by a previous MENU
panel or //OPEN-MSG-FILE statement) cannot be opened again as source
or target file in UPDATE mode.

### Response

Open the work message file in UPDATE mode.

## MSME100

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSME100 RANGE '(&04)' CONTAINS NO MESSAGE TO BE MODIFIED

## MSME102

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSME102 MESSAGE '(&00)' ALREADY EXISTS IN FILE '(&05)'. OPERATION ABORTED

### Meaning

The message (&00) already exists and the (global) OVERWRITE option is
set to NO.

## MSME103

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSME103 RANGE '(&04)' CONTAINS NO FREE MESSAGE-ID TO BE ADDED

### Meaning

All possible message identifiers in the given range are already assigned.
No free message-id can be automatically selected in this range.

## MSME104

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSME104 MESSAGE '(&00)' DOES NOT EXIST IN FILE '(&05)'. OPERATION ABORTED

### Meaning

If the operation was applied to a set of messages:
- all messages before the one in error have been processed
- subsequent messages will not be processed.

## MSME105

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME105 NO RENAMING ALLOWED FOR A LIST OF MESSAGE-ID'S. NOTHING PROCESSED

### Meaning

Renaming is not allowed for a list of message identifiers in one
operation.

### Response

Rename the items one by one or specify the message identifiers by means
of an interval or class.

## MSME107

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME107 'STANDARD' FILE '(&05)' MAY NOT BE CHANGED TO 'CUSTOMER' TYPE

### Meaning

It is not allowed to change the type of a message file from STANDARD
(i.e. attached to an official product developed within Siemens Nixdorf
Informationssysteme) to CUSTOMER.

### Response

Create a new message file of type CUSTOMER and copy required information
from the STANDARD message file.

## MSME108

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSME108 NOTHING COPIED OR MOVED FROM FILE '(&05)' TO FILE '(&06)'

### Meaning

Possible reasons:
- no information of the specified set is present in the input file
- all information to be copied or moved is present in the target file
and the OVERWRITE option is set to NO.

## MSME109

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME109 '(&05)' IS NOT A VALID MESSAGE FILE

### Meaning

The file contains no or an invalid identification record.

## MSME110

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSME110 SAVE FILE '(&05)' ALREADY EXISTS. CONVERSION OF OLD FILE FORMAT ABORTED

### Meaning

The file in old format (i.e. created with MSGEDIT) given for update
purposes cannot be saved because a file is already cataloged with the
name built as a save file by MSGMAKER.
As saving of the old file was requested, conversion is aborted.

### Response

Retry the operation; MSGMAKER will build another save file name.

## MSME111

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSME111 DMS ERROR COPYING OLD FILE FORMAT TO SAVE FILE '(&05)'. CONVERSION ABORTED

### Meaning

The file in old format (i.e. created with MSGEDIT) given for update
purposes cannot be saved because a DMS error was detected during copying.
As saving of the old file was requested, conversion is aborted.
It is not possible to convert a message file cataloged on a pubset whose
data organization differs from the organization of the home pubset on
which MSGMAKER is running (for example, the old file format is cataloged
on a NON-KEY disk but MSGMAKER is running on a system with PAM-KEY).
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Eliminate the cause of the error and retry the operation, or
convert the message file by means of the COPY function of MSGMAKER:
COPY MSG-ID=*ALL,INFORMATION=*ALL,
FROM-FILE=<old-format filename>,TO-FILE=<new file>.

## MSME112

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSME112 DMS ERROR COPYING TMP FILE TO FILE '(&05)'. CONVERSION OF OLD FILE FORMAT ABORTED

### Meaning

The file in old format (i.e. created with MSGEDIT) given for update
purposes has been converted to a new file format in a temporary work file,
but the old file format cannot be replaced by the temporary work file
because a DMS problem occurred.
It is not possible to convert a message file cataloged on a pubset whose
data organization differs from the organization of the home pubset on
which MSGMAKER is running (for example, the old file format is cataloged
on a NON-KEY disk but MSGMAKER is running on a system with PAM-KEY).
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Eliminate the cause of the error and retry the operation, or
convert the message file by means of the COPY function of MSGMAKER:
COPY MSG-ID=*ALL,INFORMATION=*ALL,
FROM-FILE=<old-format filename>,TO-FILE=<new file>.

## MSME113

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME113 TO-MSG-ID MUST BE DIFFERENT FROM *SAME WHEN COPYING/MOVING INTO THE SAME FILE

### Meaning

In a COPY or MOVE operation with FROM-FILE equal to TO-FILE,
TO-MSG-ID must be different from *SAME: renaming is mandatory.

### Response

Specify another TO-MSG-ID or change the FROM-FILE or TO-FILE.

## MSME114

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME114 FILE '(&05)' IS NOT AN OLD FORMAT MESSAGE FILE

### Meaning

The operation can only be performed on message files in old
format (as created by MSGEDIT).

### Response

Select another message file or specify you want a new file format.

## MSME200

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME200 SELECTION RESTRICTED TO 'STANDARD' MESSAGE FILES

### Meaning

The selected operation may be processed only within a work message file
of type STANDARD (i.e. attached to an official product developed within
Siemens Nixdorf Informationssysteme).

## MSME201

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME201 ACTION '(&07)' NOT ALLOWED: OTHER OPERATIONS ARE RESTRICTED TO 'STANDARD' MESSAGE FILES

### Meaning

The operations in the next panel are not allowed because the work message
file is not of STANDARD type (i.e. attached to an official product
developed within Siemens Nixdorf Informationssysteme).

## MSME300

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME300 INVALID TARGET MSG-ID '(&07)': RENAMING IS ALLOWED ONLY TO A SINGLE MESSAGE CLASS. NOTHING PROCESSED

### Meaning

The fixed part of the new message identifier must contain at least one
message class (3 letters), and the renamed message identifiers may not
extend beyond the new class.

### Response

Reduce the source interval or specify a lower target message identifier.

## MSME400

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME400 NO ACCESS METHOD DEFINED

## MSME401

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME401 NO DESTINATION DEFINED

## MSME402

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME402 Access methods 'BAMR', 'LOCAL-DLAM' and 'MINIMIP' are restricted to 'STANDARD' message files. No message processed

### Meaning

The access methods BAMR, LOCAL-DLAM and MINIMIP may be assigned to
messages only within a work message file of type STANDARD (i.e. attached
to an official product developed within Siemens Nixdorf
Informationssysteme).

## MSME403

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME403 ROUTING CODE '(&07)' WITHOUT 'CONSOLE' DESTINATION IN MESSAGE '(&00)'. OPERATION ABORTED

### Meaning

A routing code may not be defined without a CONSOLE destination.
If the operation was applied to a set of messages:
- all messages before the one in error have been processed
- subsequent messages will not be processed.

### Response

Suppress the routing code or add a CONSOLE destination.

## MSME500

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME500 Accesses 'ISAM' and 'DLAM' or 'LOCAL DLAM' may not be chosen together. No message processed

## MSME501

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME501 MESSAGE '(&00)': A WEIGHT MUST BE SPECIFIED WHEN DESTINATION IS 'CONSOLE'. OPERATION ABORTED

### Meaning

If the operation was applied to a set of messages:
- all messages before the one in error have been processed
- subsequent messages will not be processed.

## MSME502

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME502 MESSAGE '(&00)': A ROUTING CODE MUST BE SPECIFIED WHEN DESTINATION IS 'CONSOLE'. OPERATION ABORTED

### Meaning

If the operation was applied to a set of messages:
- all messages before the one in error have been processed
- subsequent messages will not be processed.

## MSME503

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME503 INSERT NAME '(&07)' IS A RESERVED WORD. NO MESSAGE PROCESSED

### Meaning

The insert names MSG-ID, MSG-TEXT and REPLY are reserved names. They must
not be defined.

## MSME504

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSME504 INVALID CHARACTER '(&07)' IN MESSAGE TEXT OF LANGUAGE '(&02)' FOR MESSAGE '(&00)'. OPERATION ABORTED

### Meaning

Characters which have multiple meanings depending on the variant of the
standard character set are not allowed in messages.
E.g. the hexadecimal codes X'4F', X'BB', X'BC', X'BD', X'FB', X'FD' and
X'FF' (see EBCDIC.DF.03 character code) are not allowed.
If the operation was applied to a set of messages:
- all messages before the one in error have been processed
- subsequent messages will not be processed.

## MSME505

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME505 MESSAGE '(&00)' CONTAINS THE SAME LANGUAGE '(&02)' (AT LEAST) TWICE

### Response

In dialog mode, the languages may be corrected either in the
ADD-MSG/MODIFY-MSG or MSG-TEXT panel.

## MSME507

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSME507 MESSAGE '(&00)' HAS (AT LEAST) TWICE THE SAME INSERT NAME '(&07)'. OPERATION ABORTED

### Meaning

All insert names must be different for a given message.
If the operation was applied to a set of messages:
- all messages before the one in error have been processed
- subsequent messages will not be processed.

## MSME508

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSME508 INVALID CHARACTER '(&07)' IN MEANING OF LANGUAGE '(&02)' FOR MESSAGE '(&00)'. OPERATION ABORTED

### Meaning

Characters which have multiple meanings depending on the variant of the
standard character set are not allowed in messages.
E.g. the hexadecimal codes X'4F', X'BB', X'BC', X'BD', X'FB', X'FD' and
X'FF' (see EBCDIC.DF.03 character code) are not allowed.
If the operation was applied to a set of messages:
- all messages before the one in error have been processed
- subsequent messages will not be processed.

## MSME509

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSME509 INVALID CHARACTER '(&07)' IN RESPONSE OF LANGUAGE '(&02)' FOR MESSAGE '(&00)'. OPERATION ABORTED

### Meaning

Characters which have multiple meanings depending on the variant of the
standard character set are not allowed in messages.
E.g. the hexadecimal codes X'4F', X'BB', X'BC', X'BD', X'FB', X'FD' and
X'FF' (see EBCDIC.DF.03 character code) are not allowed.
If the operation was applied to a set of messages:
- all messages before the one in error have been processed
- subsequent messages will not be processed.

## MSME510

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSME510 INVALID CHARACTER '(&07)' IN DEFAULT VALUE OF INSERT '(&09)' FOR MESSAGE '(&00)'. OPERATION ABORTED

### Meaning

Characters which have multiple meanings depending on the variant of the
standard character set are not allowed in messages.
E.g. the hexadecimal codes X'4F', X'BB', X'BC', X'BD', X'FB', X'FD' and
X'FF' (see EBCDIC.DF.03 character code) are not allowed.
If the operation was applied to a set of messages:
- all messages before the one in error have been processed
- subsequent messages will not be processed.

## MSME511

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSME511 LANGUAGE '(&02)' OF MESSAGE '(&00)' HAS NO MESSAGE TEXT. OPERATION ABORTED

### Meaning

At least a message text must be assigned to each language of a message
unit.
If the operation was applied to a set of messages:
- all messages before the one in error have been processed
- subsequent messages will not be processed.

## MSME600

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSME600 MORE THAN (&09) LANGUAGES DEFINED FOR MESSAGE '(&00)'. OPERATION ABORTED

### Meaning

The maximum number of languages for a message unit has been exceeded.
If the operation was applied to a set of messages:
- all messages before the one in error have been processed
- subsequent messages will not be processed.

## MSME601

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME601 A LINK ON FILE '(&05)' CANNOT BE SET. MSGMAKER NOT CORRECTLY INSTALLED

### Meaning

The file given in insert (&05) is not correctly installed. MSGMAKER
cannot be run.

### Response

Contact the system administrator.

## MSME800

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME800 VERSION '(&07)' HAS NO PRODUCT

### Meaning

A version may not be defined without a product name.

### Response

Suppress the version or add a product name.

## MSME900

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSME900 Insert number (&07) not defined in message text

### Meaning

Insert attributes cannot be set before the insert number is defined in
the message text.

### Response

Go back to the MSG-TEXT panel by pressing the <K1> key and define the
insert in the form "(&ii)", where ii is the insert number (for example:
(&01)).

## MSME901

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSME901 Field must be empty if the attribute is not to be selected

### Response

Select the attribute with Yes or clear the field.

## MSMIB00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMIB00 INVALID 'TEXT OUTPUT FORMAT' '(&07)'

### Meaning

Valid values for the text output format are:
U: The message text and its insert values will be converted to
upper-case characters when the message is output by an MSG7(X)
macro or /HELP-MSG-INFORMATION command.
L: The message text and its insert values will be output without any
case conversion.
The message texts and the default insert values are not
converted to upper-case until they have been stored in the message file.

## MSMID00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMID00 INVALID 'DISPLAY MSG' REPLY '(&07)'

### Meaning

Valid answers are:
Y: before each deletion of a message, the first 4 message texts will
be displayed and confirmation will be requested.
N: deletion will be executed without confirmation!

## MSMIF00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMIF00 INVALID LANGUAGE '(&07)'. NOTHING PROCESSED

### Meaning

A language must be specified by a letter (A to Z).

### Response

In dialog mode, the language may be corrected either in the
ADD-MSG/MODIFY-MSG or MSG-TEXT panel.

## MSMIF01

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMIF01 INVALID MESSAGE IDENTIFIER '(&07)'. NOTHING PROCESSED

### Meaning

A complete message identifier is composed of:
- 3 letters (A to Z) for the message class and
- 4 letters (A to Z) or digits (0 to 9) for the message number.

## MSMIF02

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMIF02 INVALID INTERVAL '(&04)'. NOTHING PROCESSED

### Meaning

The first message identifier (FROM) must be lower than or equal to
the last message identifier (TO).

## MSMIF03

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMIF03 INVALID SELECTION CHARACTER '(&07)'. USE 'X' TO SELECT AND ' ' TO DE-SELECT

### Meaning

Selection must be effected with 'x' or 'X'.
De-selection must be effected with ' ' or NULL (null character).

## MSMIF04

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMIF04 INTERVAL '(&04)' IS TOO LARGE. NOTHING PROCESSED

### Meaning

The interval of message identifiers may not extend beyond a class.

## MSMIF05

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMIF05 INVALID NAME '(&07)': EMPTY OR NOT A STRUCTURED NAME

### Meaning

A structured name in the sense of SDF is a sequence of alphanumeric
characters (plus @, # and $) which may be separated by hyphens.
A structured name must begin with a letter or @ or # or $.

## MSMIK00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMIK00 INVALID COMMAND '(&07)'

## MSMIM00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMIM00 INVALID MESSAGE CLASS '(&07)'

### Meaning

A message class is composed of 3 letters (A to Z).

## MSMIM01

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMIM01 INVALID PROBLEM NUMBER '(&07)(&09)'

### Meaning

A problem number (PM) is composed of 8 alphanumeric characters
(A to Z, 0 to 9, @, # or $), plus a number between 1 and 366 for object
corrections.

## MSMIN00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMIN00 INVALID CSECT NAME '(&07)'

### Meaning

A csect name is composed of letters, digits, #, @, $ or _, and may not
begin with a digit.

## MSMIN01

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMIN01 INVALID SELECTION: 'ALL' NOT ALLOWED WITH ANOTHER VALUE

### Meaning

ALL means to generate all messages in the specified set.

## MSMIN02

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMIN02 INVALID FILE '(&05)': FILE GENERATION GROUPS NOT SUPPORTED IN THIS FUNCTION

## MSMIO00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMIO00 INVALID NAME '(&07)'

### Meaning

The name (in the sense of SDF) must be a sequence of alphanumeric
characters (plus @, # and $). It may not begin with a digit.

## MSMIO01

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMIO01 INVALID VERSION '(&07)'

### Meaning

The version must be a number between 0 and 999.

## MSMIO02

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMIO02 INVALID DATE '(&07)'

### Meaning

The year may be given on 2 or 4 digits, the month and day on 1 or 2
digits.
A 2-digits year is automatically prefixed with the century 19 (if year
>= 60) or 20 (year < 60).

## MSMI200

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMI200 INVALID OPEN MODE '(&07)'

### Meaning

The open mode must be:
- U: for update (modifications allowed)
- R: for read only (no modification allowed)
- C: for create (file must not exist); the file is then implicitly
opened in UPDATE mode.

## MSMI201

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMI201 INVALID MENU CHOICE '(&07)'

### Meaning

The value (&07) is not in the list of possible choices.

## MSMI400

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMI400 INVALID ROUTING CODE '(&07)'. NO MESSAGE PROCESSED

### Meaning

Valid routing codes are:
- A to Z
- 0 to 9
- $, #
- @: messages without reply are sent only to the CONSLOG file and
messages waiting for a reply are sent to the main console
- *: main console.
For more detailed information, see the BS2000 manual
'System Operator's Guide'.

## MSMI401

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMI401 INVALID WEIGHT '(&07)'

### Meaning

The weight must be a number between 0 and 99 (inclusive).
The conventions for its usage when the message is sent to a console are:
00 to 19: irrelevant, user-defined weight codes
20 to 39: message is a note; default value: 30
40 to 59: message is a warning; default value: 50
60 to 79: message describes a recoverable error; default value: 70
80 to 99: message is an unrecoverable error or a question.
Default value 90: suppressible question
98: question
99: error of highest priority.

## MSMI403

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMI403 INVALID VALUE '(&07)'

### Meaning

Possible values:
Y: yes
N: no.

## MSMI500

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMI500 INVALID INSERT NUMBER '(&07)' IN MESSAGE TEXT OF LANGUAGE '(&02)' FOR MESSAGE '(&00)'. OPERATION ABORTED

### Meaning

An insert number must be comprised between 00 and 29 (inclusive).
If the operation was applied to a set of messages:
- all messages before the one in error have been processed
- subsequent messages will not be processed.

## MSMI800

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMI800 INVALID FILE TYPE '(&07)'

### Meaning

Valid file types are:
C: CUSTOMER; the message file is attached to a customer product
S: STANDARD; the message file is attached to an official
product developed within FTS.
In a standard file, a component identification must be defined and
updated for each new version of the message file; it is used for
administration of the message files.

## MSMI801

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMI801 PRODUCT NAME '(&07)' IS NOT A STRUCTURED NAME

### Meaning

A product name must be a structured name in the sense of SDF, i.e. a
sequence of alphanumeric characters (plus @, # and $) which may be
separated by hyphens.
A structured name must begin with a letter or @ or # or $.

## MSMI900

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMI900 INVALID DEFAULT VALUE '(&07)', MUST BE ENCLOSED IN QUOTES

### Meaning

An insert default value must be enclosed between quotes ('...').
A null default value ('') is different from no default value (nothing or
only a single quote ').

## MSMI901

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMI901 Invalid insert number '(&07)'

### Meaning

An insert number must be between 00 and 29 (inclusive).

## MSMKADD

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMKADD F2=prompt F3=exit K2=interrupt K3=refresh

### Meaning

Internal use.
Function keys for ADD-MSG and MODIFY-MSG panels.

## MSMKAD2

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMKAD2 F2=prompt F3=exit K1=skip K2=interrupt K3=refresh

### Meaning

Internal use.
Function keys for ADD-MSG and MODIFY-MSG panels (for list processing).

## MSMKAD3

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMKAD3 F2=prompt F3=exit K1=cancel K2=interrupt K3=refresh

### Meaning

Internal use.
Function keys for ADD-MSG and MODIFY-MSG panels (in edit mode).

## MSMKCIN

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMKCIN F2=prompt K1=cancel K2=interrupt K3=refresh

### Meaning

Internal use.
Function keys for ADD- and MODIFY-CORRECTION-INFORMATION panels.

## MSMKCMI

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMKCMI F2=prompt K1=cancel K2=interrupt K3=refresh

### Meaning

Internal use.
Function keys for ADD- and MODIFY-COMPONENT-ID panels.

## MSMKCOP

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMKCOP F2=prompt F3=exit K2=interrupt K3=refresh

### Meaning

Internal use.
Function keys for COPY and MOVE panels.

## MSMKDCI

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMKDCI K1=cancel K2=interrupt K3=refresh

### Meaning

Internal use.
Function keys for DELETE-CORRECTION-INFORMATION panel.

## MSMKDCM

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMKDCM F3=exit K1=cancel K2=interrupt K3=refresh

### Meaning

Internal use.
Function keys for DELETE-COMPONENT-ID panel.

## MSMKDEL

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMKDEL F2=prompt F3=exit K2=interrupt K3=refresh

### Meaning

Internal use.
Function keys for first DELETE-MSG panel.

## MSMKDE2

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMKDE2 F3=exit K1=skip K2=interrupt K3=refresh

### Meaning

Internal use.
Function keys for second DELETE-MSG panel.

## MSMKDOC

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMKDOC F2=prompt K1=cancel K2=interrupt K3=refresh

### Meaning

Internal use.
Function keys for ADD-, MODIFY- and DELETE-DOCUMENTATION panels.

## MSMKGEN

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMKGEN F2=prompt F3=exit K2=interrupt K3=refresh

### Meaning

Internal use.
Function keys for GENERATE-CSECT panel.

## MSMKMEN

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMKMEN F2=prompt F3=end MSGMAKER K2=interrupt K3=refresh

### Meaning

Internal use.
Function keys for MENU panel.

## MSMKMFA

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMKMFA F2=prompt K1=cancel K2=interrupt K3=refresh

### Meaning

Internal use.
Function keys for MSG-FILE-ATTRIBUTES panel.

## MSMKSH1

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMKSH1 F2=prompt F3=exit K2=interrupt K3=refresh

### Meaning

Internal use.
Function keys for SHOW panel.

## MSMKSH2

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMKSH2 F2=prompt K1=cancel K2=interrupt K3=refresh

### Meaning

Internal use.
Function keys for SHOW-OUTPUT panel.

## MSMNH00

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

MSMNH00 MSGMAKER TERMINATED AFTER /EOF

## MSMNK00

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

MSMNK00 END OF FILE REACHED

## MSMNK01

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

MSMNK01 BEGINNING OF FILE REACHED

## MSMN100

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

MSMN100 (&09) INFORMATION ITEM(S) COPIED OR MOVED FROM FILE '(&05)' TO FILE '(&06)'

### Meaning

Possible information items:
- a message
- a DOCUMENTATION line
- a COMPONENT-IDentification (restricted to FTS internal use)
- CORRECTION-INFORMATION for a message class (restricted to FTS
internal use).

## MSMN101

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

MSMN101 MESSAGE '(&00)' ALREADY EXISTS IN FILE '(&05)': TRANSFORMING 'ADD-MSG' INTO 'MODIFY-MSG'

## MSMN102

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

MSMN102 MESSAGE '(&00)' DOES NOT EXIST IN FILE '(&05)': TRANSFORMING 'MODIFY-MSG' INTO 'ADD-MSG'

## MSMN103

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

MSMN103 OLD FILE FORMAT SAVED IN '(&05)'. CONVERSION COMPLETED

### Meaning

The file in old format (i.e. created with MSGEDIT) given for update
purposes is converted to a new format.
A copy of the old file format is cataloged under the name given in (&05).

## MSMN600

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

MSMN600 MSGMAKER TERMINATED NORMALLY

## MSMN601

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

MSMN601 MSGMAKER TERMINATED ABNORMALLY

### Meaning

At least one error was detected during the execution of MSGMAKER.

## MSMQC00

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

MSMQC00 Obsolete access '(&07)' in range '(&04)' of old file format. Change or ignore this range? Reply (<access>; I=IGNORE)

### Meaning

A range of messages to be copied or converted from a file in old format
(i.e. created with MSGEDIT) contains an ACCESS-METHOD attribute not
supported in the new file format.
(&07): access method from message in old file format
(&04): range of messages whose access method must be changed.

### Response

All the messages of the range given in insert (&04) may be either ignored
or assigned to another access method whose full name (no abbreviation)
must be given as reply:
<access> = ISAM, DLAM, LOCAL-DLAM, MINIMIP or BAMR.
Default reply:
- old access = NONE -> ignore the range of messages (I)
- old access = BAMP -> new access = BAMR.

## MSMQI00

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

MSMQI00 IDENTICAL OBJECTS IN FILES 1='(&05)' AND 2='(&06)'. PRIORITY? REPLY (1; 2; T=TERMINATE)

### Meaning

Some objects (messages, documentation lines, ...) exist with the same
identifier in the input files (&05) and (&06). Which of these files has
priority?

### Response

Possible answers:
1: the first file has priority each time an identical object is detected
in both files
2: the second file has priority each time an identical object is detected
in both files
T: stops the operation; the output file is in an inconsistent state.

## MSMQJ00

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

MSMQJ00 LANGUAGE '(&02)' ALREADY EXISTS IN MESSAGE '(&00)'. OVERWRITE? REPLY (Y=YES; N=NO; YY=ALWAYS FOR ALL ITEMS; NN=NEVER; T=TERMINATE)

### Meaning

An overwrite has been detected during a COPY or MOVE operation.
Some objects may have already been processed, in the following order:
- the message classes, intervals and msg-id's specified in the operation
are processed in alphabetical order
- for each specified class, interval or msg-id, the sequence of
processing is:
- messages in alphabetical order of message identifier
- documentation of the message class
- component identifier(s) of the message class (FTS internal use)
- correction information of the message class (FTS internal use).

### Response

Possible answers:
Y/N : applies only to language (&02) of message (&00)
YY/NN: applies to all following objects (messages, documentation, ...)
processed by the current operation
T: stops the operation; objects not yet processed are ignored.

## MSMQJ01

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

MSMQJ01 MESSAGE '(&00)' ALREADY EXISTS IN TARGET FILE. OVERWRITE? REPLY (Y=YES; N=NO; YY=ALWAYS; NN=NEVER; T=TERMINATE)

### Meaning

An overwrite has been detected during a COPY or MOVE operation.
Some objects may have already been processed, in the following order:
- the message classes, intervals and msg-id's specified in the operation
are processed in alphabetical order
- for each specified class, interval or msg-id, the sequence of
processing is:
- messages in alphabetical order of message identifier
- documentation of the message class
- component identifier(s) of the message class (FTS internal use)
- correction information of the message class (FTS internal use).

### Response

Possible answers:
Y/N : applies only to message (&00)
YY/NN: applies to all following objects (messages, documentation, ...)
processed by the current operation
T: stops the operation. Objects not yet processed are ignored.

## MSMQK00

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

MSMQK00 'SHOW' FORMATTING OF MORE THAN 1 MESSAGE CLASS FROM A LARGE MESSAGE FILE MAY TAKE A WHILE. EXECUTE 'SHOW'? REPLY (Y=YES; N=NO)

### Meaning

All required information for the SHOW operation is formatted before
being displayed. This may take a long time, depending on the amount of
information.

### Response

When processing large message files, select precisely the ranges or list
of messages to be output, in order to restrict the amount of messages to
be formatted.

## MSMQL00

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

MSMQL00 DOCUMENTATION LINE '(&04)' ALREADY EXISTS (COMMENTS='(&09)'). OVERWRITE? REPLY (Y=YES; N=NO)

### Response

Possible answers:
Y: overwrite the old documentation line
N: stops the operation; nothing is processed.

## MSMQN00

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

MSMQN00 FILE '(&05)' ALREADY EXISTS. OVERWRITE ? REPLY (Y=YES; N=NO)

### Response

Possible answers:
Y: overwrite the old file
N: ignore the file name and stop the processing.

## MSMQO00

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

MSMQO00 CLASS '(&00)' ALREADY CONTAINS A COMPONENT-ID (NAME='(&09)', VERSION='(&10)', DATE='(&11)'). OVERWRITE? REPLY (Y=YES, N=NO)

## MSMQO01

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

MSMQO01 COMPONENT VERSION MODIFIED FOR CLASS '(&00)'. DELETE CORRECTION-INFORMATION OF THIS CLASS? REPLY (Y=YES; N=NO)

### Meaning

The version of the COMPONENT-ID for the class (&00) has been modified.
The old CORRECTION-INFORMATION of this class should be removed before the
next transmission of the message file.

## MSMQ100

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

MSMQ100 OLD FILE FORMAT '(&05)'. CONVERT TO NEW FORMAT? REPLY (R=REPLACE; S=SAVE AND REPLACE; T=TERMINATE)

### Meaning

The file given for update purposes is in old format (i.e. created with
MSGEDIT); it must first be converted to a new format.
A file in old format may nevertheless be used for read purposes without
conversion.

### Response

The possible options are:
R: Replace: the old file format is replaced by the new format
S: Save and replace: the old file format is replaced by the new format
and a copy of the old file format is saved with the name
"<beginning of old file name>.OLD.<TSN>.<date>.<time>".
T: Terminate: the conversion is not performed and the current operation
is aborted.

## MSMQ300

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

MSMQ300 CERTAIN INFORMATION IN 'FROM-FILE' MUST BE IN A 'STANDARD' FILE. IGNORE OR CHANGE 'TO-FILE' TO 'STANDARD'? REPLY (I=IGNORE; S=STANDARD)

### Meaning

A message with access method MINIMIP or BAMR, a component identification
or correction information was encountered in the FROM-FILE.
The TO-FILE message file must be of type STANDARD to contain such
information.
A STANDARD file is a message file attached to an official product
developed within FTS and is restricted to FTS internal use.

### Response

Possible answers:
I: the operation continues but any information restricted to STANDARD
files is ignored
S: the type of the TO-FILE message file is changed to STANDARD;
the processing continues on all selected information.

## MSMQ301

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

MSMQ301 COMPONENT-ID OF NAME '(&09)' IN CLASS '(&00)' ALREADY EXISTS. OVERWRITE? REPLY (Y=YES; N=NO; YY=ALWAYS FOR ALL ITEMS; NN=NEVER; T=TERMINATE)

### Meaning

An overwrite has been detected during a COPY or MOVE operation.
Some objects may have already been processed, in the following order:
- the message classes, intervals and msg-id's specified in the operation
are processed in alphabetical order
- for each specified class, interval or msg-id, the sequence of
processing is:
- messages in alphabetical order of message identifier
- documentation of the message class
- component identifier(s) of the message class (FTS internal use)
- correction information of the message class (FTS internal use).

### Response

Possible answers:
Y/N : applies only to component identifier of name (&09) in message
class (&00)
YY/NN: applies to all following objects (messages, documentation, ...)
processed by the current operation
T: stops the operation; objects not yet processed are ignored.

## MSMQ302

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

MSMQ302 DOCUMENTATION FOR RANGE '(&04)' ALREADY EXISTS. OVERWRITE? REPLY (Y=YES; N=NO; YY=ALWAYS FOR ALL ITEMS; NN=NEVER; T=TERMINATE)

### Meaning

An overwrite has been detected during a COPY or MOVE operation.
Some objects may have already been processed, in the following order:
- the message classes, intervals and msg-id's specified in the operation
are processed in alphabetical order
- for each specified class, interval or msg-id, the sequence of
processing is:
- messages in alphabetical order of message identifier
- documentation of the message class
- component identifier(s) of the message class (FTS internal use)
- correction information of the message class (FTS internal use).

### Response

Possible answers:
Y/N : applies only to documentation line (&09)
YY/NN: applies to all following objects (messages, documentation, ...)
processed by the current operation
T: stops the operation; objects not yet processed are ignored.

## MSMRA00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMRA00 NO ACCESS TO EDT POSSIBLE

### Meaning

EDT cannot be called as a subprogram. MSGMAKER needs it to edit the
meaning and response texts.

### Response

Contact the system administrator.

## MSMRE00

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSMRE00 INTERNAL ERROR IN '(&14)': RETURN CODE '(&01)' RECEIVED FROM MACRO '(&09)'

### Meaning

An external product called by MSGMAKER is corrupted or not compatible.

### Response

Contact the system administrator.

## MSMRH00

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMRH00 INVALID PANEL LIBRARY

### Meaning

A library for the panels of MSGMAKER must be installed under the name
associated with the link name MAPLIB or with the logical ID SYSFHS
(default: '$.SYSFHS.MSGMAKER.<version>').
Possible errors are:
- no path name is associated with the logical ID SYSFHS
- the library does not exist
- the library does not match the version of MSGMAKER
- the library is incomplete
- the library cannot be read.

### Response

Remove the link name MAPLIB (command /REMOVE-FILE-LINK) or assign it
to another MSGMAKER panel library or contact the system
administrator.

## MSMRH01

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMRH01 MSGMAKER CANNOT BE USED IN DIALOG MODE ON THIS TYPE OF TERMINAL

### Meaning

The panels of MSGMAKER cannot be displayed on terminal types '3270',
'8161' and '8162'.
Panels in 8 bit format can be used only on 8 bit terminals.

### Response

- Try another terminal type, or
- Assign link name MAPLIB to another MSGMAKER panel library (or contact
the system administrator), or
- work only in batch or procedure mode.

## MSMRH10

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMRH10 WARNING: USER ERROR AT THE TERMINAL. TRY AGAIN

### Meaning

An invalid action was initiated at the terminal.

## MSMR600

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

MSMR600 Logical ID '(&09)' not found in Software Configuration Inventory for (&10) V(&11). GETINSP macro returned '(&07)'

### Meaning

The logical identifier (&09) was not found for the product (&10) with
version (&11) because it is not correctly registered in the Software
Configuration Inventory.
The installation path manager (IMON-GPN) returned the error (&07).

### Response

Use the installation path manager to check that the product has been
correctly installed.

## MSMR70C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMR70C STATEMENT LENGTH EXCEEDS MAXIMUM SDF BUFFER SIZE

### Meaning

SDF does not support reading of a statement beyond a maximum length.

### Response

Split the statement into multiple statements.

## MSMR71C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMR71C INVALID STATEMENT OR ACTION

### Meaning

The text entered in the command line is neither a valid statement nor a
valid action.

## MSMR710

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMR710 END OF STATEMENT INPUT MEDIUM REACHED BEFORE //END STATEMENT

### Meaning

During reading of the statements, end of file (or /EOF) was reached before
the //END statement.

## MSMR720

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMR720 ERROR RECEIVED FROM SDF: DIALOG NOT POSSIBLE

### Meaning

SDF is not fully operational.

### Response

Contact the system administrator.

## MSMR73C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMR73C ERROR RECEIVED FROM SDF: PROGRAM 'MSGMAKER' NOT KNOWN IN SYNTAX FILE

### Meaning

The system syntax file does not contain the statements of MSGMAKER.

### Response

Contact the system administrator.

## MSMTDCI

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMTDCI Press <DUE> to delete all problem numbers or <K1> to cancel deletion

### Meaning

Internal use.

## MSMTDCM

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMTDCM <DUE> = delete, <K1> = cancel deletion of this component-id, <F3> = exit

### Meaning

Internal use.

## MSMTDO1

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMTDO1 Add new lines. Data fields are optional.

### Meaning

Internal use.

## MSMTDO2

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMTDO2 Modify existing lines, type new ones. Data fields are optional.

### Meaning

Internal use.

## MSMTDO3

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMTDO3 Select lines to remove with the character "x".

### Meaning

Internal use.

## MSMTDST

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMTDST USER-TASK CONSOLE

### Meaning

Internal use.
Constant text at offsets 0 and 30.

## MSMTED1

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMTED1 To set overwrite mode: <F2>. To quit EDT: <K1> (=cancel) or RETURN

### Meaning

Internal use.

## MSMTED2

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMTED2 Language EDT screen Language Msg text

### Meaning

Internal use.
Constant text at offsets 0, 20, 40 and 60.

## MSMTED3

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMTED3 < M E A N I N G (maximum 256 lines) Msg-id: (&00) Language: (&02) >!!!!!!

### Meaning

Internal use.

## MSMTED4

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMTED4 < R E S P O N S E (maximum 256 lines) Msg-id: (&00) Language: (&02) >!!!!!!

### Meaning

Internal use.

## MSMTYES

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMTYES YES NO

### Meaning

Internal use.
Constant text at offsets 0 and 10.

## MSMWB00

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMWB00 WARNING: MESSAGE TEXT FOR LANGUAGE '(&02)' OF MESSAGE '(&00)' HAS BEEN TRUNCATED

### Meaning

In the MSG-TXT panel, the message texts are truncated after
240 characters.

### Response

The truncation may be canceled with K1 or accepted with DUE.

## MSMWC00

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMWC00 WARNING: MULTIPLE INSERT DEFAULT VALUES DETECTED FOR SAME INSERT IN MESSAGE '(&00)'. ALL BUT FIRST DEFAULT VALUES ARE IGNORED

### Meaning

In this new message file format, only one default value per insert may be
defined for all languages of a message.
As several default values for the same insert were read, only the default
value of the first language in alphabetical order is taken into account.
The other default values for the same insert are ignored.
This warning is displayed only once for the whole message file(s). Other
messages could be concerned by the same problem; this warning will
nevertheless not be repeated for them.

## MSMWC01

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMWC01 WARNING: MULTIPLE 'AUTOMATIC HELP' PREFIXES DETECTED FOR SAME INSERT IN MESSAGE '(&00)'. ALL PREFIXES IGNORED EXCEPT FIRST ONE

### Meaning

Only one AUTOMATIC HELP prefix per insert may be defined for all languages
of a message.
As several prefixes for the same insert were read, only the prefix of the
first language in alphabetical order is taken into account.
The other prefixes for the same insert are ignored.
This warning is displayed only once for the whole message file(s). Other
messages could be concerned by the same problem; this warning will
nevertheless not be repeated for them.

## MSMWC02

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMWC02 WARNING: ACCESS METHOD 'NONE' NOT SUPPORTED. MESSAGES IN RANGE '(&04)' OF FILE '(&05)' IGNORED

### Meaning

A range of messages to be copied or converted from a file in old format
(i.e. created with MSGEDIT) contains an "access method" attribute not
supported in the new file format.
All messages in range (&04) are ignored, i.e. not copied or converted.
This warning is displayed only once for the whole message file(s). Other
messages could be concerned by the same problem; this warning will
nevertheless not be repeated for them.

## MSMWC03

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMWC03 WARNING: ACCESS METHOD 'BAMP' NO LONGER SUPPORTED. 'BAMR' SET AS DEFAULT FOR ALL MESSAGES IN RANGE '(&04)' OF FILE '(&05)'

### Meaning

A range of messages to be copied or converted from a file in old format
(i.e. created with MSGEDIT) contains an "access method" attribute not
supported in the new file format.
The access method of the messages in range (&04) is changed to BAMR.
This warning is displayed only once for the whole message file(s). Other
messages could be concerned by the same problem; this warning will
nevertheless not be repeated for them.

## MSMWG00

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMWG00 WARNING: INVALID OR MISSING RANGE RECORD(S) IN FILE '(&05)'. RISK OF MISSING INFORMATION

### Meaning

Invalid or missing range definitions were detected in the directory of a
message file in old format (i.e. produced with MSGEDIT).
Message attributes, messages or other objects (DOCUMENTATION, ...)
attached to these invalid ranges or attached to no range could be not
read.

### Response

Correct the old message file or use it carefully.

## MSMWI00

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMWI00 WARNING: IDENTICAL OBJECTS IN FILES '(&05)' AND '(&06)'. FIRST FILE HAS PRIORITY

### Meaning

Some objects (messages, documentation lines, ...) exist with the same
identifier in the input files (&05) and (&06).
The first file (&05) has priority each time an identical object is
detected in both files.

## MSMWJ00

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMWJ00 WARNING: NO INFORMATION FOUND IN THE SPECIFIED SET OF MESSAGE IDENTIFIERS

### Meaning

Nothing was generated in the output file(s) because no selected
information was found in the specified set of message identifiers.

## MSMWJ01

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMWJ01 WARNING: TYPE OF FILE '(&05)' CHANGED TO 'STANDARD'

### Meaning

A message with access method MINIMIP or BAMR, a component identification
or correction information was encountered in the file (&05).
The message file must be of type STANDARD to contain such information.
A STANDARD file is a message file attached to an official product
developed within FTS and is restricted to FTS internal use.
The file type was changed from CUSTOMER to STANDARD and the processing
continued.

## MSMWL00

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMWL00 WARNING: NO DOCUMENTATION TO BE DELETED IN SPECIFIED INTERVAL

## MSMWM00

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMWM00 WARNING: CLASS '(&00)(&04)' DOES NOT CONTAIN ANY CORRECTION-INFORMATION TO BE DELETED

### Meaning

(&00): message class, or
(&04): range of message classes.

## MSMWO00

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMWO00 WARNING: CLASS '(&00)(&04)' DOES NOT CONTAIN ANY COMPONENT-ID TO BE DELETED

### Meaning

(&00): message class, or
(&04): range of message classes.

## MSMWP00

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMWP00 WARNING: SAME MESSAGE ELEMENT '(&09)(&10)(&11)' MODIFIED SEVERAL TIMES

### Meaning

A same message element is modified (at least) twice, i.e.:
- a message attribute
- a message text in the same language
- a meaning or response line number in the same way (*ADD, *INSERT, ...)
for the same language
- an attribute of the same insert number.
The last modification overlaps the previous ones for the same message
element.

## MSMW100

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMW100 WARNING: RANGE '(&04)' DOES NOT CONTAIN ANY MESSAGES TO BE DELETED

## MSMW101

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMW101 WARNING: MESSAGE '(&00)' DOES NOT EXIST

## MSMW102

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMW102 WARNING: RANGE '(&04)' DOES NOT CONTAIN ANY LANGUAGE TO BE DELETED

## MSMW103

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMW103 WARNING: MESSAGE '(&00)' DOES NOT CONTAIN ANY LANGUAGE TO BE DELETED

## MSMW104

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMW104 COPY INTO OLD FORMAT MESSAGE FILE PERFORMED WITH RESTRICTIONS. PROCESSING CONTINUED

### Meaning

The COPY operation into an old format message file has the following
restrictions :
- the DOCUMENTATION, CORRECTION-INFORMATION and insert names are not
copied
- all the languages must be copied (LANGUAGES=*ALL)
- the copied information (messages and/or component-id) must not exist in
the TO-FILE; no checks for overwriting are performed.
If the information already exist in the TO-FILE, the result may be not
consistent!

### Response

Verify that the previous conditions are fulfilled.

## MSMW500

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMW500 WARNING: SUM OF INSERT DEFAULT VALUES EXCEEDS (&09) CHARACTERS IN MESSAGE '(&00)'. INSERTS COULD BE TRUNCATED AT MSG7(X) TIME

### Meaning

The sum of the insert values is limited to (&09) characters when the
message is output with a MSG7(X) macro (BS2000/OSD V1 only).

### Response

Use shorter insert values to avoid truncation.

## MSMW501

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMW501 WARNING: IN MESSAGE '(&00)' TEXT IN LANGUAGE '(&02)' PLUS INSERT DEFAULT VALUES EXCEED (&09) CHARACTERS. TRUNCATION POSSIBLE AT MSG7(X) OUTPUT TO CONSOLE

### Meaning

The message text with its insert values is limited to (&09) characters
when the message is output to the console with a MSG7(X) macro.
The output text length may vary according to the current insert values and
MSG7X options such as TIMESTAMP, DATESTAMP and TXTONLY.

### Response

Use shorter text or insert values to avoid truncation.

## MSMW502

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMW502 WARNING: CHARACTER '(&07)' NOT INDEPENDENT OF CHARACTER SET VARIANT IN MESSAGE TEXT OF LANGUAGE '(&02)' FOR MESSAGE '(&00)'

### Meaning

Some characters have multiple meanings according to the variant of the
standard character set used when the message is output (MSG7(X) macro or
/HELP-MSG-INFORMATION command). These characters have the hexadecimal
codes X'4F', X'BB', X'BC', X'BD', X'FB', X'FD' and X'FF'
(see EBCDIC.DF.03 character code).
To ensure a correct output in any case, such characters should not be
used.

## MSMW503

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMW503 WARNING: CHARACTER '(&07)' NOT INDEPENDENT OF CHARACTER SET VARIANT IN MEANING OF LANGUAGE '(&02)' FOR MESSAGE '(&00)'

### Meaning

Some characters have multiple meanings according to the variant of the
standard character set used when the message is output (MSG7(X) macro or
/HELP-MSG-INFORMATION command). These characters have the hexadecimal
codes X'4F', X'BB', X'BC', X'BD', X'FB', X'FD' and X'FF'
(see EBCDIC.DF.03 character code).
To ensure a correct output in any case, such characters should not be
used.

## MSMW504

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMW504 WARNING: CHARACTER '(&07)' NOT INDEPENDENT OF CHARACTER SET VARIANT IN RESPONSE OF LANGUAGE '(&02)' FOR MESSAGE '(&00)'

### Meaning

Some characters have multiple meanings according to the variant of the
standard character set used when the message is output (MSG7(X) macro or
/HELP-MSG-INFORMATION command). These characters have the hexadecimal
codes X'4F', X'BB', X'BC', X'BD', X'FB', X'FD' and X'FF'
(see EBCDIC.DF.03 character code).
To ensure a correct output in any case, such characters should not be
used.

## MSMW505

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMW505 WARNING: CHARACTER '(&07)' NOT INDEPENDENT OF CHARACTER SET VARIANT IN DEFAULT VALUE OF INSERT '(&09)' FOR MESSAGE '(&00)'

### Meaning

Some characters have multiple meanings according to the variant of the
standard character set used when the message is output (MSG7(X) macro or
/HELP-MSG-INFORMATION command). These characters have the hexadecimal
codes X'4F', X'BB', X'BC', X'BD', X'FB', X'FD' and X'FF'
(see EBCDIC.DF.03 character code).
To ensure a correct output in any case, such characters should not be
used.

## MSMW506

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMW506 Warning: message with only 'ACCESS=MINIMIP' will be ignored in the message file by MIP

### Meaning

Although created in a message file, messages with ACCESS-METHOD=MINIMIP
are ignored by MIP.
Such messages are created for generation in a CSECT with the
GENERATE-CSECT function of MSGMAKER. Then the CSECT must be integrated as
component of the BS2000/OSD CP.
Meaning and response texts are never generated in a CSECT with
GENERATE-CSECT.

### Response

To allow MIP to process this message from a message file, another access
method (ILAM, DLAM, ...) must be added to MINIMIP.

## MSMW900

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMW900 WARNING: DEFAULT VALUE FOR INSERT NUMBER '(&09)' OF MESSAGE '(&00)' HAS BEEN TRUNCATED

### Meaning

In the INSERT-ATTRIBUTES panel, the default values for the inserts
are truncated after 54 characters.

### Response

The truncation may be canceled with K1 or accepted with DUE.

## MSMW901

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

MSMW901 WARNING: NAME FOR INSERT NUMBER '(&09)' OF MESSAGE '(&00)' HAS BEEN TRUNCATED

### Meaning

In the INSERT-ATTRIBUTES panel, the names for the inserts
are truncated after 20 characters.

### Response

The truncation may be canceled with K1 or accepted with DUE.

## MSMZ000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMZ000 INTERNAL ERROR IN '(&14)': FILE (HANDLE='(&07)') CLOSED TWICE OR NOT OPENED

### Response

Send a maximum of information (description of the last operations, message
file, procedure, user dump, ...) to the MSGMAKER administrator.

## MSMZ100

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMZ100 INTERNAL ERROR IN '(&14)': THIS PROCESS FUNCTION SHOULD NEVER BE CALLED

### Response

Send a maximum of information (description of the last operations, message
file, procedure, user dump, ...) to the MSGMAKER administrator.

## MSMZ500

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMZ500 OUT OF MEMORY DETECTED WHEN TRYING TO ALLOCATE (&09) MORE BYTES

### Response

Send a maximum of information (description of the last operations, message
file, procedure, user dump, ...) to the MSGMAKER administrator.

## MSMZ501

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMZ501 INTERNAL ERROR IN '(&14)': DUPLICATE NAME (OLD = '(&10)', NEW = '(&07)') FOR INSERT '(&09)' OF MESSAGE '(&00)'

### Response

Send a maximum of information (description of the last operations, message
file, procedure, user dump, ...) to the MSGMAKER administrator.

## MSMZ502

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMZ502 INTERNAL ERROR IN '(&14)': C ERROR CODE '(&07)' DURING '(&10)' OPERATION ON FILE '(&05)'

### Response

Send a maximum of information (description of the last operations, message
file, procedure, user dump, ...) to the MSGMAKER administrator.

## MSMZ601

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMZ601 INTERNAL ERROR IN '(&14)': NO DIALOG FUNCTION FOR STATE '(&09)'

### Response

Send a maximum of information (description of the last operations, message
file, procedure, user dump, ...) to the MSGMAKER administrator.

## MSMZ602

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMZ602 INTERNAL ERROR IN '(&14)': NO PROCESS FUNCTION FOR STATE '(&09)', COND '(&10)', DIA_COND '(&11)'

### Response

Send a maximum of information (description of the last operations, message
file, procedure, user dump, ...) to the MSGMAKER administrator.

## MSMZ603

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMZ603 INTERNAL ERROR IN '(&14)': NO TRANSITION FOR STATE '(&09)', COND '(&10)', DIA_COND '(&11)'

### Response

Send a maximum of information (description of the last operations, message
file, procedure, user dump, ...) to the MSGMAKER administrator.

## MSMZ700

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

MSMZ700 INTERNAL ERROR IN '(&14)': NO STATEMENT DEFINED FOR INTERNAL NAME '(&07)'

### Response

Send a maximum of information (description of the last operations, message
file, procedure, user dump, ...) to the MSGMAKER administrator.

©2024 Fujitsu | BS2000 System Messages