## NKD0001

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : NO

NKD0001 SYNTAX ERROR IN '(&00)' COMMAND. COMMAND NOT PROCESSED

### Meaning

(&00): /SHOW command of the nucleus device management.

### Response

Enter the correct command.

## NKD0002

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0002 REQUESTED INFORMATION COULD NOT BE OBTAINED. RETRY COMMAND LATER

### Meaning

The current system state prevented the processing of the command.

## NKD0005

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0005 WARNING: REQUESTED INFORMATION NOT COMPLETE

### Meaning

The requested information could be obtained and displayed only partially.
Possible reasons:
1. Some of the HW units that were selected do not exist in the system.
2. In the command /SHOW-DISK-STATUS resp. /SHOW-TAPE-STATUS only
disk resp. tape units are processed.
3. The selected additional operands (e.g. INFORMATION) do not allow
to issue information about some HW units.

### Response

Check the input.

## NKD0006

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0006 SOFTWARE ERROR IN PROCEDURE '(&00)'. PROCESSING CONTINUES

### Meaning

Inconsistency in system module.
(&00): procedure of the nucleus device management information
facility (NKD).

### Response

Contact the system administrator.

## NKD0007

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0007 USER IDENTIFICATION CANNOT OBTAIN THIS INFORMATION. '(&00)' COMMAND NOT PROCESSED

### Meaning

The command is not permitted for the user ID.
(&00): /SHOW command of the nucleus device management.

## NKD0009

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0009 WARNING: (&00) MONITOR TEMPORARILY NOT AVAILABLE. INFORMATION MAY NOT BE COMPLETE

## NKD0010

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0010 (&00) MONITOR TEMPORARILY NOT AVAILABLE. RETRY '(&01)' COMMAND LATER

## NKD0011

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0011 USER ID CANNOT OBTAIN INFORMATION ON TSN (&00). COMMAND NOT PROCESSED

### Meaning

The user task and the TSN (&00) have different user IDs.

### Response

Correct the command.

## NKD0012

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : NO

NKD0012 NO INFORMATION EXISTS FOR SPECIFIED DEVICE-RANGE

## NKD0013

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0013 COMMAND '(&00)' WITHOUT EXPLICIT PARAMETERS NOT ALLOWED.COMMAND NOT PROCESSED

### Response

Use the selection parameters or '(&00)' TYPE=ALL
to obtain information about all devices.

## NKD0014

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0014 NO ALLOCATION EXISTS FOR THE TASK WITH TSN (&00). COMMAND NOT PROCESSED

## NKD0016

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0016 NO RELEVANT INFORMATION EXISTS FOR 'TSN = (&00)' AND 'INFORMATION = (&01)'. COMMAND NOT PROCESSED

### Meaning

(&00),(&01): operand values of the specified /SHOW command.

## NKD0018

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0018 MONJV NOT FOUND. JVS RETURN CODE: '(&00)'. ERROR INF IN SYSTEM MODE: /HELP JVS(&00)

### Meaning

(&00): result of an unsuccessful search for the specified MONJV by the
JV management.
Note: '(&00)' corresponds to 'JVS(&00)'.
For more detailed information on the JVS return code enter /HELP JVS(&00)
or see the manual 'System Messages'.

## NKD0019

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0019 FOUND JOB VARIABLE IS NOT AN ACTIVE MONJV

### Meaning

The entered string is the name of a job variable, but its contents does
not denote an active MONJV.

### Response

Check the command as well as the JV state and the JV contents.

## NKD0021

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0021 NO INFORMATION EXISTS FOR 'TYPE = (&00)' AND 'ATTRIBUTE = (&01)'. COMMAND NOT PROCESSED

### Meaning

(&00),(&01): operand values of the specified /SHOW command.

## NKD0023

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0023 NO INFORMATION EXISTS FOR UNIT = '(&00)'. COMMAND NOT PROCESSED

### Meaning

(&00): mnemonic of the requested unit class (list possible).

## NKD0024

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0024 NO INFORMATION EXISTS FOR 'CLASS = (&00)' AND 'ATTRIBUTE = (&01)'. COMMAND NOT PROCESSED

### Meaning

(&00),(&01): operand values of the specified /SHOW command.

## NKD0025

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0025 NO RELEVANT INFORMATION EXISTS FOR UNIT = '(&00)' AND 'INFORMATION = (&01)'. COMMAND NOT PROCESSED

### Meaning

(&00),(&01): operand values of the specified /SHOW command.

## NKD0026

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0026 SUBSYSTEM JVS NOT LOADED.COMMAND CANNOT BE PROCESSED

### Meaning

The command was issued with parameter MONJV (Monitor Job Variable).
The JVS (Job Variable Subsystem) is currently not loaded.
Therefore the command cannot be processed.

## NKD0027

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0027 NO INFORMATION EXISTS FOR UNIT = '(&00)'

### Meaning

NO INFORMATION CONCERNING THE UNITS '(&00)' EXISTS OR THE USER IS NOT
PRIVILEGED TO GET RELEVANT INFORMATION.

## NKD0028

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0028 WARNING : NO RELEVANT INFORMATION EXISTS FOR UNIT = '(&00)' AND INFORMATION = '(&01)'

### Meaning

THE UNITS '(&00)' ARE NOT GENERATED IN THE SYSTEM OR THE USER IS NOT
PRIVILEGED TO OBTAIN INFORMATION '(&01)'.

### Response

NO RESPONSE POSSIBLE. TRY OTHER MNEMONICS.

## NKD0030

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0030 OPERAND CHANGED TO 'INFORMATION = (&00)'. PROCESSING CONTINUES

### Meaning

In the specified /SHOW command only INFORMATION = (&00) is permissible as
an operand value.

## NKD0031

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0031 NO INFORMATION EXISTS FOR 'VOLUME = (&00)'. COMMAND NOT PROCESSED

### Meaning

(&00): operand value of the specified /SHOW command.

## NKD0032

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0032 NO RELEVANT INFORMATION EXISTS FOR 'ATTRIBUTE = (&00)'. COMMAND NOT PROCESSED

### Meaning

(&00): operand value of the specified /SHOW command.

## NKD0033

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0033 NO RELEVANT INFORMATION EXISTS FOR 'VOLUME = (&00)' AND 'INFORMATION = (&01)'. COMMAND NOT PROCESSED

### Meaning

(&00),(&01): operand values of the specified /SHOW command.

## NKD0034

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0034 WARNING : NO RELEVANT INFORMATION EXISTS FOR 'VOLUME = (&00)'

## NKD0035

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0035 WARNING : NO RELEVANT INFORMATION EXISTS FOR 'VOLUME = (&00)' AND 'INFORMATION = (&01)'

## NKD0036

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0036 NO INFORMATION EXISTS FOR 'LOCATION = (&00)'. COMMAND NOT PROCESSED

### Meaning

(&00): operand value of the specified /SHOW command.

## NKD0037

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0037 NO INFORMATION EXISTS FOR ROUTING-CODE = '(&00)'

### Meaning

THERE IS NO LOCATION WITH THE GIVEN ROUTING-CODE

## NKD0038

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0038 NO DEVICE OF TYPE = (&00) HAS BEEN ASSIGNED TO A LOCATION

### Meaning

Because no device of type (&00) has been assigned to a location the
command SHOW-DEVICE-STATUS with INFORMATION = LOCATION delivers no
output.

### Response

The user may try SHOW-DEVICE-STATUS with other Informationparameters
(STANDARD/ALL/SUMMARY/TYPTASK) to get information relevant to type (&00)

## NKD0039

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0039 NO INFORMATION EXISTS FOR LOCATION = '(&00)'

### Meaning

THE LOCATIONS '(&00)' DO NOT EXIST IN THE SYSTEM.

### Response

ENTER ' SH-DEV-D ' WITHOUT PARAMETERS TO GET A DISPLAY OF ALL LOCATIONS.

## NKD0040

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0040 NO SECURE QUEUE EXISTS. COMMAND NOT PROCESSED

### Meaning

No task is waiting for its /SECURE resp. /SECURE-RESOURCE-ALLOCATION
command to be processed.

## NKD0041

Destination: USER-TASK, CONSOLE Routing code: E Weight: 70

Warranty : YES

NKD0041 NO COLLECTOR TASK EXISTS. COMMAND NOT PROCESSED

### Meaning

Either RESOURCE-COLLECTION is not set or no task has been created as a
collector task. Use INFORMATION=COLLECT to obtain further information.

©2024 Fujitsu | BS2000 System Messages