## NKRREVI

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NKRREVI COMP=NKRMF,VER=940,DATE=2023-09-12,COMPNR=22212301

## NKR0000

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0000 NKR DETECTED SOFTWARE ERROR: (&00). TAKE DUMP

### Meaning

The message is issued only during STARTUP.
(&00): description of the detected error.

## NKR0001

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0001 '(&00)': SYSTEM RECONFIGURATION IMPOSSIBLE

### Meaning

(&00) was to be detached by the operating system due to a hardware error.
The reconfiguration can, however, not be processed, as otherwise no
regular continuation of the session would be possible.

### Response

1. Take dump (incl. HERS-file) and call hardware maintainance.
2. Check the I/O paths and the state of hardware units,
beginning with (&00).

## NKR0006

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0006 SYNTAX ERROR IN COMMAND '(&00)'. COMMAND REJECTED

### Meaning

(&00): reconfiguration command.

### Response

Enter correct command.

## NKR0007

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0007 INCONSISTENT NUMBER OF DEVICES IN DEVICE-RANGE.

### Meaning

During computation of device addresses using first address and number of
devices the maximum possible value of X'FF' will be exceeded.

## NKR0008

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0008 INCONSISTENT REPEAT FACTOR.

### Meaning

The following errors are possible:
1) UNIT NAME not hexadecimal or not of 4 characters.
2) With specified REPEAT factor the admissible value range for mnemonics
will be exceeded.

## NKR0009

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0009 *CHN AND *CTL MAY NOT BE MIXED IN PATH LIST.

### Meaning

The specification of *CHANNEL(...) together with *CONTROLLER(...) ist not
possible in path list.

## NKR0010

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0010 '(&01)(&00)': ATTACH-DEVICE NOT SUPPORTED.

## NKR0016

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0016 MNEMONIC '(&01) (&00)' INVALID. MN IGNORED

### Meaning

Unit (&01)(&00) is unknown in the system and has been ignored.

### Response

Check specified mnemonic and unit-class and correct the command.

## NKR0017

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0017 '(&02)(&00) (&03)(&01)': SPECIFICATION NOT PERMITTED. NO RECONFIGURATION POSSIBLE FOR THIS PATH

### Meaning

Either one of the specified units (&02)(&00) and (&03)(&01) is unknown or
the path (&02)(&00) (&03)(&01) is unknown or the combination of specified
unit-classes is not allowed.

### Response

Check specified mnmonics and unit-classes and correct the command.

## NKR0018

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0018 DEVICE TYPE NOT SUPPORTED

### Meaning

The type of the device is not supported in actual system version.

## NKR0020

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0020 /DETACH-DEVICE FOR MN '(&01)(&00)' ACCEPTED

### Meaning

At least one volume device for which I/O s are still to be performed
by the system, is to be detached.
The command will be executed after the end of all buffer I/O s, at
the latest after a waiting time of two minutes.

## NKR0021

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0021 PATH '(&02)(&00) (&03)(&01)': /REMOVE-DEVICE-CONNECTION ACCEPTED

### Meaning

At least one volume device for which I/O s are still to be performed
by the system is to be detached implicitly.
The command will be executed after the end of all buffer I/Os,
at the latest after a waiting time of two minutes.

## NKR0022

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0022 (&01)(&02)(&00) ACCEPTED.

### Meaning

The command (&00) will be processed for hardware unit (&01)(&02).

## NKR0025

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0025 PATH '(&02)(&00) (&03)(&01)' INVALID

### Meaning

The path between inner unit (&02)(&00) and outer unit (&03)(&01) is
physically not available and its configuration state is set to 'INVALID'.
This message is issued if the path is generated in BS2000 but not in the
IORSF.

## NKR0026

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0026 '(&01)(&00)' INVALID

### Meaning

Unit (&01)(&00) is physically not available and its configuration state
was set to 'INVALID'. The device is generated in BS2000, but not in the
IORSF.

## NKR0030

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0030 PATH '(&02)(&00) (&03)(&01)' DOES NOT EXIST

## NKR0031

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0031 '(&01)(&00)': CORRESPONDING CPU NOT AVAILABLE

### Meaning

(&01)(&00): mnemonic of the I/O processor to be attached.

### Response

Attach the relevant CPU, then try again.

## NKR0033

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0033 '(&01)(&00)' IS THE ONLY OPERABLE BYTE-MUX CHANNEL

### Meaning

The specified reconfiguration request would cause the last or only
operable BYTE-MUX channel to be detached.

## NKR0034

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0034 RECONFIGURATION OF THE ONLY OPERABLE CONSOLE

### Meaning

The specified reconfiguration request would cause the last or only
operable console to be detached.

## NKR0035

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0035 PATH '(&02)(&00) (&03)(&01)' IS THE LAST INCLUDED PATH

### Meaning

The reconfiguration request caused/would cause a removal of the last or
only path to
- a paging volume,
- a public volume,
- a communication device.

## NKR0036

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0036 '(&01)(&00)': PUBLIC VOLUME MOUNTED

### Meaning

As the hardware unit (&01)(&00) is vital for the system, a transition into
the state DETACHED-EXPLICITLY or DETACHED-IMPLICITLY is not permitted.

### Response

Mount the volume first on another device by means of /CHANGE-DISK-MOUNT,
then try again.

## NKR0037

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0037 '(&01)(&00)' MAY CURRENTLY NOT BE DETACHED

### Meaning

The hardware unit with the mnemonic (&01)(&00) is still allocated.

### Response

Try the appropriate reconfiguration command again with parameter FORCE=YES
or enter the /SHOW-DEVICE-STATUS command for more detailed information.

## NKR0038

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0038 RECONFIGURATION OF A SINGLE CONSOLE HARDCOPY NOT ALLOWED

## NKR0039

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0039 THE MAIN CONSOLE MAY NOT BE DETACHED

### Response

Define another console as the main console by means of the /ASR command,
then try again.

## NKR0040

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0040 '(&01)(&00)' ATTACHED

### Meaning

The reconfiguration request has been performed successfully, the hardware
unit (&01)(&00) is attached.

## NKR0041

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0041 HW UNIT '(&01)(&00)' ALREADY ATTACHED

## NKR0042

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0042 '(&01)(&00)': ATTACH ACCEPTED

### Meaning

The hardware unit (&01)(&00) will be attached after a necessary I/O has
been performed successfully.

## NKR0044

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0044 '(&01)(&00)': ATTACHMENT REJECTED

### Meaning

The hardware unit (&01)(&00) could not be attached. The reason for the
rejection has been explained in the preceding message(s).
For more detailed information on the error cause enter /HELP for the
corresponding messages, or see the manual 'System Messages'.

## NKR0045

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0045 *** '(&01)(&00)' DETACHED ***

### Meaning

The reconfiguration request has been performed successfully, the hardware
unit (&01)(&00) is detached.

## NKR0046

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0046 '(&01)(&00)' DETACHED IMPLICITLY

### Meaning

All inner paths of the unit (&01)(&00) are REMOVED-EXPLICITLY and/or
REMOVED-IMPLICITLY.
For more detailed information enter /SHOW-DEVICE-CONFIGURATION.

## NKR0047

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0047 HW UNIT '(&01)(&00)' ALREADY DETACHED

## NKR0048

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0048 *** '(&01)(&00)' DETACHED BY SYSTEM ***

### Meaning

The reconfiguration request was initiated by the operating system,
because the hardware unit (&01)(&00) could not be accessed or produced
unrecoverable hardware errors. The request was successfully performed,
(&01)(&00) is detached.

### Response

Check unit (&01)(&00) and call maintainance, if necessary.

## NKR0049

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0049 '(&01)(&00)': DETACHMENT REJECTED

### Meaning

The hardware unit (&01)(&00) could not be detached. The reason for the
rejection has been explained in the preceding NKR message(s).
For more detailed information on the error cause enter /HELP for the
corresponding NKR message(s), or see the manual 'System Messages'.

## NKR0050

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0050 PATH '(&02)(&00) (&03)(&01)' INCLUDED

### Meaning

The reconfiguration request has been performed successfully, the path
(&02)(&00) (&03)(&01) is included.

## NKR0051

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0051 PATH '(&02)(&00) (&03)(&01)' ALREADY INCLUDED

### Meaning

Path already included.

## NKR0054

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0054 PATH '(&02)(&00) (&03)(&01)': INCLUDE REJECTED

### Meaning

The path (&02)(&00) (&03)(&01) could not be included. The reason for the
rejection has been explained in the preceding NKR message(s).
For more detailed information on the error cause enter /HELP for the
preceding NKR messages, or see the manual 'System Messages'.

## NKR0055

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0055 PATH '(&02)(&00) (&03)(&01)' REMOVED

### Meaning

The reconfiguration request has been performed successfully.

## NKR0056

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0056 PATH '(&02)(&00) (&03)(&01)' REMOVED IMPLICITLY

### Meaning

Path is DETACHED-EXPLICITLY and/or DETACHED-IMPLICITLY.

### Response

Enter /SHOW-DEVICE-CONFIGURATION for more detailed information.

## NKR0057

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0057 PATH '(&02)(&00) (&03)(&01)' ALREADY REMOVED

### Meaning

Path already removed.

## NKR0059

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0059 PATH '(&02)(&00) (&03)(&01)': REMOVE REJECTED

### Meaning

The path (&02)(&00) (&03)(&01) could not be removed. The reason for the
rejection is explained in the preceding NKR message(s).
For more detailed information on the error cause enter /HELP for the
preceding NKR message(s) or see the manual 'System Messages'.

## NKR0060

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0060 HW UNIT '(&01)(&00)' ALREADY DETACH-PENDING

## NKR0061

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0061 HW UNIT '(&01)(&00)' DETACH-PENDING EXPLICITLY

## NKR0062

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0062 HW UNIT '(&01)(&00)' DETACH-PENDING IMPLICITLY

### Meaning

(&00): mnemonic of a hardware unit.
All the inner paths of (&01)(&00) are REMOVE-PENDING EXPLICITLY and/or
REMOVE-PENDING IMPLICITLY.

### Response

Enter /SHOW-DEVICE-CONFIGURATION for more detailed information.

## NKR0064

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0064 HW UNIT '(&01)(&00)' DETACH-PENDING REJECTED

### Meaning

The hardware unit (&01)(&00) could not be detached. The reason for the
rejection has been explained in the preceding NKR message(s).
For more detailed information on the error cause enter /HELP for the
preceding NKR message(s) or see the manual 'System Messages'.

## NKR0065

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0065 PATH '(&02)(&00) (&03)(&01)' ALREADY REMOVE-PENDING

### Meaning

No more commands affecting this path are accepted, if the parameter
FORCE=NO(...) is specified.

### Response

Try again with parameter FORCE=YES, or wait until the path
(&02)(&00) (&03)(&01) is no longer REMOVE-PENDING (use the command
/SHOW-DEVICE-CONFIGURATION).

## NKR0066

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0066 PATH '(&02)(&00) (&03)(&01)' REMOVE-PENDING EXPLICITLY

### Meaning

Path in state REMOVE-PENDING EXPLICITLY.

## NKR0067

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0067 PATH '(&02)(&00) (&03)(&01)' REMOVE-PENDING IMPLICITLY

### Meaning

Unit (&02)(&00) is DETACH-PENDING EXPLICITLY and/or DETACH-PENDING
IMPLICITLY.

### Response

Enter /SHOW-DEVICE-CONFIGURATION for more detailed information.

## NKR0069

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0069 PATH '(&02)(&00) (&03)(&01)': /REMOVE-DEVICE-CONNECTION PENDING REJECTED

### Meaning

The reason for this rejection has been explained in the preceding
NKR message(s).
For more detailed information on the error cause enter /HELP for the
corresponding NKR message(s) or see the manual 'System Messages'.

## NKR0071

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0071 '(&01)(&00)' VARIED OFFLINE BY SVP

## NKR0073

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0073 ALIAS DEVICE '(&00)' LINKED TO BASE DEVICE '(&01)'

### Meaning

Device (&00) and (&01) both represent the same logical (parallel
access) volume.
Parallel I/O's for (&00) and (&01) to the same PAV volume can be
executed.

## NKR0074

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0074 ALIAS DEVICE '(&00)' UNLINKED FROM BASE DEVICE '(&01)'

### Meaning

Device (&00) is not available for PAV volume. See NKR0073.

## NKR0075

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0075 DEVICE (&00) IS NOT A (&01) DEVICE

### Meaning

Device (&00) is not a (&01) device.

## NKR0076

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NKR0076 BASE DEVICE FOR ALIAS DEVICE '(&00)' NOT ATTACHED.

### Meaning

Attach for PAV alias device is not allowed if PAV base device is not
attached.

### Response

Attach PAV base device.

## NKR0080

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0080 '(&01)(&00)': INVALID INPUT FOR SVP. NO SVP ACTION PERFORMED

### Meaning

The hardware action associated with the specified reconfiguration request
could not be executed by the service processor due to unexpected internal
data.
(&01)(&00): mnemonic of an I/O system or a channel.

### Response

Take dump.

## NKR0081

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0081 '(&01)(&00)': SYSTEM INTERFACE TRANSFER ERROR. NO SVP ACTION PERFORMED

### Meaning

The hardware action associated with the specified reconfiguration request
could not be executed by the service processor due to interface problems.
(&01)(&00): mnemonic of an I/O system or a channel.

### Response

If a DETACH-command was to be processed, the SVP-action for a channel can
be tried once more by a DETACH FORCE=YES-command.

## NKR0082

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0082 '(&03)(&00)' COULD NOT BE VARIED OFFLINE DUE TO SVP-ERROR (&01). USE /HELP-MSG (&02)

### Meaning

The hardware action associated with the specified reconfiguration request
could not be executed by the service processor due to issued
MSSFCALL-response. Use /HELP-MSG (&02) to get more informations.
(&01): MSSFCALL-response

### Response

If necessary, contact the maintenance.

## NKR0083

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0083 '(&03)(&00)' COULD NOT BE VARIED ONLINE DUE TO SVP-ERROR (&01). USE /HELP-MSG (&02).

### Meaning

The hardware action associated with the specified reconfiguration request
could not be executed by the service processor due to issued MSSFCALL-
response. Use /HELP-MSG (&02) to get more informations.
(&01): MSSFCALL-response

### Response

If necessary, contact the maintenance

## NKR0084

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0084 '(&01)(&00)' COULD NOT BE VARIED OFFLINE BY SVP

### Meaning

The hardware action associated with the specified reconfiguration request
could not be executed by the service processor (SVP).
(&01)(&00): Hardware unit to be varied offline

## NKR0085

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0085 '(&01)(&00)' COULD NOT BE VARIED ONLINE BY SVP

### Meaning

The hardware action associated with the specified reconfiguration request
could not be executed by the service processor (SVP).
(&01)(&00): Hardware unit to be varied online

## NKR0086

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0086 '(&01)(&00)' FOREIGN. NO SVP ACTION PERFORMED

### Meaning

The hardware action associated with the specified reconfiguration request
could not be executed by the service processor due to the hardware state
FOREIGN.
(&01)(&00): mnemonic of an I/O system or a channel.

### Response

Connect (&01)(&00) to the own system.

## NKR0090

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0090 NO RECONFIGURATION SLOT AVAILABLE. TRY LATER

## NKR0091

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0091 TIMER EVENT COULD NOT BE SET. USE PARAMETER 'FORCE=YES'

### Meaning

Problems when setting the timer events. ($NSETTI-Macro).

### Response

Use the reconfiguration command with parameter FORCE=YES.

## NKR0092

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0092 '(&01)(&00)': /DETACH-DEVICE PENDING ACCEPTED

### Meaning

The timer event is set. The command will be executed after the allocations
have been returned or after the specified waiting time (default 15
minutes) has elapsed.

## NKR0093

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0093 PATH '(&02)(&00) (&03)(&01)': /REMOVE-DEVICE-CONNECTION PENDING ACCEPTED

### Meaning

The timer event is set. The command will be executed after the allocations
have been returned or after the specified waiting time (default 15
minutes) has elapsed.

## NKR0094

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0094 SLOT POOL PROBLEMS. USE PARAMETER 'FORCE=YES'

### Meaning

Software error when processing /DETACH-DEVICE or /REMOVE-DEVICE-CONNECTION
with specified waiting time.

### Response

Use reconfiguration command with parameter FORCE=YES.

## NKR0095

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0095 '(&01) (&00)': CANCEL PENDING IN PROCESS

### Meaning

(&01) (&00): hardware unit or path between two hardware units.

## NKR0096

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0096 '(&01) (&00)': PENDING STATE COULD NOT BE CANCELLED OR CANCEL PENDING IN PROCESS

### Meaning

Cancel pending processing problems or CANCEL PENDING already in process.

### Response

Use SHOW-DEVICE-CONFIGURATION to inform about configuration state.
If configuration state is DETACH-PENDING use the appropriate
reconfiguration command with the parameter FORCE=YES.

## NKR0097

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0097 '(&01) (&00)': CANCEL DETACH-PENDING EXECUTED

### Meaning

(&01) (&00) is again ATTACHED .

## NKR0098

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NKR0098 PATH '(&02)(&00) (&03)(&01)': /INCLUDE FOR A SECOND AVAILABLE PATH TO A TRANSDATA-DEVICE NOT ALLOWED

## NKR0100

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0100 '(&01)(&00)': /UNLOCK-DEVICE REJECTED

### Meaning

Possible reasons:
a) Device is not a disk, MBK or SCSI tape device.
b) Device characteristics for MBK or tape device unknown.
c) MBK or tape device already attached.
d) Device is 'detached implicitly' or 'detach pending implicitly'.

## NKR0101

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0101 '(&01)(&00)': /UNLOCK-DEVICE ACCEPTED

### Meaning

The requested unconditional unassign will be processed.

## NKR0102

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0102 '(&01)(&00)': /UNLOCK-DEVICE PROCESSED

### Meaning

The requested unconditional device deallocation has been processed.

## NKR0103

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0103 '(&01)(&00)': /UNLOCK-DEVICE NOT PROCESSED

### Meaning

The requested unconditional unassign could not be processed.

## NKR0107

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0107 '(&02)(&00) (&03)(&01)': CANCEL REMOVE-PENDING EXECUTED

### Meaning

(&02)(&00) (&03)(&01) is again INCLUDED.

## NKR0110

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0110 '(&01)(&00)' ATTACHED AND ASSIGNED

## NKR0111

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0111 '(&01)(&00)' ASSIGNED ELSEWHERE

### Response

Check whether the hardware unit (&01)(&00) is free or used by another
system.
If it is free, reset hardware reservation by means of /UNLOCK-DEVICE.

## NKR0112

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0112 '(&01)(&00)' COULD NOT BE ASSIGNED

### Response

Check configuration and try again.

## NKR0113

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0113 ASSIGNMENT FOR '(&01)(&00)' LOST

### Response

Check whether the device (&01)(&00) is free or used by a foreign system.
If it
is free, attach it again.

## NKR0114

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0114 '(&01)(&00)' UNASSIGNED

## NKR0115

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0115 '(&01)(&00)' COULD NOT BE UNASSIGNED

### Meaning

The device (&01)(&00) could not be unassigned.

### Response

Reset the hardware-reservation for the device (&01)(&00) by means of
/UNLOCK-DEVICE.

## NKR0116

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0116 ASSIGN FOR '(&01)(&00)' IN PROCESS

### Meaning

The operating system attempts to assign the device (&01)(&00) for the own
system.

## NKR0117

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0117 '(&01)(&00)' ASSIGNED

### Meaning

The device (&01)(&00) has been assigned for the own system.

## NKR0118

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0118 DEVICE '(&00)' RESERVED TO HOST WITH PATHGROUP-ID '(&01)'

### Meaning

Check whether device (&00) is correctly reserved to host with
given pathgroup (&01). If reservation is held without good reason
break it by means of /UNLOCK-DEVICE.
Syntax of pathgroup: 11 times SYSID of the host or
Byte 1: SYSID, Bytes 2-7: CPU-ID, Bytes 8-11: IPL time.

## NKR0119

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0119 DEVICE '(&00)' RESERVED TO GUEST SYSTEM '(&01)'

### Meaning

Check whether device (&00) is correctly reserved to guest system
with index (&01). If reservation is held without good reason
break it by means of /UNLOCK-DEVICE.

## NKR0120

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0120 '(&01)(&00)': DEVICE-TYPE INCONSISTENT

### Meaning

Device-type and available device-features for device (&01)(&00)
inconsistent.
The device-type must be adapted to the available device-features or the
generated device-features must be made available.
After this the device may be attached.

## NKR0121

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0121 RECONFIGURATION REQUEST FROM CONTROL UNIT (&00)

### Meaning

A DETACH/ATTACH request has been executed by the control unit.

## NKR0122

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0122 DEVICE ERROR ON SCD (&00), STATUS=X'(&01)', SB=X'(&02)'

### Meaning

Please call maintenance!

### Response

Enter any character

## NKR0123

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0123 '(&01) (&00)' I/O ERROR

### Meaning

I/O Error occurred during determination of device and controller
properties.

## NKR0124

Destination: CONSOLE Routing code: G Weight: 99

Warranty : YES

NKR0124 '(&00)'; NED1='(&02)' FOR CHN='(&01)' AND NED2='(&04)' FOR CHN='(&03)' NOT EQUAL

### Meaning

Different Node Element Descriptors NED1 and NED2 for device (&00)
on channel paths (&01) and (&03).
Meaning of NED1 and NED2 for FC channel:
Last 5 digits of System Serial Number /
Last 3 digits of Device Serial Number /
INQUIRY byte 0

### Response

Check configuration.
Possible invalid attachment or wrong I/O definition file.
Possible wrong attachment of the LUN to one of the paths
for FC channel.

## NKR0125

Destination: CONSOLE Routing code: G Weight: 99

Warranty : YES

NKR0125 ********** CONFIGURATION CONFLICT **********

### Meaning

BS2000 has detected a configuration conflict.
See following NKR message.

### Response

Call maintenance !

## NKR0126

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0126 DEVICE '(&00)' NOT AVAILABLE FOR CHANNEL '(&01)'

### Meaning

Device (&00) is not available for channel (&01).
Possible reasons:
- LUN Mapping not done.

### Response

Call maintenance.

## NKR0130

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0130 RESERVATION OF THE I/O RECONFIGURATION DONE.

### Meaning

The caller reserved the I/O reconfiguration (NKR) for his requests.
The reservation exists until the caller sends the "UNLOCK_NKR" OR ANOTHER
task sends the "UNLOCK_NKR FORCE=YES" request.

## NKR0131

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0131 I/O RECONFIGURATION RESERVATION REJECTED.

### Meaning

Reservation rejected because the caller is not owner of the system
privilege "NKRLOCK".

## NKR0132

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0132 THE I/O RECONFIGURATION IS ALREADY RESERVED FOR THE CALLER.

## NKR0133

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0133 THE I/O RECONFIGURATION IS BUSY,RESERVATION REQUEST REJECTED.

### Meaning

Units in state "PENDING ", that means DETACH requests still running.

## NKR0135

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0135 RESET OF THE I/O RECONFIGURATION RESERVATION.

## NKR0136

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0136 THE I/O RECONFIGURATION IS NOT RESERVED,REQUEST REJECTED.

### Meaning

The caller sends a request "Reset the I/O-Reconfiguration reservation",
but the I/O-reconfiguration is not reserved.

## NKR0137

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0137 THE I/O RECONFIGURATION IS RESERVED FOR ANOTHER TASK,REQUEST/COMMAND REJECTED.

### Meaning

The caller initiated a I/O reconfiguration request, but the I/O
recinfiguration is reserved for another TSN.

## NKR0138

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0138 TASK IDENTIFIER OF CALLER UNKOWN,I/O RECONFIGURATION RESERVATION REQUEST REJECTED.

## NKR0139

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0139 SYSTEMERROR, I/O RECONFIGURATION RESERVATION REQUEST REJECTED.

### Meaning

In the validation routine of system privilege "NKRLOCK" an error occurred.
Please inform the system administrator.

## NKR0140

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0140 DETACH FOR '(&01)(&00)' ALLOWED.

## NKR0141

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0141 DETACH FOR '(&01)(&00)' NOT ALLOWED.

## NKR0143

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0143 THE LAST OPERABLE CONSOLE IS GOING TO BE DETACHED

### Meaning

The last operable console will be detached. There is still one other
attached but inoperable console.

### Response

Make inoperable console operable.

## NKR0144

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NKR0144 VM GLOBAL I/O RECONFIGURATION PROCESSED WITH ERROR '(&00)'

### Meaning

VM global I/O reconfiguration processed with error.
For further information see attached message and messages to
console.

## NKR0145

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0145 REMOVE PATH '(&02)(&00) (&03)(&01)' ALLOWED.

## NKR0146

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0146 REMOVE PATH '(&02)(&00) (&03)(&01)' NOT ALLOWED.

## NKR0147

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0147 DEVICE '(&00)' NOT ASSIGNED TO GUEST SYSTEM.

### Meaning

The device (&00) is not assigned to the guest system.

### Response

Assign device to guest system (ADD-VM-DEVICE) and attach device
once more.

## NKR0148

Destination: CONSOLE Routing code: G Weight: 99

Warranty : YES

NKR0148 VM GLOBAL I/O RECONFIGURATION NOT ALLOWED

### Meaning

A VM global reconfiguration request was rejected because the guest
system is protected against such modifications of the I/O
configuration by a system parameter.

### Response

The VM global reconfiguration request will be no more rejected
if the reconfiguration is previously executed in guest system or
if the global /DETACH is executed with FORCE=UNCOND or
if the guest system protection is reset.

## NKR0149

Destination: CONSOLE Routing code: G Weight: 99

Warranty : YES

NKR0149 VM GLOBAL I/O RECONFIGURATION ACTIVE

### Meaning

A global reconfiguration request from privileged VM is active.

### Response

Wait and retry.

## NKR0150

Destination: CONSOLE Routing code: G Weight: 99

Warranty : YES

NKR0150 PATH BETWEEN (&00) '(&01)' AND (&02) '(&03)' NOT OPERATIONAL.

### Meaning

Permanent I/O error on specified path.
Path will be detached by system.

### Response

Check I/O units.
Path must be included again explicitly with the /INCLUDE-DEVICE-CONNECTION
command.

## NKR0151

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0151 NED='(&00)' FOR DEVICE '(&01)' AND DEVICE '(&02)' EQUAL.

### Meaning

The devices (&01) and (&02) have the same Node Element
Descriptor NED.

### Response

Check configuration.
Possible invalid attachment or wrong I/O definition file.

## NKR0155

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NKR0155 VM NOT PRIVILEGED FOR IMPLICIT DEVICE ASSIGNMENT

### Meaning

The virtual machine is not privileged for implicit device assignment
during ATTACH-DEVICE.

### Response

Give the privilege to the VM or assign the device explicitly
by means of ADD-VM-DEVICE.

## NKR0156

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NKR0156 IMPLICIT ASSIGNMENT NOT PERMITTED FOR DEVICE '(&00)'

### Meaning

Implicit assignment for device (&00) to virtual machine not
permitted with ATTACH-DEVICE.

### Response

Allow implicit assignment for device to VM or assign device explicitly
by means of ADD-VM-DEVICE.

## NKR0157

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NKR0157 DEVICE '(&00)' ASSIGNED EXCLUSIVELY TO OTHER VM

### Meaning

Device (&00) assigned exclusively to other virtual machine.

## NKR0158

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NKR0158 DEVICE '(&00)' CANNOT BE ASSIGNED TO VM '(&01)'

### Meaning

Device (&00) cannot be assigned to virtual machine as a result of
internal error.

### Response

Contact system administrator.

## NKR0159

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NKR0159 MAXIMUM NUMBER OF SHARERS FOR DEVICE '(&00)' ALREADY REACHED

### Meaning

Device (&00) already attached by 16 sharers.

### Response

Detach device by other system to allow new /ATTACH.

## NKR0160

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0160 (&00) (&01) NOT DEFINED

### Meaning

The io-unit (&01) is not defined.

### Response

Correct and retry.

## NKR0161

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0161 (&00) (&01) ALREADY DEFINED

### Meaning

The io-unit (&01) is already defined.

### Response

Correct and retry.

## NKR0162

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0162 (&00) (&01) NOT DETACHED

### Meaning

The io-unit (&01) is not detached.

### Response

Detach io-unit (&01) and retry request.

## NKR0163

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : YES

NKR0163 (&00) (&01) REMOVED

### Meaning

The io-unit (&01) has been removed.

## NKR0164

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : YES

NKR0164 (&00) (&01) OF TYPE (&02) ADDED

### Meaning

The io-unit (&01) of type (&02) has been added.

## NKR0165

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : YES

NKR0165 (&00) (&01) MODIFIED

### Meaning

The io-unit (&01) has been modified.

## NKR0166

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0166 '(&00)' FOR (&01) (&02) REJECTED

### Meaning

The required action for io-unit (&02) was rejected.

## NKR0167

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0167 NO (&00) ENTRY FREE

### Meaning

There is no free table entry for the io-unit in the system.

### Response

Delete a no more used io-unit entry (DEL-IO-UNIT) and try again.

## NKR0168

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0168 INTERNAL ERROR (&00)

### Meaning

A system internal error has occurred.
For some errors a further message will be displayed.
(&00): error code
Abort with error code
01: error $HDRCHCK.
02: action unknown.
07: inconistent tables.
13: error during $VMGINF, see also previous system message.
Try again for error code
03: shortage in bourse call ($NBSSIG).
04: insufficent class 3 memory ($GETMEM).
05: error during Get Subchannel Info.
06: information could not be sent to all guest systems ($VMGTDM).
08: IO lock could not be obtained exclusively ($GTLOCK).
09: error during creation of volume table ($VTENPR).
10: error calling DAR manager ($DARMGT)
11: error reading standard volume label ($VTVLIN).
12: the disks of the pubset could not be determined ($NDVGMN)
possible reason:
- pubset not imported until now.
Execute IMPORT-/EXPORT-PUBSET.

## NKR0169

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0169 CONFIGURATION UPDATE REJECTED

### Meaning

The required configuration update action was rejected.

## NKR0170

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0170 CONFIGURATION UPDATE REJECTED BY (&00) WITH RC = (&01)

### Meaning

The required action was rejected by the component (&00) with return
information (&01).

## NKR0171

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0171 '(&00)' FOR (&01) (&02) NOT SUPPORTED

### Meaning

The required action for io-unit (&02) is not supported.

## NKR0172

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0172 PATH TO (&00) (&01) NOT REMOVED.

### Meaning

Path to io-unit (&01) not removed.

### Response

Remove path and retry command.

## NKR0173

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0173 CONFIGURATION UPDATE NOT SUPPORTED.

### Meaning

The modification of the I/O configuration is not supported by the
operating system and/or the machine type.

## NKR0174

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0174 CONFIGURATION UPDATE ALREADY ACTIVE.

### Meaning

The START command for the modification of the I/O configuration has
already been given.

### Response

Give your modification commands.

## NKR0175

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : YES

NKR0175 CONFIGURATION UPDATE STARTED.

### Meaning

The modification of the I/O configuration has been started
successfully.

## NKR0176

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0176 CONFIGURATION UPDATE NOT ACTIVATED.

### Meaning

The START command for the modification of the I/O configuration has
not been given.

### Response

Start the modification and try again.

## NKR0177

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : YES

NKR0177 CONFIGURATION UPDATE STOPPED.

### Meaning

The modification of the I/O configuration is finished.

## NKR0178

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0178 GUEST SYSTEM NOT PRIVILEGED FOR RECONFIGURATION.

### Meaning

The guest system has not the privileg to execute the command.

### Response

Retry on a privileged system.

## NKR0179

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0179 RECONFIGURATION NOT PROCESSED BY GUEST SYSTEM '(&00)'.

### Meaning

The command was rejected by guest system (&00).

### Response

Look at console messages on guest system (&00) and check the reason
for the rejection.

## NKR0180

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0180 NUMBER OF GUEST SYSTEMS RUNNING: '(&00)'. NUMBER OF GUEST SYSTEMS SUPPORTING RECONFIGURATION: '(&01)'.

### Meaning

(&00) guest systems are running and (&01) guest systems are supporting
the reconfiguration.
For guest systems in the status RUNNING (DIFF) (different I/O
configuration after migration) no reconfiguration can be made.

### Response

Check for guest systems not supporting the reconfiguration.
The command will be executed only on the systems supporting
this function.

## NKR0181

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0181 ERROR IN OPERAND '(&00)' ((&01))

### Meaning

Error in operand (&00). For further information see (&01):
HIGH: Address or address range too high.
NSUP: Not supported.
UNIQ: Not unique. Addition: Name of device or control unit.
INCO: (&00)='CHANNEL-PATH-ID': Channel types inconsistent.
(&00)='*CONTROLLER': Control unit types inconsistent.
(&00)='CONTROLLER-ADDRESS': Control unit addresses inconsistent.
OUTR: Address not contained in address range. Addition: Range.
CUTY: Device type and control unit type inconsistent. Addition: Type.
MISS: Input missing.
ALLO: Input not allowed.

### Response

Retry command with correct operand.

## NKR0182

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0182 ADDRESS RANGE NOT UNIQUE ((&00))

### Meaning

There is a conflict in the address range of the control unit to be
modified and the control unit (&00).

### Response

Connect control unit to another channel or remove one of the two
control units and add it again with unique address range.

## NKR0183

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NKR0183 IORSF-CAPACITY INSUFFICIENT

### Meaning

There is not enough free space in the active IORSF to add the requested
IO-unit.

### Response

First remove all no more used IO-units with REMOVE-IO-UNIT, then try
again. If it's not possible, then write the active IORSF to the disk
with STOP-CONFIGURATION-UPDATE LEVEL=<n>. After an IMPL with this IORSF
and a new STARTUP new IO-units can be added again.

## NKR0184

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NKR0184 SVP-ERROR AT ACTION (&00), RC=(&01)

### Meaning

The specified SVP-action was terminated with errors. The requested
modification of the active IORSF could not be executed.

### Response

None.

## NKR0185

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NKR0185 ADDRESS (&00) NOT IN THE ADDRESS-RANGE OF CONTROLLER (&01)

### Meaning

The requested device address is not included in the address range of the
given control unit stored in the IORSF.

### Response

Correct the device address.
Otherwise correct the address range of the control unit with a REMOVE-
and following ADD-IO-UNIT command.

## NKR0186

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NKR0186 CMPG-ASSOCIATION FOR DEVICE (&00) NOT UNIQUE

### Meaning

The attachments of the device to be added are devided in different CMPG-
entries in the IORSF. That means, that there are already devices in the
configuration, that have only a subgroup of attachments of this device.
The addition of the device to the IORSF is not possible.

### Response

Decrease the number of attachments of the device.
Otherwise:
First remove all devices with a subgroup of the attachments of this
device, then add the device with the full number of attachments and
then add the other devices again.

## NKR0187

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NKR0187 DEVICE (&00) STILL ACTIVE

### Meaning

The IORSF-Modification was not possible, because there was still an
Input-/Output operation running on this device.

### Response

Retry request.

## NKR0188

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0188 CHANNEL (&00) NOT UNIQUE

### Meaning

The channel may be specified only once for the control unit or device.

## NKR0189

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0189 MAXIMUM NUMBER OF CHANNELS FOR CONTROL UNIT OR DEVICE EXCEEDED

### Meaning

To many channels defined for control unit or device.

## NKR0190

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NKR0190 SVP-REQUEST '(&00)' TERMINATED WITH ERROR '(&01)'. REFER TO /HELP-MSG (&02)

### Meaning

The specified SVP-action terminated with errors. For further information
use /HELP-MSG (&02).

### Response

See /HELP-MSG (&02).

## NKR0191

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : YES

NKR0191 ACTIVE IORSF WAS WRITTEN TO LEVEL (&00)

## NKR0192

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0192 OPERAND '(&00)' IGNORED.

### Meaning

OPERAND (&00) IS IGNORED IN COMBINATION WITH OTHER OPERANDS.

## NKR0193

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0193 WARNING; POSSIBLE INVALID ATTACHMENT. NO CONTROL UNIT WITH LOGICAL-ADDRESS = 0 FOUND FOR (&00) (&01)

### Meaning

A control unit with a logical address greater than zero is given for a
channel link or a SCD link where no other control unit is defined with
logical address zero.

### Response

The control unit will be added or modified; nevertheless you should
check the correctness of the control unit definition.

## NKR0194

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0194 DYNAMIC I/O CONFIGURATION NOT SUPPORTED BY '(&00)' GUEST SYSTEM(S). COMMAND PHASE = '(&01)'. IGNORE ? (Y/N)

### Meaning

(&00) guest system(s) do not support dynamic I/O configuration,
because they are in the status RUNNING (DIFF) (different I/O
configuration after migration).
Phase=Check: The configuration update isn't yet started.
Phase=Process: The configuration update is possibly processed by
some guest systems.

### Response

Answer with 'Y' to perform dynamic I/O configuration on the other
guest systems or answer with 'N' to terminate without execution.

## NKR0195

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0195 '(&00)' GUEST SYSTEM(S) DIDN'T RESPOND TO RECONFIGURATION REQUEST. COMMAND PHASE = '(&01)'. IGNORE ? (Y/N)

### Meaning

(&00) guest system(s) which do support the required function
didn't respond.
Phase=Check: The reconfiguration isn't yet started.
Phase=Process: The reconfiguration is possibly processed by
some guest systems.

### Response

Answer with 'Y' to perform the reconfiguration on the other
guest systems or answer with 'N' to terminate without execution.

## NKR0196

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0196 DYNAMIC I/O CONFIGURATION REJECTED BY GUEST SYSTEM '(&00)'. COMMAND PHASE = '(&01)'. IGNORE ? (Y/N)

### Meaning

Configuration update request rejected by guest system (&00).
Phase=Check: The configuration update isn't yet started.
Phase=Process: The configuration update is possibly processed by
some guest systems.

### Response

Answer with 'Y' to perform dynamic I/O configuration on the other
guest systems or answer with 'N' to terminate without execution.

## NKR0197

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0197 OTHER GUEST SYSTEM(S) IN STARTUP PHASE.

### Meaning

ACTIVE IORSF update not possible during startup of other guest
system(s).

### Response

Retry command later.

## NKR0198

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NKR0198 WARNING; CHANNEL '(&00)' OF TYPE '(&01)' DEFINED FOR SAME SCD.

### Meaning

There is already a channel of another type defined for the same SCD.
Check if different channel types are allowed for the SCD.

## NKR0199

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0199 I/O TASK TERMINATED ABNORMALLY. TAKE DUMP

## NKR0200

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NKR0200 COMMAND SUPPORTED ONLY WITH VM2000 VERSION 7 OR HIGHER

## NKR0201

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0201 DYNAMIC I/O CONFIGURATION NOT SUPPORTED BECAUSE OF SHARED DEVICE '(&00)'

### Meaning

Modification not allowed for shared devices.

## NKR0202

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

NKR0202 NUMBER OF GUEST SYSTEMS CHANGED SINCE START-CONF-UPD. COMMAND PHASE = '(&00)'. IGNORE ? (Y/N)

### Meaning

Number of guest systems has changed since start of dynamic update
of I/O configuration. It may be possible that one guest system is
in restart processing.
Phase=Check: The configuration update isn't yet started.
Phase=Process: The configuration update is possibly processed by
some guest systems.

### Response

Answer with 'Y' to perform dynamic I/O configuration or answer with
'N' to terminate without execution.

## NKR0203

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NKR0203 CONFIGURATION LIMITS EXCEEDED ((&00) AT CHANNEL (&01))

### Meaning

The requested update of the configuration would leed to a violation
of the configuration limits of the server.
The command is rejected.

## NKR0204

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NKR0204 IDENTICAL DEVICE ADDRESSES OF (&00) AND (&01) AT CHANNEL (&02)

## NKR0210

Destination: USER-TASK, CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0210 DEVICE '(&00)' NOT AVAILABLE

### Meaning

- Device does not exist or
- no path available for device or
- device access prohibited by storage management tool or
- device not assigned to guest system.

## NKR0220

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NKR0220 ERROR IN $STAM-CALL FOR PUBSET '(&00)'; ERROR CODE = '(&01)'

### Meaning

$STAM reports error. Error Codes:
NFND - MRSCAT entry cannot be found
CINV - CATID invalid
NINI - MRSCAT not initialized
INTE - Internal error
NPUB - Name of PUBRES device not in MRSCAT

## NKR0221

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NKR0221 DEVICE '(&00)' IS NO PUBRES/VOLRES DEVICE

### Meaning

Device (&00) is no PUBRES/VOLRES device.

## NKR0222

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NKR0222 ONLINE CATALOG ON DEVICE '(&00)' DOES NOT CONTAIN NAMES OF PUBSET DEVICES

### Meaning

The Online Catalog on device (&00) does not contain the names of
the devices belonging to the pubset. During import of the pubset
BS2000 writes the device names into the Online
Catalog.

## NKR0223

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NKR0223 MIRROR PUBSET (UNIT=(&00)) INCOMPLETE. CONTINUE ? (Y/N)

### Meaning

Some standard volumes of the PUBSET doesn't have a mirror volume.
It is not possible to process the whole mirror PUBSET specified
by mirror volume (&00).

### Response

Answer 'Y' to process as much mirror volumes as possible.
Answer 'N' to terminate.

## NKR0224

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NKR0224 $NDVGMN CALL FOR DEVICE '(&00)' REJECTED WITH ERROR '(&01)'

### Meaning

The disks of the pubset could not be determined.
Possible reasons:
- pubset not imported until now.
Execute IMPORT-/EXPORT-PUBSET and try again.
- PUBRES unit not found in Online Catalog of device.
For CLONE pubsets the process is repeated with PUBRES of original unit.

## NKR0230

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0230 PATHGROUP STATE FOR DEVICE '(&00)' INCONSISTENT

### Meaning

The control unit has another pathgroup state as BS2000.

### Response

Reset paths to control unit.

## NKR0240

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

NKR0240 TAPE DEVICE(S) STILL ACTIVE

©2024 Fujitsu | BS2000 System Messages