## PDT0200

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

PDT0200 NO TRACE WITH IDENTIFICATION '(&00)' EXISTS

### Meaning

The specified trace ID, identified by its trace name, its subsystem name
and its version, is not known to the trace manager.

## PDT0201

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

PDT0201 TRACE WITH IDENTIFICATION '(&00)' HAS ALREADY BEEN SWITCHED ON

### Meaning

The specified trace, identified by its trace name, its subsystem name
and its version, has already been switched on.

## PDT0202

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

PDT0202 TRACE WITH IDENTIFICATION '(&00)' RUNS PERMANENTLY. SWITCHING NOT POSSIBLE

### Meaning

The specified trace, identified by its trace name, its subsystem name
and its version, is permanently active and cannot be switched by the
trace manager.

## PDT0203

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

PDT0203 TRACE WITH IDENTIFICATION '(&00)' CANNOT BE SWITCHED BY THE TRACE MANAGER

### Meaning

The specified trace, identified by its trace name, its subsystem name
and its version, is activated by routines which are unknown to the trace
manager or the routine returned an errorcode.

### Response

More information can be found in the SERSLOG file.

## PDT0204

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

PDT0204 REQUESTED TRACE DOES NOT EXIST

### Meaning

There are no existing traces corresponding to the selection criteria
declared in the /SHOW-TRACE-STATUS command.

## PDT0205

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

PDT0205 TASK LOCK MANAGER ERROR WHILE PROCESSING A TLM OPERATION IN THE TRACE MANAGER INTERNAL TABLES

### Meaning

The trace manager did not get a lock on the trace manager internal
tables due to a task lock manager error.

### Response

Contact the maintenance staff and/or retry the command later.

## PDT0206

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

PDT0206 INTERNAL ERROR IN MODULE '(&00)'. SYSTEM DUMP TAKEN

### Meaning

An internal error occurred in a trace manager system routine.

## PDT0207

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

PDT0207 INSUFFICIENT CLASS (&00) MEMORY. NO PROCESSING BY TRACE MANAGER INITIATED. RETRY COMMAND LATER

### Meaning

Unsuccessful memory request for internal work areas.

## PDT0208

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

PDT0208 TRACE WITH IDENTIFICATION '(&00)' HAS ALREADY BEEN SWITCHED OFF

### Meaning

The trace identified by its trace name, its subsystem name and
its version has already been switched off.

## PDT0209

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

PDT0209 ACTION REQUESTED IS RESTRICTED TO $TSOS IDENTIFICATION. COMMAND REJECTED

### Meaning

The user is not authorized to request this action.

### Response

Retry the command under the $TSOS identification.

## PDT0210

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

PDT0210 INVALID ON/OFF PATTERN. TRACE WITH IDENTIFICATION '(&00)' CANNOT BE SWITCHED BY THE TRACE MANAGER

### Meaning

The trace manager contains incorrect ON or OFF masks, or the address of
the switch in the module writing the traces is invalid or inaccessible.

### Response

Contact the system diagnostics staff.

## PDT0213

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

PDT0213 NO SYSLST OUTPUT ALLOWED FROM THE CONSOLE. COMMAND REJECTED

### Meaning

The operator may not ask for output on SYSLST because the console has
no SYSLST.

### Response

Retry the command without the OUTPUT operand.

## PDT0214

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : YES

PDT0214 SEVERAL ERRORS FOR VARIOUS TRACES

### Meaning

Several trace identifications have been rejected for different reasons.
The appropriate error messages have been displayed.

## PDT0215

Destination: CONSOLE Routing code: * (main console) Weight: 30

Warranty : NO

PDT0215 LOCK ON TRACE MANAGER TABLES CANNOT BE CREATED. TRACE MANAGER CONTINUES WITH RESTRICTED FUNCTIONALITY

### Meaning

An error code has been received from the task lock manager; the trace
manager lock is not created. The trace manager will continue without
permitting the dynamic definition of traces.

## PDT0216

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : NO

PDT0216 ERROR '(&00)' DURING TRACE MANAGER INITIALIZATION. STARTUP CONTINUES

### Meaning

Startup continues although the trace manager status is undefined.
(&00) = 0020nnnn or 00000020 : request memory error
= 0024nnnn : internal error; contact maintenance staff
= 000nFFFF : invalid call; contact maintenance staff.

### Response

See "Meaning" above.

©2024 Fujitsu | BS2000 System Messages