## NVLCOPY

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NVLCOPY Copyright (C) (&01) (&00). All rights reserved

## NVLLOAD

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NVLLOAD Program '(&00)', Version '(&01)' of '(&02)' loaded from file '(&03)'

## NVL0000

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0000 VOLIN VERSION (&00) READY

## NVL0001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0001 VOLIN RESTRICTED TO SYSTEM ADMINISTRATOR. VOLIN TERMINATED

## NVL0002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0002 ENTER VSN AND DEVICE TYPE AND / OR UNIT, OR TERMINATE VOLIN WITH 'END'

### Meaning

The message announces the first RDATA for a parameter set.

## NVL0003

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0003 ENTER ADDITIONAL INITIALIZATION PARAMETERS OR TERMINATE INPUT WITH 'EOT=YES'

## NVL0004

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0004 SYNTAX ERROR IN PARAMETER '(&00)'

### Meaning

Certain errors don't allow to determine the erroneous parameter.
In this case an empty string is indicated.
If 'END' is indicated as erroneous parameter, a typing error in any other
parameter may be possible. The erroneous parameter itself therefore can
not be identified.
Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0005 KEY WORD '(&00)' INCORRECT OR INVALID

### Meaning

Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0006

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0006 VSN AND / OR DEVICE TYPE AND / OR UNIT NOT SPECIFIED. ALL GIVEN PARAMETERS WILL BE IGNORED

### Meaning

VOLIN expects as obligate input the VSN and at least one of the two items
device type or unit (device mn).
Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0007

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0007 THE VALUE SPECIFIED AS SIZE OF THE F1-LABEL IS TOO HIGH

### Meaning

The parameter F1-Label-Size (SDF syntax) resp. F1SIZE/VTOC (ISP syntax)
exceeds the limit 32766 or the number of blocks available on the disk.
Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0008

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0008 DEVICE TYPE AND / OR UNIT UNKNOWN OR NOT SUPPORTED

### Meaning

The disk type specified by the parameter DEVICE (ISP syntax only) or
determined by the parameter UNIT could not be found in the VOLIN disk
characteristic tables.
If no typing error was made when specifying this parameters, it is
not possible to format and initialize the disk with the current VOLIN
version.
The device type STDDISK is not allowed for VOLIN.

## NVL0010

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0010 DISK '(&00)': STANDARD VOLUME LABEL INVALID

### Meaning

The volume assigned for the initialization of disk (&00) does not carry
a valid BS2000 standard volume label (SVL).
The initialization is terminated if the disk was requested by means of
parameter OVERWRITE-DISK (SDF syntax) resp. parameter CHECK (ISP syntax).

## NVL0011

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0011 VALUE OF PARAMETER 'F1SIZE' NOT POSITIVE

### Meaning

Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0013

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0013 ERROR WHEN ACQUIRING DEVICE OR DISK. ERROR CODE: '(&00)'

### Meaning

(&00) = 3003: device temporarily not available (allocated to another task)
3103: device permanently not available (not attached)
3203: device allocation not allowed
3303: device not defined
4004: volume temporarily not available
4104: volume permanently not available (rejected by operator)
4204: volume allocation not allowed
Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

### Response

Check the device or disk status and enable allocation for special use.

## NVL0014

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0014 DEVICE REQUESTED IN PARAMETER 'UNIT' DOES NOT MATCH DEVICE TYPE IN PARAMETER 'DEVICE'

### Meaning

Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0015

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0015 VOLIN: SYSTEM ERROR WHILE PAGE FIXING. INITIALIZATION TERMINATED WITH DUMP

### Meaning

It is not possible to fix a page required for I/O.

### Response

If this message recurs, send the error documentation to
diagnosis department.

## NVL0016

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0016 VOLIN: ERROR AT MEMORY RELEASE.

### Meaning

If class 3 memory, initialization is terminated with dump.

### Response

If this message recurs, send the error documentation to
diagnosis department.

## NVL0017

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0017 INITIALIZATION OF VOLUME '(&00)' ON UNIT '(&01)' COMPLETED. VOLUME FORMAT: '(&02)'

### Meaning

The volume (&00) may now be used in BS2000.

## NVL0018

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0018 VOLUME '(&00)' CANNOT BE USED DUE TO ERROR(S). INITIALIZATION TERMINATED ABNORMALLY

### Meaning

More detailed error messages precede this message.

## NVL0019

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0019 SYSTEM ERROR. INITIALIZATION ABORTED. VOLIN TERMINATED. DUMP WRITTEN TO 'SYSLST'

### Meaning

The program detects an illogical condition causing the program to
terminate
abnormally.
Possible reasons:
- a system error
- a VOLIN program error
- a hardware error on the disk used or its controller.
Under IPL-Exec, the dump is issued directly on printer. If no printer is
connected, the dump is lost.

### Response

If this message recurs, send the error documentation to
diagnosis department.

## NVL0022

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0022 OVERWRITING COMPLETED. TEST PATTERN '(&00)' WRITTEN ON ALL BLOCKS OF DISK '(&01)'

## NVL0024

Destination: USER-TASK, CONSOLE Routing code: A Weight: 98

Warranty : NO

NVL0024 OVERWRITE DISK '(&00)' IN NEW FORMAT '(&01)'? REPLY (Y=YES; N=NO)

### Meaning

This is the last opportunity to prevent the BS2000 disk (&00) from
being overwritten in case the wrong disk is mounted or assigned.

### Response

Y: the volume will be overwritten in format (&01)
N: the volume remains unchanged; a new mount message is displayed;
another volume can be assigned.

## NVL0026

Destination: USER-TASK, CONSOLE Routing code: A Weight: 98

Warranty : NO

NVL0026 DEVICE ERROR ON DISK '(&00)' DURING INITIALIZATION. REPLY (R=RETRY; T=TERMINATE INITIALIZATION)

### Meaning

A device error on disk (&00) could not be corrected by the error recovery
routine.

### Response

R: retry error recovery again
T: terminate the initialization of this volume.
If this message recurs, contact the maintenance staff to check the disk
and
its control unit.

## NVL0027

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0027 SYSTEM ERROR (REQM). VOLIN ABORTED DUE TO INSUFFICIENT MEMORY

### Meaning

It is not possible to obtain sufficient memory for the I/O and the
work pages.

### Response

If this message recurs, send the error documentation to
diagnosis department.

## NVL0030

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0030 REPLY TO PRECEDING MESSAGE INVALID. CORRECT REPLY

## NVL0031

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0031 INITIALIZATION STARTED FOR VOLUME '(&00)' ON UNIT '(&01)' IN FORMAT '(&02)'

## NVL0032

Destination: USER-TASK, CONSOLE Routing code: A Weight: 98

Warranty : NO

NVL0032 OVERWRITE NON-STANDARD DISK '(&00)' ON DEVICE '(&01)' IN NEW FORMAT '(&02)'? REPLY (Y=YES; N=NO)

### Meaning

The volume assigned by the operator is no BS2000 disk because
it has no valid standard volume label (SVL).

### Response

Y: the correct disk has been assigned
N: the wrong disk is mounted.
A new mount message follows for mounting the correct disk specified.

## NVL0033

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0033 RELEASE STARTED FOR VOLUME '(&00)' ON UNIT '(&01)'

### Meaning

Release of disk by SPACEPRO.

## NVL0034

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0034 VOLIN: SYSTEM ERROR DURING '(&00)'. INITIALIZATION TERMINATED WITH DUMP

### Response

Send the error documentation to diagnosis department.

## NVL0035

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0035 VERSIONS OF VOLIN AND BS2000 NOT COMPATIBLE. VOLIN TERMINATED ABNORMALLY

### Meaning

The VOLIN version started has not been released for the BS2000 version of
the current system.

## NVL0036

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0036 READ ERROR ON SYSDATA

### Meaning

An access error or
a record with more than 251 characters was encountered on SYSDTA.
Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0037

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0037 DISK '(&00)'. ASSIGNED VOLUME HAS VSN '(&01)', FORMAT '(&02)'. DEVICE TYPE '(&03)' ENCODED IN VOLUME LABEL DOES NOT AGREE WITH CURRENT DEVICE TYPE '(&04)'

### Meaning

The device type encoded in the volume label is (&03). However, according
to the system tables the disk device has device type (&04).

### Response

Check device type.

## NVL0038

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0038 DISK '(&00)'. ASSIGNED VOLUME NOT EMPTY. OLD VSN '(&01)', EXISTING FORMAT '(&02)'

### Meaning

The volume assigned for initialization of disk (&00) is a BS2000
disk with VSN (&01) and format (&02).
The subsequent message NVL0024 permits the disk to be rejected.

## NVL0041

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0041 DISK DEVICE '(&00)' REJECTED. NEW MOUNT REQUEST FOR INITIALIZATION OF DISK '(&01)' FOLLOWS

### Meaning

The system administrator rejected disk device (&00).

## NVL0042

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0042 VOLIN ACQUIRES DISK DEVICE FOR INITIALIZATION OF DISK '(&00)'

### Meaning

If the operating system cannot assign the device automatically, a mount
message is issued by the device management.

## NVL0043

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0043 DISK '(&00)'. PARAMETERS 'OVERWRITE-DISK' (SDF) RESP. 'CHECK' (ISP) AND/OR 'UNIT' PERMIT NO OTHER DEVICE ASSIGNMENT. INITIALIZATION TERMINATED ABNORMALLY

### Meaning

The initialization of disk (&00) cannot be retried with another volume,
because parameters OVERWRITE-DISK (SDF syntax) resp. CHECK (ISP syntax)
and/or UNIT require a particular volume.

### Response

Change the parameter(s) OVERWRITE-DISK resp. CHECK and/or UNIT and retry
the initialization.

## NVL0049

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0049 DEVICE CHARACTERISTICS ON DISK '(&00)' CANNOT BE READ. INITIALIZATION TERMINATED ABNORMALLY

### Response

Contact the maintenance staff to check the disk.

## NVL0054

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0054 INVALID BLOCK SIZE ON DISK '(&00)'. INITIALIZATION TERMINATED ABNORMALLY

### Meaning

The disk has been formatted with a block size unknown to VOLIN.

### Response

Contact the maintenance staff to format the disk again.

## NVL0055

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0055 UNRECOVERABLE ERROR WHEN TESTING DISK. INITIALIZATION TERMINATED ABNORMALLY

### Response

Contact the maintenance staff to check the disk.

## NVL0056

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0056 UNRECOVERABLE ERROR WHEN READING IDENTIFIER. INITIALIZATION TERMINATED ABNOMALLY

### Response

Contact the maintenance staff to check the disk.

## NVL0061

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0061 INVALID DEVICE CHARACTERISTICS ON DISK '(&00)'. INITIALIZATION TERMINATED ABNORMALLY

### Response

Contact the maintenance staff to check the disk.

## NVL0062

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0062 Volume '(&00)' with '(&01)' HP exceeds maximum volume capacity of 32 GB

### Meaning

BS2000 supports a maximum of 16777215 halfpages (each 2048 bytes) per
volume, i.e. approximately 32 GB.

## NVL0065

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0065 DEVICE REQUESTED IN PARAMETER VALUE 'UNIT=(&00)' IS UNKNOWN

### Meaning

(&00): mnemonic device name (mn).
Batch task : the program is terminated with TERM MODE=ABNORMAL.
Interactive task: the processing of the current parameter set is
terminated. A new parameter set can be entered after
the corresponding VOLIN prompting.

## NVL0066

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0066 DISK '(&00)', FORMAT '(&01)': ASSIGNED VSN '(&02)' AND FORMAT '(&03)'. FORMATTING OF VOLUME REQUIRED BUT LABEL CREATION ONLY IS SPECIFIED

### Meaning

The subsequent message NVL0067 permits to withdraw the specification to
create labels only or to reject the disk.

## NVL0067

Destination: USER-TASK, CONSOLE Routing code: A Weight: 98

Warranty : NO

NVL0067 OVERWRITE STANDARD DISK '(&00)', USING THE STANDARD PARAMETER FOR FORMATTING? REPLY (Y=YES; N=NO)

### Meaning

The volume assigned is a standard BS2000 disk.
For the initialization of a BS2000 disk with given format, the volume
has to be formatted.
If desired, the specification to create labels only is ignored, and the
volume is formatted using the standard values of the formatting
parameters.

### Response

Y: the volume is overwritten and formatted in accordance with the
message
N: the state of the volume remains unchanged.
A new mount message follows for mounting another volume.

## NVL0068

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0068 VOLIN: '(&00)' SYSTEM ERROR. PROGRAM RUN ABORTED

### Response

If this message recurs again, send the error documentation to
diagnosis department.

## NVL0075

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0075 ATTACHED DEVICE TYPE DOES NOT MATCH REQUESTED DEVICE TYPE

### Meaning

The disk type specified in parameter 'DEVICE' (ISP syntax only) or
determined by UNIT input (that is the generated type) does not match the
type of the attached device. Capacity of the attached device is lower
than that of the expected one.
Initialization will be terminated abnormally.

### Response

Restart VOLIN after correction of UGEN parameter.

## NVL0076

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0076 CAPACITY OF ATTACHED DEVICE GREATER THAN THAT OF THE REQUESTED DEVICE. REPLY (C=CONTINUE; T=TERMINATE)

### Meaning

The disk type specified in parameter 'DEVICE' (ISP syntax only) or
determined by UNIT input (that is the generated type) does not match the
type of the attached device. Capacity of the attached device is greater
than that of the expected one.

### Response

C: Continue, format and initialize disk
T: Terminate initialization abnormally.

## NVL0079

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0079 (&00) PER CENT OF DISK (&01) (&02) ARE PROCESSED

### Meaning

The message shows the progress of overwriting process of VOLIN.
&00 = value of per cent in steps of ten
&01 = VSN
&02 = '-'

## NVL0100

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0100 INITIALIZATION OR LOADING OF SUBSYSTEM VOLIN NOT POSSIBLE: ERROR CODE '(&00)'

### Meaning

Return code description:
X'0041FFFF': error during the subsystem connection.
Reasons: - see detailed console messages.
- simultaneous loading of VOLIN subsystem (SS).
In this case wait and retry.

### Response

Check the DSSM context (DSSM: Dynamical SubSystem Management).

## NVL0101

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0101 LOADING OF SUBSYSTEM VOLIN VIA COMMAND NOT POSSIBLE

### Meaning

The subsystem will be loaded in program VOLIN.

## NVL0102

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0102 VERSIONS OF TU PROGRAM PART AND SUBSYSTEM VOLIN INCONSISTENT. VOLIN RUN ABORTED

### Meaning

The version of the interface parameter list does not agree with this one
required by the subsystem.

### Response

Check DSSM context (DSSM: Dynamical SubSystem Management).

## NVL0103

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0103 ADDRESS OF INTERFACE PARAMETER LIST CHANGED. VOLIN RUN ABORTED

### Meaning

The address of the interface parameter list has been changed after the
initialization of the subsystem.
This is not allowed.

### Response

Send the error documentation to diagnosis department.

## NVL0104

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0104 SPECIFIED VALUE OF PARAMETER 'FORMAT' DOES NOT AGREE WITH PHYSICAL DISK STRUCTURE OF '(&00)'. INITIALIZATION TERMINATED ABNORMALLY

## NVL0109

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0109 PRIVATE DISKS ARE ONLY PERMITTED FOR AN ALLOCATION UNIT OF 6 K

### Meaning

If no allocation unit was given explicitely, the allocation unit given
implicitely by a format statement is not permitted.

## NVL0110

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0110 DISK CAPACITY TOO SMALL FOR DISK ADMINISTRATION DATA. DISK HAS TO BE FORMATTED

### Meaning

The capacity is too small for disk administration data
(IPL, SVL and format 5 labels).

### Response

The disk has to be formatted.

## NVL0111

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0111 UTILITY ROUTINE '(&00)' VERSION (&01) READY FOR INPUT

## NVL0122

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0122 REPAIR IS NOT SUPPORTED.

## NVL0146

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0146 DISK CAPACITY GREATER EQUAL 32GB IS NOT PERMITTED FOR PRIVATE DISKS

## NVL0147

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0147 A REQUEST THAT EXCEEDS THE REAL CAPACITY OF THE ATTACHED DEVICE WILL BE IGNORED.

### Meaning

A DEVICE CAN BE FORMATED ONLY WITH ITS REAL MAXIMUM CAPACITY.

## NVL0148

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0148 (&00) SESSION FOR DEVICE (&01) TERMINATED

### Meaning

SNAP/CLONE session for device (&01) terminated by VOLIN.

## NVL0149

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0149 TERMINATION OF (&00) SESSION FOR DEVICE (&01) FAILED

### Meaning

Termination of SNAP/CLONE session for device (&01) by VOLIN failed.

## NVL0150

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NVL0150 INITIALIZATION OF (&00) DEVICE (&01) NOT ALLOWED

### Meaning

SNAP/CLONE device (&01) may not be overwritten by VOLIN.

## NVL0151

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

NVL0151 TERMINATE (&00) SESSION FOR DEVICE (&01) ? REPLY (Y=YES; N=NO; C=CANCEL)

### Meaning

SNAP/CLONE session for device (&01) active.

### Response

Y: Terminate SNAP/CLONE session and
continue volume initialization.
N: Continue volume initialization without
termination of SNAP/CLONE session.
C: Cancel volume initialization.

©2024 Fujitsu | BS2000 System Messages