## SENREVI

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SENREVI COMP=SENMF,VERS=91A,DATE=201215

## SEN0001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN0001 CONSISTENCY CHECK (&00) '(&01)'

### Meaning

(&00): <CC-no.>/<CC-weight>/<CC-subnumber>
error weight of the consistency check (CC):
05: dump only: DBH will continue;
70: faulty request; 71: system bottleneck;
72: faulty DBH; 82: system dump;
83: faulty system;
(&01): DCM or DMS return code.

### Response

Send dump(s) to the diagnosis department.

## SEN0002

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN0002 SESDCN SYSTEM INITIALIZATION: INTERNAL SYSTEM ERROR

## SEN0003

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN0003 SESDCN CANNOT BE LOADED DUE TO A RESOURCE BOTTLENECK: (&00) '(&01)'

### Meaning

(&00): <CC no.>/<CC weight>/<CC subnumber>
Error weight of the consistency check (CC):
05: dump only: DBH will continue;
70: faulty request; 71: system bottleneck;
72: faulty DBH; 82: system dump;
83: faulty system;
(&01): DCM or DMS return code.

### Response

Forward dump for system diagnosis.

## SEN0004

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN0004 SESDCN SYSTEM INITIALIZATION: INSUFFICIENT USER ADDRESS SPACE

### Response

Increase user address space and restart SESDCN.

## SEN0006

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN0006 SESDCN SYSTEM INITIALIZATION: ERROR WHILE LOADING '(&00)'

### Meaning

An error occurred during system initialization of the SESDCN program
when one of the LLMs (module name &00) needed by the SESDCN was being
dynamically loaded (e.g. LLM not found in module library).

### Response

Restart SESDCN.

## SEN0007

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN0007 CONTROL BLOCK ('PTAB' ENTRY) FOR REMOTE DUMP DBH NOT FOUND. REMOTE DUMP WAS NOT POSSIBLE.

### Response

Forward dump for diagnosis.

## SEN1000

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1000 FIRST SDF STATEMENT IS NOT THE 'SET-DCN-OPTIONS' STATEMENT

### Response

Restart SESDCN with the SET-DCN-OPTIONS as the first SDF statement.

## SEN1001

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1001 ERRORED OR INVALID SDF STATEMENT

### Response

Restart SESDCN with a correct SDF statement.

## SEN1002

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1002 LINK NAME '(&00)' NOT NEEDED IN 'ADD-NETWORK-LINK-LIST' STATEMENT

### Meaning

This message is intended as a warning. Superfluous link names are ignored
as they do not result in incorrect system behavior. SESDCN does not abort.
- (&00): Superfluous link name

### Response

Remove the superfluous link name.

## SEN1003

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1003 DBH ASSIGNED TO SEVERAL DCNS (&00)

### Meaning

In the SESDCN start parameters, a DBH has been assigned to several DCNs.
This is not permitted.
- (&00): CATALOG=<catalog-name>, DBH=<dbh-name>, DCN=<dcn-name>,
CNF=<configuration-name>
CATALOG=<catalog-name>, DBH=<dbh-name>, DCN=<dcn-name>,
CNF=<configuration-name>
(The insert indicates the paths of both involved catalogs.)

### Response

Modify SESDCN start parameters.

## SEN1004

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1004 LINK NAME SPECIFIED MORE THAN ONCE IN 'ADD-NETWORK-LINK-LIST' STATEMENT

### Response

Specify a unique link name.

## SEN1005

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1005 LINK-NAME FROM THE 'ADD-DISTRIBUTION-RULE-LIST' STATEMENT IS NOT INCLUDED IN THE 'ADD-NETWORK-LINK-LIST' STATEMENT.

### Response

Add missing link name(s) to the 'ADD-NETWORK-LINK-LIST' statement and
restart SESDCN.

## SEN1006

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1006 CATALOG NAME SPECIFIED MORE THAN ONCE IN 'ADD-DISTRIBUTION-RULE-LIST' STATEMENT

### Response

Specify a unique catalog name.

## SEN1008

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1008 DISTRIBUTION RULE ENTRIES DIFFERENT FROM CATALOG: (&00)

### Meaning

(&00): catalog name
When the secondary DCN was started, catalog specifications were made
which are different from those already in the distribution rule.
The catalog specifications in the distribution rule remain valid.
Those ones in the start parameters of the secondary DCN are ignored.
The starting of the secondary DCN is continued.

### Response

Ensure that the catalog specifications match the specifications of the
master DCN.

## SEN1013

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1013 INVALID DCN NAME IN THE 'SET-DCN-OPTIONS' STATEMENT.

### Response

Correct the DCN name in the 'SET-DCN-OPTIONS' statement and restart
SESDCN. Valid DCN names are: A,...,Z,0,...,9 and <blank>.

## SEN1019

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1019 INVALID CONFIGURATION NAME IN THE 'SET-DCN-OPTIONS' STATEMENT

### Response

Correct the configuration name in the 'SET-DCN-OPTIONS' statement and
restart SESDCN. Valid configuration names are: A,...,Z,0,...,9 and
<blank>.

## SEN1020

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1020 NO CATALOG DESCRIPTION SPECIFIED IN THE 'ADD-DISTRIBUTION-RULE-LIST' STATEMENT.

### Meaning

Add missing catalog description(s) to the 'ADD-DISTRIBUTION-RULE-LIST'
statement and restart SESDCN.

## SEN1021

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1021 MORE CATALOG DESCRIPTIONS SPECIFIED THAN PERMITTED

### Meaning

More catalog descriptions were specified in the
'ADD-DISTRIBUTION-RULE-LIST' statement than are permitted. The maximum
permitted number of catalog descriptions is 200.

### Response

Correct the 'ADD-DISTRIBUTION-RULE-LIST' statement and restart SESDCN.

## SEN1023

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1023 INVALID DBH NAME IN THE 'ADD-DISTRIBUTION-RULE-LIST' STATEMENT

### Response

Correct the DBH name in the 'ADD-DISTRIBUTION-RULE-LIST' statement and
restart SESDCN. Valid DBH names are: A,...,Z,0,...,9 and <blank>.

## SEN1024

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1024 INVALID CATALOG NAME IN THE 'ADD-DISTRIBUTION-RULE-LIST' STATEMENT

### Response

Correct the catalog name in the 'ADD-DISTRIBUTION-RULE-LIST' statement and
restart SESDCN.

## SEN1031

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1031 TOO MANY LINK NAMES SPECIFIED

### Meaning

More link names were specified in the 'ADD-NETWORK-LINK-LIST' statement
than are permitted. The maximum number of link names permitted is 200.

### Response

Correct the 'ADD-NETWORK-LINK-LIST' statement and restart SESDCN.

## SEN1033

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1033 INVALID PROCESSOR NAME IN THE 'ADD-NETWORK-LINK-LIST' STATEMENT

### Response

Correct the processor name in the 'ADD-NETWORK-LINK-LIST' statement and
restart SESDCN.

## SEN1034

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1034 INVALID DCN NAME IN THE 'ADD-NETWORK-LINK-LIST' STATEMENT

### Meaning

Correct the DCN name in the 'ADD-NETWORK-LINK-LIST' statement and
restart SESDCN. Valid DCN names are: A,...,Z,0,...,9 and <blank>.

## SEN1036

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1036 FILE NAME TOO LONG FOR SESDCN LOG FILE

### Meaning

An attempt was made to assign a log file to the SESDCN program via the
link name SESDLG. The name of the file, however, is too long. The maximum
permitted length is 54 characters including the catalog ID and user ID.

## SEN1037

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1037 INVALID CONFIGURATION NAME IN 'ADD-NETWORK-LINK-LIST' STATEMENT

### Meaning

An illegal value was specified for 'CONFIGURATION-NAME' in the network
description.

### Response

Modify the configuration name accordingly. Letters, digits and '*BLANK'
are permitted.

## SEN1040

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1040 SDF IS NOT AVAILABLE ON THIS SYSTEM.

### Meaning

'SESDCN' cannot be started, since SDF is not available.

### Response

Generate SDF in the system and restart SESDCN.

## SEN1041

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1041 NO SDF SYNTAX FILE FOR 'SESDCN'

### Meaning

'SESDCN' cannot be started because there is no SDF syntax file.

### Response

Ask the system administrator to mount the SDF syntax file.

## SEN1042

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1042 INVALID HOST NAME IN 'ADMINISTRATOR' PARAMETER OF 'SET-DCN-OPTIONS' STATEMENT

### Meaning

An illegal processor name was specified for 'ADMINISTRATOR' in the
'SET-DCN-OPTIONS' statement.

## SEN1043

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1043 NO ERROR DIALOG POSSIBLE VIA SDF

## SEN1044

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN1044 SDF ERROR DIALOG REJECTED BY USER

### Meaning

SESDCN (not SDF) detected an error when the SESDCN start parameters were
entered in the SDF dialog. The SDF correction dialog proposed as a result
was rejected by the user. SESDCN was therefore terminated.

### Response

Restart SESDCN.

## SEN2001

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN2001 INVALID CATALOG NAME

## SEN2002

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN2002 INVALID PROCESSOR NAME

## SEN2003

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN2003 INVALID TSN

## SEN2004

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN2004 INVALID USER ID

## SEN2005

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN2005 INVALID 'SESDCN' ADMINISTRATION STATEMENT

## SEN2006

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN2006 INVALID DCN NAME

## SEN2007

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN2007 INVALID DBH NAME

## SEN2008

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2008 INVALID CONFIGURATION NAME IN 'SESDCN' ADMINISTRATION STATEMENT

## SEN2009

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2009 'SESDCN' ADMINISTRATION STATEMENT REJECTED

## SEN2010

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2010 'SESDCN' ADMINISTRATION STATEMENT ACCEPTED

## SEN2011

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2011 'SESDCN' ADMINISTRATION STATEMENT REJECTED; NO ACTIVE USER

## SEN2012

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2012 'SESDCN' ADMINISTRATION STATEMENT REJECTED; TRANSACTION IN EXTERNAL 'PTC' STATE

## SEN2013

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2013 'SESDCN' ADMINISTRATION STATEMENT REJECTED; NO ACTIVE TRANSACTION

## SEN2014

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2014 END OF THE 'SESDCN' ADMINISTRATION STATEMENT

## SEN2015

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2015 'SESDCN' ADMINISTRATION STATEMENT REJECTED; NO CATALOG IN DISTRIBUTION RULE

## SEN2016

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2016 'SESDCN' ADMINISTRATION STATEMENT REJECTED; SPECIFIED USER DOES NOT EXIST

## SEN2017

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2017 'SESDCN' ADMINISTRATION STATEMENT REJECTED; NO ACTIVE TRANSACTION EXISTS FOR SPECIFIED USER

## SEN2018

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2018 'SESDCN' ADMINISTRATION STATEMENT REJECTED AS END-OF-TRANSACTION PROCESSING IS ALREADY RUNNING FOR THIS TRANSACTION

## SEN2019

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2019 'SESDCN' ADMINISTRATION STATEMENT REJECTED; TRANSACTION ALREADY ROLLED BACK

## SEN2020

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2020 'SESDCN' ADMINISTRATION STATEMENT REJECTED; ANOTHER 'SESDCN' ADMINISTRATION STATEMENT CURRENTLY BEING PROCESSED

## SEN2021

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2021 DISTRIBUTION RULE OVERFLOW

### Meaning

No further catalog can be added to the SESDCN distribution rule.

### Response

Stop SESDCN and all data base handlers and SESAM applications
running in the same SESAM configuration as SESDCN. Eliminate
if possible all catalog entries, which are no longer needed,
from the SESDCN start parameters, and start SESDCN again.

## SEN2022

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN2022 CATALOG WITH DIFFERENT LOCATION ALREADY IN DISTRIBUTION RULE

## SEN2031

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN2031 INCORRECT PASSWORD

### Meaning

The password is syntactically incorrect in the OPT,ADM statement.

### Response

Repeat the OPT,ADM statement with the syntactically correct password.

## SEN2032

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN2032 INCORRECT BS2000 USER ID

### Meaning

The BS2000 user ID is syntactically incorrect in the OPT,ADM statement.

### Response

Repeat the OPT,ADM statement with the syntactically correct BS2000 user
ID.

## SEN2033

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN2033 INCORRECT APPLICATION NAME

### Meaning

The application name is syntactically incorrect in the OPT,ADM statement.

### Response

Repeat the OPT,ADM statement with the syntactically correct application
name.

## SEN2034

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN2034 INCORRECT KDCSIGN-NAME

### Meaning

The KDCSIGN-NAME is syntactically incorrect in the OPT,ADM statement.

### Response

Repeat the OPT,ADM statement with the syntactically correct KDCSIGN-NAME.

## SEN2035

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN2035 SESDCN LOADED WITHOUT ADMINISTRATION AUTHORIZATION

### Meaning

An OPT,ADM statement was sent to an SESDCN that was loaded without
administration authorization (ADMINISTRATOR=*NONE in SET-DCN-OPTIONS
statement).

### Response

If necessary, end SESDCN and restart with administration authorization.

## SEN2041

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN2041 CATALOG TO BE DELETED NOT IN DISTRIBUTION RULE

## SEN2042

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN2042 CATALOG ALREADY DELETED BY PREVIOUS REQUEST

## SEN2043

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN2043 PROCESSOR TO BE DELETED NOT IN DISTRIBUTION RULE

## SEN2044

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2044 PROCESSOR NAME TO BE SUBSTITUTED IS NOT INCLUDED IN THE DISTRIBUTION RULE.

## SEN2045

Destination: CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2045 CATALOG WITH IDENTICAL LOCATION ALREADY IN DISTRIBUTION RULE

## SEN2046

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2046 PROCESSOR NAME TO BE UPDATED USER-OWN PROCESSOR

### Meaning

In the UPDPRO administration command or the SESAM MODIFY-DISTRIBUTION-
RULE-ENTRY statement, the name of the processor of the user was entered
as the processor name. This processor, on which the SESDCN to be
administered is running, must not be specified.

### Response

Repeat administration with a different processor name to be replaced if
required.

## SEN2047

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2047 TRANSACTION CANNOT BE RESET AT PRESENT BECAUSE OF RESOURCE BOTTLENECK

### Response

Repeat the administration statement for resetting the transaction later.

## SEN2048

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2048 TRANSACTION CANNOT BE RESET AT PRESENT BECAUSE OF LONG RUNNING STATEMENT

### Meaning

Transaction cannot be reset at present because a long running statement
is beeing treated by SESAM for the concerned user.

### Response

Repeat the administration statement for resetting the transaction later.

## SEN2050

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2050 'SESDCN' ADMINISTRATION STATEMENT: (&00)

## SEN2051

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2051 'SESDCN' ADMINISTRATION STATEMENT (&00) EXECUTED

## SEN2052

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2052 'SESDCN' ADMINISTRATION: MORE RESPONSES EXISTING

### Meaning

Because of a response area being too small all responses can't be
issued. Successor responses can be fetched by the ADM-command NEXT.

### Response

For getting more rows at the result of the command the length of the
response area in the statement must be defined greater(administration
with CALL-DML).

## SEN2053

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN2053 END OF 'SESDCN' ADMINISTRATION STATEMENT, NO SUCCESSOR RESPONSES EXISTING.

### Meaning

Because any sucessor responses don't exist, an issue isn't possible.

## SEN3001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3001 DMS ERROR SESDCN BACKUP FILE: (&00)

### Meaning

DMS error occurred during open of SESDCN backup file. For more detailed
information about the DMS error code enter the command /HELP-MESS in
system mode or refer to the BS2000 'System Messages' manual.
(&00): DMS error code.

### Response

Analyze the DMS error.

## SEN3002

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3002 SESDCN RESTART NECESSARY. DATA FOR RESTART STILL STORED IN SESDCN LOGGING FILE

## SEN3003

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3003 CURRENT SESDCN LOGGING FILE: (&00)

## SEN3004

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3004 INTERNAL SYSTEM ERROR WHEN OPENING SESDCN LOGGING FILE

### Response

Submit dump to SESAM diagnostics staff.

## SEN3006

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3006 SESDCN-DCAM APPLICATION OPENED

## SEN3007

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3007 OPEN OF SESDCN-DCAM APPLICATION REJECTED DUE TO ERROR. DCAM RETURNCODE: (&00)

### Response

Take action according to DCAM returncode.

## SEN3008

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3008 DISTRIBUTION RULE SUPPLEMENTED BY ENTRIES NOT YET EXISTING

## SEN3009

Destination: CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3009 CATALOG ALREADY EXISTS IN THE DISTRIBUTION RULE WITH DIFFERENT LOCATIONS. ENTRY REJECTED.

## SEN3010

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3010 NO FREE DISTRIBUTION RULE ENTRY; INSUFFICIENT SPACE FOR DISTRIBUTION RULE TABLE

### Response

Modify SESDCN control statement.

## SEN3011

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3011 DISTRIBUTION RULE COMPLETELY CREATED

## SEN3012

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3012 '(&00)' SPECIFICATION FOR HOME PROCESSOR IN CONTROL STATEMENTS DIFFERENT FROM '(&01)' SPECIFICATION IN SESDCN LOGGING FI LE

### Response

Modify the control statements or assign the correct SESDCN logging file.

## SEN3013

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3013 INSUFFICIENT MEMORY FOR SESDCN COMMON MEMORY POOL

### Response

Check the SESDCN control statements.

## SEN3014

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3014 SESDCN LOGGING FILE WITH INVALID VERSION

### Meaning

The SESDCN logging file, accessed by default name SES.DLG<k>
(<k>: configuration-name) or allocated via link name SESDLG, has a
different version to program SESDCN.

### Response

Allocate the correct SESDCN logging file and restart program SESDCN.

## SEN3015

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3015 SESDCN LOGGING FILE WITH INVALID CONFIGURATION NAME: (&00)

### Meaning

The SESDCN logging file, accessed by default name SES.DLG or allocated via
link name SESDLG, belongs to a configuration which is different from that
of the program SESDCN.
(&00): name of the configuration to which belongs the SESDCN logging file.

### Response

Allocate the correct SESDCN logging file and restart program SESDCN.

## SEN3016

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3016 SESDCN LOGGING FILE '(&00)' CATALOGED UNDER MORE THAN ONE CAT ID; RENAME OR DELETE SUPERFLUOUS FILE(S)

### Meaning

The SESDCN logging file has been cataloged under more than one catalog
identification (CAT ID); it may not be cataloged under more than one.

### Response

Rename or delete superfluous SESDCN logging file.

## SEN3017

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SEN3017 COLD START PERFORMED BECAUSE OF 'COLDSTART' OPTION

### Meaning

A cold start was requested and performed.

## SEN3018

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SEN3018 COLD START NOT POSSIBLE BECAUSE TRANSACTIONS ARE IN PTC STATE

### Meaning

A cold start was requested by means of the start parameters but could not
be performed because transactions are in PTC state.

## SEN3019

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3019 REMOTE-ACCESS-OPTION OF SECONDARY DCN DOES NOT MATCH REMOTE-ACCESS-OPTION OF THE MASTER DCN

### Meaning

When SESDCN was started, it was determined that a SESDCN with a different
REMOTE-ACCESS option has already been started in this configuration.

### Response

Ensure that the REMOTE-ACCESS option of the secondary DCN matches that of
the master DCN and restart the new DCN.

## SEN3020

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3020 'SESDCN' READY

## SEN3021

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN3021 SECONDARY DCN STARTED UNDER USER ID WITH SECOLTP PRIVILEGE

### Meaning

An attempt was made to start a secondary DCN under a user ID with the
SECOLTP privilege. This secondary DCN is to connect to a configuration
which is not subject to transaction processing.

### Response

Check the assignment of security levels to SESAM configurations.

## SEN3022

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN3022 SECONDARY DCN STARTED IN USER ID WITHOUT SECOLTP PRIVILEGE

### Meaning

An attempt was made to start a secondary DCN under a user ID without the
SECOLTP privilege. This secondary DCN is to connect to a configuration
which is subject to transaction processing.

### Response

Check the assignment of security levels to SESAM configurations.

## SEN3023

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN3023 STARTUP OF SESDCN DCAM APPLICATION REJECTED; APPLICATION (&00) ALREADY EXISTS

### Meaning

A SESDCN with the same configuration and NAM specification as the current
one has already been loaded.

### Response

If necessary start SESDCN with a different configuration and/or NAM
specification.

## SEN3024

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN3024 ERROR ON CLOSING THE FILE (&00)

### Response

Submit the error documentation (dump and the file specified in the
message) for SESAM diagnosis.

## SEN3025

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN3025 SECONDARY DCN STARTED, SESDCN LOGGING FILE NOT FOUND

### Meaning

When the user attempted to start a secondary SESDCN in a distributed
configuration, no SESDCN logging file existed under the default name
SES.DLG<c> (<c> configuration name) or the link name SESDLG. The logging
file may have been deleted by the user after it was created by the master
DCN.

### Response

Terminate the entire configuration (including all its SESDCN, SESAM DBH
and user tasks). Start new configuration.

## SEN3026

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3026 SESDCN DCAM APPLICATION (&00) OPENED ON VIRTUAL HOST (&01)

## SEN3027

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN3027 HOST NAME (&00) OF SECONDARY DCN IS NOT THE SAME AS HOST NAME (&01) OF MASTER DCN

### Meaning

The DCN tasks of the current configuration are running on
different machines, because the DCAM application name of this
configuration is not listed in file
$TSOS.SYSDAT.BCAM.APPLICATIONS.

### Response

Terminate each task of the configuration and activate the virtual
host. Afterwards start the tasks of the configuration again.

## SEN4001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4001 MAXIMUM NUMBER OF CONNECTIONS TO DBHS EXCEEDED

### Meaning

Table overflow in the connection module (PTAB)

### Response

Wait until connections become free when DBHs are terminated.

## SEN4002

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4002 FURTHER CONNECTIONS CANNOT CURRENTLY BE ESTABLISHED BY DBCON

### Meaning

The internal table for managing DCAM connections (CHATX) in the user
connection module is full.

### Response

Wait until connections become free when application programs terminate.

## SEN4003

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN4003 FURTHER CONNECTIONS CANNOT CURRENTLY BE ESTABLISHED BY SESDCN

### Meaning

The internal table for managing DCAM connections (CHATX) in SESDCN is
full.

### Response

Wait until connections become free when application programs terminate.

## SEN4005

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4005 OPERATING SYSTEM COMPONENTS FOR INTERTASK COMMUNICATION NOT GENERATED; SESAM CANNOT BE EXECUTED

### Response

Restart BS2000 with the appropriate generation.

## SEN4006

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4006 OPERATING SYSTEM COMPONENTS FOR INTERTASK COMMUNICATION CANNOT BE EXECUTED BECAUSE OF LACK OF MEMORY

### Meaning

No more memory is available for the management areas of the operating
system components for intertask communication.

### Response

Repeat request later.

## SEN4007

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4007 INTERNAL ERROR: 'PK' ELEMENT DOES NOT CORRESPOND TO 'CHATX' ENTRY

### Meaning

Internal system error

### Response

Forward SESDCN dump for SESAM diagnosis.

## SEN4008

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4008 INTERNAL ERROR: DBH ENTRY NOT FOUND IN INTERNAL TABLE (PK)

### Meaning

Internal system error

### Response

Forward SESDCN dump for SESAM diagnosis.

## SEN4009

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN4009 INCOMPLETE BLOCK. PROCESSOR '(&00)', PARTNER '(&01)'

### Meaning

When a block was broken into fragments (as a result of MAXLN), not all the
fragments were received after 5 minutes.

### Response

Increase the time specification in the LETT parameter of the BCTIMES
command.

## SEN4010

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4010 LACK OF DCAM MEMORY FOR 'REMOTE-SEND' TO USER TASK: (&00) (&01). AT PRESENT, NO TRANSMISSION IS POSSIBLE

### Meaning

DCAM scratch pad memory is too small.

### Response

Check PDN generation, if error persists. Otherwise, retry job.

## SEN4011

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4011 NO RESPONSE MESSAGE FROM SESAM(&00) AFTER (&01) ATTEMPTS

### Meaning

SESDCN has been waiting unsuccessfully for a response from the DBH
(resource bottleneck at DBH). This has a negative effect on the
administration behavior of SESDCN.

### Response

Check the load options SYSTEM-LIMITS (THREADS parameter) and
SYSTEM-STRATEGIES (RETRIEVAL-CONTROL parameter) for the DBH being accessed

## SEN4012

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEN4012 DATA LOSS ON THE DCAM RECEIVE BUFFER ON RECEIPT OF A MESSAGE FROM THE PARTNER (&00) (&01)

### Meaning

(&00) = processor name; (&01) = DCAM application name.

### Response

Increase the time specification in the LETT parameter of the /BCTIMES
command.

## SEN4013

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4013 DCAM REPORTS '(&00)' (RESOIRCE BOTTLENECK) FOR REMOTE SEND TO USER '(&01)'.

### Meaning

After several attempts to send a message to the User (&01), DCAM reports
(&00). DCAM/BCAM is currently overloaded (see the DCAM manual for more
detailed information). The program is terminated.

### Response

Check DCAM generation and start program again.

## SEN4014

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4014 WHEN SENDING A MESSAGE TO PROCESSOR (&00), DCAM APPLICATION (&01) REPORTS DCAM '(&02)'

### Meaning

See the DCAM manual for a precise explanation of the DCAM message. For
example,
DCAM message "1004...." means lack of storage space.

### Response

If this situation occurs frequently, check the PDN generation.

## SEN4015

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4015 WHEN RECEIVING A MESSAGE FROM PROCESSOR (&00), DCAM APPLICATION (&01) REPORTS DCAM '(&02)'

### Meaning

See the DCAM manual for a precise explanation of the DCAM message.
For example, DCAM message "04001400" means loss of data due to timeout.

### Response

If this situation occurs frequently, check the PDN generation. In the case
of a timeout, increase the time value in the LETT parameter of the
BCTIMES command.

## SEN4016

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4016 RECEIVE MESSAGE FROM PROZESSOR (&00), DCAM APPLICATION (&01) INCOMPLETE

### Meaning

A message was split into submessages because the message length exceeded
MAXLN (see DCAM manual), and all submessages were not received within
5 minutes.

### Response

If this situation occurs frequently, check the PDN generation. In the case
of a timeout, increase the time value in the LETT parameter of the
BCTIMES command.

## SEN4017

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4017 A SUBMESSAGE THAT CANNOT BE ASSIGNED TO ANY MESSAGE HAS BEEN RECEIVED BY PROCESSOR (&00), DCAM APPLICATION (&01)

### Meaning

A message was split into submessages because the message length exceeded
MAXLN (see DCAM manual), and some submessages were lost or the submessages
were not received in the order in which they were sent.

### Response

If this situation occurs frequently, check the PDN generation.

## SEN4018

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4018 UNEXPECTED RETURN '(&00)' FROM DCAM-SVC (&01)

### Meaning

See the DCAM manual for a precise explanation of the DCAM message.
For example, DCAM message "100C...." means termination of DCS.

### Response

If this situation occurs frequently, check the state of the DCS subsystem.

## SEN4019

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4019 VIRTUAL HOST (&00) IS NOT ACTIVE

### Meaning

DBH/DCN of current configuration are started on a virtual host,
which is no longer active. Therefore communication between
DBH/DCN an applications is not possible.

### Response

Terminate all tasks of the current configuration and activate the
virtual host. Then start the tasks of the configuration again.

## SEN4020

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4020 DCAM APPLICATION (&00) CANNOT BE STARTED, BECAUSE THE VIRTUAL HOST IS NOT ACTIVE.

### Meaning

The DCAM application (&00) is assigned to a virtual host in the
file $TSOS.SYSDAT.BCAM.APPLICATIONS. The virtual host is not active.

### Response

Check why the virtual host is not active and activate it. Start
task again or start task on the machine where the virtual host
is active.

## SEN4041

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4041 CATALOG DOES NOT EXIST

## SEN4042

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4042 CATALOG ALREADY DELETED

## SEN4043

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEN4043 PROCESSOR NOT EXISTING

©2024 Fujitsu | BS2000 System Messages