## HJT0010

Destination: USER-TASK Routing code: Weight:

Warranty : NO

HJT0010 CISC-Compilation has used (&00) MB of Memory

## HJT0011

Destination: USER-TASK Routing code: Weight:

Warranty : NO

HJT0011 CISC-Compilation needs more than (&00) MB of Memory

## HJT0020

Destination: USER-TASK Routing code: Weight:

Warranty : NO

HJT0020 CISCFW-STATISTICS: (&00)

## HJT0021

Destination: USER-TASK Routing code: Weight:

Warranty : NO

HJT0021 JITSYS-Diag: (&00)

## HJT0022

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HJT0022 JITSYS-Error: (&00)

### Meaning

JITSYS internal Problem, please contact System-Administration

## HJT0030

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HJT0030 JITSYS can't read Class2-Parameters, Standard-Values (JTABSMEM=(&00), JTMAXMEM=(&01), JTSTDMEM=(&02)) used

## HJT0031

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

HJT0031 Specified JIT-Memory-Limit (&00) MB is reduced to (&01) MB, due to class-2-Option JTMAXMEM.

### Meaning

The via the comand
MOD-DBL-DEFAULTS SCOPE=*CMD-CALLS(CISC-COMPILATION=*YES(WORKSPACE=nn))
adjusted JIT-WORKSPACE is greater than the maximum value for this
parameter. The Maximum is adjusted by the System Administrator with
the class-2-Option JTMAXMEM. WORKSPACE is reduced to this value.

## HJT0032

Destination: CONSOLE Routing code: * (main console) Weight: 20

Warranty : NO

HJT0032 JIT-Memory-Limit (&00) MB for the current program exceeded.

### Meaning

JIT-Workspace for the current Program is exceeded,
you can adjust the JIT-Workspace with the comand
MOD-DBL-DEFAULTS SCOPE=*CMD-CALLS(CISC-COMPILATION=*YES(WORKSPACE=nn))
The Standard-Value for this
Parameter is given by the Class-2-Option JTSTDMEM.
Program-Run continues

## HJT0034

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HJT0034 Main Memory Shortage, Memory Management delivers no more JIT-Memory

### Meaning

Although the JIT-Memory-Limit JTABSMEM isn't yet reached
Memory-Managment delivers no more JIT-Memory
Perhaps there isn't enough Main-Memory configured or the
'Minimal Memory Size' is too small defined.
JTABSMEM should be at most 40 percent of the available
Main-Memory and should be at least 64 MB below the 'Minimal Memory Size'.
You can receive the values of these Parameters with the comand
/SHOW-SYSTEM-INFORMATION
If there is a DAB configured, JTABSMEM should be reduced by the
DAB-Memory-Size.
Please contact your System-Administration to check this.

## HJT0035

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HJT0035 JIT Memory Saturation: Level changes from (&00) to (&01)

### Meaning

Level 0: no JIT-Memory-Restrictions
Level 1: CISCFW only uses the JIT Minimum Memory Size
Level 2: New Programs run in Interpreter-Mode
Level 3: No Programstart possible

## HJT0036

Destination: CONSOLE Routing code: * (main console) Weight: 20

Warranty : NO

HJT0036 Main Memory Saturation, Memory Management delivers no more Big-Pages for JIT-Memory

## HJT0037

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HJT0037 System-Parameter JTSHMEM is reduced to (&00) MB, because JTABSMEM is only (&01) MB

## HJT0038

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HJT0038 Attention: The System-Parameter JTABSMEM (&00) is greater than the recommended size: (&01)

### Meaning

JTABSMEM should not be greater than 40% of the available Main-Memory
JTABSMEM should be at least 64 MB below the Minimal-Memory-Size
If JTABSMEM is adjusted to 0, JITSYS uses automatically the recommended
size

## HJT0039

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

HJT0039 JTABSMEM has changed from: (&00) MB to (&01) MB

## HJT0040

Destination: CONSOLE Routing code: * (main console) Weight: 20

Warranty : NO

HJT0040 Main Memory Saturation resolved, there are again Big-Pages for JIT-Memory

©2024 Fujitsu | BS2000 System Messages