## SNX2000

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SNX2000 AN ERROR HAS OCCURRED IN A PERIPHERAL COMPONENT - A SERVICE CALL WAS INITIATED. REPLY (EOT(CONTINUE))

### Meaning

X2000 informs BS2000 of an error in a peripheral component that cannot be reported via
an I/O. The message must be acknowledged by the operator.

### Response

Customer Support checks the peripheral units and connections with the help of the logging
file /var/log/messages.

## SNX2010

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SNX2010 MESSAGE FROM &01: CO-SKP SHUTDOWN (REASON: &02)
SNX2010 MESSAGE FROM &01: CO-SKP AVAILABLE AGAIN

### Meaning

&01: name of the MU which reports the message, &02 shutdown or not reachable
The other MU was stopped via normal stop (shutdown) or abnormally stopped (system crash). In the 2nd case (not reachable) the SNX2000 message will be sent, too. When the 2nd MU is working again, the message CO-SKP AVAILABLE AGAIN is sent.

### Response

Check the 2nd MU and if wanted please start it again.
Hint: After a crash an MU automatically starts.

## SNXCD01

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

SNXCD01 WRITE MEDIA ON DEVICE '(&00)' STARTED

### Meaning

Write process on device '(&00)' was started.

## SNXCD02

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

SNXCD02 WRITE MEDIA ON DEVICE '(&00)' SUCCESSFULLY FINISHED

### Meaning

Write process on device '(&00)' was successfully finished.

## SNXCD03

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

SNXCD03 WRITE MEDIA ON DEVICE '(&00)' FAILED

### Meaning

Error during writing data on device '(&00)'.

### Response

Insert appropriate empty medium, give notice to BS2000 by means of
/CHECK-TAPE and retry write process with /UNLOAD.

## SNXCD04

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

SNXCD04 BUFFER ON DEVICE '(&00)' NOT WRITTEN TO MEDIA

### Meaning

No data written on device '(&00)'. Data buffered in X2000.

## SNXCD05

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

SNXCD05 BUFFERED DATA ((&00)) ON DEVICE '(&01)' EXIST - WRITE POSSIBLE

### Meaning

Buffered data for device '(&01)' exist after /ATTACH.
(&00) = size of buffered data.
An appropriate empty medium is in drive.

### Response

Clear buffered data by means of INIT or start write process with
/UNLOAD.

## SNXCD06

Destination: CONSOLE Routing code: G Weight: 99

Warranty : NO

SNXCD06 BUFFERED DATA ((&00)) ON DEVICE '(&01)' EXIST - BUT WRITE IMPOSSIBLE

### Meaning

Buffered data for device '(&01)' exist after /ATTACH.
(&00) = size of buffered data.
No appropriate medium in drive.

### Response

Insert appropriate medium in drive and inform BS2000 by means
of /CHECK-TAPE. Clear buffered data with INIT or initiate write
process by means of /UNLOAD.

©2024 Fujitsu | BS2000 System Messages