## HLV0000

Destination: USER-TASK, CONSOLE Routing code: E Weight: 99

Warranty : NO

HLV0000 (&00)

## HLV0001

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HLV0001 VMHEL FILE '(&00)' OPENED WITH 'SPACE=(&01)'

### Meaning

The VMHEL file has been opened by means of the command
/START-VMHEL-LOGGING
or /CHANGE-VMHEL-FILE or during the startup.
(&00): name of the VMHEL file,
(&01): primary allocation

## HLV0002

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HLV0002 VMHEL FILE '(&00)' CLOSED

### Meaning

The VMHEL file has been closed by means of the command
/STOP-VMHEL-LOGGING or /CHANGE-VMHEL-FILE or during the shutdown.
(&00): name of the VMHEL file

## HLV0003

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HLV0003 GLOBAL HW ERROR LOGGING IS ACTIVE. FILE : '(&00)'

### Meaning

(&00): name of the VMHEL file

## HLV0004

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HLV0004 GLOBAL HW ERROR LOGGING INACTIVE.

## HLV0005

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HLV0005 TELESERVICE ALARM BY VMHEL IS ACTIVE. MONITORING INTERVALL FROM (&00) TO (&01).

### Meaning

The threshold monitoring of VMHEL and calling of teleservice is active.
Calling of teleservice is done only in the specified time interval.

## HLV0006

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HLV0006 TELESERVICE ALARM BY VMHEL IS DEACTIVATED.

### Meaning

The threshold monitoring of VMHEL and calling of teleservice
is deactivated.

## HLV0010

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HLV0010 GLOBAL HW ERROR LOGGING NOT ACTIVE. (&00) COMMAND REJECTED.

### Meaning

All VMHEL commands except for /START-VMHEL-LOGGING and /SHOW-VMHEL-STATUS
are only permitted if global HW error logging is active.

### Response

Issue a /START-VMHEL-LOGGING command and retry command.

## HLV0011

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HLV0011 GLOBAL HW ERROR LOGGING ALREADY ACTIVE. /START-VMHEL-LOGGING COMMAND IGNORED.

### Meaning

The /START-VMHEL-LOGGING command is only permitted, if global
HW error logging is not active.

## HLV0012

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HLV0012 GLOBAL HW ERROR LOGGING ALREADY STOPPED. /STOP-VMHEL-LOGGING COMMAND IGNORED.

### Meaning

The /STOP-VMHEL-LOGGING command is only permitted, if global
HW error logging is active.

## HLV0050

Destination: CONSOLE Routing code: H Weight: 50

Warranty : NO

HLV0050 CALL TELESERVICE. GLOB.THRESHOLD FOR CTID (&00), PRIO (&01), (&02), SEQ# (&03) REACHED

## HLV0100

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HLV0100 INTERNAL ERROR. COMMAND PROCESSING ABORTED.

## HLV0101

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HLV0101 SYSTEM ERROR. (&00) NOT AVAILABLE. /START-VMHEL-LOGGING COMMAND NOT PROCESSED.

### Meaning

Global HW error logging could not be activated because a necessary
resource was not available for the VMHEL system.
(&00): memory, VMHEL task, bourse, slotpool, slot, EXVT anchor

## HLV0102

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HLV0102 SYSTEM ERROR. (&00) COULD NOT BE RELEASED BY GLOBAL HW ERROR LOGGING. /STOP-VMHEL-LOGGING COMMAND NOT PROCESSED.

### Meaning

A resource could not be released by VMHEL.
(&00): memory, VMHEL task, bourse or slotpool.

## HLV0105

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HLV0105 BOURSE CALLING ERROR. COMMAND PROCESSING ABORTED.

### Meaning

A bourse calling error occurred while trying to communicate with the
VMHEL system task.

## HLV0106

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HLV0106 SYSTEM ERROR. GLOBAL HW ERROR LOGGING NOT ACTIVATED. DMS ERROR '(&00)' WHEN PROCESSING FILE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00). COMMAND PROCESSING ABORTED.

### Meaning

While processing the VMHEL file a DMS error occurred.
(&00): DMS error code,
(&01): file name

### Response

Remove error cause and try /START-VMHEL-LOGGING.

## HLV0107

Destination: CONSOLE Routing code: H Weight: 70

Warranty : NO

HLV0107 SYSTEM ERROR. DMS ERROR '(&00)' WHEN PROCESSING FILE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00). DATA NOT STORED.

### Meaning

While processing the VMHEL file a DMS error occurred.
(&00): DMS error code,
(&01): file name

### Response

Try /CHANGE-VMHEL-FILE.

## HLV0108

Destination: CONSOLE Routing code: H Weight: 70

Warranty : YES

HLV0108 INTERNAL TABLE FOR GLOBAL THRESHOLD MODIFICATIONS FULL. NO MODIFICATION PERFORMED.

### Meaning

The limit of number of entries for modification of global threshold is
reached. No modification performed.

### Response

All additional settings could be cleared by /MODIFY-VMHEL-CHECK
CHECK=*STD.

## HLV0109

Destination: CONSOLE Routing code: H Weight: 70

Warranty : YES

HLV0109 INTERNAL TABLE FOR GLOBAL LOGGING MODIFICATIONS FULL. NO MODIFICATION PERFORMED.

### Meaning

The limit of number of entries for modification of logging is reached.
No modification performed.

### Response

All additional settings could be cleared by /MODIFY-VMHEL-LOGGING
LOGGING=*STD.

## HLV0110

Destination: CONSOLE Routing code: H Weight: 50

Warranty : YES

HLV0110 USER IS NOT AUTHORIZED TO ISSUE THE COMMAND. COMMAND REJECTED.

### Meaning

The user does not have the privilege to issue the command.

## HLV1001

Destination: CONSOLE Routing code: H Weight: 50

Warranty : NO

HLV1001 STARTUP ERROR. GLOBAL HW ERROR LOGGING NOT ACTIVATED. (&00) NOT AVAILABLE. STARTUP CONTINUES.

### Meaning

Global HW error logging could not be activated because a necessary
resource was not available for the VMHEL system.
(&00): memory, VMHEL task, bourse, slotpool, slot, EXVT anchor

### Response

Try /START-VMHEL-LOGGING later.

## HLV1002

Destination: CONSOLE Routing code: H Weight: 50

Warranty : NO

HLV1002 STARTUP ERROR. GLOBAL HW ERROR LOGGING NOT ACTIVATED. BOURSE CALLING ERROR. STARTUP CONTINUES.

### Meaning

Global HW error logging could not be activated because a bourse calling
error occurred while trying to communicate with the VMHEL system task.

### Response

Try /START-VMHEL-LOGGING later.

## HLV1003

Destination: CONSOLE Routing code: H Weight: 50

Warranty : NO

HLV1003 STARTUP ERROR. GLOBAL HW ERROR LOGGING NOT ACTIVATED. DMS ERROR '(&00)' WHEN PROCESSING FILE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

While processing the VMHEL file a DMS error occurred.
(&00): DMS error code,
(&01): file name

### Response

Remove error cause and try /START-VMHEL-LOGGING.

## HLV9000

Destination: CONSOLE Routing code: H Weight: 70

Warranty : NO

HLV9000 SYSTEM ERROR. GLOBAL HW ERROR LOGGING ABORTED.

### Meaning

A system error has resulted in an abnormal termination of the
VMHEL task.

## HLV9001

Destination: CONSOLE Routing code: H Weight: 70

Warranty : NO

HLV9001 SYSTEM ERROR: DMS ERROR '(&00)' WHEN PROCESSING FILE '(&01)'. IN SYSTEM MODE: /HELP-MSG DMS(&00).

### Meaning

A DMS error resulted in an abnormal VMHEL task termination. Global
HW error logging aborted.
(&00): DMS error code
(&01): file name

## HLV9002

Destination: CONSOLE Routing code: H Weight: 70

Warranty : NO

HLV9002 SYSTEM ERROR. BOURSE CALLING ERROR.

### Meaning

A bourse calling error resulted in an abnormal VMHEL task termination.
Global HW error logging aborted.

## HLV9003

Destination: CONSOLE Routing code: H Weight: 70

Warranty : NO

HLV9003 SYSTEM ERROR. VMHEL SPECIFIC DISC SPACE ON PUBSET USED UP.

### Meaning

The specific disc space for the global HW error logging is used up.
Global HW error logging aborted.

### Response

Remove the error cause (perhaps delete old HEL files) and reactivate
the global HW error logging with a /START-VMHEL-LOGGING.

©2024 Fujitsu | BS2000 System Messages