## CPR0101

Destination: USER-TASK Routing code: Weight:

Warranty : NO

CPR0101 File '(&00)' was accessed with RFA. It is not possible to write a checkpoint.

### Meaning

(&00) File name

### Response

Clear the RFA connection and try to write the checkpoint again.

## CPR0102

Destination: USER-TASK Routing code: Weight:

Warranty : NO

CPR0102 POSIX is active in current task. No /RESTART-PROGRAM possible

### Response

Remove POSIX connection and repeat /RESTART-PROGRAM

## CPR0103

Destination: USER-TASK Routing code: Weight:

Warranty : NO

CPR0103 Error occured when accessing the file '(&00)'

### Meaning

(&00) Filename

### Response

Analyse the WRCPT returncode.
Correct the error.
Repeat to write the checkpoint.

## CPR0105

Destination: USER-TASK Routing code: Weight:

Warranty : NO

CPR0105 File '(&00)' was accessed with access method DIV. It is not possible to write a checkpoint

### Meaning

Close the file and repeat the attempt to write the checkpoint.

©2024 Fujitsu | BS2000 System Messages