## NDE0001

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0001 (&17) DEVICE (&00)(&10)(&09)(&11) STATE CHANGED TO: '(&07)'

## NDE0008

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0008 HOST ACCESS FOR (&17) SYSTEM '(&10)' CHANGED TO: '(&08)'

### Meaning

STORAGE-SYSTEM: specifies the STORAGE system of emulated devices
by its serial number (&10).
Possible access states (&08):
DIRECT : Direct access.
NO : No access from host
INITIALIZING : Host is initializing datastructures.
UNMANAGEABLE : Storage system not manageable, as StorMan server is
not reachable.
NO-INST : StorMan server finds no available instance to manage
the storage system.
IN-DELETE : No access and no BS2000 device configured. The storage
system will be removed from configuration tables, if it
is not rediscovered by StorMan within waittime.
--------------------------------------------------------------------------

### Response

None

## NDE0019

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0019 CONNECTION STATE FROM STORAGE SYSTEM PORT '(&10),(&07)' TO '(&12),(&08)' CHANGED TO '(&16)'

### Meaning

The connection state of a storage system port to a remote system port has
changed. The ports are characterized by their system serial number and
portname.
Possible connection states (&16):
*DOWN: Connection down
*UP: Connection up

## NDE0020

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0020 STATE OF 'REMOTE COPY' CHANGED TO '(&07)' FOR PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13)

### Meaning

'REMOTE COPY' State: State of the remote copy operations for a remote
copy pair. Possible values: *ACTIVE, *IN-HOLD or *ERROR.

## NDE0021

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0021 STATE OF REMOTE COPY PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13) SOURCE UNIT CHANGED TO '(&07)'

### Meaning

SOURCE-UNIT: first device of a remote copy pair which is accessed by the
local host.

## NDE0022

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0022 STATE OF REMOTE COPY TARGET UNIT (&00)(&10)(&09)(&11) CHANGED TO '(&07)'

### Meaning

TARGET-UNIT: second device of a remote copy pair.

## NDE0023

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0023 LINK STATE OF REMOTE COPY PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13) CHANGED TO: '(&07)'

### Meaning

LINK-STATE: State of the connection between source unit and target unit
of a remote copy pair. Possible values: *AVAILABLE, *NOT-AVAILABLE or
*UNDEFINED.

## NDE0024

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0024 'TARGET-ACCESS' FOR REMOTE COPY PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13) CHANGED TO: '(&07)'

### Meaning

TARGET-ACCESS: Access to the target unit of the remote copy pair.
Possible values: *BY-SOURCE, *DIRECT or *NONE.

## NDE0025

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0025 REMOTE COPY PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13) SYNCHRONIZED AGAIN

### Meaning

The internal synchronisation process is completed for the remote copy
pair in state *ACTIVE.

## NDE0026

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0026 REMOTE COPY PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13) OUT OF SYNCHRONIZATION

### Meaning

The remote copy pair is out of synchronization. The pending updates are
kept internal by the storage system.

## NDE0027

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0027 SOURCE-UNIT AND TARGET-UNIT OF REMOTE COPY PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13) SWAPPED

### Meaning

The SOURCE- and TARGET-UNIT of the remote copy pair were swapped due to
a configuration change on the storage system.

### Response

Get more information using the command
/SHOW-REMOTE-COPY-STATUS ... INFORMATION=*ALL.

## NDE0028

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0028 REMOTE COPY PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13) CONSISTENT AGAIN

### Meaning

The remote copy pair in state *ACTIVE is consistent now.

## NDE0029

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0029 REMOTE COPY PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13) OUT OF CONSISTENCY

### Meaning

The remote copy pair is out of consistency.

## NDE0032

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0032 COPY-MODE OF REMOTE COPY PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13) CHANGED TO '(&07)'

### Meaning

COPY-MODE of a remote copy pair specifies the processing mode of the
remote replication.

## NDE0044

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0044 NEW DEVICE '(&00)' AVAILABLE ON STORAGE SYSTEM '(&10)'

## NDE0045

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0045 DEVICE '(&00)' REMOVED FROM STORAGE SYSTEM '(&10)'

## NDE0050

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0050 SNAP STATE CHANGED TO '(&07)' FOR SNAP PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13)

### Meaning

SNAP State: Processing state of SNAP mirroring for a SNAP pair.
Possible values: *UNUSED, *CREATED, *COPY-ON-WRITE, *COPIED,
*RESTORED, *RESTORE-IN-PROG, *CREATE-IN-PROG,
*TERMINATE-IN-PROG, *COPY-IN-PROG, *FAILED,
*POINT-IN-TIME, *INVALID, *UNKNOWN.

## NDE0053

Destination: USER-TASK, CONSOLE Routing code: D Weight: 99

Warranty : NO

NDE0053 SNAP SAVEPOOL (&07) ON STORAGE SYSTEM (&10) REACHED ALARM STATUS 'NORMAL': (&08) PERCENT FULL

### Meaning

The common SAVEPOOL has reached a space saturation level of alarm status
NORMAL.

### Response

/SHOW-STORAGE-CONFIGURATON ...,INFO=*SAVE-POOLS informs about
current alarm status settings.

## NDE0057

Destination: USER-TASK, CONSOLE Routing code: D Weight: 99

Warranty : NO

NDE0057 SNAP SAVEPOOL (&07) ON STORAGE SYSTEM (&10) REACHED ALARM STATUS 'ATTENTION': (&08) PERCENT FULL

### Meaning

The common SAVEPOOL has reached a space saturation level of alarm status
ATTENTION.
At 100 % saturation COPY-ON-WRITE operation will stop and the SNAP pair
will change to status *FAILED.

### Response

Terminate no longer required SNAP pairs using /STOP-SNAP-SESSION.

## NDE0058

Destination: USER-TASK, CONSOLE Routing code: D Weight: 99

Warranty : NO

NDE0058 SNAP SAVEPOOL (&07) ON STORAGE SYSTEM (&10) REACHED ALARM STATUS 'WARNING': (&08) PERCENT FULL

### Meaning

The common SAVEPOOL has reached a space saturation level of alarm status
WARNING.
At 100 % saturation COPY-ON-WRITE operation will stop and the SNAP pair
will change to status *FAILED.

### Response

Terminate no longer required SNAP pairs using /STOP-SNAP-SESSION.

## NDE0059

Destination: USER-TASK, CONSOLE Routing code: D Weight: 99

Warranty : NO

NDE0059 SNAP SAVEPOOL (&07) ON STORAGE SYSTEM (&10) REACHED ALARM STATUS 'CRITICAL': (&08) PERCENT FULL

### Meaning

The common SAVEPOOL has reached a space saturation level of alarm status
CRITICAL.
At 100 % saturation COPY-ON-WRITE operation will stop and the SNAP pair
will change to status *FAILED.

### Response

Terminate no longer required SNAP pairs using /STOP-SNAP-SESSION.

## NDE0060

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0060 CLONE STATE CHANGED TO '(&07)' FOR CLONE PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13)

### Meaning

CLONE State: Processing state of CLONE mirroring for a CLONE pair.
Possible values: *CREATED,*COPY-ON-ACCESS,*COPIED,
*RESTORED,*RESTORE-IN-PROG,*CREATE-IN-PROG,
*TERMINATE-IN-PROG,*COPY-IN-PROG,*PRECOPY,
*RECREATED,*SYNCHRONIZING,*SYNCHRONIZED,*SPLIT,
*SUSPENDED,*FAILED,*INVALID,*INACTIVE,*UNUSED.

## NDE0061

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0061 CLONE PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13) SWAPPED

### Meaning

The original- and clone-unit of a clone pair were swapped due to
a command input.

### Response

Get more information using the command
/SHOW-CLONE-SESSION-STATUS... .

## NDE0073

Destination: USER-TASK, CONSOLE Routing code: D Weight: 99

Warranty : NO

NDE0073 THIN PROVISIONING POOL (&07) ON STORAGE SYSTEM (&10) REACHED ALARM STATUS 'NORMAL': (&08) PERCENT FULL

### Meaning

The specified THIN PROVISIONING POOL has reached the space saturation
level of alarm status NORMAL.

### Response

/SHOW-STORAGE-CONFIGURATON ...,INFO=*THIN-POOLS informs about the
current alarm status settings.<

## NDE0074

Destination: USER-TASK, CONSOLE Routing code: D Weight: 99

Warranty : NO

NDE0074 THIN PROVISIONING DEVICE (&00)(&10)(&09)(&11) REACHED USED SPACE SATURATION: (&08) PERCENT FULL

### Meaning

The used space of the given THIN PROVISIONING DEVICE has reached a space
saturation level, which triggers this warning.

### Response

Extend pool by allocating more devices.

## NDE0077

Destination: USER-TASK, CONSOLE Routing code: D Weight: 99

Warranty : NO

NDE0077 THIN PROVISIONING POOL (&07) ON STORAGE SYSTEM (&10) REACHED ALARM STATUS 'ATTENTION': (&08) PERCENT FULL

### Meaning

The specified THIN PROVISIONING POOL has reached the space saturation
level of alarm status ATTENTION.

### Response

The resources of the THIN PROVISIONING Pool have to be extended.

## NDE0078

Destination: USER-TASK, CONSOLE Routing code: D Weight: 99

Warranty : NO

NDE0078 THIN PROVISIONING POOL (&07) ON STORAGE SYSTEM (&10) REACHED ALARM STATUS 'WARNING': (&08) PERCENT FULL

### Meaning

The specified THIN PROVISIONING POOL has reached the space saturation
level of alarm status WARNING.

### Response

The resources of the THIN PROVISIONING Pool have to be extended.

## NDE0080

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0080 STATE OF STORAGE CLUSTER (&07) CHANGED TO '(&08)'

### Meaning

Possible values for insert 8: NORMAL, DISABLED, HALT, UNKNOWN

## NDE0081

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0081 PHASE OF STORAGE CLUSTER (&07) CHANGED TO '(&08)'

### Meaning

Possible values for insert 8: NORMAL, DISABLED, INITIALIZED, COPYING
MAINTENANCE, FAILED-OVER, COPYING-BACK, FAILBACK-READY, FAILED-BACK,
UNKNOWN, FAILED.

## NDE0083

Destination: USER-TASK, CONSOLE Routing code: D Weight: 99

Warranty : NO

NDE0083 FLEXIBLE TIERED POOL (&07) ON STORAGE SYSTEM (&10) REACHED ALARM STATUS 'NORMAL': (&08) PERCENT FULL

### Meaning

The specified FLEXIBLE TIERED POOL has reached the space saturation
level of alarm status NORMAL.

### Response

/SHOW-STORAGE-CONFIGURATON ...,INFO=*FLEX-POOLS informs about the
current alarm status settings.<

## NDE0087

Destination: USER-TASK, CONSOLE Routing code: D Weight: 99

Warranty : NO

NDE0087 FLEXIBLE TIERED POOL (&07) ON STORAGE SYSTEM (&10) REACHED ALARM STATUS 'ATTENTION': (&08) PERCENT FULL

### Meaning

The specified FLEXIBLE TIERED POOL has reached the space saturation
level of alarm status ATTENTION.

### Response

The resources of the FLEXIBLE TIERED Pool have to be extended.

## NDE0088

Destination: USER-TASK, CONSOLE Routing code: D Weight: 99

Warranty : NO

NDE0088 FLEXIBLE TIERED POOL (&07) ON STORAGE SYSTEM (&10) REACHED ALARM STATUS 'WARNING': (&08) PERCENT FULL

### Meaning

The specified FLEXIBLE TIERED POOL has reached the space saturation
level of alarm status WARNING.

### Response

The resources of the FLEXIBLE TIERED Pool have to be extended.

## NDE0100

Destination: CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE0100 (&07)-ADMIN-SCOPE FOR SHC-OSD CHANGED TO '(&08)'

## NDE1000

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1000 DEVICE '(&00)' NOT FOUND

### Meaning

Possible Reasons:
- the device is not configured in BS2000
- the MN is no device of a supported storage system

### Response

Check the device with /SHOW-DISK or /SHOW-DEVICE-CONFIGURATION.

## NDE1001

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1001 DEVICE (&00)(&10)(&09)(&11) NOT ATTACHED

## NDE1002

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1002 CONTROLLER UNIT '(&01)' NOT FOUND ON A SUPPORTED STORAGE SYSTEM

### Meaning

The controller unit is not generated as an emulated controller of a
supported Storage system or not generated at all.

## NDE1003

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1003 VOLUME '(&02)' NOT ONLINE, NOT UNIQUE OR NOT ON A SUPPORTED STORAGE SYSTEM

## NDE1004

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1004 PUBSET '(&03)' NOT FOUND ON A SUPPORTED STORAGE SYSTEM

## NDE1005

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1005 PUBSET '(&03)' NOT HOMOGENEOUS

### Meaning

Not all volumes of the pubsets were found or do not have the same
mirror properties.

## NDE1006

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1006 (&07) '(&02)(&03)' (&08) (&00) NOT FREE

### Meaning

The specified PUBSET (&03) is allocated or
The specified VOLUME (&02) ON DEVICE with mn (&00) is allocated.

## NDE1008

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1008 VOLUME '(&02)' COULD NOT BE ALLOCATED ON DEVICE '(&00)'

### Meaning

Either the volume itself could not be allocated (e.g. if it already is
allocated by a different system or if a NKVD013 message has been rejected)
or the corresponding pubset could not be occupied.

## NDE1015

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1015 DEVICE (&10)(&09)(&11) NOT DEFINED

### Meaning

The device to be processed is not defined, SHC-OSD knows only its internal
device number. However, the chosen function requests the device to be
defined.

## NDE1017

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1017 COMMAND (&04) REJECTED FOR CURRENT TASK/SYSTEM-ADMIN-SCOPE

### Meaning

The current settings of SYSTEM-ADMIN-SCOPE and TASK-ADMIN-SCOPE do not
allow the processing of the command with the given operands.

### Response

Display the current settings:
/SHOW-SHC-PROCESSING
Modify the settings:
/MODIFY-SHC-PROCESSING SYSTEM-ADMIN-SCOPE=*PARAMETERS(...),
TASK-ADMIN-SCOPE=*PARAMETERS(...)

## NDE1020

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1020 NO REMOTE COPY FUNCTION FOR (&07) (&00)(&01)(&02)(&03)(&10)(&09)(&11)

### Meaning

The unit specifies the selected MN of the device, VSN of the volume, catid
of the pubset or MN of the controller selected by the command input.
Values for insert 7:
UNIT, if Insert 0 is specified.
CONTROLLER, if Insert 1 is specified.
VOLUME, if Insert 2 is specified.
PUBSET, if Insert 3 is specified.
SERIAL-NO, if Insert 11 is specified.
MN LIST, if at least one listelement is invalid.

### Response

Correct and retry.

## NDE1021

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1021 (&07) (&00)(&01)(&02)(&03)(&10)(&09)(&11) IS (HAS) NO SOURCE-UNIT

### Meaning

The unit specifies the selected MN of the device, VSN of the volume, catid
of the pubset or MN of the controller selected by the command input.
Values for insert 7:
UNIT, if Insert 0 is specified.
CONTROLLER, if Insert 1 is specified.
VOLUME, if Insert 2 is specified.
PUBSET, if Insert 3 is specified.
SOURCE-UNIT: first device of a remote copy pair which is addressed by the
local host.

## NDE1022

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1022 (&07) (&00)(&01)(&02)(&03)(&10)(&09)(&11) IS OR HAS NO TARGET UNIT

### Meaning

Values for insert 7:
UNIT, if Insert 0 is specified.
CONTROLLER, if Insert 1 is specified.
VOLUME, if Insert 2 is specified.
PUBSET, if Insert 3 is specified.
TARGET-UNIT: second device of a remote copy pair.

## NDE1024

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1024 REMOTE CONTROLLER UNIT '(&01)' NOT FOUND

### Meaning

Possible reasons:
- No remote controller unit with this MN found.
- The controller unit was found, but it is emulated in the local storage
system.

## NDE1025

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1025 NO DIRECT ACCESS FROM LOCAL HOST TO SOURCE-UNIT (&00)(&10)(&09)(&11)

### Meaning

SOURCE-UNIT: first device of a remote copy pair which is accessed by the
local host.

## NDE1026

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1026 NO ACCESS FROM HOST TO TARGET UNIT (&06)(&12)(&14)(&13)

### Meaning

TARGET-UNIT: second device of a remote copy pair.

## NDE1027

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1027 REMOTE-COPY PAIR (&00)(&10)(&09)(&11),(&06)(&12)(&14)(&13) STATE IS *ACTIVE. COMMAND '(&04)' NOT PROCESSED.

## NDE1028

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1028 VOLUMES IN (&07) '(&01)(&02)(&03)' NOT UNIQUE

### Meaning

Values for insert 7:
CONTROLLER, if Insert 1 is specified.
VOLUME, if Insert 2 is specified.
PUBSET, if Insert 3 is specified.

## NDE1029

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1029 TARGET UNIT (&00)(&10)(&09)(&11) IN STATE '*DISABLED' DUE TO PENDING UPDATES

## NDE1036

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1036 DIFFERENT LENGTHS OF CATALOG IDENTIFIERS OF 'PUBSET' AND 'NEW-PUBSET'

## NDE1043

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1043 PUBSET TYPE OF PUBSET '(&03)' NOT SUPPORTED

### Meaning

1. Local and remote replication functions do not support integrated
renaming of SM Pubsets or Volume Sets (operand NEW-PUBSET).
2. The commands /START-SNAP-SESSION, /START-CLONE-SESSION,
/ACTIVATE-SNAP/-CLONE and /HOLD-REMOTE-COPY
with operand HOLD-IO=*UNTIL-... are not supported for Volume Sets.

## NDE1044

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1044 PUBSET '(&03)' ALREADY EXISTS

### Meaning

Volume(s) were found ONLINE or allocated that may belong to a pubset
with the same catalog id as the one specified for renaming.

## NDE1045

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1045 COMMAND '(&04)' NOT COMPLETED, PUBSET RENAMING NOT POSSIBLE

### Meaning

The renaming of the local mirror units requested by the command can't
be processed. Possible reasons:
- Splitting of all local mirror pairs of the pubset is not yet completed.
- The split local mirror units are not consistent as a pubset.

### Response

Splitting local mirror pairs must be done on a defined consistency point
or by using the option HOLD-IO.

## NDE1047

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1047 SHC-OSD SUSPENDS IO ACCESS TO PUBSET '(&03)'

### Meaning

While executing a command with option HOLD-IO=*UNTIL-SPLIT,
IOs to the pubset (&03) are suspended. They will be resumed automatically
after the current IOs are terminated and all necessary
actions to the affected mirror pairs are executed.

## NDE1048

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1048 SHC-OSD RESUMES IO ACCESS TO PUBSET '(&03)'

## NDE1057

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1057 FUNCTION (&08) NOT SUPPORTED FOR (&07)

## NDE1058

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1058 ALL REMAINING LOCAL MIRRORS OF DEVICE (&00)(&10)(&09)(&11) RESERVED FOR SNAPSETS

### Meaning

The combination of PUBSET-setting of SNAPSET-Limit and MULTI-SNAP=NO
has reached the maximum of 16 mirrors.

### Response

Reduce the SNAPSET-Limit.

## NDE1063

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1063 SOURCE-UNIT OF THE REMOTE COPY PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13) NOT IN STATE '*READY'

### Meaning

SOURCE-UNIT: first device of a remote copy pair which is accessed by the
local host.

## NDE1066

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1066 NO REMOTE-LINK AVAILABLE BETWEEN SOURCE-UNIT (&00)(&10)(&09)(&11) AND TARGET-UNIT (&06)(&12)(&14)(&13)

### Meaning

SOURCE-UNIT: first device of a remote copy pair which is accessed by the
local host.
TARGET-UNIT: second device of a remote copy pair.

## NDE1067

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1067 REMOTE COPY PAIR (&00)(&10)(&09)(&11),(&06)(&12)(&14)(&13) NOT YET SYNCHRONIZED

### Meaning

The synchronization of the remote copy pair is not yet completed due
to pending updates
- after setting the COPY-MODE to SYNCHRONOUS,
- after resuming the remote copy function with /RESUME-REMOTE-COPY,
- before suspending the remote copy function with /HOLD-REMOTE-COPY.
SOURCE-UNIT: first device of a remote copy pair which is accessed by the
local host.

### Response

To suspend the remote copy function, use /HOLD-REMOTE-COPY with
option FORCE=*YES.

## NDE1069

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1069 NO CURRENT INFORMATION AVAILABLE ABOUT SOME REMOTE COPY PAIRS

### Meaning

There is no access to some Source-Units or Target-Units of Remote Copy
pairs for the moment. As result some internal administration data tables
of SHC-OSD are not updated.

## NDE1070

Destination: USER-TASK, CONSOLE Routing code: 0 Weight: 70

Warranty : YES

NDE1070 REMOTE COPY MODE CHANGED TO '(&07)' FOR REMOTE COPY PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13)

## NDE1073

Destination: USER-TASK, CONSOLE Routing code: 0 Weight: 70

Warranty : YES

NDE1073 (&04)(&07) PROCESSED FOR PAIR (&00)(&10)(&09)(&11),(&06)(&12)(&14)(&13)

## NDE1078

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1078 REMOTE-COPY-UNIT '(&00)' USED FOR PAGING ALLOCATION

### Meaning

The Source-Unit/Target-Unit of the remote copy pair is used for paging.
Modifying the target access would lead to system crash.

## NDE1079

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1079 NO DEVICE OF SELECTED (&07) (&00)(&01)(&02)(&03)(&10) ATTACHED

### Meaning

No device selected by the operand UNIT is attached.
Values for insert 7:
UNIT, if Insert 0 is specified.
CONTROLLER, if Insert 1 is specified.
VOLUME, if Insert 2 is specified.
PUBSET, if Insert 3 is specified.

## NDE1082

Destination: USER-TASK, CONSOLE Routing code: 0 Weight: 70

Warranty : YES

NDE1082 SHORTAGE OF MEMORY DURING PROCESSING OF COMMAND '(&04)'

## NDE1087

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1087 (&07) '(&02)(&03)' NOT ALLOCATED, HOLD-IO=*UNTIL-... NOT PERMITTED

### Meaning

The specified volume/pubset is not allocated although HOLD-IO=*UNTIL-...
was specified.
Values for insert 7:
VOLUME, if Insert 2 is specified.
PUBSET, if Insert 3 is specified.

### Response

Retry command with HOLD-IO=*NO.

## NDE1088

Destination: USER-TASK, CONSOLE Routing code: 0 Weight: 70

Warranty : YES

NDE1088 (&07) MB PENDING UPDATES STILL TO BE COPIED FROM (&00)(&10)(&09)(&11)

### Meaning

Pending updates of the specified size are copied from the SOURCE
unit (&00) to the corresponding TARGET
unit to synchronize the replication pair.

## NDE1089

Destination: USER-TASK, CONSOLE Routing code: 0 Weight: 70

Warranty : YES

NDE1089 (&07) MB PENDING UPDATES STILL TO BE COPIED TO UNIT (&00)(&10)(&09)(&11)

### Meaning

Pending updates of the specified size are copied from the TARGET
unit to the SOURCE unit (&00)
to synchronize the replication pair.

## NDE1100

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1100 PUBSET '(&03)' IS IN STATE '(&07)'

### Meaning

1. All commands support pubsets only if they are locally imported
or completely exported.
2. SHOW-commands support SM-pubsets only if they are locally imported.

## NDE1101

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1101 MORE THAN ONE SHARER FOR PUBSET '(&03)' AND REQUIREMENTS FOR HOLD-IO FOR SHARED PUBSETS NOT MET: '(&07)'

### Meaning

Requirements:
1. Command execution on master
2. MSCF connections between master and all slave computers are active.
3. SHC-OSD is started on all slave computers.
Rejection due to &07

## NDE1102

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1102 NOT ALL VOLUMES OF PUBSET '(&03)' ALLOCATED

### Meaning

Possible Reasons:
1. The Pubset could not be allocated.
2. The list of volumes for the SM-Pubset in state EXPORTED can't be
provided due to not unique VSNs mounted on the devices.

### Response

- Please enter /DETACH-DEVICE for unused devices to avoid not
unique VSNs.
- Check the system allocation for all volumes of the pubset.

## NDE1103

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1103 NO RECONFIGURATION LOCK FOR PUBSET '(&03)'

### Meaning

The imported Pubset could not be locked against reconfiguration.

## NDE1104

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1104 DAB CACHING ACTIVE FOR PUBSET '(&03)' ON HOST '(&07)'

### Meaning

The imported Pubset uses DAB for caching.
The specified action may lead to data inconsistency.
Values for Insert 07:
*LOCAL-HOST: own (local) host
<hostname> : BCAM name of partner computer in MSCF cluster.

## NDE1105

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1105 PUBSET '(&03)' VOLUME CATALOG NOT READABLE OR INCONSISTENT

### Meaning

The Pubset Online Catalog could on the PUBRES volume could not be read
or is inconsistent. This may occur if the PUBRES was only initializied
but no pubset has yet been built.
PUBRES: First volume of a pubset, e.g. PUBA00.

## NDE1106

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1106 '(&04)' WAITS FOR DEVICES TO COMPLETE SYNCHRONIZATION

### Meaning

'(&04)' is a command of SHC-OSD where the user specified to wait for
the completion of a synchronization process it initialized.
The command can be terminated in dialog mode by pressing the K2 key.

## NDE1107

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1107 NO ALLOCATION POSSIBLE FOR PUBSET '(&03)'

### Meaning

Possible Reasons:
1. The Pubset could not be allocated.
2. The list of volumes for the SM-Pubset in state EXPORTED can't be
provided due to not unique VSNs mounted on the devices.

### Response

Please input command /DETACH-DEVICE for not used devices to avoid not
unique VSNs.

## NDE1108

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1108 DEVICE (&00)(&10)(&09)(&11) NO REMOTE COPY SOURCE-UNIT, '(&04)' WITH SELECT=*TARGET-UNIT NOT POSSIBLE

### Meaning

(&04) was called with SELECT=*TARGET-UNIT. The device (&00) specified by
the UNIT operand is no remote copy source unit; there is no corresponding
target unit existing. The command is rejected.

## NDE1109

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1109 REMOTE-COPY TARGET-UNIT CORRESPONDING TO DEVICE (&00)(&10)(&09)(&11) UNKNOWN, '(&04)' WITH SELECT=*TARGET-UNIT NOT POSSIBLE

### Meaning

(&04) was called with SELECT=*TARGET-UNIT. For the device (&00) specified
by the operand UNIT no remote copy Target-Unit can be found due to
unavailable direct or remote access to the storage system.
The command is rejected.

### Response

- Provide direct access attaching (/ATTACH-DEVICE) a device or the
corresponding remote copy Target-Unit or
- Provide remote access enabling the remote link directors.

## NDE1110

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1110 TARGET-UNIT OF DEVICE (&00)(&10)(&09)(&11) IS NOT SYNCHRONIZED, '(&04)' WITH SELECT=*TARGET-UNIT REJECTED

### Meaning

(&04) was called with SELECT=*TARGET-UNIT. The device (&00) specified by
the UNIT operand and its remote copy Target-Unit are not synchronized, not
in synchronous remote copy mode or not in remote copy state '*IN-HOLD'.
The command is rejected.

### Response

a) set the remote copy mode to SYNCHRONOUS or
b) resume the remote copy function and wait for the synchronization to
complete or
c) suspend the remote copy function.

## NDE1111

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1111 VOLUME '(&02)' ALLOCATED BY DRV, 'HOLD-IO=*UNTIL-SPLIT' NOT POSSIBLE

### Meaning

DRV = Dual Recording by Volume.
Even in Mode DRV-MONO commands with option HOLD-IO=
*UNTIL-... are not possible.

### Response

1. export pubset
2. Stop DRV mode with /SET-DRV-PARAMETER ..,RECORDING-MODE=SRV
3. import pubset

## NDE1112

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1112 DEVICE '(&00)' IN PHASE MOUNTING

### Meaning

rename currently not possible,
check for pending mount message for the device

## NDE1113

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1113 DEVICE '(&00)' NOT-READY

## NDE1119

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1119 NO TARGET-UNIT(S) CORRESPONDING TO (&07) (&00)(&01)(&02)(&03)(&10)(&09)(&11) FOUND

### Meaning

No remote copy TARGET-UNIT could be determined for the device(s) specified
by the operand UNIT.
Possible reasons:
- the specified device(s) is (are) no remote copy SOURCE-UNIT(s).
- the remote copy TARGET-UNIT(s) is (are) unknown in the local host.
Values for insert 7:
UNIT, if Insert 0 is specified.
CONTROLLER, if Insert 1 is specified.
VOLUME, if Insert 2 is specified.
PUBSET, if Insert 3 is specified.

## NDE1120

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1120 ERROR SUSPENDING OR RESUMING IO ACCESS TO PUBSET (&03) FOR COMMAND (&04)

### Meaning

Error during the execution of command (&04) with option HOLD-IO.
Resuming of IO access failed as the IO access was already resumed
by timeout monitoring before the mirror action was finished.
The mirror action runtime was too long.
The command ends with error because the data on the mirrors
may not be consistent.

### Response

In any case, you have to synchronize the mirror pairs again using
the appropriate RESUME, RESTART or RESTORE command.

## NDE1125

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1125 STORAGE SYSTEM INFORMATION IN INITIALIZATION

### Meaning

Initial update of informations about storage system configuration
is not yet completed.

### Response

Wait and retry.

## NDE1126

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1126 DEVICE UNKNOWN OR STORAGE SYSTEM NOT SUPPORTED

### Meaning

Device is on a storage system-(type), that is not supported by SHC-OSD.

### Response

Check device list or command or unit-specification.

## NDE1127

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1127 DEVICE ON STORAGE SYSTEM NOT ACCESSIBLE BY SHC-OSD

### Meaning

SHC-OSD does not know the storage system due to no available
CIMOM-Server.

### Response

For Storage system check if StorMan and management instance are running
and have proper communication. Check definitions using
/SHOW-SHC-ENVIRONMENT.

## NDE1133

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1133 WAITING OF '(&04)' FOR DEVICES TO COMPLETE SYNCHRONIZATION ABORTED

## NDE1135

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1135 CHECK-DISK FAILED FOR DEVICE '(&00)'

### Meaning

A Check-Disk call by SHC-OSD in order to detect volume events like
mount, dismount or identity change was not successful.

### Response

Enter command:
/CHECK-DISK <device-MN>,ACTION=*REPORT
and check for related console messages.

## NDE1139

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1139 VOLUME '(&02)' MULTIPLE MOUNTED ON UNITS (&07)

### Meaning

Different devices may have the same VSN due to mirroring.
These devices are mounted by Device-Management if accessible, causing a
not unique characterisation of volumes in SHC-OSD commands.

### Response

Options to achieve a unique relation between VSN and mnemonic:
1. Detach not used (not concerned) devices.
2. Create different VSNs by renaming volumes using PVSREN.
3. Specify device mnemonics in SHC-OSD commands.

## NDE1140

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1140 DUPLICATE MN IN MN-LIST

## NDE1141

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1141 DEVICES ON DIFFERENT STORAGE SYSTEMS

### Meaning

Devices of different storage systems are mixed in a device list or
pubset specification. This kind of specification is not allowed.

### Response

Check device list.

## NDE1142

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE1142 MIRROR PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13) ALREADY EXISTS

### Meaning

Creation of a new mirror pair, which already exists is rejected.

### Response

Check input specification

## NDE1143

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE1143 ERROR OCCURRED DURING PROCESSING OF MIRROR PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13)

## NDE1144

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1144 MN'S OR DEVICE NUMBERS OF THE UNIT AND OF THE TARGET UNIT IDENTICAL: (&00)(&10)(&09)(&11)

### Response

Please check the concerned units with /SHOW-STORAGE-DEVICE-CONFIG.

## NDE1145

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1145 UNIT (&00)(&10)(&09)(&11) AND TARGET UNIT (&06)(&12)(&14)(&13) ON SAME STORAGE SYSTEM

## NDE1146

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1146 UNIT (&00)(&10)(&09)(&11) AND TARGET-UNIT (&06)(&12)(&14)(&13) OF DIFFERENT (META) TYPE OR DIFFERENT SIZE

### Meaning

Only units of same meta type and size are allowed for remote copy pairs.
TARGET-UNIT: second device of a remote copy pair.

### Response

Please check the units concerned with /SHOW-STORAGE-DEVICE-CONFIG.

## NDE1148

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1148 DIFFERENT NUMBER OF DEVICES FOR UNIT AND TARGET-UNIT

### Meaning

The operands UNIT and/or TARGET-UNIT are specifying devices by MN-list.
In this case the number of Source Units has to match exactly the number
of the Target Units specified.
TARGET-UNIT: second device of a remote copy pair.

### Response

Correct and retry.

## NDE1165

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1165 SWAP-REMOTE-COPY FOR (&07) (&00)(&01)(&02)(&03)(&10)(&09)(&11) WITH 'RESUME-PARAMETER=*RESTORE-TO-SOURCE' NOT POSSIBLE IN SECURE MODE

## NDE1170

Destination: USER-TASK Routing code: Weight:

Warranty : YES

NDE1170 UNIT (&00)(&10)(&09)(&11) IS A SOURCE-UNIT WITH CONCURRENT TARGET-UNITS

## NDE1171

Destination: USER-TASK Routing code: Weight:

Warranty : YES

NDE1171 TARGET-UNIT OF UNIT (&00)(&10)(&09)(&11) IS NOT UNIQUE

### Meaning

UNIT has Concurrent Target-Units.

## NDE1173

Destination: USER-TASK Routing code: Weight:

Warranty : YES

NDE1173 SOURCE UNIT (&00)(&10)(&09)(&11) HAS CONCURRENT TARGET UNIT IN STATE ACTIVE

## NDE1177

Destination: USER-TASK Routing code: Weight:

Warranty : YES

NDE1177 UNIT (&00)(&10)(&09)(&11) IS A SOURCE UNIT

## NDE1178

Destination: USER-TASK Routing code: Weight:

Warranty : YES

NDE1178 UNIT (&00)(&10)(&09)(&11) IS A TARGET UNIT

## NDE1179

Destination: USER-TASK Routing code: Weight:

Warranty : YES

NDE1179 UNIT (&00)(&10)(&09)(&11) IS A CASCADED TARGET UNIT

## NDE1184

Destination: USER-TASK Routing code: Weight:

Warranty : YES

NDE1184 UNIT (&00)(&10)(&09)(&11) IS A (&07)

## NDE1193

Destination: USER-TASK Routing code: Weight:

Warranty : YES

NDE1193 COMMAND NOT ALLOWED WHEN TARGET UNIT LARGER THAN SOURCE UNIT

## NDE1199

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1199 COMMAND NOT ALLOWED IN THE CURRENT REMOTE COPY STATE OR MODE

### Meaning

At least one of the devices affected by the command is a remote copy
mirror (too) in a state or mode, which is in conflict to the command.

### Response

Please check remote copy state and accessibility using /SHOW-REMOTE-COPY.

## NDE1200

Destination: CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE1200 SHC-OSD TASK INITIALISATION ERROR. REASON: '(&07)'

## NDE1201

Destination: CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE1201 SHC-OSD TASK READY. SHC-OSD VERSION '(&07)'/'(&08)'

## NDE1202

Destination: CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE1202 SHC-OSD TASK ABNORMAL TERMINATION

### Meaning

A SHC-OSD task was terminated abnormally. A user dump may be created
for diagnostic purposes.

## NDE1203

Destination: CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE1203 SHC-OSD TASK INITIALIZATION WARNING: /ASSIGN-SYSOUT TO FILE FAILED, SHC-OSD INITIALISATION CONTINUED

### Meaning

File $TSOS.SYSOUT.SHC-OSD.USERTASK cannot be opened.

### Response

Remove the blocking state by using /REMOVE-FILE-ALLOC-LOCKS or
/DELETE-FILE.

## NDE1204

Destination: CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE1204 SYSOUT-PROTOCOL-FILE: SYSOUT.SHC-OSD.USERTASK IS LOCKED, SUBSYSTEM SHC-OSD IS ALREADY RUNNING. TASK WILL BE TERMINATED

### Meaning

The SHC-OSD subsystem and its user task are already running.

## NDE1205

Destination: CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE1205 SHC-OSD INSTALLATION FAILED, PLEASE INSTALL POSIX-SH AND RETRY

### Meaning

POSIX-SH package needs to be installed.

## NDE1206

Destination: CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE1206 NO SHC-OSD LOGGING DUE TO MISSING DIRECTORY IN POSIX FILE SYSTEM

### Meaning

SHC-OSD directory var/shcosd/log needs to be created in POSIX.

## NDE1207

Destination: CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE1207 NO SHC-OSD LOGGING DUE TO NO FREE SPACE AVAILABLE IN POSIX FILE SYSTEM

### Meaning

SHC-OSD directory var/shcosd/log in POSIX is full.

## NDE1208

Destination: CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE1208 NO SHC-OSD LOGGING DUE TO '(&07)' ERROR '(&08)'

### Meaning

Open or write of SHC-OSD logging file in POSIX failed.

## NDE1210

Destination: CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE1210 DMS-ERROR '(&07)' DURING PROCESSING OF FILE '(&08)'

### Meaning

DMS-Error during processing of the configuration file.

## NDE1410

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1410 NO OR TOO FEW FREE AND MATCHING SNAP UNITS

### Meaning

Unit and SNAP-Unit have to match in device-type, size, meta-properties
and stripe-size to form a snap-pair.

### Response

Make further devices with appropriate properties available.

## NDE1413

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1413 REQUESTED SAVE-POOL IS FULL

### Meaning

The current Snap operation can not be completed because the related
save-pool is in saturation.

### Response

For an overview over all save-pools enter:
/SHOW-STORAGE-CONFIGURATION UNIT=*ALL,INF=*SAVE-POOLS
Then a) select a less saturated save-pool with matching device type
or b) terminate snap pairs of same device type and storage
system using /STOP-SNAP-SESSION

## NDE1430

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1430 NO SNAP FUNCTION FOR DEVICE (&00)(&10)(&09)(&11)

### Meaning

The specified device is no SNAP device

### Response

Check the device mentioned above with /SHOW-STORAGE-DEVICE-CONFIG.

## NDE1431

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1431 DIFFERENT NUMBER OF DEVICES FOR UNIT AND SNAP-UNIT

### Meaning

A list of SNAP-Units with more than one element is accepted, only if
the operand UNIT is specified via PUBSET.
In this case the number of Original-Units of the Pubset has to match
exactly the number of SNAP-Units.

## NDE1434

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1434 SNAP-UNIT (&06)(&12)(&14)(&13) USED IN OTHER SNAP PAIR

## NDE1435

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1435 UNIT (&00)(&10)(&09)(&11) IS A VIRTUAL DEVICE OR A SNAP-UNIT

## NDE1437

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1437 MN'S OR DEVICE NUMBERS OF THE UNIT AND OF THE SNAP-UNIT IDENTICAL: (&00)(&10)(&09)(&11)

### Response

Please check the concerned units with /SHOW-STORAGE-DEVICE-CONFIG.

## NDE1438

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1438 UNIT (&00)(&10)(&09)(&11) AND SNAP-UNIT (&06)(&12)(&14)(&13) OF DIFFERENT (META) TYPE OR DIFFERENT SIZE

### Meaning

Only units of same size and meta type are allowed for SNAP pairs.

### Response

Please check the units concerned with /SHOW-STORAGE-DEVICE-CONFIG.

## NDE1440

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1440 STATE OF UNIT (&00)(&10)(&09)(&11) WRONG: '(&07)'

### Meaning

Possible reason for this message:
The unit has more than one SNAP-UNIT paired with.
At least one snap unit is in wrong state indicated in insert 7:
- RESTORE-FROM-SNAP ordered, while another SNAP-UNIT is 'CREATED'.
- START-SNAP-SESSION ordered, while another SNAP-UNIT is 'RESTORED'.
The unit has at least one CLONE-UNIT paired with, which is in wrong state.

### Response

Check all states of SNAP pairs using /SHOW-SNAP-SESSION-STATUS <unit>
and change wrong SNAP-states.
Check state(s) of CLONE pair(s) using /SHOW-CLONE-SESSION-STATUS <unit>
and change wrong CLONE-state(s).

## NDE1441

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1441 STATE OF SNAP-UNIT (&06)(&12)(&14)(&13) WRONG: '(&07)'

### Meaning

Possible reason for this message:
For a given command snap unit is in wrong state as indicated in insert 7:
- START-SNAP-SESSION ordered, but SNAP-UNIT is not 'UNUSED'.
- ACTIVATE-SNAP ordered, but SNAP-UNIT is not 'CREATED'.
- RESTORE-FROM-SNAP ordered, but SNAP-UNIT is not 'COPY-ON-WRITE'.

### Response

Check state of SNAP pair using /SHOW-SNAP-SESSION-STATUS <unit>
and change wrong SNAP-state.

## NDE1442

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1442 UNIT (&00)(&10)(&09)(&11) IS A TARGET-UNIT AND RESTORE-FROM-SNAP

### Meaning

RESTORE-FROM-SNAP is not supported, if the original device is
also used as TARGET-UNIT of a remote copy pair
and not in REMOTE-COPY state 'READY'.
TARGET-UNIT: second device of a remote copy pair.

### Response

Check the REMOTE-COPY state(s) of the original remote copy pair
using /SHOW-REMOTE-COPY.

## NDE1443

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1443 UNIT (&00)(&10)(&09)(&11) IS A ORIGINAL-UNIT OF A SNAP PAIR

## NDE1449

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1449 NO MATCHING OR NO UNIQUE SNAP-UNIT ASSIGNED TO (&00)(&10)(&09)(&11) AND 'SNAP-UNIT=(&07)' SPECIFIED

## NDE1453

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1453 UNIT (&00)(&10)(&09)(&11) IS NO SNAP-UNIT

## NDE1454

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1454 UNIT (&00)(&10)(&09)(&11) IS UNUSED SNAP-UNIT

## NDE1460

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1460 VOLUME (&02) RESERVED FOR SNAP UNITS

### Meaning

Volumes with this special notation are reserved for usage as SNAP units.
Thus marked "unused", these devices could be chosen as SNAP units,
if *AUTO-SELECT is specified.

### Response

For any other usage of these devices the VSN has to be changed.
Creation of pubset(s) out of these devices will do so.

## NDE1470

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1470 MIXED SNAP-UNIT TYPES FOR UNIT (&00)

### Meaning

Creation of SnapOPC+ SNAP sessions allows the assignment of multiple
SNAP-UNITs for a single volume. The creation is rejected, if the new
SNAP-UNITs are not of the same volume type (SDVs or none SDVs).

### Response

Check the RAID Information of the volumes with /SHOW-STORAGE-DEVICE-CONFIG

## NDE1484

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1484 SNAP PAIR (&00)(&10)(&09)(&11),(&06)(&12)(&14)(&13) ALREADY ACTIVATED, COMMAND NOT PROCESSED

### Response

Please check the concerned units with /SHOW-SNAP-SESSION-STATUS.

## NDE1492

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1492 SNAP PAIR (&00)(&10)(&09)(&11),(&06)(&12)(&14)(&13) ALREADY ACTIVATED, SNAP-UNIT ALREADY RENAMED TO '(&02)'

### Meaning

At /ACTIVATE-SNAP a new catid for the SNAP-Units was requested. However
(at least) for this unit, the command has been issued before with a
different catid.

### Response

Please check the concerned units with /SHOW-SNAP-SESSION-STATUS.

## NDE1496

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1496 SNAP PAIR(S) ALREADY ACTIVATED, COMMAND NOT PROCESSED

### Response

Please check stati with /SHOW-SNAP-SESSION-STATUS.

## NDE1511

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1511 CLONE-PAIR IS ALREADY CASCADED

### Meaning

Cascaded clone pairs are built when a clone-unit is simultanously used as
original-unit for another clone pair.

## NDE1530

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1530 NO CLONE OR WRONG CLONE-TYPE FOR UNIT (&00)(&10)(&09)(&11)

### Response

Please check the concerned unit with /SHOW-STORAGE-DEVICE-CONFIG
if a Clone-session exists or if the Clone-type is supported.

## NDE1531

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1531 DIFFERENT NUMBER OF DEVICES FOR UNIT AND CLONE-UNIT

### Meaning

A list of CLONE-Units with more than one element is accepted, only if
the operand UNIT is specified via PUBSET.
In this case the number of Original-Units of the Pubset has to match the
number of CLONE-Units exactly.

### Response

Correct and retry.

## NDE1534

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1534 CLONE-UNIT (&06)(&12)(&14)(&13) USED IN OTHER SNAP OR CLONE PAIR

## NDE1535

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1535 UNIT (&00)(&10)(&09)(&11) IS A CLONE UNIT

### Meaning

Command cannot be executed because unit is a CLONE unit or a CLONE
pair with COPY-COMPLETE-DATA=*NO attribute in case of remote-copy
commands.

### Response

Get more information using the command
/SHOW-CLONE-SESSION-STATUS ... .

## NDE1537

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1537 MN'S OR DEVICE NUMBERS OF THE UNIT AND OF THE CLONE-UNIT IDENTICAL: (&00)(&10)(&09)(&11)

## NDE1538

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1538 UNIT (&00)(&10)(&09)(&11) AND CLONE-UNIT (&06)(&12)(&14)(&13) OF DIFFERENT (META) TYPE OR DIFFERENT SIZE

### Meaning

Only units of same meta type and size are allowed for CLONE pairs.

### Response

Please check the units concerned with /SHOW-STORAGE-DEVICE-CONFIG.

## NDE1540

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1540 STATE OF UNIT (&00)(&10)(&09)(&11) WRONG: '(&07)'

### Meaning

Possible reason for this message:
a) 'RESTORE-FROM-CLONE' only allowed, if all CLONE-UNITs in state:
- Copied
b) 'RESTART-CLONE-SESS' only allowed, for CLONE-UNIT(s) in state:
- Copied
and no other CLONE-UNIT in state:
- Restored
c) SNAP pair(s) exists with same original unit, the SNAP unit(s) being
in wrong state

### Response

Check the CLONE pair(s) state(s) using /SHOW-CLONE-SESSION-STATUS.
Check the SNAP pair(s) state(s) using /SHOW-SNAP-SESSION-STATUS.

## NDE1541

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1541 STATE OF CLONE-UNIT (&06)(&12)(&14)(&13) WRONG: '(&07)'

### Meaning

/RESTORE-FROM-CLONE only processed for CLONE pairs in status:
- SPLIT (ETERNUS DX)
/RESTART-CLONE-SESSION only processed for CLONE pairs in status:
- SPLIT (ETERNUS DX)
/ACTIVATE-CLONE only processed for CLONE pairs in status:
- SYNCHRONIZED (ETERNUS DX)

### Response

Check the CLONE pair(s) state(s) using /SHOW-CLONE-SESSION-STATUS.

## NDE1542

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1542 UNIT (&00)(&10)(&09)(&11) IS A TARGET-UNIT AND RESTORE-FROM-CLONE

### Meaning

RESTORE-FROM-CLONE is not supported, if the original device is
also used as TARGET-UNIT of a remote copy pair and not in state READY.
TARGET-UNIT: second device of a remote copy pair.

### Response

Check the REMOTE-COPY state(s) of the originals using /SHOW-REMOTE-COPY.

## NDE1543

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1543 UNIT (&00)(&10)(&09)(&11) IS A ORIGINAL-UNIT OF A CLONE PAIR

### Meaning

Due to this given mirror attribute, action is rejected.

### Response

Check all mirror attributes of this device.

## NDE1548

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1548 CLONE TYPE NOT UNIQUE FOR UNIT (&00)(&10)(&09)(&11)

### Meaning

The clone type (MIRROR or COPY) needs to be specified explicitly.

### Response

Specify the operand CLONE-TYPE.

## NDE1549

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1549 NO MATCHING OR NO UNIQUE CLONE-UNIT ASSIGNED TO (&00)(&10)(&09)(&11) AND 'CLONE-UNIT=(&07)' SPECIFIED

## NDE1553

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1553 UNIT (&00)(&10)(&09)(&11) NO CLONE-UNIT

## NDE1584

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1584 CLONE PAIR (&00)(&10)(&09)(&11),(&06)(&12)(&14)(&13) ALREADY ACTIVATED, COMMAND NOT PROCESSED

### Response

Please check the concerned units with /SHOW-CLONE-SESSION-STATUS.

## NDE1592

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1592 CLONE PAIR (&00)(&10)(&09)(&11),(&06)(&12)(&14)(&13) ALREADY ACTIVATED, CLONE-UNIT ALREADY RENAMED TO (&02)

### Meaning

At /ACTIVATE-CLONE a new catid for the CLONE-Units was requested. However
(at least) for this unit, the command has been issued before with a
different catid.

### Response

Please check the concerned units with /SHOW-CLONE-SESSION-STATUS.

## NDE1596

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1596 CLONE PAIR(S) ALREADY ACTIVATED, COMMAND NOT PROCESSED

### Response

Please check stati with /SHOW-CLONE-SESSION-STATUS.

## NDE1600

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1600 NO LICENSE FOR STORAGE CLUSTER

### Meaning

Storage Cluster support requires a license.

### Response

The required license keys are registered on ETERNUS SF.

## NDE1601

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1601 STORAGE CLUSTER (&07) NOT FOUND

### Meaning

Specified Storage Cluster not found.

### Response

Inform about all Storage Clusters using
/SHOW-STORAGE-CLUSTER-CONFIG
Use capital letters to specify CLUSTER-NAME.

## NDE1602

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1602 INVALID STATUS OR PHASE OF STORAGE CLUSTER (&07)

### Meaning

Command can't be processed for the current status or phase of the
Storage Cluster.

### Response

Check the status and phase of the Storage Cluster using
/SHOW-STORAGE-CLUSTER-CONFIG.

## NDE1603

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1603 NO REMOTE CONNECTION AVAILABLE FOR STORAGE CLUSTER (&07)

### Meaning

The Storage Cluster requires an active remote connnection between
the two storage systems.

### Response

Check the status of remote connection for the Storage Cluster using
/SHOW-STORAGE-CLUSTER-CONFIG and/or
/SHOW-STORAGE-CONFIG ... INFORMATION=*PORT-STATUS

## NDE1604

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1604 FAILOVER REJECTED FOR STORAGE CLUSTER (&07): AUTOFAILBACK ENABLED

### Meaning

Autofailback is activated for this Storage Cluster, a failover would
lead to an immediate failback.

### Response

Check the settings of the Storage Cluster using
/SHOW-STORAGE-CLUSTER-CONFIG.

## NDE1605

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1605 FAILOVER WITH FORCE OPTION REJECTED FOR STORAGE CLUSTER (&07)

### Meaning

This command is not processed in this status of the Storage Cluster.
The Force Option just needs to be used in error cases only.

### Response

Try the command again without the Force Option

## NDE1606

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1606 VOLUMES IN DIFFERENT STORAGE CLUSTERS

### Meaning

Volumes of different storage clusters are mixed.

### Response

Check storage cluster assignment of specified volumes.

## NDE1607

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1607 STORAGE CLUSTER NAME (&07) NOT UNIQUE

### Meaning

Specified Storage Cluster name is not unique

### Response

Inform about all Storage Clusters using
/SHOW-STORAGE-CLUSTER-CONFIG
Use capital letters to specify CLUSTER-NAME.

## NDE1608

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1608 FAILBACK TO PRIMARY STORAGE NOT POSSIBLE FOR STORAGE CLUSTER (&07)

### Meaning

Fibrechannel connection to primary storage is not available.

### Response

Check the Fibrechannel connection from the server to the primary storage.

## NDE1609

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1609 COMMAND (&04) REJECTED FOR STORAGE CLUSTER (&07) DUE TO REMOTE-LINK=*NOT-AVAILABLE

### Meaning

FAILOVER-STORAGE IS REJECTED DUE TO 'SPLIT BRAIN':
PRIMARY AND SECONDARY STORAGE ARE BOTH AVAILABLE BUT REMOTE CONNECTION
IS NOT. PROCESSING WOULD LEAD TO DATA CORRUPTION.

## NDE1610

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1610 COMMAND '(&04)' NOT SUPPORTED FOR STORAGE CLUSTER VOLUMES

### Meaning

For Storage Cluster volumes not all combinations for additional
Clones, Snaps and Remote-Copy pairs are supported.

### Response

Check the supported combinations in SHC-OSD documentation.

## NDE1611

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1611 COMMAND REJECTED, UNIT (&00)(&10)(&09)(&11) IS STORAGE CLUSTER VOLUME

### Meaning

The chosen replication function is not supported for Storage-Cluster
volumes.

### Response

Check the supported combinations in SHC-OSD documentation.

## NDE1800

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1800 DEVICE '(&00)' NOT FOUND OR NOT IN STORAGE SYSTEM

### Meaning

Possible Reasons:
- the device is not defined in BS2000
- the device is not an emulated device of a Storage system
- the Storage system is not accessible

## NDE1802

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1802 COMMUNICATION ERROR TO STORMAN SERVER

### Meaning

A communication error to the StorMan server has occured.
Possible reasons:
- The specified values to define the StorMan connection are wrong.
(Default Host- and Port-Names are specified in SYSPAR.SHC-OSD.<ver>)

### Response

- Check definitions using /SHOW-SHC-ENVIRONMENT.

## NDE1803

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1803 Management instance NOT AVAILABLE

### Meaning

Possible reasons:
- Management instance not started or not available.
- Error in definition of the Management instance.

### Response

- Check definitions using /SHOW-SHC-ENVIRONMENT.
- Check availability of SMI-S Provider.

## NDE1804

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1804 NO AUTHORIZATION INFORMATION FOR STORAGE SYSTEM AVAILABLE

### Meaning

The authorization information for the Storage System is not contained
in StorMan repository.

## NDE1805

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1805 AUTHORIZATION INFORMATION FOR STORAGE SYSTEM INVALID

### Meaning

The authorization information for the Storage System in StorMan
repository is not valid.

## NDE1806

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1806 STORMAN REMOTE X2000 CALL FAILED

### Meaning

A StorMan call to X2000 was terminated with errors.

### Response

Please provide StorMan logging files and contact your local support
center.

## NDE1807

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1807 NO STORAGE SYSTEM FOUND

### Meaning

No storage system could be discoverd by SHC-OSD.
Possible reasons:
- No storage system is connected or defined for this host.
- The installation prerequisites for the subsystem SHC-OSD are not
completely met.

## NDE1809

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1809 STORMAN ACTION SUCCESSFUL WITHOUT STATUS UPDATE

### Meaning

StorMan action successful finished, but StorMan could not update status.

### Response

Possible responses:
- Waiting: Automatic update by system within the next 10 minutes.
- Active: Start status update by
/SHOW-STORAGE-CONFIG ...,UPDATE=*DISCOVER or
/SHOW-STORAGE-DEVICE-CONFIG ....,UPDATE=*DISCOVER

## NDE1810

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1810 OPERATING SYSTEM VERSION OF STORAGE SYSTEM IS NOT SUPPORTED

### Meaning

The current version of SHC-OSD does not support operating system version
or firmware version of the storage system.

## NDE1811

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1811 FUNCTION NOT SUPPORTED FOR STORAGE SYSTEMS

### Meaning

The current version of StorMan and/or SHC-OSD does not support the
function for the selected storage system.

### Response

Further details are described in the manual.

## NDE1812

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1812 STORMAN SERVER DISABLED BY COMMAND

### Meaning

The connection to all StorMan servers has been disabled in order to run
SHC-OSD without StorMan.

### Response

Enable StorMan connection: /MODIFY-SHC-ENVIRONMENT CONNECTED-STORMAN=
*PARAMETERS(HOST-NAME= ... or *FIRST-AVAILABLE)

## NDE1813

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1813 STORMAN SERVER DISABLED BY DISCOVER-MODE SETTING

## NDE1814

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1814 STORAGE SYSTEM WITH SERIALNUMBER '(&10)' NOT FOUND

### Meaning

There is currently no storage system found with the specified
serial number.

## NDE1815

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1815 SERIAL NUMBER '(&10)' OF STORAGE SYSTEM NOT UNIQUE

### Meaning

The specified serial number is not unique.

## NDE1816

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1816 LOGICAL VOLUME '(&11)' NOT FOUND IN STORAGE SYSTEM '(&10)'

### Meaning

The specified logical volume is not contained in the storage system.

## NDE1817

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1817 MIRROR INFORMATION OF STORAGE SYSTEM NOT AVAILABLE

### Meaning

The Storage system has currently no information available about
local- and remote mirrors, due to a missing fibre channel connection
between StorMan server and storage system.

## NDE1818

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1818 UNIT (&00)(&10)(&09)(&11) HAS NO STORID IN STORMAN DATABASE

### Response

Insert StorId using StorMan commands.

## NDE1819

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1819 COMMAND '(&04)' WITH OPERAND 'UNIT=*BY-CONTROLLER' NOT SUPPORTED

### Meaning

The specified Storage system supports no specification by controller MN
and the command is rejected.

## NDE1820

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1820 COMMAND REJECTED DUE TO STATUS OF SNAP PAIR, WAIT AND RETRY

### Meaning

The creation or termination of the SNAP-PAIR is rejected due to an
uncompleted internal restore process by command /RESTORE-FROM-SNAP,
not reflected by the STATE of the SNAP-PAIR.

### Response

Please wait and retry the command after the restore process is completed.

## NDE1822

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1822 RESTORE SUB STEP RESTART FAILED

### Meaning

The sub-step RESTART of the RESTORE command has failed.

### Response

Please wait and retry the command step by step using RESTART, ACTIVATE
and SWAP-Commands after checking the current state.

## NDE1823

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1823 RESTORE SUB-STEP SUSPEND(ACTIVATE) FAILED

### Meaning

The sub-step SUSPEND of the RESTORE command has failed.

### Response

Please wait and retry the command step by step using ACTIVATE-
and SWAP-Commands after checking the current state.

## NDE1824

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1824 RESTORE SUB STEP SECOND SWAP FAILED

### Meaning

The sub-step "SECOND SWAP" of the RESTORE command has failed.

### Response

Please wait and retry the last command sub-step "SECOND SWAP" after
checking the state.

## NDE1825

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1825 NO STORAGE MANAGEMENT ACCESS TO UNIT (&00)(&10)(&09)(&11)

## NDE1826

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1826 NO STORAGE MANAGEMENT ACCESS TO REPLICATION-UNIT (&06)(&12)(&14)(&13)

## NDE1830

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1830 STORMAN SERVER (&07) NOT FOUND

### Meaning

A StorMan server with the given host name was not found.

### Response

Check host name in command and STORMAN-HOST lines in file
SYSPAR.SHC-OSD.<vers>. Please note that input is case sensitive.

## NDE1831

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1831 STORMAN SERVER (&07) NOT CONNECTABLE

### Meaning

A StorMan server with the given name is not available.

### Response

Check StorMan status for the specified StorMan server with
/SHOW-SHC-PROCESSING.
Start StorMan on server.

## NDE1832

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1832 STORMAN SERVER (&07) ALREADY CONNECTED

### Meaning

A StorMan server with the given name is already connected.

### Response

Check name in command. /SHOW-SHC-PROCESSING shows the CONNECTED
settings to each StorMan server.

## NDE1833

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1833 NO SUITABLE STORMAN SERVER FOUND

### Meaning

There is no connectable StorMan server listed in SYSPAR.SHC-OSD.<vers>.

### Response

Check StorMan status for all specified StorMan server with
/SHOW-SHC-PROCESSING.
Start StorMan on server.

## NDE1834

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : NO

NDE1834 STORMAN SERVER (&07) FAILED WITH ERROR '(&08)'

### Meaning

The StorMan server with the given name was not able to set
the requested StorMan parameter.

## NDE1835

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : NO

NDE1835 SHC-OSD CONNECTED TO STORMAN SERVER (&07)

### Meaning

The StorMan server with the given name is now used by SHC-OSD.

## NDE1836

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : NO

NDE1836 SHC-OSD DISCONNECTED FROM STORMAN SERVER (&07)

### Meaning

The StorMan server with the given name is no longer used by SHC-OSD.

## NDE1837

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1837 WAITING FOR UPDATED STORMAN DATA

## NDE1838

Destination: USER-TASK, CONSOLE Routing code: D Weight: 70

Warranty : NO

NDE1838 WARNING: MIRRORING DATA MAY NOT BE UP-TO-DATE UNTIL NEXT STORMAN UPDATER FINISHED

## NDE1839

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1839 UNIT (&00)(&10)(&09)(&11) AND CLONE-UNIT (&06)(&12)(&14)(&13) ON DIFFERENT STORAGE SYSTEMS

### Meaning

The devices of the chosen clone pair are not in the same
storage system.

### Response

Clone pairs have to reside on the same storage system.

## NDE1840

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1840 UNIT (&00)(&10)(&09)(&11) AND SNAP-UNIT (&06)(&12)(&14)(&13) ON DIFFERENT STORAGE SYSTEMS

### Meaning

The devices of the chosen Snap pair are not in the same storage system.

### Response

Snap pairs have to reside on the same storage system.

## NDE1841

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1841 NO REMOTE LINK CONNECTION CONFIGURED BETWEEN STORAGE SYSTEMS

### Response

Please configure the remote link connection between the systems.

## NDE1842

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1842 ERROR IN REC BUFFER CONFIGURATION

### Meaning

Error during processing of Remote-Copy pairs of ETERNUS DX storage
systems.
Possible reasons:
REC buffer not configured
REC buffer wrong configured
REC buffer, source volume and target volume do not correspond
REC buffer is in state not active

## NDE1850

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1850 ALL SNAP MIRROR OF DEVICE (&00)(&10)(&09)(&11) RESERVED FOR SNAPSETS

### Meaning

The current SNAP pairs to the given device are reserved for SNAPSET use.
The creation of normal SNAP pairs is rejected for this device.

## NDE1852

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1852 TOO MANY LOCAL MIRRORS ASSOCIATED TO DEVICE (&00)(&10)(&09)(&11), MAXIMUM NUMBER EXCEEDED

### Meaning

Local mirror refers to SNAP- or CLONE-Mirror in a storage system.
If the specific limit is reached, further /START-SNAP-SESSION resp.
/START-CLONE-SESSION commands are rejected.

### Response

Delete old assignments using /STOP-SNAP-SESSION or /STOP-CLONE-SESSION.

## NDE1853

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1853 STORAGE DEVICE(S) LOCKED

### Meaning

Storage device(s) locked, as another action is running on this device(s).

### Response

Wait and retry action.

## NDE1854

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1854 CLONE-PAIR(S) POSSIBLY INCONSISTENT

### Meaning

Possible reason: device(s) is(are) an active asynchronous
remote copy target.

### Response

Hold the Remote copy session with command /HOLD-REMOTE-COPY.

## NDE1860

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1860 REMOTE COPY PAIR (&00)(&10)(&09)(&11),(&06)(&12)(&14)(&13) NOT IN STATE *ACTIVE

### Meaning

/HOLD-REMOTE-COPY is not supported, if the state of
the REMOTE COPY pair is not ACTIVE.

### Response

Enter /RESUME-REMOTE-COPY command to change to ACTIVE state.

## NDE1861

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1861 REMOTE COPY PAIR (&00)(&10)(&09)(&11),(&06)(&12)(&14)(&13) NOT IN STATE '*IN-HOLD'

### Meaning

RESUME- and SWAP-REMOTE-COPY are not supported, if the state of
the remote copy pair is not '*IN-HOLD'.

### Response

Issue HOLD-REMOTE-COPY command to reach '*IN-HOLD' state.

## NDE1862

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1862 REMOTE COPY PAIR (&00)(&10)(&09)(&11),(&06)(&12)(&14)(&13) ALREADY IN STATE *IN-HOLD, COMMAND NOT PROCESSED.

### Meaning

A /HOLD-REMOTE-COPY command for the specified REMOTE COPY pair has been
rejected, as this pair has already reached the state IN-HOLD.

### Response

Check the REMOTE COPY pair using /SHOW-REMOTE-COPY-STATUS.

## NDE1863

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1863 REMOTE COPY PAIR (&00)(&10)(&09)(&11),(&06)(&12)(&14)(&13) ALREADY IN STATE *IN-HOLD, TARGET UNIT ALREADY RENAMED TO (&02).

### Meaning

/HOLD-REMOTE-COPY requested a new catalog id for the Target-Units.
However (at least) for this unit, the command has been issued before
with a different catid.

### Response

Check catalog id of the Target-Units using /SHOW-STORAGE-DEVICE-CONFIG.

## NDE1866

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1866 NO REMOTE-LINK AVAILABLE BETWEEN SOURCE AND TARGET STORAGE SYSTEM

### Response

Please check the connection between the two systems.

## NDE1867

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1867 RANGE OF CASCADED REPLICATION EXCEEDED

## NDE1870

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1870 SNAP PAIR FOR UNIT (&00)(&10)(&09)(&11) CREATED

## NDE1872

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1872 AUTOMATIC ATTACH OF SNAP UNIT(S) FAILED

### Meaning

/ATTACH-DEVICE processing has not finished within SHC-OSD waiting time
and has probably failed. /ATTACH-DEVICE in BS2000 requires a successful
VM2000 assignment (/ADD-VM-DEVICE).

### Response

If message occurs at START-SNAP-SESSION command, check SNAP(s) and VM2000
settings for assignment. Try direct VM-Assignment (/ADD-VM-DEVICE) and
direct /ATTACH-DEVICE.
Otherwise, the reason for the failed /ATTACH-DEVICE order can possibly
be found in the CONSLOG.

## NDE1879

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE1879 SNAP PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13) RESTORED

### Meaning

/RESTORE-FROM-SNAP command was successfully processed.

## NDE1880

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1880 NO COPY LICENSE ON ETERNUS DX STORAGE SYSTEM

### Meaning

The copy license on the ETERNUS DX storage system to manage local and/or
remote replication is missing.

### Response

Activation of the COPY LICENSE for local and/or remote replication on
the ETERNUS DX storage system.

## NDE1881

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1881 COPY TABLE SIZE NOT SETUP ON ETERNUS DX STORAGE SYSTEM

### Meaning

The COPY TABLE SIZE on the ETERNUS DX Storage System is not configured.
No local or remote replication pairs can be created.

### Response

Configure the COPY TABLE SIZE on the ETERNUS DX Storage System.

## NDE1882

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1882 COPY TABLE SIZE TOO SMALL ON ETERNUS DX STORAGE SYSTEM

### Meaning

The configured COPY TABLE SIZE on the ETERNUS DX Storage System
is too small.

### Response

Increase the COPY TABLE SIZE on the ETERNUS DX Storage System.

## NDE1883

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1883 VOLUME(S) FORBIDDEN FOR ADVANCED COPY OPERATIONS

### Meaning

Flag 'forbid advanced copy' is set in ETERNUS DX for one or more
logical volume(s).

### Response

Reset this flag by ETERNUS DX WebUI or CLI for full SHC-OSD
functionality.

## NDE1886

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE1886 CLONE PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13) SWAPPED

### Meaning

As part of a /SWAP-CLONE-SESSION command Original- and Clone-Unit of the
clone pair were swapped.

## NDE1887

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE1887 CLONE PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13) RESTARTED

### Meaning

As part of a /RESTORE-FROM-CLONE command the clone pair was restarted.

## NDE1888

Destination: USER-TASK, CONSOLE Routing code: D Weight: 66

Warranty : NO

NDE1888 CLONE PAIR (&00)(&10)(&09)(&11), (&06)(&12)(&14)(&13) ACTIVATED

### Meaning

As part of a /ACTIVATE-CLONE command the Clone-Unit was activated.

## NDE1890

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1890 MANAGEMENT INSTANCE (&07) NOT FOUND ON STORMAN SERVER (&08)

## NDE1892

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1892 SMI-S PROVIDER (CIMOM-SERVER) ADDED TO STORMAN SERVER (&08) BUT NOT RUNNING OR NOT FOUND

### Meaning

StorMan could not establish a connection to the added CIMOM server
(SMI-S Provider).
Possible reasons:
- Error in definition of the CIMOM server (name / IP address not found).
- CIMOM server not started or not reachable.

### Response

- Check definitions using /SHOW-SHC-ENVIRONMENT.
- Check network connection and availability of CIMOM server.

## NDE1893

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1893 SOURCE-UNITS ON DIFFERENT STORAGE SYSTEMS

### Meaning

When working with PUBSETs it is assumed, that all SOURCE-UNITs of the
specified pubset are located in the same Storage System.

### Response

Please check the remote mirror properties of all mirror pairs of the
PUBSET and adjust (if possible) by using /SWAP-REMOTE-COPY.

## NDE1897

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1897 COMMAND NOT ALLOWED WITHOUT FORCE=*YES IN THE CURRENT STATE OR COPY-MODE

### Meaning

At least one specified pair has a state or COPY-MODE that requires
option FORCE=*YES for processing the command.

### Response

Repeat the command with option FORCE=*YES.

## NDE1898

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1898 CONCURRENT TARGET-UNITS ON SAME STORAGE SYSTEM NOT SUPPORTED FOR REMOTE COPY PAIR (&00)(&10)(&09)(&11),(&06)(&12)(&14)(&13)

### Meaning

SHC-OSD does not support concurrent target units residing on the same
storage system.

### Response

Select different storage systems for remote mirror pairs.

## NDE1899

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE1899 COMMAND NOT ALLOWED IN THE CURRENT MIRRORING STATE OR MODE

### Meaning

At least one specified mirror pair is in a state or mode that does not
allow the processing of the command.

### Response

Please check the state, mode and accessibility of the mirror pairs.
Some commands offer an "FORCE" operand which forces the action without
conserving dataconsistency.

## NDE1999

Destination: USER-TASK Routing code: Weight: 70

Warranty : NO

NDE1999 (&07)(&08)

### Meaning

Information note.

## NDE2000

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE2000 COMMAND '(&04)' PROCESSED WITH PARTIAL SUCCESS

### Meaning

Final message of a SHC-OSD command for which not all parts have been
successfully processed.

## NDE2001

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE2001 COMMAND '(&04)' COMPLETED UNSUCCESSFULLY

### Meaning

Final message of a SHC-OSD command which has not been
successfully processed.

## NDE2002

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE2002 INTERNAL ERROR IN COMMAND '(&04)'

### Meaning

Final message of a SHC-OSD command which could not be processed
successfully due to an internal error.

## NDE2003

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE2003 COMMAND '(&04)' SUCCESSFUL, NO ACTION NECESSARY

### Meaning

Final message of a SHC-OSD command for which no processing was necessary.

## NDE2004

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE2004 COMMAND '(&04)' SUCCESSFUL, PROCESSING NOT YET COMPLETED

### Meaning

Final message of a SHC-OSD command that has been started successfully,
but the processing is not finished yet.

## NDE2005

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE2005 COMMAND '(&04)' CANNOT BE PROCESSED AT THE MOMENT. REASON: '(&07)'

### Meaning

Final message of a SHC-OSD command that cannot be started at the moment
for internal reasons:
- FITC timeout at datatransfer to SHC-OSD user task (direction see reason)
SEND TIMEOUT: order not yet started as user task is too busy.
RECEIVE TIMEOUT: order not finished within given time.
- Error in restart of SHC-OSD task for example if subsystem POSIX is
not available.

## NDE2006

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE2006 NO OUTPUT INFORMATION FOR COMMAND '(&04)'

### Meaning

Final message of a SHC-OSD SHOW-command with no output information for
the specified input operands.
Other possible reasons:
- For ETERNUS DX: StorMan and/or CIMOM is not accessible.
- For SM-PUBSET: the CATID is unknown to DMS.

### Response

For ETERNUS DX: Please check the StorMan and CIMOM settings
with /SHOW-SHC-ENVIRONMENT.
For SM-PUBSET: Create Master-Catalog-Entry for CATID using
/ADD-MASTER-CATALOG-ENTRY.

## NDE2007

Destination: USER-TASK, CONSOLE Routing code: 0 Weight: 70

Warranty : YES

NDE2007 COMMAND '(&04)' NOT PROCESSED FOR DEVICE (&00)(&10)(&09)(&11) (&07) (&06)(&12)(&14)(&13)

## NDE2009

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE2009 SYNCHRONOUS PROCESSING OF COMMAND '(&04)' ABORTED BY K2 KEY OR CANCEL-JOB

### Meaning

Final message of a SHC-OSD command which synchronous processing was
interrupted by input of key K2.

## NDE2010

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE2010 COMMAND '(&04)' COMPLETED WITH WARNINGS

### Meaning

Final message of a SHC-OSD command which has been processed successfully
after output of warning message(s).

## NDE2012

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE2012 NOT ALLOWED PARAMETER COMBINATION IN COMMAND '(&04)'

### Meaning

Final message of a SHC-OSD command which could not be processed
successfully due to an invalid parameter combination.

## NDE2014

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE2014 STORMAN ERROR '(&07)' IN COMMAND '(&04)'

### Meaning

A SHC-OSD command (&04) could not be processed successfully, due to a
StorMan error (&07).
Further details to StorMan errors:
--------------------------------------------------------------------------
EC! Error ! Details and explanations
--+------------------------------+----------------------------------------
1!STORMAN_NO_ACTION !No action necessary
2!STORMAN_NOT_COMPLETE !Function only partially completed
3!STORMAN_VER_NOT_SUPP !StorMan client version not supported
7!STORMAN_INV_PARAMETERS !Specified parameters invalid
--+------------------------------+----------------------------------------
8!STORMAN_INVALID_STORID !Specified StorID is invalid
10!STORMAN_STORID_NOT_FOUND !Specified StorID is unknown
13!STORMAN_COMMUNIC_ERROR !Error in StorMan client-server
! ! communication
14!STORMAN_STORAGE_LOCKED !Storage system currently locked
16!STORMAN_FAULT !Error in function
18!STORMAN_NOT_FOUND !Resource not found in StorMan data base
21!STORMAN_FCT_NOT_POSSIBLE !Function could not be performed
22!STORMAN_RESOURCE_NOT_AVAILABLE!Provider not available
25!STORMAN_PROVIDER_AUTH_FAILED !provider user password invalid
--+------------------------------+----------------------------------------
29!STORMAN_MIRROR_ERROR !Error during replication function
! ! Check subcode for more information
30!STORMAN_RETRY_LATER !Function currently not possible
35!STORMAN_SYSTEM_LOCKED !ETERNUS DX system ist currently locked
37!STORMAN_PROVIDER_ERROR !Provider returned an error
! ! Check subcode for more information
--------------------------------------------------------------------------

### Response

For further details the current StorMan logging file (most recent date)
from the StorMan installation directory on the StorMan server is required.

## NDE2015

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE2015 COMMAND '(&04)' COMPLETED SUCCESSFULLY

### Meaning

Final message of a SHC-OSD command which has been successfully processed.

## NDE2016

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE2016 INVALID PARAMETER IN COMMAND '(&04)': (&07)

### Meaning

Final message of a SHC-OSD command which could not be processed
successfully due to an invalid parameter.

## NDE2017

Destination: USER-TASK Routing code: Weight: 70

Warranty : YES

NDE2017 COMMAND CANNOT BE PROCESSED IN THE CURRENT STATE OF REPLICATION

### Meaning

The command can't be processed in the current status of the replication
pair, as it is not supported by the storage system.

### Response

Please check the status of the replication pair(s).

©2024 Fujitsu | BS2000 System Messages