## SNF0100

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SNF0100 Error '(&00)' from interface '(&01)'

### Meaning

(&00) : main code from interface
(&01) : system/internal interface name

## SNF0101

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SNF0101 Recipient file is currently not active.

## SNF0102

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SNF0102 Backup file '(&00)' created

### Meaning

(&00) : filename

## SNF0103

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SNF0103 Backup of recipient file not possible for the moment. Request is in delay.

### Meaning

The recipient file is currently opened by at least one method.
Backup will be performed as soon as possible.

## SNF0104

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SNF0104 Backup of recipient file already in progress. Request is rejected.

©2024 Fujitsu | BS2000 System Messages