## SEAREVI

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SEAREVI COMP=SEAMF,VERS=91A,DATE=201215

## SEA4002

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4002 KEYWORD IS MISSING. PROGRAM RUN TERMINATED

### Meaning

The function or the keyword NAME or SPACE was not specified.

### Response

Enter function or NAME or SPACE in 1P0 statement.

## SEA4004

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4004 SYNTAX ERROR IN 1P0 STATEMENT. PROGRAM RUN TERMINATED

### Response

Correct concerned statement and repeat program run.

## SEA4005

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4005 INVALID LIST FUNCTION. PROGRAM RUN ABORTED

### Response

Correct 1P0 statement, repeat program run.

## SEA4010

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4010 STATEMENT IGNORED

### Meaning

Erroneous statement. The program run is continued.

### Response

Correct the statement concerned and repeat the program run.

## SEA4011

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4011 INVALID LIMITATION

### Meaning

In global and single limitations, inconsistent specifications were made.

### Response

Check and correct the limitation statement, repeat program run.

## SEA4012

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4012 ERROR IN SEQUENCE

### Meaning

An invalid sequence has been detected in input statements.
(1P1, 1P2, 1P3, 1P4 ...).

### Response

Correct configuration of statements and repeat program run.

## SEA4013

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4013 INVALID SAN

### Meaning

The symbolic attribute names must begin with an alphabetic character.
The program run is continued.

### Response

Correct erroneous symbolic attribute names and repeat program run.

## SEA4014

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4014 SYNTAX ERROR IN 1P1-1P5 STATEMENT. PROGRAM RUN ABORTED

### Response

Correct the statement concerned and repeat the program run.

## SEA4015

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4015 TOO MANY DELETE PASSWORDS

### Meaning

Max. 120 statements are allowed. The program is continued.

### Response

The SEPA run must be split up into several runs. Repeat program run.

## SEA4016

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4016 TOO MANY CHANGE PASSWORDS

### Meaning

See SEA4015.

### Response

See SEA4015.

## SEA4017

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4017 INTERNAL ERROR. PROGRAM RUN TERMINATED WITH DUMP

### Response

Send error documents, repeat program run.

## SEA4018

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4018 NEGATION ERROR

### Meaning

Sequence specification does not contain 'N' in the fourth column. The
program run is continued, the password is ignored.

### Response

Correct concerned statement and repeat program run.

## SEA4019

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4019 INCONSISTENCY IN AUTHORIZATION

### Meaning

An inconsistency was noticed; program run is continued.

### Response

Correct error(s) in statement and repeat program run.

## SEA4020

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4020 SAN NOT ASCENDING

### Meaning

SAN specified have to be listed in ascending order. Program run is
continued, password is ignored.

### Response

Correct error(s) in statement and repeat program run.

## SEA4021

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4021 1P0 STATEMENT MISSING

### Meaning

Runtime control statement is missing. Program run is terminated.

### Response

Provide 1P0 statement and repeat program run.

## SEA4022

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4022 KEYWORD MULTIPLY DEFINED

### Meaning

Function in 1P0 statement is multiply defined. Program run is terminated.

### Response

Correct 1P0 statement and repeat program run.

## SEA4025

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4025 PASSWORD CATALOG NOT GENERATED

### Meaning

The request cannot be executed, because no password catalog is existing.
Program run is terminated.

### Response

Start GEN, repeat program run.

## SEA4026

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4026 PASSWORD CATALOG DESTROYED

### Meaning

List of passwords is destroyed.

### Response

Reconstructions are necessary, repeat program run.

## SEA4027

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4027 PASSWORD ORDER NOT ASCENDING

### Meaning

Password order in 1P1 statement is not ascending. Password is ignored,
program run is continued.

### Response

Correct statement, repeat program run.

## SEA4028

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4028 PRIMARY KEYS NOT ASCENDING

### Meaning

Primary keys in 1P3/1P4 are not sorted in ascending order. Program run is
continued, password is ignored.

### Response

Sort and reissue statement, repeat program run.

## SEA4030

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4030 LENGTH OF PASSWORD NOT 3 CHARACTERS

### Meaning

Syntactical error; program run is continued.

### Response

Correct statement, repeat program run.

## SEA4031

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4031 LIST FUNCTION IS NOT EXECUTED

### Meaning

List operand inconsistent with request.

### Response

Start new list function and restart SEPA run.

## SEA4033

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4033 NO DATA EXISTING FOR UPDATE

### Meaning

Although indicated in 1P1 statement, no 1P2-1P4 statements follow.
Program run is continued.

### Response

Insert statements missing, repeat program run.

## SEA4034

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4034 NOT ALL PASSWORDS GENERATED

### Meaning

Remark on SYSDTA: password is not accepted.

## SEA4035

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4035 MORE THAN 100 PASSWORDS

### Meaning

The maximum number of 100 statements can be handled. Program run is
continued.

## SEA4036

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4036 ERROR CONCERNING 1P1-CP DATA

## SEA4037

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4037 ERROR CONCERNING 1P1-DP DATA

## SEA4038

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4038 HEXADECIMAL STRING INVALID AS ENTRY. CORRECT ENTRY

## SEA4039

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4039 PASSWORD '(&00)' ALREADY AVAILABLE IN PASSWORD CATALOG. RUN IS CONTINUED

### Response

Possibly delete available password (KW). An overall view of all passwords
can be obtained using LIST.

## SEA4040

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4040 PASSWORD '(&00)' NOT AVAILABLE IN PASSWORD CATALOG. RUN IS CONTINUED

### Meaning

During deletion or modification it was detected that the password (KW)
is not available in the password catalog.

### Response

Correct statement; if necessary, repeat run.

## SEA4041

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4041 PASSWORD '(&00)' MULTIPLY SPECIFIED IN MODIFICATION STATEMENT. RUN IS CONTINUED

### Response

Correct statement; if necessary, repeat program run.

## SEA4042

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA4042 FOR PASSWORD '(&00)' CONTRADICTION IN PASSWORD ASSIGNMENT. RUN IS CONTINUED

### Meaning

The password cannot be deleted and modified in the same program run.

### Response

Correct statement, repeat program run.

## SEA4043

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA4043 PASSWORD '(&00)' NOT GENERATED DUE TO PRECEDING ERRORS

### Response

Repeat statement with corrected control operands.

## SEA4044

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA4044 PASSWORD CATALOG EMPTY

### Meaning

The password catalog is empty.

## SEA4045

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA4045 NO TABLE ON SPECIFIED SPACE

### Meaning

There is no table on the specified space.

### Response

Specify the space the table is on.

## SEA4046

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA4046 TABLE DOES NOT SUPPORT CALL-DML.

### Meaning

Table can only be processed with SQL. SEPA can only be used with tables
which support CALL-DML.

## SEA4047

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA4047 TABLE IS A PARTITIONED TABLE.

### Meaning

SEPA cannot be used with Partitioned Tables.

## SEA4048

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA4048 SCHEMA NAME NOT IN CORRECT FORMAT.

## SEA4049

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA4049 TABLE NAME NOT IN CORRECT FORMAT.

## SEA4050

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA4050 FILE NAME NOT IN CORRECT FORMAT.

## SEA4051

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA4051 PASSWORD NOT IN CORRECT FORMAT.

## SEA4052

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA4052 INTERNAL ERROR. ERRONEOUS METADATA FOR SPACE

### Response

Repair the space with RECOVER.

## SEA4053

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA4053 SQLSTATUS (&00) OCCURRED WHEN PROCESSING FILE. (DMS ERROR: &01))

### Meaning

A DMS error (&01) occurred when processing the file.

### Response

Eliminate the DMS error as described in the BS2000 manual
'System Messages'.

## SEA4055

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA4055 SPACE IS CORRUPT.

### Response

Repair the space with RECOVER

## SEA4056

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA4056 DMS ERROR (&00) OCCURRED WHEN PROCESSING THE SPECIFIED FILE.

### Response

Eliminate the DMS error as described in the BS2000 manual
'System Messages'.

## SEA4057

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA4057 TABLE IS CORRUPT

### Meaning

The table has been flagged as corrupt.

### Response

Repair the space in which the table is located with RECOVER

## SEA4058

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SEA4058 TOO MANY INDIVIDUAL CONSTRAINTS FOR A PASSWORD

### Meaning

The internal memory area for PK0 records has overflowed.

### Response

Assign individual constraints more restrictively or define several
passwords.

## SEA4059

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SEA4059 PRIMARY KEY VALUE TOO LONG

### Meaning

A primary key value was specified which is longer than permitted in the
definition.

### Response

Specify a primary key value of the correct length.

## SEA4060

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SEA4060 INVALID PASSWORD

### Meaning

The specified password has a hexadecimal representation X'404040' or
X'000000' or X'FFFFFF'.

### Response

Specify a valid password

## SEA4061

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA4061 FILE (&00) DOES NOT EXIST.

## SEA4062

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SEA4062 THE CATALOG SPACE MUST NOT BE PROCESSED USING SEPA.

## SEA7000

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA7000 CONSISTENCY CHECK (&00) (&01) OCCURRED IN SESADM

### Meaning

A system error occurred in SESADM. A user dump will be generated and the
program aborted.

### Response

Submit dump to SESAM diagnostics staff.

## SEA7001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SEA7001 SESADM TERMINATED WITHOUT ADMINISTRATION

### Meaning

SESADM was terminated immediately after loading.

## SEA7002

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SEA7002 NO ADMINISTRATION YET PERFORMED FOR SPECIFIED PROGRAM

### Meaning

SESADM was terminated immediately after the program to be administered
was specified.

## SEA7003

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7003 INCORRECT SYNTAX IN SESADM STATEMENT OR END STATEMENT MISSING AT THE END OF A SESADM INPUT FILE

### Meaning

The SESADM statement must be entered with the syntax described in SESADM
user syntax file. Every SESADM input file must be terminated with an END
statement.
Also the message will occurr if after a semantic error at
PREPARE-FOREIGN-COPY
the SDF-Statement END is read.

### Response

Correct syntax of the SESADM statement or add END statement to the end of
the SESADM input file.

## SEA7004

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7004 SDF IS NOT AVAILABLE.

### Meaning

SDF is not loaded in the system or still has to be loaded by the
administrator.

## SEA7005

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7005 SDF SYNTAX FILE DOES NOT EXIST.

### Response

Ask the system administrator to add the SDF syntax file

## SEA7006

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7006 ERROR DIALOG IS NOT POSSIBLE.

### Meaning

Error dialog is not permitted in expert mode.

## SEA7007

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7007 INVALID SEMANTICS IN SESAM STATEMENT

### Response

Correct the semantic error.

## SEA7008

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7008 ERROR (STATUS (&00)) DURING INITIALISATION OF DBCON

### Meaning

Status is discriped in the Message Manual!

### Response

Eliminate the reason for the error and start SESADM again.

## SEA7009

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7009 SESADM IS RUNNING IN A CONFIGURATION WITHOUT SESDCN; IT IS ONLY POSSIBLE TO ADMINISTER THE STANDARD DBH OF YOUR OWN CONFIGURATION.

### Meaning

An attempt was made to administer a SESAM DBH of a foreign configuration
or a further SESAM DBH of your own configuration.

### Response

Start SESDCN in the configuration to which SESADM is assigned in its
configuration file, or assign SESADM to a different configuration, in
which SESDCN is already active.

## SEA7010

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7010 SPECIFIED DCN NOT KNOWN IN DISTRIBUTION RULE

### Meaning

There is no DCN in the distribution rule which corresponds to the DCN
identification in the START-DCN-ADMINISTRATION statement (processor name,
configuration name, DCN name).

### Response

Specify a START-DCN-ADMINISTRATION statement with an identifiable DCN.

## SEA7011

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7011 SPECIFIED SESAM-DBH IS UNKNOWN IN DISTRIBUTION RULE

### Meaning

No DBH corresponding to the DBH identification in the
START-DBH-ADMINISTRATION statement (processor name, configuration name,
DBH name) is known to the distribution rule.

### Response

Specify START-DBH-ADMINISTRATION with an identifiable DBH.

## SEA7012

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7012 DCN/DBH TO BE ADMINISTERED NOT AVAILABLE.

### Meaning

The DCN/DBH to be administered is included in the distribution rule, but
is not an active task, or the DBH failed.

### Response

Enter new START-DCN-ADMINISTRATION or START-DBH-ADMINISTRATION statement.

## SEA7013

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7013 SESADM IS RUNNING IN A CONFIGURATION WITHOUT SESDCN; SESDCN CANNOT BE ADMINISTERED.

### Response

- Start SESDCN in the configuration to which SESADM is assigned in its
configuration file and then restart SESADM
- or assign SESADM to a different configuration, in which SESDCN is
already active.

## SEA7014

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7014 ERROR IN DCN/DBH ADMINISTRATION

## SEA7015

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7015 RESPONSE TRUNCATED

### Meaning

The response area is too small. The response message was truncated.

## SEA7016

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA7016 RESOURCE BOTTLENECK (STATUS (&00))

### Meaning

A memory bottleneck or overflow occurred.

## SEA7017

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA7017 SYSTEM ERROR (STATUS (&00))

## SEA7018

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA7018 ERRONEOUS OPERAND

### Meaning

This message is issued in the SDF error dialog.

## SEA7019

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7019 ADMINISTRATION CALL ABORTED

## SEA7020

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7020 /ADMINISTRATION CALL STOP-DBH ACCEPTED

## SEA7021

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7021 REQUESTING USER ROLLED BACK BY SYSTEM

### Meaning

The system has removed the requesting user.
Possible causes:
Rollback by administration or internal restart

### Response

Repeat START-DBH-ADMINISTRATION statement.

## SEA7022

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7022 'SESDCN' ADMINISTRATION STATEMENT REJECTED; ANOTHER 'SESDCN' ADMINISTRATION STATEMENT CURRENTLY BEING PROCESSED

### Response

Repeat SESDCN ADMINISTRATION STATEMENT

## SEA7023

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7023 USER-CLOSE REJECTED BECAUSE OF A PENDING END-LOCK-SEQUENCE

### Response

Execute END-LOCK-SEQUENCE before closing DBH Administration Session

## SEA7024

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7024 OUTPUT INTO A TEMPORARY FILE NOT POSSIBLE IN THE CURRENT RUNNING ENVIRONMENT

### Meaning

SESADM is running in the batch mode, a 'SHOW-FILE' command is not possible

## SEA7025

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7025 NO TEMPORARY FILE EXISTING

### Meaning

A tmporary file is existing only when a 'MODIFY-OUTPUT-MODE
OUTPUT=*SHOW-FILE'
command was given before and an administration command was sent to DBH or
DCN

## SEA7026

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7026 THE FILE CONTAINING THE SPACE NAMES DOES NOT EXIST

### Meaning

The file given within the SESADM Statement 'PREPARE-FOREIGN-COPY' for
'SPACE-NAMES=*FROM-FILE' does not exist.

## SEA7027

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7027 THE FILE CONTAINING THE SPACE NAMES IS EMPTY

### Meaning

The file given within the SESADM Statement 'PREPARE-FOREIGN-COPY' for
'SPACE-NAMES=*FROM-FILE' is empty.

## SEA7028

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7028 THE FILE CONTAINING THE SPACE NAMES HAS TOO MANY LINES

### Meaning

The file given within the SESADM Statement 'PREPARE-FOREIGN-COPY' for
'SPACE-NAMES=*FROM-FILE' contains more than 399 lines.

### Response

Shorten the number of lines to 399.

## SEA7029

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7029 INCORRECT SPACE NAME IN FILE '(&00)' ON LINE (&01)

### Meaning

The file given within the SESADM Statement 'PREPARE-FOREIGN-COPY' for
'SPACE-NAMES=*FROM-FILE' contains an incorrect space name on the reported
line.

### Response

Correct the file containing the space names.

## SEA7030

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7030 THE ACCESS TO THE FILE CONTAINING THE SPACE NAMES RETURNS THE DMS ERROR: '(&00)'

### Meaning

The access to the file given within the SESADM Statement
'PREPARE-FOREIGN-COPY' for 'SPACE-NAMES=*FROM-FILE' returned a DMS Error.

### Response

Correct the file containing the space names.

## SEA7031

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7031 ADM: FORCED LOCK REQUEST CANNOT BE IMPLEMENTED DUE TO (&00). COMMAND REJECTED.

### Meaning

A lock request for a lock sequence (Forced mode) could not be forced
because the respective object is already locked by another lock sequence,
a transaction in PTC status or a transaction of an internal system user.

### Response

Try again later! Terminate the PTC transaction if necessary.

## SEA7032

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7032 ADM: NO OUTPUT INTO S-VARIABLE.

### Meaning

An error occurred writing the specified S-Variable.
The content of the S-Variable specified in Command or assigned
to the stream SYSINF is not changed. The administration
command works well else.

### Response

Check occurred messages from SDF-P.

## SEA7033

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7033 ADM: OUTPUT INTO S-VARIABLE WRONG.

### Meaning

An error occurred writing the specified S-Variable.
The content of the S-Variable specified in Command or assigned
to the stream SYSINF can be partly changed. Therefore it is not
usable in further run of the procedure. The administration
command works well else.

### Response

Check occurred messages from SDF-P.

## SEA7034

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7034 ADM: SDF HAS DETECTED AN ERROR. ALL STATEMENTS WERE IGNORED UNTIL '//STEP' WAS RECOGNIZED.

### Meaning

None.

### Response

None.

## SEA7035

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7035 AN ERROR DURING INITIALIZING MAIL SERVICE OCCURRED.

### Meaning

During initializing the mail service for SESADM an error possibly
concerning
the mail file occurred.
The output destination is changed to the standard value, in interactive
mode all outputs are directed to SYSOUT, in batch mode to SYSLST.

### Response

After correcting the error causes repeat the SESADM control statement
MODIFY-OUTPUT-MODE *OUTPUT=*MAIL. It is possible that a restart of SESADM
is necessary.

## SEA7036

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7036 ERROR AT PROCESSING THE FILE SENT BY MAIL.

### Meaning

During writing the output in a file an error occurred. A possible
DVS-Error
is issued in an additional message. The output destination is changed to
the
satndard value. The next MODIFY-OUTPUT-MODE statement will send the
uncomplete
file.

### Response

After correcting the error causes change the output dsetiniation to mail
by using
the SESADM control statement MODIFY-OUTPUT-MODE.

## SEA7037

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7037 INITIALIZING MAIL SERVICE SUCCESSFUL.

### Meaning

The mail service is successfully initialized. An answer of DBH or DCN can
be sent by
mail.

### Response

None.

## SEA7038

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7038 MODIFICATION OF OUTPUT DESTINATION FOR FOLLOWING ADMINISTRATION STATEMENTS PERFORMED.

### Meaning

The user is informed about the successful modification.

### Response

None.

## SEA7039

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7039 SENDING FILE CONTAINING ANSWERS OF ADMINISTRATION STATEMENTS BY MAIL CAUSED.

### Meaning

SEnding the file containing the answers of administrations statements
to the address specified in the mail file is caused. If a failure occurs
a specific message will be issued in some cases.

### Response

None.

## SEA7040

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7040 ANY ANSWER DO NOT EXIST. A MAIL IS NOT SENT.

### Meaning

At modificating the output destination *MAIL by MODIFY-OUTPUT-MODE
the file containing the answers will be sent normally.
If the file ist empty, no mail will be sent.

### Response

None.

## SEA7041

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7041 THE ANSWER OF THE ADMINISTRATION STATEMENT SAVED FOR SENDING BY MAIL.

### Meaning

A received answer from DBH or DCN is stored in a temporary file. This
file will be sent by mail at the next MODIFY-OUTPUT-MODE. The message
do not inform about the result of the actual administration statement.

### Response

None.

## SEA7042

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7042 LOCK SEQUENCE ABORTED

### Meaning

Probably the lock sequence is aborted by another SESADM.

### Response

None.

## SEA7043

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEA7043 VALUES FOR OPERANDS ARE SEMANTICALLY WRONG.

### Meaning

Invalid semantics in SESADM statement concers at least two operands.
For example RECONFIGURE-DBH-SESSION does not allow all operands
with the value *UNCHANGED.

### Response

None.

## SEA7044

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEA7044 ERROR IN SESADM STATEMENT: ALL OPERANDS ARE ASSIGNED TO THE SESADM STANDARD VALUE.

### Meaning

All operands are assigned to the SESADM standard value which is not
allowed
for the current statement.
For RECONFIGURE-DBH-SESSION at least one operand must be different
from the value *UNCHANGED.

### Response

Correct the statement.

©2024 Fujitsu | BS2000 System Messages