## DCM0200

Destination: CONSOLE Routing code: C Weight: 99

Warranty : NO

DCM0200 VTSU-B NOT LOADED

### Meaning

VTSU-B is not loaded. As a result it cannot be called.

## DCM0202

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

DCM0202 VTSU-B INIT: DMS ERROR '(&01)' WHEN OPENING FILE '(&00)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

File (&00) exists but cannot be opened.
Possible reasons:
- The file is defective.
- The file is protected by a password.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Take measures in correspondence to the DMS error code.
If necessary specify the password.
If the file is defective, reconstruct the file.
Contact the system administrator, if necessary.

## DCM0203

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

DCM0203 VTSU-B INIT: DMS ERROR '(&01)' WHEN ACCESSING FILE '(&00)'. IN SYSTEM MODE: HELP-MSG DMS(&01)

### Meaning

The user is not authorized to read the file (&00).
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## DCM0204

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

DCM0204 VTSU-B INIT: DMS ERROR '(&01)' WHEN CLOSING FILE '(&00)'. IN SYSTEM MODE: /HELP-MSG DMS(&01)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Check the file, if necessary contact the system administrator.

## DCM0205

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

DCM0205 VTSU-B INIT: VTSU CONTROL RECORD MISSING IN FILE '(&00)'

### Meaning

The first line must be /BEGIN VTSU PARAMS or /BEGIN VTSU-PARAMS.

### Response

Correct the file.

## DCM0206

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

DCM0206 VTSU-B INIT: INVALID OR UNKNOWN PARAMETER '(&00)' IN FILE '(&01)'

### Response

Correct the file.

## DCM0207

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

DCM0207 VTSU-B INIT: END RECORD MISSING IN FILE '(&00)'

### Meaning

The very last line of the file (&00) must be /END PARAMS or /END-PARAMS.

### Response

Correct the file.

## DCM0208

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCM0208 'CSTRING' OPERAND: '(&00)' UNKNOWN OR ILLEGAL BY SUBSYSTEM VTSUTRAC INITIALIZATION

### Meaning

The value of the CSTRING operand in the /CREATE-SUBSYSTEM command
contains unknown or illegal parameters.

### Response

Correct the operand value and try again.

## DCM0209

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCM0209 WARNING: INTERNAL ERROR X'(&00)' IN '(&01)' INTERFACE. 7 BIT CODED CHARACTER SET ASSUMED

### Meaning

Internal error in system interface.

### Response

Analyse the received error code and contact the system administrator.

## DCM0210

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCM0210 WARNING: INVALID USER DEFAULT CODED CHARACTER SET. STANDARD 7 BIT CODED CHARACTER SET ASSUMED

### Meaning

The user default coded character set is invalid.
Possible causes are :
(1) the default coded character set is not known by XHCS-SYS
(2) the default coded character set (not EDF03IRV) has a restricted
compatibility with its reference coded character set
(3) the default coded character set is not a EBCDIC one
(4) the special routines for arabic coded character set support
are not present.

### Response

- Ask the system administrator to define the desired 8 bit coded
character set in the XHCS-SYS tables or
- ask the system administrator for the list of 8 bit character sets
supported by XHCS-SYS and supported by this terminal and have such
a code defined as user default character set or set in XHCS tables
- ask the system administrator to install the special routines for
arabic coded character set support

## DCM0211

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCM0211 WARNING: USER DEFAULT CODED CHARACTER SET NOT SUPPORTED BY TERMINAL. 7 BIT CODED CHARACTER SET ASSUMED

### Meaning

The user default coded character set is a 8 bit coded character set that
the terminal does not support.

### Response

- Employ a terminal supporting this 8 bit coded character set or
- modify the set up of the terminal for this 8 bit coded character set
(with SIDATA) or
- ask the system administrator to modify the user default coded
character set to one supported by the terminal.

## DCM0212

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCM0212 WARNING: XHCS NOT AVAILABLE. 7 BIT CODED CHARACTER SET ASSUMED

### Meaning

The subsystem XHCS-SYS is not available. As a result the use of the
8 bit functionality is not possible. Only the 7 bit functionality is
available.

### Response

Ask the system administrator to remove user default coded character set or
to install XHCS.

## DCM0213

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCM0213 WARNING : INVALID USER DEFAULT CODED CHARACTER SET WITH 7 BIT TERMINAL. 7 BIT CODED CHARACTER SET ASSUMED

### Meaning

On a 7-bit terminal, only blanks or EDF03IRV is allowed as user default
coded character set name.

### Response

- Check user default character set name and employ an adequate terminal or
- ask the system administrator to change the user default coded character
set to EDF03IRV.

## DCM0214

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCM0214 WARNING: XHCS NOT PRESENT. 7 BIT CODED CHARACTER SET ASSUMED

### Meaning

The subsystem XHCS-SYS is not present. As a result the use of the 8 bit
functionality is not possible. Only the 7 bit functionality is available.

### Response

Contact the system administrator about XHCS-SYS availability.

## DCM0215

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCM0215 VTSU-B V21.0B VTSUCB V06

## DCM0216

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCM0216 REQUESTED VARIANT IS NOT SUPPORTED

## DCM0217

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCM0217 NO MEMORY AVAILABLE

## DCM0218

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCM0218 ESC-SEQUENCE NOT ALLOWED

## DCM0219

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCM0219 OVERFLOW OF BUFFER

## DCM0220

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCM0220 ERROR IN TABLE

## DCM0221

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCM0221 ENCRYPTION HAS BEEN REQUESTED FOR THIS APPLICATION

### Meaning

The terminal does not support encryption mechanism.

### Response

Contact the system administrator.

## DCM0222

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

DCM0222 VTSU-B INIT: INVALID LINE FORMAT IN FILE '(&00)' AT LINE '(&01)'. LINE IGNORED

### Meaning

The specified line does not respect the described format.
The line is ignored for the current session.

### Response

Correct the specified line. The correction will be effective only after
the next loading of the subsystem.

## DCM0223

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

DCM0223 VTSU-B INIT: INVALID VARIANT '(&00)' IN FILE '(&01)' AT LINE '(&02)'. LINE IGNORED

### Meaning

The 8-bit variant given at the specified line is not valid :
- either the 8-bit variant is not supported by XHCS-SYS
- or the variant is an ISO variant.
The line is ignored for the current session.

### Response

Correct the 8-bit variant. The correction will be effective only after the
next loading of the subsystem.

## DCM0224

Destination: CONSOLE Routing code: C Weight: 70

Warranty : NO

DCM0224 VTSU-B INIT: INVALID DEVICE TYPE '(&00)' IN FILE '(&01)' AT LINE '(&02)'. LINE IGNORED

### Meaning

The device type given at the specified line is not valid.
The line is ignored for the current session.

### Response

Correct the device type. The correction will be effective only after the
next loading of the susbsystem.

©2024 Fujitsu | BS2000 System Messages