## JVS04AC

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS04AC WARNING: INCORRECT TIME CONVERSION FROM UTC TO LT. PROCESSING CONTINUES

### Meaning

This message is issued if the GTIME macro for converting the time from
UTC to local time is terminated incorrectly when output of a catalog
entry is initiated by a SHOW-JV-ATTRIBUTES command.
The date/time specifications converted incorrectly are indicated
with ????-??-?? or ??:??:??.

### Response

Have the startup parameter file checked by the system administrator
and corrected if necessary.

## JVS04AD

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS04AD ERROR DURING PRESENTATION VARIABLE PRODUCTION

### Meaning

A problem has been encountered during the production of presentation
variables by the command server.
Possible reasons:
- subsystem SDF-P not available
- lack of space for SSTA buffer
- return code from SSTA interface.

## JVS04A0

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS04A0 SUBSYSTEM 'JV' NOT ACCESSIBLE. COMMAND REJECTED

### Meaning

The subsystem JV (Job Variable Services) could not be connected to
the system.
Possible reasons:
- The job variable subsystem is not available.
- An error occurred in the system function for setting up the
subsystem connection.

### Response

Contact the system administrator.

## JVS04A1

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS04A1 SYNTAX ERROR IN JV COMMAND. CORRECT COMMAND

### Meaning

The command is rejected because one or more of the operands specified
in it contains a syntax error.

## JVS04A2

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

JVS04A2 JOB VARIABLE '(&00)' DELETED

### Meaning

Deletion of the specified job variable is acknowledged.
The output was caused by the operand OUTPUT=SYSOUT in the DELETE-JV
command.

## JVS04A3

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

JVS04A3 ERROR WHEN DELETING JOB VARIABLE '(&00)'

### Meaning

This message indicates that the specified job variable could not be
deleted. The reason is given in the following message.

## JVS04A6

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS04A6 SYSTEM ERROR DURING OUTPUT TO SYSOUT. COMMAND REJECTED

### Meaning

An error has occurred during execution of a YTIEOUT macro.
Possible reasons:
- unrecoverable I/O error
- illegal operand
- excessively long message.

### Response

If the error is fatal, contact the system administrator. Generate
diagnostic material if necessary.

## JVS04A9

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS04A9 /MODIFY-JV-CONDITIONALLY: BRANCH DESTINATION NOT FOUND. PROCEDURE ABORTED

## JVS04BB

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS04BB ERROR DURING MODIFYING A JV. COMMAND REJECTED

### Meaning

Possible reasons:
- both JVTYPE=INTGEGER and JVTYPE=BOOLEAN was specified
- in addition to a specified substring the JVTYPE=INTEGER
or BOOLEAN or NULLSTR=YES was given.

## JVS04BC

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS04BC WARNING: NOT ALL JOB VARIABLES DISPLAYED OR DELETED

### Meaning

Possible cause:
- The sum of the job variable names affected by the DELETE-JV or
SHOW-JV-ATTRIBUTES command resulted in saturation of the memory space.
- The processing of the command is interrupted by a /CANCEL-JOB command.

### Response

It is a good idea to repeat the command unchanged in order to process
those job variable names not affected the first time.

## JVS04BD

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS04BD ERROR WHEN ACCESSING SYSTEM FUNCTION. COMMAND REJECTED

### Meaning

The error occurred while attempting to access one of the system
functions ($TANC, $APCB, $EZOTYP, $JCBRW, $GTIME, $RDUID etc.).

### Response

Inform the system administrator so that diagnostic material
can be generated.

## JVS04BE

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS04BE SPECIFIED USER ID DOES NOT EXIST. COMMAND REJECTED

### Meaning

Possible reasons:
- no DEFAULT-PUBSET could be found
- the specified PVS does not contain the desired user ID
- the specified user id 'SYSJV' is reserved and must not be
used in this command.

### Response

Reissue the command with the correct PVS ID or request the system
administrator to add the user ID to the appropriate PVS.

## JVS04BF

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS04BF REQUESTED ACCESS TO JV NOT PERMITTED DUE TO EXISTING JV PROTECTION. COMMAND REJECTED

### Meaning

Possible reasons:
- the job variable is protected with Basic-ACL or GUARDS
- the subsystem GUARDS is not loaded.

### Response

If possible, change the access authorization accordingly or
ask the system administrator to start the subsystem GUARDS.

## JVS04B1

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS04B1 PASSWORD NOT SPECIFIED. COMMAND REJECTED

### Meaning

The user has attempted to access a job variable without specifying the
necessary password.

### Response

Enter the required password by means of the PASSWORD operand or the
ADD-PASSWORD command and then repeat the rejected JV command.

## JVS04B2

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS04B2 SPECIFIED JOB VARIABLE SUBSTRING EMPTY OR ILLEGAL. COMMAND REJECTED

### Meaning

Possible reasons:
- the job variable is empty
- the specified substring of the job variable is empty
- the values specified in the substring entry exceed the maximum
permissible job variable length (256 bytes).

### Response

Check the length of the job variable contents using SHOW-JV-ATTRIBUTES
and then repeat the JV command after correcting the error.

## JVS04B3

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS04B3 SYNTAX ERROR IN JV NAME. CORRECT COMMAND

### Response

Correct the job variable name and then repeat the command.

## JVS04B4

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS04B4 LINK NAME NOT DEFINED BEFOREHAND. COMMAND REJECTED

### Response

Define the job variable link name by means of the SET-JV-LINK command
and then repeat the JV command.

## JVS04B5

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS04B5 SYSTEM ERROR DURING JVS OPERATION: REQUEST MEMORY ERROR. COMMAND REJECTED

### Meaning

Operating system error. Possible error causes:
- there is not enough memory space to complete command processing
- an illegal operand has been specified for $GETMEM.

### Response

Inform the system administrator so that diagnostic material can be
generated.

## JVS04B6

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS04B6 EXPIRATION DATE FOR JOB VARIABLE NOT YET REACHED. COMMAND REJECTED

### Meaning

The expiration date in the job variable catalog entry is later than the
current date, thus making it impossible to delete or modify the
job variable.

### Response

Modify the retention period of the job variable by means of the
MODIFY-JV-ATTRIBUTES command and then repeat the rejected JV command.

## JVS04B7

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS04B7 SYSTEM ERROR DURING JVS OPERATION: RELEASE MEMORY ERROR. COMMAND REJECTED

### Meaning

Operating system error. Possible causes:
- the specified area was not requested by means of $GETMEM
- an invalid operand was specified for $RETMEM.

### Response

Inform the system administrator so that diagnostic material can be
generated.

## JVS04B8

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS04B8 ONLY READ ACCESS PERMITTED. COMMAND REJECTED

### Response

Change the access authorization by means of the MODIFY-JV-ATTRIBUTES
command and then repeat the rejected JV command.

## JVS04CA

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS04CA ERROR DURING UPDATE OF CE LIMIT. COMMAND PROCESSING TERMINATED ABNORMALLY

### Meaning

The update of the CE limit counter is terminated abnormally.
The CMS operation concerned could not be processed completely.

### Response

Inform the system administrator so that diagnostic material can be
generated.

## JVS04C8

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS04C8 CE LIMIT REACHED. COMMAND REJECTED

### Meaning

This message is issued if the current CE counter exceeds the CE contingent
specified in the file SYSSRPM when a JV catalog entry is entered into the
TSOSCAT.

### Response

Delete JVs no longer required or
ask the system administrator to increase the CE contingent for the user's
job variables with the aid of the MODIFY-USER command.

## JVS04D0

Destination: USER-TASK Routing code: Weight: 30

Warranty : YES

JVS04D0 MONITORING JOB VARIABLE '(&00)' IS NOT ACCESSIBLE. REASON: '(&01)'. IN SYSTEM MODE: /HELP-MSG JVS(&01)

### Meaning

An internal call to access monitoring job variable (&00) was not
successful. Return code (&01) has the same meaning as message JVS(&01).

### Response

Consult message JVS(&01).

## JVS04D1

Destination: USER-TASK Routing code: Weight: 30

Warranty : YES

JVS04D1 JOB VARIABLE '(&00)' NOT ASSIGNED TO JOB

### Meaning

The JV (&00) isn't a monitoring job variable, i.e. either it has not
been assigned to a job or the job to which it was assigned has already
terminated.

## JVS04D2

Destination: USER-TASK Routing code: Weight: 30

Warranty : YES

JVS04D2 MONITORING JOB VARIABLE '(&00)' ALREADY ASSIGNED TO ANOTHER JOB

### Meaning

The specified monitoring job variable has already been assigned to a job
and is still being used.

### Response

Wait until the job in question terminates or use a different monitoring
job variable.
If this message is displayed even though the monitoring job variable is
not really being used (as may happen after a system crash), it can be made
available again by means of the MODIFY-JV-ATTRIBUTES command.

## JVS04D3

Destination: USER-TASK Routing code: Weight: 30

Warranty : YES

JVS04D3 MONITORING JOB VARIABLE '(&00)' CANNOT BE CREATED. REASON: '(&01)'. IN SYSTEM MODE: /HELP-MSG JVS(&01)

### Meaning

An internal call to create the specified monitoring job variable was not
successful. Return code (&01) has the same meaning as message JVS(&01).

### Response

Consult message JVS(&01).

## JVS04D4

Destination: USER-TASK Routing code: Weight: 30

Warranty : YES

JVS04D4 SYNTAX ERROR IN NAME OF MONITORING JOB VARIABLE '(&00)'. CORRECT COMMAND

### Meaning

The name specified for the monitoring job variable contains a syntax
error.

## JVS04D5

Destination: USER-TASK Routing code: Weight: 30

Warranty : YES

JVS04D5 CATALOG ENTRY FOR MONITORING JOB VARIABLE '(&00)' CANNOT BE UNLOCKED. REASON: '(&01)'. IN SYSTEM MODE: /HELP-MSG JVS(&01)

### Meaning

An internal call to cancel a catalog lock for the specified monitoring
job variable was not successful. Return code (&01) has the same
meaning as message JVS(&01). The catalog lock is automatically
reset after a certain interval (system task: 60 seconds, dialog
task: 120 seconds, batch task: 600 seconds).
Possible cause:
The monitoring job variable is accessed via MSCF-connection between two
hosts and this connection has been severed.

### Response

Consult message JVS(&01).

## JVS04D6

Destination: USER-TASK Routing code: Weight: 30

Warranty : YES

JVS04D6 MONITORING JOB VARIABLE '(&00)' HAS NO TSN

### Meaning

The job associated with the monitoring job variable has not yet got
a TSN.

### Response

Try again after a short interval.

## JVS04D7

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS04D7 MONJV '(&00)' CANNOT BE WRITTEN/REMOVED FROM THE GCF-CATALOG. REASON: '(&01)'

### Meaning

Possible reasons:
An internal call to write or remove the MONJV (&00) to/from the
GCF-catalog was not successful. The function $GCFROP reports
(&01) within maincode.

## JVS04D8

Destination: USER-TASK Routing code: Weight: 30

Warranty : YES

JVS04D8 MONITORING JOB VARIABLE '(&00)' CANNOT BE PROVIDED WITH LINK NAME. REASON: '(&01)'. IN SYSTEM MODE: /HELP-MSG JVS(&01)

### Meaning

An internal call to link the monitoring job variable (&00) via the
link name was not successful. Return code (&01) has the same meaning
as message JVS(&01).

### Response

Consult message JVS(&01).

## JVS04D9

Destination: CONSOLE Routing code: R Weight: 99

Warranty : NO

JVS04D9 THE GCF-CATALOG COULD NOT BE PROCESSED SUCCESSFUL. GCF FUNCTION '(&00)' REPORTS '(&01)'

### Meaning

Possible reasons:
- Error during initialisation/termination of the subsystem JV.
$GCFFOP reports an unrecoverable error (&01) during the function
status, create, open or close.
- error during the import of a pubset. $GCFROP reports an unre-
coverable error (&01) during the function read next one, remove or
add.
(&00): function
(&01): error code.

## JVS04E0

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS04E0 COMMAND CANNOT BE EXECUTED WITHOUT CHANGING CALL ENVIRONMENT. COMMAND REJECTED

### Response

Determine the cause of the error using the preceding message JVS04xx,
remove the error if possible, and repeat the command.

## JVS04E1

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS04E1 COMMAND CANNOT BE EXECUTED AT THE MOMENT. COMMAND REJECTED

### Response

Determine the cause of the error using the preceding message JVS04xx,
remove the error if possible, and repeat the command.
Depending on the type of error, a repeat of the command with unchanged
call operands may be successful even if no measures have been taken to
remove the error.

## JVS04F0

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS04F0 SPECIAL JOB VARIABLE MUST NOT BE COPIED. COMMAND REJECTED

### Meaning

The COPY-JV command must not be used here as special job variables may
not be copied.

### Response

Use MODIFY-JV instead of COPY-JV.

## JVS04F3

Destination: USER-TASK Routing code: Weight: 99

Warranty : YES

JVS04F3 ERROR WHEN ACCESSING JOB VARIABLE '(&00)'

### Meaning

This message indicates that the job variable (&00) could not be
accessed. The reason is given in the following message.

## JVS0401

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS0401 REQUESTED CATALOG NOT ACCESSIBLE. COMMAND REJECTED

### Meaning

One of the specified path names contains the catalog ID of a catalog
that cannot be accessed.

### Response

Contact the system administrator.

## JVS0402

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS0402 REQUESTED CATALOG IN QUIET MODE. WAITING TIME EXPIRED. COMMAND REJECTED

### Meaning

One of the specified path names contains the catalog ID of a catalog which
is in quiet mode. There has been no change in this status during the
scheduled waiting time.

### Response

Contact the system administrator.

## JVS0403

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS0403 MRSCAT CONTAINS INCORRECT INFORMATION. COMMAND REJECTED

### Meaning

According to the MRSCAT (multiprocessor system catalog), a certain
catalog ID is available for remote access, which in actual fact it is not.

### Response

Contact the system administrator.

## JVS0404

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS0404 SYSTEM ERROR DURING JVS OPERATION: CATALOG MANAGEMENT ERROR. COMMAND REJECTED

### Meaning

Operating system error.
One of the specified path names contains the catalog ID of a remote
catalog which is in quiet mode. As it is not possible to place the
job in the wait state, the catalog cannot be accessed.

### Response

Inform the system administrator so that diagnostic material
can be generated.

## JVS0405

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS0405 SYSTEM ERROR DURING JVS OPERATION: MSCF COMMUNICATION ERROR. COMMAND REJECTED

### Meaning

Communication error.
An error has occurred in the MSCF communication facility when
accessing a remote catalog.

### Response

Request the system administrator to check the MSCF connection. If no
error can be found there, it must have been a temporary fault and
you should simply repeat the job.

## JVS0406

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS0406 CMS OPERATION ABORTED BY USER

### Meaning

The CMS was called while a master change was in progress.
The user did not want to wait with execution of the operation until
termination of the master change.

### Response

Release any existing locks. Try again later, if necessary.

## JVS0407

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS0407 CMS WRITE OPERATION NOT PROCESSED

### Meaning

The process of writing a catalog entry to the TSOSCAT has not been
executed because a master change was being processed.

### Response

If necessary repeat the aborted operation, including all previous
operations connected to it.

## JVS041F

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS041F SYSTEM ERROR DURING JVS OPERATION: CATALOG MANAGEMENT ERROR. COMMAND REJECTED

### Meaning

During a catalog operation an unrecoverable error occurred in CMS, which
normally terminates the task abnormally. Because the task concerned is the
JOIN task (TSN=RP01 or RP02) instead of the task the catalog operation is
aborted with this message.

## JVS0410

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS0410 A FUNCTION USED BY CATALOG MANAGEMENT REPORTS ERROR. PROCESSING ABORTED

### Meaning

Possible reasons:
- conversion between the old and the new catalog format could not be
processed.
- error during processing of the TASKLIST on the slave host in the
shared PVS network.
- error during processing of internal tables in MSCF processing.

### Response

Try function again. If the error occurs again contact the system
administrator.

## JVS0412

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0412 REQUESTED CATALOG NOT FOUND. COMMAND REJECTED

### Meaning

One of the specified path names contains the catalog ID of a catalog which
does not have an entry in the MRSCAT (multiprocessor system catalog).

### Response

Possible responses:
- Check the contents of the entries in the MRSCAT and then repeat the
JV command.
- Request the system administrator to enter the required catalog ID
in the MRSCAT.

## JVS042C

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS042C SYSTEM ERROR DURING JVS OPERATION: PAM ERROR. COMMAND REJECTED

### Meaning

Operating system error.
The request is illegal (e.g. invalid number or page parameter, or
page parameter specified by class 2 program).

### Response

Inform the system administrator so that diagnostic material can
be generated.

## JVS042D

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS042D SYSTEM ERROR DURING JVS OPERATION. PPAM HAS PASSED TO UPAM: 'WAIT' AND 'CONTINGENCY' REQUESTED

### Meaning

Operating system error.

### Response

Contact the system administrator and request diagnostic material,
if necessary.

## JVS042F

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS042F SYSTEM ERROR DURING JVS OPERATION: RESIDENT PAGE SPACE EXHAUSTED. COMMAND REJECTED

### Meaning

Operating system error.
A class 2 program has attempted to create more resident
pages than were reserved at execution time.

### Response

Inform the system administrator so that diagnostic material
can be generated.

## JVS0422

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS0422 SYSTEM ERROR DURING JVS OPERATION: CATALOG MANAGEMENT ERROR. COMMAND REJECTED

### Meaning

Operating system error.
The requested logical half-page is not available for the job variable.

### Response

Inform the system administrator so that diagnostic material can
be generated.

## JVS0423

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS0423 SYSTEM ERROR DURING JVS OPERATION: PAM ERROR. COMMAND REJECTED

### Meaning

Operating system error.
CMS has attempted to change the status of a page not assigned to CMS.

### Response

Inform the system administrator so that diagnostic material can
be generated.

## JVS0424

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS0424 SYSTEM ERROR DURING JVS OPERATION: SYSTEM ADDRESS SPACE EXHAUSTED. COMMAND REJECTED

### Meaning

Operating system error.
CMS has requested more contiguous memory than is currently available.

### Response

Repeat the command after a short interval.
Inform the system administrator so that diagnostic material can
be generated.

## JVS0425

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS0425 SYSTEM ERROR DURING JVS OPERATION: CATALOG MANAGEMENT ERROR. COMMAND REJECTED

### Meaning

Operating system error.
Possible errors:
- CMS issued a command which DQPAM did not recognize
- DQPAM requested an illegal function.

### Response

Inform the system administrator so that diagnostic material can
be generated.

## JVS0426

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS0426 SYSTEM ERROR DURING JVS OPERATION: CATALOG MANAGEMENT ERROR. COMMAND REJECTED

### Meaning

Operating system error.
DQPAM has detected a buffer address that crosses a page boundary
and is therefore not permitted.

### Response

Inform the system administrator so that diagnostic material can
be generated.

## JVS0427

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS0427 SYSTEM ERROR DURING JVS OPERATION: PAM ERROR. COMMAND REJECTED

### Meaning

Operating system error.
DQPAM detected an I/O error while performing the requested function.

### Response

Inform the system administrator so that diagnostic material can
be generated.

## JVS0428

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS0428 SYSTEM ERROR DURING CATALOG ACCESS DUE TO INVALID DEVICE ACCESS AUTHORIZATION

### Meaning

PPAM has detected that a disk access function was called by catalog
management with an invalid device access authorization.

### Response

Contact the system administrator and request diagnostic material,
if necessary.

## JVS0429

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS0429 SYSTEM ERROR DURING JVS OPERATION: PAM ERROR. COMMAND REJECTED

### Meaning

Operating system error.
DQPAM has detected an invalid SLOT address.

### Response

Inform the system administrator so that diagnostic material can
be generated.

## JVS043B

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS043B SYSTEM ERROR DURING JVS OPERATION: CATALOG MANAGEMENT ERROR. COMMAND REJECTED

### Meaning

Operating system error.
The routine for the catalog access has returned an error in the lock
mechanism for the catalog entries.

### Response

Inform the system administrator so that diagnostic material can
be generated.

## JVS043C

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS043C NO MORE SPACE AVAILABLE FOR CATALOG FILE. COMMAND REJECTED

### Meaning

The user has not been allocated enough space. The routine for the
catalog access requires another catalog block, but the requested
catalog has reached its maximum size.

### Response

Request the system administrator to allocate additional space for the
catalog file.

## JVS043D

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS043D SYSTEM ERROR DURING JVS OPERATION: TSOSCAT DESTROYED. COMMAND REJECTED

### Meaning

Operating system error.
The structure of the job variable catalog entry is invalid.

### Response

Inform the system administrator so that diagnostic material can
be generated.

## JVS043E

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS043E JOB VARIABLE TO BE CREATED ALREADY EXISTS

## JVS0430

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0430 SYSTEM ERROR DURING JVS OPERATION: CATALOG MANAGEMENT ERROR. COMMAND REJECTED

### Meaning

Operating system error.
The routine for the catalog access requires more storage space than is
available ($GETMEM error).

### Response

Retry the JV command later.

## JVS0431

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0431 OPERAND ILLEGAL. CORRECT COMMAND

### Meaning

The JV command contains one of the following errors:
- invalid operand registers have been passed to CMS.
- general error in CMS.
Message DMS0331 lists further possible errors. Either enter
/HELP-MSG DMS0331 in system mode to request more detailed information
about the error or contact the system administrator.
Retry the command after LOGOFF BUT.

## JVS0432

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS0432 SYSTEM ERROR DURING JVS OPERATION: CATALOG MANAGEMENT ERROR. COMMAND REJECTED

### Meaning

Operating system error.
The catalog entry of the job variable is locked by another task.

## JVS0433

Destination: USER-TASK Routing code: Weight: 10

Warranty : NO

JVS0433 REQUESTED JOB VARIABLE NOT CATALOGED. COMMAND REJECTED

### Response

Use the CREATE-JV command to create the job variable.

## JVS0434

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0434 SYSTEM ERROR DURING JVS OPERATION: CATALOG MANAGEMENT ERROR. COMMAND REJECTED

### Meaning

Operating system error.

### Response

Retry the JV command later.

## JVS0435

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0435 JOB VARIABLE NOT ACCESSIBLE DUE TO ACTIVE JV PROTECTION. COMMAND REJECTED

### Meaning

The user attempted to access a job variable whose catalog entry
is inaccessible due to the current protection attributes.
One of the following protection mechanisms can be active:
- standard protection
- basic access control (BASIC-ACL)
- profile protection (GUARDS).

## JVS0436

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

JVS0436 SYSTEM ERROR DURING JVS OPERATION: CATALOG MANAGEMENT ERROR. COMMAND REJECTED

### Meaning

Operating system error.
The risk of a deadlock was recognized when attempting to lock a catalog
entry.

### Response

Inform the system administrator so that diagnostic material can be
generated.

## JVS0438

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0438 NOT MANY FREE BLOCKS LEFT FOR PVS ID IN CATALOG FILE 'TSOSCAT'

### Meaning

Only 5 to 7 catalog blocks are still available in TSOSCAT.

### Response

Request the system administrator to enlarge TSOSCAT accordingly by
means of the MODIFY-FILE-ATTRIBUTES command.

## JVS0439

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0439 NO FREE CATALOG BLOCKS LEFT FOR PVS ID IN CATALOG FILE 'TSOSCAT'

### Response

Request the system administrator to enlarge TSOSCAT accordingly by
means of the MODIFY-FILE-ATTRIBUTES command.

## JVS044A

Destination: USER-TASK Routing code: Weight:

Warranty : NO

JVS044A INVALID GUARD NAME SPECIFIED. COMMAND REJECTED

### Meaning

An invalid GUARD name has been detected during the syntax check.

## JVS044B

Destination: USER-TASK Routing code: Weight:

Warranty : NO

JVS044B INVALID MANAGEMENT CLASS SPECIFIED. COMMAND REJECTED

### Meaning

Possible reasons:
- the management class ist not accessible by the specified user,
- the management class is unknown in the pubset,
- the pubset is not a SM-pubset,
- the pubset is not accessible.

## JVS044C

Destination: USER-TASK Routing code: Weight:

Warranty : NO

JVS044C ACCESS TO RULE CONTAINER FOR DEFAULT PROTECTION COULD NOT BE EXECUTED. COMMAND REJECTED

### Meaning

Possible reasons:
- reading the standard protection rule is not possible, f.e. because
the catalog is not accessible.
- the guard, indicated in the standard protection rule, which contains
the attribute values respectively the list of user ID's, may not be
used according to the guard scope.
- internal error, the guard user is unknown to the GUARD access control.

### Response

If possible, change the access authorization accordingly.

## JVS0440

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0440 ILLEGAL JV NAME. CORRECT COMMAND

### Meaning

Possible errors:
- no JV name has been specified
- a foreign user ID has been specified (prerogative of the system
administrator)
- the coownership of the system administrator was restricted for this
job variable.
- the JV name contains illegal characters.

### Response

Correct the JV name and repeat the CREATE-JV or MODIFY-JV-ATTRIBUTES
command.

## JVS0441

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0441 NEW JV NAME ILLEGAL. CORRECT COMMAND

### Meaning

Possible errors:
- a user ID was specified which is not equal to the user ID of JV name
- a catalog ID was specified which is not equal to the catalog ID of JV
name
- the new JV name contains illegal characters.

### Response

Correct the new JV name and repeat the MODIFY-JV-ATTRIBUTES command.

## JVS0442

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0442 NEGATIVE RETENTION PERIOD. CORRECT COMMAND

### Meaning

The MODIFY-JV-ATTRIBUTES command is not permitted as a negative value
has been specified for the retention period.

## JVS0444

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0444 JV NAME OR NEW JV NAME ALREADY CATALOGED. COMMAND REJECTED

### Meaning

The attempt to catalog a job variable that is already cataloged
has been rejected.

### Response

Check the job variable status.

## JVS0445

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0445 INVALID RETENTION PERIOD SPECIFICATION. COMMAND REJECTED

### Meaning

Following error has occurred in the MODIFY-JV-ATTRIBUTES
command:
the retention period is errored; there is no creation date in
the catalog entry.

### Response

Check the job variable status.

## JVS0447

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0447 JV NAME BEING USED BY CJC FUNCTION. COMMAND REJECTED

### Meaning

The catalog entry of the job variable cannot be modified or deleted
as long as a CJC function (WAIT-EVENT, ADD-CJC-ACTION) is accessing
this job variable.
CJC: Conditional Job Control.

### Response

If necessary, repeat the command once the CJC function has stopped
accessing the job variable.

## JVS0448

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0448 MONITORING JOB VARIABLE MUST NOT BE CHANGED. COMMAND REJECTED

### Meaning

The MODIFY-JV-ATTRIBUTES command cannot be used as it is not permissible
to modify the name or attributes of a monitoring job variable.

## JVS0449

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0449 ONLY DEFAULT ATTRIBUTES PERMITTED FOR TEMPORARY JOB VARIABLE. COMMAND REJECTED

### Meaning

When creating temporary job variables, only the default protection
attributes can be used. These values cannot be modified.

### Response

Use the default values for all protection attributes of the temporary
job variable and then repeat the rejected command.

## JVS0451

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS0451 NO JV LINK TABLE ENTRY EXISTS

### Meaning

No JV link table entry has been made for requested job variable(s)
in this task.

## JVS0457

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

JVS0457 RELEASE ALL JV LINK NAMES OF THE TASK? REPLY (Y=YES; N=NO)

### Meaning

This question follows in connection with the command
REMOVE-JV-LINK LINK=*ALL and the user has the possibility to withdraw
the entered command.

## JVS0458

Destination: USER-TASK Routing code: Weight: 98

Warranty : NO

JVS0458 REQUEST FOR RELEASING ALL JV LINK NAMES WITHDRAWN BY CALLER

### Meaning

The JV link names of the task will not be released, because the request
for release was not confirmed.

## JVS046A

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS046A DELETE REQUEST WITHDRAWN BY CALLER

### Meaning

The request to delete a job variable or all job variables of a given
catalog ID or user ID was ignored as the caller did not confirm
the deletion request.

## JVS0460

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0460 DELETE COMMAND ILLEGAL AS JOB VARIABLE CATALOGED UNDER FOREIGN USER ID. COMMAND REJECTED

### Meaning

Only the owner of a job variable and the system administrator are
authorized to delete this JV.

### Response

Request the owner or system administrator to delete the job variable.

## JVS0463

Destination: USER-TASK, CONSOLE Routing code: R Weight: 30

Warranty : NO

JVS0463 WARNING: JVS ERROR '(&01)' WHEN DELETING JV '(&00)'. PROCESSING CONTINUES

### Meaning

During execution of the REMOVE-USER command an error has occurred
while deleting the job variable.

## JVS0464

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0464 WARNING: DELETE ERROR. '(&00)' STILL HAS CATALOG ENTRIES FOR JV. PROCESSING CONTINUES

### Meaning

The system administrator has attempted to delete the catalog entry of
user ID (&00) from the user catlog by means of the REMOVE-USER command.
In the process a fatal error occurred when deleting a job variable, with
the result that user ID (&00) is only locked instead of deleted.

### Response

Delete the relevant job variable and then repeat the REMOVE-USER command.

## JVS0465

Destination: USER-TASK Routing code: Weight: 90

Warranty : YES

JVS0465 DELETE ALL JOB VARIABLES '(&00)' OF USER ID? REPLY (Y=YES; N=NO; T=TERMINATE COMMAND; ?=EXPLAIN ADDITIONAL OPTIONS)

### Meaning

A partially qualified job variable name may cover more than one
job variable.
This message is displayed whenever the user ID is switched.

### Response

Reply T: Deletion is aborted as of the specified user ID.
Y: The deletion request is confirmed; the job variables are
deleted.
N: The job variables of the specified user ID are not deleted.
?: Explanations of the additional options will be displayed,
followed by renewed display of the task.
,CHECK=(SINGLE; MULTIPLE; PVS; NO):
The specifications in check mode correspond to the
DIALOG-CONTROL operand with the values JV-CHANGE (SINGLE),
USER-ID-CHANGE (MULTIPLE), CATALOG-CHANGE (PVS), NO.
Any other response is interpreted as 'N'.

## JVS0466

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0466 DELETION OF MONITORING JOB VARIABLE NOT PERMITTED. COMMAND REJECTED

### Response

Wait until the job variable is no longer being used as a monitoring job
variable.
If this message is issued even though the job variable to be deleted is
not being used as a monitoring job variable, the JV can be reset with
the aid of the MODIFY-JV-ATTRIBUTES (MONJV-PROTECTION operand).

## JVS0468

Destination: USER-TASK Routing code: Weight: 90

Warranty : YES

JVS0468 DELETE ALL JOB VARIABLES '(&00)' OF CATALOG ID? REPLY (Y=YES; N=NO; T=TERMINATE; ?=EXPLAIN ADDITIONAL OPTIONS)

### Meaning

A partially qualified job variable name may cover more than one
job variable. This message is displayed for each local catalog
of the system.

### Response

Reply T: Deletion is aborted as of the specified catalog ID.
Y: The deletion request is confirmed; the job variables are
deleted.
N: The job variables of the specified catalog are not
deleted.
?: Explanations of the additional options will be displayed,
followed by renewed display of the task.
,CHECK=(SINGLE; MULTIPLE; PVS; NO):
The specifications in check mode correspond to the
DIALOG-CONTROL operand with the values JV-CHANGE (SINGLE),
USER-ID-CHANGE (MULTIPLE), CATALOG-CHANGE (PVS), NO.
Any other reply is interpreted as 'N'.

## JVS0469

Destination: USER-TASK Routing code: Weight: 90

Warranty : YES

JVS0469 DELETE JOB VARIABLE '(&00)'? REPLY (Y=YES; N=NO; T=TERMINATE; ?=EXPLAIN ADDITIONAL OPTIONS)

### Meaning

Check mode 'CHECK=SINGLE' has been set. This means that the deletion
request has to be confirmed separately for each job variable.

### Response

Reply T: Deletion is aborted as of the specified job variable.
Y: The deletion request is confirmed; the job variable is deleted.
N: The job variable is not deleted.
?: Explanations of the additional options will be displayed,
followed by renewed display of the task.
,CHECK=(SINGLE; MULTIPLE; PVS; NO):
The specifications in check mode correspond to the
DIALOG-CONTROL operand with the values JV-CHANGE (SINGLE),
USER-ID-CHANGE (MULTIPLE), CATALOG-CHANGE (PVS), NO.
Any other reply is interpreted as 'N'.

## JVS0470

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS0470 WARNING: JV VALUE CONTAINS FEWER BYTES THAN REQUESTED. PROCESSING CONTINUES

### Meaning

The output job variable value contains fewer characters than were
requested by the substring specification in the SHOW-JV command.

## JVS0471

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS0471 SPECIAL JOB VARIABLE '$SYSJV.LAST-MSG' NOT ACCESSIBLE. COMMAND REJECTED

### Meaning

The contents of special job variable SYSJV.LAST-MSG could not be
output by means of the SHOW-JV command.
Possible reasons:
1) The command was issued in interactive mode, which is not permitted.
2) An operating system error has occurred.

### Response

1) Repeat the command in procedure or batch mode.
2) Inform the system administrator so that diagnostic material
can be generated.

## JVS0472

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0472 NAME OF SPECIAL JOB VARIABLE NOT PERMITTED. CORRECT COMMAND

### Meaning

The name of the special job variable specified in the SHOW-JV command
is illegal.
Permissible names for special job variables can either be output by the
system using the command SHOW-JV-ATTRIBUTES $SYSJV.
or looked up in the "Job Variables" manual.

## JVS0474

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS0474 WARNING: JV VALUE TRUNCATED. PROCESSING CONTINUES

### Meaning

An error has occurred while processing the SHOW-JV command. As the
value of the job variable is greater than the specified substring
specification, it has been truncated on the right.

## JVS0480

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0480 SPECIAL JOB VARIABLE MUST NOT BE SET. COMMAND REJECTED

### Meaning

The MODIFY-JV command must not be used here as special job variables
can only be accessed in read mode.

## JVS0487

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

JVS0487 SYSTEM PART OF MONITORING JOB VARIABLE IS WRITE-PROTECTED. COMMAND REJECTED

### Meaning

The MODIFY-JV command has been rejected as it is not permitted to
modify the first 128 bytes of a monitoring job variable.

## JVS14A4

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS14A4 CATALOG INDEX AT MAXIMUM SIZE

### Meaning

Request the system administrator to erase files or JVs that are no
longer required.

### Response

Files and JVs, that are no longer required should be erased by the
system administrator.

## JVS14A5

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

JVS14A5 CATALOG INDEX DESTROYED

### Meaning

The CMS operation cannot be executed because the catalog index of the
specified SM pubset is destroyed.

### Response

Retry, as the catalog index may be reconstructed in the meantime.
Reconstruction will be performed during the next IMPORT-PUBSET at the
latest.

©2024 Fujitsu | BS2000 System Messages