## DCA0D02

Destination: CONSOLE Routing code: C Weight: 99

Warranty : NO

DCA0D02 FORCED CLOSURE OF APPLICATION (&00)

### Meaning

Due to a system error a forced closure was performed for the application
with the symbolic name (&00). The user task is continued.

### Response

None.

## DCA0D03

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCA0D03 DCS DUMP INITIATED. WAIT FOR TERMINATION OF DUMP.

### Meaning

A system error is detected by DCAM. A DCS DUMP is caused.
The user task is continued after dump has been issued.

### Response

None.

## DCA0D04

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCA0D04 DCS DUMP TERMINATED. YOUR TASK IS CONTINUED

### Meaning

A DCS DUMP was issued. The user task is continued now.

### Response

None.

## DCA0D05

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCA0D05 NO MORE P1-PCB'S AVAILABLE FOR THIS TASK.

### Meaning

The number of P1-PCB's for one task is limited by P1-Eventing.
DCAM is unable to start a contingency.

### Response

None.

## DCA0D06

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCA0D06 CONTROLBLOCK-SERVICES IN P1 WERE WITHDRAWN WITH DCAM V8.0.

### Meaning

This function is no more available. Static controlblocks and dsects
may be used instead.

### Response

None.

## DCA0F01

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCA0F01 INSUFFICIENT MEMORY AVAILABLE. COMMAND TERMINATED

### Meaning

REQM error. Not enough memory available for link entries.

### Response

Repeat command.

## DCA0F02

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCA0F02 INSUFFICIENT MEMORY AVAILABLE. COMMAND TERMINATED

### Meaning

REQM error. Not enough memory available for name manager.

### Response

Repeat command.

## DCA0F03

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCA0F03 NO SUCH LINK NAME. COMMAND TERMINATED

### Meaning

No link entry exists with the given link name.

### Response

None.

## DCA0F04

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCA0F04 INTERNAL RETURN CODE OUT OF RANGE. COMMAND TERMINATED

### Meaning

REQM return code greater than 4.

### Response

Get memory dump, write error message

## DCA0F05

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCA0F05 INTERNAL RETURN CODE OUT OF RANGE. COMMAND TERMINATED

### Meaning

Name manager sets return code greater than 8 (ENABLE) or greater than 0
(SETDI).

### Response

Get memory dump, write error message.

## DCA0F06

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCA0F06 INVALID PARAMETER VALUE. COMMAND TERMINATED

### Meaning

Given parameter is invalid.

### Response

Repeat command with correct parameter.

## DCA0F07

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCA0F07 INVALID PARAMETER KEYWORD. COMMAND TERMINATED

### Meaning

Invalid keyword has been used.

### Response

Repeat command with correct keyword.

## DCA0F08

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCA0F08 LINK PARAMETER MISSING. COMMAND TERMINATED

### Meaning

Obligatory keyword LINK is missing.

### Response

Repeat command with LINK keyword.

## DCA0F09

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DCA0F09 SS DCAM NOT AVAILABLE

### Meaning

The DCAM Subsystem was not created properly.

### Response

Make sure the DCAM Subsystem is created.

©2024 Fujitsu | BS2000 System Messages