# SVR

## SVR0000

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0000 (&00) started with device (&01), console (&02), BS2-Sys (&03)

### Meaning

&00 = IPL, DIPL or VIPL
The IPL has been started. BS2000 is loaded from device &01, &02 is defined as the
console, and &03 is used as the BS2000 system name.

## SVR0001

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0001 (&00) returncode: IPL OK

### Meaning

&00 = IPL, DIPL or VIPL
IPL was performed without errors. BS2000 has been started.

## SVR0002

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0002 (&00) returncode: (&01)

### Meaning

&00 = IPL, DIPL or VIPL IPL was aborted with an error (&01 = cause of error).

### Response

Eliminate the error and recommence IPL.

## SVR0003

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0003 unknown (&00) returncode: (&01)

### Meaning

&00 = IPL, DIPL or VIPL, &01 = Return code IPL was aborted with an unspecified error code.

### Response

Back up the RMAssist Trace and send it to the Support Center for diagnosis
(var/opt/SMAW/X2000/tmp/rma_trace*) or create new diagnostic data via the SEM.

## SVR0004

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0004 START-(&00) aborted

### Meaning

&00 = IPL, DIPL or VIPL The IPL has been aborted.

### Response

Recommence IPL. If this does not help, reboot the system.

## SVR0005

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0005 START-(&00) aborted ((&01))

### Meaning

&00 = IPL, DIPL or VIPL
IPL was aborted with errors (&01 = cause of error).

### Response

Recommence IPL. If this does not help, eliminate the errors. A reboot of the system may suffice.

## SVR0006

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0006 invalid command (&00)

### Meaning

&00 = incorrect RMAssist command
An incorrect command was entered.

### Response

Notify Customer Support.

## SVR0007

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0007 WARNING: Console device for IPL with VMID=(&00) cannot be checked

### Meaning

The specified VMID is wrong or is not configured.

### Response

Enter the right VMID.

## SVR0008

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0008 (&00) started

### Meaning

&00 = IOHDUMP or IVMDUMP
IOHDUMP or IVMDUMP has been started.

## SVR0010

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0010 WARNING: IPL INFO FOR VMID (&00) cannot be written - IPL continues"

### Meaning

The info file with the IPL data could not be written.

## SVR0011

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0011 NO IPL - bs2000 guest system in hold state

### Meaning

The BS2000 guest system is in the STOP status.

### Response

Re-initialize and start the guest system.

## SVR0012

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0012 IOHDUMP=(&00)

### Meaning

IOHDUMP &00 is created.

## SVR0013

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0013 IOHDUMP finished: OK

### Meaning

IOHDUMP has been completed.

## SVR0015

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0015 IOHDUMP finished with error

### Meaning

Generation of the IOHDUMP was not completed.

### Response

Repeat IOHDUMP

## SVR0016

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0016 IVMDUMP=(&00)

### Meaning

IVMDUMP &00 is being generated.

## SVR0017

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0017 IVMDUMP ist fertiggestellt

### Meaning

IVMDUMP &00 is being generated.

## SVR0018

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0018 IVMDUMP finished with error

### Meaning

IVMDUMP was not completed.

## SVR0040

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0040 MDEBUG is running - no action

### Meaning

The mdebug program is loaded. The specified command is not executed.

### Response

Terminate the mdebug program.

## SVR0042

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0042 (&00)-Parameter error - no start of IPL

### Meaning

&00 = IPL, DIPL or VIPL
An incorrect parameter was entered in the IPL.

### Response

Enter the parameter/data correctly.

## SVR0048

Destination: CONSOLE (message is issued without MIP, in English only)

Warranty : NO

SVR0048 error by SLED DUMP

### Meaning

An error occurred when generating or writing a SLED DUMP.

### Response

Repeat the DIPL.

©2024 Fujitsu | BS2000 System Messages