## ETMAC01

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ETMAC01 Output information incomplete

## ETMAC02

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ETMAC02 No entries in the ACF-trace-table

## ETMAC03

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ETMAC03 Requested task not active

## ETMAC04

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ETMAC04 Invalid parameter combination; task=*all only supported for state=*tp

## ETMBC00

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMBC00 SYSTEM ERROR ETMBC00 TERMINATED SESSION; ***SSSTACON: ERROR FOR "GET M-LOCK"***

### Meaning

The M-Lock is used to ensure that code accessing internal data of the
bourse mechanism (which supports serialisation) runs uninterruptible
under a single task. If an attempt to get the M-Lock failed, a system
error has occurred and the session is terminated.

### Response

Take SLED and send it to your systems engineer.

## ETMBC01

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMBC01 SYSTEM ERROR ETMBC01 TERMINATED SESSION; ***ETMBON1: ERROR FOR "GET I-LOCK"***

### Meaning

The I-Lock is used to ensure that code accessing internal data of the
FITC mechanism (Fast Inter-Task Communication) runs uninterruptible
under a single task. If an attempt to get the I-Lock failed, a system
error has occurred and the session is terminated.

### Response

Take SLED and send it to your systems engineer.

## ETMBC02

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMBC02 SYSTEM ERROR ETMBC02 TERMINATED SESSION; ***ETMBON1: ERROR FOR "RELEASE I-LOCK"***

### Meaning

The I-Lock is used to ensure that code accessing internal data of the
FITC mechanism (Fast Inter-Task Communication) runs uninterruptible
under a single task. If an attempt to release the I-Lock failed, a
system error has occurred and the session is terminated.

### Response

Take SLED and send it to your systems engineer.

## ETMBC03

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMBC03 SYSTEM ERROR ETMBC03 TERMINATED SESSION; ***SSSTACON: ERROR ON "RELEASE M-LOCK"***

### Meaning

A request was made to release the M-Lock when it was not held.

### Response

Take SLED and send it to your systems engineer.

## ETMBC04

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMBC04 SYSTEM ERROR ETMBC04 TERMINATED SESSION; ***SSSTACON: SYNCHRONOUS INTERRUPT WHILE M-LOCK WAS HELD***

### Response

Take SLED and send it to your systems engineer.

## ETMBC05

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMBC05 SYSTEM ERROR ETMBC05 TERMINATED SESSION; *** ETMCON2: ERROR WHILE SCHEDULING A TPR-CONTINGENCY ***

### Meaning

During scheduling of a TPR-contingency an invalid function
was specified within the system table XVT.

### Response

Take SLED and send it to your systems engineer.

## ETMBC06

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMBC06 SYSTEM ERROR ETMBC06 TERMINATED SESSION; *** ETMBON1: INVALID FLAG DETECTED IN BOURSE PEND ROUTINE ***

### Meaning

The Bourse Pend routine was called to handle an
invalid wait state.

### Response

Take SLED and send it to your systems engineer.

## ETMBC10

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMBC10 SYSTEM ERROR ETMBC10 TERMINATED TASK; ***ETMCON1: INCORRECT $UNMASK***

### Meaning

A TPR PCB-run may not be masked down to a level which is lower than
that of an interrupted PCB-run.

### Response

Take DUMP and send it to your systems engineer.

## ETMBS01

Destination: USER-TASK, CONSOLE Routing code: A Weight: 79

Warranty : NO

ETMBS01 INSTRUCTION-SIMULATION FOR PRIVILEGED INSTRUCTION

### Meaning

One of the following instructions was used in the TU-program:
LWI, STWI, LBF, STBF or PUSH and POP.

### Response

As support for the simulation of these instructions may be withdrawn
in the future, the instructions should not be used.

## ETMCC00

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMCC00 SYSTEM ERROR ETMCC00 TERMINATED SESSION; UNEXPECTED ACKNOWLEDGEMENT

### Meaning

The system was terminated because the inter-logical machine processing
received an acknowledgement when none was expected.

### Response

If necessary take SLED and send it to your systems engineer.

## ETMDR01

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMDR01 Dynamic reconfiguration with function '(&00)' started

### Meaning

(&00): Function ADD, REMOVE or MIGRATE.

## ETMDR02

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMDR02 Dynamic reconfiguration with function '(&00)' finished

### Meaning

(&00): Function ADD, REMOVE or MIGRATE.

## ETMDR03

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMDR03 Live Migration from source configuration '(&00)' to target configuration '(&01)' finished. Initial configuration was '(&02)'

### Meaning

(&00), (&01), (&02): Configuration name.

## ETMDR04

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMDR04 Dynamic Reconfiguration with function '(&00)' rejected. Reason: Cluster Recovery Lock not obtained from MSCF

### Meaning

(&00): function ADD, REMOVE or MIGRATE.

### Response

Call system service.

## ETMDR05

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMDR05 Dynamic Reconfiguration with function '(&00)' rejected. Reason: At least one Extra-CPU attached

### Meaning

(&00): function REMOVE.

### Response

Detach all attached Extra-CPU's by command
/DETACH-DEVICE *EXTRA-CPU(*ALL).

## ETMDR10

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ETMDR10 Dynamic reconfiguration aborted with error. Reason: '(&00)'

### Meaning

(&00): The reason for abortion is for system diagnosis only.

## ETMEV01

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMEV01 SYSTEM ERROR ETMEV01 TERMINATED TASK; ***ETCONP1: WRONG INFORMATION CODE FROM NAME MANAGER***

### Meaning

The Name Manager passed an invalid value to the routine ETCKILL,
which destroys all TU-Contingencies during (normal) task termination.

### Response

Take systemdump and send it to your systems engineer.

## ETMEV02

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMEV02 SYSTEM ERROR ETMEV02 TERMINATED TASK; ***ETCONP1: PROHIBITED RETURN CODE OCCURRED***

### Meaning

One of the following functions lead to task termination:
- Request for class-4/5-memory failed.
- Release of class-4/5-memory failed.
- Enabling of a dummy name by the name manager was rejected.

### Response

Take systemdump and send it to your systems engineer.

## ETMEV03

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMEV03 USER ERROR ETMEV03 TERMINATED PROGRAM; ***ETCONP1: RETCO/EXIT ON BASE PROCESS!***

### Meaning

A TU-program was terminated because the program called the macro
RETCO or EXIT (STXIT) although the program was not in a contingency
but rather in the base process.

### Response

Please correct your program.

## ETMEV04

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMEV04 USER ERROR ETMEV04 TERMINATED PROGRAM; ***ETCONP1: RETCO IN STXIT-CONTINGENCY!***

### Meaning

A TU-program was terminated because the RETCO-macro was called within a
STXIT-contingency. STXIT-contingencies must be closed by calling the
EXIT-macro.

### Response

Please correct your program.

## ETMEV10

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMEV10 SYSTEM ERROR ETMEV10 TERMINATED TASK; ***ETSIDRI: PROHIBITED RETURN CODES OCCURRED***

### Meaning

One of the following errors in serialisation processing lead to
task termination:
1. Prohibited return code from the parameter processor.
2. Prohibited return code from the name manager.
3. Prohibited return code from the routines: creating or scheduling
of TU-PCB's
4. Prohibited return code from the bourse macro-calls.
5. Prohibited return code from Release-Memory.
6. Prohibited return code from $ENQL-macro-call.

### Response

Take Systemdump and send it to your systems engineer.

## ETMEV11

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMEV11 SYSTEM ERROR ETMEV11 TERMINATED TASK; ***ETSILIST: WRONG HANDLING IN $ENQL-MACRO***

### Meaning

The system error was caused by either
1. Wrong use of the $ENQL-parameter, or
2. Prohibited return code from a bourse-macro-call.

### Response

Take systemdump and send it to your systems engineer.

## ETMEV20

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMEV20 SYSTEM ERROR ETMEV20 TERMINATED STEP; ***ETEIDRI: PROHIBITED RETURN CODE FROM NAME MANAGER***

### Meaning

A prohibited return code occurred when enabling names,
setting name-specific values, accessing a name or
disabling a name.

### Response

Take systemdump and send it to your systems engineer.

## ETMEV21

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMEV21 SYSTEM ERROR ETMEV21 TERMINATED STEP; ***ETEIDRI: PROHIBITED RETURN CODE FROM PARAMETER PROCESSOR***

### Meaning

The Parameter Processor produced a return code which indicates a system
error.

### Response

Take systemdump and send it to your systems engineer.

## ETMEV22

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMEV22 SYSTEM ERROR ETMEV22 TERMINATED STEP; ***ETEIDRI: PROHIBITED RETURN CODE FROM BOURSE MACRO CALL***

### Meaning

The bourse macro call produced a return code which indicates a system
error.

### Response

Take systemdump and send it to your systems engineer.

## ETMEV23

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMEV23 SYSTEM ERROR ETMEV23 TERMINATED STEP; ***ETEIDRI: PROHIBITED RETURN CODE FROM FITC***

### Meaning

The FITC-connection-routine produced a return code which indicates a
system error.

### Response

Take systemdump and send it to your systems engineer.

## ETMEV24

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMEV24 System error ETMEV24 terminated step;***ETEIDRI: unexpected return code of an internal procedure*****

### Meaning

One of the the routines responsible to initiate the wait state for a
synchronous SOLSIG request or to schedule a TU-contingency for an
asynchronous SOLSIG request provides an illegal returncode.

### Response

Please take systemdump and send it to your systems engineer.

## ETMEV25

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMEV25 SYSTEM ERROR ETMEV25 TERMINATED TASK; ***UEV/SER/FEV/CO: INDICATION OF SYSTEM INCONSISTENCE***

### Meaning

The call of an external system interface supplies an unexpected return
code.

### Response

Take systemdump and send it to your systems engineer.

## ETMEV26

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMEV26 User error ETMEV26 terminated program; ***ETEIDRI: maximum of allowed TU-contingencies reached***

### Meaning

Upon the occurrence of an event which was requested by a permanent
asynchronous SOLSIG request, the limit for TU-contingencies has been
reached. Therefore the user program is terminated.
This situation may occur when the TU-basis process cannot be
interrupted by the TU-contingency because it has increased its priority
by means of LEVCO to a higher value than the TU-contingency. Another
reason may be that during a wait state of a TU-contingency new events
are scheduling too many TU-contingecies.

### Response

Please correct your program.

## ETMEV30

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMEV30 SYSTEM ERROR ETMEV30 TERMINATED STEP; ***ETCODRI: PROHIBITED RETURN CODE FROM NAME MANAGER***

### Meaning

A prohibited return code occurred when enabling names, setting
name-specific values, accessing a name or disabling a name. The
return code indicates an error in the operating system.

### Response

Take systemdump and send it to your systems engineer.

## ETMEV31

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMEV31 SYSTEM ERROR ETMEV31 TERMINATED STEP; ***ETCODRI: PROHIBTED RETURN CODE FROM PARAMETER PROCESSOR***

### Meaning

The Parameter Processor produced a return code which indicates a system
error.

### Response

Take systemdump and send it to your systems engineer.

## ETMEV40

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMEV40 SYSTEM ERROR ETMEV40 TERMINATED TASK; ***ETMEVSP: PROHIBITED RETURN CODE OCCURRED***

### Meaning

Enabling of a dummy name by the Name Manager was rejected.

### Response

Take systemdump and send it to your systems engineer.

## ETMFE01

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMFE01 SYSTEM ERROR ETMFE01 TERMINATED TASK; ***ETMFEV: ERROR IN SVC 187-ROUTINE***

### Meaning

Possible reasons are invalid return codes from $RQM1, $RLM1,
Parameter Processor, Name Manager etc.

### Response

Take Systemdump and send it to your systems engineer.

## ETMFE02

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMFE02 SYSTEM ERROR ETMFE02 TERMINATED TASK; ***ETMFEV: ERROR ON DELETING FEV-ITEMS***

### Meaning

Invalid return code from $RLM1.

### Response

Take Systemdump and send it to your systems engineer.

## ETMFI01

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMFI01 SYSTEM ERROR ETMFI01 TERMINATED TASK; ***ITC: UNEXPECTED RETURN CODE!***

### Meaning

Invalid return code from Inter-Task Communication.

### Response

Take system dump and send it to your systems engineer.

## ETMFI02

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMFI02 SYSTEM ERROR ETMFI02 TERMINATED TASK; ***FITC: UNEXPECTED RETURN CODE!***

### Meaning

Invalid return code from Fast Inter-Task Communication.

### Response

Take system dump and send it to your systems engineer.

## ETMGT00

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT00 CREATION OF SUBSYSTEM GET-TIME FAILED

### Meaning

DSSM reports error at creation of GET-TIME subsystem.
Functions GTIME/CTIME for user programs not supported.
A subsequent start of the subsystem is not possible.

### Response

The system has to be restarted (STARTUP).

## ETMGT01

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT01 TODR-EPOCH FOR SESSION: EPOCH=(&00)

### Meaning

Display of the Epoch Designation.

### Response

None.

## ETMGT02

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT02 CONNECTION TO SUBSYSTEM GET-TIME FAILED

### Meaning

Initialisation of subsystem GET-TIME cannot be performed.
Functions GTIME/CTIME for user programs not supported.
A subsequent start of the subsystem is not possible.

### Response

The system has to be restarted (STARTUP).

## ETMGT07

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT07 DIFF IN PARAM FILE MISSING - STARTUP TERMINATED

### Meaning

The GTIME parameter DIFF is missing.
STARTUP is terminated.

### Response

The STARTUP parameter must be corrected.

## ETMGT10

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT10 GTIME-VALUES FOR SESSION: ZONE=(&00), DIFF=(&01)

### Meaning

The parameters for the GTIME-functions have the following values:
&00: local time-zone
&01: time difference for changing the clock

### Response

None.
If DIFF<>0, i.e. there is a conversion to daylight saving time,
but neither SEASON nor CHDATE is given, the message ETMGT17 will
follow next.
If the values of ZONE and / or DIFF have changed since the last
BS2000-session, the dialog with the console will follow with the
messages ETMGT11 and ETMGT12; should the occasion arise, the
messages ETMGT13 and ETMGT14, too.

## ETMGT11

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT11 DIFF OR ZONE HAS CHANGED SINCE LAST SESSION

### Meaning

The values of DIFF and / or ZONE have changed since the last
BS2000-session.

### Response

The question ETMGT12 is following.

## ETMGT12

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT12 DO YOU ACCEPT CURRENT PARAMS DIFF AND ZONE? REPLY (Y/N)

### Meaning

The operator has to prove the possibility whether the
GTIME-parameter ZONE and / or DIFF have changed actually
because ZONE and DIFF are changing only in special circumstances.

### Response

The message ETMGT13 follows in case of syntactically false
input at the console.
In case of 'Y' STARTUP continues with the new GTIME-values;
False GTIME-parameters can lead to failures.
In case of 'N' the message ETMGT14 is following.

## ETMGT13

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT13 ILLEGAL REPLY

### Meaning

The answer concerning the message before was wrong.

### Response

The message follows once more.

## ETMGT14

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT14 GTIME-PARAMS DIFF OR ZONE MUST BE CORRECTED - STARTUP TERMINATED

### Meaning

The message ETMGT12 was answered with 'N', the parameter
DIFF and / or ZONE was changed wrongly.

### Response

The GTIME-parameter must be corrected, and after that STARTUP again.

## ETMGT15

Destination: CONSOLE Routing code: E Weight: 99

Warranty : NO

ETMGT15 NO CHDATE FOR THE LAST SEASON CHANGE EXISTS IN THE GTIME PARAMETER DECLARATIONS. REPLY(EOT(CONTINUE WITH WRONG TIME VALUES); T(TERMINATE)).

### Meaning

EXTEND THE GTIME PARAMETER FILE WITH ADDITIONAL
CHDATES AND INITIATE THEN A NEW STARTUP. REASON: THE ACTUAL
SESSION HAS NO INFORMATION ABOUT THE LAST SEASON CHANGE.
THEREFORE TIME ASCERTAINMENTS AND TIME CALCULATIONS
CAN LEAD TO WRONG RESULTS.

## ETMGT17

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT17 SEASON AND CHDATE MANDATORY IF DIFF<>0 - STARTUP TERMINATED

### Meaning

There is a conversion to daylight saving time but the
GTIME-parameters SEASON or CHDATE are invalid.

### Response

Startup of the system is terminated. The STARTUP-parameters
must be corrected.

## ETMGT18

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT18 FUTURE CHDATE MISSING. EXTEND CHDATE LIST AND REPEAT STARTUP BEFORE NEXT SEASON CHANGE!

### Meaning

The last date for changing the clock is already past.

### Response

The CHDATEs must be checked, because the specified parameters will be
invalid in about 6 months at the latest.

## ETMGT30

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT30 NO ZONE DIFFERENCE FROM SVP/IPL AND MORE THAN ONE GTIME ZONE IN PARAM FILE

### Meaning

It is not possible to determ a unique zone for system run.
The param file contains information about several zones, but in SVP
no zone is specified and in the SVL no zone is saved.

### Response

The message ETMGT31 is following.

## ETMGT31

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT31 ENTER ZONE OR TERMINATE STARTUP: ZONE=? (SHH:MM (S:SIGN, HH:HOURS, MM: MINUTES); T(ERMINATION))

### Meaning

The zone difference has to be input.

### Response

In case of wrong answer the message ETMGT32 is following.
To avoid this error, reduce the param file with informations about all
time zones to one only with informations about the currently needed, or
adjust the zone at SVP.

## ETMGT32

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT32 INCORRECT ZONE DIFFERENCE. CORRECT INPUT: ZONE=? (SHH:MM; T(ERMINATION))

### Meaning

The zone difference given with ETMGT31 is wrong.

### Response

The operator has to give the correct zone difference as input.
In case of incorrect input the message ETMGT32 is repeated until
a correct answer is given or termination is choosed.

## ETMGT33

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT33 INCORRECT DIFFERENCE BETWEEN TWO CHDATES. ACTION=? (C(ORRECT); I(GNORE); A(IGNORE ALL FOLLOWING PARAMS); T(ERMINATE))

### Meaning

The desired difference between two CHDATEs is not correct.
Either the param file contains errors or the paramfile has been
specified more than one time in Startup dialog.

### Response

The following run can be controlled by the answer.
It is possible to correct (C) or ignore (I) this current CHDATE,
to ignore all (A) following params or to terminate (T) the Startup.
In case of repeated specification of paramfile in Startup dialog it
is recommended to ignore all following params.

## ETMGT34

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT34 WARNING! MORE THAN ONE GTIME PARAM BLOCK FOR SELECTED ZONE IN PARAM FILE. PLEASE CHECK PARAM FILE!

### Meaning

One more param block containing information about the zone of the system
has been found in the param file.

### Response

This message is a warning for the user, that his param file contains
errors. It is recommended to check the param file.

## ETMGT35

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT35 NO GTIME PARAMETER ZONE FROM SVP/IPL/INPUT. CONTINUE WITH DEFAULT INITIALISATION? REPLY (Y/N)

### Meaning

No GTIME params were found according zone difference of
SVP/IPL/input of operator.

### Response

Message ETMGT36 is following.

## ETMGT36

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT36 REPLY (Y (WITH ZONE FROM SVP/SVL/INPUT); N (TERMINATE); SHH:MM (ZONE FOR INIT; S:SIGN, HH:HOURS, MM:MINUTES))

### Meaning

This message follows ETMGT35.

### Response

Complete GTIME param file or set correct zone difference in SVP for
next Startup.
You can take a default initialisation to correct the param file. In this
case there are no CHDATEs in the system. The zone information is taken
from SVP/SVL/operator input. In case of explicite input of zone
information a initialisation with this zone can be performed.

## ETMGT37

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT37 GTIME INITIALISED WITH DEFAULT PARAMS! PLEASE REPAIR PARAM FILE AND TERMINATE SESSION!

### Meaning

This system run should only be used to correct the param file.

## ETMGT38

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT38 SEASON OF STARTUP IS NOT UNIQUE

### Meaning

The startup happened in the ambiguous time of changing the season by
turning the clock back.

### Response

Message ETMGT39 is following.

## ETMGT39

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT39 DAYLIGHT SAVING TIME (SUMMER) OR STANDARD TIME (WINTER) IN SVP CLOCK AT STARTUP BEGIN? REPLY (DST (DAYLIGHT SAVING TIME); ST (STANDARD TIME))

### Meaning

It is not possible to decide, wether the Startup has been started at
daylight saving time or standard time. An input of the operator is
necessary.

### Response

Input of the operator, with which time the SVP clock (daylight saving time
or standard time) was loaded when Startup began.

## ETMGT40

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT40 CREATION OF SYSTEM TASK "TIME" FAILED. AUTOMATIC SEASON CHANGE OR CLOCK SYNCHRONISATION NOT POSSIBLE!

### Meaning

A consistent system run can only be guaranteed until the
next season change.
Synchronsation of system clock with external time servers are
not performed.
Diagnose data are generated automatically.

### Response

The system has to be restarted before season change (STARTUP).
To make possible clock synchronisation the system has to be restarted
(STARTUP).

## ETMGT41

Destination: USER-TASK Routing code: Weight:

Warranty : NO

ETMGT41 /390-Server: No synchronization of the system time by means of SKP-X/MU-Clock. x86-Server: No delivery of time quality to user of GTIME.

### Meaning

- Creation of supporting task TIMC terminated abnormally.
- No access to corresponding data of SKP-X/MU.
- No access to corresponding data of BS2-CONN-EXT-REF.

## ETMGT42

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT42 *** TIME HAS CHANGED FROM DAYLIGHT SAVING TIME TO STANDARD TIME ***

## ETMGT43

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT43 *** TIME HAS CHANGED FROM STANDARD TIME TO DAYLIGHT SAVING TIME ***

## ETMGT45

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT45 LOADING OF TODR AFTER HW-DAMAGE NOT POSSIBLE

## ETMGT50

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT50 AUTOMATIC SEASON CHANGE IN FUTURE NOT POSSIBLE. SYSTEM ERROR OCCURED IN RUN OF TASK "TIME".

### Meaning

An internal error for task TIME occurred.
A consistent system run can only be guaranteed until the
next season change.
Diagnose data are generated automatically.

### Response

The system has to be restarted before next season change (STARTUP).

## ETMGT51

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT51 AUTOMATIC SEASON CHANGE IN FUTURE NOT POSSIBLE. THE LIST OF CHDATES IS EXHAUSTED.

### Meaning

A consistent system run can only be guaranteed until the
next season change.

### Response

Extend CHDATE list in GTIME PARAMS of STARTUP PARAM FILE!
The system has to be restarted before next season change (STARTUP).

## ETMGT52

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT52 NO AUTOMATIC SEASON CHANGE, BECAUSE GTIME PARAMETER DIFF=0.

### Meaning

No automatic season change will be performed, because the value of the
GTIME parameter DIFF means there is no season change.
The system runs with Standard Time.

## ETMGT55

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT55 *** AUTOMATIC START OF SUBSYSTEM TSDRIVER FAILED! ***

### Meaning

The automatic start of the TSDRIVER subsystem returns with error.

### Response

To start the subsystem please use the command START-SUBSYSTEM.

## ETMGT58

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT58 CLOCK SYNCHRONISATION CAN NOT BE PERFORMED. SYSTEM ERROR OCCURED IN RUN OF TASK "TIME".

### Meaning

An internal error inhibits clock synchronisation.
Diagnose data are generated automatically.

### Response

To make possible clock synchronisation the system has to be restarted
(STARTUP).

## ETMGT59

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT59 RE-ADJUSTMENT OF TASK MANAGEMENT PARAMETERS CAN NOT BE PERFORMED DUE TO UNKNOWN CPU ID

## ETMGT60

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT60 *** AUTOMATIC RESTART AS RESTART OPTION NOT ALLOWED! ***

### Meaning

An internal error for task TIME occurred.
The task tried to save STARTUP information in SVL.
A consistent system run can only be guaranteed until the
next season change.
Diagnose data are generated automatically.

### Response

The next STARTUP must not be an AUTOMATIC RESTART.

## ETMGT61

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMGT61 *** AUTOMATIC RESTART AS RESTART OPTION ALLOWED AGAIN! ***

### Meaning

The saving of STARTUP information in SVL was successful.

### Response

The next STARTUP may be an AUTOMATIC RESTART!

## ETMIM01

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM01 SYSTEM ERROR ETMIM01 TERMINATED SESSION; ***ETMIA$X: INTERRUPT NOT ALLOWED OR STATE UNKNOWN!***

### Meaning

Interrupt not allowed in the current program state or
state unknown.

### Response

Take SLED and send it to your systems engineer.

## ETMIM02

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM02 SYSTEM ERROR ETMIM02 TERMINATED SESSION; ***ETMIA$X: PROGRAM ERROR / SVC AS PENDING INTERRUPT!***

### Meaning

This error is probably caused by a program error or a SVC in SIH.

### Response

Take SLED and send it to your systems engineer.

## ETMIM03

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM03 SYSTEM ERROR ETMIM03 TERMINATED SESSION; ***ETMIA$X: PROGRAM ERROR / SVC IN SYSTEM WAIT STATE!***

### Meaning

A program error or a SVC occurred while the system was in the state
System Wait (IDLE).

### Response

Take SLED and send it to your systems engineer.

## ETMIM05

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM05 SYSTEM ERROR ETMIM05 TERMINATED SESSION; ***ETMIA$X: PROHIBITED INTERRUPT OCCURRED!***

### Meaning

The session was terminated because an interrupt which was unknown to
the system occurred.

### Response

Take SLED and send it to your systems engineer.

## ETMIM06

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM06 SYSTEM ERROR ETMIM06 TERMINATED SESSION; ***ETMIA$R: PROHIBITED 64-BIT INTERRUPT OCCURRED!***

### Meaning

The session was terminated because an interrupt which was unknown to
the system occurred.

### Response

Take SLED and send it to your systems engineer.

## ETMIM08

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMIM08 OVERFLOW OF TIME-OF-DAY-CLOCK PROCESSED SUCCESSFULLY

## ETMIM09

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMIM09 SYSTEM ERROR ETMIM09 TERMINATED SESSION; ***ETMPT5: INTERNAL ERROR DURING TIME-OF-DAY-CLOCK OVERFLOW

### Meaning

The TIME-OF-DAY-CLOCK overflow cannot be handled.

### Response

Take SLED.

## ETMIM10

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMIM10 SYSTEM ERROR ETMIM10 TERMINATED SESSION; ***ETMPT5: NO SLOTPOOL FOR PCB EXTENSIONS AVAILABLE

### Meaning

At system startup the slotpool for PCB extensions cannot be
installed.

### Response

Take SLED.

## ETMIM21

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM21 SYSTEM ERROR ETMIM21 TERMINATED SESSION; ***ETMDISP: KAI-SCHEDULER FOUND UNKNOWN ADDRESS IN $Q-SLOT!***

### Meaning

The task initiator determined that an invalid start address for a
KAI-process was passed in the $Q-slot.

### Response

Take SLED and send it to your systems engineer.

## ETMIM22

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM22 SYSTEM ERROR ETMIM22 TERMINATED SESSION; ***ETMDISP: KAI-SCHEDULER GOT UNDEFINED RETURN CODE FROM A $QPP3-FUNCTION!***

### Meaning

The session was terminated because a $QPP3-function returned an
unexpected value to the task initiator.

### Response

Take SLED and send it to your systems engineer.

## ETMIM23

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM23 SYSTEM ERROR ETMIM23 TERMINATED SESSION; ***ETMDISP: KAI-SCHEDULER GOT UNDEFINED TID IN $Q-SLOT!***

### Meaning

A PEND/UNPEND of the system or the task with TID<>0 is not allowed.

### Response

Take SLED and send it to your systems engineer.

## ETMIM25

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM25 SYSTEM ERROR ETMIM25 TERMINATED SESSION; ***ETMDISP: ETMRFNAT FOR SYSTEM OR TID NE 0 IS NOT ALLOWED***

### Meaning

Function Attach for the system or a task not in control is not
allowed.

### Response

Take SLED and send it to your systems engineer.

## ETMIM41

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM41 SYSTEM ERROR ETMIM41 TERMINATED SESSION; ***ETMEIA: AT ADDRESS: (&00) CALLER CAUSED SYSTEM TERMINATION***

### Meaning

This is a general $CRASH-call which is branched to from various
routines.

### Response

Take SLED and send it to your systems engineer.

## ETMIM42

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM42 SYSTEM ERROR ETMIM42 TERMINATED SESSION; ***ETMEIA: PROHIBITED INTERRUPT OCCURRED!***

### Meaning

The interrupt which occurred is unknown and therefore forbidden.

### Response

Take SLED and send it to your systems engineer.

## ETMIM43

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM43 SYSTEM ERROR ETMIM43 TERMINATED SESSION; ***ETMEIA: ERROR IN $NSTEVA-CALL! ***

### Meaning

If a program error occurs in TU, then a TPR-PCB is created for
the STXIT processing using the $NSTEVA macro. A prohibited return
code from this processing (caused by an invalid TID or invalid
parameters) led to system termination.

### Response

Take SLED and send it to your systems engineer.

## ETMIM44

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM44 SYSTEM ERROR ETMIM44 TERMINATED SESSION; ***ETMEIA: AT LOCATION: (&00) PROGRAM ERROR BEFORE CLASS 2 IS LOADED!***

### Meaning

An error during STARTUP caused system termination. STARTUP will not
be continued.

### Response

Take SLED and send it to your systems engineer.

## ETMIM45

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM45 SYSTEM ERROR ETMIM45 TERMINATED SESSION; ***ETMEIA: $TERM-ERROR!***

### Meaning

Task Termination failed because of an invalid TID, an invalid parameter
or saturation of some system resource. $TERM is called in SIH.

### Response

Take SLED and send it to your systems engineer.

## ETMIM46

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM46 SYSTEM ERROR ETMIM46 TERMINATED STEP; ***ETMEIA: PAGING ERROR CAUSED BY HARDWARE ERROR!***

### Meaning

Memory Management reported a Paging Error caused by a
hardware error.
The error occurred in program state TU.

### Response

None.

## ETMIM47

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM47 SYSTEM ERROR ETMIM47 TERMINATED SESSION; ***ETMEIA: HARDWARE ERROR CANNOT BE HANDLED (NO PCB AVAILABLE)!***

### Meaning

The session was terminated because no PCB was available to
process the hardware error.

### Response

Take SLED and send it to your systems engineer.

## ETMIM48

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM48 SYSTEM ERROR ETMIM48 TERMINATED STEP; ***ETMEIA: STEP TERMINATION DUE TO HARDWARE ERROR!***

### Meaning

No further information.

### Response

None.

## ETMIM50

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM50 SYSTEM ERROR ETMIM50 TERMINATED SESSION; ***ETMEIA: AT LOCATION: (&00) HARDWARE ERROR BEFORE CLASS 2 IS LOADED!***

### Meaning

An error during STARTUP caused system termination. STARTUP will not
be continued.

### Response

Take SLED and call maintenance.

## ETMIM51

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM51 SYSTEM ERROR ETMIM51 TERMINATED SESSION; ***ETMSF: PCB-LINK DESTROYED!***

### Meaning

Although the PCB was not the permanent TPR-PCB, no predecessor for
it could be found in the PCB chain when $DEST attempted to remove
all PCB's during task termination.

### Response

Take SLED and send it to your systems engineer.

## ETMIM52

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM52 SYSTEM ERROR ETMIM52 TERMINATED SESSION; ***ETMSF: FNDT ON PCB WITH LINK=0 OR FNDT ON PERMANENT PCB OR FNDT ON TU-PCB!***

### Meaning

During function detach an attempt was made to remove a PCB which is
the permanent PCB for TU-SVC's, a TU-PCB or a PCB, which has no
predecessor. This is not allowed.

### Response

Take SLED and send it to your systems engineer.

## ETMIM53

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM53 SYSTEM ERROR ETMIM53 TERMINATED SESSION; ***UNEXPECTED RECONFIGURATION RETURN CODE WAS FOUND DURING PERIODIC LM-CHECK!***

### Meaning

A $RECONF-call (Reconfiguration) produced a prohibited return code.
The call is used as a CPU-check.

### Response

Take SLED and send it to your systems engineer.

## ETMIM54

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM54 SYSTEM ERROR ETMIM54 TERMINATED SESSION; ***ERROR DURING PROCESSING OF BLOCKED LOGICAL MACHINES!***

### Meaning

A $RECONF-call produced a prohibited return code indicating that
either: the current Logical Machine (LM) is bound to a physical CPU
at present and therefore cannot be unblocked,
or: the generated system possibly does not contain the necessary
reconfiguration modules.

### Response

Take SLED and send it to your systems engineer.

## ETMIM55

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM55 SYSTEM ERROR ETMIM55 TERMINATED SESSION; ***ETMSF: $P3FNAT ONLY ALLOWED FOR TASK IN CONTROL!***

### Meaning

Asynchronous 'function attach' is no longer supported.

### Response

Take SLED and send it to your systems engineer.

## ETMIM56

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM56 SYSTEM ERROR ETMIM56 TERMINATED TASK; ***ETMSF: FNDT ON PERMANENT TPR-PCB! ***

### Meaning

No further information.

### Response

Take SYSTEM DUMP and send it to your systems engineer.

## ETMIM57

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM57 SYSTEM ERROR ETMIM57 TERMINATED SESSION; ***ETMSF: $TERM-ERROR!***

### Meaning

Task Termination failed because of an invalid TID, an invalid parameter
or saturation of some system resource. $TERM is called in SIH.

### Response

Take SLED and send it to your systems engineer.

## ETMIM58

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM58 SYSTEM ERROR ETMIM58 TERMINATED TASK; ***ETMSF: PP2-PC WAS NOT UPDATED***

### Meaning

The PP2-PC was not updated by Termination Processing after TERM.

### Response

Take Systemdump and send it to your systems engineer.

## ETMIM59

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM59 SYSTEM ERROR ETMIM59 TERMINATED TASK; ***NEHMATBL: INTERRUPTED PCB NOT EXISTENT***

### Meaning

No further information.

### Response

Take Systemdump and send it to your systems engineer.

## ETMIM70

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM70 SYSTEM ERROR ETMIM70 TERMINATED TASK; ***ETMSF: $PBINF RETURNS INVALID RETURN CODE***

### Meaning

The $PBINF-call was made in order to get the program name after SVC 79.

### Response

Take Systemdump and send it to your systems engineer.

## ETMIM71

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM71 SYSTEM ERROR ETMIM71 TERMINATED TASK; ***ETMSF: $CHKPRV RETURNS INVALID RETURN CODE***

### Meaning

$CHKPRV was called to get the privileges of the caller after SVC 79.

### Response

Take Systemdump and send it to your systems engineer.

## ETMIM72

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM72 PROGRAM (&00) WANTS TO INTERFACE WITH THE SYSTEM. REPLY (Y = ACCEPT; N = ABORT)

### Meaning

A user-program in the non-privileged state TU has called SVC 79
to become privileged (TPR).
The above message is sent to the console. The operator should
answer the message.
The message is only sent to the console if the user has the
user identification $TSOS or $SERVICE. In the other cases the SVC
is ignored.

### Response

Y : The user gains control in the privileged state.
N : The SVC 79 call is ignored.

## ETMIM80

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM80 SYSTEM ERROR ETMIM80 TERMINATED TASK; ***ETMSERV: $NSTEVA RETURNS INVALID RETURN CODE***

### Meaning

The $NSTEVA call was made because a 24-bit-address was given in
the parameter list of a TU caller in XS-mode.

### Response

Take Systemdump and send it to your systems engineer.

## ETMIM81

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM81 SYSTEM ERROR ETMIM81 TERMINATED TASK; ***ETMSERV: INVALID 24-BIT-ADDRESS IN XS-BIT-MODE***

### Meaning

If a caller uses a 24-bit-address as parameter in TPR,
then the task will be terminated.

### Response

Take Systemdump and send it to your systems engineer.

## ETMIM82

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM82 SYSTEM ERROR ETMIM82 TERMINATED TASK; ***ETMSERV: $SNAP RETURNS INVALID RETURN CODE***

### Meaning

$SNAP was called when a $ACCTLT-error occurred.

### Response

Take Systemdump and send it to your systems engineer.

## ETMIM83

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM83 SYSTEM ERROR ETMIM83 ISSUED $SNAP; ***ETMSERV: $ACCTLT-ERROR***

### Meaning

$ACCTLT was called to release the TLT-lock but
the release of the lock was not successful.

### Response

The System-administrator should send the dump
to your systems engineer.

## ETMIM84

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM84 SYSTEM ERROR ETMIM84 TERMINATED TASK; ***ETMSERV: PARAMETER LIST IS NOT ALIGNED***

### Meaning

The task was terminated because the parameter list of a BASR call
in TPR was not aligned.

### Response

Take Systemdump and send it to your systems engineer.

## ETMIM85

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM85 SYSTEM ERROR ETMIM85 TERMINATED TASK; ***ETMSERV: $NSTEVA RETURNS INVALID RETURN CODE***

### Meaning

The $NSTEVA call was caused by an SVC from TU with an
unaligned parameter area or a wrong unit numer in the
function header.

### Response

Take Systemdump and send it to your systems engineer.

## ETMIM86

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM86 SYSTEM ERROR ETMIM86 TERMINATED TASK; ***ETMSERV: PARAMETER LIST IS NOT ALIGNED***

### Meaning

The task was terminated because the parameter list of a SVC
in TPR was not aligned.

### Response

Take Systemdump and send it to your systems engineer.

## ETMIM87

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM87 SYSTEM ERROR ETMIM87 TERMINATED SESSION; ***ETMSERV: PARAMETER LIST IS NOT ALIGNED***

### Meaning

A BASR interface in SIH was called with an unaligned parameter
area, therefore the task is terminated.

### Response

Take SLED and send it to your systems engineer.

## ETMIM88

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

ETMIM88 OBSOLETE SPL RUNTIME SYSTEM IN USE. PROCESSING CONTINUED

### Meaning

The SPL Runtime System issued an SVC 15 which will no longer be
supported in future. The SVC was ignored, a SERSLOG entry was
written and processing continued.

### Response

Please relink the program with an SPL Runtime System more recent
than V1.3C42.

## ETMIM89

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM89 SYSTEM ERROR ETMIM89 TERMINATED TASK; ***ETMSERV: PARAMETER LIST IS NOT ALIGNED***

### Meaning

A TPR interface was called with a wrong unit number in
the function header, therefore the task is terminated.

### Response

Take Systemdump and send it to your systems engineer.

## ETMIM90

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM90 SYSTEM ERROR ETMIM90 TERMINATED SESSION; ***ETMSERV: WRONG UNIT NUMBER AT AN SIH INTERFACE

### Meaning

A SIH interface was called with a wrong unit number in
the function header, therefore the session is terminated.

### Response

Take SLED and send it to your systems engineer.

## ETMIM91

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM91 SYSTEM ERROR ETMIM91 TERMINATED SESSION; ***ETMSLMG: AT SLOT ADDRESS: (&00), SLOT INCONSISTENCY***

### Meaning

The return of a slot was rejected with primary code <> 0, probably
because of an invalid slot address. Program state was SIH.

### Response

Take SLED and send it to your systems engineer.

## ETMIM92

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM92 SYSTEM ERROR ETMIM92 TERMINATED SESSION; ***ETMSLMG: SLOT LACK IN ONE OF THE TASK MANAGEMENT'S SLOT POOLS!***

### Meaning

A $GETS call produced a prohibited return code; no slot was available.

### Response

Take SLED and send it to your systems engineer.

## ETMIM93

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMIM93 SYSTEM ERROR ETMIM93 TERMINATED TASK; ***ETMSLMG: BOURSE OR PCB SLOT INCONSISTENCY***

### Meaning

The return of a slot was rejected with primary code <> 0, probably
because of an invalid slot address. Program state was TPR.

### Response

Take DUMP and send it to your systems engineer.

## ETMLMP2

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMLMP2 SYSTEM ERROR ETMLMP2 TERMINATED SESSION; (&00) (&01)

### Meaning

The system was terminated by the system lock manager in state TPR.
(&00) gives information about where the crash occurred, detailing the
following fields as appropriate:
STATE= System state, SIH (System Interrupt Handling) or
TPR (Task Privileged)
P-CTR= Program Counter
IW= Interrupt Weight
LSF= Lock Status Field.
These are followed by the message (&01), as described below, which
explains further the reason for the crash. (Note: the messages (&00)
and (&01) are intended mainly for use within the Company to help
diagnose the problem.)
LOCK HELD BY AN INTERRUPTED TASK LACKS A LOCK RECOVERY ROUTINE.
A task was interrupted while holding a system lock for which no
recovery routine is defined.
LOCK HIERARCHY VIOLATED - SYSTEM DEADLOCK POSSIBLE.
An attempt was made to get a system lock while a higher priority
lock was already held. This could lead to a deadlock. This system
crash will only occur when the system is in test mode.
RECONFIGURATION FAILED AFTER BEING CALLED FROM SPINWAIT.
The return code has indicated that reconfiguration processing
was not successful. Reconfiguration was called after a spin-
wait for a lock exceeded the allotted time.
REPEATED $CRASH CALLS IN NUCLEUS LOCK MAMAGER.
This message is displayed if there is a further $CRASH call
necessary after the nucleus lock manager has already initiated
a system crash. In this case, the fields (&01) are not displayed.

### Response

If necessary, take SLED and send it to your systems engineer.

## ETMLMP3

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMLMP3 SYSTEM ERROR ETMLMP3 TERMINATED SESSION; (&00) (&01)

### Meaning

The system was terminated by the system lock manager in state SIH.
(&00) gives information about where the crash occurred, detailing the
following fields as appropriate:
STATE= System state, SIH (System Interrupt Handling) or
TPR (Task Privileged)
P-CTR= Program Counter
IW= Interrupt Weight
LSF= Lock Status Field.
These are followed by the message (&01), as described below, which
explains further the reason for the crash. (Note: the messages (&00)
and (&01) are intended mainly for use within the Company to help
diagnose the problem.)
LOCK HELD BY AN INTERRUPTED TASK LACKS A LOCK RECOVERY ROUTINE.
A task was interrupted while holding a system lock for which no
recovery routine is defined.
LOCK HIERARCHY VIOLATED - SYSTEM DEADLOCK POSSIBLE.
An attempt was made to get a system lock while a higher priority
lock was already held. This could lead to a deadlock. This system
crash will only occur when the system is in test mode.
RECONFIGURATION FAILED AFTER BEING CALLED FROM SPINWAIT.
The return code has indicated that reconfiguration processing
was not possible.
REPEATED $CRASH CALLS IN NUCLEUS LOCK MAMAGER.
This message is displayed if there is a further $CRASH call
necessary after the nucleus lock manager has already initiated
a system crash. In this case, the fields (&01) are not displayed.

### Response

If necessary, take SLED and send it to your systems engineer.

## ETMNM09

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMNM09 ERROR DURING $RDUID-CALL IN MODULE ETMNMGR

### Meaning

Unexpected return code while checking the User-Id in module ETMNMGR
of the Name Manager.

### Response

If necessary, take DUMP and send it to your systems engineer.

## ETMNM10

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMNM10 ERROR DURING $GETUGR-CALL IN MODULE ETMNMGR

### Meaning

Unexpected return code while checking the Group-Id in module ETMNMGR
of the Name Manager.

### Response

If necessary, take DUMP and send it to your systems engineer.

## ETMNM11

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMNM11 ERROR DURING $GETSL-CALL IN MODULE ETMNMGR

### Meaning

Unexpected return code while fetching a slot in module ETMNMGR
of the Name Manager.

### Response

If necessary, take DUMP and send it to your systems engineer.

## ETMNM12

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMNM12 ERROR DURING $NCCPLV-CALL IN MODULE ETMNMGR

### Meaning

Unexpected return code while changing the PCB-Level in module ETMNMGR
of the Name Manager.

### Response

If necessary, take DUMP and send it to your systems engineer.

## ETMNM13

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMNM13 ERROR DURING $NBCREA-CALL IN MODULE ETMNLCK

### Meaning

Unexpected return code while creating a bourse during Startup in
module ETMNLCK of the Name Manager.

### Response

If necessary, take DUMP and send it to your systems engineer.

## ETMNM14

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMNM14 ERROR DURING $NBRSIG-CALL IN MODULE ETMNLCK

### Meaning

Timeout while waiting for the release of a lock in module ETMNLCK
of the Name Manager.

### Response

If necessary, take DUMP and send it to your systems engineer.

## ETMPC17

Destination: USER-TASK, CONSOLE Routing code: A Weight: 30

Warranty : NO

ETMPC17 CMD NOT ACCESSIBLE NOW. PLEASE TRY LATER

### Meaning

No further information.

### Response

None.

## ETMPC20

Destination: USER-TASK, CONSOLE Routing code: A Weight: 30

Warranty : NO

ETMPC20 PCS NOT STARTED. CMD IGNORED

### Meaning

No further information.

### Response

None.

## ETMPR01

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMPR01 SYSTEM ERROR ETMPR01 TERMINATED SESSION; ***PEND/UNPEND : UNDEFINED Q# IN TCB***

### Meaning

The queue-number found in the TCB specifies the current queue.
The Pend/Unpend-routine searched this queue but did not find
the task.

### Response

Take SLED and send it to your systems engineer.

## ETMPR02

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMPR02 SYSTEM ERROR ETMPR02 TERMINATED SESSION; ***ETMPSHEL : PEND WITH Q-LOCK AND INVALID PENDCODE***

### Meaning

Pends while holding the Q-lock are only allowed for special cases.
At present only the Dispatcher is allowed to do so with Pendcode
PRQTIC.
The check-routine in module ETMPSHEL has detected a Pendcode
unequal PRQTIC.

### Response

Take SLED and send it to your systems engineer.

## ETMPR03

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMPR03 SYSTEM ERROR ETMPR03 TERMINATED SESSION; ***PEND/UNPEND : INCONSISTENT Q-LOCK-STATUS DETECTED***

### Meaning

During Pend/Unpend processing the current Q-lock-status is checked
against the expected Q-lock-status. The system was terminated
because the current status differed from the expected status.

### Response

Take SLED and send it to your systems engineer.

## ETMPR10

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMPR10 SYSTEM ERROR ETMPR10 TERMINATED TASK; ***ETMIN: REQM IS NOT SUCCESSFUL***

### Meaning

A workarea in class 5 memory is requested for the functions Eventing,
Serialization, STXIT, etc., during task creation. The task was
terminated because this request failed (system error).

### Response

Take systemdump and send it to your systems engineer.

## ETMPR11

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMPR11 SYSTEM ERROR ETMPR11 TERMINATED SESSION; ***ETMIN : CREATION OF CATEGORY-DATA-LOCK NOT SUCCESSFUL***

### Meaning

The Task Scheduler PRIOR needs a lock to protect its category-
specific data. Failure to create this lock during Startup meant
that the subsystems PCS/JMS would not have been able to perform
essential functions. The session was therefore terminated.

### Response

Take SLED and send it to your systems engineer.

## ETMPR20

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMPR20 SYSTEM ERROR ETMPR20 TERMINATED TASK; ***ETMCS: CATEGORY-DATA-LOCK NOT GOTTEN***

### Meaning

For ACCESS=WRITE to category-specific data the Task Scheduler
PRIOR must get a lock.
This lock did not become available within the specified time limit.

### Response

Take systemdump and send it to your systems engineer.

## ETMPR21

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMPR21 SYSTEM ERROR ETMPR21 TERMINATED TASK; ***ETMCS: ERROR DURING RELEASE OF CATEGORY-DATA-LOCK***

### Meaning

After writing category-specific data of the Task Scheduler PRIOR
it was not possible to release the lock which protects the
category-specific data.

### Response

Take systemdump and send it to your systems engineer.

## ETMPR30

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMPR30 PCS/ETMPRS: START/CANCEL PERIODIC ROUTINE: PAR-ERR

### Meaning

System-internal problems by START/STOP of the PCS
(connect/disconnect of the periodic routines of the PCS).

## ETMRK00

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK00 SYSTEM ERROR ETMRK00 TERMINATED SESSION; (&00)

### Meaning

The system was terminated by reconfiguration. (&00), as described
below, explains further the reason for the crash. (Note: the
messages (&00) are intended mainly for use within the Company
to help diagnose the problem.)
RECONFIGURATION IN USE - The reconfiguration lock was not
released within the set time-limit.
RECONFIGUR'N FOR MONO SYSTEM - Reconfiguration was called when the
system was in mono mode.
RECONFIGUR'N FOR CPU0 IN APS - CPU0 may not be detached in an
Attached Processor System (APS).
CALLER'S PARAMETERS INVALID - Invalid caller index for $RECONF call.
UNINTERRUPTIBLE CPU LOOP - Suspected loop and system not in
fault tolerant mode
INVALID $Q SLOT - System $Q slot has invalid format
SYSTEM LOCK(S) HELD - System lock(s) held and no valid
logical machine context available.
SYSTEM COMPONENT IDENTITY? - Reconfiguration request for unrecog-
nised system component.
NO $Q SLOTS AVAILABLE - Reconfiguration's pool of system $Q
slots exhausted.
NO RECONF'N SLOTS AVAILABLE - Reconfiguration's pool of Action
Request (ARQ) slots exhausted.
NO RECONF SAVEAREA AVAILABLE - No reconfiguration procedure linkage
save areas available.
LOGICAL MACHINE NR. INVALID - Logical machine number out of range.
RECONFIGURATION BUFFER ERROR - Logical machine context in unexpected
state.
RECONFIGUR'N SOFTWARE ERROR - No valid context or
No blocked logical machine.
RECONFIGUR'N SVP CALL ERROR - Unexpected return code from $SVP.
RECONF RECOVERY BUFFER ERROR - Reconfiguration recovery buffer
unavailable.
NO RECONF'N TERMINATION SLOT - Pool of reconfiguration termination
request slots exhausted.
RECONF'N: GP HARDWARE STATE - Bad parameters for GP reconfiguration
during Startup.
RECONF'N: IOP HARDWARE STATE - Bad parameters for IOP reconfigura-
tion during Startup.
ETMRK2A : BOURSE ERROR - Returncode from $NENQBO not 0.
ETMRK2A : REQM/RELM PROBLEM - Returncode from $REQM or $RELM not 0.
ACTIVITY PROCESS ACTIVE - Kernel activity process was active
and no valid context available.
INVALID ACTIVITY ORDER CODE - Unexpected activity order code
detected.

### Response

If necessary, take SLED and send it to your systems engineer.

## ETMRK01

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK01 SYSTEM ERROR ETMRK01 TERMINATED SESSION; ETMRK2E - COULD NOT INITIATE MESSAGE OUTPUT

### Meaning

An attempt to pass a message to the Message Task failed. The system
crash only occurs when the system is not in fault tolerant mode.

### Response

If necessary, take SLED and send it to your systems engineer.

## ETMRK02

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK02 SYSTEM ERROR ETMRK02 TERMINATED SESSION; PROBLEM DETECTED BY (&00)

### Meaning

A system software problem has been detected by the reconfiguration
module (&00). (&00) is ETMRK2B or ETMRK2C. The message ETMRK28
will have been output with the address where the error was detected.

### Response

If necessary, take SLED and send it to your systems engineer.

## ETMRK03

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK03 SYSTEM ERROR ETMRK03 TERMINATED SESSION; ETMRK2F-BOURSE ENQUEUE FAILED

### Meaning

Return code from $NENQBO not 0.

### Response

If necessary, take SLED and send it to your systems engineer.

## ETMRK04

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK04 SYSTEM ERROR ETMRK04 TERMINATED SESSION; ETMRK2B-RELEASE MSG-PARM MEMORY FAILED

### Meaning

The returncode from $RELM to release the message task parameter area
was not 0. The system crash only occurs when the system is not in
fault tolerant mode.

### Response

If necessary, take SLED and send it to your systems engineer.

## ETMRK05

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK05 SYSTEM ERROR ETMRK05 TERMINATED SESSION

### Meaning

An error occurred while the System was being initialized. A short
explanation of the error is given in the preceding message ETMRK15.

### Response

Correct the error and load the System again.

## ETMRK06

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK06 SYSTEM ERROR ETMRK06 TERMINATED SESSION; STCK CONDITION CODE NE ZERO

### Meaning

An STCK (Store clock) instruction returned a non-zero condition code.
A system crash is necessary to avoid the system using an invalid
TOD (Time-of-Day) clock value.

### Response

Check why the TOD clock was in an unexpected state (with help from
a maintenance technician, if necessary).
If necessary, take SLED and send it to your systems engineer.

## ETMRK07

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK07 SYSTEM ERROR ETMRK07 TERMINATED SESSION; SCK CONDITION CODE NE ZERO

### Meaning

An SCK (Set clock) instruction returned a non-zero condition code
indicating that the TOD (Time-of-day) clock was secured or not
operational. A system crash is necessary to avoid the system
operating with an incorrect value of the TOD clock.

### Response

Check why the TOD clock was not in the expected state.
If necessary, take SLED and send it to your systems engineer.

## ETMRK08

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK08 SYSTEM ERROR ETMRK08 TERMINATED SESSION; TOD-SYNCHRONISATION FAILED

### Meaning

An attempt to synchronise the TOD- (Time-of-day) clocks has failed.
Because the system cannot operate successfully without the
TOD-clocks being synchronised, the system session is terminated.

### Response

a) Check that the generated system configuration is suitable for
the available hardware (on some computer models the TOD-clocks
can only be synchronised if the number of generated CPUs is
equal to the number of available CPUs).
If necessary, generate a suitable system anew.
b) If the generated configuration is correct, take SLED and send it
to your systems engineer. If a hardware error is
suspected, call a maintenance technician.

## ETMRK1A

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK1A (&00) (&01) ALREADY ATTACHED

### Meaning

Command /ATTACH-DEVICE was rejected, because
(&00) (&01) was already attached.
(&00): may be:
SIDE : Side
SE : Storage Element
CPU : Central Processing Unit
(&01): HW-Unit Id.

### Response

None.

## ETMRK1B

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK1B (&00) (&01) ALREADY DETACHED

### Meaning

Command /DETACH-DEVICE was rejected,
because (&00) (&01) was already detached.
(&00): may be:
SIDE : Side
SE : Storage Element
CPU : Central Processing Unit
(&01): HW-Unit Id.

### Response

None.

## ETMRK1C

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK1C ATTACHMENT OF CPU (&00) NOT POSSIBLE DUE TO (&01)

### Meaning

Command /ATTACH-DEVICE (&00) was rejected because of (&01).
(Note: The messages (&01) are intended mainly for use within
the Company to help diagnose the problem).
(&01): may be:
NO LM AREA : No Logical Machine local area could be allocated.
NO REC BUF : No reconfiguration buffer was available.
CACHE RTN : Call of Cache Routine failed.
SOFTWARE : Software failure.
HARDWARE : Hardware failure.
$SVP FAIL : Call of $SVP failed.
NO SUPPORT : The reconfiguration modules are not available in
the system.

### Response

None or take SLED and in case of 'HARDWARE' call hardware maintenance.

## ETMRK1D

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK1D DETACHMENT OF CPU (&00) NOT POSSIBLE DUE TO (&01)

### Meaning

Command /DETACH-DEVICE CPU (&00) was rejected because of (&01).
(Note: The messages (&01) are intended mainly for use within
the Company to help diagnose the problem).
(&01): may be:
SOFTWARE : Software failure.
IOP-REJECT : A request for I/O-Reconfiguration was rejected.
NO SUPPORT : The reconfiguration modules are not available in
the system.

### Response

None, or take SLED.

## ETMRK1E

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK1E DO YOU ACCEPT ACTUAL DATE '(&00)' AND TIME OF DAY '(&01)' ? REPLY (Y = YES; N = NO)

### Meaning

The operator must check the current date and time of day and
decide whether the system's date and/or time of day should
be modified.

### Response

Y: Date and time of day are correct and accepted.
N: Date and time of day should be modified.
Requests to update these values will follow (ETMRK12 and ETMRK13).

## ETMRK1F

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK1F ILLEGAL REPLY

## ETMRK10

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK10 MULTIPLE HARDWARE ERRORS

### Meaning

Multiple CPU errors have occurred on the only ATTACHED CPU.

### Response

If appropriate call maintenance technician.

## ETMRK11

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK11 LOOP IN (&00) SUSPECTED. PROGRAM COUNTER (&01) **************

### Meaning

In a multiprocessor system, a CPU has remained uninterruptible
in state (&00) for too long. The CPU was halted with the
program counter at (&01) and restarted in the task initiator.
Any task which was active on the processor will be terminated.

### Response

Take SLED if further analysis is desired.

## ETMRK12

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK12 ENTER ACTUAL DATE. REPLY (YYYYMMDD = DATE)

### Response

The operator must enter the current date in the correct format.

## ETMRK13

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK13 ENTER ACTUAL TIME. REPLY (HHMMSS = TIME)

### Response

The operator must enter the current time in the correct format.

## ETMRK14

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK14 RELEASE MEMORY FAILED

### Meaning

Release of class 3/ 4 memory failed after reconfiguration processing.

### Response

Take SLED to aid diagnosis.

## ETMRK15

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK15 SYSTEM INITIALISATION (&00) *** RE-IPL AFTER ERROR ANALYSIS

### Meaning

Error (&00) occurred when initialising the system.
(&00): gives an abbreviated explanation of the error.

### Response

Correct error and re-ipl.

## ETMRK16

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK16 NUMBER OF PHYSICAL GPS (&00) NUMBER OF GENERATED GPS

### Meaning

(&00) = < : Operating system was generated for more GPs then available
(e.g. Bi-system running on mono configuration).
(&00) = > : More GPs available than the system can serve.
System runs on generated processors only.

### Response

None (but there are processor models where the TOD (Time-of-day)
clocks can only be synchronised successfully if the number of
generated GPs is equal to the number of available GPs; see also
ETMRK08).

## ETMRK18

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK18 (&00) (&01) ATTACHED

### Meaning

Command /ATTACH-DEVICE was successfully processed.
(&00) (&01) is now attached.
(&00): may be:
SIDE : Side
SE : Storage Element
CPU : Central Processing Unit
(&01): HW-Unit Id.

### Response

None.

## ETMRK19

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK19 (&00) (&01) DETACHED **********************************************

### Meaning

HW-Unit (&00) was logically detached.
(&00): may be:
SIDE : Side
SE : Storage Element
CPU : Central Processing Unit
(&01): HW-Unit Id.

### Response

None.

## ETMRK20

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ETMRK20 (&00) (&01) attached by system

### Meaning

Due to a CPU failure a spare CPU has been attached by system.
(&00): may be:
CPU
(&01): HW-Unit Id.

## ETMRK22

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK22 (&00) (&01) ATTACHMENT REJECTED

### Meaning

Command /ATTACH-DEVICE for (&00) (&01) was
rejected. The reason is given in a preceding
or following message.
(&00): may be:
SIDE : Side
SE : Storage Element
CPU : Central Processing Unit
(&01): HW-Unit Id.

### Response

None.

## ETMRK23

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK23 (&00) (&01) DETACHMENT REJECTED

### Meaning

Command /DETACH-DEVICE for (&00) (&01) was rejected.
The reason is given by a preceding message.
(&00): may be:
SIDE : Side
SE : Storage Element
CPU : Central Processing Unit
(&01): HW-Unit Id.

### Response

None.

## ETMRK25

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK25 (&00) RECONFIGURATION NOT AVAILABLE

### Meaning

The reconfiguration modules are not available in the system. If
present (&00) shows which reconfiguration function is not available.

### Response

Generate the system with reconfiguration modules.

## ETMRK27

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ETMRK27 (&00) (&01) THE ONLY OPERABLE HW-UNIT

### Meaning

(&00) (&01) is the only operable HW-Unit in the system,
therefore the /DETACH-DEVICE command was rejected.
(&00): may be:
SIDE : Side
SE : Storage Element
CPU : Central Processing Unit
(&01): HW-Unit Id.

### Response

None.

## ETMRK28

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK28 SYSTEM ERROR DETECTED AT (&00)

### Meaning

A system error was detected. For diagnostic purposes (&00)
gives the module and offset in module, where the error occurred.

### Response

Take SLED.

## ETMRK29

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK29 (&00) (&01) SYSTEM INTERFACE TRANSFER ERROR

### Meaning

A System Interface error occurred when communicating with the
Service Processor.
(&00): may be:
SIDE : Side
SE : Storage Element
CPU : Central Processing Unit
(&01): HW-Unit Id.

### Response

None or take SLED and/or call a maintenance technician.

## ETMRK3A

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK3A I/O DEVICE (&00) ERROR (ETSVP RC NE 0). SYSTEM INITIALISATION CONTINUES

### Meaning

Execution of a hardware detach of an I/O device which was not
defined in the BS2000 configuration has failed.
As the device cannot disturb the running system, Startup continues.

### Response

None.

## ETMRK3B

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK3B NEW TIME VALUE LESS THAN CURRENT SYSTEM CLOCK

### Meaning

The new value for time and date (as determined by the system
or the operator) is earlier than the value currently in one
of the system's time-of-day (TOD) clocks. This is not
allowed as it can lead to inconsistencies in time values used
by BS2000 (time values must always be increasing).

### Response

a) Input a new time value which is greater than the current
system time.
b) Perform a new IPL to reset the system time (if necessary,
the Service Processor clock should be reset first).
c) If hardware problems with the system's clocks are suspected,
call maintenance technician.

## ETMRK30

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK30 (&00) (&01) UNEXPECTED CONFIGURATION STATE: FOREIGN

### Meaning

The operating system has detected that the HW-Unit (&00) (&01)
doesn't belong to the configuration.
(&00): may be:
SIDE : Side
SE : Storage Element
CPU : Central Processing Unit
(&01): HW-Unit Id.

### Response

None.

## ETMRK31

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK31 (&00) (&01) UNEXPECTED CONFIGURATION STATE: UNDEFINED

### Meaning

The HW-Unit (&00) (&01) was reported to be in an undefined state
(i.e. component does not exist physically).
(&00): may be:
SIDE : Side
SE : Storage Element
CPU : Central Processing Unit
(&01): HW-Unit Id.

### Response

None

## ETMRK33

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK33 (&00) (&01) SVP BUSY

### Meaning

The command could not be carried out because the
Service Processor was busy.
(&00): may be:
SIDE : Side
SE : Storage Element
CPU : Central Processing Unit
(&01): HW-Unit Id.

### Response

HW-Unit should be attached later per /ATTACH-DEVICE-command.

## ETMRK34

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK34 RECONFIGURATION ERROR: (&00)

### Meaning

Something unexpected has happened during reconfiguration.
(&00) gives further information about error and diagnosis.
(&00) = 'STA=*BLOCK': VM2000 status of CPU is 'BLOCKED'.

### Response

If appropriate take SLED for further analysis and send it
to your system engineer.

## ETMRK38

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK38 PATH BETWEEN CHANNEL (&00) AND DEVICE (&01) NOT AVAILABLE. CHECK CONFIGURATION

### Meaning

The path (&00)/(&01) is not available for the system.

### Response

Bring system tables into agreement with the actual hardware
installation either by /REMOVE-DEVICE-CONNECTION command or
by turning on the hardware component.

## ETMRK39

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK39 ***ATTENTION: SERVICE PROCESSOR (SVP) DAMAGE***

### Meaning

SVP-Damage.

### Response

To guarantee that the message will not be ignored an acknowledge is
requested. Call maintenance technician.

## ETMRK4A

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK4A OBJECT SE (STORAGE-ELEMENT) NOT EXISTING ON THIS HARDWARE

### Meaning

The storage element cannot be reconfigured on this hardware.

### Response

None

## ETMRK4B

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK4B OBJECT SIDE NOT EXISTING ON THIS HARDWARE

### Meaning

The HW-Unit SIDE cannot be reconfigured on this hardware.

### Response

None

## ETMRK4C

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK4C DETACHMENT OF SE NOT POSSIBLE AT THE MOMENT

### Meaning

The command /DET *SE is rejected. The specified SE was previously used
for reconfiguration of another storage element.

### Response

None

## ETMRK4D

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK4D ONLY ONE SIDE-RECONFIGURATION ACCEPTED. RECONFIGURATION REJECTED

### Meaning

More then one SIDE cannot be specified in the /ATT *SIDE or /DET *SIDE
command.

### Response

None

## ETMRK4E

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK4E (&00) (&01) -ATTACHMENT REJECTED DUE TO STATE DETACHED-IMPLICITLY

### Meaning

The HW-Unit (&00) (&01) is in 'DETACH-PENDIG' state. Please wait for
end message of the previous command /DET *SIDE.
(&00): may be:
SE : Storage Element
CPU : Central Processing Unit
(&01): HW-Unit Id.

### Response

None

## ETMRK40

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK40 (&00) (&01) DETACH-PENDING STATE, RECONFIGURATION REJECTED

### Meaning

The HW-Unit (&00) (&01) is in 'DETACH-PENDIG' state. Please wait for
end message of the previous command /DET *SIDE.
(&00): may be:
SE : Storage Element
CPU : Central Processing Unit
(&01): HW-Unit Id.

### Response

None

## ETMRK41

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK41 (&00) (&01) COULD NOT BE ATTACHED BY SVP

### Meaning

The HW-Unit (&00) (&01) is not attached due to SVP-Error
(&00): may be:
SIDE : Side
SE : Storage Element
CPU : Central Processing Unit
(&01): HW-Unit Id.

### Response

None

## ETMRK42

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK42 (&00) (&01) COULD NOT BE DETACHED BY SVP

### Meaning

The HW-Unit (&00) (&01) is not detached due to SVP-Error
(&00): may be:
SIDE : Side
SE : Storage Element
CPU : Central Processing Unit
(&01): HW-Unit Id.

### Response

None

## ETMRK43

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK43 SIDE (&00) WAS REPORTED SVP-ERROR (&01)

### Meaning

The Command is rejected due to SVP Error
(&00): may be:
SIDE : SIDE Id.
(&01): SVP-Error (MSSF Call Response) and /HELP hint

### Response

None

## ETMRK44

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK44 SE (STORAGE-ELEMENT) (&00) WAS REPORTED SVP-ERROR (&01)

### Meaning

The Command is rejected due to SVP Error.
(&00): may be:
SE : Storage Element Id.
(&01): SVP-Error (MSSF Call Response) and /HELP hint

### Response

None

## ETMRK45

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK45 (&00) (&01) SIDE TO BE DETACHED CONTAINTS ALL ACTIVE CPU's

### Meaning

The Command /DET *SIDE is rejected. This SIDE contains all active CPU's
(&00): may be:
SIDE : SIDE
(&01): HW-Unit Id.

### Response

None

## ETMRK46

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK46 (&00) (&01) SIDE TO BE DETACHED CONTAINTS ALL ACTIVE SE's

### Meaning

The Command /DET *SE is rejected. This SIDE contains all active SE's
(&00): may be:
SE : Storage Element
(&01): HW-Unit Id.

### Response

None

## ETMRK47

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK47 (&00) (&01) DETACHED PARTIALLY

### Meaning

The command /DET *SIDE was executed but one/more SE(s) or one/more
CPU(s) could not be detached.The Duplex-Mode is not possible.
The reason is specified a previous message.
(&00): may be:
SE : Storage Element
CPU : Central Processing unit
(&01): HW-Unit Id.

### Response

None

## ETMRK48

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK48 (&00) (&01) DETACHED BY SYSTEM

### Meaning

The CPU was detached by system. The reason can be found within the
SERSLOG-file.
(&00): may be:
CPU :
(&01): HW-Unit Id.
To guarantee that the message will not be ignored an acknowledge is
requested.

### Response

Arbitrary.

## ETMRK49

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK49 (&00) (&01)-ID. INVALID. RECONFIGURATION REJECTED

### Meaning

The HW-Unit (&00) (&01) does not exist.
(&00): may be:
CPU : Central Processing Unit
(&01): HW-Unit Id.

### Response

None

## ETMRK5A

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ETMRK5A All Extra-CPU's already attached

### Meaning

Command /ATTACH-DEVICE *EXTRA-CPU rejected, because
all available Extra-CPU's were already attached

## ETMRK5B

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ETMRK5B All Extra-CPU's already detached

### Meaning

Command /DETACH-DEVICE *EXTRA-CPU rejected, because
all available Extra-CPU's were already detached

## ETMRK5C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ETMRK5C Attachment of CPU (&00) not allowed for CPU from (&01) pool

### Meaning

Command /ATTACH-DEVICE (&00) was rejected because a CPU was
specified which is not attachable by this command.
(&00): HW-Unit Id.
(&01): may be:
EXTRA : Extra-CPU
SPARE : Spare-CPU
NORMAL : Normal-CPU

### Response

Extra-CPUs only can be attached by command /ATTACH-DEVICE *EXTRA-CPU
Spare-CPUs only can be attached by system

## ETMRK5D

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ETMRK5D Detachment of CPU (&00) not allowed for CPU from (&01) pool

### Meaning

Command /DETACH-DEVICE *CPU(&00) was rejected because of a CPU was
specified which is not detachable by this command.
(&00): HW-Unit Id.
(&01): may be:
EXTRA : Extra-CPU
SPARE : Spare-CPU
NORMAL : Normal-CPU

### Response

Extra-CPU only can be detached with command /DETACH-DEVICE *EXTRA-CPU

## ETMRK5E

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ETMRK5E Object EXTRA-CPU not existing on this hardware

### Meaning

The HW-Unit EXTRA-CPU cannot be reconfigured on this hardware.

## ETMRK50

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMRK50 ABNORMAL TASK TERMINATION BY RECONFIGURATION***

### Meaning

The task was active when reconfiguration occurred and it was not
possible to save its context. The task was therefore terminated.

### Response

None.

## ETMRK51

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK51 MFA - INVALID LOGICAL MACHINE NUMBER!!

### Meaning

An invalid logical machine number of the failed GP was detected
while processing an MFA-interrupt.

### Response

If necessary, take SLED and send it to your systems engineer.

## ETMRK52

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK52 MFA - RECONFIGURATION BUFFER IS NOT FREE!!

### Meaning

The Reconfiguration Buffer could not be obtained, so the
context of the failed CPU cannot be stored.

### Response

If necessary, take SLED and send it to your systems engineer.

## ETMRK53

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK53 MFA - RECONFIGURATION FAILED!!

### Meaning

The failed CPU could not be detached.

### Response

If necessary, take SLED and send it to your systems engineer.

## ETMRK54

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMRK54 MFA - EXTERNAL INTERRUPT CODE NOT MFA!!

### Meaning

The Interrupt-Code is not Malfunction-Alert.

### Response

If necessary, take SLED and send it to your systems engineer.

## ETMRK58

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ETMRK58 Extra-CPU (&00) attached

### Meaning

Command /ATTACH-DEVICE *EXTRA-CPU (&00) was successfully processed.
(&00): HW-Unit Id.

## ETMRK59

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ETMRK59 Extra-CPU (&00) detached

### Meaning

Command /DETACH-DEVICE *EXTRA-CPU (&00) was successfully processed.
(&00): HW-Unit Id.

## ETMSE01

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMSE01 SYSTEM ERROR ETMSE01 TERMINATED TASK; *** ETMSTXE / ETMTOSM: SYSTEM ERROR ***

### Meaning

None.

### Response

Take systemdump and send it to your systems engineer.

## ETMSE02

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMSE02 SYSTEM ERROR ETMSE02 TERMINATED TASK; ***ETMINTR: PROHIBITED RETURN CODE OCCURRED***

### Meaning

The task was terminated because a $NCTING or a $RELM macro produced
a prohibited return code.

### Response

Take systemdump and send it to your systems engineer.

## ETMSE03

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMSE03 SYSTEM ERROR ETMSE03 TERMINATED TASK; ***ETMTOSMT: PROHIBITED RETURN CODE OCCURRED!***

### Meaning

A return code which indicated a system error occurred.

### Response

Take systemdump and send it to your systems engineer.

## ETMSE04

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMSE04 SYSTEM ERROR ETMSE04 TERMINATED TASK; ***ECETTL: SYSTEM ERROR!***

### Meaning

No further information.

### Response

Take system dump and send it to your systems engineer.

## ETMSE05

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMSE05 PROGRAM ERROR ETMSE05: - ETMTOSM / ETMSTXE - TERMINATED PROGRAM

### Meaning

1. User program error;
2. Program Termination via TERM-Function from the EXIT-Macro;

### Response

User dump will be produced.

## ETMSE06

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMSE06 MAXIMUM RUNTIME OF ABEND-STXIT-ROUTINE EXCEEDED (300 SEK)! PROGRAM TERMINATED

### Meaning

No further information

## ETMSE07

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

ETMSE07 TASK CPU TIME LIMIT exceeded. Task will be terminated.

## ETMSE10

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMSE10 SYSTEM ERROR ETMSE10 TERMINATED TASK; ***ETMSINF: PROHIBITED RETURN CODE OCCURRED***

### Meaning

A return code which indicated a system error occurred.

### Response

Take systemdump and send it to your systems engineer.

## ETMTF01

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTF01 SYSTEM ERROR ETMTF01 TERMINATED SESSION; ***ETMTIMER: ERROR FOR "GET/REL C-LOCK"***

### Meaning

An invalid return code on calling the macro $LOCK (GET/REL C-Lock) led
to system termination. The call was either in SIH or in TPR.

### Response

Take SLED and send it to your systems engineer.

## ETMTF02

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTF02 SYSTEM ERROR ETMTF02 TERMINATED SESSION; ***ETMTIMXP: ERROR FOR "GET/REL C-LOCK"***

### Meaning

An invalid return code on calling the macro $LOCK (GET/REL C-Lock) led
to system termination.

### Response

Take SLED and send it to your technical support.

## ETMTF14

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

ETMTF14 NO CLOCK SYNCHRONISATION PERFORMED. DIFFERENCE BETWEEN SYSTEM CLOCK AND TIME SERVER IS GREATER THAN 15 MINUTES

### Meaning

A time server is connected to the server, which however cannot be
used, since its time differs too much from the system time.

### Response

Check system time and time server (on S server the time server is
configured via SKP manager, on SQ server via SQ manager, and on
SE server via SE manager).
If system clock differs more than 15 minutes, for synchronisation
of system clock the system has to be restarted (clock initialisation
in STARTUP).

## ETMTF20

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTF20 SYSTEM ERROR ETMTF20 TERMINATED SESSION; ***ETMTIMXP: ERROR FOR "RELEASE C-LOCK"***

### Meaning

An error occurred on calling the macro $LOCK to release the C-Lock,
probably because the C-Lock was not held.

### Response

Take SLED and send it to your systems engineer.

## ETMTF21

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTF21 SYSTEM ERROR ETMTF21 TERMINATED SESSION; ***ETMTIMXP: ERROR FOR "$NCTING-CALL"***

### Meaning

The macro $NCTING, which links a TPR-PCB into the PCB-chain of a
task, returned a prohibited return code. $NCTING was
called in SIH, when a real-time interval had elapsed.
The call was made for STXIT processing.

### Response

Take SLED and send it to your systems engineer.

## ETMTL10

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL10 SYSTEM ERROR ETMTL10 LED TO SNAPSHOT; ***NLMLOCK2: ERROR WHILE PROMPTING OPERATOR***

### Meaning

An error occurred while a question was being output
to the operator. As this error had no serious effect
on the system, only a snapshot dump was taken.

### Response

Send snapshot dump to your systems engineer.

## ETMTL11

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL11 ***TASK (&00) TASK-LOCK TIME LIMIT REACHED!***

### Meaning

A task which is waiting for the operator to reply
to a question holds a task-lock. The time-limit
for holding the lock has been reached and the
operator is prompted to input the reply. If the
operator does not respond to the question, the
task will be cancelled after the second reminder.

### Response

The operator should answer the outstanding question.

## ETMTL12

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL12 ***TASK (&00) TASK-LOCK TIME RUNOUT; TERMINATION IN ONE MINUTE!***

### Meaning

A task which has held a task-lock longer than the
specified time-limit is still waiting for a reply
from the operator. This is the final warning; the
task will be terminated if the operator does not
reply to the question within the next minute.

### Response

The operator should answer the question immediately.

## ETMTL13

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL13 SYSTEM ERROR ETMTL13 TERMINATED TASK; ***NLMLOCK2: TASK-LOCK TIME RUNOUT***

### Meaning

A task which was waiting for a response from the operator held a
task-lock for longer than the specified lock-holding-time limit.
The task has been terminated so that the lock can be freed, thus
avoiding problems which might have arisen had the task continued
to hold the lock.

### Response

None.

## ETMTL14

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL14 ***TASK (&00) TASK-LOCK TIME LIMIT REACHED!***

### Meaning

A task which is waiting for paging holds a task-
lock. The time-limit for holding the lock has
been reached without the lock being released.
The lock-holding-time limit will be extended
to give the task another chance to release the
lock.

### Response

None.

## ETMTL15

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL15 ***TASK (&00) TASK-LOCK TIME RUNOUT; TERMINATION IN ONE MINUTE!***

### Meaning

A task which holds a task-lock is still waiting for paging.
This is a final warning before terminating the task.

### Response

None.

## ETMTL16

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL16 SYSTEM ERROR ETMTL16 TERMINATED TASK; ***NLMLOCK2: TASK-LOCK TIME RUNOUT! ***

### Meaning

A task which was waiting for paging held a task-lock for
longer than the specified lock-holding-time limit. The task
has been terminated so that the lock can be freed, thus avoid-
ing problems which might have arisen had the task continued
to hold the lock.

### Response

Take systemdump and send it to your systems engineer.

## ETMTL17

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL17 ***TASK (&00) TASK-LOCK TIME LIMIT REACHED!***

### Meaning

A task which is in a VPASS wait holds a task-
lock. The time-limit for holding the lock has
been reached without the lock being released.
The lock-holding-time limit will be extended
to give the task another chance to release
the lock.

### Response

None.

## ETMTL18

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL18 ***TASK (&00) TASK-LOCK TIME RUNOUT; TERMINATION IN ONE MINUTE!***

### Meaning

A task which holds a task-lock is still in a VPASS wait state.
This is a final warning before terminating the task.

### Response

None.

## ETMTL19

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL19 SYSTEM ERROR ETMTL19 TERMINATED TASK; ***NLMLOCK2: TASK-LOCK TIME RUNOUT! ***

### Meaning

A task in a VPASS wait state held a task-lock for longer than
the specified lock-holding-time limit. The task has been termin-
ated so that the lock can be freed, thus avoiding problems which
might have arisen had the task continued to hold the lock.

### Response

Take systemdump and send it to your systems engineer.

## ETMTL20

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL20 ***TASK (&00) TASK-LOCK TIME LIMIT REACHED!***

### Meaning

A task which is waiting for another lock holds
a task-lock. The time-limit for holding this
lock has been reached without the lock being
released. The lock-holding-time limit will be
extended in the hope that the possible dead-
lock will clear itself.

### Response

None.

## ETMTL21

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL21 ***TASK (&00) TASK-LOCK TIME RUNOUT; TERMINATION IN ONE MINUTE!***

### Meaning

A task which holds a task-lock is still waiting for another
lock. This is a final warning before terminating the task.

### Response

None.

## ETMTL22

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL22 SYSTEM ERROR ETMTL22 TERMINATED TASK; ***NLMLOCK2: TASK-LOCK TIME RUNOUT! ***

### Meaning

A task which was waiting for another lock held a task-lock for
longer than the specified lock-holding-time limit. The task has
been terminated so that this lock can be freed, thus avoiding
problems which might have arisen had the task continued to hold
the lock.

### Response

Take systemdump and send it to your systems engineer.

## ETMTL23

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL23 ***TASK (&00) TASK-LOCK TIME LIMIT REACHED!***

### Meaning

A task which is in a bourse-wait state holds a task-lock.
The time-limit for holding this lock has been reached
without the lock being released. The lock-holding-time
limit will be extended in the hope that the possible
deadlock will clear itself.

### Response

None.

## ETMTL24

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL24 ***TASK (&00) TASK-LOCK TIME RUNOUT; TERMINATION IN ONE MINUTE!***

### Meaning

A task which holds a task-lock is still in a bourse wait state.
This is a final warning before terminating the task.

### Response

None.

## ETMTL25

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL25 SYSTEM ERROR ETMTL25 TERMINATED TASK; ***NLMLOCK2: TASK-LOCK TIME RUNOUT! ***

### Meaning

A task which was in a bourse wait state held a task-lock for
longer than the specified lock-holding-time limit. The task has
been terminated so that this lock can be freed, thus avoiding
problems which might have arisen had the task continued to hold
the lock.

### Response

Take systemdump and send it to your systems engineer.

## ETMTL26

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL26 ***TASK (&00) TASK-LOCK TIME LIMIT REACHED!***

### Meaning

A task which is in an FITC-wait state holds a task-lock.
The time-limit for holding this lock has been reached
without the lock being released. The lock-holding-time
limit will be extended in the hope that the possible
deadlock will clear itself.

### Response

None.

## ETMTL27

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL27 ***TASK (&00) TASK-LOCK TIME RUNOUT; TERMINATION IN ONE MINUTE!***

### Meaning

A task which holds a task-lock is still in an FITC wait state.
This is a final warning before terminating the task.

### Response

None.

## ETMTL28

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL28 SYSTEM ERROR ETMTL28 TERMINATED TASK; ***NLMLOCK2: TASK-LOCK TIME RUNOUT! ***

### Meaning

A task which was in an FITC wait state held a task-lock for
longer than the specified lock-holding-time limit. The task has
been terminated so that this lock can be freed, thus avoiding
problems which might have arisen had the task continued to hold
the lock.

### Response

Take systemdump and send it to your systems engineer.

## ETMTL29

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL29 ***TASK (&00) TASK-LOCK TIME LIMIT REACHED!***

### Meaning

A task which is waiting for a dump-task to finish holds
a task-lock. The time-limit for holding this lock has
been reached without the lock being released. The lock-
holding-time limit will be extended in the hope that
the possible dead-lock will clear itself.

### Response

None.

## ETMTL30

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL30 ***TASK (&00) TASK-LOCK TIME RUNOUT; TERMINATION IN ONE MINUTE!***

### Meaning

A task which holds a task-lock is still waiting for a dump-
task to finish. This is a final warning before terminating
the task which holds the lock.

### Response

None.

## ETMTL31

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL31 SYSTEM ERROR ETMTL31 TERMINATED TASK; ***NLMLOCK2: TASK-LOCK TIME RUNOUT! ***

### Meaning

A task which was waiting for an associated dump-task to terminate
held a task-lock for longer than the specified lock-holding-time
limit. The task has been terminated so that the lock can be freed
and a renewed attempt to take the dump will be made. This will
hopefully help to avoid problems which might have arisen had the
task continued to hold the lock.

### Response

Take systemdump and send it to your systems engineer.

## ETMTL32

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL32 ***TASK (&00) TASK-LOCK TIME LIMIT REACHED!***

### Meaning

A task which is being terminated holds a task-lock. The
time-limit for holding the lock has been reached without
the lock being released. The lock-holding-time limit will
be extended to give the task another chance to release
the lock.

### Response

None.

## ETMTL33

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL33 SYSTEM ERROR ETMTL33 TERMINATED TASK; ***NLMLOCK2: TASK-LOCK TIME RUNOUT! ***

### Meaning

A task which was being terminated held a task-lock for longer
than the specified lock-holding-time limit. The task has been
abnormally terminated so that the lock can be freed, thus avoid-
ing problems which might have arisen had the task continued to
hold the lock.

### Response

Take systemdump and send it to your systems engineer.

## ETMTL34

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL34 ***TASK (&00) TASK-LOCK TIME LIMIT REACHED!***

### Meaning

A task which holds a task-lock appears to be in an
endless loop. The time-limit for holding the lock has
been reached without the lock being released. The lock-
holding-time limit will be extended in the hope that
the possible deadlock will clear itself.

### Response

None.

## ETMTL35

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL35 ***TASK (&00) TASK-LOCK TIME RUNOUT; TERMINATION IN ONE MINUTE!***

### Meaning

The task holding a task-lock still appears to be looping.
This is a final warning before terminating the task which
holds the lock.

### Response

None.

## ETMTL36

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL36 SYSTEM ERROR ETMTL36 TERMINATED TASK; ***NLMLOCK2: TASK-LOCK TIME RUNOUT! ***

### Meaning

The task holding a task-lock still seemed to be in an endless loop,
even after the extended lock-holding-time limit was reached. A
further attempt to terminate the task was made in the hope of
avoiding problems which might arise if the task continues to hold
the lock.

### Response

Take systemdump and send it to your systems engineer.

## ETMTL37

Destination: USER-TASK, CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL37 TASK=(&00) ADDR=(&01) NAME=(&02) PCTR=(&03)

### Meaning

This message is intended for internal use in diagnosing
problems which might arise with task locks. It supplies further
information relating to a preceding message (in the range ETMTL11 ...
ETMTL36) which has indicated that a task has been or will be
terminated because of time runout of a task lock.
(&00) is the TSN (Task Sequence Number) of the task which held the lock.
(&01) is the address of the affected lock.
(&02) is the name of the affected lock. As some lock names include
non-printing characters, the name is printed in both EBCDIC
and hexadecimal forms.
(&03) is the program counter of the $GTLOCK(I)-call.

### Response

Take whatever action is appropriate for the preceding message, using
the information given in this message to help diagnose the problem.
If this is not possible, take a system dump and send it to your
system engineer.

## ETMTL39

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL39 SYSTEM ERROR ETMTL39 LED TO SNAPSHOT; ***NLMLOCK2: ERROR DURING RELEASE OF TLT-LOCK***

### Meaning

$ACCTLT reported an error during the release of a
task's TLT-lock. As this error had no serious effect
on the system, only a snapshot dump was taken.

### Response

Send snapshot dump to your systems engineer.

## ETMTL40

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL40 SYSTEM ERROR ETMTL40 LED TO SNAPSHOT; ***NLMLOCK2: ERROR DURING MESSAGE OUTPUT***

### Meaning

$MSG7X reported an error during message processing. As
this error had no serious effect on the system, only a
snapshot dump was taken.

### Response

Send snapshot dump to your systems engineer.

## ETMTL41

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL41 SYSTEM ERROR ETMTL41 TERMINATED SESSION; ***NLMLOCK3: NO MEMORY AVAILABLE FOR LOCK-INITIALISATION***

### Meaning

No class 3 memory was available for the Task Lock Manager
data areas. Under these circumstances it is not possible
for the system to continue operating.

### Response

Take SLED and send it to your systems engineer.

## ETMTL42

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL42 SYSTEM ERROR ETMTL42 TERMINATED SESSION; ***NLMLOCK3: INTERRUPT WHILE HOLDING TL-CLASS-LOCK***

### Meaning

A synchronous interrupt occurred while the Task-Lock
Manager (TL) class lock was held. The session was
terminated to allow a SLED to be taken.

### Response

Take SLED and send it to your systems engineer.

## ETMTL43

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL43 SYSTEM ERROR ETMTL43 LED TO SNAPSHOT; ***NLMLOCK3: INTERRUPT WHILE HOLDING TL-CLASS-LOCK***

### Meaning

An error (synchronous interrupt) occurred while the Task-Lock
Manager (TL) class lock was held. As the system was in fault-
tolerant mode, only a snapshot dump was taken.

### Response

Send snapshot dump to your systems engineer.

## ETMTL44

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL44 $HVAL DETECTED INVALID PARAMETER ADDRESS

### Meaning

The address of a Task Lock Manager parameter list is invalid and
led to an exception on hard validation. The address output with the
dump indicates where hard validation detected the error.

### Response

Take system dump and send it to your systems engineer.

## ETMTL45

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL45 ***NLMLOCK3: TASK-LOCK-MANAGER ERROR LOG:

### Meaning

This is the header for an entry made in the Error Logging File
by the Task-Lock Manager. A brief explanation of the cause of
the error is also output with this message.

### Response

None.

## ETMTL46

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL46 SYSTEM ERROR ETMTL46 LED TO SNAPSHOT; ***NLMLOCK3: ERROR DURING RELEASE OF CLASS-3 MEMORY***

### Meaning

An error occurred during the release of Class 3 memory
by the Task Lock-Manager. As this error had no serious
effect on the system, only a snapshot dump was taken.

### Response

Send snapshot dump to your systems engineer.

## ETMTL51

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL51 SYSTEM ERROR ETMTL51 LED TO SNAPSHOT; ***NLMLOCK4: ERROR DURING RELEASE OF TLT-LOCK***

### Meaning

$ACCTLT reported an error during the release of a
task's TLT-lock. As this error had no serious effect
on the system, only a snapshot dump was taken.

### Response

Send snapshot dump to your systems engineer.

## ETMTL52

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL52 SYSTEM ERROR ETMTL52 TERMINATED TASK; ***NLMLOCK4: TASK-LOCK DEADLOCK FOR DUMP TASK***

### Meaning

A dump task required a task-lock which was held by the task which
was to be dumped. To avoid a deadlock the dump task was terminated.
The termination of the task which should have been dumped will be
completed without a dump being created.

### Response

None.

## ETMTL53

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL53 SYSTEM ERROR ETMTL53 LED TO SNAPSHOT; ***NLMLOCK4: TASK-LOCK DEADLOCK FOR DUMP TASK***

### Meaning

A dump task required a task-lock which was held by the task which
was to be dumped. To avoid a deadlock the dump task was terminated.
The termination of the task which should have been dumped will be
completed without a dump being created. A snapshot dump is produced
as an alternative to the unavailable system dump.

### Response

Send snapshot dump to your systems engineer.

## ETMTL61

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL61 SYSTEM ERROR ETMTL61 LED TO SNAPSHOT; ***NLMLOCK5: ERROR IN $VALID***

### Meaning

$VALID reported an error to the Task-Lock Manager. As this
error had no serious effect on the system, only a snapshot
dump was taken.

### Response

Send snapshot dump to your systems engineer.

## ETMTL71

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL71 SYSTEM ERROR ETMTL71 LED TO SNAPSHOT; ***NLMLOCK6: ERROR IN $VALID***

### Meaning

$VALID reported an error to the Task-Lock Manager. As this
error had no serious effect on the system, only a snapshot
dump was taken.

### Response

Send snapshot dump to your systems engineer.

## ETMTL72

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

ETMTL72 SYSTEM ERROR ETMTL72 LED TO SNAPSHOT; ***NLMLOCK6: ERROR DURING RELEASE OF TLT-LOCK***

### Meaning

$ACCTLT produced an error-returncode on release of a
task's TLT-lock. As this error had no serious effect
on the system, only a snapshot dump was taken.

### Response

Send snapshot dump to your systems engineer.

©2025 Fujitsu | BS2000 System Messages