## NPC0027

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0027 (&00) BUFFERTASK ERROR DURING '(&01)' MACRO PROCESSING FOR (&02). RC: '(&03)'.

### Meaning

Error in buffertask of subsystem (&00) during call of the (&01) macro for
(&02).
(&00): subsystem name.
(&01): macro name.
(&02): reason for macro call.
(&03): return code from the macro.

## NPC0029

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0029 (&00) DMS ERROR FOR '(&01)'. DMS ERROR CODE: '(&02)'. ERROR INF IN SYSTEM MODE: /HELP-MESS DMS(&02)

### Meaning

Error in subsystem (&00) while writing buffers. No more data are put
out to the file with linkname '(&01)'.
For more detailed information about the DMS error code enter the
SDF command /HELP-MESS or see the manual 'BS2000 System Messages'
or one of the BS2000 DMS manuals.

## NPC0030

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0030 (&00) BUFFER TASK '(&01)' DISABLED

### Meaning

After a DMS error in subsystem (&00) the buffer task puts out
no more data.
(&01): TSN of the buffer task.

### Response

The data gathering should be brought to an end if all buffer tasks
are disabled.

## NPC0033

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0033 ALL (&00) TAPES FOR '(&01)' WRITTEN. BUFFER TASK DISABLED.

### Meaning

All tapes of (&00) file with linkname (&01) are written.

### Response

The data gathering should be brought to an end if all buffer tasks
are disabled.

## NPC0034

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0034 NUMBER OF VSNS FOR (&00) TAPE FILE '(&01)' IS ZERO. BUFFER TASK DISABLED.

### Meaning

After RDTFT in buffer task of subsystem (&00) the number of VSN's
of '(&01)' is zero.
(&01): linkname of the file.

## NPC0035

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0035 KDCMON TERMINATED BY '/STOP-SUBSYSTEM KDCMON,FORCED=YES'.

### Meaning

The system administrator has deleted the KDCMON subsystem, thereby
automatically terminating all tasks still connected to KDCMON.

## NPC0036

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0036 '/RESUME-SUBSYSTEM' NOT SUPPORTED BY COSMOS. REASON FOR FOLLOWING DSSM MESSAGES.

## NPC0037

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0037 COSMOS TERMINATED BY '/STOP-SUBSYSTEM COSMOS,FORCED=YES'

### Meaning

The system administrator has deleted the COSMOS subsystem, thereby
automatically terminating all tasks still connected to COSMOS.

## NPC0038

Destination: USER-TASK Routing code: Weight: 50

Warranty : NO

NPC0038 (&00) ERROR DURING '(&01)' MACRO PROCESSING FOR (&02). RC: '(&03)'.

### Meaning

Error in subsystem (&00) during call of the (&01) macro for (&02).
(&01): macroname.
(&02): reason for macro call.
(&03): return code from the macro.

## NPC0039

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0039 COSMOS FILE '(&00)' TOO SMALL FOR WRAP-AROUND OUTPUT

### Meaning

The file with link name '(&00)' is too small for the output in the
wrap-around mode. The file must be allocated at least big enough for
the informations on the measurement, the module list, the configuration
and the events 4 and 8.

### Response

Allocate more space for the file.

## NPC0050

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0050 ERROR IN COSMOS-PARAMS

### Meaning

Invalid values in COSMOS-params.
The statement has been rejected.

## NPC0051

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0051 NO MEMORY SPACE ALLOCATED FOR FILE: (&00)

### Meaning

Possible reasons:
- No memory space has been allocated for the file.
- The value of the primary allocation is smaller than the block size.

### Response

Allocate the memory space by means of the command /MODIFY-FILE-ATTRIBUTES

## NPC0052

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0052 REQUESTED FILE '(&00)' NOT CATALOGED IN PUBSET

### Meaning

The requested file is not cataloged in the requested pubset.

### Response

Create the file by means of the command /CREATE-FILE.

## NPC0053

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0053 ERROR IN IC-LIST OF EIA-EVENT

### Meaning

Invalid values in interruptcode-list of EIA-event.
The statement has been rejected.

## NPC0054

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0054 ERROR IN STATEMENT '//ADD-/REMOVE-COSMOS-EVENT'

### Meaning

Invalid values in eventlist of command ADD-/REMOVE-COSMOS-EVENT.
The statement has been rejected.

## NPC0055

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0055 '//SET-COSMOS-PARAMETER' STATEMENT NOT SPECIFIED

### Meaning

The statement //ADD-COSMOS-EVENT, //REMOVE-COSMOS-EVENT,
//MODIFY-COSMOS-PARAMETER, //INIT-COSMOS or //START-MEASUREMENT-PROGRAM
COSMOS cannot be specified unless //SET-COSMOS-PARAMETER statement
is specified.
The statement has been rejected.

### Response

Enter the statement //SET-COSMOS-PARAMETER and repeat your original
entry.

## NPC0056

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0056 STATEMENT '(&00)' NOT ALLOWED

### Meaning

The statement //SET-COSMOS-PARAMETER, //MODIFY-COSMOS-PARAMETER,
//ADD-COSMOS-EVENT or //REMOVE-COSMOS-EVENT are not allowed between the
statements //INIT-COSMOS and //START-MEASUREMENT-PROGRAM COSMOS.
The statement has been rejected.

## NPC0057

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0057 SYSTEM ERROR DURING CREATE OF SUBSYSTEM COSMOS.

### Meaning

Error in starting of the subsystem COSMOS during //INIT-COSMOS or
//START-MEASUREMENT-PROGRAM COSMOS.
You can determine the detailed error cause using the trace entries
of the //SHOW-SM2-STATUS function.

## NPC0058

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0058 SYSTEM ERROR IN COSMOS-MODULES

### Meaning

A system error has occured in COSMOS during program execution.
You can determine the detailed error cause using the trace entries of
the //SHOW-SM2-STATUS function.

## NPC0059

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0059 WARNING : '(&00)' NOT FOUND IN SYSTEM

### Meaning

When defining the monitoring program COSMOS, an value (JOBNAME,CATEGORY,
TSN,USERID) for the parameter TASK-SELECTION was specified that could
not be found in the system at the time of the measurement initialization
or the measurement start.

## NPC0060

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0060 WARNING : MACRO-ERROR DURING COSMOS EXECUTION

### Meaning

During COSMOS-execution a macro returned an error.
For more infos you can determine the detailed error cause using
the trace entries of the //SHOW-SM2-STATUS function.

## NPC0061

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0061 ERROR IN COSMOS-WRITETASK

### Meaning

The buffer task for the file with linkname '(&00)' returns an error.
You can determine the detailed error cause using the trace entries
of the //SHOW-SM2-STATUS function.

## NPC0062

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0062 MONITORING PROGRAM COSMOS ALREADY INITIALIZE. STATEMENT REJECTED

### Meaning

An attempt was made to initialize the monitoring program COSMOS
that has already been initialize or start.

## NPC0063

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPC0063 ERROR DURING START OF UTM MEASUREMENT. MEASUREMENT PROGRAM COSMOS NOT STARTED.

### Meaning

Event UTM cannot be opened, because the subsystem UTM is not created.
Statement //INIT-COSMOS or //START-MEASURMENT-PROGRAM COSMOS rejected.

### Response

Create subsystem UTM first and then start the COSMOS measurement.

## NPC0064

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPC0064 ERROR DURING PROCESSING OF COSMOS MEASUREMENT FILE: '(&00)'

### Meaning

You can determine the detailed error cause using the trace
entries of the //SHOW-SM2-STATUS function.

## NPC0065

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPC0065 INVALID FCBTYPE OF COSMOS MEASUREMENTFILE

### Meaning

The indicated file exists already and does not have the FCBTYP PAM.

### Response

Create a new file or access a file with correct FCBTYP PAM.

## NPC0066

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPC0066 DMS-ERROR IN COSMOS-MEASUREMENTFILE '(&01)'. DMS-CODE '(&00)'. /HELP-MSG DMS(&00).

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG
or see the BS2000 manual 'System messages'.

## NPC0067

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPC0067 ERROR DURING MACROPROCESSING 'DCAMPNSM'.

## NPC0068

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPC0068 FILE WITH LINKNAME 'COSFIL' NOT FOUND.

### Meaning

Possible reasons:
- The COSMOS measurement file assigned by LINK=COSFIL is not in the
COSMOS parameter list.
- The COSMOS measurement file assigned by LINK=COSFIL does not exist.

### Response

Enter the statement //SET-COSMOS-PARAMETER with the COSMOS measurement
file assigned by LINK=COSFIL as parameter or create a COSMOS measurement
file with LINK=COSFIL.

## NPC0069

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPC0069 ERROR DURING RDTFT-MACROPROCESSING.

## NPC0070

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPC0070 SUBSYSTEM COSMOS NOT FOUND.

## NPC0071

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPC0071 TO MANY MEASUREMENT FILES SPECIFIED.

### Meaning

More than one measurement file for OUTPUT=*WRAP-AROUND(...) was
specified.

### Response

Enter the statement //SET-COSMOS-PARAMETER with only one measurement
file for WRAP-AROUND.

## NPC0072

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPC0072 WRONG MEASUREMENT FILE SPECIFIED

### Meaning

For VM2000- and COSMOS-Events the same measurement file was specified.

### Response

Correct the statement and try again.

## NPC0073

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPC0073 MEASUREMENT FILE FOR VM2000-EVENTS NOT SPECIFIED

### Meaning

Measurement file for VM2000-Events was not specified in statement
//SET-/MODIFY-COSMOS-PARAMETER.

### Response

Correct statement and try again or close the VM2000-Events.

## NPC0074

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPC0074 ERROR DURING START OF SUBSYSTEM BCAM-COS. MEASUREMENT PROGRAM COSMOS NOT STARTED.

### Meaning

The event BCAM resp. BCPT cannot be opened, because the subsystem
BCAM-COS could not be loaded.
The instruction //INIT-COSMOS resp. //START-MEASUENT-PROGRAM COSMOS was
rejected.
BCAM-COS is not installed or has wrong version.

### Response

Install subsystem BCAM-COS first and then start the COSMOS measurement.

## NPC0075

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NPC0075 ERROR DURING START OF SUBSYSTEM DCAM-COS. MEASUREMENT PROGRAM COSMOS NOT STARTED.

### Meaning

The event DCAM cannot be opened, because the subsystem DCAM-COS could not
be loaded. Statement //INIT-COSMOS or //START-MEASURMENT-PROGRAM COSMOS
rejected.
DCAM-COS is not installed or has wrong version.

### Response

Install subsystem DCAM-COS first and then start the COSMOS measurement.

## NPC0100

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

NPC0100 KDCMON version (&00) for BS2000 version (&01) started.

©2025 Fujitsu | BS2000 System Messages