## NJA0001

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

NJA0001 D.E.R initialized successfully

### Meaning

The device error recovery has been successfully initialized.

### Response

## NJA0002

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

NJA0002 Error during initialization of D.E.R (&00) returncode: (&01)

### Meaning

An error occurred during the initialization of the device error
recovery, which may degrade some logging functions of the D.E.R
The standard device error recovery actions are still functional.
(&00): identifier of the failing system function
(&01): returncode of the failing system function
Such an error never occurs if the operating system is correctly
configured.
Some diagnostic information was written to the software error
logging file (SERSLOG).

### Response

Call the software service.
Necessary diagnostic material:
Software error logging file (SERSLOG) or Dump (SLED).

## NJA0003

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

NJA0003 D.E.R server task DER1 started

### Meaning

The D.E.R server task (TSN=DER1) has been started successfully.

### Response

## NJA0004

Destination: CONSOLE Routing code: A Weight: 99

Warranty : NO

NJA0004 D.E.R server task DER1 stopped

### Meaning

The D.E.R server task (TSN=DER1) has been terminated, caused by
an invalid order, but restarts automatically.
Such an error never occurs if the operating system is correctly
configured.
Some diagnostic information was written to the software error
logging file (SERSLOG).

### Response

Call the software service.
Necessary diagnostic material:
Software error logging file (SERSLOG) and Dump (SLED).

## NJA0010

Destination: CONSOLE Routing code: A Weight: 30

Warranty : NO

NJA0010 Syntax error in command '(&00)'. Command rejected

## NJA0101

Destination: CONSOLE Routing code: X Weight: 01

Warranty : NO

NJA0101 D.E.R-TRACE: (&00) (&01) (&02) ((&03)): (&04)

### Meaning

This message issues a trace record of the device error recovery
(D.E.R). It is issued, if the trace function, which is normally
deactivated, is switched on for diagnostic purpose.
Activation of the trace function is only possible by a REP-
correction at the moment.
Meaning of message inserts:
(&00): Time in format 'YYYY-MM-DD-hh:mm:ss.uuuuuu' (26 char.)
(&01): D.E.R call identifier (8 char.)
(&02): Record identifier (3 char.)
(&03): Meaning (32 char.)
(&04): Data: 44 bytes, printable hex. (88 char.)

### Response

Call the software service.
Necessary diagnostic material:
CONSLOG-file with these messages

## NJA0201

Destination: CONSOLE Routing code: X Weight: 01

Warranty : NO

NJA0201 D.E.R-DIAG: AREA-DUMP written successfully ((&00))

### Meaning

This message confirms the successsful writing of a diagnostic dump.
This function is normally deactivated and may only be switched on
by a REP correction.
The text insert gives further explanations about the result.

### Response

Call the software service.
Necessary diagnostic material: The written dump file

## NJA0202

Destination: CONSOLE Routing code: X Weight: 01

Warranty : NO

NJA0202 D.E.R-DIAG: Error when writing an AREA-dump ((&00))

### Meaning

The writing of a diagnostic dump was unsuccessful.
The text insert gives further explanations about the result.

### Response

Call the software service.
Necessary diagnostic material: This message

## NJA0203

Destination: CONSOLE Routing code: X Weight: 01

Warranty : NO

NJA0203 D.E.R-DIAG: SYSTEM-DUMP written successfully ((&00))

### Meaning

This message confirms the successsful writing of a diagnostic dump.
This function is normally deactivated and may only be switched on
by a REP correction.
The text insert gives further explanations about the result.

### Response

Call the software service.
Necessary diagnostic material: The written dump file

## NJA0204

Destination: CONSOLE Routing code: X Weight: 01

Warranty : NO

NJA0204 D.E.R-DIAG: Error when writing a SYSTEM-dump ((&00))

### Meaning

The writing of a diagnostic dump was unsuccessful.
The text insert gives further explanations about the result.

### Response

Call the software service.
Necessary diagnostic material: This message

©2025 Fujitsu | BS2000 System Messages