## SEDREVI

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SEDREVI COMP=SEDMF,VERS=91A,DATE=201215

## SED2001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED2001 INTERNAL ERROR: (&00)

### Meaning

An internal error occurred while executing the current RECOVERY statement.

### Response

Refer to the SQL state of the application program.

## SED2002

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED2002 UNABLE TO ACCESS LOGFILE (&00)

### Meaning

An error occurred while executing the current RECOVERY statement
to open the logfile (&00).

### Response

Refer to the SQL state of the application program.

## SED2202

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2202 ERROR WHEN ASSIGNING OUTPUT FILE (&00)

### Meaning

The specified output file (&00) could not be assigned using the
/ASSIGN-SYSLST command. More detailed information about the error
was already output by the command interpreter.

### Response

Specify a file for the output file parameter to which the SYSLST file can
be assigned using the ASSIGN-SYSLST command.

## SED2203

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2203 DMS ERROR (&01) OCCURRED AT COMMAND SHOW-FILE-ATTRIBUTES ON FILE (&00)

### Meaning

none

### Response

none

## SED2204

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2204 VERSION OF INPUT-FILE IS (&00)

### Meaning

The SESAM/SQL version of the input-file is not the actual version.
The file cannot be processed.

### Response

Retry with the same SESAM/SQL version of the input-file.

## SED2205

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2205 SHORTAGE OF RESOURCES

### Meaning

There is no more mainmemory for SEDI70

### Response

none

## SED2206

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2206 (&00) IS NOT EXISTING

### Meaning

none

### Response

none

## SED2207

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2207 THE FILE (&00) CANNOT BE OPENED BECAUSE OF DMS ERROR (&01)

### Meaning

none

### Response

none

## SED2208

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2208 FILE (&00) CANNOT BE OPENED

### Meaning

none

### Response

none

## SED2209

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2209 ERROR RETURNED FROM EXTERNAL FUNCTION (&00)

### Meaning

The external function (&00) recognized and reported an error.

### Response

Generate dump and submit to diagnostics.

## SED2210

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2210 ERROR RETURNED FROM SDF CALL (&00), RETURNCODE X"(&01)"

### Meaning

An unexpected return code was returned for the SDF macro call (&00);
return code X"(&01)".

### Response

Remove error if possible, or generate dump and submit for diagnostics.

## SED2211

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2211 PROGRAM NOT KNOWN IN SDF SYNTAX FILE OR WRONG VERSION OF SDF SYNTAX FILE

### Meaning

The SEDI70 program is not known in the SDF syntax file or the version
of the SDF syntax file is incorrect.

### Response

Assign the correct SDF syntax file.

## SED2212

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2212 NO EXECUTABLE SDF STATEMENT ENTERED

### Meaning

Only the //END statement was submitted to SEDI70.

## SED2213

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2213 INTERNAL ERROR ON DATA CONVERSION

### Meaning

Error on data conversion from internal to external format
while processing the input-file.

### Response

please send dump and input-file to the
software-service for diagnostics

## SED2214

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2214 INTERNAL ERROR

### Meaning

Error on interpreting file-structure
while processing the input-file.

### Response

please send dump and input-file to the
software-service for diagnostics

## SED2215

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2215 FILE (&00) IS NOT EXISTING

### Meaning

none

### Response

none

## SED2216

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2216 FILENAME (&00) IS AMBIGIOUS

### Meaning

none

### Response

none

## SED2220

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2220 FORMAT OF STATEMENT (&00) IN SYNTAX FILE INCORRECT, OR WRONG SYNTAX FILE ASSIGNED

### Meaning

The format of the entered statement differs from the format expected for
statement (&00), or a wrong SDF syntax file was assigned.

### Response

Enter correct statement or assign correct syntax file.

## SED2221

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2221 SYNTAX ERROR IN CREATE-REPORT STATEMENT, OPTION (&00), PARAMETER (&01)

### Meaning

A syntax error was detected in the CREATE-REPORT statement.
(&00) refers to the option concerned.
(&01) refers to the parameter concerned.

### Response

Correct syntax error.

## SED2222

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2222 BY-SELECT NOT FOLLOWED BY ANY CRITERIA

### Meaning

USERS *BY-SELECT was specified, but the parameters HOST-NAME, APPLICATION-
NAME and CUSTOMER-NAME contained no value other than *NONE.

### Response

Specify USERS *ALL, or specify a value other than *NONE for the HOST-NAME,
APPLICATION-NAME or CUSTOMER-NAME parameter.

## SED2223

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2223 INVALID INTERVAL SPECIFIED IN OPTIONS SUB-NUMBER-FROM UND SUB-NUMBER-TO

### Meaning

The interval specified in the options SUB-NUMBER-FROM and SUB-NUMBER-TO
contains a SUB-NUMBER-FROM value that exceeds the SUB-NUMBER-TO value.

### Response

Specify lower value for SUB-NUMBER-FROM than for SUB-NUMBER-TO.

## SED2224

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SED2224 LOGGING FILE (&00) IS ON TAPE AND WILL THEREFORE BE SKIPPED.

### Meaning

keiner

### Response

keiner

## SED6100

Destination: USER-TASK, CONSOLE Routing code: U Weight: 98

Warranty : NO

SED6100 INCORRECT INPUT. REPLY (R=REPEAT; H=HALT)

### Meaning

The input is not correct. Defective control statement or space for
response or inquiry area exhausted.

### Response

R: Repeat input
H: Terminate program.

## SED6101

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6101 STATUSXX

### Meaning

Output of status messages.

## SED6102

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6102 ' H 'LABEL' ' OR ' W 'LABEL' '

### Meaning

Text output.

## SED6103

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6103 SEDI61 - DATA OUTPUT ON TAPE

### Meaning

Text output.

## SED6104

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6104 ' T ..': OUTPUT STRUCTURE

### Meaning

Program execution message.

## SED6105

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6105 ' A ..' OR ' AC'..' ' OR ' AX'..' ': DML STATEMENT

### Meaning

Text output.

## SED6106

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6106 ' F ..' OR ' FC'..' ' OR ' FX'..'': VALUE FOR INQUIRY AREA

### Meaning

Text output.

## SED6107

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6107 ' Q ..' OR ' QC'..' ' OR ' QX'..' ': FILE IDENTIFIER

### Meaning

Text output.

## SED6108

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6108 '$' OR ' * ': REQUEST COMPLETE

### Meaning

Program execution message.

## SED6109

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6109 ERROR '(&00)'

### Meaning

An entry was identified as incorrect or an error occurred during
processing, the cause of which was a logically incorrect entry.
(&00): Error number (See the manual "SESAM/SQL-Server Messages",
chapter "Messages from SEDI61/SEDI61L")

## SED6110

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6110 RECORDS OUTPUT:...(&00)

### Meaning

Output of text.
(&00): Number of records output

## SED6111

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6111 BLOCKS OUTPUT:..(&00)

### Meaning

Output of text.
(&00): Number of blocks output

## SED6112

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6112 USER ADDRESS SPACE TOO SMALL

### Meaning

It is impossible to allocate sufficient address space due to main memory
shortage. The program is terminated.

### Response

Make the virtual address space expand and reload program.

## SED6113

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6113 END OF FILE REACHED DURING PROCESSING OF INPUT FILE

### Meaning

EOF was reached while the input file was being processed, although no END
statement has been encountered.

## SED6115

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SED6115 AN ERROR OCCURRED (STATUS (&00)) DURING EXECUTION OF AN INTERNAL ATTRIBUTE INFORMATION.

### Meaning

An error occurred (Status <> '00') during execution of an internal
attribute information. For that reason the output cannot be formatted
according to the information given by the T statement.

### Response

Check the status (see the manual "SESAM/SQL-Server Messages") and fix
the problem if possible.

## SED6300

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6300 WROUT,HEXADECIMAL,STATUSXX

### Meaning

This message lists possible control statements for SEDI63:
WROUT Log to printer and terminal
HEXADECIMAL Print edit responses and output in hexadecimal format
STATUSXX Output additional error information in status messages

## SED6301

Destination: USER-TASK, CONSOLE Routing code: U Weight: 98

Warranty : NO

SED6301 INCORRECT INPUT. REPLY (R=REPEAT; H=HALT)

### Meaning

The input is not correct, invalid or defective control statement or space
for response or inquiry area is exhausted.

### Response

R: Repeat input
H: Terminate program.

## SED6302

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6302 ' A ..' OR ' AC'..' ' OR ' AX'..' ': DML STATEMENT

### Meaning

Text output.

## SED6303

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6303 ' F ..' OR ' FC'..' ' OR ' FX'..' ': VALUE FOR INQUIRY AREA

### Meaning

Text output.

## SED6304

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6304 ' Q ..' OR ' QC'..' ' OR ' QX'..' ': FILE IDENTIFIER

### Meaning

Text output.

## SED6305

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6305 '$NN' OR ' * ': END OF REQUEST

### Meaning

Program execution message.

## SED6306

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6306 NN: REPEAT FACTOR

### Meaning

Text output.

## SED6307

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED6307 END OF FILE REACHED DURING PROCESSING OF INPUT FILE

### Meaning

EOF was reached while the input file was being processed, although no END
statement has been encountered.

## SED6308

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SED6308 ERROR ON DYNAMICALLY LINKING MODULE (&00). PROGRAM TERMINATED WITH DUMP.

### Meaning

An error occurred while dynamically linking the module (&00), because, for
instance, the module was not found in the assigned module libraries.

### Response

Assign the module library containing the module and repeat the run. If the
error occurs again, send the error documentation in for system diagnosis.

## SED8000

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8000 NO OPEN ON SESAM DB '(&00)' POSSIBLE

## SED8001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8001 NAME OF TRANSFER FILE

## SED8002

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8002 NAME OF DATABASE

## SED8003

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8003 IDENTIFICATION FOR NAM STATEMENT

## SED8004

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8004 PASSWORD

## SED8005

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8005 DATABASE CANNOT BE CLOSED

## SED8006

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8006 SESAM STATUS: '(&00)'

## SED8007

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8007 DATABASE WAS RESET

## SED8008

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8008 DMS ERROR '(&00)'. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or refer to the BS2000 'System Messages' manual.

## SED8009

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8009 THE SPECIFIED FILE '(&00)' IS NOT A VALID TRANSFER FILE

## SED8010

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8010 A SECOND HEADER RECORD WAS FOUND IN THE TRANSFER FILE

## SED8011

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8011 ONLY THE 1ST PART OF THE TRANSFER FILE WAS STORED IN THE DATABASE

## SED8012

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8012 THE TRANSFER FILE CANNOT BE CLOSED

## SED8013

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8013 ATTRIBUTE '(&00)' DOES NOT MATCH ATTRIBUTE IN DATABASE

## SED8014

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8014 THE DATABASE CANNOT BE RESET

## SED8015

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8015 PROGRAM ERROR

## SED8016

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8016 'SEZIX140' AND 'SEZRC140' CANNOT BE FOUND

## SED8017

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8017 NAME OF TRANSFER FILE: '(&00)'

## SED8018

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8018 NUMBER OF LOADED RECORDS: (&00)

## SED8019

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8019 NAME OF TO-DATABASE: '(&00)'

## SED8021

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED8021 NO OPEN ON TRANSFER FILE (&00) POSSIBLE

### Response

Check transfer file (locked?, not existing? ...).

## SED8022

Destination: USER-TASK, CONSOLE Routing code: U Weight: 30

Warranty : NO

SED8022 PROCESSING STARTED

## SED9001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED9001 CONSISTENCY CHECK IN SERVICE TASK (&00) XX/(&01)/(&02) (&03)

### Meaning

Internal error in service task
(&00) : module name
(&01) : error weight
(&02) : error number
(&03) : error subnumber

### Response

Submit the error documentation compiled by the service task to diagnostics
staff.

## SED9002

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED9002 DMS ERROR (&00) IN SERVICE TASK

### Meaning

An error occurred during a DMS operation.

### Response

Use the /HELP-MSG-INFORMATION DMS(&00) command to display the DMS message
text and take appropriate action.

## SED9003

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED9003 BS2000 SORTING ABORTED WITH MESSAGE SRT(&00) DUE TO DMS ERROR

### Meaning

A sort operation with the BS2000 sort was aborted with the message
SRT(&00). A possible reason is that there is not sufficient space for
creating a SORT work file.

### Response

Analyze the cause using the SYSLST and SYSOUT files and the SORT manual.
Remove the cause and repeat SQL statement.

## SED9010

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED9010 HSMS JOB TERMINATED SUCCESSFULLY.

## SED9011

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED9011 HSMS JOB TERMINATED WITH WARNING OR ERROR.

### Meaning

The HSMS job was not fully executed.

### Response

Refer to the HSMS log for the cause of the error, and repeat
the COPY or RECOVER or CREATE REPLICATION if necessary.

## SED9012

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED9012 HSMS JOB REJECTED DUE TO AN INTERNAL ERROR.

### Meaning

The HSMS statement generated by SESAM was not executed due to an internal
error. The error was caused by HSMS or by SESAM.

### Response

Save service task dump and protocol and submit it to diagnostics staff.

## SED9013

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED9013 HSMS JOB ABORTED BECAUSE OF TIMEOUT.

### Meaning

The maximum wait time for the acceptance or the termination of an HSMS
request elapsed. If the request was already accepted but not yet
terminated, then HSMS statement processing was continued asynchronously.

### Response

Possibly the maximum wait time (REQUEST-WAIT-LIMITS) is to be modified
by the HSMS administrator.
Repeat the COPY or RECOVER or CREATE REPLICATION after eliminating
the cause of the error; if necessary wait for the termination of
the previous asynchronously continued HSMS request.

## SED9015

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED9015 HSMS BACKUP FILES

## SED9016

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED9016 HSMS RESTORE FILES

## SED9017

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED9017 ASYNCHRONOUS HSMS JOB STARTED SUCCESSFULLY.

## SED9018

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED9018 ASYNCHRONOUS HSMS JOB ABNORMALLY TERMINATED DURING INITIALISATION.

### Meaning

The HSMS job was not fully executed.

### Response

Refer to the HSMS log for the cause of the error, and repeat
the COPY if necessary.

## SED9020

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED9020 ARCHIVE JOB TERMINATED SUCCESSFULLY

## SED9021

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED9021 ARCHIVE JOB TERMINATED WITH WARNING OR ERROR

### Meaning

The ARCHIVE job was not fully executed.

### Response

Refer to the ARCHIVE log for the cause of the error, and repeat
the COPY or RECOVER or CREATE REPLICATION if necessary.
Moreover, possibly a HSMS run had been intended, but the name of the
HSMS parameter file was incorrect.

## SED9022

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED9022 ARCHIVE JOB REJECTED DUE TO AN INTERNAL ERROR

### Meaning

The ARCHIVE statement generated by SESAM was not executed due to an
internal error. The error was caused by ARCHIVE or by SESAM.

### Response

Save service task dump and protocol and submit it to diagnostics staff.

## SED9025

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED9025 ARCHIVE BACKUP FILES

## SED9026

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SED9026 ARCHIVE RESTORE FILES

©2025 Fujitsu | BS2000 System Messages