## SPA0001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPA0001 '(&00)' ERROR CODE '(&01)'. SPOOLOUT REQUEST ABORTED

### Meaning

An error occurred during spoolout request processing.
(&00): EAM : EAM error
REQ : user request error
PUTQ: put queue error
REQM: request memory error
DMS : DMS error
CAT : catalog error.
(&01): specific error code belonging to (&00)
04: queue routine error
0C: catalog error
10: EAM processing error
18: password validation failure
1C: $REQM error (LOGOFF only)
20: $RELM error (LOGOFF only)
24: parameter validation failure
28: cannot erase unowned file
2C: non-shareable file
30: record size and block size are zero
34: creation date, expiration date or last page used is 0
38: file not SAM, PAM or ISAM
3C: invalid parameter address
40: EAM OMF (object module file) not existing
44: EAM file contains no data
48: invalid ERASE option (FGG (file generation group) files)
54: RFA mode not supported in SPOOL
58: DEVIN for a not SAM tape file
60: tape without STD labels
64: system file is not PRIMARY
68: system file does not exist
6C: FLUSH/CLOSE error on system file
70: File currently in use and therefore locked.
If a DMS error code is output, for more detailed information about this
error code enter /HELP-MSG in system mode or see the BS2000 manual
'System Messages'.

## SPA0002

Destination: USER-TASK, CONSOLE Routing code: S Weight: 99

Warranty : NO

SPA0002 $VALID ERROR FOR SPOOL REQUEST P/L

### Meaning

The parameter list address is not correct.

## SPA0003

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPA0003 SPOOL NOT LOADED OR NOT READY. COMMAND TERMINATED

### Response

Try again later or contact the system administrator.

## SPA0004

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPA0004 SYSTEM ERROR. COMMAND REJECTED

### Meaning

A system error has occurred during the command processing.

### Response

Contact the system administrator.

## SPA0005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPA0005 INVALID PARAMETER LIST ALIGNMENT. COMMAND REJECTED

### Meaning

The address of the $SSVRQ parameter list is not aligned.

### Response

Correct the address and try again the command.

## SPA0006

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPA0006 ERROR CODE '(&00)' IN TSN REASSIGNMENT INTERFACE. STARTUP ABORTED. IN SYSTEM MODE: /HELP-MSG DMS(&00).

### Meaning

An error (&00) has occurred during processing of the TSN reassignment.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## SPA0007

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPA0007 OLD EQUISAMQ FILE CANNOT BE PROCESSED DUE TO DMS ERROR '(&00)'. STARTUP CONTINUED AS COLD START. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

During the EQS startup, the queue file cannot be processed due
to DMS error (&00).
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## SPA0008

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPA0008 $DCALOCK ERROR CODE '(&00)' FOR FILE '(&01)'. PROCESSING CONTINUED

### Meaning

The attempt to restore the lock on the print file (&01) resulted in an
error.
For more detailed information about the $DCALOCK error code see the
BS2000 manual 'System Messages'.

## SPA0009

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPA0009 WARNING: BLOCKS DESTROYED OF OLD EQUISAMQ FILE. PROCESSING CONTINUED WITH RECORD ALREADY PROCESSED

### Meaning

A problem occurs during the check of the EQUISAMQ file.
The records already processed by the $VRIF macro are kept and
the remaining records of the file are lost.

## SPA0010

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPA0010 DMS ERROR '(&00)' DURING PROCESSING 'GET,'FILE' OR 'OPEN' MACRO. STARTUP ABORTED. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

## SPA0011

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPA0011 EQUISAMQ ACCESS NOT POSSIBLE. 'IMCAT' OR 'EXCAT' PROCESSING FOR SPOOL JOBS ABORTED. PROCESSING CONTINUED

### Meaning

The EQUISAMQ file is locked by a further /IMCAT or /EXCAT command or by
the SPOOL startup. The state of the SPOOL jobs for the processed PVS is
not changed in the EQUISAMQ file.

## SPA0012

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPA0012 REQUEST MEMORY ERROR. 'IMCAT' OR 'EXCAT' PROCESSING FOR SPOOL JOBS ABORTED. PROCESSING CONTINUED

### Meaning

An internal problem of request memory occurs during the processing. The
state of the SPOOL jobs for the processed PVS is not changed in the
EQUISAMQ file.

## SPA0013

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SPA0013 DMS ERROR '(&00)' ON EQUISAMQ FILE. IN SYSTEM MODE: /HELP-MSG DMS(&00)

### Meaning

(&00): DMS error code.
For more detailed information about the DMS error code enter /HELP-MSG in
system mode or see the BS2000 manual 'System Messages'.

### Response

Take measure corresponding the DMS error code.
If required, take a system dump and create a new EQUISAMQ file by making
a cold start.

## SPA0015

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0015 Invalid specification in the string operand given during the start-up of SPOOLSYS subsystem. SPOOLSYS subsystem start-up aborted

## SPA0016

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0016 Internal error during the anchor processing of the SPOOLSYS XVT. SPOOLSYS subsystem start-up aborted

## SPA0017

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0017 Invalid specification in the '(&00)' parameter file. SPOOLSYS subsystem start-up aborted

## SPA0018

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0018 '(&00)' subsystem not loaded or not ready. Command terminated

### Meaning

(&00): subsystem name

### Response

Contact the System Administrator and retry later.

## SPA0100

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0100 DMS error '(&00)' with interface '(&01)' for file '(&02)'. Further information: /HELP-MSG DMS(&00)

### Meaning

(&00) : DMS error code
(&01) : DMS interface name
(&02) : filename

## SPA0101

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0101 System error. Command abnormally terminated

### Meaning

An error occurred during the call of a system interface.
More information can be found in SERSLOG file with RECTYPE=SPA0000.

## SPA0102

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0102 Command abnormally terminated

### Meaning

The command has been abnormally terminated.
More information can be found in the previous message(s).

## SPA0103

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0103 Command currently processed by another task

### Meaning

The command may not be processed simultaneously by several tasks.

### Response

Retry command later.

## SPA0104

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0104 FROM-FILE and TO-FILE operands may not be equivalent

### Meaning

The FROM-FILE and TO-FILE operands may not refer to the same file.

### Response

Correct command and retry.

## SPA0105

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPA0105 Original tsn '(&00)' of print job has been changed into tsn '(&01)'

### Meaning

The print job TSN has been changed because this tsn already exists
on the system where the print job has been moved.
(&00) : original print job tsn
(&01) : new print job tsn

## SPA0106

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPA0106 SPOOL task '(&00)' error '(&01)' from '(&02)' interface for tsn '(&03)'. Processing aborted

### Meaning

An error (&01) occurred on (&00) task, when processing (&02) interface
on print job (&03).

### Response

Contact the Print-Service Administrator.

## SPA0107

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPA0107 Internal error '(&00)' from module '(&01)'. Processing aborted

### Meaning

An internal error (&00) occurred in (&01) module.
This message is sent for diagnosis purposes.

### Response

Contact the Print-Service Administrator.

## SPA0108

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0108 SPOOL subsystem currently being loaded or unloaded. Retry command later

### Meaning

The system standard EQUISAMQ file is to be processed by the current
command; however, the SPOOL subsystem, which also uses this file
is currently in an intermediate status

### Response

Wait until SPOOL is completely loaded or unloaded
and try the command again.

## SPA0109

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPA0109 Class '(&00)' memory request error. Processing aborted

### Meaning

(&00) : memory class

### Response

Contact the System Administrator.

## SPA0110

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0110 /MOVE-PRINT-JOBS command currently processed. Retry command later

### Meaning

The system standard EQUISAMQ file is to be processed by SPOOL subsystem;
however, a /MOVE-PRINT-JOBS command currently uses this file.

### Response

Wait until the command is completely processed
and try again to start/resume or stop/hold SPOOL subsystem.

## SPA0111

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0111 Command successfully processed

## SPA0112

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0112 No print job corresponds to the specified operand values. Command not processed

## SPA0113

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0113 Command partially processed

## SPA0114

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0114 '(&00)' print job(s) processed. Command terminated

### Meaning

(&00) : number of print jobs corresponding to the selection criteria
that have been moved.

## SPA0115

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0115 '(&00)' print job(s) not processed due to '(&01)' error

### Meaning

(&00): number of print jobs corresponding to the selection criteria
that have not been moved.
(&01): error cause:
- 'file lock' means that an error occurred when trying to lock
a file related to one of the selected print jobs
(a.o. when the file is located on a non accessible pubset,...)
- 'sysdprnt catid' means that the current default SYSDPRNT catid
does not correspond to the one associated with the print job
to move
- 'SPOOL status' means that SPOOL subsystem was loaded
when tsn collision occurred during processing of distributed
print jobs
'WRONG HOST' means that the target host does not fit for the
print job: either a client copy of a print job is moved onto its
server host or a server copy of a print job is moved onto
its client host.

## SPA0116

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0116 '(&00)' subsystem ready: /MOVE-PRINT-JOBS command may not be processed. Retry command later

### Meaning

(&00): subsystem name
A /MOVE-PRINT-JOBS command that processes distributed print jobs
is not allowed while (&00) subsystem is present.

### Response

Unload (&00) subsystem, wait until it is not ready
and try the command again.

## SPA0117

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPA0117 Print job with tsn '(&00)' suspended in '(&01)' EQUISAMQ file

### Meaning

(&00): print job tsn
(&01): filename of the EQUISAMQ file specified as 'TO-FILE' operand
The current print job has been temporarily suspended,
as a currently being moved print job with the same tsn has
a higher priority.
Reason: the default SYSDPRNT catid has been temporarily switched,
so that the print job could not be processed.

### Response

Switch again the default SYSDPRNT catid,
use the /MOVE-PRINT-JOBS command with FROM-FILE= to move print jobs
- really or not- and the suspended print jobs will automatically
be schedulable again.

## SPA0118

Destination: CONSOLE Routing code: S Weight: 99

Warranty : NO

SPA0118 Print job with tsn '(&00)' resumed in '(&01)' EQUISAMQ file

### Meaning

(&00): print job tsn
(&01): filename of the EQUISAMQ file specified as 'FROM-FILE' operand
The current print job had been previously suspended with SPA0117 message.
As the default SYSDPRNT catid has been switched again,
the print job may now be processed as usual.

## SPA0119

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0119 '(&00)' print job(s) suspended in '(&01)' EQUISAMQ file

### Meaning

(&00): number of print jobs that have been suspended
(&01): filename of the EQUISAMQ file specified as 'TO-FILE' operand
A more precise information about the suspended print jobs
has been sent to console - SPA0117 message.

## SPA0120

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0120 '(&00)' print job(s) resumed in '(&01)' EQUISAMQ file

### Meaning

(&00): number of print jobs that have been resumed
(&01): filename of the EQUISAMQ file specified as 'FROM-FILE' operand
A more precise information about the resumed print jobs
has been sent to console - SPA0118 message.

## SPA0121

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0121 /MOVE-PRINT-JOBS command currently processed. Retry command later

### Meaning

A /MOVE-PRINT-JOBS command currently uses the system standard
EQUISAMQ file in order to process distributed print jobs.
SPOOL subsystem may not be ready during this processing.

### Response

Wait until the command is completely processed
and try again to start/resume SPOOL subsystem.

## SPA0122

Destination: USER-TASK Routing code: Weight:

Warranty : NO

SPA0122 /MOVE-PRINT-JOBS command currently processed. '(&00)' subsystem may not be loaded. Retry command later

### Meaning

(&00): subsystem name
A /MOVE-PRINT-JOBS command currently uses the system standard
EQUISAMQ file in order to process distributed print jobs.
(&00) subsystem may not be ready during this processing.

### Response

Wait until the command is completely processed
and try again to start/resume the subsystem.

©2025 Fujitsu | BS2000 System Messages