## FTRCOPY

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FTRCOPY COPYRIGHT (C) 2025 FUJITSU TECHNOLOGY SOLUTIONS GMBH. ALL RIGHTS RESERVED.

## FTRLOAD

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FTRLOAD PROGRAM 'FT', VERSION '12.1C95' OF '2025-11-07' LOADED

## FTRREVI

Destination: USER-TASK Routing code: Weight:

Warranty : NO

FTRREVI COMP=FTCMF,VER=495,DATE=071125

## FTRSTRT

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

FTRSTRT PROGRAM 'FT', VERSION '12.1C95' OF '2025-11-07' STARTED

## FTR0000

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : YES

FTR0000 (&01)Request (&00) accepted

### Meaning

The command has been stored in the local system's request queue.
File transfer will begin once all the resources have been
assigned in both the local and the remote system.
(&00): request ID assigned by the local FT system.
This request ID is a possible selection criterion
if you subsequently want to cancel the FT.
(&01): Name of instance; empty for standard instance.

## FTR0005

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0005 (&01)Request (&00). File '(&02)' transferred

### Meaning

The file transfer request (&00) has been successfully completed.
Follow-up processing has been started for both the local system and the
remote system, as requested, provided no error occurred. Local errors
are indicated by a message.
(&01): Name of instance; empty for standard instance.

## FTR0006

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0006 (&01)Request (&00). Directory '(&02)' transferred

### Meaning

The directory transfer request (&00) has been successfully completed.
Follow-up processing has been started for both the local system and the
remote system, as requested, provided no error occurred. Local errors
are indicated by a message.
(&01): Name of instance; empty for standard instance.

## FTR0020

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0020 (&01)'(&00)' not found

### Meaning

The command was not executed
because either the send file is not/no longer or the receive file is no
longer in the catalog or on a volume of the relevant system.
(&01): Name of instance; empty for standard instance.

### Response

Correct the file name, read in file from tape or restore the send file.
Repeat the command.

## FTR0035

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0035 (&01)File locked to prevent multiple access

### Meaning

The command was not executed because either the send file or the
receive file is already locked by another process to prevent it
from being updated simultaneously.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the command later or unlock the file.
After a system crash you may need to verify files that
are not closed correctly.
If the lock is caused by an FT request, it will be canceled
automatically when the request is finished.

## FTR0041

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0041 (&01)Request queue full

### Meaning

The command was not executed because the maximum number of
permissible file transfer requests has been reached.
(&01): Name of instance; empty for standard instance.

### Response

Notify the FT administrator. Repeat the command later.

## FTR0108

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0108 (&01)Request (&00). Remote system not accessible

### Meaning

The command could not be accepted because the partner system is
currently not available.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the command later. If the error persists, contact the system or
network administrator.

## FTR0236

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0236 (&01)Current instance '(&00)' no longer found

### Meaning

The command was rejected. The instance (&00) could not be found.
(&01): Name of instance; empty for standard instance.

## FTR0301

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0301 (&01)Partner '(&00)' entered state NOCON

### Meaning

The partner system (&00) changed state to NOCON.
This state means that the partner is no longer accessible.
(&01): Name of instance; empty for standard instance.

### Response

If necessary, check whether there is a problem with the network
connection to the partner system.

## FTR0302

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0302 (&01)Partner '(&00)' entered state ACTIVE

### Meaning

The partner system (&00) changed state to ACTIVE.
(&01): Name of instance; empty for standard instance.

### Response

For information only.

## FTR0303

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0303 (&01)Partner '(&00)' entered state LUNK

### Meaning

The partner system (&00) changed state to LUNK.
The state LUNK means that the local FT system is not known to the
remote FT system.
(&01): Name of instance; empty for standard instance.

### Response

Ask the FT administrator of the remote system to add the local FT
system to the network description file of the remote system.

## FTR0304

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0304 (&01)Partner '(&00)' entered state RUNK

### Meaning

The partner system (&00) changed state to RUNK.
The state RUNK means that the remote system is not known to the local
system.
(&01): Name of instance; empty for standard instance.

### Response

Make the remote system known on the local system
(BCAM generation, HOSTS, TNS).

## FTR0305

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0305 (&01)Partner '(&00)' entered state INACT

### Meaning

The partner system (&00) changed state to INACT.
The state INACT means that the FT administrator has suspended
outbound requests for this partner system.
(&01): Name of instance; empty for standard instance.

### Response

Cancel the lock if appropriate.

## FTR0306

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0306 (&01)Partner '(&00)' entered state AINACT

### Meaning

The partner system (&00) entered the state AINACT.
State AINACT means that the partner system has been deactivated
automatically because several consecutive tries to reach a
connection have failed.
(&01): Name of instance; empty for standard instance.

### Response

Check whether the partner system should be accessible
and activate it again.

## FTR0307

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0307 (&01)Partner '(&00)' may be unreachable

### Meaning

Several consecutive attempts to establish a connection to the partner
system (&00) have failed. Further attempts will be made.
(&01): Name of instance; empty for standard instance.

### Response

For information only.

## FTR0308

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0308 (&01)Partner '(&00)' does not allow more inbound requests

## FTR0309

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0309 (&01)Partner '(&00)' added

### Meaning

The specified remote system has been added to the request and
network description file.
(&01): Name of instance; empty for standard instance.

## FTR0310

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0310 (&01)Partner '(&00)' removed

### Meaning

The specified remote system has been removed from the request and
network description file.
(&01): Name of instance; empty for standard instance.

## FTR0311

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0311 (&01)Partner '(&00)' entered state LAUTH

### Meaning

The partner system (&00) changed state to LAUTH.
The state LAUTH means that the local system could not be authenticated
by the remote system.
(&01): Name of instance; empty for standard instance.

### Response

Send the current key file to the administrator of the remote system.

## FTR0312

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0312 (&01)Partner '(&00)' entered state RAUTH

### Meaning

The partner system (&00) changed state to RAUTH.
The state RAUTH means that the remote system could not be
authenticated by the local system. The reason may
be that the key in the key file is not up-to-date or
there has been an attempt to intrude by a non-authorized system.
(&01): Name of instance; empty for standard instance.

### Response

Contact the system administrator of the remote system.

## FTR0313

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0313 (&01)Partner '(&00)' entered state DIERR

### Meaning

The partner system (&00) changed state to DIERR.
Data integrity errors were detected on the connection.
This can either be a problem of the
transport system, or targeted manipulation
of the transmission data.
(&01): Name of instance; empty for standard instance.

## FTR0314

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0314 (&01)Partner '(&00)' entered state NOKEY

### Meaning

The partner system (&00) changed state to NOKEY.
The state NOKEY means that the partner does not accept a connection
without encryption or that there is no key.
(&01): Name of instance; empty for standard instance.

### Response

Create a new key pair.

## FTR0315

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0315 (&01)Partner '(&00)' entered state IDREJ

### Meaning

The partner system (&00) changed state to IDREJ.
The local identification was not accepted by the partner system
or by an intermediate instance.
Possible reasons:
- Both the local identification and the migrated ID
%.<processor>.<entity> are entered in the
request description of the partner system.
- The identification is rejected by an intermediate instance
for security reasons.
(&01): Name of instance; empty for standard instance.

### Response

Have the partner entry of your instance checked.

## FTR0320

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0320 (&01)Abnormal termination initiated

### Meaning

An abnormal FT termination due to an internal error has been
initiated.
(&01): Name of instance; empty for standard instance.

### Response

Check the reason for the abnormal termination and start FT again.

## FTR0330

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0330 (&01)Request queue 85 percent full

### Meaning

About 85 percent of the slots in the request queue are
occupied. The queue may get full if additional requests are entered.
New requests will be rejected by FT.
(&01): Name of instance; empty for standard instance.

### Response

Enlarge the request queue if necessary.

## FTR0331

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0331 (&01)At least 20 percent of request queue unoccupied

### Meaning

At least 20 percent of the FT request queue is unoccupied.
This message occurs only if a previous FTR0330 has warned about a
possible overflow of the request queue. The danger has
receded.
(&01): Name of instance; empty for standard instance.

### Response

For information only.

## FTR0340

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0340 (&01)Transfer '(&00)' successfully completed

### Meaning

The request described by the insert (&00) has been
completed successfully.
(&00): *LOC/*REM;SID;PARTNER;USERID;FILE
As the length of the insert cannot exceed 180 characters, the filename
is truncated if necessary. This is indicated by the character '*' as the
last character of the filename.
(&01): Name of instance; empty for standard instance.

### Response

For information only.

## FTR0341

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0341 (&01)Transfer '(&00)' terminated with error

### Meaning

The request described by the insert (&00) has been
terminated with an error.
(&00): MSGNR;*LOC/*REM;SID;PARTNER;USERID;FILE
As the length of the insert cannot exceed 180 characters, the filename
is truncated if necessary. This is indicated by the character '*' as
the last character of the filename.
(&01): Name of instance; empty for standard instance.

### Response

For information only.

## FTR0360

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0360 (&01)openFT control process started

### Response

For information only.

## FTR0361

Destination: USER-TASK, CONSOLE Routing code: @ (conslog) Weight: 99

Warranty : NO

FTR0361 (&01)openFT control process terminated

### Response

For information only.

## FTR0500

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0500 (&01)openFT (&00) starting. Protocols: (&02)

### Meaning

The file transfer system openFT has been activated
for the protocols (&02).
(&01): Name of instance; empty for standard instance.

## FTR0501

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0501 (&01)openFT terminated

### Meaning

The file transfer system openFT has been terminated
in response to an administrator command.
(&01): Name of instance; empty for standard instance.

## FTR0502

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0502 (&01)No log records available for the selection criteria

### Meaning

No log records meet the selected criteria.
(&01): Name of instance; empty for standard instance.

### Response

Change the selection criteria.

## FTR0503

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0503 (&01)No partner available for the selection criteria

### Meaning

There are no partners that meet the specified selection criteria.
(&01): Name of instance; empty for standard instance.

### Response

Change the selection criteria.

## FTR0504

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0504 (&01)No requests available for the selection criteria

### Meaning

There are no requests that meet the specified selection criteria.
(&01): Name of instance; empty for standard instance.

### Response

Change the selection criteria.

## FTR0505

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0505 (&01)Requests executed; (&00) files were transferred

### Meaning

The file transfer requests have been successfully completed. A total of
(&00) files have been transferred. If you have specified commands for
follow-up processing, follow-up processing is executed for every
file.
(&01): Name of instance; empty for standard instance.

## FTR0506

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0506 (&01)No instances available

## FTR0507

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0507 (&01)No information available

## FTR0508

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0508 (&01)No ADM traps available for the selection criteria

### Meaning

No ADM traps meet the selected criteria.
(&01): Name of instance; empty for standard instance.

### Response

Change the selection criteria.

## FTR0509

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0509 (&01)Protocol: (&00) not installed or not licensed

### Meaning

Configuration and activation of protocol don't match.
(&01): Name of instance; empty for standard instance.

### Response

Check configuration and activation of protocol.

## FTR0510

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0510 (&01)Requests executed; (&00) directories were transferred

### Meaning

The Directory transfer requests have been successfully completed.
A total of (&00) directories have been transferred.
If you have specified commands for follow-up processing,
follow-up processing is executed for every file.
(&01): Name of instance; empty for standard instance.

## FTR0511

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0511 (&01)Requests accepted; (&00) file transfers initiated

### Meaning

The file transfer requests have been successfully accepted.
A total of (&00) file transfers have been initiated. If you
have specified commands for follow-up processing,
follow-up processing is executed for every file.
(&01): Name of instance; empty for standard instance.

## FTR0560

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0560 (&01)Cancel all specified requests? Reply (y=yes; n=no)

### Meaning

A CANCEL-TRANSFER command applies to more than one file transfer.
Y / J: All the transfer requests affected are deleted.
N: The entire deletion request is withdrawn.
(&01): Name of instance; empty for standard instance.

## FTR0561

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0561 (&01)Do you really want to delete this key pair set? Reply (y=yes; n=no)

### Meaning

Deletion of a key pair set prevents connection to all partners
working with these keys. If the last key pair set is deleted,
there is no encryption.
(&01): Name of instance; empty for standard instance.

## FTR0562

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0562 (&01)(&00):

## FTR0600

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0600 (&01)Shutdown processing delayed. FT tasks pending

### Meaning

openFT could not be terminated.
(&01): Name of instance; empty for standard instance.

### Response

Check if there are console messages that need to be answered for FT
tasks connected to the FT subsystem.

## FTR0604

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0604 (&01)Request (&00). Follow-up processing not started

### Meaning

The follow-up processing of a transfer request was not started because
the local processing admission may be incorrect.
(&01): Name of instance; empty for standard instance.

### Response

Correct the local processing admission and repeat the command.

## FTR0605

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0605 (&01)Tracefile changed

### Meaning

There has been a switch to a new trace file.
(&01): Name of instance; empty for standard instance.

## FTR0606

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0606 (&01)Trace terminated

### Meaning

The trace status has been switched off.
(&01): Name of instance; empty for standard instance.

## FTR0607

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0607 (&01)Trace started: (&00)

### Meaning

The trace status for the protocols specified in (&00) has been
switched on.
(&01): Name of instance; empty for standard instance.

## FTR0700

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0700 (&01)Parameter '(&00)' and '(&02)' must not be specified at the same time

### Meaning

The selected parameters could not be specified simultaneously.
(&01): Name of instance; empty for standard instance.

### Response

Omit one of the two parameters and repeat the command.

## FTR0701

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0701 (&01)Input error

## FTR0702

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0702 (&01)Length of parameter value '(&00)' invalid

### Meaning

The specified parameter length (&00) is invalid; see the command syntax.
(&01): Name of instance; empty for standard instance.

### Response

Change the length of the parameter value (&00) and repeat the command.

## FTR0703

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0703 (&01)Mandatory parameter missing

### Meaning

A mandatory parameter is missing; see the command syntax.
(&01): Name of instance; empty for standard instance.

### Response

Correct the command and try again.

## FTR0704

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0704 (&01)Mandatory parameter '(&00)' missing

### Meaning

The mandatory parameter (&00) was not specified.
(&01): Name of instance; empty for standard instance.

### Response

Correct the command and try again.

## FTR0705

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0705 (&01)Parameter '(&00)' specified more than once

### Meaning

The parameter (&00) was specified more than once.
(&01): Name of instance; empty for standard instance.

### Response

Correct the command and try again.

## FTR0706

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0706 (&01)Parameter '(&00)' can only be specified together with '(&02)'

### Meaning

The parameter (&00) can only be specified together with (&02).
(&01): Name of instance; empty for standard instance.

### Response

Add the parameter (&02) to the command and repeat the command.

## FTR0707

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0707 (&01)Invalid parameter '(&00)'

### Meaning

An invalid parameter (&00) was specified; see the command syntax.
(&01): Name of instance; empty for standard instance.

### Response

Correct the command and try again.

## FTR0708

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0708 (&01)Value of parameter '(&00)' not within valid range

### Meaning

The parameter value (&00) is not within the specified value range;
see the command syntax.
(&01): Name of instance; empty for standard instance.

### Response

Correct the parameter value (&00) and repeat the command.

## FTR0709

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0709 (&01)Too many positional parameters

### Meaning

The maximum number of positional parameters was exceeded.
(&01): Name of instance; empty for standard instance.

### Response

Correct the command and try again.

## FTR0710

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0710 (&01)Invalid parameter value '(&00)'

### Meaning

The assigned parameter value (&00) is incorrect; see the command syntax.
(&01): Name of instance; empty for standard instance.

### Response

Correct the parameter value (&00) and repeat the command.

## FTR0711

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0711 (&01)Parameter '(&00)' or '(&02)' must be specified

### Meaning

At least one of the parameters must be specified.
(&01): Name of instance; empty for standard instance.

### Response

Specify one or both parameter(s) and repeat the command.

## FTR0800

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0800 (&01)Request (&00). Internal error. Job variable not accessible

### Meaning

The command was not executed because
- the system was generated without job variables, or
- the maximum number of job variables allowed for the user has
been reached, or
- a temporary job variable was specified, or
- the specified job variable is not accessible to the user, or
- the specified job variable is monitoring another FT request, or
- the password specified for the job variable is incorrect.
(&01): Name of instance; empty for standard instance.

### Response

Correct the command and try again.

## FTR0801

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0801 (&01)Request (&00). Internal error

### Meaning

(&00): FTAM, NDMS, FJAM or operating system error that is neither
a DMS error nor a transport system error, possibly the
transfer ID
The FT system continues to run after the message has been issued.
(&01): Name of instance; empty for standard instance.

## FTR0802

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0802 (&01)Request (&00). Warning: Job variable contents inconsistent

### Meaning

At the end of the file transfer request, the contents of the
job variable monitoring the request were found to be inconsistent.
Possible reason: During the transfer, the job variable was accessed
externally in a mode other than read mode.
The result of the transfer is not affected and is given in the result
list or asynchronous end message.
(&01): Name of instance; empty for standard instance.

## FTR0803

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0803 (&01)Request (&00). Follow-up processing could not be started

### Meaning

The command was not executed because the specifications in one of the
PROCESSING-ADMISSION operands are incorrect.
(&01): Name of instance; empty for standard instance.

### Response

Define the required PROCESSING ADMISSION or correct it.
Repeat the command if necessary.

## FTR0804

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0804 (&01)Request (&00). Request data inconsistent

## FTR0850

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0850 (&01)Internal error. Job variable not accessible

### Meaning

The command was not executed because
- the system was generated without job variables, or
- the maximum number of job variables allowed for the user has
been reached, or
- a temporary job variable has been specified, or
- the specified job variable is not accessible to the user, or
- the specified job variable is monitoring another FT request, or
- the password specified for the job variable is incorrect.
(&01): Name of instance; empty for standard instance.

### Response

Correct the command and try again.

## FTR0851

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0851 (&01)Internal error (&00)

## FTR0852

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0852 (&01)Current instance '(&00)' does not match with the openFT version

### Meaning

The openFT configuration files SYSOPF, SYSPTF, SYSRQF, SYSLOG, SYSFSA,
SYSPKF and SYSKEY do not match with the version of openFT.
Please rename or backup the incompatible configuration files. Please
copy afterwards either the corresponding files for this instance to
$SYSFJAM, or start openFT without these files. In the latter case the
files SYSOPF, SYSPTF, SYSFSA, SYSRQF and SYSLOG will be recreated
automatically after start of openFT.
(&01): Name of instance; empty for standard instance.

### Response

Rename or backup invalid or incompatible configuration files.

## FTR0853

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0853 (&01)Load error. Error Code (&00)

### Meaning

The command could not be executed because openFT code could not be
loaded.
PPBIND error codes: DSSM error codes:
0C080600 Load module not found 00000008 Subsystem not generated
0C080610 Wrong file type (not OML) 18000008 Subsystem component not
0C08061C Library inconsistent found
0C080620 Directory of library
inconsistent
(&01): Name of instance; empty for standard instance.

### Response

Check that the library SYSLNK.openFT.<version> supplied with openFT
is installed on TSOS and FT has been added to the subsystem
catalog. The product PAMINT must also be installed.

## FTR0854

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0854 (&01)Writing of log records no more possible.

### Meaning

There is not enough space on the disk/partition on which the logging
files are stored.
(&01): Name of instance; empty for standard instance.

### Response

Increase the disk space (or have it increased).

## FTR0855

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0855 (&01)No space left on device for internal files

### Meaning

There is not enough space on the disk/partition on which the internal
files are stored.
(&01): Name of instance; empty for standard instance.

### Response

Increase the disk space (or have it increased).

## FTR0856

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0856 (&01)Error during ops generation

## FTR0857

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0857 (&01)Error in key file '(&00)'

## FTR0858

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0858 (&01)Internal error. Set / release file-locks not possible

### Meaning

A problem occurred when setting/resetting the file locks
for all open requests in FT-REQUEST-FILE.
(&01): Name of instance; empty for standard instance.

### Response

Check whether the request file SYSRQF is accessible
on the config user ID of the current instance.

## FTR0859

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0859 (&01)Function not supported because of teleservice restriction

### Meaning

Possible reasons:
MOD-FT-OPT PART-CHECK=STD is not supported.
Only one partner with the name TELESERV is supported.
(&01): Name of instance; empty for standard instance.

### Response

Correct and repeat the command.

## FTR0860

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0860 (&01)Teleservice restriction for FTAC because of FT

### Meaning

FT for Teleservice enforces Teleservice restriction for FTAC.
(&01): Name of instance; empty for standard instance.

### Response

Correct and repeat the command.

## FTR0861

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0861 (&01)Teleservice restriction for (&00)

## FTR0862

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0862 (&01)Protocol stack '(&00)' not licensed or not installed

### Meaning

The required transfer protocol is not
licensed or not installed.
(&01): Name of instance; empty for standard instance.

### Response

Install or license the transfer protocol

## FTR0863

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0863 (&01)FTAC subsystem not available

### Meaning

Install openFT-AC
(&01): Name of instance; empty for standard instance.

## FTR0864

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0864 (&01)Server '(&00)' accepts no requests

### Meaning

The control process cannot access the server to assign
new requests.
(&01): Name of instance; empty for standard instance.

### Response

Check if the server is blocked e.g. by a systemdump or the output
of a message and correct the error situation.

## FTR0865

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0865 (&01)Not all files transferred successfully

### Meaning

At least one source file could not be transferred to
the local system. The previous messages
indicate the files concerned:
Transfer of file '<file>' failed. Reason: '<rc>'
(&01): Name of instance; empty for standard instance.

## FTR0999

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR0999 (&01)openFT panic (&00). Abnormal termination

## FTR1020

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1020 (&01)openFT already started

### Meaning

openFT can only be started once in each instance.
(&01): Name of instance; empty for standard instance.

### Response

Terminate openFT if necessary.

## FTR1021

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1021 (&01)Request must be canceled without FORCE option first

### Meaning

Before the FORCE option is used, the command must be called
without the FORCE option.
(&01): Name of instance; empty for standard instance.

### Response

Issue the command without the FORCE option first.

## FTR1022

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1022 (&01)Instance '(&00)' already exists

### Meaning

The command was rejected because an instance (&00) already exists.
(&01): Name of instance; empty for standard instance.

### Response

Select a new instance name and/or CONFIG-USERID or directory, and
repeat the command.

## FTR1023

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1023 (&01)Maximum number of instances exceeded

### Meaning

The command was not executed because the maximum permissible number
of instances has been reached.
(&01): Name of instance; empty for standard instance.

### Response

Delete instances that are no longer required.

## FTR1024

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1024 (&01)Standard instance '(&00)' must not be deleted

### Meaning

The standard instance must always exist.
(&01): Name of instance; empty for standard instance.

## FTR1025

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1025 (&01)Instance '(&00)' not found

### Meaning

The command was rejected. The instance (&00) could not be found.
(&01): Name of instance; empty for standard instance.

### Response

Select an existing instance.

## FTR1026

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1026 (&01)Instance '(&00)' must not be modified

### Meaning

The modification of instances is not permitted when FT is started or
when pre-/post-processing is active in the instance.
(&01): Name of instance; empty for standard instance.

### Response

Terminate openFT and ensure that all requests are terminated.
Repeat the command.

## FTR1027

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1027 (&01)Config user ID '(&00)' not accessible

### Meaning

The USERID specified in the command cannot be accessed.
(&01): Name of instance; empty for standard instance.

### Response

Check USERID.

## FTR1028

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1028 (&01)Warning: config user ID '(&00)' not accessible

### Meaning

The USERID specified in the command cannot be accessed.
(&01): Name of instance; empty for standard instance.

### Response

If existing FT configuration files (the request file, for example) are
to be used, it must be ensured that the
CONFIG-USERID is accessible before the instance is created. Otherwise,
it is possible to create the USERID afterwards.

## FTR1029

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1029 (&01)Maximum number of key pairs exceeded

### Meaning

The maximum number of key pairs has been reached.
(&01): Name of instance; empty for standard instance.

### Response

Before new key pair set can be created, an older key pair set must be
deleted, before a key pair can be imported a key pair of the same
length must be deleted.

## FTR1030

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1030 (&01)Warning: last key pair used for encryption deleted

### Meaning

The last key pair of the length configured in the options has been
deleted. Without a key pair encrypted transfer and data integrity
checking are not possible.
(&01): Name of instance; empty for standard instance.

### Response

Create a new key pair set or import a key pair
of the configured length.

## FTR1031

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1031 (&01)Warning: No key pair available

### Meaning

All transfers are carried out without encryption.
(&01): Name of instance; empty for standard instance.

### Response

Create a new key pair set, if necessary or
import a set of the configured length.

## FTR1032

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1032 (&01)Last key pair must not be deleted

### Meaning

The last key pair usable for encryption must not be
deleted.
(&01): Name of instance; empty for standard instance.

## FTR1033

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1033 (&01)The public key files could not be updated

### Meaning

The contents of the SYSPKF file could not be fully updated.
Possible reasons:
- The SYSPKF file is locked.
- There is not enough disk space to allow the file to be created.
(&01): Name of instance; empty for standard instance.

### Response

Take the appropriate action depending on the cause of the error:
- Unlock the file.
- Allocate disk space or have your system
administrator do it.
Update the key with UPDATE-FT-PUBLIC-KEY.

## FTR1034

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1034 (&01)Command only permissible for FT, FTAC or ADM administrator

### Meaning

Only the FT, FTAC or ADM administrator is permitted to use
the command.
(&01): Name of instance; empty for standard instance.

### Response

Have the command executed by the FT, FTAC or ADM administrator.

## FTR1035

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1035 (&01)Command only permissible for FT administrator

### Meaning

Only the FT administrator is permitted to use the command.
(&01): Name of instance; empty for standard instance.

### Response

Have the command executed by the FT administrator.

## FTR1036

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1036 (&01)User not authorized for other user Ids

### Meaning

The user is not authorized to use a different user ID in the command.
(&01): Name of instance; empty for standard instance.

### Response

Specify your own ID, or have the command executed by the
FT or FTAC administrator.

## FTR1037

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1037 (&01)Key reference unknown

### Meaning

The specified key reference is unknown.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the command with an existing key reference.

## FTR1038

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1038 (&01)Request (&00) is in the termination phase and can no longer be canceled

## FTR1039

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1039 (&01)openFT not active

### Meaning

openFT is not started.
(&01): Name of instance; empty for standard instance.

### Response

Start openFT, if necessary.

## FTR1040

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1040 (&01)Config user ID unknown or not enough space

### Meaning

The CONFIG USERID of the current instance (SYSFJAM) is unknown or the
disk space allocated is insufficient to allow creation of the
FT-REQUEST-FILE, the file for storing trace data, or the key files.
(&01): Name of instance; empty for standard instance.

### Response

Either create the CONFIG-USERID or increase its disk space allocation
or have your system administrator do it.

## FTR1041

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1041 (&01)Specified file is not a valid trace file

## FTR1042

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1042 (&01)openFT could not be started

## FTR1043

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1043 (&01)Partner with same attribute '(&00)' already exists in partner list

### Meaning

There is already a partner entry with the same attribute '(&00)'
in the partner list.
(&01): Name of instance; empty for standard instance.

### Response

The attribute '(&00)' in partner entries must be unique. Correct the
command accordingly and try again.

## FTR1044

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1044 (&01)Maximum number of partners exceeded

### Meaning

The partner list already contains the maximum permissible number
of partner entries.
(&01): Name of instance; empty for standard instance.

### Response

Delete partners that are no longer required.

## FTR1045

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1045 (&01)No partner found in partner list

### Meaning

A partner for the specified selection could not be found
in the partner list.
(&01): Name of instance; empty for standard instance.

### Response

Check if the specified partner name or address was correct.
If you try to import a key file, check if there exists a static partner
with the identification within the key file.
If necessary, repeat the command using the correct name or address.

## FTR1046

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1046 (&01)Modification of partner protocol type not possible

### Meaning

The protocol type of the partner entry cannot be changed subsequently.
(&01): Name of instance; empty for standard instance.

### Response

Delete the partner from the partner list, if necessary, and enter it
again with a new protocol type.

## FTR1047

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1047 (&01)Request (&00) not found

### Meaning

The request with the transfer ID (&00) could not be found.
(&01): Name of instance; empty for standard instance.

### Response

Specify the existing transfer ID and repeat the command.

## FTR1048

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1048 (&01)Active requests could not yet be deleted

### Meaning

Active requests for the specified partner were cancelled.
After the negotiation of termination with the partner the requests
will be automatically deleted.
(&01): Name of instance; empty for standard instance.

## FTR1049

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1049 (&01)CCS name '(&00)' unknown

## FTR1050

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1050 (&01)ftscript process could not be started(&00)

## FTR1051

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1051 (&01)Error displaying an ftscript user

## FTR1052

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1052 (&01)ftscript user number limit exceeded

## FTR1053

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1053 (&01)ftscript chapter not found

## FTR1054

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1054 (&01)ftscript ID not found

## FTR1055

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1055 (&01)ftscript file not found

## FTR1056

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1056 (&01)ftscript request is still running

## FTR1057

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1057 (&01)Inbound requests cannot be modified

## FTR1058

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1058 (&01)The ADM trap server configuration is invalid

### Meaning

The ADM trap server configuration must consist of trap server and
FTAC transfer admission.
(&01): Name of instance; empty for standard instance.

### Response

Specify ADM trap server and FTAC transfer admission.

## FTR1059

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1059 (&01)Monitoring is not active

### Meaning

This command is not supported when monitoring is not active.
(&01): Name of instance; empty for standard instance.

### Response

Activate monitoring in the operating parameters
and repeat the command.

## FTR1060

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1060 (&01)File could not be created (&02)

## FTR1061

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1061 (&01)Higher-level directory not found

## FTR1062

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1062 (&01)File already exists

## FTR1063

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1063 (&01)Resulting file name too long

## FTR1064

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1064 (&01)File locked to prevent multiple access

## FTR1065

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1065 (&01)File not found

## FTR1066

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1066 (&01)Not enough space for file

## FTR1067

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1067 (&01)Syntax error in resulting file name

## FTR1068

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1068 (&01)Access to file denied (&02)

## FTR1069

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1069 (&01)Error accessing file (&02)

## FTR1070

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1070 (&01)Configuration data invalid (&00)

## FTR1071

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1071 (&01)Import of configuration data not possible while remote administration server is started

## FTR1072

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1072 (&01)Parameter value *BY-TRANSPORT-SYSTEM no more supported

### Meaning

The configuration of the port in the transport system (BCAM mapping)
is not supported any more. If a non-standard port is needed
(other than 1100) it must be given as part of the address parameter.
(&01): Name of instance; empty for standard instance.

### Response

The partner was added using port 1100, it may be necessary
to correct its address.

## FTR1073

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1073 (&01)Command aborted

### Meaning

The user has interrupted the command.
(&01): Name of instance; empty for standard instance.

## FTR1074

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1074 (&01)Command only permissible for ADM administrator on a remote administration server

### Meaning

Only the ADM administrator is permitted to use the command on a
remote administration server.
(&01): Name of instance; empty for standard instance.

### Response

Have the command executed by the ADM administrator or
the server is not a remote administration server.

## FTR1075

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1075 (&01)BCMAP not possible. '(&00)' on port '(&02)' not accessible

### Meaning

Possible reasons:
BCMAP already active.
Port is used by another application.
(&01): Name of instance; empty for standard instance.

## FTR1076

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1076 (&01)Selected key file not found

## FTR1077

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1077 (&01)Change of transport access system not possible. Reason: (&00)

## FTR1078

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1078 (&01)Too short time interval since last logging file switch

### Meaning

At this moment the logging file cannot be switched,
as the time dependant part of the logging file name does not differ
from this name part in the actual logging file name.
(&01): Name of instance; empty for standard instance.

### Response

If necessary, repeat the command after an appropriate waiting time.

## FTR1079

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1079 (&01)ftscript interpreter or other ftmodsuo running. Command aborted

### Meaning

The ftmodsuo command cannot be executed
because the process which executes ftscript jobs
or another ftmodsuo command
is occupying the ftscript working storage.
(&01): Name of instance; empty for standard instance.

### Response

You might cancel running ftscript jobs with ftcans
and repeat the ftmodsuo command after some time.

## FTR1080

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1080 (&01)ftscript jobs exist. Command aborted

### Meaning

The ftscript working directory cannot be changed while
valid ftscript runs exist in the old working directory.
(&01): Name of instance; empty for standard instance.

### Response

Delete the ftscript jobs with ftdels and repeat the command.

## FTR1081

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1081 (&01)The old ftscript working directory is not accessible

### Meaning

The ftscript working directory cannot be changed,
when the old working directory is not accessible.
(&01): Name of instance; empty for standard instance.

### Response

Verify that Your password is set for openFT
and that Your actual ftscript working storage is accessible.

## FTR1082

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1082 (&01)User data encryption not supported

### Meaning

User data encryption is supported only when
openFT-CR is installed.
(&01): Name of instance; empty for standard instance.

### Response

Install openFT-CR

## FTR1083

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1083 (&01)Structure of key file not supported

### Meaning

The key cannot be imported because of the not supported
key file structure.
(&01): Name of instance; empty for standard instance.

## FTR1084

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1084 (&01)Invalid password

## FTR1085

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1085 (&01)Password missing

## FTR1086

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1086 (&01)Duplicate key pair

### Meaning

No import of duplicate keys allowed.
(&01): Name of instance; empty for standard instance.

## FTR1087

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1087 (&01)Key expired

### Meaning

The expiration date lies in the past.
(&01): Name of instance; empty for standard instance.

## FTR1092

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1092 (&01)Warning: The RSA key length was aligned to the minimum key length

### Meaning

The RSA key length was less than the configured
minimum key length and had to be enlarged.
It can also mean that the suggested RSA key length value RSA-PROP
was not specified and was therefore set to the specified value of
the minimum RSA key length RSA-MIN, since both parameters must
always be specified if they were both previously set to the value
FTOPT.
(&01): Name of instance; empty for standard instance.

## FTR1096

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1096 (&01)The not specified RSA-MIN was set to the value of the RSA-PROP

### Meaning

The not specified minimum RSA key length value RSA-MIN was set to
the value of the proposed RSA key length RSA-PROP, since both
parameters must always be specified if they were both previously set
to the value FTOPT.
(&01): Name of instance; empty for standard instance.

## FTR1097

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1097 (&01)RSA-MIN and RSA-PROP parameters were set to FTOPT

### Meaning

If only one of the parameters RSA-MIN or RSA-PROP is set to the
value FTOPT, the unset one of these two parameters is also set to
FTOPT.
(&01): Name of instance; empty for standard instance.

## FTR1108

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1108 (&01)Subsystem crypt not available

## FTR1109

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR1109 (&01)Crypt subsystem not enabled for 3k and 4k keys

## FTR2014

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2014 (&01)No file attribute changes requested

### Meaning

No further file attributes besides the file name were specified.
(&01): Name of instance; empty for standard instance.

### Response

Enter the desired file attributes in addition to the file name.

## FTR2015

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2015 (&01)openFT is not authorized to execute requests for this user

## FTR2016

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2016 (&01)Directory '(&00)' is not empty

## FTR2017

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2017 (&01)File attributes do not match request parameters(&00)

### Meaning

The specified attribute combination is not permissible.
(&01): Name of instance; empty for standard instance.

### Response

Specify a permissible combination.

## FTR2018

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2018 (&01)Attributes could not be modified(&00)

### Meaning

The properties of the file could not be changed as specified in the
command. The following reasons are possible:
For the remote file:
- No access rights to the file.
- The required combination of access rights is not supported by the
remote system.
- If the remote system is a BS2000: the file is protected by ACL.
For the local file:
- No access rights to the file.
- The requested transfer attributes are not compatible with
the BS2000 properties of the file (see manual).
(&01): Name of instance; empty for standard instance.

## FTR2019

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2019 (&01)'(&00)' could not be created(&02)

### Meaning

The command was not executed because the file owner and user
requesting the creation of a receive file are not the same.
(&01): Name of instance; empty for standard instance.

### Response

Match the user ID in the receiving system's TRANSFER-ADMISSION to the
ID of the receive file's owner.
Repeat the command.

## FTR2021

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2021 (&01)CCS name unknown

### Meaning

CCS path is incorrect or data structure is incorrect.
Max 80 characters per comment line.
The request could not be carried out because the CCS names of the send
and receive files could not be mapped to each other or because
the partner system does not support the transparent receipt of files.
(&01): Name of instance; empty for standard instance.

## FTR2022

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2022 (&01)Higher-level directory not found

### Meaning

In the case of a receive request, the local file could not be created
because the specified path does not exist.
(&01): Name of instance; empty for standard instance.

### Response

Create or correct the path for the receive file and repeat the command.

## FTR2023

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2023 (&01)'(&00)' already exists

### Meaning

The command was not executed because an existing receive file
cannot be created again with WRITE-MODE=NEW.
WRITE-MODE=NEW may also have been set due to a restriction in the
access authorization used.
(&01): Name of instance; empty for standard instance.

### Response

Either delete the receive file and repeat the command, or repeat the
command specifying WRITE-MODE=REPLACE-FILE or using different
access authorization.

## FTR2024

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2024 (&01)Transfer of file generation groups not supported

### Meaning

The command was not executed because the FT system only transfers
single file generations.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the command using the name of a single file generation.

## FTR2025

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2025 (&01)Error accessing '(&00)'(&02)

### Meaning

The FT system continues to run after the message has been issued.
(&02): Further details, possibly DMS error
(&01): Name of instance; empty for standard instance.

### Response

Take the appropriate action in accordance with the error code.

## FTR2026

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2026 (&01)Resulting file name '(&00)' too long(&02)

### Meaning

The relative file name was specified in the transfer request.
The absolute file name completed by openFT is longer than permitted.
(&01): Name of instance; empty for standard instance.

### Response

Shorten the file name or path and repeat the command.

## FTR2027

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2027 (&01)No file or directory name specified

### Meaning

The command was not executed because the file name was neither
specified explicitly nor by the 'TRANSFER-ADMISSION' used.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the command, specifying the file ID explicitly or a
TRANSFER-ADMISSION that defines the file ID.

## FTR2028

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2028 (&01)Invalid management password

## FTR2029

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2029 (&01)'(&00)' not available(&02)

### Meaning

The command was not executed because the volume for either
the send file or the receive file is not mounted, unknown or reserved,
the file extends over more than one private disk, or an attempt has been
made to transfer a file migrated by HSMS.
(&01): Name of instance; empty for standard instance.

### Response

Inform the operator if necessary or carry out an HSMS recall for the
file. Repeat the command.

## FTR2030

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2030 (&01)Home directory not found(&00)

## FTR2031

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2031 (&01)Renaming not possible(&00)

## FTR2032

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2032 (&01)Not enough space for '(&00)'

### Meaning

The command was not (fully) executed because
- the permissible storage space on the receive system is used up for
the user ID specified in TRANSFER-ADMISSION, or
- the send file contains too long a sequence of empty blocks, or
- the primary and/or secondary allocation of the password-protected
receive file is too small.
The receive file can not be created/extended after the problem occurs.
(&01): Name of instance; empty for standard instance.

### Response

Take the appropriate action depending on the cause of the error:
- delete all files no longer required on the receive system, or
- ask the system administrator to allocate more storage space, or
- remove empty blocks from the send file, or
- increase the receive file's primary/secondary allocation.
If WRITE-MODE=EXTEND-FILE is specified, restore the receive file.
Repeat the command.

## FTR2033

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2033 (&01)File owner unknown

### Meaning

The command was not executed because the owner of either the send
file or the receive file was not defined in the local system or because
the file owner and the user requesting the creation of a receive file
are not the same.
(&01): Name of instance; empty for standard instance.

### Response

Define the file owner, correct TRANSFER-ADMISSION or FILE-NAME.
Repeat the command.

## FTR2034

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2034 (&01)Invalid file password

### Meaning

The command was not executed because the password for the send file or
the receive file is missing or incorrect.
(&01): Name of instance; empty for standard instance.

### Response

Correct the password in the file description or the command.
Repeat the command.

## FTR2036

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2036 (&01)Retention period of file not yet expired

### Meaning

The command was not executed because the retention period protecting
the receive file against overwriting has not yet expired
(RETENTION PERIOD).
(&01): Name of instance; empty for standard instance.

### Response

Correct the transfer direction, retention period or file name.
Repeat the command.

## FTR2037

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2037 (&01)'(&00)' is read only

## FTR2038

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2038 (&01)File structure not supported(&00)

## FTR2039

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2039 (&01)Syntax error in resulting file name '(&00)'(&02)

### Meaning

The local file cannot be accessed because, for example,
the absolute file name is too long.
(&01): Name of instance; empty for standard instance.

### Response

Shorten the path or file name. Repeat the command.

## FTR2040

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2040 (&01)Transparent file transfer not supported

### Meaning

The request could not be carried out because the CSS names of the send
and receive files cannot be mapped to each other or because the partner
system does not support the receipt of files in a transparent format.
(&01): Name of instance; empty for standard instance.

## FTR2042

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2042 (&01)Extension of file not possible for transparent transfer

### Meaning

The command could not be executed because it is not possible
to add to a file in a transparent transfer.
(&01): Name of instance; empty for standard instance.

### Response

Start transfer without EXTEND.

## FTR2043

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2043 (&01)Access to '(&00)' denied(&02)

### Meaning

The command was not executed because either the send file or
the receive file only permits certain access modes (e.g. read only).
(&01): Name of instance; empty for standard instance.

### Response

Correct the file name or file protection
attributes. Repeat the command.

## FTR2044

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2044 (&01)Follow-up processing exceeds length limit

### Meaning

Prefix + suffix (from prof) + local follow-up processing
together are too long.
(&01): Name of instance; empty for standard instance.

### Response

Shorten the follow-up processing, or use procedures.
Repeat the command.

## FTR2045

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2045 (&01)Processing admission invalid

### Meaning

The command was not executed because the specifications in one of the
PROCESSING-ADMISSION operands were incorrect.
(&01): Name of instance; empty for standard instance.

### Response

Define the required PROCESSING ADMISSION or correct it.
Repeat the command if necessary.

## FTR2046

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2046 (&01)Local transfer admission invalid

### Meaning

The command was not executed because the specifications in one of
the TRANSFER-ADMISSION operands were incorrect.
(&01): Name of instance; empty for standard instance.

### Response

Define the required TRANSFER ADMISSION or correct it.
Repeat the command if necessary.

## FTR2047

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2047 (&01)Request rejected by local FTAC

### Meaning

The command was not executed because the request was rejected by the
product FTAC-BS2000 due to a lack of authorization.
(&01): Name of instance; empty for standard instance.

### Response

Use the return code in the log record to determine and
remove the cause. Repeat the command.

## FTR2048

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2048 (&01)Function not supported for protocol '(&00)'

### Meaning

The desired function is not available for the selected protocol.
(&01): Name of instance; empty for standard instance.

### Response

Select a different protocol.

## FTR2049

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2049 (&01)Remote follow-up processing not supported

### Meaning

Remote follow-up processing is only available for the openFT protocol.
(&01): Name of instance; empty for standard instance.

### Response

Select a different protocol, or specify follow-up
processing by means of an FTAC profile.

## FTR2050

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2050 (&01)Data integrity check not supported

### Meaning

The partner system does not support the data integrity check function.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the request without a file integrity check.

## FTR2051

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2051 (&01)User data encryption not possible for this request

### Meaning

The data encryption function is not supported.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the request without data encryption or install
openFT-CR (or have it installed).

## FTR2052

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2052 (&01)Administration request rejected by remote administration server

### Meaning

The command was not executed because the request was rejected by the
remote administration server.
(&01): Name of instance; empty for standard instance.

### Response

Use the return code in the log record on the remote
administration server to determine and remove the cause.
Repeat the command.

## FTR2053

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2053 (&01)Destination format not supported for transparent transfer

### Meaning

The destination file organization parameter is not supported
for transparent transfer
(&01): Name of instance; empty for standard instance.

### Response

Repeat the request without destination file organization parameter.

## FTR2054

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2054 (&01)Invalid command

### Meaning

The specified command is not allowed in this context.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the request with a valid command.

## FTR2055

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2055 (&01)Transfer of protection attributes not supported

### Meaning

The transfer of protection attributes is not supported
- when the target file is to be extended
- with transparent transfer
- with ftp or ftam transfer
- with inhomogeneous transfer
(&01): Name of instance; empty for standard instance.

## FTR2056

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2056 (&01)Syntax error in partner name '(&00)'

### Meaning

The syntax of the partner name is wrong.
(&01): Name of instance; empty for standard instance.

### Response

Correct partner name. Repeat the command.

## FTR2057

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2057 (&01)openFT is not authorized to execute administration requests

## FTR2058

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2058 (&01)User data encryption is mandatory

### Meaning

The data encryption function is mandatory.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the request with data encryption.

## FTR2070

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2070 (&01)Request (&00). openFT is no longer authorized to execute requests for this user

## FTR2071

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2071 (&01)Request (&00). User data encryption not installed

### Meaning

The user data encryption function cannot be used unless openFT-CR
is installed.
(&01): Name of instance; empty for standard instance.

### Response

Use openFT-CR.

## FTR2072

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2072 (&01)Request (&00) has been canceled

### Meaning

The FT request was canceled because
- the command /CANCEL-FILE-TRANSFER or /NCANCEL was specified, or
- the time specified in /TRANSFER-FILE or /NCOPY has been reached.
Follow-up processing has been started for the local system, provided no
error occurred. Follow-up processing is started for the
remote system once all the resources are allocated. Local errors are
indicated by the message FTR0050 at the start of follow-up processing.
(&01): Name of instance; empty for standard instance.

## FTR2073

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2073 (&01)Request (&00). Encryption error

### Meaning

Encryption not possible.
(&01): Name of instance; empty for standard instance.

## FTR2074

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2074 (&01)Request (&00). '(&02)' could not be created(&03)

### Meaning

The command was not executed because the file owner and user
requesting the creation of a receive file are not the same.
(&01): Name of instance; empty for standard instance.

### Response

Match the user ID in the receive system's TRANSFER ADMISSION to the
ID of the receive file owner.
Repeat the command.

## FTR2075

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2075 (&01)Request (&00). Higher-level directory no longer found

## FTR2076

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2076 (&01)Request (&00). I/O error for '(&02)'(&03)

### Meaning

The file can no longer be accessed. It may have been deleted during a
transfer.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the request.

## FTR2077

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2077 (&01)Request (&00). File now locked to prevent multiple access

### Meaning

The command was not executed because the send file or the
receive file is already locked by another process so that it cannot be
simultaneously updated.
File is inaccessible or remote Pubset is not connected.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the command later or unlock the file.
After a system crash you may need to verify files that
are not closed correctly.
If the lock is caused by an FT request, it will be released
automatically when the request is finished.

## FTR2078

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2078 (&01)Request (&00). '(&02)' no longer available(&03)

### Meaning

The command was not executed because the volume for either
the send file or the receive file is not mounted, unknown or reserved,
the file extends over more than one private disk, or an attempt has been
made to transfer a file migrated by HSMS.
(&01): Name of instance; empty for standard instance.

### Response

Inform the operator if necessary or carry out an HSMS recall for the
file. Repeat the command.

## FTR2079

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2079 (&01)Request (&00). '(&02)' no longer found

### Meaning

The local send or receive file can no longer be accessed because,
for example, it was deleted during an interruption of the openFT system.
(&01): Name of instance; empty for standard instance.

### Response

Restore the file.
Repeat the command.

## FTR2080

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2080 (&01)Request (&00). Home directory no longer found(&02)

## FTR2081

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2081 (&01)Request (&00). '(&02)' gets no more space

### Meaning

The command was not (any further) executed because
- the permissible disk space on the receiving system for the user ID
specified in TRANSFER-ADMISSION has been used up, or
- the send file contains too long a sequence of empty blocks, or
- the primary and/or secondary allocation of the password-protected
receive file is too small.
The receive file can not be created/extended once this problem occurs.
(&01): Name of instance; empty for standard instance.

### Response

Take the appropriate action depending on the cause of the error:
- delete all files no longer required on the receiving system, or
- ask the system administrator to allocate more disk space, or
- remove empty blocks from the send file, or
- increase the receive file's primary/secondary allocation.
If WRITE-MODE=EXTEND-FILE is specified, restore the receive file.
Repeat the command.

## FTR2082

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2082 (&01)Request (&00). File owner no longer known

### Meaning

The command was not executed because the owner of the send file or
receive file is not defined on the relevant system or because the file
owner and the user who wants to create a receive file are not the same.
(&01): Name of instance; empty for standard instance.

### Response

Define the file owner, or correct TRANSFER-ADMISSION or FILE-NAME.
Repeat the command.

## FTR2083

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2083 (&01)Request (&00). Pre-/post-processing error(&02)

### Meaning

The command executed as part of local pre-/post-processing returned a
result other than OK.
(&01): Name of instance; empty for standard instance.

### Response

Correct and repeat the command.

## FTR2084

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2084 (&01)Request (&00). Exit code (&02) for pre-/post-processing(&03)

### Meaning

The command executed as part of local pre-/post-processing returned
the exit code (&02).
(&01): Name of instance; empty for standard instance.

### Response

Correct the command using the exit code (&02) and issue it again.

## FTR2085

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2085 (&01)Request (&00). File password no longer valid

### Meaning

The command was not executed because the password for send file or
or the receive file is missing or incorrect.
(&01): Name of instance; empty for standard instance.

### Response

Correct the password in the file description or the command.
Repeat the command.

## FTR2086

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2086 (&01)Request (&00). '(&02)' is now read only

## FTR2087

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2087 (&01)Request (&00). File structure error(&02)

### Meaning

The command was executed due to a file structure error.
File structure errors include:
- The attributes of the send file are incomplete.
- The data of the send file is incompatible with its structure
attributes.
- The records of the send file are too long.
- If WRITE-MODE=EXTEND-FILE or -e is specified, the send file and
receive file have different structures
(e.g. fixed-/variable-length records).
- The send file or receive file is a member of an old LMS library
(not PLAM).
- The source file has an odd block factor (e.g. BLKSIZE=(STD,1))
and the receive file is to be stored on an NK4 pubset.
(&01): Name of instance; empty for standard instance.

### Response

Correct the file or file attributes. If WRITE-MODE=EXTEND-FILE or -e
is specified, restore the receive file. Repeat the command.

## FTR2088

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2088 (&01)Request (&00). NDMS error (&02)

### Meaning

The request was rejected because the partner system currently does not
have the resources available to accept requests.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the request a little later.
If the error persists, contact the FT administrator.

## FTR2089

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2089 (&01)Request (&00). Recovery failed(&02)

### Meaning

The restart attempts were unsuccessful (for example, a
pre-/post-processing command could not be completed before the
termination of openFT).
(&01): Name of instance; empty for standard instance.

### Response

Repeat the command.

## FTR2090

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2090 (&01)Request (&00). Error in file transfer completion

### Meaning

An error occurred during the final phase of the file transfer.
If it was a long transfer, the recipient is advised to check
if the file has still been transferred correctly. However, error
follow-up processing will be started if it was specified.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the request, if necessary

## FTR2091

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2091 (&01)Requests only partially completed; (&00) of (&02) files were transferred

### Meaning

In the case of a synchronous send request with wildcards, not all files
were successfully transferred.
(&01): Name of instance; empty for standard instance.

### Response

Transfer unsuccessfully transferred files again.

## FTR2092

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2092 (&01)Request (&00). Access to '(&02)' no longer permissible(&03)

### Meaning

The command was not executed because either the send file or
the receive file only permits certain access modes (e.g. read only) or
because a directory was specified as either the source or destination of
a file transfer.
(&01): Name of instance; empty for standard instance.

### Response

Correct the transfer direction, write mode, file name or file protection
attributes. Repeat the command.

## FTR2093

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2093 (&01)Request (&00). FTAM error (&02)

### Meaning

The request was rejected by FTAM with the specified FTAM diagnostic code.
(&01): Name of instance; empty for standard instance.

## FTR2094

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2094 (&01)Request (&00). Retention period of file not yet expired

### Meaning

The command was not executed because the retention period protecting the
receive file against overwriting has not yet expired (RETENTION PERIOD).
(&01): Name of instance; empty for standard instance.

### Response

Correct the transfer direction, retention period or file name.
Repeat the command.

## FTR2095

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2095 (&01)Request (&00). Extension of file not possible for transparent transfer

### Meaning

The command could not be executed because it is not possible to add to
a file in a transparent transfer.
(&01): Name of instance; empty for standard instance.

### Response

Start transfer without EXTEND.

## FTR2096

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2096 (&01)Request (&00). File structure not supported(&02)

## FTR2097

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2097 (&01)Request (&00). Resulting file name '(&02)' too long(&03)

### Meaning

The relative file name was specified in the transfer request.
The absolute file name completed by openFT is longer than permitted.
(&01): Name of instance; empty for standard instance.

### Response

Shorten the file name or path and repeat the command.

## FTR2099

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2099 (&01)Request (&00). Transfer of protection attributes not supported

### Meaning

The transfer of protection attributes is not supported
- with transparent transfer
- when the target file is extended
- with ftp or ftam transfer
- with inhomogeneous transfer
(&01): Name of instance; empty for standard instance.

## FTR2100

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2100 (&01)Requests only partially completed; (&00) of (&02) directories were transferred

### Meaning

In the case of a synchronous send request with wildcards,
not all directories were successfully transferred.
(&01): Name of instance; empty for standard instance.

### Response

Transfer unsuccessfully transferred directories again.

## FTR2109

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2109 (&01)Request (&00). Connection setup rejected by local transport system

## FTR2110

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2110 (&01)Request (&00). Data integrity check indicates an error

### Meaning

The integrity of the data was violated.
(&01): Name of instance; empty for standard instance.

## FTR2111

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2111 (&01)Encryption/data integrity check not possible. Encryption switched off

### Meaning

There is no key pair or the key length was set to 0. Requests can
only be carried out without data encryption or a data integrity check.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the request without data encryption, create
a key or set a key length >0.

## FTR2112

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2112 (&01)Request (&00). Data integrity check not supported by partner

### Meaning

The partner system does not support the data integrity check.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the request without a data integrity check.

## FTR2113

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2113 (&01)Request (&00). User data encryption not possible for this request

### Meaning

The partner system does not support the data encryption function.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the request without data encryption or install/enable secure
mechanism (or have it installed) on the remote system. For OPENFT and FTP
enable encryption, for FTP install/enable a TLS secure ftp server.

## FTR2114

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2114 (&01)Request (&00). Identification of local system rejected by remote system '(&02)'

### Meaning

For security reasons or because of an inconsistency, the partner did
not accept the instance identification of the local system (for
example, because in a network description file both the instance
identification and migration identification %.prozessor.entity occur
for different partners).
(&01): Name of instance; empty for standard instance.

### Response

Ensure that the local identification has been entered correctly on the
partner system and has not been assigned to a different partner.

## FTR2115

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2115 (&01)Request (&00). Interrupted by remote system

## FTR2116

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2116 (&01)Local application '(&00)' not defined

### Meaning

The local application is not defined in the transport system, or
the tnsxd process will not run in UNIX.
(&01): Name of instance; empty for standard instance.

### Response

Make the local application known to the local transport
system or start the tnsxd process.

## FTR2117

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2117 (&01)Local application '(&00)' not available

### Meaning

If FTAM is installed, possibly the subsystem OSS is not started.
(&01): Name of instance; empty for standard instance.

## FTR2118

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2118 (&01)Request (&00). Authentication of local system failed

### Meaning

The local system could not be authenticated by the partner system.
(&01): Name of instance; empty for standard instance.

### Response

Give the current public key file to the partner and
name it correctly there. Repeat the command.

## FTR2119

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2119 (&01)Request (&00). Local system unknown in remote system

### Meaning

The local system is not known on the partner system
(e.g. BS2000/OSD or z/OS).
(&01): Name of instance; empty for standard instance.

### Response

Make the local system known on the partner system
and repeat the command.

## FTR2120

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2120 (&01)Remote system '(&00)' unknown

### Meaning

The partner specified as the remote system cannot be expanded to an
address on the local system.
(&01): Name of instance; empty for standard instance.

### Response

Correct the specification for the partner or add the
partner to the partner list and repeat the command.

## FTR2121

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2121 (&01)Request (&00). Authentication of partner failed

### Meaning

The remote system could not be authenticated by the local system.
(&01): Name of instance; empty for standard instance.

### Response

Get the current public key file from the partner
and name it correctly.

## FTR2122

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2122 (&01)Request (&00). FT session rejected or disconnected. Reason (&02)

## FTR2123

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2123 (&01)Request (&00). OSS call error (&02)

### Meaning

The command wsa not executed because the session instance detected a
communication error.
(&00): error code.
(&01): Name of instance; empty for standard instance.

### Response

Take the appropriate action in accordance with the error code.

## FTR2124

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2124 (&01)Request (&00). No free connection

### Meaning

No more transfers are possible because the maximum number of
simultaneous transfers has been reached.
(&01): Name of instance; empty for standard instance.

### Response

Check whether the transport system is working
(or have it checked).

## FTR2125

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2125 (&01)Request (&00). Connection lost

### Meaning

No data transfer took place because of a line interrupt or a line
protocol error.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the request.

## FTR2126

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2126 (&01)Request (&00). Transport system error. Error code (&02)

### Meaning

An error occurred in the transport system during processing of a
/START-FT command or ftstart or a file transfer or file management
request.
(&01): Name of instance; empty for standard instance.

### Response

Take the appropriate action in accordance with the error code. Most
often the occurrence of this message indicates that the partner
addressed is not known to the transport system. Contact system
administrator to make sure there is a BCIN for the partner system.

## FTR2127

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2127 (&01)Request (&00). No data traffic within (&02) seconds

### Meaning

No data transfer took place within the period of seconds specified
because, for example, the connection is interrupted, the partner is not
sending and the local system is waiting for data.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the request.

## FTR2128

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2128 (&01)OSS version not supported

### Meaning

At least OSS version V04.1 required
(&01): Name of instance; empty for standard instance.

## FTR2129

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2129 (&01)No further files will be transferred

### Meaning

Check the previous transfer error code
(&01): Name of instance; empty for standard instance.

## FTR2130

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2130 (&01)Local application '(&00)' not available. Incorrect hostname: '(&02)'.

### Meaning

Provided hostname cannot be converted into IP address.
(&01): Name of instance; empty for standard instance.

## FTR2140

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2140 (&01)Request (&00). Remote system: openFT is not authorized to execute requests for this user

## FTR2141

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2141 (&01)Request (&00). Remote system: Directory '(&02)' is not empty

### Meaning

The command could not be executed because there are files in the
specified directory of the partner system.
(&01): Name of instance; empty for standard instance.

### Response

Delete all the files in the directory first and
repeat the command.

## FTR2142

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2142 (&01)Request (&00). Remote system: File attributes do not match the request parameters(&02)

### Meaning

The command could not be executed because the file attributes on the
remote system do not agree with the request parameters
(e.g. a directory was specified instead of a remote file).
(&01): Name of instance; empty for standard instance.

### Response

Check the file name on the remote system and correct it.
Repeat the command.

## FTR2143

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2143 (&01)Request (&00). Remote system: Attributes could not be modified(&02)

### Meaning

The properties of the file could not be modified as desired in the
command. Possible reasons are:
For the remote file:
- No access rights to the file.
- The combination of access rights required is not supported by the
remote system.
- If the remote system is a BS2000: the file is protected by ACL.
(&01): Name of instance; empty for standard instance.

## FTR2144

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2144 (&01)Request (&00). Remote system: File/directory '(&02)' could not be created(&03)

### Meaning

The command was not executed because the file owner and user
requesting the creation of a receive file are not the same.
(&01): Name of instance; empty for standard instance.

### Response

Match the user ID in the receive system's TRANSFER-ADMISSION to the
ID of the receive file owner.
Repeat the command.

## FTR2145

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2145 (&01)Request (&00). Remote system: CCS name unknown or not supported

### Meaning

The request could not be carried out because the CSS names of the send
and receive files cannot be mapped to each other or because the partner
system does not support the receipt of files in a transparent format.
(&01): Name of instance; empty for standard instance.

## FTR2146

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2146 (&01)Request (&00). Remote system: Higher-level directory not found

### Meaning

The command was not executed because the higher-level directory could
not be found on the partner system.
(&01): Name of instance; empty for standard instance.

### Response

Create the directory on the remote system or correct the remote
directory name and repeat the command.

## FTR2147

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2147 (&01)Request (&00). Remote system: File/directory '(&02)' already exists

### Meaning

The command was not executed. Possible reasons:
- The command was not executed because an existing receive file
cannot be created with 'WRITE-MODE=NEW' or the -n option.
WRITE-MODE=NEW or -n may also have been set by a restriction in
the access authorization used.
- ftcredir: The specified directory already exists.
(&01): Name of instance; empty for standard instance.

### Response

Either delete the receive file before repeating the command or reenter
the command specifying WRITE-MODE=REPLACE-FILE or using
different access authorization.

## FTR2148

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2148 (&01)Request (&00). Remote system: Transfer of file generation groups not supported

### Meaning

The command was not executed because the FT system can only transfer
single file generations.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the command using the name of a single file generation.

## FTR2149

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2149 (&01)Request (&00). Remote system: Access error for '(&02)'(&03)

### Meaning

The FT system continues to run after output of the message.
(&00): DMS error, possibly the transfer ID
(&01): Name of instance; empty for standard instance.

### Response

Take the appropriate action in accordance with the error code.

## FTR2150

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2150 (&01)Request (&00). Remote system: Resulting file name too long(&02)

### Meaning

The file name that results from command parameters and potential
file-name processing as specified by an admission profile exceeds
the allowed maximum file name length.
Possible reasons:
- Values assigned outside the valid range
- Invalid operand separators
- Invalid value assignment characters
- Partially qualified file names
- File name exceeding the maximum buffer length
(&01): Name of instance; empty for standard instance.

### Response

Repeat the command using the correct syntax.

## FTR2151

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2151 (&01)Request (&00). Remote system: File locked to prevent multiple access

### Meaning

The command was not executed because either the send file or the
receive file is already locked by another process to prevent it from
being updated simultaneously.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the command later or unlock the file on the remote system.
After a system crash in BS2000 you may need to verify files
not closed correctly.
If the lock is caused by an FT request, it will be released
automatically when the request is finished.

## FTR2152

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2152 (&01)Request (&00). Remote system: No file or directory name specified

### Meaning

The command was not executed because the file ID was neither
specified explicitly nor by the 'TRANSFER-ADMISSION' used.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the command, specifying the file ID explicitly or using a
TRANSFER ADMISSION that defines the file ID.

## FTR2153

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2153 (&01)Request (&00). Remote system: Invalid management password

## FTR2154

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2154 (&01)Request (&00). Remote system: File/directory '(&02)' not available(&03)

### Meaning

The command was not executed because the volume for either
the send file or the receive file is not mounted, unknown or reserved,
the file extends over more than one private disk, or an attempt has
been made to transfer a file migrated by HSMS.
(&01): Name of instance; empty for standard instance.

### Response

Inform the operator if necessary or carry out an HSMS recall for the
file. Repeat the command.

## FTR2155

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2155 (&01)Request (&00). Remote system: File/directory '(&02)' not found

### Meaning

The command was not executed because the send file is not or no longer
in the catalog or on a volume of the remote system.
(&01): Name of instance; empty for standard instance.

### Response

Correct the remote file name, read the file in from tape or restore the
send file. Repeat the command.

## FTR2156

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2156 (&01)Request (&00). Remote system: Home directory not found(&02)

## FTR2157

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2157 (&01)Request (&00). Remote system: Renaming not possible(&02)

## FTR2158

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2158 (&01)Request (&00). Remote system: Not enough space for '(&02)'

### Meaning

The command was not executed (any further) because
- the permissible storage space on the receive system for the
user ID specified in TRANSFER-ADMISSION has been used up, or
- the send file contains too long a sequence of empty blocks,
or
- the primary and/or secondary allocation of the password-
protected receive file is too small.
The receive file is no longer created/extended after the problem
has occurred.
(&01): Name of instance; empty for standard instance.

### Response

Take the appropriate action depending on the cause of the error:
- delete all files no longer required on the receive system, or
- ask the system administrator to allocate more storage space, or
- remove empty blocks from the send file, or
- increase the receive file's primary/secondary allocation.
If WRITE-MODE=EXTEND-FILE is specified, restore the receive file.
Repeat the command.

## FTR2159

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2159 (&01)Request (&00). Remote system: File owner unknown

### Meaning

The command was not executed because the owner of either the send
file or the receive file was not defined on the relevant system or
because the file owner and the user requesting the creation of a
receive file are not the same.
(&01): Name of instance; empty for standard instance.

### Response

Define the file owner, correct TRANSFER-ADMISSION or FILE-NAME.
Repeat the command.

## FTR2160

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2160 (&01)Request (&00). Remote system: Invalid file password

### Meaning

The command was not executed because the password for the send file
or the receive file is missing or incorrect.
(&01): Name of instance; empty for standard instance.

### Response

Correct the password in the file description or the command.
Repeat the command.

## FTR2161

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2161 (&01)Request (&00). Remote system: Retention period of file not yet expired

### Meaning

The command was not executed because the retention period protecting
the receive file against overwriting has not yet expired.
(&01): Name of instance; empty for standard instance.

### Response

Correct the transfer direction, retention period or file name.
Repeat the command.

## FTR2162

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2162 (&01)Request (&00). Remote system: File/directory '(&02)' is read only

### Meaning

The file or directory is write-protected.
(&01): Name of instance; empty for standard instance.

### Response

Correct the remote file name or remove the write protection of the
remote file. Repeat the command.

## FTR2163

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2163 (&01)Request (&00). Remote system: File structure not supported(&02)

### Meaning

The request cannot be carried out because the file structure is not
supported. For example, an attempt was made to get a PLAM library or
ISAM file from the BS2000 system.
(&01): Name of instance; empty for standard instance.

### Response

Transfer the file transparently.

## FTR2164

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2164 (&01)Request (&00). Remote system: Syntax error in resulting file name(&02)

### Meaning

The file name that results from command parameters and potential
file-name processing as specified by an admission profile is not
acceptable to the remote system or cannot be converted to the remote
file-name encoding.
Possible reasons:
- Values assigned outside the valid range
- Invalid operand separators
- Invalid value assignment characters
- Partially qualified file names
- Unicode file name is not supported
- File name separator not found
- Remote system unable to decode the filename properly
(&01): Name of instance; empty for standard instance.

### Response

Repeat the command using the correct syntax.

## FTR2165

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2165 (&01)Request (&00). Remote system: Transparent file transfer not supported

### Meaning

The request could not be carried out because the partner system does
not support the transfer of files in a transparent format.
(&01): Name of instance; empty for standard instance.

## FTR2166

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2166 (&01)Request (&00). Remote system: Extension of file not possible for transparent transfer

### Meaning

The command could not be executed because it is not possible to add to
a file in a transparent transfer.
(&01): Name of instance; empty for standard instance.

## FTR2167

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2167 (&01)Request (&00). Remote system: Access to '(&02)' denied(&03)

### Meaning

The command was not executed because the remote file only permits
certain access modes.
(&01): Name of instance; empty for standard instance.

### Response

Correct the transfer direction, file name or file protection
attributes on the remote system. Repeat the command.

## FTR2168

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2168 (&01)Request (&00). Remote system: Follow-up processing exceeds length limit

### Meaning

The length of follow-up processing was exceeded;
see the command syntax description.
(&01): Name of instance; empty for standard instance.

### Response

Shorten the follow-up processing, or use procedures.
Repeat the command.

## FTR2169

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2169 (&01)Request (&00). Remote system: Transfer admission invalid

### Meaning

The command was not executed because the specifications in one of
the TRANSFER-ADMISSION operands are incorrect or the request was
rejected by FTAC because of insufficient authorization.
(&01): Name of instance; empty for standard instance.

### Response

Define the requisite TRANSFER-ADMISSION or correct it or check the
authorization entered in FTAC. Repeat the command if necessary.

## FTR2170

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2170 (&01)Request (&00). Remote system: Function not supported(&02)

## FTR2171

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2171 (&01)Request (&00). Remote system: Follow-up processing admission invalid

### Meaning

The command was not executed because the specifications in one of the
PROCESSING-ADMISSION operands are incorrect.
(&01): Name of instance; empty for standard instance.

### Response

Define the required PROCESSING ADMISSION or correct it.
Repeat the command if necessary.

## FTR2172

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2172 (&01)Request (&00). Remote system: Request queue full

### Meaning

The command was not executed because the maximum number of
permissible file transfer requests has been reached.
(&01): Name of instance; empty for standard instance.

### Response

Notify the FT administrator. Repeat the command later.

## FTR2173

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2173 (&01)Request (&00). Remote system: User data encryption is mandatory

### Meaning

The remote system only accepts requests using
data encryption.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the request using data encryption.

## FTR2174

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2174 (&01)No files corresponding to specified pattern found

### Meaning

Specify the correct file name pattern.
(&01): Name of instance; empty for standard instance.

## FTR2195

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2195 (&01)Request (&00). Remote system: openFT is no longer authorized to execute requests for this user

## FTR2196

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2196 (&01)Request (&00) has been canceled in the remote system

### Meaning

The request was deleted on the remote system before termination.
(&01): Name of instance; empty for standard instance.

## FTR2197

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2197 (&01)Request (&00). Remote system: File/directory '(&02)' could not be created(&03)

### Meaning

The command was not executed because the file owner and user
requesting the creation of a receive file are not the same.
(&01): Name of instance; empty for standard instance.

### Response

Match the user ID in the receive system's TRANSFER-ADMISSION to the
ID of the receive file owner. Repeat the command.

## FTR2198

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2198 (&01)Request (&00). Remote system: Higher-level directory no longer found

## FTR2199

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2199 (&01)Request (&00). Remote system: I/O error for '(&02)'(&03)

### Meaning

An error occurred at input/output. Possible cause:
- BS2000: DMS error
- The send or receive files was deleted during transfer.
The FT system continues to run after the message has been issued.
(&01): Name of instance; empty for standard instance.

### Response

Take the appropriate action in accordance with the error code.

## FTR2200

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2200 (&01)Request (&00). Remote system: File now locked to prevent multiple access

### Meaning

The command was not executed because either the send file or the
receive file is already locked by another process to prevent it from
being updated simultaneously. An attempt is made, for example, to access
a library opened in z/OS.
File is inaccessible or remote Pubset is not connected.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the command later or unlock the file.
After a system crash you may need to verify files not closed correctly.
If a lock is caused by an FT request, it will be released
automatically when the request is finished.

## FTR2201

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2201 (&01)Request (&00). Remote system: File/directory '(&02)' no longer available(&03)

### Meaning

The command was not executed because the volume for either
the send file or the receive file is not mounted, unknown or reserved,
or because the file extends over more than one private disk or an
attempt has been to transfer a file migrated by HSMS.
(&01): Name of instance; empty for standard instance.

### Response

Inform the operator if necessary or carry out an HSMS recall for the
file. Repeat the command.

## FTR2202

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2202 (&01)Request (&00). Remote system: File/directory '(&02)' no longer found

### Meaning

The command was not executed because the remote file is not or no
longer in the catalog or on a volume of the corresponding system
(e.g. after a restart).
(&01): Name of instance; empty for standard instance.

### Response

Restore the remote file.
Repeat the command.

## FTR2203

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2203 (&01)Request (&00). Remote system: Home directory no longer found(&02)

## FTR2204

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2204 (&01)Request (&00). Remote system: File/directory '(&02)' gets no more space

### Meaning

The command was not executed (any further) because
- the permissible storage space on the receive system for the
user ID specified in TRANSFER-ADMISSION has been used up, or
- the send file contains too long a sequence of empty blocks,
or
- the primary and/or secondary allocation of the password-
protected receive file is too small.
The receive file can no longer be created/extended after the problem
occurs.
(&01): Name of instance; empty for standard instance.

### Response

Take the appropriate action depending on the cause of the error:
- delete all files no longer required on the receive system, or
- ask the system administrator to allocate more storage space, or
- remove empty blocks from the send file, or
- increase the receive file's primary/secondary allocation.
If WRITE-MODE=EXTEND-FILE is specified, restore the receive file.
Repeat the command.

## FTR2205

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2205 (&01)Request (&00). Remote system: File owner no longer known

### Meaning

The command was not executed because the owner of either the send
file or the receive file is not defined on the relevant system, or
because the file owner and the user requesting the creation of the
receive file are not the same.
(&01): Name of instance; empty for standard instance.

### Response

Define the file owner, correct TRANSFER-ADMISSION or FILE-NAME.
Repeat the command.

## FTR2206

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2206 (&01)Request (&00). Remote system: Pre-/post-processing error(&02)

### Meaning

The command executed in local pre-/postprocessing returned a result
value other than OK.
(&01): Name of instance; empty for standard instance.

### Response

Correct the pre-/post-processing command and issue it again.

## FTR2207

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2207 (&01)Request (&00). Remote system: Exit code (&02) during pre-/post-processing(&03)

### Meaning

The command executed in remote pre-/postprocessing returned the exit
code (&02).
(&01): Name of instance; empty for standard instance.

### Response

Correct the pre-/post-processing command in accordance
with the exit code and issue it again.

## FTR2208

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2208 (&01)Request (&00). Remote system: File password no longer valid

### Meaning

The command was not executed because the password for the send file
or receive file is missing or incorrect.
(&01): Name of instance; empty for standard instance.

### Response

Correct the password in the file description or the command.
Repeat the command.

## FTR2209

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2209 (&01)Request (&00). Remote system: File/directory '(&02)' is now read only

## FTR2210

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2210 (&01)Request (&00). Remote system: File structure error(&02)

### Meaning

The command was not executed due to a file structure error.
File structure errors include:
- The attributes of the send file are incomplete.
- The data of the send file is incompatible with its structure
attributes.
- The records of the send file are too long.
- If WRITE-MODE=EXTEND-FILE or the -e parameter are specified,
the send file and receive file have different structures
(e.g. fixed-/variable-length records).
- BS2000: The send or receive file is a member of an old LMS
library (not PLAM).
- BS2000: The send file has an odd block factor (e.g.
BLKSIZE=(STD,1)), and the receive file is stored on an NK4
pubset.
(&01): Name of instance; empty for standard instance.

### Response

Correct the file or file attributes. If WRITE-MODE=EXTEND-FILE is
specified, restore the receive file. Repeat the command.

## FTR2211

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2211 (&01)Request (&00). Remote system: NDMS error (&02)

### Response

Repeat the request a little later.
If the error persists, contact the FT administrator.

## FTR2212

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2212 (&01)Request (&00). Remote system: Recovery failed(&02)

### Meaning

The restart could not be carried out. It may not have been possible to
complete restart-capable pre-/post-processing before termination of the
server process (waiting time: max. 10 minutes).
(&01): Name of instance; empty for standard instance.

### Response

Repeat the command.

## FTR2213

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2213 (&01)Request (&00). Remote system: Resource bottleneck

### Meaning

The order was rejected because the partner system currently
does not have the resources available to accept requests.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the request a little later.

## FTR2214

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2214 (&01)Request (&00). Remote system: Access to '(&02)' is no longer permissible(&03)

### Meaning

The command was not executed because the send file or receive file only
permits certain access modes (e.g. read only) or a directory was
specified as the source or destination of a file transfer.
(&01): Name of instance; empty for standard instance.

### Response

Correct the transfer direction, write mode, file name or file
protection attributes. Repeat the command.

## FTR2215

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2215 (&01)Request (&00). FTAM error (&02)

### Meaning

The request was rejected by FTAM with the specified FTAM diagnostic code.
(&01): Name of instance; empty for standard instance.

## FTR2216

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2216 (&01)Request (&00). Remote system: File structure not supported(&02)

### Meaning

The request cannot be carried out because the file structure is not
supported. An attempt was made, for example, to get a PLAM library or
ISAM file from BS2000.
(&01): Name of instance; empty for standard instance.

### Response

Transfer the file transparently.

## FTR2217

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2217 (&01)Request (&00). Remote system: Retention period of file not yet expired

### Meaning

The command was not executed because the retention period protecting
the receive file against overwriting has not yet expired.
(&01): Name of instance; empty for standard instance.

### Response

Correct the transfer direction, retention period or file name.
Repeat the command.

## FTR2218

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2218 (&01)Request (&00). Remote system: Extension of file not possible for transparent transfer

### Meaning

The command could not be executed because it is not possible to add to
a file in a transparent transfer.
(&01): Name of instance; empty for standard instance.

## FTR2225

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2225 (&01)Information output canceled

### Meaning

A show command was interrupted, for example.
(&01): Name of instance; empty for standard instance.

### Response

Repeat the command.

## FTR2226

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2226 (&01)Job variable contents inconsistent

### Meaning

The command cannot be accepted because the contents of the specified
job variable are inconsistent.
Possible reason: The job variable was accessed by the user in a mode
other than read mode while it was monitoring an FT request.
The contents of the job variable can no longer be used.
(&01): Name of instance; empty for standard instance.

## FTR2227

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2227 (&01)Job variable not in use by openFT

### Meaning

A process other than openFT is using the job variable.
(&01): Name of instance; empty for standard instance.

### Response

Correct the name of the job variable and repeat the command.

## FTR2228

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR2228 (&01)Job variable not found

### Response

Correct the name of the job variable and repeat the command.

## FTR3000

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3000 en

## FTR3001

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3001 account

## FTR3002

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3002 transport unit size

## FTR3003

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3003 cancel date

## FTR3004

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3004 cancel time hhmm

## FTR3005

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3005 connection limit

## FTR3006

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3006 (&00)

## FTR3007

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3007 file creation password

## FTR3008

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3008 date/time

## FTR3009

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3009 directory

## FTR3010

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3010 future file size

## FTR3011

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3011 file name

## FTR3012

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3012 file access password

## FTR3013

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3013 FTAC LOGGING: all FTAC access checks

## FTR3014

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3014 FTAC LOGGING: rejected FTAC access checks

## FTR3015

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3015 FTAC LOGGING: modifying FM requests and FTAC access rejections

## FTR3016

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3016 FTAC: not installed

## FTR3017

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3017 FTAM server: not started

## FTR3018

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3018 FTAM server: started

## FTR3019

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3019 identification

## FTR3020

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3020 IDENTIFICATION: (&00)

## FTR3021

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3021 key reference

## FTR3022

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3022 legal qualification

## FTR3023

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3023 LOCAL SYSTEM NAME: (&00),(&02)

## FTR3024

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3024 FT LOGGING: all FT requests

## FTR3025

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3025 FT/FTAC LOGGING: No information can be obtained on the logging status

## FTR3026

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3026 FT LOGGING: failed FT requests

## FTR3027

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3027 FT LOGGING: switched off

## FTR3028

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3028 maximum number of inbound requests

## FTR3029

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3029 maxisp

## FTR3030

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3030 maxosp

## FTR3031

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3031 Jan,Feb,Mar,Apr,May,Jun,Jul,Aug,Sep,Oct,Nov,Dec

## FTR3032

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3032 management password

## FTR3033

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3033 name

## FTR3034

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3034 new file name

## FTR3035

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3035 no

## FTR3036

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3036 openFT: not started

## FTR3037

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3037 owner ID

## FTR3038

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3038 o p e n F T P A R A M E T E R I N F O R M A T I O N

## FTR3039

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3039 TUSIZE MAXOSP MAXISP LOCRQ REMRQ MAXISQE TIMEXIST CHARACTERSET KEYL

## FTR3040

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3040 parameter list

## FTR3041

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3041 partner

## FTR3042

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3042 partner address

## FTR3043

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3043 partner name

## FTR3044

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3044 follow-up proc

## FTR3045

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3045 polling interval

## FTR3046

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3046 polling number

## FTR3047

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3047 port number

## FTR3048

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3048 prefix

## FTR3049

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3049 process limit

## FTR3050

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3050 processor name

## FTR3051

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3051 password

## FTR3052

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3052 reason code

## FTR3053

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3053 record length

## FTR3054

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3054 routing info

## FTR3055

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3055 maximum number of requests

## FTR3056

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3056 request lifetime

## FTR3057

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3057 security level

## FTR3058

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3058 start date

## FTR3059

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3059 openFT: started

## FTR3060

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3060 start time hhmm

## FTR3061

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3061 station name

## FTR3062

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3062 new account number

## FTR3063

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3063 transfer admission

## FTR3064

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3064 request ID

## FTR3065

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3065 o p e n F T R E Q U E S T Q U E U E I N F O R M A T I O N

## FTR3066

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3066 TID <-> S BYTECOUNT I USERID LOCAL FILENAME REMSYS DIAGCODE

## FTR3067

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3067 --------------------------------------------------------------------------- ----

## FTR3068

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3068 FT TRACE: started

## FTR3070

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3070 user ID

## FTR3071

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3071 yes

## FTR3072

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3072 command

## FTR3073

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3073 CCS name

## FTR3075

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3075 administrator ID

## FTR3076

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3076 openFT is started

## FTR3077

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3077 CMX not installed

## FTR3078

Destination: USER-TASK, CONSOLE Routing code: C Weight: 99

Warranty : NO

FTR3078 global request ID

©2025 Fujitsu | BS2000 System Messages