## SEKREVI

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

SEKREVI COMP=SEKMF,VERS=91A,DATE=201215

## SEK0001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK0001 CONSISTENCY CHECK (&00) '(&01)'

### Meaning

(&00): <CC-no.>/<CC-weight>/<CC-subnumber>
error weight of the consistency check (CC):
05: dump only: DBH will continue;
70: faulty request; 71: system bottleneck;
72: faulty DBH; 82: system dump;
83: faulty system;
(&01): DCM or DMS return code.

### Response

Submit dump(s) to diagnostics department.

## SEK0002

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK0002 IN CONFIGURATION '(&00)' SESAM '(&01)' NOT AVAILABLE

## SEK0003

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK0003 IN CONFIGURATION '(&00)' SESAM '(&01)' NOT AVAILABLE. INPUT REPLY : (R : REPEAT; H : HALT)

### Meaning

DBH (&01) in configuration (&00), specified in the DBCON start
parameters, is not available.

### Response

Possible input:
R : DBCON will try to connect to DBH (&01)
in configuration (&00) once again;
H : current request will be aborted;
To subpress this message, insert parameter NOTYPE into the
DBCON start parameters.

## SEK0004

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK0004 SESDCN (&00) IN CONFIGURATION (&01) (PROCESSOR (&02)) NOT AVAILABLE

## SEK0005

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK0005 MODIFY START PARAMETER CNF=(&00), NAM=(&01). INPUT REPLY : (R : REPEAT; H : HALT; NAM=X : NEW DBH NAME X)

### Meaning

DBH (&01) in configuration (&00), specified in the DBCON start
parameters, is not available.
Start parameter NAM can be modified.

### Response

Possible input:
R : DBCON will try to connect to DBH (&01)
in configuration (&00) once again;
H : current request will be aborted;
NAM=x : Input new DBH name. DBCON will try to connect to
DBH x in configuration (&00);
To subpress this message, insert parameter NOTYPE into the
DBCON start parameters.

## SEK0006

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK0006 SESAM (&00) IN CONFIGURATION (&01) ON HOST (&02) FOR CATALOG (&03) NOT AVAILABLE.

### Meaning

A statement concerning the catalog cannot be delivered to the
databasehandler

### Response

If the databasehandler is in the own configuration, check whether the
databasehandler is available.
If the databasehandler is not in the own configuration, check the
concerning entry within the distribution rule and - if this is right -
check whether the databasehandler and SESDCN are available.

## SEK0007

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK0007 SESAM (&00) IN CONFIGURATION (&01) ON HOST (&02) FOR CDML-STATEMENT (&03) NOT AVAILABLE.

### Meaning

The CDML-statement cannot be delivered to the databasehandler.

### Response

If the databasehandler is in the own configuration, check whether the
databasehandler is available.
If the databasehandler is not in the own configuration, check the
concerning entry within the distribution rule and - if this is right -
check whether the databasehandler and SESDCN are available.

## SEK0008

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK0008 CONNECTION TO SESAM (&00) IN CONFIGURATION (&01) ON MACHINE (&02) IS NOT POSSIBLE, BECAUSE THE CURRENT PROGRAM RUNS ON MACHINE (&03)

### Meaning

DBH or DCN or application are started on different machines.
Communication between application, DCN and DBH is not possible.

### Response

Terminate each task of the configuration and activate the virtual
host. Afterwards start the tasks of the configuration again.

## SEK0009

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK0009 MEMORY POOL OF APPLICATION USERS IS CREATED BY A PROGRAM, THAT RUNS ON MACHINE (&00). THE CURRENT PROGRAM RUNS ON MACHINE (&01)

### Meaning

The memory pool was created by a program running on the machine
(&00) which is no longer active.
Communication between applications and DBH is not possible.

### Response

Terminate each task of the configuration and activate the virtual
host. Afterwards start the tasks of the configuration again.

## SEK0010

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK0010 DCN POOL IS CREATED BY DCN, THAT RUNS ON MACHINE (&00). THE CURRENT PROGRAM RUNS ON MACHINE (&01). DISTRIBUTION IS NOT POSSIBLE.

### Meaning

The memory pool was created by DCN running on machine (&00) which
is no longer active. Distributed communication is not possible.
DBCON tries to communicate non distributed.

### Response

Terminate each task of the configuration and activate the virtual
host. Afterwards start the tasks of the configuration again.

## SEK1001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SEK1001 OPEN COMMUNICATION SESAM(&00)

### Meaning

Communication with the DBH opened.
(&00): SESAM communication name (DBH load option DBH-IDENTIFICATION
= (CONFIGURATION-NAME,DBH-NAME)).

## SEK1002

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SEK1002 SESAM(&00) ALREADY EXISTS

### Meaning

The DBH cannot be loaded with the specified communication ID (&00).

### Response

Change the value of CONFIGURATION-NAME or DBH-NAME in the load options.

## SEK1003

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK1003 NO USER ADDRESS SPACE AVAILABLE FOR COMMUNICATION

### Response

Expand the virtual address space or load SESAM DBH with options which
require less user address space.

## SEK1004

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK1004 CLOSE COMMUNICATION SESAM(&00)

### Meaning

The current SESAM session has been terminated.
(&00): SESAM communication name.

## SEK1005

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK1005 OPERATING SYSTEM COMPONENTS FOR INTERTASK COMMUNICATION NOT GENERATED. SESAM CANNOT BE EXECUTED.

### Response

Restart BS2000 with the appropriate generation.

## SEK1006

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK1006 OPERATING SYSTEM COMPONENTS FOR INTERTASK COMMUNICATION CANNOT BE EXECUTED BECAUSE OF LACK OF MEMORY

### Meaning

No more memory is available for the management areas of the operating
system components for intertask communication.

### Response

Repeat request later.

## SEK1011

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SEK1011 OPEN COMMUNICATION SESAM(&00) ON VIRTUAL HOST (&01)

### Meaning

Communication with DBH is open.
(&00): SESAM communication name (DBH load option DBH-IDENTIFICATION
= (CONFIGURATION-NAME,DBH-NAME)). (&01) name of virtual host.

## SEK2005

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK2005 INVALID ADMINISTRATION STATEMENT

## SEK2009

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK2009 ADMINISTRATION STATEMENT REJECTED

## SEK2010

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK2010 ADMINISTRATION STATEMENT ACCEPTED

## SEK3001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3001 NAM SPECIFICATION AT START INCORRECT OR SESAM DBH NOT LOADED

### Response

Correct the NAM specification at START or load SESAM again.

## SEK3003

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3003 ERROR DURING DISCONNECT

### Response

Send the user dump of the UTM application off for diagnosis.

## SEK3004

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3004 TRANSACTION ROLLED BACK BY SESAM

### Meaning

The SESAM-DBH rolled back the transaction because of a deadlock, a
longlock or upon instruction by the database administrator.

## SEK3005

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3005 DISCONNECTION OF THE SESAM-DBH

### Meaning

SESAM DBH run was terminated.

### Response

If the disconnection of the SESAM DBH was performed due to an error,
submit the user dump of the SESAM DBH and of the UTM application
to the diagnosis department.

## SEK3006

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3006 SESAM LOADED WITH 'TRANSACTION-SECURITY=*NO' OPTION. STATEMENT 'BEGIN TRANSACTION' REJECTED WITH STATUS '9N'

### Response

Reload SESAM with the 'TRANSACTION-SECURITY=*YES' option.

## SEK3008

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3008 KDCDB MACRO OR CONNECTION MODULE SESUTMC IS NOT THE CURRENT SESAM/SQL VERSION

### Meaning

The KDCDB macro used to generate KDCROOT is not compatible with the
current version of SESAM/SQL or the database connection module SESUTMC is
not the current SESAM/SQL version.

### Response

Generate KDCROOT with the KDCDB macro from the current SESAM/SQL version
or use the connection module SESUTMC from the current SESAM/SQL version.

## SEK3010

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3010 SESAM AND UTM RESTARTED WITH DIFFERENT BACKUP STATUS

### Meaning

Following a crash, SESAM and UTM were restarted under different
conditions: e.g. warm start for SESAM and cold start for UTM.

### Response

Start the UTM application and SESAM/SQL DBH under the same conditions.

## SEK3011

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3011 NO MORE USER ADDRESS SPACE AVAILABLE TO TASK OF UTM APPLICATION

### Response

Modify the UTM application appropriately.

## SEK3013

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3013 DBCON OR SESAM SYSTEM ERROR

### Response

Send the user dump of the UTM application off for diagnosis.

## SEK3014

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3014 CONFIGURATION AT RESTART DIFFERENT FROM THAT AT ABORT

### Meaning

Either processing took place without the aid of SESAM-DCN prior to the
abort and with it at restart, or vice versa.

### Response

Reconstruct the configuration as it existed prior to restart.

## SEK3016

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3016 SESAM CONFIGURATION AT SYSTEM RECOVERY DIFFERENT FROM THAT AT ABORT

### Meaning

The SESAM configuration identifier in the CNF start parameter for the
system recovery is different to the one valid when SESAM was aborted.

## SEK3021

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3021 ERROR ON DYNAMICALLY LOADING SECUTM1

### Meaning

The connection module SESUTMC was not able to dynamically load the entry
SECUTM1.

### Response

Check the assigned SESAM module library.

## SEK3022

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3022 STATUS ON INITIALIZING DBCON; (&00) / (&01)

### Meaning

(&00): Status number
(&01): Status subnumber
Refer to the section on 'CALL-DML messages' in the manual 'SESAM/SQL
Messages' for further details on the status number and status'
subnumber.

### Response

Evaluate the status with regard to possible user or generation errors
and, where appropriate, send in a user dump from the UTM application for
diagnosis.

## SEK3031

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3031 SESAM START PARAMETERS ARE NOT PERMITTED

### Meaning

SESAM start parameters (.SESAM ...) must not be specified in the start
procedure for the UTM application.
The parameters for the connection module must be set via the configuration
file of the UTM application.

### Response

Transfer the values of the SESAM start parameters to the configuration
file of the UTM application, remove the SESAM start parameters from the
start procedure and restart the UTM application.

## SEK3032

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3032 ERROR '(&00)/(&01)' IN START PARAMETERS

### Meaning

(&00): Status number
(&01): Status subnumber
In the start procedure of the utm application SESAM start parameters
(.SESAM ...) are incorrect.
More detailed information on this error is provided in status number and
status subnumber.
Refer to the section on 'CALL-DML messages' in the manual 'SESAM/SQL
Messages' for further details on the status number and status' subnumber.

### Response

Correct the SESAM start parameters and restart the application.

## SEK3035

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3035 USER CALL NOT A DML OR SQL STATEMENT

### Meaning

The error indicates a probable UTM or IUTMDB error.

### Response

Submit error documentation to diagnostics department.

## SEK3036

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3036 START PARAMETERS NOT PERMISSIBLE AFTER 'SYSTEM READY'

### Meaning

The error indicates a probable UTM or IUTMDB error.

### Response

Submit error documentation to diagnostics department.

## SEK3040

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3040 'DBCON' CALLED BY UTM WITH INVALID OPCODE

### Meaning

The SESAM connection module DBCON was called by UTM with an invalid opcode
(not defined at IUTMDB).

### Response

Forward error documentation for system diagnosis.

## SEK3041

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3041 'DBCOBN' CALLED BY UTM WITH INVALID OPCODE

### Meaning

The SESAM connection module DBCOBN was called by UTM with an invalid
opcode (not expected by SESAM).

### Response

Forward error documentation for system diagnosis.

## SEK3042

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3042 STACKING OF SESAM-UTM CONVERSATIONS NOT PERMISSIBLE WITH START PARAMETER 'UTMVG=NO'

### Response

If possible, use the start parameter UTMVG=JA, or continue without
stacking SESAM-UTM conversations.

## SEK3043

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3043 CONVERSATION EXIT NOT PERMISSIBLE WITH START PARAMETER 'UTMVG=YES'

### Response

Use the start parameter UTMVG=NO, or correct the program and start the
application again.

## SEK3048

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3048 SYSTEM ERROR BY SESAM DURING TRANSACTION JOB. PROGRAM TERMINATED WITH DUMP

### Response

Send the dump to the SESAM diagnosis.

## SEK3051

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3051 END TRANSACTION REQUEST BY UTM TO SESAM ILLEGAL. UTM APPLICATION ABORTED WITH DUMP

### Meaning

A request for termination of the CALL-DML transaction has been entered at
IUTMDB before an end transaction was performed. Probable error in the
application program and UTM.

### Response

The CALL-DML statement terminating the transaction must be entered before
the UTM transaction can be terminated. Modify the application program
accordingly. Submit dump(s) to SESAM diagnostics department.

## SEK3052

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3052 SYSTEM ERROR IN SQL RUNTIME SYSTEM

### Meaning

The SQL runtime system has detected a fatal internal error. A dump has
been generated for diagnostic purposes. As a result of this system error,
the UTM application has been aborted.

### Response

Submit error documentation to system diagnostics staff. Restart the UTM
application.

## SEK3053

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3053 SYSTEM ERROR IN 'DBCON' DURING FORMULATION OF SQL RESPONSE

### Meaning

'DBCON' detected a fatal internal error during the formulation of an SQL
response. A dump has been generated for diagnostic purposes. The UTM
application has been aborted as a result of this system error.

### Response

Submit error documentation to system diagnostics staff. Restart the UTM
application.

## SEK3054

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3054 INCONSISTENCY IN CONVERSATION- OR TRANSACTION-SPECIFIC MEMORY AREA TRANSFERRED TO 'DBCON' BY UTM.

### Meaning

'DBCON' has detected an inconsistency in the conversation-specific or
transaction-specific memory area. These memory areas are made available by
UTM. This indicates an interface error at the IUTMDB. A dump is generated
for diagnostic purposes.

### Response

Submit error documentation to system diagnostics staff. Restart the UTM
application.

## SEK3055

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3055 DMS ERROR (&00) WHEN OPENING SESDCN LOG FILE

### Meaning

A DMS error occurred when opening the SESDCN log file. For more
information on the DMS error code, use /HELP-MESS in system mode or refer
to the BS2000 'System Messages' manual.
(&00): DMS error code

### Response

Analyze the DMS error.

## SEK3056

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3056 INVALID LENGTH SUPPLIED BY UTM FOR TRANSACTION-SPECIFIC MEMORY AREA

### Meaning

The length specification for the transaction-specific memory area which is
transferred by UTM to SESAM/SQL is invalid. Presumably, this is a UTM
error. The UTM application is therefore terminated.

### Response

Submit diagnostic documentation (user dump and UTM dumps) to system
diagnostics. Start UTM application again.

## SEK3057

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3057 LENGTH OF TRANSACTION-SPECIFIC MEMORY AREA MODIFIED BY SESAM/SQL

### Meaning

SESAM/SQL has modified the transaction-specific memory area to be passed
by UTM to SESAM/SQL. This is not permitted. The UTM application is
therefore terminated.

### Response

Submit diagnostic documentation (user dump and UTM dumps) to system
diagnostics. Start UTM application again.

## SEK3070

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3070 INTERNAL REQUEST FOR RESETTING TRANSACTION FOR USER (&00) ON DBH SESAM(&01) ON PROCESSOR (&02) NOT POSSIBLE BEACAUSE OF RESOURCE BOTTLENECK

### Response

Reset the transaction specified in the message on the specified DBH using
the administration statement ROLLBACK-PTC-TRANSACTION or
ROLLBACK-TRANSACTION.

## SEK3071

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK3071 STATUS DELETE REQUEST FROM SESDCN FOR DBH SESAM(&00) ON PROCESSOR (&01) NOT POSSIBLE BEACAUSE OF RESOURCE BOTTLENECK

### Response

Reset those transactions on the DBH specified in the message, which
are in the state PTC and which were initiated on that processor and
in that configuration where this message was issued, using the
administration statement ROLLBACK-PTC-TRANSACTION.

## SEK4000

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4000 SESAM-SDF SYNTAX FILE IS NOT AVAILABLE

### Meaning

The SESAM-SDF syntax file specified in the 'SYNTAX-FILE' parameter
at the procedure call is not available.

### Response

Call procedure with correct value of the "SYNTAX-FILE" parameter.

## SEK4001

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4001 FOLLOW-UP PROCEDURE IS NOT AVAILABLE

### Meaning

The follow-up procedure specified in the "PROCEDURE-NAME" parameter at
the procedure call is not available.

### Response

Call procedure with correct value of the "PROCEDURE-NAME" parameter.

## SEK4002

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4002 THE 'CONNECT-SESAM-CONFIGURATION' COMMAND HAS BEEN SUCCESSFULLY DEFINED

## SEK4010

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4010 THE 'TO-FILE' PARAMETER WAS NOT SUPPLIED WITH A VALUE

### Meaning

The "TO-FILE" parameter was not supplied with a value when calling the
'CONNECT-SESAM-CONFIGURATION' command.

### Response

The name of the global configuration file must be specified in the
"TO-FILE" parameter.

## SEK4011

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4011 THE GLOBAL CONFIGURATION FILE IS NOT CATALOGED

### Meaning

When calling the 'CONNECT-SESAM-CONFIGURATION' command, the "TO-FILE"
parameter contained the name of a global configuration file that is not
cataloged.

### Response

Specify the name of an available global configuration file in the
"TO-FILE" parameter.

## SEK4012

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4012 THE 'CONFIGURATION-LINK' PARAMETER WAS NOT SUPPLIED WITH A VALUE

### Meaning

The "CONFIGURATION-LINK" parameter was not supplied with a value when
calling the 'CONNECT-SESAM-CONFIGURATION' command.

### Response

The "CONFIGURATION-LINK" parameter must contain the link name to be
searched for in the global configuration file.

## SEK4013

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4013 ERROR WHEN READING THE GLOBAL CONFIGURATION FILE

### Meaning

An error occurred when reading the global configuration file. More
detailed
information on this error is provided in preceding DMS and SDF-P messages.

### Response

Correct the error and call the "CONNECT-SESAM-CONFIGURATION" command
again.

## SEK4014

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4014 LINK NAME NOT UNIQUE

### Meaning

There are at least two occurrences of the link name being searched for in
the global configuration file.

### Response

A link name may occur once only in the global configuration file.
Rename one of the link names in the file and call the "CONNECT-SESAM-
CONFIGURATION" command again.

## SEK4015

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4015 ERROR WHEN WRITING THE LOCAL CONFIGURATION FILE

### Meaning

An error occurred when writing the local configuration file. More detailed
information on this error is provided in preceding DMS and SDF-P messages.

### Response

Correct the error and call the "CONNECT-SESAM-CONFIGURATION" command
again.

## SEK4016

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4016 SPECIFIED CONFIGURATION LINK NOT FOUND

### Meaning

The link name specified when calling the "CONNECT-SESAM-CONFIGURATION"
command was not found in the global configuration file.

### Response

Specify a link name that is present in the global configuration file, or
add the link name in the file.

## SEK4020

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4020 IN THIS VERSION THE START-LLM (&00) IS NOT SUPPORTED FOR SPARC64-HARDWARE.

### Meaning

The linked-in variant ist not available for SPARC64-architecture.

### Response

Use the independent variant instead.

## SEK4021

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4021 FILE (&00) IS NO LONGER AVAILABLE

### Meaning

A file was specified in the DEFAULT-PATH-NAME parameter for the
GET-INSTALLATION-PATH parameter but this file is no longer
available.
The function GET-INSTALLATION-PATH may have issued a message.

### Response

Make file accessible again.

## SEK4022

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4022 ERROR IN COMMAND (&00)

## SEK4023

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4023 INADEQUATE VERSION OF PRODUCT "(&00)" WITH IMON INSTALLED. INSTALLED PRODUCT VERSION = "(&01)", EXPECTED PRODUCT VERSION >= "(&02)"

### Meaning

SESAM cannot run with Version (&01) of product (&00) installed
with IMON.

### Response

Install the correct product version and restart the program.

## SEK4024

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4024 NO FREE LINK NAME BETWEEN BLSLIB00 AND BLSLIB99

### Meaning

When attempting to assign a file needed to load SESAM modules, no free
link name was found between the link names BLSLIB00 and BLSLIB99.

### Response

Release obsolete link assignments between BLSLIB00 and BLSLIB99
using the REMOVE-FILE-LINK command, and restart the program.

## SEK4025

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4025 THE FILE NEEDED BY SESAM TO LOAD SESAM MODULES CANNOT BE RELEASED USING THE "(&00)" COMMAND.

### Meaning

Before SESAM modules were loaded, a file with a link name between
BLSLIB00 and BLSLIB99 was assigned using the SET-FILE-LINK
command. An error occurred when releasing this link name.
It is possible that the file link has already been released.

### Response

If the link assignment to the file still exists, send a dump and trace
to Diagnostics.

## SEK4026

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4026 A LINK ASSIGNMENT ORIGINALLY SET BY THE APPLICATION PROGRAM CANNOT BE REESTABLISHED USING THE "(&00)" COMMAND.

### Meaning

Before SESAM modules were loaded, a link name between BLSLIB00 and
BLSLIB99, which was set by the application program, was changed. An error
occurred when reestablishing the original link assignment. It is possible
that the
file is no longer cataloged. Continued correct execution of the
application
program is not guaranteed.

### Response

Identify why the file needed by the application program can no longer
be accessed. If applicable, render the file accessible and restart the
program.

## SEK4027

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK4027 THE FILE NEEDED BY SESAM TO LOAD SESAM MODULES CANNOT BE ASSIGNED USING THE "(&00)" COMMAND

### Meaning

Before SESAM modules are loaded, a file with a link name between
BLSLIB00 and BLSLIB99 should be assigned. An error occurred when
assigning this file. It is possible that the file is not cataloged.

### Response

If necessary, use IMON to install the product to which the file belongs,
and render the file accessible.

## SEK4031

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SEK4031 IF THE CONNECTION MODULE "(&00)" IS AVAILABLE, THEN THE CONNECTION MODULE "(&01)" MUST NOT BE AVAILABLE

### Meaning

Only one connection module can be bound in an application.
Otherwise there is more than one entry with the same name.

### Response

Check the application, whether exactly one SESAM connection module
(SESLINK, SESMOD, SESDCAM, SESUTMC) is bound.
Correct the application and restart it.

## SEK4032

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SEK4032 THE CONNECTION MODULE "(&00)" IS NOT AVAILABLE

### Meaning

For a correct communication with SESAM it is necessary, that the
connection module (&00) is available.

### Response

Check, whether the SESAM connection module is bound correctly.
Correct the application and restart it.

## SEK4033

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SEK4033 THE CONNECTION MODULE "(&00)" IS MULTIPLE AVAILABLE

### Meaning

For a correct communication with SESAM it is necessary, that the
connection module (&00) is available only one time.

### Response

Check, whether the SESAM connection module is bound correctly.
Correct the application and restart it.

## SEK9102

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK9102 INSUFFICIENT USER ADDRESS SPACE AVAILABLE FOR THE DCN POOL

### Meaning

The DCN pool could not be opened. The DBH cannot process any requests from
application programs which make use of distribution.

### Response

Increase the user address space and restart the DBH.

## SEK9103

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK9103 INSUFFICIENT USER ADDRESS SPACE AVAILABLE FOR THE UTM POOL

### Meaning

The DBH could not open the UTM pool. No UTM requests can be processed in
the current session.

### Response

Increase the user address space and restart the DBH.

## SEK9105

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK9105 MEMORY POOL (SESTHB) NO LONGER AVAILABLE FOR UTM

### Meaning

When the first statement from the first UTM or DCAM application was
received by the DBH, the memory pool for SESAM application users was no
longer available, since the only task of the application has meanwhile
crashed.

## SEK9106

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK9106 MEMORY POOL (SESDCN) OF SESAM-DCN NO LONGER AVAILABLE

### Meaning

When the first statement of the first SESAM-DCN user (remote or local)
arrived, the memory pool of the SESAM-DCN was no longer available, as the
SESAM-DCN (and the user program, if running on the same installation)
crashed.

### Response

Start the SESAM-DCN and, if required, the user program again.

## SEK9107

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK9107 CONSISTENCY CHECK HAS OCCURRED IN SESAM DBH AND IN THE REQUESTING TASK '(&00)'

### Meaning

A consistency check has caused an application program to initiate a dump
for the DBH.

### Response

Submit the dumps for the application program and the DBH for SESAM
diagnosis.

## SEK9108

Destination: USER-TASK, CONSOLE Routing code: U Weight: 50

Warranty : NO

SEK9108 DMS ERROR '(&01)' WHEN OPENING DCN LOG FILE '(&00)'

### Meaning

The DCN log file (&00) cannot be opened. For more information on the DMS
error code use either /HELP-MSG in system mode or refer to the BS2000
'System Messages' manual. The SESAM DBH can continue operation but can
only process requests from local users without distribution.

### Response

Correct the DMS error and submit the request to the SESAM DBH again. The
DBH will again try to open the DCN log file.

## SEK9109

Destination: USER-TASK, CONSOLE Routing code: U Weight: 99

Warranty : NO

SEK9109 SESDCN LOGGING FILE '(&00)' CATALOGED UNDER MORE THAN ONE CAT ID; RENAME OR DELETE SUPERFLUOUS FILE(S)

### Meaning

The SESDCN logging file has been cataloged under more than one catalog
identification (CAT ID); it may not be cataloged under more than one.

### Response

Rename or delete superfluous SESDCN logging file.

## SEK9110

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK9110 ERROR WHEN CREATING THE DBH REQUEST COUNTER MEMORY POOL

### Meaning

The DBH could not create the memory pool for the communication request
counter; e.g. user address space is too small.

### Response

Increase the user address space in the Join entry of the user ID.

## SEK9111

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK9111 USER ADDRESS SPACE TOO SMALL

### Meaning

There is not enough memory available in the virtual address space.

### Response

Have the size of the virtual address space increased.

## SEK9112

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK9112 ERROR ON LINKING TO DBH-REQUESTCOUNTER-MEMORY-POOL

### Meaning

The DBH secondary task was unable to link to the existing memory pool
for the communication request counter because the DBH start task has
been terminated, for example.

## SEK9113

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK9113 DUMP INITIATED BY USER TASK ON MACHINE '(&00)' WITH USER ID '(&01)' AND TSN '(&02)'.

### Meaning

A dump is created on machine (&00) under user ID (&01) by the task
with TSN (&02). If * is specified as the TSN, the TSN of the user task
cannot be identified uniquely because it is a UTM or DCAM task of
a different SESAM configuration or on a different machine.

### Response

Send the dump of the DBH task and user task to Diagnostics.

## SEK9114

Destination: USER-TASK, CONSOLE Routing code: U Weight: 70

Warranty : NO

SEK9114 MEMORY-POOL OF SESAM-DCN IS INCONSISTENT.

### Meaning

A memory pool used by all tasks of this configuration is inconsistent.

### Response

Terminate all SESAM-DCN Tasks and all application programs of this
configuration.
Afterwards start SESAM-DCN and application programs again.

©2025 Fujitsu | BS2000 System Messages