## NDW0001

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0001 Error during initialization of PTAM slot-pools. Startup aborted

### Meaning

The initialization of the PTAM slot-pools failed.
Startup processing will be aborted.

### Response

Take SLED to get diagnose information.

## NDW0002

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0002 Error during intialization of PTAM CCW-chain generator. Startup aborted

### Meaning

During the initialization of the PTAM CCW-chain generator an error
occured.
Startup processing will be aborted.

### Response

Take SLED to get diagnose information.

## NDW0003

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0003 Error during initialization of PTAM contingency. Startup aborted

### Meaning

During the initialization of the PTAM contingency an error occured.
The Startup processing will be aborted.

### Response

Take SLED to get diagnose information.

## NDW0004

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0004 Error during initialization of PTAM bourse. Startup aborted

### Meaning

During the initialization of the PTAM bourse an error occured.
The Startup processing will be aborted.

### Response

Take SLED to get diagnose information.

## NDW0100

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0100 Device (&00): Device Type (&01) not supported

### Meaning

The Device Type (&01) is not supported by PTAM.
/ATTACH of Device (&00) is rejected.

### Response

Check the UGEN-cards of the I/O-configuration.

## NDW0101

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0101 Device (&00): SenseID (&01) supported

### Meaning

The SenseID (&01) of Device (&00) is supported by PTAM.

## NDW0102

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0102 Device (&00): SenseID (&01) not supported

### Meaning

The SenseID (&01) of Device (&00) is not supported by PTAM.
The verification of the I/O-configuration is not possible, but /ATTACH
is accepted.

## NDW0103

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0103 Device (&00): Read Device Characteristics command with SenseID (&01) failed

### Meaning

On Device (&00) the Read Device Characteristics I/O was terminated with an
error. /ATTACH of this device is rejected.

### Response

Check UGEN-cards for I/O-configuration.

## NDW0104

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0104 Device (&00): SenseID (&01) incompatible with Device Type (&02)

### Meaning

The SenseID (&01) of the Device (&00) is not compatible with the Device
Type (&02). /ATTACH is accepted.

### Response

Check UGEN-cards of I/O-configuration.

## NDW0105

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0105 Device (&00): Data Compression not supported for Device Type (&01) and SenseID (&02)

### Meaning

The Device (&00) does not support data compression, but for Device Type
(&01) this feature is mandatory. /ATTACH will be rejected.

### Response

Check UGEN-cards of I/O-configuration.

## NDW0106

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0106 Device (&00) unavailable

### Meaning

The device (&00) in a library is unavailable. /ATTACH will be rejected.

### Response

Check device state.

## NDW0107

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0107 NO KEY FOR ENCRYPTING/DECRYPTING DATA ON TAPE (&00)

### Meaning

No key got from MAREN for encrypting or decrypting of data
on tape (&00).

### Response

Contact MAREN administration.
Without key only unencrypted writing is possible.
Encrypted data blocks cannot be decrypted without key.

## NDW0199

Destination: USER-TASK, CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0199 (&00)

## NDW0201

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0201 PTAM detected data inconsistency in system memory

### Meaning

During /ATTACH of a device PTAM detected an inconsistency in system
memory. A snapshot dump has been taken.
Processing continues.

### Response

Call system administrator.

## NDW0202

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0202 System memory destroyed

### Meaning

System memory has been overwritten. The system is stopped via $CRASH.

### Response

Take SLED to get diagnose information.

## NDW0301

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0301 Device (&00): Tape position (&01) saved for VSN (&02), (&03) blocks buffered

### Meaning

Tape position and buffer were saved.

## NDW0302

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NDW0302 Device (&00): Saving of tape position failed for VSN (&01)

### Meaning

Saving of tape position and buffer failed.

©2025 Fujitsu | BS2000 System Messages