## DFP00CA

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP00CA INVALID VALUE FOR 'BLOCK' OPERAND

### Meaning

The value for the BLOCK operand in the FPAMACC operand list is outside the
permitted range of values.
Permitted: 1 to 2**23-1

### Response

Correct the program.

## DFP00CB

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP00CB INVALID OPERAND VALUE FOR 'WAITLST'

### Meaning

There is an illegal value in the WAITLST operand in the FPAMACC operand
list with the OPCODE 'WAIT'.
Possible reasons:
- the value does not represent the operand list address of an active
FPAMACC call started by the same task.
- the operand list address is not in the same ENVIRONMENT.
- the OPENID specified in WAIT is not identical to the OPENID in the
operand list specified by WAITLST.

### Response

Correct the program.

## DFP00CE

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP00CE INVALID OPERAND VALUE FOR 'LEN'

### Meaning

The LEN operand in the FPAMACC operand list contains a value which is
outside the permitted range of values.
Permitted: 1 to x: BLKSIZE (in 4K)
x=1 for MAXIOLN=*MINI
x=8 for MAXIOLN=*MAXI.

### Response

Correct the program.

## DFP00CF

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP00CF INVALID OPERAND VALUE FOR 'OPCODE'

### Meaning

The OPCODE operand in the FPAMACC operand list contains a value which
does not belong to the permitted range of values.
Permitted: 1 for READ
2 for WRITE
3 for READ WAIT
4 for WRITE WAIT
5 for READ EQUALIZE
6 for WAIT.

### Response

Correct the program.

## DFP00C8

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP00C8 INVALID OPERAND VALUE FOR 'OPENID'

### Meaning

Possible reasons:
- the OPENID operand in the FPAMACC operand list does not contain
an OPENID allocated by FASTPAM for this task (which has not
yet been returned by CLOSE).
- a non privileged task (TU) tries to access a file opened by a privileged
task (TPR).

### Response

Correct the program.

## DFP00C9

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP00C9 INVALID OPERAND VALUE FOR 'IOAREA'

### Meaning

The address range specified by the IOAREA operand together with the LEN
operand in the FPAMACC operand list
- is not completely in the IOAREA pool belonging to the OPENID or
- is not aligned for 4K or
- was released completely or partially (with a non resident IOAREA pool)
or
- the user does not have a write access privilege.

### Response

Correct the program.

## DFP000A

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP000A INVALID OPERAND VALUE FOR 'MAXIOLN'

### Meaning

The MAXIOLN operand in the FPAMSRV operand list contains a value which
does not belong to the permitted range of values.
Permitted: 1 for MAXIOLN=*MINI
8 for MAXIOLN=*MAXI
0 for MAXIOLN=*NOT_SPECIFIED (only at connection to
an existing ENVIRONMENT).

### Response

Correct the program.

## DFP000B

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP000B INVALID OPERAND VALUE FOR 'EVENTNG'

### Meaning

The EVENTNG operand in the FPAMSRV operand list contains a value which
does not belong to the permitted range of values.
Permitted: 1 for EVENTNG=*NO
2 for EVENTNG=*YES
0 for EVENTNG=*NOT_SPECIFIED (only at connection to
an existing ENVIRONMENT).

### Response

Correct the program.

## DFP000C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP000C ILLEGAl OPEN MODE

### Meaning

Possible reasons:
- the MODE operand in the FPAMSRV operand list contains a value which
is outside the permitted range of values.
Permitted: 1 for MODE=*INPUT
2 for MODE=*INOUT
3 for MODE=*OUTIN.
- open mode was set at an illegal value by a /SET-FILE-LINK command.

### Response

Correct the program.

## DFP000D

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP000D INVALID OPERAND VALUE FOR 'EIID'

### Meaning

Possible reasons:
- the EIID operand in the FPAMSRV operand list is not a currently
valid event item id for this task.
- EVENTNG=*YES was specified when trying to create an ENVIRONMENT
by an FPAMSRV call. However, the EIID operand was not specified.

### Response

Correct the program.

## DFP000E

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP000E INVALID BLOCKSIZE

### Meaning

Possible reasons:
- the BLKSIZE operand in the FPAMSRV operand list (*OPEN function)
contains
a value which is outside the permissible range of values.
Permitted: 1-8 for MAXIOLN=*MAXI
1 for MAXIOLN=*MINI.
- the logical block size was determined by a /SET-FILE-LINK command
and is not a multiple of 4K or is higher than the permissible
range of values.

### Response

Correct the program.

## DFP000F

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP000F INVALID OPERAND VALUE FOR 'ENVID'

### Meaning

Possible reasons:
- the ENVID operand in the FPAMSRV operand list (*OPEN or *DISENV
function) does not have an ENVIRONMENT code assigned by FASTPAM
for this task.
- the task has already been disconnected from the ENVIRONMENT.

### Response

Correct the program.

## DFP0001

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0001 INVALID OPERAND VALUE FOR 'ENVNAME'

### Meaning

The ENVNAME operand in the FPAMSRV operand list (*ENAENV function)
includes a value which is outside the permitted range of values.
Permitted: 1-54 characters from the character set
(A...Z,0...9,$,#,@), where the
1st character must be #,@ or a letter
($ is also permitted for users with privileged tasks).

### Response

Correct the program.

## DFP0002

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0002 INVALID OPERAND VALUE FOR 'IPONAME'

### Meaning

The IPONAME operand in the FPAMSRV operand list (*ENAIPO function)
includes a value which is outside the permitted range of values.
Permitted: 1-54 characters from the character set
(A...Z,0...9,$,#,@), where the
1st character must be #,@ or a letter
($ is also permitted for users with privileged tasks).

### Response

Correct the program.

## DFP0005

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0005 INVALID OPERAND VALUE FOR 'ACCLSTS'

### Meaning

The address range specified by the ACCLSTS operand together with ACCNUMB
in the FPAMSRV operand list (*ENAENV function)
- is not aligned at a 4K boundary or
- is not fully assigned or
- the user has no write access privilege or
- it is partially but not fully located in a memory pool or
- it belongs to the system address space (storage class 5 is only
permitted
for privileged tasks (TPR)).

### Response

Correct the program.

## DFP0006

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0006 INVALID OPERAND VALUE FOR 'ACCNUMB'

### Meaning

The operand for ACCNUMB in the FPAMSRV operand list (*ENAENV function)
includes a value which is outside the permitted range of values.
Permitted: 1-500 for users without the JOINFILE privilege
DMS-TUNING-RESOURCES=*EXCLUSIVE,
1-5000 with the JOINFILE privilege or
for users with privileged tasks (TPR).

### Response

Correct the program.

## DFP0007

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0007 INVALID OPERAND VALUE FOR 'IPOADDR'

### Meaning

The address range specified by the IPOADDR operand together with IPOSIZE
in the FPAMSRV operand list (*ENAIPO function)
- is not aligned at a 4K boundary or
- is not fully assigned or
- the user does not have a write access privilege or
- it is partially but not completely located in a memory pool or
- it belongs to the system address space (storage class 5 is only
permitted
for privileged tasks (TPR)).
- the ALET value specifying the DATA SPACE is not equal to zero but is
not a valid ALET.

### Response

Correct the program.

## DFP0008

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0008 INVALID OPERAND VALUE FOR 'IPOSIZE'

### Meaning

Possible reasons:
- the IPOSIZE operand in the operand list (*ENAIPO function)
includes a value which is outside the permitted range of values.
Permitted: 1 to 2**19.
- the IPOSIZE operand was not specified when an IOAREA pool was
created.

### Response

Correct the program.

## DFP0009

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0009 INVALID OPERAND VALUE FOR 'SHARUPD'

### Meaning

The SHARUPD operand in the FPAMSRV operand list (*OPEN function)
includes a value which is outside the permitted range of values.
Permitted: 1 for SHARUPD=*NO
2 for SHARUPD=*YES.

### Response

Correct the program.

## DFP0010

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0010 INVALID OPERAND VALUE FOR 'IPOID'

### Meaning

Possible reasons:
- the IPOID operand in the FPAMSRV operand list (*OPEN or *DISIPO
function) does not contain an IOAREA pool code assigned by FASTPAM for
this task.
- the task has already closed the connection to the IOAREA pool.

### Response

Correct the program.

## DFP0011

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0011 INVALID OPERAND VALUE FOR 'OPENID'

### Meaning

Possible reasons:
- the OPENID operand in the FPAMSRV operand list (*CLOSE function)
does not have an OPENID assigned by FASTPAM for this task.
- the task has already returned the OPENID via CLOSE.

### Response

Correct the program.

## DFP0012

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0012 INVALID OPERAND VALUE FOR 'RES'

### Meaning

The RES operand in the FPAMSRV operand list contains a value which is
outside the permitted range of values.
Permitted: 1 for RES=*NO
2 for RES=*YES
0 for *NOT-SPECIFIED (only if connected to an
existing ENVIRONMENT).

### Response

Correct the program.

## DFP0013

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0013 INVALID OPERAND VALUE FOR 'LASTBLK'

### Meaning

Possible reasons:
- the LASTBLK operand in the FPAMSRV operand list (*CLOSE function)
is negative or
- the logical block specified is not completely inside the file.
The file is consecutively numbered in units of the size BLKSIZE.
LASTBLK determines which unit should logically belong to the file.

### Response

Correct the program.

## DFP0028

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0028 INTERNAL SYSTEM ERROR DURING FASTPAM CALL

### Meaning

FASTPAM detected a system error during processing of a FPAMACC or FPAMSRV
macro.
The FASTPAM call is cancelled with the return code X'0028' and a
SERSLOG entry, record type DFP0028, is created.
In the case of serious errors, the program or task is cancelled with a
system dump and the termination code DFP0028 appears inserted in the
EXC0732 or EXC0736 message.

### Response

Contact the systems diagnostics staff.

## DFP0029

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0029 END OF THE FASTPAM IO CANNOT BE REPORTED

### Meaning

An IO initiated by an asynchronous FASTPAM call with P1-EVENTING
was terminated.
The user can no longer be informed of the job end since the signal bourse
has
been destroyed.
This may be caused by a preceding error in the program termination
during which a FASTPAM file was not properly closed.
Note:
'DFP0029' occurs only as a termination code , i.e. inserted in the
EXC0732 or EXC0736 message which indicates abnormal termination of the
user
program (in the case of non privileged tasks (TU)) or of the privileged
task.

### Response

If an error already in diagnosis did not occur in the program termination,
contact the systems diagnostics staff.

## DFP003B

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP003B DIFFERENT OPERAND VALUE FOR 'ACCLSTS'

### Meaning

The user wants a connection to an existing ENVIRONMENT with a different
operand value for ACCLSTS.

### Response

Correct the program.

## DFP003C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP003C DIFFERENT OPERAND VALUE FOR 'ACCNUMB'

### Meaning

The user wants a connection to an existing ENVIRONMENT with a different
operand value for ACCNUMB.

### Response

Correct the program.

## DFP003D

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP003D DIFFERENT OPERAND VALUE FOR 'IPOADDR'

### Meaning

The user wants a connection to an existing IOAREA pool with a different
operand value for IPOADDR.

### Response

Correct the program.

## DFP003E

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP003E DIFFERENT OPERAND VALUE FOR 'IPOSIZE'

### Meaning

The user wants a connection to an existing IOAREA pool with a different
operand value for IPOSIZE.

### Response

Correct the program.

## DFP003F

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP003F DIFFERENT OPERAND VALUE FOR 'MAXIOLN'

### Meaning

The user wants a connection to an existing ENVIRONMENT with a different
operand value for MAXIOLN.

### Response

Correct the program.

## DFP0032

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0032 NON RESIDENT MEMORY

### Meaning

A resident memory could not be used.
The user system can continue to operate for test purposes. However,
FASTPAM performance is affected adversely.
For the cause, see subreturncode2 (FPAMSR2 or SUBCODE2(SPL) field) in the
function head of the FPAMSRV operand list:
- subcode2=X'01', FASTPAM PRIVILEGE MISSING:
the user id of the task which created the ENVIRONMENT
or IOAREA pool does not have the FASTPAM privilege.
- subcode2=X'02', REAL MEMORY SHORTAGE:
- subcode2=X'03', USER LIMIT EXCEEDED:
the resident main memory allocation specified at the
start of the program has been exceeded.
- subcode2=X'04', EXISTING NOT RESIDENT:
connecting to a non resident ENVIRONMENT
or IOAREA pool.
- Subcode2=X'05', DATA SPACE ADDRESS:
only non resident DATA SPACES are supported in this
FASTPAM version.

### Response

subcode2=X'01': contact system administrator.
subcode2=X'02': contact system administrator.
subcode2=X'03': correct the program call; if the allocation for the USER
ID
is insufficient, contact the system administrator.
subcode2=X'04': correct the program.
subcode2=X'05': correct the program.

## DFP0033

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0033 DMS ERROR DURING OPEN/CLOSE

### Meaning

A DMS error code is returned in the FPAMDMSC field of the FPAMSRV
operand list.

### Response

Evaluate the DMS error code.

## DFP0035

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0035 IO RUNNING

### Meaning

An IO is running on the memory pages to be made resident while
the *ENAENV or *ENAIPO function is executed.
This return code only occurs during creation of the ENVIRONMENT or
IOAREA pool. IOs can run during connection.

### Response

Correct the program.

## DFP0036

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0036 ENVIRONMENT OR IOAREA CANNOT BE RELEASED SINCE FILES ARE OPEN

### Meaning

Files with the same ENVIRONMENT or IOAREA pool are still open while the
function *DISIPO or *DISENV is executing.

### Response

Correct the program.

## DFP0037

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0037 SHORTAGE OF RESOURCES

### Meaning

Possible reasons:
- shortage of address space
- shortage of main memory
- the address space allocated to the user is exhausted
- the user job has already assigned too many FPAMACC parameter lists.
The corresponding system work areas occupy more than 999 memory pools
of 1000K each.

### Response

Contact the system admimistrator or correct the program.

## DFP0038

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0038 ONLY TPR USERS CAN MAKE A CONNECTION

### Meaning

A TU user (non privileged task) issued a FPAMSRV job with the *ENAENV or
*ENAIPO function for an ENVIRONMENT or IOAREA pool which was created from
TPR (privileged task).

### Response

Correct the program.

## DFP0039

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0039 NO PRIVILEGE FOR CONNECTION

### Meaning

The user tries to connect with a resident FASTPAM ENVIRONMENT
or a resident IOAREA pool without the DMS-TUNING-RESOURCES=*EXCLUSIVE
privilege being included in his JOINFILE entry.

### Response

Correct the program.

## DFP004A

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP004A OVERLAPPING DIV RANGE

### Meaning

The specified user memory overlaps with a DIV window. The return
code X'004A' only apears if the ENVIRONMENT or IOAREA pool is to be
made resident.
DIV: Data in virtual memory

### Response

Correct the program.

## DFP004B

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP004B OVERLAPPING FASTPAM AREA

### Meaning

The specified user memory overlaps with a user memory area already
assigned as FASTPAM user memory.
The return code X'004B' only appears if the ENVIRONMENT or IOAREA pool
is to be made resident.

### Response

Correct the program.

## DFP004C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP004C MEMORY FOR FPAMACC PARAMETER LISTS NOT FULLY REQUESTED

### Response

Correct the program.

## DFP004D

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP004D FILE NOT A PAM FILE

### Meaning

The file to be opened is not in PAM format.

### Response

Correct the program.

## DFP004E

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP004E THE OPERAND 'LASTBLK' MAY NOT BE SPECIFIED

### Meaning

The LASTBLK operand was specified in the FPAMSRV call with the *CLOSE
function. This is ignored as the file was opened with MODE=*INPUT or
SHARUPD=*YES.
The file is closed normally.

### Response

Correct the program.

## DFP0040

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0040 DIFFERENT OPERAND VALUE FOR 'EVENTNG'

### Meaning

The user wants a connection to an existing ENVIRONMENT with a different
operand value for EVENTNG.

### Response

Correct the program.

## DFP0041

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0041 DIFFERENT OPERAND VALUE FOR 'EIID'

### Meaning

The user wants a connection to an existing ENVIRONMENT but the operand
value specified here for EIID in the FPAMSRV macro does not specify the
same event item as the EIID specified during its creation.

### Response

Correct the program.

## DFP0042

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0042 OPERAND VALUE FOR 'BLKSIZE' DOES NOT MATCH THE CATALOG ENTRY

### Meaning

The logical block size specified by BLKSIZE with FASTPAM OPEN (in 4K
units)
does not match the catalog entry.

### Response

Correct the program.

## DFP0046

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0046 NO EVENT ITEM CONNECTION

### Meaning

The user wants to make a connection to an existing FASTPAM ENVIRONMENT
with FPAMSRV. However, he is not connected to the appropriate event item.

### Response

Correct the program.

## DFP0047

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0047 EVENT ITEM SCOPE TOO SMALL

### Meaning

The event item specified with the FPAMSRV call (*ENAENV function) by the
EIID operand has a smaller scope than the memory pool which contains
the FPAMACC parameter lists.

### Response

Correct the program.

## DFP0048

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0048 ENVIRONMENT NAME EXISTING

### Meaning

The task is already connected to the ENVIRONMENT.

### Response

Correct the program.

## DFP0049

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0049 IOAREA POOL NAME EXISTING

### Meaning

The task is already connected to the IOAREA pool.

### Response

Correct the program.

## DFP005A

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP005A 'WRCHK' NOT SUPPORTED. NO FASTPAM OPEN PERFORMED

### Meaning

The WRITE-CHECK=YES entry in the /SET-FILE-LINK command is not supported
by
FASTPAM.

### Response

Correct the program.

## DFP005B

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP005B USER AREA IS IN A MEMORY POOL WITHOUT 'FIXED' ATTRIBUTE

### Meaning

If the FPAMACC parameter lists or the FASTPAM IOAREA is in a memory pool,
FASTPAM requires that the FIXED=YES parameter be specified when the memory
pool is created. Since this was not the case, the FPAMSRV call (*ENAENV
or *ENAIPO function) was rejected.

### Response

Correct the program.

## DFP0050

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0050 RFA NOT SUPPORTED. NO FASTPAM OPEN PERFORMED

### Meaning

RFA: remote file access.

### Response

Correct the program.

## DFP0051

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0051 SPD NOT SUPPORTED. NO FASTPAM OPEN PERFORMED

### Meaning

SPD: shared private disk

### Response

Correct the program.

## DFP0052

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0052 PPD NOT SUPPORTED. NO FASTPAM OPEN PERFORMED

### Meaning

PPD: protected private disk

### Response

Correct the program.

## DFP0053

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0053 TAPE NOT SUPPORTED. NO FASTPAM OPEN PERFORMED

### Response

Correct the program.

## DFP0054

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0054 DUMMY FILE NOT SUPPORTED. NO FASTPAM OPEN PERFORMED

### Response

Correct the program.

## DFP0055

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0055 SECONDARY ALLOCATION TOO SMALL. NO FASTPAM OPEN PERFORMED

### Meaning

The memory space to be occupied by the secondary allocation is
insufficient to take up a logical block.

### Response

Correct the program.

## DFP0056

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0056 'ENVID' OR 'IPOID' OPERAND ONLY PERMITTED FOR TPR USERS

### Meaning

An FPAMSRV call issued from TU (non privileged task) with the
*OPEN or *DISENV or *DISIPO function refers to a FASTPAM ENVIRONMENT or a
FASTPAM IOAREA pool which was created from TPR (privileged task).

### Response

Correct the program.

## DFP0057

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0057 IOAREA POOL NOT ALLOCATED

### Response

Correct the program.

## DFP0058

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0058 'BLKCTRL' NOT SUPPORTED. NO FASTPAM OPEN PERFORMED

### Meaning

FASTPAM only supports files with the BLKCTRL=NO attribute.

### Response

Correct the program.

## DFP0059

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0059 TPR OPEN ID. NO FASTPAM OPEN PERFORMED

### Meaning

Only TPR users may use the open ID, which is specified as the operand
value for OPENID.
TPR: privileged task.

### Response

Correct the program.

## DFP012C

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP012C IO ERROR DURING FASTPAM FILE ACCESS

### Meaning

Hardware error during FASTPAM file access.

### Response

Contact system administrator.

## DFP012D

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP012D PATH ACTIVE. FPAMACC CALL REJECTED

### Meaning

The system work area belonging to the FPAMACC operand list is still
occupied by an IO that was started by the same FPAMACC operand list.

### Response

Correct the program.

## DFP012E

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP012E PATH NOT ACTIVE (WAIT ONLY)

### Meaning

The WAITLST operand in the FPAMACC operand list indicates a FPAMACC
operand list with which an IO was not started.
Possible reasons for return code X'012E':
- faulty programming.
- WAITLST designates an asynchronous IO job which can be terminated
synchronously.

### Response

If synchronous termination has not occurred, correct the program.

## DFP012F

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP012F CHAIN ERROR

### Meaning

The FPAMACC job was not executed because an error occurred in one of the
jobs chained to it.

### Response

Search for the error in the chain.

## DFP0133

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0133 ILLEGAL WAIT OPERATION FOR AN IO WITH P1 EVENTING

### Meaning

An FPAMACC call with the 'WAIT' OPCODE was issued, but EVENTNG=*YES was
specified when the file was being opened.
In principle, WAIT calls are not allowed for files which are processed
with P1 EVENTING.

### Response

Correct the program.

## DFP0134

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0134 WAIT NOT BY SAME TASK

### Response

Correct the program.

## DFP014A

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP014A FILE CANNOT BE EXTENDED. POSSIBLE REASON: INTERVENTION BY SYSTEM ADMINISTRATOR

### Meaning

It is not possible to make a secondary allocation since the class 4
extent list is missing.
This is an indication that the system administratror has issued a
/REPAIR-DISK-FILES or /REMOVE-FILE-ALLOCATION-LOCKS command
for the file which has just been opened.
If this is not the case, there must be a system error.

### Response

Contact the system administrator.

## DFP0140

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0140 END OF FILE. FPAMACC CALL REJECTED

### Meaning

There is an IO after the end of the file.
In the case of return code X'0140', the IO is not carried out.
In contrast to UPAM, the pages which still belong to the file are not
necessarily processed.

### Response

Correct the program.

## DFP0141

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0141 NO DISC SPACE AVAILABLE

### Meaning

During secondary allocation, no more disk space could be allocated.

### Response

Contact the system administrator.

## DFP0142

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0142 USER ID EXHAUSTED

### Meaning

The memory allocated for the user id is exhausted. The FPAMACC call must
be
rejected as it would extend the file and hence lead to a new memory
allocation.

### Response

Delete files or contact the system administrator.

## DFP0143

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0143 PUBLIC VOLUME NOT ATTACHED

### Meaning

The file must be extended in order to proces the FPAMACC call. However,
the
appropriate allocator call passed the return code X'0445'. This means
that
the required public volume is not attached.

### Response

Contact the system administrator.

## DFP0144

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP0144 CATALOG ENTRY FOR SPECIFIED FILE HAS REACHED MAXIMUM SIZE, REQUEST POSSIBLY NOT COMPLETELY SATISFIED. REORGANIZE FILE BY COPYING AND RETRY ACTION.

### Meaning

Catalog entry of specified file has maximum number of extents an cannot
be increased.

### Response

Reorganize specified file by copying and retry action.

## DFP022F

Destination: USER-TASK Routing code: Weight: 99

Warranty : NO

DFP022F FPAMACC PARAMETER LIST NOT ACCESSIBLE. IO END MESSAGE NOT POSSIBLE

### Meaning

Possible reasons:
- this user error can only occur with a non resident FASTPAM-ENVIRONMENT.
An IO triggered by an asynchronous FASTPAM job with P1-EVENTING was
terminated. However, the user parameter list cannot be provided with the
return information.
Reason: The storage area is released or write-protected.
- for users of privileged tasks, the termination code 'DFP022F' can also
mean that the FPAMSRV or FPAMACC parameter list cannot be accessed at
the start of job processing.
'DFP022F' appears only as a termination code within the
EXC0732 or EXC0736 message with which abnormal termination of the user
program (in the case of non privileged tasks) or the privileged task is
indicated.

### Response

Correct the program.

©2025 Fujitsu | BS2000 System Messages