## NKVCOPY

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NKVCOPY Copyright (C) (&01) (&00). All rights reserved

## NKVD002

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD002 DISK MONITOR NOT AVAILABLE

## NKVD003

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD003 NKA-SYSTEMTASK NOT AVAILABLE

## NKVD010

Destination: CONSOLE Routing code: D Weight: 30

Warranty : NO

NKVD010 DISK '(&00)' MOUNTED ON DEVICE '(&01)'

## NKVD011

Destination: CONSOLE Routing code: D Weight: 30

Warranty : NO

NKVD011 DISK '(&00)' DISMOUNTED FROM DEVICE '(&01)'

## NKVD013

Destination: CONSOLE Routing code: D Weight: 90

Warranty : NO

NKVD013 MOUNT DISK '(&00)' ON DEVICE '(&01)'; (&02) (USE='(&03)',SYS-ALLOC='(&04)', (&05)). '(&06)'

### Meaning

Request to mount the disk and switch on the device.
If required by the message, the operator has to confirm that (s)he is
ready
to mount the disk.
(&00) : volume serial number (VSN) of the disk, if specified by the user
(&01) : mnemonic of device proposed by the system
(&02) : reason for displaying the message, if the disk is
already mounted but cannot be assigned by the
operator
(&03) : usage mode (USE = DMS / SPECIAL)
(&04) : current SYSTEM-ALLOCATION (ALL / SHARE / EXCL)
(&05) : supplementary text, describing the application
(&06) : description of the operator reply.

### Response

ETX: the requested volume is mounted on the device proposed by the system
N : the requested volume is not available
MN : the requested volume is mounted on the device <MN>.
Mount the specified disk and switch on the device. Reply to the message,
if required.
No reply is required, if the system recognizes that the disk is mounted
and confirms this by displaying message NKVD017.
The system recognizes the mounting automatically only if the disk has a
standard label and if a VSN was specified by the user.

## NKVD014

Destination: CONSOLE Routing code: D Weight: 90

Warranty : NO

NKVD014 REMOUNT DISK '(&00)' ON DEVICE '(&01)'; (&02) (SYS-ALLOC='(&03)'). '(&04)'

### Meaning

Request to remount the specified disk, switch on the device and confirm
the mounting by entering a reply.
The operator has either to confirm that (s)he is ready to remount the
specified disk or to terminate processing of the disk by rejecting the
message.
(&00): volume serial number (VSN) of the disk, if specified by the user
(&01): mnemonic of the device proposed by the system
(&02): reason for displaying the REMOUNT message
(&03): current SYSTEM-ALLOCATION
(&04): description of the operator reply.

### Response

Note: Not all answers described here are always allowed.
Refer to insert (&04) to see the currently allowed answers.
ETX = YES: the requested volume is mounted on the device proposed by
the system
N = NO : the requested disk is not available to the requesting task.
Processing of the disk is terminated
MN : the requested disk is mounted on the device <MN>
T : remount processing is to be terminated. The current I/O for
the task displaying the message will be terminated with
error.
*TA : Processing is to be continued on the second disc containing
the mirrored data. The concerned device is determined and
checked by SHC-OSD.
No reply is required, if the system recognizes that the disk is mounted
and confirms this by displaying message NKVD018.
The system recognizes the mounting automatically only if the disk has a
standard label and if a VSN was specified by the user.

## NKVD015

Destination: CONSOLE Routing code: D Weight: 50

Warranty : NO

NKVD015 DISK VSN '(&00)' IS NOT UNIQUE IN THE SYSTEM

### Meaning

Either more than one disk with the specified VSN is online, or it has
been requested more than once. No automatic allocation can be performed
for this VSN.

## NKVD017

Destination: CONSOLE Routing code: D Weight: 50

Warranty : NO

NKVD017 MOUNTING OF DISK '(&00)' ON DEVICE '(&01)' FOR TASK '(&02)' COMPLETED

### Meaning

The mounting of a disk requested by message NKVD013 has been recognized
by the system. No further activities by the operator are required for this
disk. If the disk was mounted without a reply to NKVD013, it is assumed
that a reply is no longer required or possible, as an implicit reply has
been given by the system.

## NKVD018

Destination: CONSOLE Routing code: D Weight: 50

Warranty : NO

NKVD018 REMOUNTING OF DISK '(&00)' ON DEVICE '(&01)' FOR TASK '(&02)' COMPLETED

### Meaning

The remounting of a disk requested by message NKVD014 has been recognized.
by the system. No further activities by the operator are required for this
disk. If the disk was mounted without a reply to NKVD014, it is assumed
that a reply is no longer required or possible, as an implicit reply has
been given by the system.

## NKVD019

Destination: CONSOLE Routing code: D Weight: 30

Warranty : NO

NKVD019 DISK '(&00)' ON DEVICE '(&01)' NOT EXCLUSIVELY AVAILABLE TO HOME SYSTEM. ASSIGNED SYSTEMS: '(&02)'; SVL-ALLOC: '(&03)'

### Meaning

The specified disk is already allocated by (a) foreign system(s),
preventing exclusive use by the user's own system. If this allocation is
not correct (abnormal system termination), a reset of the MRS-protocol
is possible by means of /UNLOCK-DISK.
(&00) : volume serial number (VSN) of the disk concerned
(&01) : mnemonic of device on which the disk is mounted
(&02) : SYS IDs of the sharing systems
(&03) : mode of allocation: SHARE (SPD mode) or EXCLUSIVE
(exclusive allocation for one system only).

## NKVD020

Destination: CONSOLE Routing code: D Weight: 30

Warranty : NO

NKVD020 SRV-ALLOCATION-REQUEST FOR DRV-DISK '(&00)' ON DEVICE '(&01)'

### Meaning

It is required to allocate a disk in single-recording-mode, which
was previously used in dual-recording-mode. In the following
mount-request the allocation has to be confirmed or rejected.

## NKVD021

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD021 REMOUNT FOR DISK '(&00)' ON DEVICE '(&01)' FAILED. ACCESS RIGHT FOR DISK NOW WITHDRAWN (CANCELLED)

### Meaning

As an unrecoverable error occurred during remount, the access right for
the user has been withdrawn. No further I/O operations for the disk are
permitted. The device is now free for the mounting of other disks. If the
disk is allocated in the usage mode DMS, the disk operands ASSIGN-TIME
and USER-ALLOCATION have been changed implicitly by the system. The disk
can be made available by the system only after it has been released by all
the users.

## NKVD022

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD022 DISK '(&00)' ON DEVICE '(&01)' CANCELLED BY OPERATOR

### Meaning

Confirmation that the disk has been cancelled as requested by the operator
in the command /CHANGE-DISK-MOUNT. No further I/O operations for the disk
are permitted. The device is now free for the mounting of other disks
if it is no fixed device.

## NKVD023

Destination: CONSOLE Routing code: D Weight: 30

Warranty : NO

NKVD023 ALLOCATION-REQUEST FOR INCONSISTENT OR NOT UP-TO-DATE DUALCOPY DISK '(&00)' ON DEVICE '(&01)'. NO AUTOMATIC ALLOCATION

### Meaning

An allocation of a disk, which was previously used in dualcopy-mode, is
required. This disk is inconsistent or not up-to-date (the copy-process
has been aborted).
In the subsequent mount-message the allocation can be confirmed or
rejected. If confirmed, the inconsistency-flag is reset.

## NKVD024

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD024 DISK MOUNTED ON DEVICE '(&00)' NOT INITIALIZED. DISK CAN ONLY BE PROCESSED IN CONJUNCTION WITH USE=SPECIAL

### Meaning

A disk that is not initialized can only be processed in the usage mode
USE=SPECIAL (cf. message NKVD013).

## NKVD026

Destination: CONSOLE Routing code: D Weight: 30

Warranty : NO

NKVD026 DEVICE DEFECTIVE. REMOUNT DISK '(&00)' ON DEVICE '(&01)'

### Meaning

The disk must be remounted. Processing of the disk is interrupted.
The disk will be requested again with message NKVD014.

## NKVD027

Destination: CONSOLE Routing code: D Weight: 50

Warranty : NO

NKVD027 Assignment of GS-Volume '(&00)' on device '(&01)' for DRV is not allowed

## NKVD028

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD028 NO ADDITIONAL SUBTASK POSSIBLE

### Meaning

The maximum number of temporary auxiliary tasks is reached, or no task
creation is possible due to resource bottleneck. The request can be
processed only after another auxiliary task terminated its request or
after the bottleneck has been removed.

## NKVD029

Destination: CONSOLE Routing code: D Weight: 50

Warranty : NO

NKVD029 DISK '(&00)' ON DEVICE '(&01)' IS INCONSISTENT. ALLOCATION NOT PERMITTED

### Meaning

The disk contains inconsistent data. Allocation in
single recording mode for USE=DMS is not permitted.
Such an inconsistent disk can be produced for instance
by a premature break of a previous VOLIN-Job for the
concerned disk.

## NKVD030

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD030 DISK '(&00)' ON DEVICE '(&01)' WAS CANCELLED BY SYSTEM (&02)

### Meaning

The disk cannot be made available to the user any more.
Possible reasons for this situation may be :
1. While reading the disk the system has recognized
an inconsistency in the standard volume label (SVL)
of the concerned disk. This may be caused by an
erroneous use of the command /UNLOCK-DISK by a
foreign system which has destroyed the allocation-
information of the own system in the SVL of the
disk.
2. If the operator removes a device of a fixed disk
with command /DETACH ...,FORCE=YES the disk will
also be cancelled by system because it is no more
possible to remount the disk on an alternate device.
The cancel of the allocated disk by the system causes
that no further I/O operations for the disk are permitted.

## NKVD031

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD031 REMOUNT OF DISK '(&00)' ON DEVICE '(&01)' COMPLETED

### Meaning

The remount-recover for disk (&00) which has been initiated
by system or by command /CHANGE-DISK-MOUNT has been
terminated successfully. The disk is available again for
a further processing by the user.
If the operator mounted the disk without a reply of the
message NKVD014 this message will give a hint to the
operator that a reply of this message is no longer
required or possible because the reply has been given
by the system itself.

## NKVD035

Destination: CONSOLE Routing code: D Weight: 30

Warranty : NO

NKVD035 DISK '(&00)' ON DEVICE '(&01)' CANNOT BE ALLOCATED WITH RECORDING MODE SRV. ASSIGNED SYSTEMS: '(&02)'

### Meaning

The specified disk is already allocated by (a) foreign system(s) with
recording mode DRV. If this allocation is not correct (abnormal system
termination), a reset of the MRS-protocol is possible by means of
/UNLOCK-DISK.
(&00) : volume serial number (VSN) of the disk concerned
(&01) : mnemonic of device on which the disk is mounted
(&02) : SYS IDs of the sharing systems

## NKVD036

Destination: CONSOLE Routing code: D Weight: 30

Warranty : NO

NKVD036 DISK IDENTITY CHANGED ON DEVICE '(&00)' FROM '(&01) (&02)' TO '(&03) (&04)'

### Meaning

The disk monitor recognized that the identity of the disk (label type and
VSN, if standard format) has been changed by the user.

## NKVD038

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD038 DISK MOUNTED ON DEVIVE '(&00)' HAS NO STANDARD-VOLUME-LABEL. UNLOCK-REQUEST FOR DISK REJECTED

### Meaning

Command /UNLOCK-DISK is allowed only for disks with
a BS2000-standard-volume-label (SVL). As disk which is
mounted on device (&00) has no SVL, command
/UNLOCK-DISK has been rejected.

## NKVD039

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD039 UNLOCK FOR DISK '(&00)' ON DEVICE '(&01)' REJECTED FOR SYSTEM IDENTIFIER '(&02)' AS DISK IS IN USE AND SYSTEM IDENTIFIER DENOTES OWN SYSTEM

## NKVD040

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD040 DISK MONITOR TERMINATED. RESTART NOT POSSIBLE. SHUTDOWN INITIATED

### Meaning

Disk processing is no longer possible.

## NKVD041

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD041 SPECIFIED DISK-DEVICE '(&00)' NOT DEFINED. COMMAND REJECTED FOR THIS DEVICE

## NKVD042

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD042 SPECIFIED DISK '(&00)' UNKNOWN. COMMAND REJECTED FOR THIS DISK

## NKVD043

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD043 SPECIFIED VSN '(&00)' OF DISK IS NOT UNIQUE. COMMAND NOT PROCESSED FOR THIS DISK

### Meaning

As the VSN is not unique, the mnemonic of the device assigned to the disk
has to be specified.

## NKVD045

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD045 DISK '(&00)' ON DEVICE '(&01)' IS A FIXED DISK. MOVE AND EXCHANGE NOT POSSIBLE. COMMAND NOT PROCESSED FOR THIS DISK

## NKVD046

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD046 NO ALTERNATIVE DEVICE AVAILABLE FOR DISK '(&00)' ON DEVICE '(&01)'. COMMAND NOT PROCESSED FOR THIS DISK

## NKVD047

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD047 QUIET FOR DMS LOCK HANDLING FOR DISK '(&00)' ON DEVICE '(&01)' FAILED. COMMAND NOT PROCESSED FOR THIS DISK

### Meaning

Before this command is processed, the release of the disk's
VTOC-LOCK by the own system has to be ensured. The lock can
only be reset while the disk is mounted. See also the information
displayed by means of command /SHOW-DISK-STATUS with regard
to VTOC-TSN and VTOC-SYSTEM.

## NKVD048

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD048 DEVICE REMOVED FOR DISK '(&00)' ON DEVICE '(&01)'. DISK WAITING FOR AVAILABLE DEVICE

### Meaning

The device of the disk has been removed. The disk is now waiting for an
alternative device (action state NO-DEVICE in output of the command
/SHOW-DISK-STATUS).
Upon the release of a suitable device message NKVD049 documents the wait
state to have ended. Remount of the disk is requested by NKVD014.
With the aid of the EXCHANGE function in the /CHANGE-DISK-MOUNT command
the operator can transfer the wait state to another disk thus obtaining an
appropriate device. The waiting for a device can be ended
with the aid of the CANCEL function in the /CHANGE-DISK-MOUNT command.
Consequently the disk
is no longer available to the user, thus terminating his/her processing.

## NKVD049

Destination: CONSOLE Routing code: D Weight: 50

Warranty : NO

NKVD049 WAITING OF DISK '(&00)' FOR ALTERNATIVE DEVICE ENDED

### Meaning

The waiting of the disk for an alternative device, initiated by message
NKVD048, has ended.

## NKVD050

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD050 NEW OPERAND FOR DISK MONITOR: '(&00) = (&01)'

### Meaning

New value of disk monitoring. The setting of the DISK-MOUNT operand in
the /MODIFY-MOUNT-PARAMETER command is protocoled.

## NKVD051

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD051 UNLOCK REQUEST FOR DISK '(&00)' ON DEVICE '(&01)' WITH SHARING SYSTEMS '(&02)' REJECTED FOR SPECIFIED SYSTEM '(&03)'

### Meaning

UNLOCK function in /UNLOCK-DISK command was incorrect.

## NKVD052

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD052 UNLOCK REQUEST FOR DISK '(&00)' ON DEVICE '(&01)' FOR SYSTEM '(&02)' COMPLETED

## NKVD053

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD053 REMOUNTING OF DISK '(&00)' ON DEVICE '(&01)' NOT PERMITTED BECAUSE THE ACTUAL DEVICE WAS REQUESTED BY THE USER WITH DEVICE-MNEMONIK. COMMAND NOT PROCESSED FOR THIS DISK

### Meaning

Disk (&00) was allocated by the user in conjunction
with a specification of a device-mnemonik. Therefore,
disk (&00) is fix assigned to the device on which
the disk has been mounted until now. A remountig
of the disk on the alternative device (&01) as
requested with the 'MOVE'- or the 'EXCHANGE'-function
is not allowed.
If the device on which the disk has been mounted until
now is defective either the device has to be repaired by
a hardware-technician or the disk has to be cancelled
by the operator .

## NKVD054

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD054 SPECIFIED ACTION FOR DISK '(&00)' ON DEVICE '(&01)' NOT PERMITTED. COMMAND NOT PROCESSED FOR THIS DISK

### Meaning

The command has not been processed, as the requested function
in the command /CHANGE-DISK-MOUNT is not possible because of the
current state of the disk.
For more detailed information on the current state enter the command
/SHOW-DISK-STATUS.

## NKVD055

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD055 SPECIFIED ACTION FOR DISK '(&00)' ON DEVICE '(&01)' NOT PERMITTED. COMMAND NOT PROCESSED FOR THIS DISK

### Meaning

The command is not permitted as the disk is used in the
HOME-PUBSET or in a PAGING-PUBSET.

## NKVD056

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NKVD056 NO DISK ASSIGNED TO SPECIFIED DEVICE '(&00)'. COMMAND NOT PROCESSED FOR THIS DEVICE

### Meaning

A disk can only be specified by a device-mnemonik if the
disk is assigned to this device.

## NKVD057

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD057 UNLOCK FOR DISK '(&00)' ON DEVICE '(&01)' FOR SYSTEM '(&02)' FAILED (&03)

### Meaning

(&03) specifies the detailed reason if necessary.

## NKVD058

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD058 SYNTAX ERROR IN MESSAGE REPLY. REPLY FOR TASK '(&00)' REJECTED

## NKVD059

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD059 CANCEL FOR PUBLIC DISK NOT PERMITTED. REPLY FOR TASK '(&00)' REJECTED

### Meaning

Use of a public disk cannot be terminated nor can the device of a
public disk be withdrawn.

## NKVD060

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD060 SPECIFIED DISK DEVICE '(&00)' NOT DEFINED. REPLY FOR TASK '(&01)' REJECTED

### Meaning

The specified device is not defined. The reply to message NKVD012, NKVD013
or NKVD014 is rejected, the message is displayed again.

## NKVD061

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD061 USE OF DEVICE '(&00)' NOT POSSIBLE DUE TO WRONG DEVICE-TYPE. REPLY FOR TASK '(&01)' REJECTED

### Meaning

The specified device cannot be used due to its type. The reply to message
NKVD013 or NKVD014 is rejected, the message displayed again.

## NKVD062

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD062 SPECIFIED DEVICE '(&00)' NOT AVAILABLE DUE TO ITS CONFIGURATION-STATE. REPLY FOR TASK '(&01)' REJECTED

### Meaning

The specified device is due to it's configuration-state
(for example DETACHED, DETACH-PENDING, ATTACH-PENDING)
not available for mounting of a disk.
The reply to message NKVD013 or NKVD014
is rejected, the message is displayed again.

### Response

Check the configuration state by means of one of the commands
/SHOW-DEVICE-STATUS or /SHOW-DEVICE-CONFIGURATION.

## NKVD063

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD063 SPECIFIED DEVICE '(&00)' IS ALREADY ASSIGNED TO A DISK. REPLY FOR TASK '(&01)' REJECTED

### Meaning

The specified device is not available. The reply to message NKVD013 or
NKVD014 is rejected, the message is displayed again.

### Response

Check whether the device is assigned to another disk by means of the
/SHOW-DISK-STATUS command.

## NKVD064

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD064 ALL DEVICES OF SAME TYPE AS DEVICE '(&00)' ARE SECURED. REPLY FOR TASK '(&01)' REJECTED

### Meaning

The device is currently not available due to type-reservations
by other tasks. See also the output of command
/SHOW-DEVICE-STATUS ...,INFORMATION=SUMMARY.
The reply to NKVD013 or NKVD014 is rejected, the message is
displayed again.

## NKVD065

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD065 DISK '(&00)' CAN ONLY BE ASSIGNED ON DEVICE '(&01)' (REQUEST BY MEANS OF DEVICE-MNEMONIK). REPLY FOR TASK '(&02)' REJECTED

### Meaning

No assignment to an alternative device is permitted by the user. The reply
to NKVD013 or NKVD014 is rejected, the message is displayed again.

## NKVD066

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD066 SPECIFIED DEVICE '(&00)' CURRENTLY RESERVED FOR AN APPLICATION BY DEVICE-MNEMONIK. REPLY FOR TASK '(&01)' REJECTED

### Meaning

The device specified in the reply is reserved for another application
with device-mnemonik (cf. /SHOW-DEVICE-STATUS UNIT=... ).
The disk will be requested again in message NKVD013 or NKVD014 on
the device proposed by the system.

## NKVD069

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD069 DEVICE ASSIGNMENT CANNOT BE MODIFIED FOR DISK '(&00)' ON DEVICE '(&01)'. REPLY FOR TASK '(&02)' REJECTED

### Meaning

A disk is allocated on the device specified in the reply. The device
allocation of this disk cannot be modified. The reply is rejected, the
message is displayed again.

## NKVD070

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD070 DISK '(&00)' ON DEVICE '(&01)' USED FOR PAGING. COMMAND '(&02)' NOT PROCESSED FOR THIS DISK DUE TO NON-RESIDENT DISK MONITOR

### Meaning

The MOVE function of the command /CHANGE-DISK-MOUNT is only supported with
regard to paging disks, if the code of the DISK-MONITOR was generated in
the resident memory.

## NKVD071

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD071 REMOUNT ON ANOTHER DEVICE NOT PERMITTED DUE TO NON-RESIDENT DM. REPLY FOR TASK '(&00)' REJECTED

### Meaning

The disk must be made available again on the device proposed by the
system.
No MOVE of PAGING-disks is possible, if the code of the DISK-MONITOR is
not
generated in the resident memory.

## NKVD072

Destination: CONSOLE Routing code: D Weight: 90

Warranty : NO

NKVD072 UNLOCK FOR DISK '(&00)' ON DEVICE '(&01)' FOR SYSTEMS '(&02)' ONLY IF THE SYSTEMS ARE TERMINATED (ABNORMALLY). REPLY (<VSN>=CONTINUE; NO=ABORT UNLOCK)

### Meaning

Other systems (cf. /SHOW-DISK-STATUS,INF=SYSTEM) can only be reset, if
they
do not use the disk; i.e. they have terminated (abnormally) or the disk is
in the state CANCELLED.

## NKVD073

Destination: CONSOLE Routing code: D Weight: 30

Warranty : NO

NKVD073 DISK '(&00)' CANNOT BE ASSIGNED TO DEVICE '(&01)'. DEVICE ALREADY RESERVED FOR AN APPLICATION BY DEVICE-MNEMONIK

### Meaning

The disk is mounted on a device reserved for another
application by means of device-mnemonik and could
therefore not be used for the actual request.
The disk will be requested on an appropriate device
by means of message NKVD013 or NKVD014.

## NKVD074

Destination: CONSOLE Routing code: D Weight: 50

Warranty : NO

NKVD074 DISK '(&00)' CANNOT BE ASSIGNED TO DEVICE '(&01)'. USER REQUESTS ASSIGNMENT TO DEVICE '(&02)'

### Meaning

Processing of the disk was restricted by the user to a particular device.
The disk is to be remounted on the device (&02).

## NKVD075

Destination: CONSOLE Routing code: D Weight: 50

Warranty : NO

NKVD075 DISK '(&00)' CANNOT BE ASSIGNED TO DEVICE '(&01)'. DEVICE DOES NOT SUPPORT USER DEVICE DESCRIPTION

### Meaning

The device cannot be used as it is not of type requested by user. Message
NKVD013 or NKVD014 will request the disk again on a suitable device.

## NKVD076

Destination: CONSOLE Routing code: D Weight: 50

Warranty : NO

NKVD076 NO DEVICE OF THIS TYPE AVAILABLE FOR MOUNTED DISK. DISMOUNT DISK '(&00)' FROM DEVICE '(&01)'

### Meaning

The specified device is not available. Message NKVD013 or NKVD014 will
request the disk again on an available device.

## NKVD077

Destination: CONSOLE Routing code: D Weight: 50

Warranty : NO

NKVD077 DEVICE NOT AVAILABLE FOR MOUNTED DISK. DISMOUNT DISK '(&00)' FROM DEVICE '(&01)'

### Meaning

The specified device is not available. Message NKVD013 or NKVD014 will
request the disk again on an available device.

## NKVD078

Destination: CONSOLE Routing code: D Weight: 50

Warranty : NO

NKVD078 EXCHANGE NOT PERMITTED FOR PUBLIC DISKS. DISMOUNT DISK '(&00)' FROM DEVICE '(&01)'

### Meaning

It is not allow to withdraw the device for a PUBLIC disk.

## NKVD079

Destination: CONSOLE Routing code: D Weight: 50

Warranty : NO

NKVD079 DISK MONITOR NON-RESIDENT. MOVE OF PUBLIC DISK NOT POSSIBLE. DISMOUNT DISK '(&00)' FROM DEVICE '(&01)'

### Meaning

As the code of the disk monitor has not been generated in the resident
memory, a MOVE of the public disk is not permitted.

## NKVD080

Destination: CONSOLE Routing code: D Weight: 50

Warranty : NO

NKVD080 MONITOR ACTION FOR DISK '(&00)' ON DEVICE '(&01)' FOR TASK '(&02)' ABORTED, AS DISK IS NO LONGER IN USE

### Meaning

User terminated processing of the disk.

## NKVD081

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD081 REMOUNTING OF DISK '(&00)' ON DEVICE '(&01)' FOR TASK '(&02)' ABORTED BY OPERATOR

## NKVD082

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD082 DISK '(&00)' ON DEVICE '(&01)' IS A BS2000 DISK AND CAN THEREFORE NOT BE ASSIGNED TO A REQUEST FOR NON-STANDARD DISK

### Meaning

For reasons of data security it is not possible to assign a BS2000 disk
to a program requesting a NON-STANDARD disk.

## NKVD083

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD083 DISK MONITOR REQUEST ALREADY ACTIVE FOR DISK '(&00)' ON DEVICE '(&01)'. COMMAND NOT PROCESSED FOR THIS DISK

### Meaning

For the specified disk another monitor request is already active.
This request has to be completed first.

## NKVD084

Destination: CONSOLE Routing code: D Weight: 30

Warranty : NO

NKVD084 ACCESS TO VOL-, F1-, F5 LABEL OF DISK '(&00)' LOCKED BY OWN SYSTEM (VTOC-LOCK). CATALOG MAY BE LOCKED

### Meaning

Disk processing has been interrupted at a critical stage, e.g. by
dismounting of the disk or detaching of its device; processing can be
impaired considerably.
The disk must be remounted immediately. If no suitable device is
available,
the EXCHANGE function in the /CHANGE-DISK-MOUNT command must be used in
order to obtain a device, and the disk must be mounted.

## NKVD085

Destination: CONSOLE Routing code: D Weight: 50

Warranty : NO

NKVD085 WRONG DISK '(&00)' WITH TIME STAMP '(&01)' MOUNTED ON DEVICE '(&02)'. REPLACE MOUNTED DISK BY DISK WITH TIME STAMP '(&03)'

## NKVD088

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NKVD088 SPECIFIED DEVICE '(&00)' DETACHED. COMMAND FOR THIS DEVICE NOT POSSIBLE

## NKVD089

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD089 REMOUNTING OF DISK '(&00)' ON DEVICE '(&01)' FOR TASK '(&02)' ABORTED BY DRV, AS DISK IS USED FOR PAGING ONLY

### Meaning

DRV terminated usage of the disk.
Disk ist still used for PAGING only.
Files will be processed on the second disk.

## NKVD090

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD090 FOR DEVICE '(&00)' COMMAND TEMPORARILY NOT POSSIBLE. ASSIGNED DISK IS IN USE WITH USE MODE SPECIAL

## NKVD091

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD091 /UNLOCK-DISK FOR DISK '(&00)' ON DEVICE '(&01)' NOT PERMITTED. COMMAND NOT PROCESSED FOR THIS DISK

### Meaning

The command is not permitted as the disk is used as a shared PVS.
Reset of abnormally terminated foreign systems is processed by
system internal mechanisms.

## NKVD092

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NKVD092 ERROR ON INITIALIZING DISK MONITOR. SESSION RUNS WITHOUT MONITOR TASK

### Meaning

Task ' DM' is not available in the current session.
Only the HOME-PVS and PAGING disks can be allocated.

## NKVD099

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD099 NO FOREIGN SYSTEMS ASSIGNED TO DISK '(&00)' ON DEVICE '(&01)'. COMMAND NOT PROCESSED FOR THIS DISK

### Meaning

No allocating system is entered in the MRS-protocol of the disk
(cf. /SHOW-DISK-STATUS VOL=<vsn>,INF=SYSTEMS).

## NKVD103

Destination: CONSOLE Routing code: D Weight: 70

Warranty : NO

NKVD103 Target device not accessible. Answer for task '(&00)' rejected

### Meaning

The destination of the target device by the subsystem SHC-OSD was
not successfull or the state of the target device prohibits the
switching.

## NKVD104

Destination: CONSOLE Routing code: D Weight: 90

Warranty : NO

NKVD104 ERROR DURING MRSCAT ACCESS FOR CATALOG ID '(&00)'. REASON '(&01)'

### Meaning

(&01) is a description of the error:
01 : unknown PUBSET type
02 : catalog entry not found
03 : catalog id invalid
04 : MRSCAT not initialized
05 : no PUBRES-MN in catalog
06 : internal error

## NKVD105

Destination: CONSOLE Routing code: D Weight: 90

Warranty : NO

NKVD105 UNLOCK FOR PUBSET (&03) STARTING WITH DISK '(&00)' ON DEVICE '(&01)' FOR SYSTEMS '(&02)' ONLY IF THE SYSTEMS ARE TERMINATED. REPLY (<VSN>=CONTINUE; NO=ABORT UNLOCK)

### Meaning

Other systems (cf. /SHOW-DISK-STATUS ,INF=SYSTEMS) may only
be reset, if they do not use the disks; i. e. they have
terminated (abnormally) or all disks are in the state
CANCELLED.

## NKVD106

Destination: CONSOLE Routing code: D Weight: 90

Warranty : NO

NKVD106 $NDVGMN REPORTS ERROR (&01) ON DEVICE '(&00)'

## NKVD107

Destination: CONSOLE Routing code: D Weight: 90

Warranty : NO

NKVD107 WRONG ALLOCATION TIME ON DISK '(&00)' ON DEVICE '(&01)'

## NKVLOAD

Destination: USER-TASK Routing code: Weight:

Warranty : NO

NKVLOAD Program '(&00)',Version '(&01)' of '(&02)' loaded from file '(&03)'

## NKVT002

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT002 TAPE MONITOR NOT AVAILABLE

## NKVT010

Destination: CONSOLE Routing code: T Weight: 30

Warranty : NO

NKVT010 TAPE '(&00)' MOUNTED ON DEVICE '(&01)'

## NKVT011

Destination: CONSOLE Routing code: T Weight: 30

Warranty : NO

NKVT011 TAPE '(&00)' DISMOUNTED FROM DEVICE '(&01)'

## NKVT012

Destination: CONSOLE Routing code: T Weight: 90

Warranty : NO

NKVT012 PREMOUNT TAPE '(&00)' ON DEVICE '(&01)'; (USE='(&02)',WR='(&03)', TYPE='(&04)',(&05)). (&06)

### Meaning

If required, the operator has to confirm that (s)he is
ready to mount the specified tape.
(&00) : volume serial number (VSN) of the requested tape,
if specified by the user
(&01) : mnemonic of device proposed by the system
(&02) : usage mode (USE = DMS / SPECIAL)
(&03) : mode of access (WRITE-RING = ON / OFF / UNDEF)
(&04) : recording mode (volume-type)
(&05) : supplementary text, describing the application.
(&06) : description of operator reply.

### Response

ETX: the requested tape will be mounted
N : the requested tape is not available
MN : the requested tape will be mounted on device <MN>.
Mount the specified tape and switch on the device.
If required by the message, the operator has to confirm
that (s)he is ready to mount the tape.
No reply is required, if the system recognizes that the tape is mounted
and confirms this by displaying message NKVT017.
The system recognizes the mounting automatically only if the tape has a
standard label and if a VSN was specified by the user.

## NKVT013

Destination: CONSOLE Routing code: T Weight: 90

Warranty : NO

NKVT013 MOUNT TAPE '(&00)' ON DEVICE '(&01)'; (&02) (USE='(&03)',WR='(&04)', TYPE='(&05)',(&06)). '(&07)'

### Meaning

If required by the message, the operator has to confirm
that (s)he is ready to mount the specified volume.
(&00) : volume serial number (VSN) of the requested tape,
if specified by the user.
(&01) : mnemonic of device proposed by the system.
(&02) : reason for displaying the message, if the tape
is already mounted but cannot be assigned.
(&03) : usage mode (USE = DMS / SPECIAL)
(&04) : access (WRITE-RING = ON / OFF / UNDEF )
(&05) : recording mode (volume-type)
(&06) : supplementary text, describing the application.
(&07) : description of the operator reply.

### Response

ETX: the requested tape is mounted on the device proposed by the system
N : the requested tape is not available
MN : the requested tape is mounted on the device <MN>.
Mount the specified volume, switch on the device and
reply to the message, if required.
No reply is required, if the system recognizes that the tape is mounted
and confirms this by displaying message NKVT017.
The system recognizes the mounting automatically only if this is supported
by the device. Recognition of the tape by the system also requires that
the tape has a standard label and that its VSN was specified by the user.

## NKVT014

Destination: CONSOLE Routing code: T Weight: 90

Warranty : NO

NKVT014 REMOUNT TAPE '(&00)' ON DEVICE '(&01)'; (&02) (TYPE='(&03)'). '(&04)'

### Meaning

If required by the message, the operator has either to confirm that (s)he
is ready to remount the specified tape or terminate processing of the tape
by rejecting the message.
(&00) : volume serial number (VSN) of the tape, if specified by the user.
(&01) : mnemonic of device proposed by the system.
(&02) : reason for displaying the remount message.
(&03) : recording mode (volume-type).
(&04) : description of the operator reply.

### Response

Note: Not all answers described here are always allowed.
Refer to insert (&04) to see the currently allowed answers.
ETX: the requested tape is mounted on the device proposed by the system
N : the requested tape is not available to the requesting task.
Processing
of the tape is terminated
MN : the requested tape is mounted on the device <MN>
T : Remounting is terminated. The current I/O for the task issueing
the message is terminated with the error TAPE POSITION LOST.
Remount the specified tape and switch on the device. Reply to the message.
No reply is required, if the system recognizes that the tape is mounted
and confirms this by displaying message NKVT018.
The system recognizes the mounting automatically only if supported
by the device, if the tape has a standard label and if its VSN was
specified by the user.

## NKVT015

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKVT015 TAPE VSN '(&00)' NOT UNIQUE IN THE SYSTEM

### Meaning

The specified VSN exists more than once, or has been requested more than
once. No automatic allocation can be performed for this VSN.

## NKVT016

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT016 LOCATION '(&00)' IS NOT CORRECTLY DEFINED

## NKVT017

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKVT017 MOUNTING OF TAPE '(&00)' ON DEVICE '(&01)' FOR TASK '(&02)' COMPLETED

### Meaning

The mounting of a tape requested in message NKVT013 has been recognized
by the system. No further activities by the operator are required for this
tape. If the tape was mounted without a reply to NKVT013, it is assumed
that a reply is no longer required or possible, as an implicit reply has
been given by the system.

## NKVT018

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKVT018 REMOUNTING OF TAPE '(&00)' ON DEVICE '(&01)' FOR TASK '(&02)' COMPLETED

### Meaning

The remounting of a tape requested in message NKVT014 has been recognized
by the system. No further activities by the operator are required for this
tape. If the tape was mounted without a reply to NKVT014, it is assumed
that a reply is no longer required or possible, as an implicit reply has
been given by the system.

## NKVT021

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT021 REMOUNT FOR TAPE '(&00)' ON DEVICE '(&01)' FAILED. ACCESS RIGHT FOR TAPE WITHDRAWN (CANCELLED)

### Meaning

Due to an unrecoverable error during remount, the access right for the
user has been withdrawn. No further I/O operations for the tape are
permitted. The device is now free for the mounting of other tapes.
Only after release by its current user the tape can again be made
available for usage DMS (c.f. /SHOW-RESOURCE-ALLOCATION or
/SHOW-TAPE-STATUS).

## NKVT022

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT022 TAPE '(&00)' ON DEVICE '(&01)' CANCELLED BY OPERATOR

### Meaning

The tape has been cancelled by the operator by means of the command
/CHANGE-TAPE-MOUNT. No further I/O operations for the tape are permitted.
The device is now free for the mounting of other tapes.
Only after release by its current user the tape can again be made
available for USE=DMS (cf. /SHOW-RESOURCE-ALLOCATION or
/SHOW-TAPE-STATUS).

## NKVT024

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKVT024 EMPTY TAPE MOUNTED ON DEVICE '(&00)'. TAPE CAN ONLY BE PROCESSED WITH USE=SPECIAL

### Meaning

An empty tape can only be processed in usage mode SPECIAL (cf. message
NKVT013).

## NKVT025

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKVT025 DENSITY OF MOUNTED TAPE NOT SUPPORTED BY DEVICE '(&00)'. TAPE CAN ONLY BE PROCESSED ON THIS DEVICE WITH USE=SPECIAL

### Meaning

This tape cannot be read on the device (&00) because this
device does not support the density with which the tape
has been written.
On device (&00) the tape can only be used in use-mode
USE=SPECIAL. For to work with the tape in use-mode
USE=DMS it is necessary to remount the tape on another
device which supports the requested density.
This tape may only be processed in USE-mode SPECIAL (cf. message NKVT013).

## NKVT026

Destination: CONSOLE Routing code: T Weight: 30

Warranty : NO

NKVT026 DEVICE DEFECTIVE. REMOUNT TAPE '(&00)' ON DEVICE '(&01)'

### Meaning

The tape must be remounted. Processing of the tape is interrupted.
The tape will be requested again with message NKVT014.

## NKVT028

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT028 NO ADDITIONAL SUBTASK POSSIBLE

### Meaning

The maximum permissible number of temporary auxiliary tasks has been
reached, or due to a resource bottleneck no more tasks can be created.
The request can only be performed when an existing auxiliary task
terminates its action or when resources for task creation are available.

## NKVT030

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT030 TAPE '(&00)' WAS CANCELLED BY SYSTEM

### Meaning

The tape has been cancelled by the system. No further I/O operations
for the tape are permitted. The device is now free for the mounting of
other tapes.

## NKVT031

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT031 REMOUNT OF TAPE '(&00)' ON DEVICE '(&01)' COMPLETED

### Meaning

The remount-recover for tape (&00) which has been initiated
by system or by command /CHANGE-TAPE-MOUNT has been
terminated successfully. The tape is available again for
a further processing by the user.
If the operator mounted the tape without a reply of the
message NKVT014 this message will give a hint to the
operator that a reply of this message is no longer
required or possible because a reply has been given
by the system itself.

## NKVT032

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT032 REPOSITIONING OF TAPE '(&00)' ON DEVICE '(&01)' COMPLETED

### Meaning

After repositioning the tape is again available to the user.

## NKVT033

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT033 REPOSITIONING FOR TAPE '(&00)' ON DEVICE '(&01)' FAILED

### Meaning

Repositioning of the tape can be repeated after the subsequent message
NKVT014 has been replied to.

## NKVT034

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT034 REPOSITIONING FOR TAPE '(&00)' ON DEVICE '(&01)' FAILED. TAPE CANCELLED BY SYSTEM

### Meaning

Due to an unrecoverable error during repositioning of the specified tape
(undefined tape position), the access right for the tape has been
cancelled
by system. No further I/O operations for the tape are permitted. The
device is free for the mounting of other tapes.

## NKVT036

Destination: CONSOLE Routing code: T Weight: 30

Warranty : NO

NKVT036 TAPE IDENTITY CHANGED ON DEVICE '(&00)' FROM '(&01) (&02)' TO '(&03) (&04)'

### Meaning

The tape monitor recognized that the identity of the tape (label type and
VSN, if standard format) has been changed by the user.

## NKVT037

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT037 ACTION MOVE FOR TAPE (&00) ON DEVICE (&01) NOT ALLOWED. DEVICE IS ATL-CONTROLLED. COMMAND NOT PROCESSED.

### Meaning

The specified action is not performed, because for ATL-controlled
devices and tapes necessary exchanges of devices are automatically
recognized and performed.

## NKVT040

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT040 TAPE MONITOR TERMINATED. RESTART NOT POSSIBLE

### Meaning

Tape monitoring is no longer possible. The operator has to initiate
SHUTDOWN.

## NKVT041

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT041 SPECIFIED TAPE-DEVICE '(&00)' NOT DEFINED. COMMAND REJECTED FOR THIS DEVICE

## NKVT042

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT042 SPECIFIED TAPE '(&00)' UNKNOWN. COMMAND REJECTED FOR THIS TAPE

## NKVT043

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT043 SPECIFIED VSN '(&00)' OF TAPE NOT UNIQUE. COMMAND NOT PROCESSED FOR THIS TAPE

### Meaning

As the VSN of the tape is not unique, the tape has to be specified by
means of the mnemonic of the device assigned to the tape.

## NKVT044

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT044 TAPE POSITION OF TAPE '(&00)' ON DEVICE '(&01)' UNDEFINED. MOVE, EXCHANGE AND POSITIONING NOT POSSIBLE. COMMAND NOT PROCESSED FOR THIS TAPE

### Meaning

While the tape position is undefined, processing of the tape cannot be
interrupted. If processing is interrupted by manipulating the device
while the tape position is undefined, the system will cancel the tape
due to an unrecoverable error.

## NKVT046

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT046 FOR TAPE '(&00)' ON DEVICE '(&01)' NO ALTERNATIVE DEVICE AVAILABLE. COMMAND NOT PROCESSED FOR THIS TAPE

## NKVT048

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT048 DEVICE (&01) REMOVED FOR TAPE '(&00)'. TAPE IS NOW WAITING FOR AVAILABLE ALTERNATIVE DEVICE: TYP = '(&02)', LOCATION = '(&03)'

### Meaning

The device of tape has been removed. The tape is now waiting for an
alternative device (cf. ACTION-STATE NO_DEVICE in the output of the
command /SHOW-TAPE-STATUS).
Upon release of a suitable device Message NKVT049 documents cease of this
wait state. Mount of the tape is requested by NKVT012, NKVT013 or
NKVT014.
With the aid of the function EXCHANGE in the command /CHANGE-TAPE-MOUNT
the operator can transfer the wait state to another tape, thus obtaining
an appropriate device.
With the aid of the function CANCEL of the command /CHANGE-TAPE-MOUNT
the operator can terminate the waiting for a device by withdrawing the
access right from the user, i.e. by aborting processing.
If /CHANGE-TAPE-MOUNT is not possible (NO DEVICE for scratch request)
/CANCEL has to be used to abort processing.
(&00): VSN of tape in state NO DEVICE
(&01): MN of last used device if existing
(&02): volumetype to be supported by suitable alternative device
(&03): location of suitable alternative device if defined

## NKVT049

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKVT049 WAITING OF TAPE '(&00)' FOR ALTERNATIVE DEVICE TERMINATED

### Meaning

Waiting of the tape for an alternative device, started by NKVT048, has
terminated.

## NKVT050

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT050 NEW OPERAND FOR TAPE MONITORING: '(&00) = (&01)' FOR LOCATION '(&02)'

### Meaning

The setting of the values of the operands TAPE-MOUNT, ALLOCATE-TAPE,
UNLOAD-RELEASED-TAPE and NEXT-TAPE-MOUNT that can be specified
in the command MODIFY-MOUNT-PARAMETERS are protocoled.

## NKVT053

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT053 REMOUNTING OF TAPE '(&00)' ON DEVICE '(&01)' NOT PERMITTED BECAUSE THE ACTUAL DEVICE WAS REQUESTED BY THE USER WITH DEVICE-MNEMONIK. COMMAND NOT PROCESSED FOR THIS TAPE

### Meaning

Tape (&00) was allocated by the user in conjunction
with a specification of a device-mnemonik. Therefore,
tape (&00) is fix assigned to the device on which
the tape was mounted until now. A remounting
of the tape on the alternative device (&01) as
requested with the 'MOVE'- or 'EXCHANGE'-function
is not allowed.
If the device on which the tape has been mounted until
now is defective either the device has to be repaired by
a hardware-technician or the tape has to be cancelled
by the operator.

## NKVT054

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT054 SPECIFIED ACTION FOR TAPE '(&00)' ON DEVICE '(&01)' NOT PERMITTED. COMMAND NOT PROCESSED FOR THIS TAPE

### Meaning

The command has not been processed, as the requested function
of the command /CHANGE-TAPE-MOUNT is not possible because of the
current state the tape.
For more detailed information on the current state enter the command
/SHOW-TAPE-STATUS.

## NKVT056

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT056 NO TAPE ASSIGNED TO SPECIFIED DEVICE '(&00)'. COMMAND NOT PROCESSED FOR THIS DEVICE

### Meaning

A tape can only be specified by a device-mnemonik, if the tape is
assigned to this device.

## NKVT058

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT058 SYNTAX ERROR IN MESSAGE REPLY. REPLY FOR TASK '(&00)' REJECTED

## NKVT060

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT060 SPECIFIED DEVICE '(&00)' NOT DEFINED. REPLY FOR TASK '(&01)' REJECTED

### Meaning

The specified device is not defined. The reply to message NKVT012, NKVT013
or NKVT014 is rejected. The message will be reissued.

## NKVT061

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT061 USE OF DEVICE '(&00)' NOT POSSIBLE DUE TO WRONG DEVICE-TYPE. REPLY FOR TASK '(&01)' REJECTED

### Meaning

The specified device cannot be used because of its type. The reply to
NKVT012,NKVT013 or NKVT014 is rejected. The message will be reissued.

## NKVT062

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT062 SPECIFIED DEVICE '(&00)' NOT AVAILABLE DUE TO ITS CONFIGURATION-STATE. REPLY FOR TASK '(&01)' REJECTED

### Meaning

The specified device is due to it's configuration-state
(for example DETACHED, DETACH-PENDING, ATTACH-PENDING)
not available for mounting a tape.
The reply for message NKVT012, NKVT013 or
NKVT014 is rejected. The message will be reissued.

### Response

Check the configuration-state by means of one of the commands
/SHOW-DEVICE-STATUS or /SHOW-DEVICE-CONFIGURATION.

## NKVT063

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT063 SPECIFIED DEVICE '(&00)' ALREADY ASSIGNED TO ANOTHER TAPE. REPLY FOR TASK '(&01)' REJECTED

### Meaning

The specified device is not available. The reply to NKVT013 or NKVT014 is
rejected. The message will be reissued.

### Response

Check by means of the command /SHOW-TAPE-STATUS, whether the device is
assigned to another tape.

## NKVT064

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT064 ALL DEVICES OF SAME TYPE AS DEVICE '(&00)' ARE SECURED. REPLY FOR TASK '(&01)' REJECTED

### Meaning

The device is currently not available due to type-reservations by
other tasks. See also the output of /SHOW-DEVICE-STATUS INF=SUM.
The reply to message NKVT012, NKVT013 or NKVT014 is rejected. The message
will be reissued.
The device is not occupied by a particular tape, but the change of device
types implied by the requested assignment of an alternative device is not
possible.

## NKVT065

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT065 TAPE '(&00)' CAN ONLY BE ASSIGNED TO DEVICE '(&01)' (REQUEST BY DEVICE-MNEMONIK). REPLY FOR TASK '(&02)' REJECTED

### Meaning

The user does not permit an assignment to an alternative device. The
reply to NKVT013 or NKVT014 is rejected. The message will be reissued.

## NKVT066

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT066 SPECIFIED DEVICE '(&00)' CURRENTLY RESERVED BY DEVICE-MNEMONIK FOR AN APPLICATION. REPLY FOR TASK '(&01)' REJECTED

### Meaning

The device specified in the reply is secured for another application
with device-mnemonik (cf. /SHOW-DEVICE-STATUS UNIT= ). The tape will be
requested again in message NKVT012, NKVT013 or NKVT014 on the device
proposed by the system.

## NKVT067

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT067 DEVICE '(&00)' NOT AVAILABLE FOR TAPE '(&01)'

## NKVT068

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

NKVT068 ASSIGNED VSN '(&00)' ALREADY RESERVED FOR AN APPLICATION (&01); TAPE CANNOT BE ASSIGNED TO TASK '(&02)'

### Meaning

The assignment of tape (&00) by the operator has been
rejected by one of the following reasons :
1. The assigned tape-VSN is already reserved in the own
system by the requesting or another task in
USE-MODE=DMS. Therefore the same tape cannot be
assigned for the actual second request in USE-MODE=DMS.
The operator can get more information about the
allocation-state of the tape in the own system by
command /SHOW-TAPE-STATUS.
2. If there was specified a MAREN-message (&01), MAREN
rejects the allocation of the tape. The operator can
use the /HELP-command for MAREN-message (&01) or
call MAREN directly for to inform about the reason
of the rejection by MAREN.
Message NKVT013 will be repeated.

## NKVT069

Destination: CONSOLE Routing code: D Weight: 99

Warranty : NO

NKVT069 NO ASSIGNMENT TO ANOTHER DEVICE POSSIBLE FOR TAPE '(&00)' ON DEVICE '(&01)'. REPLY FOR TASK '(&02)' REJECTED

### Meaning

A tape is allocated on the device specified in the message reply. For
this tape no change of device allocation is permitted. The reply is
rejected. The message will be reissued.

## NKVT073

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKVT073 TAPE '(&00)' CANNOT BE ASSIGNED TO DEVICE '(&01)'. DEVICE ALREADY RESERVED BY AN APPLICATION BY DEVICE-MNEMONIK

### Meaning

The tape is mounted on a device reserved for another
application by means of device-mnemonik and could
therefore not be used for the actual request.
The tape will be requested on an appropriate device
by means of message NKVT012, NKVT013 or NKVT014.

## NKVT074

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKVT074 TAPE '(&00)' CANNOT BE ASSIGNED TO DEVICE '(&01)'. USER REQUESTS ASSIGNMENT TO DEVICE '(&02)'

### Meaning

The user restricted processing of the tape (&00) to a particular device.
The tape is to be moved from device (&01) to device (&02).

## NKVT075

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKVT075 TAPE '(&00)' CANNOT BE ASSIGNED TO DEVICE '(&01)'. DEVICE DOES NOT SUPPORT USER DEVICE DESCRIPTION (WRONG TYPE AND/OR WRONG LOCATION)

### Meaning

The device cannot be used due to its type or due to its location.
The tape will be requested again on an appropriate device by
means of message NKVT013 or NKVT014.

## NKVT076

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKVT076 NO DEVICE OF THIS TYPE AVAILABLE FOR MOUNTED TAPE. DISMOUNT TAPE '(&00)' FROM DEVICE '(&01)'

### Meaning

The device cannot be used due to type reservations by other tasks.
See also the output of /SHOW-DEVICE-STATUS INF=SUM.
The reply to message NKVT012, NKVT013 or NKVT014 is rejected. The message
will be reissued.
The device is not occupied by a particular tape, but the change of device
types implied by the requested assignment of an alternative device is not
possible.

## NKVT077

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKVT077 DEVICE IS NOT AVAILABLE FOR MOUNTED TAPE. DISMOUNT TAPE '(&00)' FROM DEVICE '(&01)'

### Meaning

The specified device is not available. The tape will be requested again
on an available device by means of NKVT013 or NKVT014.

## NKVT080

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKVT080 MONITOR-ACTION FOR TAPE '(&00)' ON DEVICE '(&01)' FOR TASK '(&02)' ABORTED, AS TAPE IS NO LONGER IN USE

## NKVT081

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT081 REMOUNTING OF TAPE '(&00)' ON DEVICE '(&01)' FOR TASK '(&02)' ABORTED BY OPERATOR

## NKVT083

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT083 MONITOR ALREADY ACTIVE FOR TAPE '(&00)' ON DEVICE '(&01)'. COMMAND NOT PROCESSED FOR THIS TAPE

### Meaning

For the specified tape another monitor action has to be completed first
(cf. the ACTION value in the output of the command /SHOW-TAPE-STATUS).
After the termination acknowledgement for the current monitor action can
be reissued.

## NKVT086

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKVT086 WARNING: LAST BLOCK OF TAPE '(&00)' WILL BE LOST, IF TAPE CANNOT BE REMOUNTED

### Meaning

For positioning of the tape a temporary erase of the last block written on
the tape was necessary. Positioning was interrupted in this critical
phase.
If remount is aborted, this last block will be lost.

## NKVT087

Destination: CONSOLE Routing code: T Weight: 50

Warranty : NO

NKVT087 LAST BLOCK OF TAPE '(&00)' LOST

### Meaning

For positioning of the tape a temporary erase of the last block written on
the tape was necessary. This last block has been lost as the remount
was aborted.

## NKVT088

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

NKVT088 SPECIFIED TAPE DEVICE '(&00)' IS DETACHED . COMMAND FOR THIS DEVICE NOT POSSIBLE

## NKVT090

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT090 FOR DEVICE '(&00)' COMMAND TEMPORARILY NOT POSSIBLE. ASSIGNED TAPE IS IN USE

## NKVT092

Destination: CONSOLE Routing code: T Weight: 99

Warranty : NO

NKVT092 ERROR DURING INITIALIZATION OF TAPE MONITOR. SESSION RUNS WITHOUT MONITOR TASK

### Meaning

Task ' TM' is not available in the current session.
Tapes cannot be allocated.

## NKVT093

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT093 POSITION AND BLOCKS OF TAPE '(&00)' ON DEVICE '(&01)' CANNOT BE SAVED. COMMAND REJECTED FOR THIS TAPE

### Meaning

Position and data of the specified tape cannot be saved. REMOUNT recovery
will be initiated.

## NKVT094

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT094 POSITION AND BLOCKS OF TAPE '(&00)' ON DEVICE '(&01)' NOT SAVED. ASSIGNMENT TO ANOTHER DEVICE NOT POSSIBLE. ANSWER FOR TASK '(&02)' REJECTED

### Meaning

Position and data of the specified tape are not saved. The tape must be
mounted on the proposed device.

## NKVT095

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT095 BLOCKS OF TAPE '(&00)' ON DEVICE '(&01)' LOST

### Meaning

Blocks of the specified tape are lost because remount was aborted.

## NKVT096

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT096 OVERWRITING THE TAPE ON DEVICE '(&00)' NOT ALLOWED

### Meaning

It is not allowed to overwrite the tape because of possible
input/output errors.

## NKVT097

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT097 UNLOADING OF TAPE '(&00)' FROM DEVICE '(&01)' INITIATED

## NKVT098

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT098 I/O-ERROR ON DEVICE '(&00)' (&01). COMMAND NOT SUCCESSFUL FOR THIS DEVICE

### Meaning

An I/O-Error prevents a successful command-execution
(&01) is a short description of the error on device (&00).

## NKVT100

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

NKVT100 UNRECOVERABLE ERROR DURING RESTART OF TAPE MONITOR. TAKE DUMP

### Meaning

The tape monitor terminated because of error during restart.

## NKVT101

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT101 location of device '(&00)' cannot be changed

### Meaning

A volume is assigned to device (&00). Change of location is
possible for free devices only.

### Response

Use command /SHOW-DEVICE-STATUS for more information.

## NKVT102

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT102 Device '(&00)' in location '(&01)' is allocated

### Meaning

Device (&00) in location (&01) is allocated. Command
REMOVE-DEVICE-DEPOT UNIT=*ALL is not allowed.

### Response

Use command /SHOW-DEVICE-STATUS for more information.

## NKVT110

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT110 INVENTORY FOR DEVICE '(&00)' STARTED

## NKVT111

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT111 INVENTORY FOR DEVICE '(&00)' COMPLETED

## NKVT112

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT112 INVENTORY FOR DEVICE '(&00)' ABORTED

## NKVT113

Destination: USER-TASK, CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT113 INVENTORY FOR DEVICE '(&00)' COMPLETED WITH WARNING

### Meaning

An error occurred during inventory or there is at least one volume
without label. The inventory was not aborted. Previous messages might
give informations about the problem.

### Response

Issue SHOW-TAPE INFORMATION INF=CARTRIDGE-LOADER to get informations
about the volumes obtained by inventory.
Check existing error messages and retry the inventory if necessary.

## NKVT115

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT115 DEVICE '(&00)' IS IN RANDOM MODE

## NKVT116

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT116 DEVICE '(&00)' IS NO LONGER IN RANDOM MODE

## NKVT117

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT117 INVENTORY FOR DEVICE '(&00)' ABORTED. MODE IS SET TO MANUAL

## NKVT118

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT118 INVENTORY FOR DEVICE '(&00)' NOT POSSIBLE. MODE IS SET TO MANUAL

### Meaning

Possible reasons:
1. Unload is not possible because of volumes in IO cell and device.
2. Stacker is empty.
3. Unload is not possible because there is a volume in the device
and no IO cell exists.

## NKVT120

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT120 COMMAND FOR DEVICE '(&00)' CURRENTLY NOT POSSIBLE. INVENTORY IS IN PROCESS

## NKVT121

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT121 VOLUME ON DEVICE '(&00)' NOT COMPLETELY FORMATTED. CURRENT CAPACITY '(&01) %'

## NKVT125

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT125 UNLOAD ON DEVICE '(&00)' NOT POSSIBLE. DESTINATION CELL IS OCCUPIED

### Meaning

While unloading a cartridge the automatic cartridge facility has
determined that the destination cell is occupied, probably by
manual intervention.

## NKVT126

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT126 LOAD ON DEVICE '(&00)' NOT POSSIBLE. SOURCE CELL IS EMPTY

### Meaning

While loading a cartridge the automatic cartridge facility has
determined that the source cell is empty, probably by manual
intervention.

## NKVT131

Destination: CONSOLE Routing code: T Weight: 70

Warranty : NO

NKVT131 Tape '(&00)' on device '(&01)' has wrong medium type

### Meaning

Requested VSN was recognized but type does not correspond to
mounted type. Possible reasons:
- WORM requested but no WORM medium mounted
- no WORM requested but WORM medium mounted
- wrong level (e. g. TAPE-U2 requested but TAPE-U3 mounted).

### Response

Check input or inform responsible administrator.

## NKV0001

Destination: CONSOLE Routing code: * (main console) Weight: 30

Warranty : YES

NKV0001 SYNTAX ERROR IN COMMAND. COMMAND REJECTED

## NKV0004

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

NKV0004 COMMAND PARTIALLY PROCESSED

## NKV0005

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

NKV0005 COMMAND NOT PROCESSED FOR OBJECTS IN INPUT LIST

## NKV0006

Destination: CONSOLE Routing code: * (main console) Weight: 70

Warranty : YES

NKV0006 COMMAND NOT PROCESSED

## NKV0007

Destination: CONSOLE Routing code: * (main console) Weight: 99

Warranty : NO

NKV0007 WARNING: PARAMETER SCRATCH-TAPES IS IGNORED. LOCATION FOR SCRATCH REQUEST IS SELECTED BY MAREN

## NKV1000

Destination: USER-TASK Routing code: Weight: 30

Warranty : NO

NKV1000 NKV DETECTED SOFTWARE-ERROR: '(&00)'. TAKE DUMP

### Meaning

(&00): description of the detected error.

©2025 Fujitsu | BS2000 System Messages